Cisco Prime Infrastructure API
Prime Infrastructure API Documentation

GET_WlanControllerDetails

# GET WlanControllerDetails

- Jump To

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Response Formats | xml json
HTTP Methods | GET

Represents detail information about a WLAN controller.

## Resource URL

/webacs/api/v1/data/WlanControllerDetails

Since : 1.2

## Response Parameters

Type | Attribute Name | Description
--- | --- | ---
AlarmSeverityEnum | alarmStatus | Allowed values: CRITICAL MAJOR MINOR WARNING CLEARED INFORMATION
int | apCount | number of access
WLCApGroups[] | apGroups | AP groups and their profiles for this device.
Type | Attribute Name | Description
--- | --- | ---
String | apGroupDescription | The supplied description of the AP group.
String | apGroupName | The name of the AP group.
WLCApGroupMappings[] | apGroupProfileMappings | Profiles mapped to this AP group.
Type | Attribute Name | Description
--- | --- | ---
String | interfaceName | The name of the interface or interface group for this mapping.
boolean | nacOverrideSupport | Is NAC override supported?
String | profileName | The name of the profile for this mapping.
AuditStatusEnum | auditStatus | Audit status Allowed values: NA MISMATCH IDENTICAL UNREACHABLE
boolean | autoRefresh | auto refresh state
String | capwapTransportMode | Current CAPWAP transport mode
WLCCDPNeighbor[] | cdpNeighbors | CDP neighbors for this controller.
Type | Attribute Name | Description
--- | --- | ---
CDPDuplexEnum | duplexMode | The duplex mode between the local device and the neighbor. Allowed values: NA UNKNOWN HALFDUPLEX FULLDUPLEX
String | farEndInterface | The interface on the neighbor device connected to the local device.
int | interfaceIndex | The index of the local interface.
String | nearEndInterface | The interface on the local device connected to the neighbor device.
String | neighborCapabilities | Neighbor capabilities as reported by SNMP.
String | neighborDeviceName | The neighbor device's name.
String | neighborDevicePlatformType | The neighbor device's platform type.
String | neighborVersion | Neighbor device's firmware version.
String | contact | contact
String | cryptoCard1Supported | Crypto Card One
String | cryptoCard2Supported | Crypto card two
int | dot11aClientCount | number of dot11a/n clients associated with the controller
int | dot11bClientCount | number of dot11bgn clients associated with the controller
String | gigCardSupported | Gig Ethernet/Fiber Card
String | ipAddress | management IP address of the WLAN controller
String | lastBackup |
String | location | device location set in MIB2
String | macAddress | Burned-in MAC address
String | mobilityGroupName | Mobility group name
String | modelNumber | Model number
String | name | device name
int | numberOfAPsSupported | Number of APs supported
WLCPorts[] | ports | Represents port information for this controller.
Type | Attribute Name | Description
--- | --- | ---
StatusEnum | adminStatus | The desired state of this port. Allowed values: UNKNOWN ENABLED DISABLED
PortDuplexModeEnum | desiredDuplexMode | The configured duplex mode. Allowed values: UNKNOWN AUTONEGOTIATE HALFDUPLEX10MBPS FULLDUPLEX10MBPS HALFDUPLEX100MBPS FULLDUPLEX100MBPS FULLDUPLEX1000SX HALFDUPLEX1000MBPS FULLDUPLEX1000MBPS HALFDUPLEX10000MBPS FULLDUPLEX10000MBPS
int | portNumber | The assigned number of the port.
String | productDescription | Product description
boolean | reachabilityStatus | SNMP reachability
String | rfGroupName | RF group name
String | serialNumber | Serial number
String | softwareVersion | software version running on the controller
String | type | device type

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

## Sample XML Payload

https://192.168.116.207/webacs/api/v1/data/WlanControllerDetails/42

    <?xml version="1.0" encoding="UTF-8" standalone="yes"?>
    <queryResponse rootUrl="/webacs/data" requestUrl="https://192.168.116.207/webacs/api/v1/data/WlanControllerDetails/42" responseType="getEntity">
        <entity url="/webacs/data/className/15" type="className" dtoType="wlanControllerDetailsDTO_$$_javassist_5947">
            <wlanControllerDetailsDTO id="15" displayName="String value">
                <alarmStatus>CRITICAL</alarmStatus>
                <apCount>1</apCount>
                <apGroups>
                    <apGroup>
                        <apGroupDescription>String value</apGroupDescription>
                        <apGroupName>String value</apGroupName>
                        <apGroupProfileMappings>
                            <apGroupProfileMapping>
                                <interfaceName>String value</interfaceName>
                                <nacOverrideSupport>true</nacOverrideSupport>
                                <profileName>String value</profileName>
                            </apGroupProfileMapping>
                        </apGroupProfileMappings>
                    </apGroup>
                </apGroups>
                <auditStatus>NA</auditStatus>
                <autoRefresh>true</autoRefresh>
                <capwapTransportMode>String value</capwapTransportMode>
                <cdpNeighbors>
                    <cdpNeighbor>
                        <duplexMode>NA</duplexMode>
                        <farEndInterface>String value</farEndInterface>
                        <interfaceIndex>1</interfaceIndex>
                        <nearEndInterface>String value</nearEndInterface>
                        <neighborCapabilities>String value</neighborCapabilities>
                        <neighborDeviceName>String value</neighborDeviceName>
                        <neighborDevicePlatformType>String value</neighborDevicePlatformType>
                        <neighborVersion>String value</neighborVersion>
                    </cdpNeighbor>
                </cdpNeighbors>
                <contact>String value</contact>
                <cryptoCard1Supported>String value</cryptoCard1Supported>
                <cryptoCard2Supported>String value</cryptoCard2Supported>
                <dot11aClientCount>1</dot11aClientCount>
                <dot11bClientCount>1</dot11bClientCount>
                <gigCardSupported>String value</gigCardSupported>
                <ipAddress>String value</ipAddress>
                <lastBackup>String value</lastBackup>
                <location>String value</location>
                <macAddress>String value</macAddress>
                <mobilityGroupName>String value</mobilityGroupName>
                <modelNumber>String value</modelNumber>
                <name>String value</name>
                <numberOfAPsSupported>1</numberOfAPsSupported>
                <ports>
                    <port>
                        <adminStatus>UNKNOWN</adminStatus>
                        <desiredDuplexMode>UNKNOWN</desiredDuplexMode>
                        <portNumber>1</portNumber>
                    </port>
                </ports>
                <productDescription>String value</productDescription>
                <reachabilityStatus>true</reachabilityStatus>
                <rfGroupName>String value</rfGroupName>
                <serialNumber>String value</serialNumber>
                <softwareVersion>String value</softwareVersion>
                <type>String value</type>
            </wlanControllerDetailsDTO>
        </entity>
    </queryResponse>

## Sample JSON Payload

https://192.168.116.207/webacs/api/v1/data/WlanControllerDetails/42.json

    {
      "queryResponse" : {
        "@rootUrl" : "\/webacs\/data",
        "@requestUrl" : "https : \/\/192.168.116.207\/webacs\/api\/v1\/data\/WlanControllerDetails\/42",
        "@responseType" : "getEntity",
        "entity" : {
          "@url" : "\/webacs\/data\/className\/15",
          "@type" : "className",
          "@dtoType" : "wlanControllerDetailsDTO_$$_javassist_5947",
          "wlanControllerDetailsDTO" : {
            "@id" : "15",
            "@displayName" : "String value",
            "alarmStatus" : "CRITICAL",
            "apCount" : 1,
            "apGroups" : {
              "apGroup" : {
                "apGroupDescription" : "String value",
                "apGroupName" : "String value",
                "apGroupProfileMappings" : {
                  "apGroupProfileMapping" : {
                    "interfaceName" : "String value",
                    "nacOverrideSupport" : true,
                    "profileName" : "String value"
                  }
                }
              }
            },
            "auditStatus" : "NA",
            "autoRefresh" : true,
            "capwapTransportMode" : "String value",
            "cdpNeighbors" : {
              "cdpNeighbor" : {
                "duplexMode" : "NA",
                "farEndInterface" : "String value",
                "interfaceIndex" : 1,
                "nearEndInterface" : "String value",
                "neighborCapabilities" : "String value",
                "neighborDeviceName" : "String value",
                "neighborDevicePlatformType" : "String value",
                "neighborVersion" : "String value"
              }
            },
            "contact" : "String value",
            "cryptoCard1Supported" : "String value",
            "cryptoCard2Supported" : "String value",
            "dot11aClientCount" : 1,
            "dot11bClientCount" : 1,
            "gigCardSupported" : "String value",
            "ipAddress" : "String value",
            "lastBackup" : "String value",
            "location" : "String value",
            "macAddress" : "String value",
            "mobilityGroupName" : "String value",
            "modelNumber" : "String value",
            "name" : "String value",
            "numberOfAPsSupported" : 1,
            "ports" : {
              "port" : {
                "adminStatus" : "UNKNOWN",
                "desiredDuplexMode" : "UNKNOWN",
                "portNumber" : 1
              }
            },
            "productDescription" : "String value",
            "reachabilityStatus" : true,
            "rfGroupName" : "String value",
            "serialNumber" : "String value",
            "softwareVersion" : "String value",
            "type" : "String value"
          }
        }
      }
    }