Cisco Prime Infrastructure API
Prime Infrastructure API Documentation

GET_AutoApRadioDetails

# GET AutoApRadioDetails

- Jump To

### Resource Information

Rate Limiting? | Yes
Sorting? | Yes
Paging? | Yes
Filtering? | Yes
Response Formats | xml json
HTTP Methods | GET

Represents a radio interface of an autonomous access point.

## Resource URL

/webacs/api/v1/data/AutoApRadioDetails

Since : 1.2

## Response Parameters

Type | Attribute Name | Description
--- | --- | ---
RadioAdminStatusEnum | adminStatus | Administrative status of the radio interface Allowed values: UNKNOWN ENABLE DISABLE
float | antennaAzimAngle | Antenna Azim. Angle
String | antennaDiversity | Antenna diversity
float | antennaElevAngle | Antenna Elev. angle
int | antennaGain | raw value from device. It is different from displayed in the UI.
String | antennaMode | Antenna mode
String | antennaName | Antenna name
String | antennaType | Antenna type (Internal or External)
String | apIpAddress | IP address of the access point
String | apName | Name of the access point
String | baseRadioMac | Base radio MAC address
String | channelControl | Radio channel control
ChannelNumberEnum | channelNumber | current operational channel number Allowed values: UNKNOWN _1 _2 _3 _4 _5 _6 _7 _8 _9 _10 _11 _12 _13 _14 _20 _21 _22 _23 _24 _25 _26 _34 _36 _38 _40 _42 _44 _46 _48 _52 _56 _60 _64 _100 _104 _108 _112 _116 _120 _124 _128 _132 _136 _140 _149 _153 _157 _161 _165 _169 _173
String | clientCount | client count connected to the radio interafce
String | ethernetMac | MAC address of the ethernet interface on the AP
String | ifDescr | SNMP ifDescr
boolean | nativePowerUseStandard | Native power use standard
Cd11HtPhyOperBandEnum | operBand | 802.11 operational band Allowed values: UNKNOWN BAND24GHZ BAND5GHZ
RadioOperStatusEnum | operStatus | operational status of the radio interface Allowed values: DOWN UP NOTASSOCIATED UNKNOWN
Dot11PhyTypeEnum | phyType | 802.11 phy type Allowed values: UNKNOWN FHSS DSSS IRBASEBAND OFDM HRDSSS ERP HT
int | powerLevel | power level of the radio
String | radioMac | Radio MAC address
AutoApRadioRoleEnum | radioRole | Radio role Allowed values: UNKNOWN WGB BRIDGE CLIENT ROOT REPEATER APBRIDGE APREPEATER IBSS NRBRIDGE APBRBRIDGE SCANNER
String | radioType | radio type (802.11a/b/g/n)

Sample payloads are for information only. They are automatically generated and the values included may not be representative of actual valid data values.

## Sample XML Payload

https://192.168.116.207/webacs/api/v1/data/AutoApRadioDetails/42

    <?xml version="1.0" encoding="UTF-8" standalone="yes"?>
    <queryResponse rootUrl="/webacs/data" requestUrl="https://192.168.116.207/webacs/api/v1/data/AutoApRadioDetails/42" responseType="getEntity">
        <entity url="/webacs/data/className/15" type="className" dtoType="autoApRadioDetailsDTO_$$_javassist_5975">
            <autoApRadioDetailsDTO id="15" displayName="String value">
                <adminStatus>UNKNOWN</adminStatus>
                <antennaAzimAngle>3.0</antennaAzimAngle>
                <antennaDiversity>String value</antennaDiversity>
                <antennaElevAngle>3.0</antennaElevAngle>
                <antennaGain>1</antennaGain>
                <antennaMode>String value</antennaMode>
                <antennaName>String value</antennaName>
                <antennaType>String value</antennaType>
                <apIpAddress>String value</apIpAddress>
                <apName>String value</apName>
                <baseRadioMac>String value</baseRadioMac>
                <channelControl>String value</channelControl>
                <channelNumber>UNKNOWN</channelNumber>
                <clientCount>String value</clientCount>
                <ethernetMac>String value</ethernetMac>
                <ifDescr>String value</ifDescr>
                <nativePowerUseStandard>true</nativePowerUseStandard>
                <operBand>UNKNOWN</operBand>
                <operStatus>DOWN</operStatus>
                <phyType>UNKNOWN</phyType>
                <powerLevel>1</powerLevel>
                <radioMac>String value</radioMac>
                <radioRole>UNKNOWN</radioRole>
                <radioType>String value</radioType>
            </autoApRadioDetailsDTO>
        </entity>
    </queryResponse>

## Sample JSON Payload

https://192.168.116.207/webacs/api/v1/data/AutoApRadioDetails/42.json

    {
      "queryResponse" : {
        "@rootUrl" : "\/webacs\/data",
        "@requestUrl" : "https : \/\/192.168.116.207\/webacs\/api\/v1\/data\/AutoApRadioDetails\/42",
        "@responseType" : "getEntity",
        "entity" : {
          "@url" : "\/webacs\/data\/className\/15",
          "@type" : "className",
          "@dtoType" : "autoApRadioDetailsDTO_$$_javassist_5975",
          "autoApRadioDetailsDTO" : {
            "@id" : "15",
            "@displayName" : "String value",
            "adminStatus" : "UNKNOWN",
            "antennaAzimAngle" : 3,
            "antennaDiversity" : "String value",
            "antennaElevAngle" : 3,
            "antennaGain" : 1,
            "antennaMode" : "String value",
            "antennaName" : "String value",
            "antennaType" : "String value",
            "apIpAddress" : "String value",
            "apName" : "String value",
            "baseRadioMac" : "String value",
            "channelControl" : "String value",
            "channelNumber" : "UNKNOWN",
            "clientCount" : "String value",
            "ethernetMac" : "String value",
            "ifDescr" : "String value",
            "nativePowerUseStandard" : true,
            "operBand" : "UNKNOWN",
            "operStatus" : "DOWN",
            "phyType" : "UNKNOWN",
            "powerLevel" : 1,
            "radioMac" : "String value",
            "radioRole" : "UNKNOWN",
            "radioType" : "String value"
          }
        }
      }
    }