# 2. New UCM Server and Site

Function | Description | Note
Deployment Model and Template Information | Deployment Model - Unified CM BE – 500 Users - Unified CM – 1000 Users - Unified CM – 2500 Users - Unified CM – 5000 Users - Unified CM – 10000 Users Unified CM Template - Unified CM Template | • Deployment Model support: - 500 users with CUCMBE6K for up to 50 remote sites on 1 Server running VMWare and co-resident CUC. Ask if they want one or two servers. One server is the default. - 1000 users with CUCM & CUC for up to 90 remote sites on 2 CUCM servers + 1 CUC Server Ask if they want two or three CUCM servers. Two servers is the default. - 2500 users with CUCM & CUC for up to 500 remote sites on 3 CUCM Servers + 1 CUC Server Ask if they want three or five servers. Three servers is the default. - 5000 users with CUCM & CUC for up to 500 remote sites on 3 CUCM Servers + 1 CUC Server Ask if they want three or five servers. Three servers is the default. - 10,000 users with CUCM & CUC for up to 500 remote sites on 5 CUCM Servers + 1 CUC Server Five servers is the only choice. • The Unified CM Template is in the ‘template/server’ directory, with a filename like ‘CUCM.tar’. SBCC reads the template names and display them in the selection list. After a template is chosen, SBCC checks the Unified CM version from the header.txt file.
Server and Site Information | - Server Names (1, 2, 3, 4 or 5) - Remote Sites (0-500) - Use 2 or 3 Digit Site Codes - Site Information CSV - Enable LDAP Synchronization - Save all data for future sessions | · 500 Users - The number of remote sites is 0-50. 1000 Users – The number of remote sites is 0-90. 2500 – 10,000 Users – The number of remote sites is 0-500. · Up to 90 sites – Use 2 digit site codes More than 90 sites – Use 3 digit site codes · Format of the Site Information CSV: Site Name, DMI Subnet, DMI Subnet Mask, SIP Gateway IP Address, Secondary SIP Gateway IP Address, Site Code (Leave the secondary SIP IP Gateway Address and Site Code blank if they will not be used)
Site Information | - Site Name - DMI Subnet - DMI Subnet Mask - IP Address of the SIP Gateway - IP Address of the second SIP gateway - Site Codes | Enter the detailed information for each site.
LDAP System Information | - LDAP System Information - LDAP Custom Filter - LDAP Directory and Authentication Information | · Choose the LDAP server type and LDAP Attribute for User ID · Create an LDAP custom filter to only include users that match a certain attribute, like users with an IP Phone · Enter the LDAP information needed for setting up directory synchronization and user authentication
Field Mapping Information | - Phone Number - Mail ID - Middle Name | Select the fields in the LDAP/CSV file which map to the specific fields in Unified CM
Unified CM Dian-Plan Information | - Phone Auto Registration w/ DN Extension Range - Voice Messaging Information - Dial Plan Template | Enter the directory number range start and range end for auto registration numbers Voice Messaging Information includes Voicemail ports, Hunt, MWI On Number and MWI OFF Number. Select the Dial Plan template for this cluster
Phone NTP and Date/Time Group Information | - Phone NTP Reference - Date/Time Group | Enter the NTP server IP address for phones and choose the NTP mode Enter the group name, time zone, date separator, date format and time format for the phones
Summary Information | Summary | Show all the parameters of the previous steps for a final confirmation.
Configuration Information | Export File - File Name Configure Server - IP Address - Username - Password | SBCC provide two ways to save the configuration: Export File - SBCC provides a default file name in the format Export_ Server_YYYYMMDDhhmm.tar (Example: Export _Server_201207061530.tar). The file name can be modified and the file is stored in the directory ‘packet/server’. Configure Server - SBCC will connect to Unified CM and then check the version. If the version of template is different, SBCC will prompt that the Unified CM version does not match and the server cannot be updated. Otherwise, if they are the same, SBCC will configure Unified CM with AXL/SOAP in real-time. * Configuration value consists of the data entered by the SBCC and the data in template packet. * The two options are multiple choice and they both can be chosen at the same time.
Update Information | Update Information | Execute the configuration changes and display the log.