# 3. New UCM and CUC Users and Device Profile s

Function | Description | Note
User Information | CSV File | There is one option for the user data source: CSV File
Field Mapping Information | User ID Phone Number Department Mail ID First Name Middle Name Last Name Manager User ID | Set field mapping between United CM and the CSV data source.
User and Device Profile Information | Device Profile Name Description User ID * Directory Number * External Phone Number Mask Line CSS Device Profile * | SBCC will load the data and display them in a table UI for batch editing. Device Profile Name, Description and User ID are read-only values. SBCC has UDP templates with default values for various phone types in directory ../Template/UDP, e.g. UDP-7960, UDP-7975, etc.
Configuration Information | Export File Configure Server CUCM: IP Address, Username, Password CUC: IP Address, Username, Password | SBCC provides two ways to save the configuration: Export File - SBCC provides a default filename in the format User_YYYYMMDDhhmm (for example User_201107061530). The filename can be modified and it will be stored in the directory ../packet/user. Configure Server SBCC will configure Unified CM through AXL in real-time. (Note: User and Device Profiles consist of data entered by the SBCC and UDP template.) SBCC will configure Unity Connection through CUPI in real-time.
Update Information | Update Information | Execute configuration changes and displays the log.