complexType UpdateCiscoCatalyst6000E1VoIPGatewayReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:NameAndGUIDRequest
properties |
base | axlapi:NameAndGUIDRequest
children | name uuid newName description callingSearchSpaceName devicePoolName commonDeviceConfigName networkLocation locationName networkLocale mediaResourceListName automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig mlppDomainId useTrustedRelayPoint cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName redirectInboundNumberIe calledPlan calledPri callerIdDn callingPartySelection callingPlan callingPri chanIe clockReference dChannelEnable channelSelectionOrder displayIE pcmType csuParam firstDelay interfaceIdPresent interfaceId intraDelay mcdnEnable redirectOutboundNumberIe numDigitsToStrip passingPrecedenceLevelThrough prefix callingLinePresentationBit connectedLineIdPresentation priProtocol securityAccessLevel sendCallingNameInFacilityIe sendExLeadingCharInDispIe sendRestart setupNonIsdnPi sigDigits span statusPoll smdiBasePort packetCaptureMode packetCaptureDuration transmitUtf8 v150 asn1RoseOidEncoding QSIGVariant unattendedPort cdpnTransformationCssName useDevicePoolCdpnTransformCss nationalPrefix internationalPrefix unknownPrefix subscriberPrefix geoLocationFilterName nationalStripDigits internationalStripDigits unknownStripDigits subscriberStripDigits nationalTransformationCssName internationalTransformationCssName unknownTransformationCssName subscriberTransformationCssName useDevicePoolCgpnTransformCssNatl useDevicePoolCgpnTransformCssIntl useDevicePoolCgpnTransformCssUnkn useDevicePoolCgpnTransformCssSubs pstnAccess imeE164TransformationName
used by |
element | updateCiscoCatalyst6000E1VoIPGateway
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="UpdateCiscoCatalyst6000E1VoIPGatewayReq"> <xsd:complexContent> <xsd:extension base="axlapi:NameAndGUIDRequest"> <xsd:sequence> <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="networkLocale" type="axlapi:XCountry" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/> <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="redirectInboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="calledPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="calledPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callerIdDn" type="axlapi:String255" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" default="Originator" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="chanIe" type="axlapi:XPRIChanIE" default="Use Number when 1B" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="dChannelEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="channelSelectionOrder" type="axlapi:XTrunkSelectionOrder" default="Top Down" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="displayIE" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="firstDelay" type="axlapi:XInteger" default="32" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="interfaceIdPresent" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="interfaceId" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="intraDelay" type="axlapi:XInteger" default="4" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="mcdnEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="redirectOutboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="numDigitsToStrip" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="passingPrecedenceLevelThrough" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="prefix" type="xsd:string" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingLinePresentationBit" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="connectedLineIdPresentation" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="priProtocol" type="axlapi:XPriProtocol" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="securityAccessLevel" type="axlapi:XInteger" default="2" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendCallingNameInFacilityIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendExLeadingCharInDispIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendRestart" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="setupNonIsdnPi" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sigDigits" nillable="false" minOccurs="0"> <xsd:annotation> <xsd:documentation>The value for sigDigits must be between 0 to 32. enable attribute is read only</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element> <xsd:element name="span" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="statusPoll" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="packetCaptureMode" type="axlapi:XPacketCaptureMode" default="None" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="packetCaptureDuration" type="axlapi:XInteger" default="0" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="transmitUtf8" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="v150" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="asn1RoseOidEncoding" type="axlapi:XASN1RoseOidEncoding" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only if PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="QSIGVariant" type="axlapi:XQSIGVariant" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="unattendedPort" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssNatl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssIntl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssUnkn" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssSubs" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/newName

diagram |
type | axlapi:UniqueString128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
The device name,using only URL-friendly characters
source | <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/description

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
Optional description of the device
source | <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callingSearchSpaceName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/devicePoolName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/commonDeviceConfigName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/networkLocation

diagram |
type | axlapi:XNetworkLocation
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use System Default
nillable | false
annotation |
documentation
The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.
source | <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/locationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/networkLocale

diagram |
type | axlapi:XCountry
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="networkLocale" type="axlapi:XCountry" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/mediaResourceListName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/automatedAlternateRoutingCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/aarNeighborhoodName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/loadInformation

diagram |
type | axlapi:XLoadInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
special | axlapi:boolean |  |  |  |
annotation |
documentation
For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.
source | <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/vendorConfig

diagram |
type | axlapi:XVendorConfig
properties |
minOcc | 0
maxOcc | 1
content | complex
source | <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/mlppDomainId

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
This setting only effects devices that support MLPP. Use -1 to set to null
source | <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useTrustedRelayPoint

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/cgpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCgpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/geoLocationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/redirectInboundNumberIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="redirectInboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/calledPlan

diagram |
type | axlapi:XNumberingPlan
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="calledPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/calledPri

diagram |
type | axlapi:XPriOfNumber
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="calledPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callerIdDn

diagram |
type | axlapi:String255
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 255 |
source | <xsd:element name="callerIdDn" type="axlapi:String255" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callingPartySelection

diagram |
type | axlapi:XCallingPartySelection
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Originator
nillable | false
source | <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" default="Originator" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callingPlan

diagram |
type | axlapi:XNumberingPlan
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="callingPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callingPri

diagram |
type | axlapi:XPriOfNumber
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="callingPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/chanIe

diagram |
type | axlapi:XPRIChanIE
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use Number when 1B
nillable | false
source | <xsd:element name="chanIe" type="axlapi:XPRIChanIE" default="Use Number when 1B" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/clockReference

diagram |
type | axlapi:XClockReference
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/dChannelEnable

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="dChannelEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/channelSelectionOrder

diagram |
type | axlapi:XTrunkSelectionOrder
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Top Down
nillable | false
source | <xsd:element name="channelSelectionOrder" type="axlapi:XTrunkSelectionOrder" default="Top Down" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/displayIE

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="displayIE" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/pcmType

diagram |
type | axlapi:XEncode
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/csuParam

diagram |
type | axlapi:XCSUParam
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/firstDelay

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 32
nillable | false
source | <xsd:element name="firstDelay" type="axlapi:XInteger" default="32" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/interfaceIdPresent

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="interfaceIdPresent" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/interfaceId

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="interfaceId" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/intraDelay

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 4
nillable | false
source | <xsd:element name="intraDelay" type="axlapi:XInteger" default="4" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/mcdnEnable

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="mcdnEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/redirectOutboundNumberIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="redirectOutboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/numDigitsToStrip

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="numDigitsToStrip" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/passingPrecedenceLevelThrough

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="passingPrecedenceLevelThrough" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/prefix

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="prefix" type="xsd:string" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/callingLinePresentationBit

diagram |
type | axlapi:XPresentationBit
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="callingLinePresentationBit" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/connectedLineIdPresentation

diagram |
type | axlapi:XPresentationBit
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="connectedLineIdPresentation" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/priProtocol

diagram |
type | axlapi:XPriProtocol
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="priProtocol" type="axlapi:XPriProtocol" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/securityAccessLevel

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 2
nillable | false
source | <xsd:element name="securityAccessLevel" type="axlapi:XInteger" default="2" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/sendCallingNameInFacilityIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendCallingNameInFacilityIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/sendExLeadingCharInDispIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendExLeadingCharInDispIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/sendRestart

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendRestart" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/setupNonIsdnPi

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="setupNonIsdnPi" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/sigDigits

diagram |
type | extension of axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
enable | xsd:boolean | optional |  |  |
annotation |
documentation
The value for sigDigits must be between 0 to 32. enable attribute is read only
source | <xsd:element name="sigDigits" nillable="false" minOccurs="0"> <xsd:annotation> <xsd:documentation>The value for sigDigits must be between 0 to 32. enable attribute is read only</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute UpdateCiscoCatalyst6000E1VoIPGatewayReq/sigDigits/@enable

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="enable" type="xsd:boolean" use="optional"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/span

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="span" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/statusPoll

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="statusPoll" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/smdiBasePort

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/packetCaptureMode

diagram |
type | axlapi:XPacketCaptureMode
properties |
minOcc | 0
maxOcc | 1
content | simple
default | None
nillable | false
source | <xsd:element name="packetCaptureMode" type="axlapi:XPacketCaptureMode" default="None" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/packetCaptureDuration

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | true
source | <xsd:element name="packetCaptureDuration" type="axlapi:XInteger" default="0" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/transmitUtf8

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="transmitUtf8" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/v150

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="v150" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/asn1RoseOidEncoding

diagram |
type | axlapi:XASN1RoseOidEncoding
properties |
minOcc | 0
maxOcc | 1
content | simple
default | No Changes
nillable | false
annotation |
documentation
Applicable for only if PRI variant is QSIG
source | <xsd:element name="asn1RoseOidEncoding" type="axlapi:XASN1RoseOidEncoding" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only if PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/QSIGVariant

diagram |
type | axlapi:XQSIGVariant
properties |
minOcc | 0
maxOcc | 1
content | simple
default | No Changes
nillable | false
annotation |
documentation
Applicable for only PRI variant is QSIG
source | <xsd:element name="QSIGVariant" type="axlapi:XQSIGVariant" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/unattendedPort

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="unattendedPort" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/cdpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCdpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/nationalPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="nationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/internationalPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="internationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/unknownPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="unknownPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/subscriberPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="subscriberPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/geoLocationFilterName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/nationalStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="nationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/internationalStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="internationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/unknownStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="unknownStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/subscriberStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="subscriberStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/nationalTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="nationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/internationalTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="internationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/unknownTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="unknownTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/subscriberTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="subscriberTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCgpnTransformCssNatl

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssNatl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCgpnTransformCssIntl

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssIntl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCgpnTransformCssUnkn

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssUnkn" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/useDevicePoolCgpnTransformCssSubs

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssSubs" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/pstnAccess

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000E1VoIPGatewayReq/imeE164TransformationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy