complexType AddCiscoCatalyst6000T1VoIPGatewayT1Req

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:APIRequest
properties |
base | axlapi:APIRequest
children | ciscoCatalyst6000T1VoIPGatewayT1
used by |
element | addCiscoCatalyst6000T1VoIPGatewayT1
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="AddCiscoCatalyst6000T1VoIPGatewayT1Req"> <xsd:complexContent> <xsd:extension base="axlapi:APIRequest"> <xsd:sequence> <xsd:element name="ciscoCatalyst6000T1VoIPGatewayT1" type="axlapi:XCiscoCatalyst6000T1VoIPGatewayT1"/> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element AddCiscoCatalyst6000T1VoIPGatewayT1Req/ciscoCatalyst6000T1VoIPGatewayT1

diagram |
type | axlapi:XCiscoCatalyst6000T1VoIPGatewayT1
properties |
content | complex
children | name description product class protocol protocolSide callingSearchSpaceName devicePoolName commonDeviceConfigName networkLocation locationName mediaResourceListName automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig traceFlag mlppDomainId mlppIndicationStatus preemption useTrustedRelayPoint retryVideoCallAsAudio cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName sendGeoLocation ports trunkSelectionOrder clockReference csuParam digitSending pcmType fdlChannel yellowAlarm zeroSupression smdiBasePort handleDtmfPrecedenceSignals cdpnTransformationCssName useDevicePoolCdpnTransformCss geoLocationFilterName pstnAccess imeE164TransformationName
source | <xsd:element name="ciscoCatalyst6000T1VoIPGatewayT1" type="axlapi:XCiscoCatalyst6000T1VoIPGatewayT1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy