complexType UpdateCiscoCatalyst6000T1VoIPGatewayPriReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:NameAndGUIDRequest
properties |
base | axlapi:NameAndGUIDRequest
children | name uuid newName description callingSearchSpaceName devicePoolName commonDeviceConfigName networkLocation locationName networkLocale mediaResourceListName automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig mlppDomainId mlppIndicationStatus mlppPreemption useTrustedRelayPoint cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName redirectInboundNumberIe calledPlan calledPri callerIdDn callingPartySelection callingPlan callingPri chanIe clockReference dChannelEnable channelSelectionOrder displayIE pcmType csuParam firstDelay interfaceIdPresent interfaceId intraDelay mcdnEnable redirectOutboundNumberIe numDigitsToStrip passingPrecedenceLevelThrough prefix callingLinePresentationBit connectedLineIdPresentation priProtocol securityAccessLevel sendCallingNameInFacilityIe sendExLeadingCharInDispIe sendRestart setupNonIsdnPi sigDigits span statusPoll smdiBasePort packetCaptureMode packetCaptureDuration transmitUtf8 v150 asn1RoseOidEncoding QSIGVariant unattendedPort cdpnTransformationCssName useDevicePoolCdpnTransformCss nationalPrefix internationalPrefix unknownPrefix subscriberPrefix geoLocationFilterName nationalStripDigits internationalStripDigits unknownStripDigits subscriberStripDigits nationalTransformationCssName internationalTransformationCssName unknownTransformationCssName subscriberTransformationCssName useDevicePoolCgpnTransformCssNatl useDevicePoolCgpnTransformCssIntl useDevicePoolCgpnTransformCssUnkn useDevicePoolCgpnTransformCssSubs pstnAccess imeE164TransformationName
used by |
element | updateCiscoCatalyst6000T1VoIPGatewayPri
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="UpdateCiscoCatalyst6000T1VoIPGatewayPriReq"> <xsd:complexContent> <xsd:extension base="axlapi:NameAndGUIDRequest"> <xsd:sequence> <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="networkLocale" type="axlapi:XCountry" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/> <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Off" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mlppPreemption" type="axlapi:XPreemption" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="redirectInboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="calledPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="calledPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callerIdDn" type="axlapi:String255" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" default="Originator" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="chanIe" type="axlapi:XPRIChanIE" default="Use Number when 1B" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="dChannelEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="channelSelectionOrder" type="axlapi:XTrunkSelectionOrder" default="Top Down" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="displayIE" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="firstDelay" type="axlapi:XInteger" default="32" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="interfaceIdPresent" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="interfaceId" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="intraDelay" type="axlapi:XInteger" default="4" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="mcdnEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="redirectOutboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="numDigitsToStrip" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="passingPrecedenceLevelThrough" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="prefix" type="xsd:string" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingLinePresentationBit" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="connectedLineIdPresentation" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="priProtocol" type="axlapi:XPriProtocol" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="securityAccessLevel" type="axlapi:XInteger" default="2" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendCallingNameInFacilityIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendExLeadingCharInDispIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendRestart" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="setupNonIsdnPi" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="sigDigits" nillable="false" minOccurs="0"> <xsd:annotation> <xsd:documentation>The value for sigDigits must be between 0 to 32. enable attribute is read only</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element> <xsd:element name="span" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="statusPoll" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="packetCaptureMode" type="axlapi:XPacketCaptureMode" default="None" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="packetCaptureDuration" type="axlapi:XInteger" default="0" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="transmitUtf8" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="v150" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="asn1RoseOidEncoding" type="axlapi:XASN1RoseOidEncoding" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only if PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="QSIGVariant" type="axlapi:XQSIGVariant" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="unattendedPort" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="nationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="internationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="unknownTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="subscriberTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssNatl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssIntl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssUnkn" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCssSubs" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/newName

diagram |
type | axlapi:UniqueString128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
The device name,using only URL-friendly characters
source | <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/description

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
Optional description of the device
source | <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callingSearchSpaceName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/devicePoolName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/commonDeviceConfigName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/networkLocation

diagram |
type | axlapi:XNetworkLocation
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use System Default
nillable | false
annotation |
documentation
The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.
source | <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/locationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/networkLocale

diagram |
type | axlapi:XCountry
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="networkLocale" type="axlapi:XCountry" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/mediaResourceListName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/automatedAlternateRoutingCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/aarNeighborhoodName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/loadInformation

diagram |
type | axlapi:XLoadInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
special | axlapi:boolean |  |  |  |
annotation |
documentation
For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.
source | <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/vendorConfig

diagram |
type | axlapi:XVendorConfig
properties |
minOcc | 0
maxOcc | 1
content | complex
source | <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/mlppDomainId

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
This setting only effects devices that support MLPP. Use -1 to set to null
source | <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/mlppIndicationStatus

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Off
nillable | false
annotation |
documentation
This setting only affects devices that support MLPP.
source | <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Off" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/mlppPreemption

diagram |
type | axlapi:XPreemption
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
annotation |
documentation
This setting only affects devices that support MLPP.
source | <xsd:element name="mlppPreemption" type="axlapi:XPreemption" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useTrustedRelayPoint

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/cgpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCgpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/geoLocationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/redirectInboundNumberIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="redirectInboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/calledPlan

diagram |
type | axlapi:XNumberingPlan
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="calledPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/calledPri

diagram |
type | axlapi:XPriOfNumber
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="calledPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callerIdDn

diagram |
type | axlapi:String255
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 255 |
source | <xsd:element name="callerIdDn" type="axlapi:String255" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callingPartySelection

diagram |
type | axlapi:XCallingPartySelection
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Originator
nillable | false
source | <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" default="Originator" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callingPlan

diagram |
type | axlapi:XNumberingPlan
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="callingPlan" type="axlapi:XNumberingPlan" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callingPri

diagram |
type | axlapi:XPriOfNumber
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Cisco CallManager
nillable | false
source | <xsd:element name="callingPri" type="axlapi:XPriOfNumber" default="Cisco CallManager" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/chanIe

diagram |
type | axlapi:XPRIChanIE
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use Number when 1B
nillable | false
source | <xsd:element name="chanIe" type="axlapi:XPRIChanIE" default="Use Number when 1B" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/clockReference

diagram |
type | axlapi:XClockReference
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/dChannelEnable

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="dChannelEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/channelSelectionOrder

diagram |
type | axlapi:XTrunkSelectionOrder
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Top Down
nillable | false
source | <xsd:element name="channelSelectionOrder" type="axlapi:XTrunkSelectionOrder" default="Top Down" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/displayIE

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="displayIE" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/pcmType

diagram |
type | axlapi:XEncode
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/csuParam

diagram |
type | axlapi:XCSUParam
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/firstDelay

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 32
nillable | false
source | <xsd:element name="firstDelay" type="axlapi:XInteger" default="32" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/interfaceIdPresent

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="interfaceIdPresent" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/interfaceId

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="interfaceId" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/intraDelay

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 4
nillable | false
source | <xsd:element name="intraDelay" type="axlapi:XInteger" default="4" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/mcdnEnable

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="mcdnEnable" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/redirectOutboundNumberIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="redirectOutboundNumberIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/numDigitsToStrip

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="numDigitsToStrip" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/passingPrecedenceLevelThrough

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="passingPrecedenceLevelThrough" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/prefix

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="prefix" type="xsd:string" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/callingLinePresentationBit

diagram |
type | axlapi:XPresentationBit
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="callingLinePresentationBit" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/connectedLineIdPresentation

diagram |
type | axlapi:XPresentationBit
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="connectedLineIdPresentation" type="axlapi:XPresentationBit" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/priProtocol

diagram |
type | axlapi:XPriProtocol
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="priProtocol" type="axlapi:XPriProtocol" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/securityAccessLevel

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 2
nillable | false
source | <xsd:element name="securityAccessLevel" type="axlapi:XInteger" default="2" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/sendCallingNameInFacilityIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendCallingNameInFacilityIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/sendExLeadingCharInDispIe

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendExLeadingCharInDispIe" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/sendRestart

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="sendRestart" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/setupNonIsdnPi

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="setupNonIsdnPi" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/sigDigits

diagram |
type | extension of axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
enable | xsd:boolean | optional |  |  |
annotation |
documentation
The value for sigDigits must be between 0 to 32. enable attribute is read only
source | <xsd:element name="sigDigits" nillable="false" minOccurs="0"> <xsd:annotation> <xsd:documentation>The value for sigDigits must be between 0 to 32. enable attribute is read only</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/sigDigits/@enable

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="enable" type="xsd:boolean" use="optional"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/span

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="span" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/statusPoll

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="statusPoll" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/smdiBasePort

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/packetCaptureMode

diagram |
type | axlapi:XPacketCaptureMode
properties |
minOcc | 0
maxOcc | 1
content | simple
default | None
nillable | false
source | <xsd:element name="packetCaptureMode" type="axlapi:XPacketCaptureMode" default="None" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/packetCaptureDuration

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | true
source | <xsd:element name="packetCaptureDuration" type="axlapi:XInteger" default="0" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/transmitUtf8

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="transmitUtf8" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/v150

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="v150" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/asn1RoseOidEncoding

diagram |
type | axlapi:XASN1RoseOidEncoding
properties |
minOcc | 0
maxOcc | 1
content | simple
default | No Changes
nillable | false
annotation |
documentation
Applicable for only if PRI variant is QSIG
source | <xsd:element name="asn1RoseOidEncoding" type="axlapi:XASN1RoseOidEncoding" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only if PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/QSIGVariant

diagram |
type | axlapi:XQSIGVariant
properties |
minOcc | 0
maxOcc | 1
content | simple
default | No Changes
nillable | false
annotation |
documentation
Applicable for only PRI variant is QSIG
source | <xsd:element name="QSIGVariant" type="axlapi:XQSIGVariant" default="No Changes" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Applicable for only PRI variant is QSIG</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/unattendedPort

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="unattendedPort" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/cdpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCdpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/nationalPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="nationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/internationalPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="internationalPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/unknownPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="unknownPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/subscriberPrefix

diagram |
type | axlapi:String16
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 16 |
source | <xsd:element name="subscriberPrefix" type="axlapi:String16" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/geoLocationFilterName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/nationalStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="nationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/internationalStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="internationalStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/unknownStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="unknownStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/subscriberStripDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
source | <xsd:element name="subscriberStripDigits" type="axlapi:XInteger" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/nationalTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="nationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/internationalTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="internationalTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/unknownTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="unknownTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/subscriberTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="subscriberTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCgpnTransformCssNatl

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssNatl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCgpnTransformCssIntl

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssIntl" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCgpnTransformCssUnkn

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssUnkn" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/useDevicePoolCgpnTransformCssSubs

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCssSubs" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/pstnAccess

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayPriReq/imeE164TransformationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy