complexType UpdateConferenceBridgeReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:NameAndGUIDRequest
properties |
base | axlapi:NameAndGUIDRequest
children | name uuid newName description product devicePoolName commonDeviceConfigName locationName loadInformation vendorConfig maximumCapacity useTrustedRelayPoint securityProfileName destinationAddress mcuConferenceBridgeSipPort sipProfile srtpAllowed normalizationScript enableTrace normalizationScriptInfos userName password httpPort useHttps
used by |
element | updateConferenceBridge
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="UpdateConferenceBridgeReq"> <xsd:complexContent> <xsd:extension base="axlapi:NameAndGUIDRequest"> <xsd:sequence> <xsd:element name="newName" type="axlapi:UniqueName128" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="product" type="axlapi:XProduct" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="locationName" type="axlapi:XFkType" default="Hub_None" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is used only by Cisco Conference Bridge Hardware.For devices with load information, if any special load information is specified, the special attribute is set to TRUE. Otherwise, the load information is the default for the product.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is used only by Cisco Video Conference Bridge(IPVC-35xx),Cisco Conference Bridge (WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS).</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="maximumCapacity" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is mandatory for Cisco Conference Bridge(WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS). Valid values for this tag are 32,64,96,128.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="securityProfileName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco IOS Enhanced Conference Bridge</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="destinationAddress" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mcuConferenceBridgeSipPort" type="axlapi:XInteger" default="5060" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="sipProfile" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="srtpAllowed" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="normalizationScript" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="enableTrace" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="normalizationScriptInfos" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Adding parameters for normalization script Info</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence minOccurs="0"> <xsd:element name="normalizationScriptInfo" type="axlapi:XNormalizationScriptInfo" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element> <xsd:element name="userName" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU and max length is 31</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="password" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU and max length is 31</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="httpPort" type="axlapi:XInteger" default="80" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useHttps" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element UpdateConferenceBridgeReq/newName

diagram |
type | axlapi:UniqueName128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
source | <xsd:element name="newName" type="axlapi:UniqueName128" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/description

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
source | <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/product

diagram |
type | axlapi:XProduct
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="product" type="axlapi:XProduct" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/devicePoolName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/commonDeviceConfigName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/locationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
default | Hub_None
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="locationName" type="axlapi:XFkType" default="Hub_None" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/loadInformation

diagram |
type | axlapi:XLoadInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
special | axlapi:boolean |  |  |  |
annotation |
documentation
This tag is used only by Cisco Conference Bridge Hardware.For devices with load information, if any special load information is specified, the special attribute is set to TRUE. Otherwise, the load information is the default for the product.
source | <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is used only by Cisco Conference Bridge Hardware.For devices with load information, if any special load information is specified, the special attribute is set to TRUE. Otherwise, the load information is the default for the product.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/vendorConfig

diagram |
type | axlapi:XVendorConfig
properties |
minOcc | 0
maxOcc | 1
content | complex
annotation |
documentation
This tag is used only by Cisco Video Conference Bridge(IPVC-35xx),Cisco Conference Bridge (WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS).
source | <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is used only by Cisco Video Conference Bridge(IPVC-35xx),Cisco Conference Bridge (WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS).</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/maximumCapacity

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
annotation |
documentation
This tag is mandatory for Cisco Conference Bridge(WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS). Valid values for this tag are 32,64,96,128.
source | <xsd:element name="maximumCapacity" type="axlapi:XInteger" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This tag is mandatory for Cisco Conference Bridge(WS-SVC-CMM) and Cisco Media Server(WS-SVC-CMM-MS). Valid values for this tag are 32,64,96,128.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/useTrustedRelayPoint

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateConferenceBridgeReq/securityProfileName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
annotation |
documentation
Valid only for Cisco IOS Enhanced Conference Bridge
source | <xsd:element name="securityProfileName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco IOS Enhanced Conference Bridge</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/destinationAddress

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="destinationAddress" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/mcuConferenceBridgeSipPort

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 5060
nillable | false
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="mcuConferenceBridgeSipPort" type="axlapi:XInteger" default="5060" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/sipProfile

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="sipProfile" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/srtpAllowed

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="srtpAllowed" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/normalizationScript

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="normalizationScript" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/enableTrace

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="enableTrace" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/normalizationScriptInfos

diagram |
properties |
minOcc | 0
maxOcc | 1
content | complex
children | normalizationScriptInfo
annotation |
documentation
Adding parameters for normalization script Info
source | <xsd:element name="normalizationScriptInfos" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Adding parameters for normalization script Info</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence minOccurs="0"> <xsd:element name="normalizationScriptInfo" type="axlapi:XNormalizationScriptInfo" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element UpdateConferenceBridgeReq/normalizationScriptInfos/normalizationScriptInfo

diagram |
type | axlapi:XNormalizationScriptInfo
properties |
minOcc | 0
maxOcc | unbounded
content | complex
children | parameterName parameterValue
source | <xsd:element name="normalizationScriptInfo" type="axlapi:XNormalizationScriptInfo" minOccurs="0" maxOccurs="unbounded"/>

element UpdateConferenceBridgeReq/userName

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
annotation |
documentation
Valid only for Cisco TelePresence MCU and max length is 31
source | <xsd:element name="userName" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU and max length is 31</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/password

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
annotation |
documentation
Valid only for Cisco TelePresence MCU and max length is 31
source | <xsd:element name="password" type="xsd:string" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU and max length is 31</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/httpPort

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 80
nillable | false
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="httpPort" type="axlapi:XInteger" default="80" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateConferenceBridgeReq/useHttps

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
Valid only for Cisco TelePresence MCU
source | <xsd:element name="useHttps" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Valid only for Cisco TelePresence MCU</xsd:documentation> </xsd:annotation> </xsd:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy