complexType UAnalogPort

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
children | portNumber attendantDn unattendedPort callerIdDn callerIdEnable callingPartySelection digitSending expectedDigits sigDigits lines prefixDn presentationBit silenceSuppressionThreshold smdiPortNumber startDialProtocol trunk trunkDirection trunkLevel trunkPadRx trunkPadTx vendorConfig timer1 timer2 timer3 timer4 timer5 timer6
used by |
element | UGatewayEndpointAnalog/port
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID |  |  |  |
source | <xsd:complexType name="UAnalogPort"> <xsd:sequence minOccurs="0"> <xsd:element name="portNumber" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="attendantDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/> <xsd:element name="unattendedPort" type="axlapi:boolean" minOccurs="0" maxOccurs="1"/> <xsd:element name="callerIdDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/> <xsd:element name="callerIdEnable" type="axlapi:boolean" minOccurs="0" maxOccurs="1"/> <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" minOccurs="0" maxOccurs="1"/> <xsd:element name="digitSending" type="axlapi:XDigitSending" minOccurs="0" maxOccurs="1"/> <xsd:element name="expectedDigits" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="sigDigits" minOccurs="0"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element> <xsd:element name="lines" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:complexType> <xsd:choice minOccurs="0"> <xsd:element name="line" type="axlapi:UPhoneLine" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>An XLine is an entry in the DeviceNumPlanMap table. The actual directory number is referenced inside the XLine object by the "dirn" or "dirnId" element. Not applicable to FXO ports</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="lineIdentifier" type="axlapi:UNumplanIdentifier" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The lineIdentifier is a shorthand method that refers to a particular directory number.</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> </xsd:complexType> </xsd:element> <xsd:element name="prefixDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/> <xsd:element name="presentationBit" type="axlapi:XPresentationBit" minOccurs="0" maxOccurs="1"/> <xsd:element name="silenceSuppressionThreshold" type="axlapi:XSilenceSuppressionThreshold" minOccurs="0" maxOccurs="1"/> <xsd:element name="smdiPortNumber" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="startDialProtocol" type="axlapi:XStartDialProtocol" minOccurs="0" maxOccurs="1"/> <xsd:element name="trunk" type="axlapi:XTrunk" minOccurs="0" maxOccurs="1"/> <xsd:element name="trunkDirection" type="axlapi:XTrunkDirection" minOccurs="0" maxOccurs="1"/> <xsd:element name="trunkLevel" type="axlapi:XTrunkLevel" minOccurs="0" maxOccurs="1"/> <xsd:element name="trunkPadRx" type="axlapi:XTrunkPad" minOccurs="0" maxOccurs="1"/> <xsd:element name="trunkPadTx" type="axlapi:XTrunkPad" minOccurs="0" maxOccurs="1"/> <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer1" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer2" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer3" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer4" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer5" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> <xsd:element name="timer6" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/> </xsd:sequence> <xsd:attribute name="uuid" type="axlapi:XUUID"/> </xsd:complexType>

attribute UAnalogPort/@uuid

type | axlapi:XUUID
facets |
Kind | Value | Annotation
pattern | \{........-....-....-....-............\} |
source | <xsd:attribute name="uuid" type="axlapi:XUUID"/>

element UAnalogPort/portNumber

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="portNumber" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/attendantDn

diagram |
type | axlapi:String255
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 255 |
source | <xsd:element name="attendantDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/unattendedPort

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="unattendedPort" type="axlapi:boolean" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/callerIdDn

diagram |
type | axlapi:String255
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 255 |
source | <xsd:element name="callerIdDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/callerIdEnable

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="callerIdEnable" type="axlapi:boolean" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/callingPartySelection

diagram |
type | axlapi:XCallingPartySelection
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="callingPartySelection" type="axlapi:XCallingPartySelection" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/digitSending

diagram |
type | axlapi:XDigitSending
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="digitSending" type="axlapi:XDigitSending" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/expectedDigits

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="expectedDigits" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/sigDigits

diagram |
type | extension of axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
enable | xsd:boolean | optional |  |  |
source | <xsd:element name="sigDigits" minOccurs="0"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="axlapi:XInteger"> <xsd:attribute name="enable" type="xsd:boolean" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute UAnalogPort/sigDigits/@enable

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="enable" type="xsd:boolean" use="optional"/>

element UAnalogPort/lines

diagram |
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
children | line lineIdentifier
source | <xsd:element name="lines" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:complexType> <xsd:choice minOccurs="0"> <xsd:element name="line" type="axlapi:UPhoneLine" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>An XLine is an entry in the DeviceNumPlanMap table. The actual directory number is referenced inside the XLine object by the "dirn" or "dirnId" element. Not applicable to FXO ports</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="lineIdentifier" type="axlapi:UNumplanIdentifier" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The lineIdentifier is a shorthand method that refers to a particular directory number.</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> </xsd:complexType> </xsd:element>

element UAnalogPort/lines/line

diagram |
type | axlapi:UPhoneLine
properties |
minOcc | 0
maxOcc | 1
content | complex
children | index label asciiLabel display dirn ringSetting consecutiveRingSetting ringSettingIdlePickupAlert ringSettingActivePickupAlert displayAscii e164Mask dialPlanWizardId mwlPolicy maxNumCalls busyTrigger callInfoDisplay recordingProfileName monitoringCssName recordingFlag audibleMwi speedDial associatedEndusers missedCallLogging
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID |  |  |  |
ctiid | xsd:nonNegativeInteger |  |  |  |
annotation |
documentation
An XLine is an entry in the DeviceNumPlanMap table. The actual directory number is referenced inside the XLine object by the "dirn" or "dirnId" element. Not applicable to FXO ports
source | <xsd:element name="line" type="axlapi:UPhoneLine" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>An XLine is an entry in the DeviceNumPlanMap table. The actual directory number is referenced inside the XLine object by the "dirn" or "dirnId" element. Not applicable to FXO ports</xsd:documentation> </xsd:annotation> </xsd:element>

element UAnalogPort/lines/lineIdentifier

diagram |
type | axlapi:UNumplanIdentifier
properties |
minOcc | 0
maxOcc | 1
content | complex
children | directoryNumber routePartitionName
annotation |
documentation
The lineIdentifier is a shorthand method that refers to a particular directory number.
source | <xsd:element name="lineIdentifier" type="axlapi:UNumplanIdentifier" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The lineIdentifier is a shorthand method that refers to a particular directory number.</xsd:documentation> </xsd:annotation> </xsd:element>

element UAnalogPort/prefixDn

diagram |
type | axlapi:String255
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 255 |
source | <xsd:element name="prefixDn" type="axlapi:String255" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/presentationBit

diagram |
type | axlapi:XPresentationBit
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="presentationBit" type="axlapi:XPresentationBit" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/silenceSuppressionThreshold

diagram |
type | axlapi:XSilenceSuppressionThreshold
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="silenceSuppressionThreshold" type="axlapi:XSilenceSuppressionThreshold" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/smdiPortNumber

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="smdiPortNumber" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/startDialProtocol

diagram |
type | axlapi:XStartDialProtocol
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="startDialProtocol" type="axlapi:XStartDialProtocol" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/trunk

diagram |
type | axlapi:XTrunk
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="trunk" type="axlapi:XTrunk" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/trunkDirection

diagram |
type | axlapi:XTrunkDirection
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="trunkDirection" type="axlapi:XTrunkDirection" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/trunkLevel

diagram |
type | axlapi:XTrunkLevel
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="trunkLevel" type="axlapi:XTrunkLevel" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/trunkPadRx

diagram |
type | axlapi:XTrunkPad
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="trunkPadRx" type="axlapi:XTrunkPad" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/trunkPadTx

diagram |
type | axlapi:XTrunkPad
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="trunkPadTx" type="axlapi:XTrunkPad" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/vendorConfig

diagram |
type | axlapi:XVendorConfig
properties |
minOcc | 0
maxOcc | 1
content | complex
source | <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer1

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer1" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer2

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer2" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer3

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer3" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer4

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer4" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer5

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer5" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

element UAnalogPort/timer6

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
source | <xsd:element name="timer6" type="axlapi:XInteger" minOccurs="0" maxOccurs="1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy