complexType GetPhoneReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
children | name uuid returnedTags
used by |
element | getPhone
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="GetPhoneReq"> <xsd:sequence> <xsd:choice> <xsd:element name="name" type="axlapi:String100"/> <xsd:element name="uuid" type="axlapi:XUUID"/> </xsd:choice> <xsd:element name="returnedTags" type="axlapi:RPhone" minOccurs="0"/> </xsd:sequence> <xsd:attribute name="sequence" type="xsd:unsignedLong" use="optional"/> </xsd:complexType>

attribute GetPhoneReq/@sequence

type | xsd:unsignedLong
properties |
use | optional
source | <xsd:attribute name="sequence" type="xsd:unsignedLong" use="optional"/>

element GetPhoneReq/name

diagram |
type | axlapi:String100
properties |
content | simple
facets |
Kind | Value | Annotation
maxLength | 100 |
source | <xsd:element name="name" type="axlapi:String100"/>

element GetPhoneReq/uuid

diagram |
type | axlapi:XUUID
properties |
content | simple
facets |
Kind | Value | Annotation
pattern | \{........-....-....-....-............\} |
source | <xsd:element name="uuid" type="axlapi:XUUID"/>

element GetPhoneReq/returnedTags

diagram |
type | axlapi:RPhone
properties |
minOcc | 0
maxOcc | 1
content | complex
children | name description product model class protocol protocolSide callingSearchSpaceName devicePoolName commonDeviceConfigName commonPhoneConfigName networkLocation locationName mediaResourceListName networkHoldMohAudioSourceId userHoldMohAudioSourceId automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig versionStamp traceFlag mlppDomainId mlppIndicationStatus preemption useTrustedRelayPoint retryVideoCallAsAudio securityProfileName sipProfileName cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName geoLocationFilterName sendGeoLocation lines numberOfButtons phoneTemplateName speeddials busyLampFields primaryPhoneName ringSettingIdleBlfAudibleAlert ringSettingBusyBlfAudibleAlert blfDirectedCallParks addOnModules userlocale networkLocale idleTimeout authenticationUrl directoryUrl idleUrl informationUrl messagesUrl proxyServerUrl servicesUrl services softkeyTemplateName loginUserId defaultProfileName enableExtensionMobility currentProfileName loginTime loginDuration currentConfig singleButtonBarge joinAcrossLines builtInBridgeStatus callInfoPrivacyStatus hlogStatus ownerUserName ignorePresentationIndicators packetCaptureMode packetCaptureDuration subscribeCallingSearchSpaceName rerouteCallingSearchSpaceName allowCtiControlFlag presenceGroupName unattendedPort requireDtmfReception rfc2833Disabled certificateOperation authenticationMode keySize authenticationString certificateStatus upgradeFinishTime deviceMobilityMode roamingDevicePoolName remoteDevice dndOption dndRingSetting dndStatus isActive isDualMode mobilityUserIdName phoneSuite phoneServiceDisplay isProtected mobileSmartClientProfileName mtpRequired mtpPreferedCodec dialRulesName sshUserId sshPwd digestUser outboundCallRollover hotlineDevice secureInformationUrl secureDirectoryUrl secureMessageUrl secureServicesUrl secureAuthenticationUrl secureIdleUrl alwaysUsePrimeLine alwaysUsePrimeLineForVoiceMessage featureControlPolicy deviceTrustMode earlyOfferSupportForVoiceCall requireThirdPartyRegistration blockIncomingCallsWhenRoaming homeNetworkId AllowPresentationSharingUsingBfcp requireOffPremiseLocation
attributes |
Name | Type | Use | Default | Fixed | Annotation
ctiid | xsd:positiveInteger |  |  |  |
uuid | axlapi:XUUID |  |  |  |
source | <xsd:element name="returnedTags" type="axlapi:RPhone" minOccurs="0"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy