complexType ListCiscoCatalyst6000T1VoIPGatewayPriRes

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:APIResponse
properties |
base | axlapi:APIResponse
children | return
used by |
element | listCiscoCatalyst6000T1VoIPGatewayPriResponse
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="ListCiscoCatalyst6000T1VoIPGatewayPriRes"> <xsd:complexContent> <xsd:extension base="axlapi:APIResponse"> <xsd:sequence> <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="ciscoCatalyst6000T1VoIPGatewayPri" type="axlapi:LCiscoCatalyst6000T1VoIPGatewayPri" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element ListCiscoCatalyst6000T1VoIPGatewayPriRes/return

diagram |
properties |
content | complex
children | ciscoCatalyst6000T1VoIPGatewayPri
source | <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="ciscoCatalyst6000T1VoIPGatewayPri" type="axlapi:LCiscoCatalyst6000T1VoIPGatewayPri" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ListCiscoCatalyst6000T1VoIPGatewayPriRes/return/ciscoCatalyst6000T1VoIPGatewayPri

diagram |
type | axlapi:LCiscoCatalyst6000T1VoIPGatewayPri
properties |
minOcc | 0
maxOcc | unbounded
content | complex
children | name description product model class protocol protocolSide callingSearchSpaceName devicePoolName commonDeviceConfigName networkLocation locationName networkLocale mediaResourceListName automatedAlternateRoutingCssName aarNeighborhoodName loadInformation mlppIndicationStatus mlppPreemption useTrustedRelayPoint cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName redirectInboundNumberIe calledPlan calledPri callerIdDn callingPartySelection callingPlan callingPri chanIe clockReference dChannelEnable channelSelectionOrder displayIE pcmType csuParam firstDelay interfaceIdPresent interfaceId intraDelay mcdnEnable redirectOutboundNumberIe numDigitsToStrip passingPrecedenceLevelThrough prefix callingLinePresentationBit connectedLineIdPresentation priProtocol securityAccessLevel sendCallingNameInFacilityIe sendExLeadingCharInDispIe sendRestart setupNonIsdnPi sigDigits span statusPoll smdiBasePort packetCaptureMode packetCaptureDuration transmitUtf8 v150 asn1RoseOidEncoding QSIGVariant unattendedPort cdpnTransformationCssName useDevicePoolCdpnTransformCss nationalPrefix internationalPrefix unknownPrefix subscriberPrefix geoLocationFilterName nationalStripDigits internationalStripDigits unknownStripDigits subscriberStripDigits nationalTransformationCssName internationalTransformationCssName unknownTransformationCssName subscriberTransformationCssName useDevicePoolCgpnTransformCssNatl useDevicePoolCgpnTransformCssIntl useDevicePoolCgpnTransformCssUnkn useDevicePoolCgpnTransformCssSubs pstnAccess imeE164TransformationName
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID |  |  |  |
source | <xsd:element name="ciscoCatalyst6000T1VoIPGatewayPri" type="axlapi:LCiscoCatalyst6000T1VoIPGatewayPri" minOccurs="0" maxOccurs="unbounded"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy