complexType ListPhoneRes

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:APIResponse
properties |
base | axlapi:APIResponse
children | return
used by |
element | listPhoneResponse
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="ListPhoneRes"> <xsd:complexContent> <xsd:extension base="axlapi:APIResponse"> <xsd:sequence> <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="phone" type="axlapi:LPhone" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element ListPhoneRes/return

diagram |
properties |
content | complex
children | phone
source | <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="phone" type="axlapi:LPhone" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ListPhoneRes/return/phone

diagram |
type | axlapi:LPhone
properties |
minOcc | 0
maxOcc | unbounded
content | complex
children | name description product model class protocol protocolSide callingSearchSpaceName devicePoolName commonDeviceConfigName commonPhoneConfigName networkLocation locationName mediaResourceListName networkHoldMohAudioSourceId userHoldMohAudioSourceId automatedAlternateRoutingCssName aarNeighborhoodName loadInformation traceFlag mlppIndicationStatus preemption useTrustedRelayPoint retryVideoCallAsAudio securityProfileName sipProfileName cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName geoLocationFilterName sendGeoLocation numberOfButtons phoneTemplateName primaryPhoneName ringSettingIdleBlfAudibleAlert ringSettingBusyBlfAudibleAlert userlocale networkLocale idleTimeout authenticationUrl directoryUrl idleUrl informationUrl messagesUrl proxyServerUrl servicesUrl softkeyTemplateName loginUserId defaultProfileName enableExtensionMobility currentProfileName loginTime loginDuration currentConfig singleButtonBarge joinAcrossLines builtInBridgeStatus callInfoPrivacyStatus hlogStatus ownerUserName ignorePresentationIndicators packetCaptureMode packetCaptureDuration subscribeCallingSearchSpaceName rerouteCallingSearchSpaceName allowCtiControlFlag presenceGroupName unattendedPort requireDtmfReception rfc2833Disabled certificateOperation authenticationMode keySize authenticationString certificateStatus upgradeFinishTime deviceMobilityMode roamingDevicePoolName remoteDevice dndOption dndRingSetting dndStatus isActive isDualMode mobilityUserIdName phoneSuite phoneServiceDisplay isProtected mobileSmartClientProfileName mtpRequired mtpPreferedCodec dialRulesName sshUserId digestUser outboundCallRollover hotlineDevice secureInformationUrl secureDirectoryUrl secureMessageUrl secureServicesUrl secureAuthenticationUrl secureIdleUrl alwaysUsePrimeLine alwaysUsePrimeLineForVoiceMessage featureControlPolicy deviceTrustMode earlyOfferSupportForVoiceCall requireThirdPartyRegistration blockIncomingCallsWhenRoaming homeNetworkId AllowPresentationSharingUsingBfcp requireOffPremiseLocation
attributes |
Name | Type | Use | Default | Fixed | Annotation
ctiid | xsd:positiveInteger |  |  |  |
uuid | axlapi:XUUID |  |  |  |
source | <xsd:element name="phone" type="axlapi:LPhone" minOccurs="0" maxOccurs="unbounded"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy