complexType UpdateCiscoCatalyst6000T1VoIPGatewayT1Req

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:NameAndGUIDRequest
properties |
base | axlapi:NameAndGUIDRequest
children | name uuid newName description callingSearchSpaceName devicePoolName commonDeviceConfigName networkLocation locationName mediaResourceListName automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig traceFlag mlppDomainId mlppIndicationStatus useTrustedRelayPoint retryVideoCallAsAudio cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName sendGeoLocation ports trunkSelectionOrder clockReference csuParam digitSending pcmType fdlChannel yellowAlarm zeroSupression smdiBasePort handleDtmfPrecedenceSignals cdpnTransformationCssName useDevicePoolCdpnTransformCss geoLocationFilterName pstnAccess imeE164TransformationName
used by |
element | updateCiscoCatalyst6000T1VoIPGatewayT1
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="UpdateCiscoCatalyst6000T1VoIPGatewayT1Req"> <xsd:complexContent> <xsd:extension base="axlapi:NameAndGUIDRequest"> <xsd:sequence> <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/> <xsd:element name="traceFlag" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Off" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="retryVideoCallAsAudio" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="sendGeoLocation" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Not valid for CTI route points and VoiceMail ports</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="ports" minOccurs="0" maxOccurs="1"> <xsd:complexType> <xsd:sequence minOccurs="0"> <xsd:element name="port" type="axlapi:XT1Port" minOccurs="1" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element> <xsd:element name="trunkSelectionOrder" type="axlapi:XTrunkSelectionOrder" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="digitSending" type="axlapi:XDigitSending" default="DTMF" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="fdlChannel" type="axlapi:XFDLChannel" default="None" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="yellowAlarm" type="axlapi:XYellowAlarm" default="F-Bit" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="zeroSupression" type="axlapi:XZeroSuppression" default="B8ZS" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="handleDtmfPrecedenceSignals" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/newName

diagram |
type | axlapi:UniqueString128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
The device name,using only URL-friendly characters
source | <xsd:element name="newName" type="axlapi:UniqueString128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The device name,using only URL-friendly characters</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/description

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
Optional description of the device
source | <xsd:element name="description" type="axlapi:String128" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Optional description of the device</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/callingSearchSpaceName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="callingSearchSpaceName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/devicePoolName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="devicePoolName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/commonDeviceConfigName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="commonDeviceConfigName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/networkLocation

diagram |
type | axlapi:XNetworkLocation
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use System Default
nillable | false
annotation |
documentation
The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.
source | <xsd:element name="networkLocation" type="axlapi:XNetworkLocation" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>The new Device Destination for Trunk to Trunk Transfer and Drop Conference Feature is required for most gateways ,except FXS gateways and phones.Not Nullable.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/locationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="locationName" type="axlapi:XFkType" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/mediaResourceListName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="mediaResourceListName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/automatedAlternateRoutingCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="automatedAlternateRoutingCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/aarNeighborhoodName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="aarNeighborhoodName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/loadInformation

diagram |
type | axlapi:XLoadInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
special | axlapi:boolean |  |  |  |
annotation |
documentation
For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.
source | <xsd:element name="loadInformation" type="axlapi:XLoadInformation" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>For devices with load information, if any special load information is specified the special attribute is set to TRUE.Otherwise,the load information is default for the product.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/vendorConfig

diagram |
type | axlapi:XVendorConfig
properties |
minOcc | 0
maxOcc | 1
content | complex
source | <xsd:element name="vendorConfig" type="axlapi:XVendorConfig" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/traceFlag

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="traceFlag" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/mlppDomainId

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
This setting only effects devices that support MLPP. Use -1 to set to null
source | <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only effects devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/mlppIndicationStatus

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Off
nillable | false
annotation |
documentation
This setting only affects devices that support MLPP.
source | <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Off" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affects devices that support MLPP.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/useTrustedRelayPoint

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="useTrustedRelayPoint" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/retryVideoCallAsAudio

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="retryVideoCallAsAudio" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/cgpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cgpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/useDevicePoolCgpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCgpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/geoLocationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/sendGeoLocation

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
Not valid for CTI route points and VoiceMail ports
source | <xsd:element name="sendGeoLocation" type="axlapi:boolean" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Not valid for CTI route points and VoiceMail ports</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/ports

diagram |
properties |
minOcc | 0
maxOcc | 1
content | complex
children | port
source | <xsd:element name="ports" minOccurs="0" maxOccurs="1"> <xsd:complexType> <xsd:sequence minOccurs="0"> <xsd:element name="port" type="axlapi:XT1Port" minOccurs="1" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/ports/port

diagram |
type | axlapi:XT1Port
properties |
minOcc | 1
maxOcc | unbounded
content | complex
children | portNumber attendantDn unattendedPort callerIdDn callerIdEnable callingPartySelection digitSending expectedDigits sigDigits prefixDn presentationBit silenceSuppressionThreshold startDialProtocol trunk trunkDirection trunkLevel trunkPadRx trunkPadTx vendorConfig callerId endpointId timer1 timer2 timer3 timer4 timer5 timer6
source | <xsd:element name="port" type="axlapi:XT1Port" minOccurs="1" maxOccurs="unbounded"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/trunkSelectionOrder

diagram |
type | axlapi:XTrunkSelectionOrder
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="trunkSelectionOrder" type="axlapi:XTrunkSelectionOrder" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/clockReference

diagram |
type | axlapi:XClockReference
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="clockReference" type="axlapi:XClockReference" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/csuParam

diagram |
type | axlapi:XCSUParam
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="csuParam" type="axlapi:XCSUParam" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/digitSending

diagram |
type | axlapi:XDigitSending
properties |
minOcc | 0
maxOcc | 1
content | simple
default | DTMF
nillable | false
source | <xsd:element name="digitSending" type="axlapi:XDigitSending" default="DTMF" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/pcmType

diagram |
type | axlapi:XEncode
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
source | <xsd:element name="pcmType" type="axlapi:XEncode" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/fdlChannel

diagram |
type | axlapi:XFDLChannel
properties |
minOcc | 0
maxOcc | 1
content | simple
default | None
nillable | false
source | <xsd:element name="fdlChannel" type="axlapi:XFDLChannel" default="None" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/yellowAlarm

diagram |
type | axlapi:XYellowAlarm
properties |
minOcc | 0
maxOcc | 1
content | simple
default | F-Bit
nillable | false
source | <xsd:element name="yellowAlarm" type="axlapi:XYellowAlarm" default="F-Bit" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/zeroSupression

diagram |
type | axlapi:XZeroSuppression
properties |
minOcc | 0
maxOcc | 1
content | simple
default | B8ZS
nillable | false
source | <xsd:element name="zeroSupression" type="axlapi:XZeroSuppression" default="B8ZS" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/smdiBasePort

diagram |
type | axlapi:XInteger
properties |
minOcc | 0
maxOcc | 1
content | simple
default | 0
nillable | false
source | <xsd:element name="smdiBasePort" type="axlapi:XInteger" default="0" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/handleDtmfPrecedenceSignals

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="handleDtmfPrecedenceSignals" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/cdpnTransformationCssName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="cdpnTransformationCssName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/useDevicePoolCdpnTransformCss

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="useDevicePoolCdpnTransformCss" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/geoLocationFilterName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="geoLocationFilterName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/pstnAccess

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | true
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:element name="pstnAccess" type="axlapi:boolean" default="true" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCiscoCatalyst6000T1VoIPGatewayT1Req/imeE164TransformationName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="imeE164TransformationName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy