complexType UpdateCommonDeviceConfigReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:NameAndGUIDRequest
properties |
base | axlapi:NameAndGUIDRequest
children | name uuid newName softkeyTemplateName userLocale networkHoldMohAudioSourceId userHoldMohAudioSourceId mlppDomainId mlppIndicationStatus useTrustedRelayPoint preemption ipAddressingMode ipAddressingModePreferenceControl allowAutoConfigurationForPhones useImeForOutboundCalls
used by |
element | updateCommonDeviceConfig
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="UpdateCommonDeviceConfigReq"> <xsd:complexContent> <xsd:extension base="axlapi:NameAndGUIDRequest"> <xsd:sequence> <xsd:element name="newName" type="axlapi:UniqueString50" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="softkeyTemplateName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/> <xsd:element name="userLocale" type="axlapi:XUserLocale" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable. The value accepted and retrieved from the database for this field will be of type XUserLocale in AXLEnums.xsd.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="networkHoldMohAudioSourceId" type="axlapi:XMOHAudioSourceId" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="userHoldMohAudioSourceId" type="axlapi:XMOHAudioSourceId" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="useTrustedRelayPoint" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Default is not applicable for CommonDeviceConfig API</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="preemption" type="axlapi:XPreemption" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="ipAddressingMode" type="axlapi:XIPAddressingMode" default="IPv4 and IPv6" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="ipAddressingModePreferenceControl" type="axlapi:XIPAddressingModePrefControl" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="allowAutoConfigurationForPhones" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> <xsd:element name="useImeForOutboundCalls" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element UpdateCommonDeviceConfigReq/newName

diagram |
type | axlapi:UniqueString50
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | false
facets |
Kind | Value | Annotation
maxLength | 50 |
source | <xsd:element name="newName" type="axlapi:UniqueString50" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCommonDeviceConfigReq/softkeyTemplateName

diagram |
type | axlapi:XFkType
properties |
minOcc | 0
maxOcc | 1
content | complex
nillable | true
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
source | <xsd:element name="softkeyTemplateName" type="axlapi:XFkType" nillable="true" minOccurs="0" maxOccurs="1"/>

element UpdateCommonDeviceConfigReq/userLocale

diagram |
type | axlapi:XUserLocale
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
annotation |
documentation
Nullable. The value accepted and retrieved from the database for this field will be of type XUserLocale in AXLEnums.xsd.
source | <xsd:element name="userLocale" type="axlapi:XUserLocale" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable. The value accepted and retrieved from the database for this field will be of type XUserLocale in AXLEnums.xsd.</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/networkHoldMohAudioSourceId

diagram |
type | axlapi:XMOHAudioSourceId
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
annotation |
documentation
Nullable
source | <xsd:element name="networkHoldMohAudioSourceId" type="axlapi:XMOHAudioSourceId" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/userHoldMohAudioSourceId

diagram |
type | axlapi:XMOHAudioSourceId
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
annotation |
documentation
Nullable
source | <xsd:element name="userHoldMohAudioSourceId" type="axlapi:XMOHAudioSourceId" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Nullable</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/mlppDomainId

diagram |
type | axlapi:String128
properties |
minOcc | 0
maxOcc | 1
content | simple
nillable | true
facets |
Kind | Value | Annotation
maxLength | 128 |
annotation |
documentation
This setting only affect devices that support MLPP. Use -1 to set to null
source | <xsd:element name="mlppDomainId" type="axlapi:String128" nillable="true" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP. Use -1 to set to null</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/mlppIndicationStatus

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
annotation |
documentation
This setting only affect devices that support MLPP
source | <xsd:element name="mlppIndicationStatus" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/useTrustedRelayPoint

diagram |
type | axlapi:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
default | false
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
Default is not applicable for CommonDeviceConfig API
source | <xsd:element name="useTrustedRelayPoint" type="axlapi:boolean" default="false" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>Default is not applicable for CommonDeviceConfig API</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/preemption

diagram |
type | axlapi:XPreemption
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
annotation |
documentation
This setting only affect devices that support MLPP
source | <xsd:element name="preemption" type="axlapi:XPreemption" default="Default" nillable="false" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This setting only affect devices that support MLPP</xsd:documentation> </xsd:annotation> </xsd:element>

element UpdateCommonDeviceConfigReq/ipAddressingMode

diagram |
type | axlapi:XIPAddressingMode
properties |
minOcc | 0
maxOcc | 1
content | simple
default | IPv4 and IPv6
nillable | false
source | <xsd:element name="ipAddressingMode" type="axlapi:XIPAddressingMode" default="IPv4 and IPv6" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCommonDeviceConfigReq/ipAddressingModePreferenceControl

diagram |
type | axlapi:XIPAddressingModePrefControl
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Use System Default
nillable | false
source | <xsd:element name="ipAddressingModePreferenceControl" type="axlapi:XIPAddressingModePrefControl" default="Use System Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCommonDeviceConfigReq/allowAutoConfigurationForPhones

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="allowAutoConfigurationForPhones" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

element UpdateCommonDeviceConfigReq/useImeForOutboundCalls

diagram |
type | axlapi:XStatus
properties |
minOcc | 0
maxOcc | 1
content | simple
default | Default
nillable | false
source | <xsd:element name="useImeForOutboundCalls" type="axlapi:XStatus" default="Default" nillable="false" minOccurs="0" maxOccurs="1"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy