complexType DoDeviceResetReq

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:APIRequest
properties |
base | axlapi:APIRequest
children | deviceName isHardReset deviceResetType
used by |
element | doDeviceReset
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
isMGCP | axlapi:boolean | optional | false |  |
annotation |
documentation
Performs either a hard or soft reset on the specified device. If resetting an MGCP box, then set isMGCP attribute to true.
source | <xsd:complexType name="DoDeviceResetReq"> <xsd:annotation> <xsd:documentation>Performs either a hard or soft reset on the specified device. If resetting an MGCP box, then set isMGCP attribute to true.</xsd:documentation> </xsd:annotation> <xsd:complexContent> <xsd:extension base="axlapi:APIRequest"> <xsd:sequence> <xsd:element name="deviceName" type="axlapi:XFkType" nillable="false"> <xsd:annotation> <xsd:documentation>The name or UUID of the device to performs a reset on. Not nullable.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:choice> <xsd:element name="isHardReset" type="axlapi:boolean" nillable="false"> <xsd:annotation> <xsd:documentation>True performs a hard reset. False performs a soft reset. Not nullable.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="deviceResetType" type="axlapi:XReset" nillable="false"> <xsd:annotation> <xsd:documentation>Not nullable</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> </xsd:sequence> <xsd:attribute name="isMGCP" type="axlapi:boolean" use="optional" default="false"/> </xsd:extension> </xsd:complexContent> </xsd:complexType>

attribute DoDeviceResetReq/@isMGCP

type | axlapi:boolean
properties |
use | optional
default | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
source | <xsd:attribute name="isMGCP" type="axlapi:boolean" use="optional" default="false"/>

element DoDeviceResetReq/deviceName

diagram |
type | axlapi:XFkType
properties |
content | complex
nillable | false
attributes |
Name | Type | Use | Default | Fixed | Annotation
uuid | axlapi:XUUID | optional |  |  |
annotation |
documentation
The name or UUID of the device to performs a reset on. Not nullable.
source | <xsd:element name="deviceName" type="axlapi:XFkType" nillable="false"> <xsd:annotation> <xsd:documentation>The name or UUID of the device to performs a reset on. Not nullable.</xsd:documentation> </xsd:annotation> </xsd:element>

element DoDeviceResetReq/isHardReset

diagram |
type | axlapi:boolean
properties |
content | simple
nillable | false
facets |
Kind | Value | Annotation
pattern | (t)|(f)|(true)|(false)|(0)|(1) |
annotation |
documentation
True performs a hard reset. False performs a soft reset. Not nullable.
source | <xsd:element name="isHardReset" type="axlapi:boolean" nillable="false"> <xsd:annotation> <xsd:documentation>True performs a hard reset. False performs a soft reset. Not nullable.</xsd:documentation> </xsd:annotation> </xsd:element>

element DoDeviceResetReq/deviceResetType

diagram |
type | axlapi:XReset
properties |
content | simple
nillable | false
annotation |
documentation
Not nullable
source | <xsd:element name="deviceResetType" type="axlapi:XReset" nillable="false"> <xsd:annotation> <xsd:documentation>Not nullable</xsd:documentation> </xsd:annotation> </xsd:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy