complexType GetPhoneRes

diagram |
namespace | http://www.cisco.com/AXL/API/9.0
type | extension of axlapi:APIResponse
properties |
base | axlapi:APIResponse
children | return
used by |
element | getPhoneResponse
attributes |
Name | Type | Use | Default | Fixed | Annotation
sequence | xsd:unsignedLong | optional |  |  |
source | <xsd:complexType name="GetPhoneRes"> <xsd:complexContent> <xsd:extension base="axlapi:APIResponse"> <xsd:sequence> <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="phone" type="axlapi:RPhone"/> </xsd:sequence> </xsd:complexType> </xsd:element> </xsd:sequence> </xsd:extension> </xsd:complexContent> </xsd:complexType>

element GetPhoneRes/return

diagram |
properties |
content | complex
children | phone
source | <xsd:element name="return"> <xsd:complexType> <xsd:sequence> <xsd:element name="phone" type="axlapi:RPhone"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element GetPhoneRes/return/phone

diagram |
type | axlapi:RPhone
properties |
content | complex
children | name description product model class protocol protocolSide callingSearchSpaceName devicePoolName commonDeviceConfigName commonPhoneConfigName networkLocation locationName mediaResourceListName networkHoldMohAudioSourceId userHoldMohAudioSourceId automatedAlternateRoutingCssName aarNeighborhoodName loadInformation vendorConfig versionStamp traceFlag mlppDomainId mlppIndicationStatus preemption useTrustedRelayPoint retryVideoCallAsAudio securityProfileName sipProfileName cgpnTransformationCssName useDevicePoolCgpnTransformCss geoLocationName geoLocationFilterName sendGeoLocation lines numberOfButtons phoneTemplateName speeddials busyLampFields primaryPhoneName ringSettingIdleBlfAudibleAlert ringSettingBusyBlfAudibleAlert blfDirectedCallParks addOnModules userlocale networkLocale idleTimeout authenticationUrl directoryUrl idleUrl informationUrl messagesUrl proxyServerUrl servicesUrl services softkeyTemplateName loginUserId defaultProfileName enableExtensionMobility currentProfileName loginTime loginDuration currentConfig singleButtonBarge joinAcrossLines builtInBridgeStatus callInfoPrivacyStatus hlogStatus ownerUserName ignorePresentationIndicators packetCaptureMode packetCaptureDuration subscribeCallingSearchSpaceName rerouteCallingSearchSpaceName allowCtiControlFlag presenceGroupName unattendedPort requireDtmfReception rfc2833Disabled certificateOperation authenticationMode keySize authenticationString certificateStatus upgradeFinishTime deviceMobilityMode roamingDevicePoolName remoteDevice dndOption dndRingSetting dndStatus isActive isDualMode mobilityUserIdName phoneSuite phoneServiceDisplay isProtected mobileSmartClientProfileName mtpRequired mtpPreferedCodec dialRulesName sshUserId sshPwd digestUser outboundCallRollover hotlineDevice secureInformationUrl secureDirectoryUrl secureMessageUrl secureServicesUrl secureAuthenticationUrl secureIdleUrl alwaysUsePrimeLine alwaysUsePrimeLineForVoiceMessage featureControlPolicy deviceTrustMode earlyOfferSupportForVoiceCall requireThirdPartyRegistration blockIncomingCallsWhenRoaming homeNetworkId AllowPresentationSharingUsingBfcp requireOffPremiseLocation
attributes |
Name | Type | Use | Default | Fixed | Annotation
ctiid | xsd:positiveInteger |  |  |  |
uuid | axlapi:XUUID |  |  |  |
source | <xsd:element name="phone" type="axlapi:RPhone"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy