> Exec Modes Show Commands (H-L)
> This section includes the commands show ha-service through show logs.
> show ha-service
> Displays information on configured home agent services.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ha-service { all | name ha_name } [ | { grep grep_options | more } ]
> all | name ha_name
> all: indicates information on all home agent services is to be displayed.
> name ha_name: indicates only the information for the HA service specified as ha_name is to be displayed.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display home agent service configuration information.
> Example
> The following commands displays information on the HA service sampleService and all services, respectively.
> show ha-service name sampleService show ha-service all
> show hardware
> Displays information on the system hardware.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show hardware { card [ card_num ] | inventory | version [ board | diags | fans] } [ | { grep grep_options | more } ]
> card [ card_num ]
> Provide the hardware information for all cards or the card specified by card_num. card_num must be a value in the range 1 through 48 and must refer to an installed card.
> inventory
> Display the hardware information for all slots in tabular format.
> version [ board | diags | fans]
> Display the CPU information for all application cards and fan controller version for the upper and lower fan trays.
> board: Only include the CPLD and FPGA version information.
> diags: Only include the CFE diagnostics version information.
> fans: Show the fan controller versions for the upper and lower fan trays.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Show the hardware information to verify part lists and hardware component versions with reserve stock
> Example
> The following displays the hardware information for a card installed in slot 1.
> show hardware card 1
> The following command displays the hardware inventory for the entire chassis.
> show hardware inventory
> The following command results in the display of the CPU version for all application cards displaying only the CPLD and FPGA information.
> show hardware version board
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hd raid
> Shows the output of the RAID established on the ASR 5000 SMCs.
> Product
> All
> Privilege
> Security Administrator, Administrator, Administrator, Operator
> Syntax
> show hd raid [ verbose ]
> Example
> show hd raid verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hd-storage-policy
> Displays ACR counter and statistic information.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Inspector
> Syntax
> show hd-storage-policy { all | counters [ all ] [ name name ] [ verbose ] | name name | statistics [ all ] [ name name ] [ verbose ] }
> all
> Specifies that ACR information for all HD storage policies configured on the system is to be displayed.
> counters [ all ] [ name name ] [ verbose ]
> Specifies that ACR counter information for HD storage policies configured on the system is to be displayed.
> name name
> Specifies that ACR information for an HD storage policy with the specified name is to be displayed.
> statistics [ all ] [ name name ] [ verbose ]
> Specifies that ACR statistic information for HD storage policies configured on the system is to be displayed.
> verbose
> Displays HD storage statitics based on instance.
> Usage
> Use this command to display ACR counter and statistic information.
> Example
> The following command displays ACR statistic information for an HD storage policy named pgwsgw:
> show hd-storage-policy statistics name pgwsgw
> show hnbgw counters
> This command displays the session counter information for Home-NodeB Gateway (HNB-GW) services and HNBs connected on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw counters [hnbgw-service service_name | hnbid hnb_identifier] [ | { grep grep_options | more } ]
> hnbgw-service service_name
> This keyword is used to filter the counter display based on the HNB-GW service name service_name configured and running on this system.
> service_name must be an existing HNB-GW service, and be from 1 to 63 alpha and/or numeric characters in length.
> hnbid hnb_identifier
> This keyword is used to filter the counter display based on Home-NodeB hnb_identifier which is connected to this system with HNB-GW service and in active or dormant state.
> hnb_identifier must be an identifier for HNB from 1 to 255 alpha and/or numeric characters in length.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view the session counter information for HNB-GW services configured and HNBs connected on this system.
> Example
> The following command displays the counters for the HNB-GW service named hnbgw1:
> show hnbgw counter hnbgw-service hnbgw1
> show hnbgw statistics hnbgw-service
> This command displays the session statistics for Home-NodeB Gateway (HNB-GW) services configured and running on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw statistics hnbgw-service service_name[hnbap-only | ranap-only | rua -only | sccp-only | sctp-only ] [ verbose] [ | { grep grep_options | more } ]
> hnbgw-service service_name
> This keyword is used to filter the session statistics display based on the HNB-GW service name service_name configured and running on this system.
> service_name must be an existing HNB-GW service, and be from 1 to 63 alpha and/or numeric characters in length.
> hnbap-only
> This keyword is used to filter the session statistics display limited to Home NodeB Application Part (HNBAP) traffic only for selected HNB-GW service which is configured and running on this system.
> ranap-only
> This keyword is used to filter the session statistics display limited to Radio Access Network Application Protocol (RANAP) traffic only for selected HNB-GW service which is configured and running on this system.
> rua-only
> This keyword is used to filter the session statistics display limited to RANAP User Adaptation (RUA) traffic only for selected HNB-GW service which is configured and running on this system.
> sccp-only
> This keyword is used to filter the session statistics display limited to Signaling Connection Control Part (SCCP) traffic only for selected HNB-GW service which is configured and running on this system.
> sctp-only
> This keyword is used to filter the session statistics display limited to Stream Control Transmission Protocol (SCTP) traffic only for selected HNB-GW service which is configured and running on this system.
> verbose
> This keyword is used to display the detailed statistics for all sessions on HNB-GW services or for selected filter and named HNB-GW service which is configured and running on this system.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view the session statistics for overall session or in selected part of user session for HNB-GW services configured and running on this system.
> Example
> The following command displays the session statistics for HNBAP part of session details for the HNB-GW service named hnbgw1:
> show hnbgw statistics hnbgw-service hnbgw1 hnbap-only
> The following command displays the session statistics for RANAP part of session with maximum details for the HNB-GW service named hnbgw1:
> show hnbgw statistics hnbgw-service hnbgw1 ranap-only verbose
> show hnbgw statistics hnbid
> This command displays the session statistics for Home-NodeB (HNB) connected to an HNB-GW service on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw statistics hnbid hnb_identifier[hnbap-only | ranap-only | rua -only] [ verbose] [ | { grep grep_options | more } ]
> hnbid hnb_identifier
> This keyword is used to filter the session statistics display based on Home-NodeB hnb_identifier which is connected to this system through an HNB-GW service.
> hnb_identifier must be an identifier for HNB from 1 to 255 alpha and/or numeric characters in length.
> hnbap-only
> This keyword is used to filter the session statistics display limited to Home NodeB Application Part (HNBAP) traffic only for selected HNB which is connected to this system through HNB-GW service.
> ranap-only
> This keyword is used to filter the session statistics display limited to Radio Access Network Application Protocol (RANAP) traffic only for selected HNB which is connected to this system through HNB-GW service.
> rua-only
> This keyword is used to filter the session statistics display limited to RANAP User Adaptation (RUA) traffic only for selected HNB which is connected to this system through HNB-GW service.
> verbose
> This keyword is used to display the detailed statistics for all HNB sessions or for selected filter and HNB which is connected to this system through HNB-GW service.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view the session statistics for overall session or in selected part of user session for selected HNB which is connected to this system through HNB-GW service..
> Example
> The following command displays the session statistics for HNBAP part of session details for the HNB having hnb112234 as identifier on this system:
> show hnbgw statistics hnbid hnb112234 hnbap-only
> The following command displays the detailed session statistics for RANAP part of session details for the HNB having hnb112234 as identifier on this system:
> show hnbgw statistics hnbid hnb112234 ranap-only verbose
> show hnbgw-service
> This command displays the configuration details for configured HNB-GW service(s) on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw-service {all | hnbgw-service service_name}
> all
> This keyword is used to display the configuration and other default parameters for all HNB-GW service configured on this system.
> hnbgw-service service_name
> This keyword displays the configuration and default parameters for specific HNB-GW service name service_name which is configured and running on this system.
> service_name must be an existing HNB-GW service, and be from 1 to 63 alpha and/or numeric characters in length.
> Usage
> Use this command to view the configuration and service parameters set for all or any specific HNB-GW service(s) on this system.
> Example
> The following command displays the configured and default paramters for all HNB-GW services configured on this system:
> show hnbgw-service all
> show hsgw-service
> Displays configuration information for HRPD Serving Gateway (HSGW) services on this system.
> Product
> HSGW
> Privilege
> Inspector
> Syntax
> show hsgw-service { all | name service_name } [ | { grep grep_options | more } ]
> all
> Displays configuration information for all HSGW services configured on this system.
> name service_name
> Displays configuration information for a specific HSGW service configured on this system.
> service_name must be an existing HSGW service, and be from 1 to 63 alpha and/or numeric characters in length.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for HSGW services on this system.
> Example
> The following command displays service statistics for the HSGW service named hsgw1:
> show hsgw-service name hsgw1
> show ims-authorization policy-control
> Displays information and statistics specific to the policy control in IP Multimedia Subsystem (IMS) authorization service.
> Product
> SCM, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ims-authorization policy-control statistics [ service ims_auth_svc_name| server { ip-address ip_address [ port port_value ] | name server_name } ] [ | { grep grep_options| more } ]
> statistics
> Displays the total collected statistics of all policy control parameters of IMS authorization service sessions since the last system restart or clear command.
> service ims_auth_svc_name
> Displays the total collected statistics of all IMS authorization sessions processed by a specific IMS authorization service since the last system restart or clear command. ims_auth_svc_name must be an existing IMS authorization service name.
> server { ip-address ip_address [ port port_value ] | name server_name }
> Displays the server-level message statistics and the server IP address.
> Specify the PCRF server IP address or server name.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display information and statistics about policy control configuration in existing IMS authorization services.
> Example
> The following command displays the existing IMS authorization service name ims_auth_gx1 on the system:
> show ims-authorization policy-control statistics service ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization policy-gate
> Displays information of installed Policy Gates for specific subscriber in IP Multimedia Subsytem (IMS) authorization service.
> Product
> SCM, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ims-authorization policy-gate { { status [ summary | full ] [ { imsi imsi_value [ nsapi nsapi_value] } | callid call_id | { ims-auth-service ims_auth_svc } [ rulename rule_name ] } | { counters [ all | { imsi imsi_value [ nsapi nsapi_value ] } | { rulename rule_name} | { callid call_id } ] }[ | { grep grep_options | more } ] ]
> status [ summary | full ]
> This option displays the status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specified criteria.
> summary: limits the display to a summary on status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based.
> full: displays the full information on status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based.
> counters all
> This option displays the counters/statistics of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specified criteria.
> all displays the all counters of the installed gates and their flow definitions along with the run-time status in an IMS authorization service based.
> imsi imsi_value [ nsapi nsapi_value ]
> This option displays all of the counters/status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specified International Mobile Subscriber Identity (IMSI) named imsi_value.
> nsapi nsapi_value specifies Network Service Access Point Identifier (NSAPI) named nsapi_value to limit the display to a single PDP context of the subscriber.
> callid call_id
> This option displays all of the counters/status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specified call identifier named call_id.
> ims-auth-service ims_auth_svc
> This option displays status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service named ims_auth_svc.
> rulename rule_name
> This option displays all of the counters/status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specific dynamic charging rule named rule_name.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display information/statistics/counters about all of the installed policy gates and their flow definitions along with the run-time status with specified criteria and filters in existing IMS authorization services.
> Example
> The following command displays the full status of the installed policy gates in an existing IMS authorization service on the system:
> show ims-authorization policy-gate status full
> The following command displays the all counters of the installed policy gates in an existing IMS authorization service on the system:
> show ims-authorization policy-gate counters all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization servers
> Displays information and statistics specific to the authorization servers used for IP Multimedia Subsytem (IMS) authorization service.
> Product
> SCM, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization servers [ ims-auth-service ims_auth_svc_name[ | { grep grep_options| more } ] ]
> server [ ims-auth-service ims_auth_svc_name ]
> Displays the information and statistics of all authorization servers configured for IMS authorization service in a system.
> ims-auth-service ims_auth_svc_name: Displays the configured authorization servers for IMS authorization for an IMS authorization service named ms_auth_svc_name.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display information and statistics about IMS authorization servers configured on a system or IMS authorization service.
> Example
> The following command displays the information and statistics of the authorization servers in IMS authorization service named ims_auth_gx1:
> show ims-authorization servers ims-auth-service ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization service
> Displays information, configuration, and statistics of all/specific IP Multimedia Subsytem (IMS) authorization service.
> Product
> SCM, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization service { { all [ verbose ] | name ims_auth_svc_name | summary ] } | { statistics [ all | name ims_auth_svc_name ] [ verbose ] } [ | { grep grep_options| more } ]
> all [ verbose ]
> Displays information and configuration of all configured IMs authorization services with a single line of information for each IMS authorization service.
> verbose: Displays all information and configuration data of every IMS authorization services configured on system.
> name ims_auth_svc_name ]
> Displays the information, statistics, and configuration data of an IMS authorization service named ms_auth_svc_name.
> summary
> Displays summarized information and configuration data of all IMS authorization services configured in a system.
> statistics [ all | name ims_auth_svc_name ] [ verbose ]
> Displays the IMS Authorization service statistics including following information:

> • | Initial authorization procedures

> • | Re-authorization procedures initiated by us

> • | Re-authorization procedures initiated by servers

> • | Various failure statistics

> If no criteria specified summarized statistics of all IMS Authorization services are displayed

> • | all: displays individual statistics for every IMS authorization service configured on system.

> • | name ims_auth_svc_name: Displays the statistics of the IMS authorization service named ims_auth_svc_name

> • | verbose: displays the detailed statistics of a configured IMS authorization service.

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display the IMS Authorization service status, counters and configuration. The status includes the state of a server table switchover. Statistics option is used for various processes and procedure status.
> Example
> The following command displays the information and configuration data of the IMS authorization service named ims_auth_gx1:
> show ims-authorization service name ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization sessions
> Displays information, configuration, and statistics of sessions active in IP Multimedia Subsystem (IMS) authorization service.
> Product
> SCM, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization session [ full | summary ] | [ all | [ ims-auth-service ims_auth_svc_name | imsi imsi_value [ nsapi nsapi_value ] | apn apn_name | ip-address ip_address | callid call_id ] [ | { grep grep_options| more } ]
> full
> Displays complete information and configuration data of all sessions in IMS authorization services configured in a system.
> summary
> Displays summarized information and configuration data of all sessions in IMS authorization services configured in a system.
> all
> Displays information and configuration of all sessions running in IMS authorization services with a single line of information for each IMS authorization session.
> ims-auth-service ims_auth_svc_name ]
> Displays the information, statistics, and configuration data of sessions in an IMS authorization service named ms_auth_svc_name.
> imsi imsi_value [ nsapi nsapi_value ]
> This option displays all of the counters/status of the running services in an IMS authorization service based on the specified International Mobile Subscriber Identity (IMSI) named imsi_value.
> nsapi nsapi_value specifies Network Service Access Point Identifier (NSAPI) named nsapi_value to limit the display to a single PDP context of the subscriber.
> apn apn_name
> This option displays all of the counters/status of the running services in IMS authorization service based on the access point name (APN) named apn_name.
> ip-address ip_address
> This option displays all of the counters/status of the running services in IMS authorization service based on the host IP address having IP address value as ip_address.
> callid call_id
> This option displays all of the counters/status of the running services in IMS authorization service based on the specified call identifier named call_id.
> summary
> Displays summarized information and configuration data of all IMS authorization services configured in a system.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display the sessions running under IMS Authorization service on a system with different filter criteria.
> Example
> The following command displays the information and statistical data of a session in IMS authorization service:
> show ims-authorization sessions full
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip
> Displays information for the IP-based interfaces’ access group and access list information along with address resolve protocol information for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip { access-group [ statistics] | access-list [ list_name ] | arp [ arp_ip_address ] | [summary ] | statistics ] ] | localhosts [ host_name ] | prefix-list [ detail [list_name] | name list_name| summary [list_name] ] | rip | route [ route_ip_address [ route_gw_address ] ] | static-route sroute_ip_address [ sroute_gw_address ] | vrf vrf-name} [ | { grep grep_options | more } ]
> access-group [ statistics ]
> Displays all configured access groups in the current context along with the priority values.
> statistics: Displays all configured access groups along with packet and byte counters for each ACL rule hit for the current context. In addition, it shows the priority values.
> access-list [ list_name ]
> Indicates the output is to display the information for all access control lists or the list specified as list_name.
> arp [ arp_ip_address ]
> Displays the address resolution protocol table or the ARP information associated with the IP address specified as arp_ip_address. arp_ip_address must be specified using the standard IPv4 dotted decimal notation.
> Important: When the VPN Manager restarts, it removes all interfaces from the kernel and thus the kernel removes all ARP entries. When this happens, the NPU still holds all of the ARP entries so that there is no traffic disruption. When this happens, from a user point of view, show ip arp is broken since this command gathers information from the Kernel and not the NPU.
> localhosts [ host_name ]
> Displays all the local host information or only for the host specified as host_name.
> prefix-list [ detail [ list_name ] | name list_name | summary [ list_name ] ]
> This keyword list information on configured IP prefix lists. With no keyword supplied, a list of all prefix lists and their entries is displayed.
> detail [ list_name ]: Lists detailed information for all prefix lists and their entries. If a list name is specified only the details for the specified prefix list are displayed. list_name must be a string of from 1 through 79 alpha and/or numeric characters.
> name list_nam: Lists the entries for a specified prefix list. list_name must be a string of from 1 through 79 alpha and/or numeric characters.
> summary [ list_name ]: Lists summary information for all prefix lists and their entries. If a list name is specified only the summary for the specified prefix list are displayed. list_name must be a string of from 1 through 79 alpha and/or numeric characters.
> rip
> Displays general RIP routing process information. (RIP is not supported at this time.)
> route [ route_ip_address [ route_gw_address ] ]
> Indicates the route information to the address specified by route_ip_address is to be displayed. The route gateway address may be specified as needed to identify the route. route_ip_address and route_gw_address must be specified using the standard IPv4 dotted decimal notation.
> static-route sroute_ip_address [ sroute_gw_address ]
> Displays the static route information for the address specified by sroute_ip_address is to be displayed. The static route gateway address may also be specified to identify the route. sroute_ip_address and sroute_gw_address must be specified using the standard IPv4 dotted decimal notation.
> vrf vrf_name
> Displays the routing information of the VRF. vrf_name is a name used to identify a VRF.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Show the IP information to verify and/or troubleshooting communication difficulties between to a remote host/node.
> Example
> The following command displays the ACL for the list named sampleACL.
> show ip access-list sampleACL
> The following command will output the static route information to remote host 1.2.3.4.
> show ip static-route 1.2.3.4
> show ip as-path-access-list
> Displays the contents of a BGP router AS path access list in the current context.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip as-path-access-list list_name
> list_name
> The name of an existing AS path access list configured in the current context.
> must be an alpha and or numeric string from 1 through 79 characters in length.
> Usage
> Use this command to display the configured entries for the specified BGP router AS path access list in the current context.
> Example
> The following command displays the contents of an AS path access list named ASlist1:
> show ip as-path-access-list ASlist1
> show ip bgp
> Disp[lays BGP information for the current context.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip bgp [ip_address/mask| debugging | filter-list list_name| neighbors [ip_adrress] | route-map map_name| vpnv4 { all [network | neighbors | summary ] | vrf vrf-name [ network ] | route-distinguisher [ network | neighbors | summary ] } [ | { grep grep_options | more } ]
> ip_address/mask
> Specify the IP address and netmask bits for the network for which information should be displayed. ip_address is an IPv4 address in dotted-decimal notation and mask is the number of subnet bits, representing a subnet mask in shorthand. These must be entered in the dotted-decimal notation/subnet bits format (1.1.1.1/24).
> debugging
> Display debug flags that are enabled.
> filter-list list_name
> Display routes that match the specified filter list.
> neighbors [ip_address]
> Display information for all neighbors or a specified neighbor. i p_address is an IPv4 address in dotted-decimal notation
> route-map map_name
> Display routes that match the specified route-map.
> vpnv4 { all [network | neighbors | summary ] | vrf vrf-name [ network ] | route-distinguisher [ network | neighbors | summary ] }
> Display all VPNv4 routing data, routing data for a VRF, or a route-distinguisher.

> • | all: displays all VPN routing information. If this is specified, the information displayed is gathered from all the VRF's known to BGP and displayed. It could contain the list of neighbors, the list of networks, or a particular network

> • | network: displays the network for which information in the BGP routing table.

> • | neighbors: shows neighbor information for the all the vrfs including the default vrf or for the VRF with a matching RD value.

> • | summary: shows summary information of neighbors for all the vrfs including the default vrf or for the VRF with a matching RD value.

> • | vrf vrf name: name used to identify a VRF. Information is only gathered from the corresponding VRF. If there is no such VRF, an error is reported.

> • | network: displays the network for which information in the BGP routing table.

> • | route-distinguisher: If specified along with the RD value, the information displayed is gathered from the corresponding VRF whose RD value is the same as the specified value. If there is no VRF associated with such an RD, an error is reported.

> • | network:displays the network for which information in the BGP routing table.

> • | neighbors:shows neighbor information for the all the vrfs including the default vrf or for the VRF with a matching RD value.

> • | summary:shows summary information of neighbors for all the vrfs including the default vrf or for the VRF with a matching RD value.

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command display to BGP information for the current context.
> Example
> The following command displays information for all BGP neighbors:
> show ip bgp neighbors
> show ip interface
> This command displays the statistical and configuration information for the IP-based interfaces including VRF table for specific context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipinterface [vrf vrf-name] [ name intfc_name [statistics] [tunnel [gre-keepalive ] ] [summary] [ | { grep grep_options | more } ]
> vrf vrf_name
> Displays the routing information of the VRF. vrf_name is a name used to identify a VRF.
> name intfc_name
> Indicates the name of the interface for which information has to be displayed. If no interface name is specified then information for all IP interfaces is displayed.
> ntfc_name is name of the configured IP interface.
> tunnel [ gre-keepalive ]
> This keyword will filter the IP interface information for tunnel type of interfaces.
> It is applicable for GRE/IP-in-IP type of tunnel interfaces only.
> gre-keepalive: This optional keyword displays the GRE keepalive information for GRE tunnel configured with this IP interface.
> statistics
> Displays the session statistics of all ingress and egress packets processed through this IP interface.
> summary
> Displays summarized information about requested IP interface/s.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display the summarized of detailed configuration and statistical information for configured IP interface. This information can be used to verify and/or troubleshooting communication difficulties between to a remote host/node.
> Example
> The following command displays the interface information, including statistics, for the IP interface sampleInterface.
> show ip interface sampleInterface statistics
> The following command displays the GRE keepalive information for an IP interface named IP_gre1.
> show ip interface IP_gre1 tunnel gre-keepalive
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip ospf
> This command displays OSPF routing information.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> showipospf [ border-routers | database [ verbose ] [ ls-id ip_addr] [ adv-router ip_addr] [ ls-type { router | network | summary | asbr-summary | external | nssa |integer} ] | debugging | interface | neighbor [ details ] | route | virtual-links ]
> border-routers
> Displays all known area border routers (ABRs) and Autonomous System border routers (ASBRs) for OSPF.
> database [ verbose ] [ ls-id ip_addr ] [ adv-router ip_addr ] [ ls-type { router | network | summary | asbr-summary | external | nssa | integer } ]
> Displays a summary of the database information for OSPF.
> verbose: Display detailed OSPF database information.
> ls-id ip_addr: Display OSPF database information for the LSAs with the specified LSID.
> adv-router ip_addr: Display OSPF database information for the advertising router with the specified LSID.
> ls-type { router | network | summary | asbr-summary | external | nssa | LSA_Numerical_Type } ]: Display OSPF database information for the specified LSA type.
> debugging
> Lists which debugging parameters are enabled.
> interface
> Displays interface information for OSPF.
> neighbor [ details ]
> Displays summary information about all known OSPF neighbors.
> details: Displays detailed information about all known OSPF neighbors.
> route [ summary ]
> Displays the OSPF routing table.
> summary: Displays the number of intra-area, inter-area, external-1 and external-2 routes.
> virtual-links
> Displays the OSPF virtual links.
> Usage
> Use this command to display OSPF information.
> Example
> To display general OSPF information, enter the following command;
> show ip ospf
> show ip policy-forward
> Displays information for IP packet redirecting policy for HA.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip policy-forward
> Usage
> Use this command to see all the settings for IP packet redirection configuration from existing HA to new HA during upgrade.
> Important: It is a customer specific command.
> Example
> The following command displays forward policy configuration for an HA:
> show ip policy-forward
> show ip pool
> This command displays statistics specific to IP pools.
> Product
> PDSN, GGSN, HA, ASN-GW, A-BG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip pool [ address {pool-name pool_name| group-name group_name} {used | free | hold | release} [limit limit]| group-name group_name| groups | hold-timer { imsi imsi| msid msid| username username[ imsi imsi| msid msid] }| overlap | pool-name pool_name| private | public | resource | static | summary | verbose | wide ]
> address {pool-name pool_name | group-name group_name} {used | free | hold | release} [ limit limit]
> Displays IP pool addresses for the specified IP pool or pool group that are currently in the specified state.
> pool-name pool_name: Show IP addresses from the IP pool with the specified name. pool_name must be the name of an existing IP pool.
> group-name group_name: Show IP addresses from the IP pool group with the specified name. group_name must be the name of an existing IP pool group.
> used: Display the IP addresses that are in a used state.
> free: Display the IP addresses that are in a free state.
> hold: Display the IP addresses that are in a hold state.
> release: Display the IP addresses that ar4e in a release state.
> limit limit: The maximum number of address to display. limit must be an integer from 1 through 524287.
> group-name group_name
> Show information about the IP pool group with the specified name. group_name must be the name of an existing IP pool group.
> groups
> List information about all IP pool groups.
> hold-timer {imsi imsi | msid msid | username username [imsi imsi | msid msid]}
> Displays hold timer address information for the specified IMSI, MSID, or username.
> imsi imsi: The IMSI for which to display hold-timer information. imsi must be a valid IMSI (International Mobile Subscriber Identity) ID which is a 15 character field that identifies the subscriber’s home country and carrier.
> msid msid: The MSID for which to display hold-timer information. msid must be a mobile subscriber ID from 7 through 16 digits.
> username username: The username for which to display hold-timer information. username must be an alpha and or numeric string of from 1 through 127 characters.
> Important: Active users cannot be displayed. If an active ID or username is entered, the following error message appears: Failure: No address matching the specified information was found! Please confirm that the options used match the network architecture/deployment,i.e. IMSI/MSID only, Username only, or IMSI/MSID plus Username. Please note that this command does not apply for addresses in the used state.
> overlap
> List information on overlapping IP pools
> pool-name pool_name
> Show information about the specified IP pool. pool_name must be the name of an existing IP pool.
> private
> Show information about IP pools marked private.
> public
> Show information about IP pools marked public.
> resource
> Show information about resource IP pools.
> static
> Show information about static IP pools.
> summary
> Show a summary of all IP pool information.
> verbose
> Show detailed information about all IP pools.
> wide
> Show detailed information formatted to more than 80 columns.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display statistics pertaining to IP Pools in the current context.
> Example
> The following command displays IP address information for an IP Pool named pool1:
> show ip pool address pool-name pool
> To display a summary list for all IP pools in the current context, enter the following command:
> show ip pool summary
> The following command displays IP pool information for all IP pools configured in the current context:
> show ip pool verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip ipsp
> Displays the names of IP pools that are enabled for the IP pool sharing protocol (IPSP) and lists the disposition of addresses in the pools.
> Product
> PDSN, HA, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> showipipsp [ summary ]
> summary
> Only show the disposition of the addresses in the participating IP pools. Do not show the names of the participating IP pools.
> Usage
> Use this command to list the names of IP pools that are participating in the IPSP and list the disposition of IP addresses in those pools.
> Important: For information on configuring and using IPSP refer to the System Administration and Configuration Guide.
> Example
> To list information on al IPSP participating pools and address disposition, enter the following command:
> show ip ipsp
> show ipms status
> Displays the status of IPMS client service with information related to system and call events. It also displays the status of IPMS servers configured.
> Product
> IPMS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipms status [summary | all | server address ip_address]
> summary
> Displays the summary of all configured IPMS client and IPMS servers.
> all
> Displays information for all configured IPMS client and IPMS servers.
> server address ip_address
> Displays status for a specific IPMS server.
> ip_address is the IP address of the desired IPMS server and must be entered in IPv4 dotted decimal notation.
> Usage
> This command is used to show/verify the status or configuration of one or all IPMS server along with system and call event information.
> Example
> The following command displays status of an IPMS server with IP address 1.2.3.4:
> show ipms status server address 1.2.3.4
> show ipsg
> Displays information and statistics specific to the IP Services Gateway service.
> Product
> IPSG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipsg { service { all [ counters ] | name name } | sessions { all | callid num | counters { criteria } | full { criteria } | ip-address address | msid num | peer-address address | summary { criteria } | username name } | statistics [ name name | peer-address address ] } [ | { grep grep_options| more } ]
> service { all [ counters ] | name name }
> Displays information about the configured IPSG service.
> all [ counters ]: Displays information about all of the configured IPSG services on the system.
> name name: Displays information about a specific IPSG service on the system. name must be an existing IPSG service name.
> sessions { all | callid num | counters { criteria } | full { criteria } | imsi num | ip-address address | msid num | peer-address address | summary { criteria } | username name }
> all: Displays session information including call ID, NAI, and home address for all current IPSG sessions. This is the default behavior for the sessions keyword.
> callid num: Displays session information for a current IPSG session based on the call ID. num must be an existing IPSG service session call ID.
> counters { criteria }: Displays session counters for sessions matching the criteria. (See criteria below.)
> full { criteria }: Displays all available session information for sessions matching the criteria. (See criteria below.)
> ip-address address:
> msid num: Displays session information for a current IPSG session based on the MSID. num must be an existing IPSG service session MSID.
> peer-address address: Displays session information for a current IPSG session based on the IP address of the device sending the RADIUS accounting messages. address must be an existing IPSG service session IP address for the device sending the RADIUS accounting messages.
> summary { criteria }: Displays a summary of available session information for sessions matching the criteria. (See criteria below.)
> username name: Displays session information for a specific IPSG session based on the username of the subscriber. name must be an existing IPSG service session subscriber username.
> criteria:
> all: Displays session information for all exisitng IPSG service sessions.
> callid num: Displays session information for a specific IPSG session based on the call ID. num must be an existing IPSG service session call ID.
> ip-address address: Displays session information for a specific IPSG session based on the IP address of the subscriber. address must be an existing IPSG service session subscriber IP address.
> msid num: Displays session information for a specific IPSG session based on the MSID. num must be an existing IPSG service session MSID.
> peer-address address: Displays session information for a current IPSG session based on the IP address of the device sending the RADIUS accounting messages. address must be an existing IPSG service session IP address for the device sending the RADIUS accounting messages.
> username name: Displays session information for a specific IPSG session based on the username of the subscriber. name must be an existing IPSG service session subscriber username.
> statistics [ name name | peer-address address ]
> Displays the total collected statistics of all IPSG sessions since the last system restart or clear command.
> name name: Displays the total collected statisitcs of all IPSG sessions processed by a specific service since the last system restart or clear command. name must be an existing IPSG service name.
> peer-address address: Displays the total collected statistics of all IPSG sessions associated with a specific IP address of the device responsable for sending the RADIUS accounting messages. Displayed statistics are from the last system restart or clear command.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to display information and statistics about existing IPSG services.
> Example
> The following command displays the existing IPSG services on the system:
> show ipsg service all
> The following command displays all the existing IPSG service sessions on the system:
> show ipsg session all
> The following command displays the cumulative IPSG session statistics on the system:
> show ipsg statistics
> The following command displays the cumulative IPSG session statistics on the system for an IPSG service named ipsg1:
> show ipsg statistics name ipsg1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ipv6
> Displays the statistics for each rule in an IPv6 access control group.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 access-group
> show ipv6 { access-group [ statistics] | access-list [ list_name ] | interface [ summary | name interface_name [ statistics ] | neighbors | route route_ip_address }
> access-group [ statistics ]
> Displays all configured access groups in the current context along with the priority values.
> statistics: Displays all configured access groups along with packet and byte counters for each IPv6 ACL rule hit for the current context. In addition, it shows the priority values.
> access-list [ list_name ]
> Indicates the output is to display the information for all access control lists or the list specified as list_name.
> interface [ summary | name interface_name [ statistics ]
> This command displays information about IPv6 interfaces. If no interface name is specified then information for IPv6 interfaces is displayed.
> summary: Displays a summary of the interface information.
> name interface_name: Displays information for the IPv6 interface specified. Must be followed by an interface_name.
> statistics: Includes the number on inbound and outbout IP packets statistics that were registered by the kernel in the information displayed.
> neighbors
> Displays the neighbor discovery table for this context.
> route route_ip_address
> Indicates the route information to the address specified by route_ip_address is to be displayed. The route gateway address may be specified as needed to identify the route. route_ip_address using colon ( : ) separated notation.
> Usage
> Show the IPv6 information to verify and/or troubleshoot communication difficulties between to a remote host/node.
> Example
> The following command displays the ACL for the list named sampleACL.
> show ipv6 access-list samplev6ACL
> The following command displays the interface information, including statistics, for the IPv6 interface samplev6Interface.
> show ipv6 interface samplev6Interface statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ipv6 pool
> Displays information for ipv6 pools.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 pools [ name ipv6 pool name|group-name name| { grep grep_options | more } ]
> name ipv6 name
> Displays information for a specified ipv6 pool.
> group-name name
> Displays information for a specified IPv6 pools group.
> name is the name of the group of IPv6 pool and must be a string having 1 to 79 alpha and/or numeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to see all the ipv6 pools.
> Example
> The following command displays ipv6 pool information:
> show ipv6 pools
> show iups-service
> This command displays information for Iu-PS services in the current context.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show iups-service { all | name srvc_name }[ rnc { all | mcc mcc_num mnc mnc_num | rnc_id } ]
> all
> Show information for all IuPS services.
> name srvc_name
> srvc_name: must be a string of 1 to 63 alphanumeric characters that identifies a specific existing IuPS service.
> rnc all
> Displays information for all configured RNCs.
> rnc mcc mcc_num mnc mnc_num
> Displays information for a specific RNC.

> • | mcc_num: The Mobile Country Code (MCC) of the RNC. Must be a 3 digit integer from 200 through 999.

> • | mnc_num: The Mobile Network Code (MNC) of the RNC. Must be a 2 or 3 digit integer from 00 through 999.

> rnc rnc_id
> rnc_id: The identification number of the RNC configuration instance. Must be an integer from 0 to 4095.
> Usage
> Use this command to display information for a specific Iu-PS service or for all Iu-PS services configured within the context. It is also possible, but not required, to fine-tune the display to only provide information for a specific RNC.
> Iu-PS services control the interface between the SGSN and the RNCs in the UMTS Radio Access Network (UTRAN). Iu-PS services include the control plane and the data plane between these nodes.
> Example
> The following command displays information for a single Iu-PS service named iups-svc-1:
> show iups-service name iups-svc-1
> The next command displays information for all Iu-PS services configured in the current context:
> show iups-service all
> This command displays information for a specific RNC for a specific Iu-PS services:
> show iups-service name iups-svc-1 rnc 123
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp sessions
> Displays information for L2TP tunnels.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> full
> Shows all available information for the specified sessions.
> summary
> Shows a summary of available information for the specified sessions.
> counters
> Shows counters for the specified L2TP sessions.
> all
> Shows all current sessions.
> callid id
> Show session information for the specified call id. The output of the command show l2tp tunnels contains a field labeled Callid Hint which lists the call id information to use with this command. This is an 8-Byte Hexadecimal number.
> username name
> Shows session information for the specified subscriber. username has a string length of 1 to 127 characters. Wildcard characters $ and * are allowed.
> msid ms_id
> Shows session information for the mobile user identified by ms_id. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed.
> lac-service service_name
> Shows all L2TP sessions in the specified LAC service.
> lns-service service_name
> Shows all L2TP sessions in the specified LNS service.
> peer-address [ operator ] peer_address
> Shows all L2TP sessions to the destination (peer LNS) at the specified IP address. The peer_address must be specified using the standard IPv4 dotted decimal notation.
> In conjunction with sessions keyword, indicates a range of peers is to be displayed.
> peer-address [ operator ] peer_address must be specified using the standard IPv4 dotted decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than to specified peer_address

> • | >: IP address less than to specified peer_address

> • | greater-than: IP address less than to specified peer_address

> • | less-than: IP address less than to specified peer_address

> Usage
> Use this command to show information for sessions in the current context.
> Important: If this command is executed from within the local context, cumulative session information is displayed for all contexts.
> Example
> The following command displays cumulative statistics for all sessions processed within the current context:
> show l2tp sessions
> The following command displays all information pertaining to the L2TP session of a subscriber named isp1vpnuser1:
> show l2tp session full username isp1vpnuser1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp statistics
> Displays statistics for all L2TP tunnels and sessions.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> lac-service service_name
> Shows L2TP statistics for all tunnels and sessions in the specified LAC service.
> lns-service service_name
> Shows L2TP statistics for all tunnels and sessions in the specified LNS service.
> peer-address peer_address
> Shows L2TP statistics for all tunnels and sessions to the destination (peer LNS) at the specified IP address. The peer_address must be specified using the standard IPv4 dotted decimal notation.
> Usage
> Use this command to display statistics for L2TP services.
> Example
> The following command displays statistics for a specific LAC service named vpn1:
> show l2tp statistics lac-service service_name
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp tunnels
> Displays information for L2TP tunnels.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> full
> Shows all available information for the specified tunnels.
> summary
> Shows a summary of available information for the specified tunnels.
> counters
> Shows counters for the specified L2TP tunnels.
> all
> Shows all current tunnels.
> callid id
> Show tunnel information for the specified call id. The output of the command show l2tp tunnels contains a field labeled Callid Hint which lists the call id information to use with this command. This is an 8-Byte Hexadecimal number.
> username name
> Shows tunnel information for the specified subscriber. username has a string length of 1 to 127 characters. Wildcard characters $ and * are allowed.
> msid ms_id
> Shows tunnel information for the mobile user identified by ms_id. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed.
> lac-service service_name
> Shows all L2TP tunnels in the specified LAC service.
> lns-service service_name
> Shows all L2TP tunnels in the specified LNS service.
> peer-address [ operator ] peer_address
> Shows all L2TP tunnels to the destination (peer LNS) at the specified IP address. The peer_address must be specified using the standard IPv4 dotted decimal notation.
> In conjunction with tunnels keyword, indicates a range of peers is to be displayed.
> peer-address [ operator ] peer_address must be specified using the standard IPv4 dotted decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than to specified peer_address

> • | >: IP address less than to specified peer_address

> • | greater-than: IP address less than to specified peer_address

> • | less-than: IP address less than to specified peer_address

> Usage
> Use this command to show information for tunnels in the current context.
> Example
> The following command displays all of the tunnels currently being facilitated by LAC services within the current context:
> show l2tp tunnels all
> The following command displays information pertaining to the L2TP tunnel(s) established for a LAC-service named vpn1:
> show l2tp tunnels full lac-service vpn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show lawful-intercept
> Displays information on sessions that are currently being lawfully intercepted.
> Product
> PDSN, HA, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, or Inspector that have li-administrator privileges.
> Syntax
> show lawful-intercept [ full ] { [ all ] [ imsi imsi_value ] [ intercept-id li_id ] [ ip-addr intercept_ip_addr ] [ msid ms_id] [ username subscriber_name ] | statistics }
> full
> Display full detailed information.
> all
> Display information for all lawful intercepts.
> imsi imsi_value
> Specifies the International Mobile Subscriber Identity (IMSI) of the intercepted subscriber session.
> imsi_value is an integer value from 1 to 15 characters.
> ipaddr intercept_ip_addr
> Specifies the IP address of the intercepted subscriber session.
> intercept_ip_addr must be specified using dotted decimal notation.
> msid ms_id
> Specifies the mobile subscriber identification number of the intercepted subscriber session.
> ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> username subscriber_name
> Specifies the username of the intercepted subscriber.
> subscriber_name refers to a previously configured user.
> statistics
> Display summary statistical information for all Lawful Intercept sessions.
> Usage
> Use this command to display lawful intercept statistics.
> Important: You must log in to the system through a Secure Shell (SSH) using a system account that has li-administrator privileges to use this command. For details on using the Lawful Intercept capability of the system, refer to System Administration and Configuration Guide.
> Example
> To show detailed information for a lawfully intercepted session with the MSID 0000100048, enter the following command
> show lawful-intercept full msid 0000100048
> show lac-service
> Displays the information for all LAC services or for a particular LAC service.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show lac-service { all | name service_name } [ | { grep grep_options | more } ]
> all
> Display information for all LAC services.
> name service_name
> Display information only for the LAC service specified by service_name.
> service_name is up to a 60 character name given to the service when it was originally configured.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to list information for LAC services configured on this system.
> Example
> The following commands display information for all LAC services and the LAC service named lac1, respectively.
> show lac-service allshow lac-service name lac1
> show leds
> Displays the current status of the LEDs for a specific card or all cards.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show leds { all | card_num } [ | { grep grep_options | more } ]
> all | card_num
> all: indicates the LED status for all cards is to be displayed.
> card_num: indicates the LED status for the card specified by card_num is to be displayed.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Display the status of the LEDs as a part of an automated periodic script which checks the LEDs of the chassis.
> Important: This command is not supported on all platforms.
> Example
> The following commands display the LED status for all cards and only card 8, respectively.
> show leds all
> Important: Refer to the descriptions for Card LEDs and System LEDs in show card info command in the Counters and Statistics Reference for information on the LED color codes.
> show license information
> Displays the installed license information as well as maximum number of sessions.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show licenseinformation { key_name | full} | { key } [ | { grep grep_options | more } ]
> key_name | full
> key_name: the output displays the information for the key specified as key_name.
> full: the output displays the full features and quantities without any hardware limits in place.
> key:
> indicates the output is to display the installed keys in encrypted format.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Show the license information to verify the proper keys have been installed. This command is also helpful in troubleshooting user system access due to the maximum number of sessions being reached.
> Example
> The following displays the encrypted installed key and the information for sampleKey respectively.
> show license information
> show linecard table
> Displays information on the rear-installed interface cards.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show linecard table [ | { grep grep_options | more } ]
> table
> Displays information on all linecard slots in tabular format.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Show the line card information to verify hardware inventories and installed components.
> Important: This command is not supported on all platforms.
> Example
> show linecard table
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show lma-service
> Displays statistic and counter information for Local Mobility Anchor (LMA) services on this system.
> Product
> P-GW
> Privilege
> Inspector
> Syntax
> show lma-service all
> show lma-service name service_name
> show lma-service session [ all | callid id | counters | full | ipv6-address { <address | >address | address | greater-than address [ less-than address ] | less-than address [ greater-than address ] } | summary | username name ]
> show lma-service statistics [ lma-service name ] } [ | { grep grep_options | more } ]
> all
> Displays information about all configured LMA services on this system.
> name service_name
> Displays configuration information for a specific LMA service configured on this system.
> service_name must be an existing LMA service, and be from 1 to 63 alpha and/or numeric characters in length.
> session [ all | callid id | counters | full | ipv6-address { < address | > address | address | greater-than address [ less-than address ] | less-than address [ greater-than address ] } | summary | username name ]
> Displays session information filtered by the following parameters:
> all: Displays all active LMA sessions using LMA services on the system.
> callid id: Displays available session information for the specific call identification number. id must be an eight-digit HEX number.
> counters: Displays session counters for active LMA sessions using LMA services on the system. This keyword can also be filtered by the following:

> • | all

> • | callid

> • | ipv6-address

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> full: Displays additional session information for active LMA sessions using LMA services on the system. This keyword includes the information in the output of the ‘all’ keyword plus additional information. This keyword can also be filtered by the following:

> • | all

> • | callid

> • | ipv6-address

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> ipv6-address:

> • | < address and less-than adress: Displays summary information for a group of IPv6 addresses that are less than the specified IPv6 address using one of these keywords. A range can be specified by including an address with the greater-than option. address must be specified in colon separated notation.

> • | > address and greater-than address: Displays summary information for a group of IPv6 addresses that are greater than the specified IPv6 address using one of these keywords. A range can be specified by including an address with the less-than option. address must be specified in colon separated notation.

> • | address: Displays summary information for a specific IPv6 address using an LMA service on this system. address must be specified in colon separated notation.

> summary: Displays the number of LMA sessions currently active for LMA services configured on the system.
> username name: Displays available session information for a specific user in a service session. name must be followed by an existing user name and must be from 1 to 127 alpha and/or numeric characters.
> statistics [ lma-service name ]
> lma-service name: Displays LMA service statistics for a specific LMA service. name must be an existing LMA srvice and be from 1 to 63 alpha and/or numeric characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for LMA services on this system.
> Example
> The following command displays service statistics for the LMA service named lma1:
> show lma-service name lma1
> show lns-service
> Displays the information for all LNS services or for a particular LNS service.
> Product
> PDSN, HA, GGSN, LNS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show lns-service { all | name service_name } [ | { grep grep_options | more } ]
> all
> Display information for all LNS services.
> name service_name
> Display information only for the LNS service specified by service_name.
> service_name is up to a 60 character name given to the service when it was originally configured.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to list information for LNS services configured on this system.
> Example
> The following commands display information for all LNS services and the LNS service named lns1, respectively.
> show lns-service allshow lns-service name lns1
> show local-user
> Displays information pertaining to local-user accounts.
> Product
> All
> Privilege
> Security Administrator
> Syntax
> show local-user [ [ username name ] [ inactive filter ] [ verbose | wide ] | statistics [ verbose ] ]
> username name
> Specifies the name of a specific local-user administrative account for which to display information.
> name can be from 3 to 16 alpha and/or numeric characters in length and is case sensitive.
> inactive filter
> Specifies a filter for displaying inactive local-user accounts. filter can be one of the following:

> • | < days : Displays accounts that have been inactive less than the specified number of days.

> • | > days : Displays accounts that have been inactive more than the specified number of days.

> • | greater-than days : Displays accounts that have been inactive more than the specified number of days.

> • | less-than days : Displays accounts that have been inactive less than the specified number of days.

> days can be configured to any integer value from 1 to 365.
> [ verbose | wide ]
> Default: wide
> Specifies how the information is to be displayed as one of the following options:

> • | verbose : The data is displayed in list format. Additional information is provided beyond what is displayed when the wide option is used.

> • | wide : The data is displayed in tabular format.

> statistics [ verbose ]
> Displays local-user statistics.
> Using the verbose keyword displays additional statistics.
> Usage
> Use this command to display information and statistics on local-user administrative accounts.
> Example
> The following command displays detailed information on local-user administrative accounts that have been inactive for more than 10 days:
> show local-user inactive greater-than 10 verbose
> The following command displays detailed information for a local-user account named Test:
> show local-user username Test verbose
> The following command displays detailed local-user account statistics:
> show local-user statistics verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show logging
> Displays the defined logging filters for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show logging [ active | verbose ] [ | { grep grep_options | more } ]
> active | verbose
> Default: all facilities are shown in concise form.
> active: indicates only the active CLI logging filter information is to be displayed.
> verbose: indicates the output should provide as much information as possible.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View log filters to trouble shoot disk utilization issues.
> Example
> show logging
> show logging active
> show logging verbose
> show logging active verbose
> show logs
> Displays active and inactive logs filtered by the options specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show logs [ active ] [ inactive ] [ callid call_id ] [ event-verbosity evt_verboseness] [ facility facility ] [ level severity_level ] [ pdu-data pdu_format ] [ pdu-verbosity pdu_verboseness ] [ proclet facility ] [ since from_date_time [ until to_date_time ] ] [ | { grep grep_options | more } ]
> active
> Indicates output is to display data from active logs.
> inactive
> Indicates output is to display data from inactive logs.
> callid call_id
> Specifies a call ID for which log information is to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> event-verbosity evt_verboseness
> Specifies the level of verboseness to use in displaying of event data as one of:

> • | min - displays minimal information about the event. Information includes event name, facility, event ID, severity level, date, and time.

> • | concise - displays detailed information about the event, but does not provide the event source within the system.

> • | full - displays detailed information about event, including source information, identifying where within the system the event was generated.

> facility facility
> Specifies the facility to modify the filtering of logged information for as one of:

> • | a10: A10 interface facility

> • | a11: A11 interface facility

> • | a11mgr: A11 Manager facility

> • | aaa-client: AAA client facility

> • | aaamgr: AAA manager logging facility

> • | aaaproxy: AAA Proxy facility

> • | acl-log: Access Control List logging facility

> • | acsctrl: Active Charging Service (ACS) Controller facility

> • | acsmgr: Active Charging Service (ACS) Manager facility

> • | alarmctrl: Alarm Controller facility

> • | all: All facilities

> • | asf: Voice Application Server Framework logging facility

> • | asfprt: ASF Protocol Task (SIP) logging facility

> • | asngwmgr: ASN Gateway Manager facility

> • | asnpcmgr: ASN Paging Controller/Location-Registry Manager facility

> • | bgp: Border Gateway Protocol (BGP) facility

> • | cli: CLI logging facility

> • | cscf: IMS/MMD CSCF

> • | cscfmgr: SIP CSCF Manager facility

> • | csp: Card Slot Port controller facility

> • | css: Content Service Selection (CSS) facility

> • | css-sig: Content Service Selection (CSS) RADIUS Signaling facility

> • | dcardctrl: IPSEC Daughtercard Controller logging facility (not used at this time)

> • | dcardmgr: IPSEC Daughtercard Manager logging facility (Not used at this time)

> • | dhcp: DHCP facility (GGSN product only)

> • | dhost: Distributed Host logging facility

> • | diameter: Diameter endpoint logging facility

> • | diameter-acct: Diameter Accounting

> • | diameter-auth: Diameter Authentication

> • | diameter-ecs: ECS Diameter signaling facility

> • | diameter-svc: Diameter Service

> • | diamproxy: DiamProxy logging facility

> • | dpath: IPSEC Data Path facility

> • | drvctrl: Driver Controller facility

> • | egtpc: eGTP-C logging facility

> • | egtpmgr: eGTP manager logging facility

> • | evlog: Event log facility

> • | famgr: Foreign Agent manager logging facility

> • | firewall: Firewall logging facility

> • | gss-gcdr: GTPP Storage Server GCDR facility

> • | gtpc: GTP-C protocol logging facility (GGSN product only)

> • | gtpcmgr: GTP-C protocol Manager logging facility (GGSN product only)

> • | gtpp: GTP-PRIME protocol logging facility (GGSN product only)

> • | gtpu: GTP-U protocol logging facility (GGSN product only)

> • | h248prt: H.248 Protocol logging facility

> • | hamgr: Home Agent manager logging facility

> • | hat: High Availability Task (HAT) process facility

> • | ims-authorizatn: IMS Authorization Service facility

> • | ip-arp: IP Address Resolution Protocol facility

> • | ip-interface: IP interface facility

> • | ip-route: IP route facility

> • | ipsec: IP Security logging facility

> • | ipsgmgr: IP Services Gateway facility

> • | ipsp: IP Pool Sharing Protocol logging facility

> • | l2tp-control: L2TP control logging facility

> • | l2tp-data: L2TP data logging facility

> • | l2tpdemux: L2TP Demux Manager logging facility

> • | l2tpmgr: L2TP Manager logging facility

> • | li: Lawful intercept facility (Logs are visible only to system accounts with li-administrator privileges.)

> • | magmgr: Mobile Access Gateway manager logging facility

> • | mme-app: Mobility Management Entity Application logging facility

> • | mmedemux: Mobility Management Entity Demux Manager logging facility

> • | mme-hss: Mobility Management Entity logging facility

> • | mme-misc: Mobility Management Entity Miscellaneous logging facility

> • | mobile-ip: Mobile IP processes

> • | mobile-ip-data: Mobile IP data facility

> • | mobile-ipv6: Mobile IPv6 logging facility

> • | multicast-proxy: Multicast Proxy logging facility

> • | nas: Network Access Signaling logging facility

> • | netwstrg: Network Storage facility

> • | npuctrl: Network Processor Unit Control facility

> • | npumgr: Network Processor Unit Manager facility

> • | nsctrl: Charging Service Controller facility (supported in conjunction with ECSv1)

> • | nsmgr: Charging Service Manager facility

> • | nsproc: Charging Service process facility

> • | orbs: Object Request Broker System logging facility

> • | ospf: OSPF logging facility

> • | pgw: PDN Gateway logging facility

> • | ppp: PPP link and packet facilities

> • | radius-acct: RADIUS accounting logging facility

> • | radius-auth: RADIUS authentication logging facility

> • | radius-coa: RADIUS change of authorization and radius disconnect

> • | rct: Recovery Control Task logging facility

> • | rdt: Redirect Task logging facility

> • | resmgr: Resource Manager logging facility

> • | rip: RIP logging facility (RIP is not supported at this time.)

> • | rohc: RObust Header Compression facility

> • | rsvp: Reservation Protocol logging facility

> • | sct: Shared Configuration Task logging facility

> • | sessctrl: Session Controller logging facility

> • | sessmgr: Session Manager logging facility

> • | sft: Switch Fabric Task logging facility

> • | sgw: Serving Gateway logging facility

> • | sipcdprt: Sip Call Distributor facility

> • | sitmain: System Initialization Task main logging facility

> • | snmp: SNMP logging facility

> • | srdb: Static Rating Database

> • | srp: Service Redundancy Protocol (SRP) logging facility

> • | ssh-ipsec: SSH IP Security logging facility stat: Statistics logging facility

> • | stat: Statistics logging facility

> • | system: System logging facility

> • | tacacsplus: TACACS+ Protocol logging facility

> • | threshold: threshold logging facility

> • | udr: User detail record facility (used with the Charging Service)

> • | user-data: User data logging facility

> • | user-l3tunnel: User layer-3 tunnel logging facility

> • | vpn: Virtual Private Network logging facility

> • | wimax-data: WiMAX DATA

> • | wimax-r6: WiMAX R6

> level severity_level
> level severity_level: specifies the level of information to be logged, severity_level, from the following list which is ordered from highest to lowest:

> • | critical - display critical events

> • | error - display error events and all events with a higher severity level

> • | warning - display warning events and all events with a higher severity level

> • | unusual - display unusual events and all events with a higher severity level

> • | info - display info events and all events with a higher severity level

> • | trace - display trace events and all events with a higher severity level

> • | debug - display all events

> pdu-data pdu_format
> Specifies output format for the display of packet data units as one of:

> • | none - output is in raw format (unformatted).

> • | hex - output being displayed in hexadecimal format.

> • | hex-ascii - output being displayed in hexadecimal and ASCII similar to a main-frame dump.

> pdu-verbosity pdu_verboseness
> Specifies the level of verboseness to use in displaying of packet data units as a value from 1 to 5 where 5 is the most detailed.
> proclet facility
> Shows the logs from a specific proclet facility. The available facilities are the same as those listed earlier.
> since from_date_time [ until to_date_time ]
> Default: no limit.
> since from_date_time: indicates only the log information which has been collected more recently than from_date_time is to be displayed.
> until to_date_time: indicates no log information more recent than to_date_time is to be displayed. until defaults to current time when omitted.
> from_date_time and to_date_time must be formatted as YYYY:MM:DD:HH:mm or YYYY:MM:DD:HH:mm:ss. Where YYYY is a 4-digit year, MM is a 2-digit month in the range 01 through 12, DD is a 2-digit day in the range 01 through 31, HH is a 2-digit hour in the range 00 through 23, mm is a 2-digit minute in the range 00 through 59, and ss is a 2 digit second in the range 00 through 59.
> to_date_time must be a time which is more recent than from_date_time.
> The use of the until keyword allows for a time range of log information while only using the since keyword will display all information up to the current time.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View log files for general maintenance or troubleshooting system issues.
> Example
> The following commands display log information for the a11mgr facility starting with February 20th, 2003 at midnight where both are equivalent.
> show logs facility a11mgr since 2003:02:20:00:00
> show logs facility a11mgr since 2003:02:20:00:00:00
> The following command displays the log information for call ID FE881D32 only in active logs.
> show logs active callid FE881D32

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883