> Crypto Map IKEv2-IPv6 Payload Configuration Mode Commands
> The Crypto Map IKEv2-IPv6 Payload Configuration Mode is used to assign the correct IPsec transform-set from a list of up to four different transform-sets, and to assign Mobile IP addresses.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.
> ipsec
> Configures the IPsec transform set to be used for this crypto template payload.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> ipsec transform-set list name
> no ipsec transform-set list
> list name
> Specifies the context configured IPsec transform set name to be used in the crypto template payload. This is a space-separated list. From 1 to 4 transform sets can be entered. name must be from 1 to 127 alpha and/or numeric characters.
> Usage
> Use this command to list the IPsec transform set(s) to use in this crypto template payload.
> Example
> The following command configures IPsec transform sets named ipset1 and ipset2 to be used in this crypto template payload:
> ipsec transform-set list ipset1 ipset2
> lifetime
> Configures the number of seconds for IPsec Child SAs derived from this crypto template payload to exist.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> lifetime sec [ kilobytes kbytes ]
> default lifetime
> default
> Returns the lifetime value to the default setting of 86400.
> sec
> Default: 86400
> Specifies the number of seconds for IPsec Child Security Associations derived from this crypto template payload to exist. sec must be an integer from 60 to 604800.
> kilobytes kbytes
> Specifies lifetime in kilo-bytes for IPsec Child Security Associations derived from this Crypto Map. kbytes must be an integer value from 1 to 2147483648.
> Usage
> Use this command to configure the number of seconds for IPsec Child Security Associations derived from this crypto template payload to exist.
> Example
> The following command configures the IPsec child SA lifetime to be 120 seconds:
> lifetime 120
> rekey
> Configures child security association rekeying.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> rekey [ keepalive ]
> [ default | no ] rekey
> default
> Returns the feature to the default setting of disabled.
> no
> Disables this feature.
> keepalive
> If specified, a session will be rekeyed even if there has been no data exchanged since the last rekeying operation. By default rekeying is only performed if there has been data exchanged since the previous rekey.
> Usage
> Use this command to enable or disable the ability to rekey IPsec Child SAs after approximately 90% of the Child SA lifetime has expired. The default, and recommended setting, is not to perform rekeying. No rekeying means the PDIF will not originate rekeying operations and will not process CHILD SA rekeying requests from the MS.
> Example
> The following command disables rekeying:
> no rekey

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883