> Network Service Entity - Peer NSEI Configuration Mode Commands
> The Network Service Entity (NSE) - Peer NSEI configuration mode configures the Frame Relay parameters for the peer NSE. This mode is a sub-mode of the Global Configuration mode. This sub-mode provides the commands and parameters to define the management functionality for the Gb interface between a BSS and an SGSN over a 2.5G GPRS Frame Relay network connection.
> Upon accessing this mode, the prompt should be similar to:
> [local]asn5000(nse-fr-peer-nsei-2344)# where the 2344 represents a user-defined instance.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> bssgp-timer
> This command has been deprecated.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the previous configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the global configuration mode.
> ns-vc
> This command creates a network service virtual circuit (NSVC) for this frame relay NSE and enters the configuration sub-mode to define the NSVC parameters. These parameters are described in the NSVC Configuration Mode chapter elsewhere in this CLI Reference Guide.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] ns-vc id ns-vc_id
> no
> Removes the specified NSVC configuration.
> id ns-vc_id
> This keyword defines the NSVC configuration identifier.
> ns-vc_id: Must be an integer from 0 to 65535
> Usage
> Access the NSVC configuration mode.
> Example
> Gain access to the NSVC configuration mode to change the 4th instance.
> ns-vc id 4

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883