> APN Schema Statistics
> The APN schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> APN Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the APN configuration. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the APN configuration. This is an internal reference number. | Counter / Int32
> apn | The name of the APN for which statistics are displayed. | String
> uplnk-bytes | The number of bytes sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int64
> dnlnk-bytes | The number of bytes sent from the APN towards MS on the GTP interface. | Counter / Int64
> uplnk-pkts | The number of IP packets sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> dnlnk-pkts | The number of IP packets sent from the APN towards MS on the GTP interface. | Counter / Int32
> uplnk-bytes-drop | The number of bytes sent from the APN towards Internet/PDN on the Gi interface dropped. | Counter / Int64
> dnlnk-bytes-drop | The number of bytes sent from the APN towards MS on the GTP interface dropped. | Counter / Int64
> uplnk-drop | The number of IP packets sent from the APN towards Internet/PDN on the Gi interface dropped. | Counter / Int32
> dnlnk-drop | The number of IP packets sent from the APN towards MS on the GTP interface dropped. | Counter / Int32
> bad-hdr | The total number of IP packets received and dropped due to bad header. | Counter / Int32
> ttl-excd | The number of IP packets dropped because they were received with a TTL value of 0. | Counter / Int32
> frag-sent | The number of times IP packets were fragmented before sending on the GTP tunnel. | Counter / Int32
> frag-fail | The number of packets which failed in fragmentation. | Counter / Int32
> inacl-drop | The number of IP packets received that were dropped due to ACL filtering. | Counter / Int32
> outacl-drop | The number of outbound IP packets that were dropped due to ACL filtering. | Counter / Int32
> inexcd-mbr-pkt-drop | Data Statistics – IP input excd MBR packets dropped | Counter / Int32
> outexcd-mbr-pkt-drop | Data Statistics – IP output excd MBR packets dropped | Counter / Int32
> inexcd-gbr-pkt-drop | Data Statistics – IP input excd GBR packets dropped | Counter / Int32
> outexcd-gbr-pkt-drop | Data Statistics – IP output excd GBR packets dropped | Counter / Int32
> inexcd-ambr-pkt-drop | Data Statistics – IP in excd APN packets AMBR dropped | Counter / Int32
> outexcd-ambr-pkt-drop | Data Statistics – IP out excd APN packets AMBR dropped | Counter / Int32
> inmisc-pkt-drop | Data Statistics – IP input misc packets dropped | Counter / Int32
> outmisc-pkt-drop | Data Statistics – IP output misc packets dropped | Counter / Int32
> inexcd-mbr-byte-drop | Data Statistics – IP input excd MBR bytes dropped | Counter / Int64
> outexcd-mbr-byte-drop | Data Statistics – IP output excd MBR bytes dropped | Counter / Int64
> inexcd-gbr-byte-drop | Data Statistics – IP input excd GBR bytes dropped | Counter / Int64
> outexcd-gbr-byte-drop | Data Statistics – IP output excd GBR bytes dropped | Counter / Int64
> inexcd-ambr-byte-drop | Data Statistics – IP in excd APN AMBR bytes dropped | Counter / Int64
> outexcd-ambr-byte-drop | Data Statistics – IP out excd APN AMBR bytes dropped | Counter / Int64
> inmisc-byte-drop | Data Statistics – IP input misc bytes dropped | Counter / Int64
> outmisc-byte-drop | Data Statistics – IP output misc bytes dropped | Counter / Int64
> bad-src-addr | The number of IP packets received for which a source violation was detected resulting in the packets being dropped. | Counter / Int32
> addr-stat | The total number of PDP contexts facilitated by the APN that used static IP addresses. | Counter / Int32
> addr-lpool | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from pools configured locally. | Counter / Int32
> addr-rad | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from a RADIUS server. | Counter / Int32
> addr-dhcp | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from DHCP. | Counter / Int32
> addr-dhcp-rly | The total number of PDP contexts facilitated by the APN that were allocated IP addresses by DHCP Relay. | Counter / Int32
> addr-no-alloc | The total number of PDP contexts facilitated by the APN that were not allocated IP addresses. | Counter / Int32
> sess-curr | The number of PDP contests currently facilitated by the APN. | Counter / Int32
> sess-curr-all | The total number of PDP contexts currently being facilitated by the entire system. | Counter / Int32
> sess-tot | The total number of PDP contexts facilitated by the APN. | Counter / Int32
> sess-tot-all | The total number of PDP contexts that have been facilitated by the entire system. | Counter / Int32
> att-pdp-ctxt | The total CPC req per APN | Counter / Int32
> att-deact-pdp-ggsn | The total DPC Req Tx per APN | Counter / Int32
> succ-deact-pdp-ggsn | The total DPC Req Tx Accepted | Counter / Int32
> att-deact-pdp-ms | The total DPC Req Rx per APN | Counter / Int32
> succ-deact-pdp-ms | The total Deactivate PDP Context Req successful from MS. | Counter / Int32
> dyn-ipv4-attempt | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were attempted. | Counter / Int32
> dyn-ipv6-attempt | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were attempted. | Counter / Int32
> dyn-ipv4-success | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. | Counter / Int32
> dyn-ipv6-success | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. | Counter / Int32
> data-fromuseravg-bps | The average data rate in bits per seconds (bps) from the user. | Counter / Int64
> data-touseravg-bps | The average data rate in bps towards the user. | Counter / Int64
> data-fromusersust-bps | The sustained data rate in bps from the user. | Counter / Int64
> data-tousersust-bps | The sustained data rate in bps towards the user. | Counter / Int64
> data-fromuseravg-pps | The average data rate in packets per seconds (pps) from the user. | Counter / Int64
> data-touseravg-pps | The average data rate in pps towards the user. | Counter / Int64
> data-fromusersust-pps | The sustained data rate in pps from the user. | Counter / Int64
> data-tousersust-pps | The sustained data rate in pps towards the user. | Counter / Int64
> qosconv-pkts-uplnk | The number of packets with Conversational QoS sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosconv-pkts-dnlnk | The number of packets with Conversational QoS sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosstrm-pkts-uplnk | The number of packets with Streaming QoS sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosstrm-pkts-dnlnk | The number of packets with Streaming QoS sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosint1-pkts-uplnk | The number of packets with Interactive QoS for priority 1 sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosint1-pkts-dnlnk | The number of packets with Interactive QoS for priority 1 sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosint2-pkts-uplnk | The number of packets with Interactive QoS for priority 2 sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosint2-pkts-dnlnk | The number of packets with Interactive QoS for priority 2 sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosint3-pkts-uplnk | The number of packets with Interactive QoS for priority 3 sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosint3-pkts-dnlnk | The number of packets with Interactive QoS for priority 3 sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosint-pkts-uplnk | Total number of packets with Interactive QoS for all priorities (priority 1, 2, and 3) sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosint-pkts-dnlnk | Total number of packets with Interactive QoS for all priorities (priority 1, 2, and 3) sent from the APN towards MS on the GTP interface. | Counter / Int32
> qosback-pkts-uplnk | The number of packets with Background QoS sent from the APN towards Internet/PDN on the Gi interface. | Counter / Int32
> qosback-pkts-dnlnk | The number of packets with Background QoS sent from the APN towards MS on the GTP interface. | Counter / Int32
> auth-req-sent | The total authentication requests sent from the APN towards AAA on Ga interface. | Counter / Int32
> auth-acc-rcvd | The total authentication accept messages received by the APN on Ga Interface from AAA. | Counter / Int32
> auth-timeout | The total authentication requests that timed out. | Counter / Int32
> acc-req-sent | The total accounting requests sent from the APN towards AAA on Ga interface. | Counter / Int32
> acc-rsp-rcvd | The total accounting response messages received by the APN on Ga Interface from AAA. | Counter / Int32
> acc-req-timeout | The total accounting requests that timed out. | Counter / Int32
> act-defbear | The total number of active default bearers. | Counter / Int32
> act-dedbear | The total number of active dedicated bearers. | Counter / Int32
> setup-defbear | The total number of default bearers setup. | Counter / Int32
> setup-dedbear | The total number of dedicated bearers setup. | Counter / Int32
> rel-defbear | The total number of released default bearers. | Counter / Int32
> rel-dedbear | The total number of released dedicated bearers. | Counter / Int32
> rel-fail-defbear | The total number of default bearers with release failures. | Counter / Int32
> rel-fail-dedbear | The total number of dedicated bearers with release failures. | Counter / Int32
> rej-defbear | The total number of rejected default bearers. | Counter / Int32
> rej-dedbear | The total number of rejected dedicated bearers. | Counter / Int32
> mod-uebear | The total number of UE-initiated modified bearers. | Counter / Int32
> mod-nwbear | The total number of network-initiated modified bearers. | Counter / Int32
> ue-init-modfail | The total number of failed UE-initiated modified bearers. | Counter / Int32
> nw-init-modfail | The total number of failed network-initiated modified bearers. | Counter / Int32
> pdn-ipv4-actsess | The total number of active IPv4 sessions. | Counter / Int32
> pdn-ipv4-setupsess | The total number of IPv4 session setup. | Counter / Int32
> pdn-ipv4-relsess | The total number of released IPv4 sessions. | Counter / Int32
> pdn-ipv6-actsess | The total number of active IPv6 sessions. | Counter / Int32
> pdn-ipv6-setupsess | The total number of IPv6 session setup. | Counter / Int32
> pdn-ipv6-relsess | The total number of released IPv6 sessions. | Counter / Int32
> pdn-ipv4v6-actsess | The total number of active IPv4-in-IPv6 sessions. | Counter / Int32
> pdn-ipv4v6-setupsess | The total number of IPv4-in-IPv6 session setup. | Counter / Int32
> pdn-ipv4v6-relsess | The total number of released IPv4-in-IPv6 sessions. | Counter / Int32
> addr-ipv6-stateless-autocnf | The total number of allocated IPv6 addresses from stateless auto-configuration. | Counter / Int32
> qci1-actbear | The total number of QCI1 active bearers. | Counter / Int32
> qci1-setupbear | The total number of QCI1 bearers setup. | Counter / Int32
> qci1-relbear | The total number of QCI1 released bearers. | Counter / Int32
> qci1-uplinkpkt-fwd | The total number of QCI1 uplink packets forwarded. | Counter / Int32
> qci1-dwlinkpkt-fwd | The total number of QCI1 downlink packets forwarded. | Counter / Int32
> qci1-uplinkbyte-fwd | The total number of QCI1 uplink bytes forwarded. | Counter / Int64
> qci1-dwlinkbyte-fwd | The total number of QCI1 downlink bytes forwarded. | Counter / Int64
> qci1-uplinkpkt-drop | The total number of QCI1 uplink packets dropped. | Counter / Int32
> qci1-dwlinkpkt-drop | The total number of QCI1 downlink packets dropped. | Counter / Int32
> qci1-uplinkbyte-drop | The total number of QCI1 uplink bytes dropped. | Counter / Int64
> qci1-dwlinkbyte-drop | The total number of QCI1 downlink bytes dropped. | Counter / Int64
> qci2-actbear | The total number of QCI2 active bearers. | Counter / Int32
> qci2-setupbear | The total number of QCI2 bearers setup. | Counter / Int32
> qci2-relbear | The total number of QCI2 released bearers. | Counter / Int32
> qci2-uplinkpkt-fwd | The total number of QCI2 uplink packets forwarded. | Counter / Int32
> qci2-dwlinkpkt-fwd | The total number of QCI2 downlink packets forwarded. | Counter / Int32
> qci2-uplinkbyte-fwd | The total number of QCI2 uplink bytes forwarded. | Counter / Int64
> qci2-dwlinkbyte-fwd | The total number of QCI2 downlink bytes forwarded. | Counter / Int64
> qci2-uplinkpkt-drop | The total number of QCI2 uplink packets dropped. | Counter / Int32
> qci2-dwlinkpkt-drop | The total number of QCI2 downlink packets dropped. | Counter / Int32
> qci2-uplinkbyte-drop | The total number of QCI2 uplink bytes dropped. | Counter / Int64
> qci2-dwlinkbyte-drop | The total number of QCI2 downlink bytes dropped. | Counter / Int64
> qci3-actbear | The total number of QCI3 active bearers. | Counter / Int32
> qci3-setupbear | The total number of QCI3 bearers setup. | Counter / Int32
> qci3-relbear | The total number of QCI3 released bearers. | Counter / Int32
> qci3-uplinkpkt-fwd | The total number of QCI3 uplink packets forwarded. | Counter / Int32
> qci3-dwlinkpkt-fwd | The total number of QCI3 downlink packets forwarded. | Counter / Int32
> qci3-uplinkbyte-fwd | The total number of QCI3 uplink bytes forwarded. | Counter / Int64
> qci3-dwlinkbyte-fwd | The total number of QCI3 downlink bytes forwarded. | Counter / Int64
> qci3-uplinkpkt-drop | The total number of QCI3 uplink packets dropped. | Counter / Int32
> qci3-dwlinkpkt-drop | The total number of QCI3 downlink packets dropped. | Counter / Int32
> qci3-uplinkbyte-drop | The total number of QCI3 uplink bytes dropped. | Counter / Int64
> qci3-dwlinkbyte-drop | The total number of QCI3 downlink bytes dropped. | Counter / Int64
> qci4-actbear | The total number of QCI4 active bearers. | Counter / Int32
> qci4-setupbear | The total number of QCI4 bearers setup. | Counter / Int32
> qci4-relbear | The total number of QCI4 released bearers. | Counter / Int32
> qci4-uplinkpkt-fwd | The total number of QCI4 uplink packets forwarded. | Counter / Int32
> qci4-dwlinkpkt-fwd | The total number of QCI4 downlink packets forwarded. | Counter / Int32
> qci4-uplinkbyte-fwd | The total number of QCI4 uplink bytes forwarded. | Counter / Int64
> qci4-dwlinkbyte-fwd | The total number of QCI4 downlink bytes forwarded. | Counter / Int64
> qci4-uplinkpkt-drop | The total number of QCI4 uplink packets dropped. | Counter / Int32
> qci4-dwlinkpkt-drop | The total number of QCI4 downlink packets dropped. | Counter / Int32
> qci4-uplinkbyte-drop | The total number of QCI4 uplink bytes dropped. | Counter / Int64
> qci4-dwlinkbyte-drop | The total number of QCI4 downlink bytes dropped. | Counter / Int64
> qci5-actbear | The total number of QCI5 active bearers. | Counter / Int32
> qci5-setupbear | The total number of QCI5 bearers setup. | Counter / Int32
> qci5-relbear | The total number of QCI5 released bearers. | Counter / Int32
> qci5-uplinkpkt-fwd | The total number of QCI5 uplink packets forwarded. | Counter / Int32
> qci5-dwlinkpkt-fwd | The total number of QCI5 downlink packets forwarded. | Counter / Int32
> qci5-uplinkbyte-fwd | The total number of QCI5 uplink bytes forwarded. | Counter / Int64
> qci5-dwlinkbyte-fwd | The total number of QCI5 downlink bytes forwarded. | Counter / Int64
> qci5-uplinkpkt-drop | The total number of QCI5 uplink packets dropped. | Counter / Int32
> qci5-dwlinkpkt-drop | The total number of QCI5 downlink packets dropped. | Counter / Int32
> qci5-uplinkbyte-drop | The total number of QCI5 uplink bytes dropped. | Counter / Int64
> qci5-dwlinkbyte-drop | The total number of QCI5 downlink bytes dropped. | Counter / Int64
> qci6-actbear | The total number of QCI6 active bearers. | Counter / Int32
> qci6-setupbear | The total number of QCI6 bearers setup. | Counter / Int32
> qci6-relbear | The total number of QCI6 released bearers. | Counter / Int32
> qci6-uplinkpkt-fwd | The total number of QCI6 uplink packets forwarded. | Counter / Int32
> qci6-dwlinkpkt-fwd | The total number of QCI6 downlink packets forwarded. | Counter / Int32
> qci6-uplinkbyte-fwd | The total number of QCI6 uplink bytes forwarded. | Counter / Int64
> qci6-dwlinkbyte-fwd | The total number of QCI6 downlink bytes forwarded. | Counter / Int64
> qci6-uplinkpkt-drop | The total number of QCI6 uplink packets dropped. | Counter / Int32
> qci6-dwlinkpkt-drop | The total number of QCI6 downlink packets dropped. | Counter / Int32
> qci6-uplinkbyte-drop | The total number of QCI6 uplink bytes dropped. | Counter / Int64
> qci6-dwlinkbyte-drop | The total number of QCI6 downlink bytes dropped. | Counter / Int64
> qci7-actbear | The total number of QCI7 active bearers. | Counter / Int32
> qci7-setupbear | The total number of QCI7 bearers setup. | Counter / Int32
> qci7-relbear | The total number of QCI7 released bearers. | Counter / Int32
> qci7-uplinkpkt-fwd | The total number of QCI7 uplink packets forwarded. | Counter / Int32
> qci7-dwlinkpkt-fwd | The total number of QCI7 downlink packets forwarded. | Counter / Int32
> qci7-uplinkbyte-fwd | The total number of QCI7 uplink bytes forwarded. | Counter / Int64
> qci7-dwlinkbyte-fwd | The total number of QCI7 downlink bytes forwarded. | Counter / Int64
> qci7-uplinkpkt-drop | The total number of QCI7 uplink packets dropped. | Counter / Int32
> qci7-dwlinkpkt-drop | The total number of QCI7 downlink packets dropped. | Counter / Int32
> qci7-uplinkbyte-drop | The total number of QCI7 uplink bytes dropped. | Counter / Int64
> qci7-dwlinkbyte-drop | The total number of QCI7 downlink bytes dropped. | Counter / Int64
> qci8-actbear | The total number of QCI8 active bearers. | Counter / Int32
> qci8-setupbear | The total number of QCI8 bearers setup. | Counter / Int32
> qci8-relbear | The total number of QCI8 released bearers. | Counter / Int32
> qci8-uplinkpkt-fwd | The total number of QCI8 uplink packets forwarded. | Counter / Int32
> qci8-dwlinkpkt-fwd | The total number of QCI8 downlink packets forwarded. | Counter / Int32
> qci8-uplinkbyte-fwd | The total number of QCI8 uplink bytes forwarded. | Counter / Int64
> qci8-dwlinkbyte-fwd | The total number of QCI8 downlink bytes forwarded. | Counter / Int64
> qci8-uplinkpkt-drop | The total number of QCI8 uplink packets dropped. | Counter / Int32
> qci8-dwlinkpkt-drop | The total number of QCI8 downlink packets dropped. | Counter / Int32
> qci8-uplinkbyte-drop | The total number of QCI8 uplink bytes dropped. | Counter / Int64
> qci8-dwlinkbyte-drop | The total number of QCI8 downlink bytes dropped. | Counter / Int64
> qci9-actbear | The total number of QCI9 active bearers. | Counter / Int32
> qci9-setupbear | The total number of QCI9 bearers setup. | Counter / Int32
> qci9-relbear | The total number of QCI9 released bearers. | Counter / Int32
> qci9-uplinkpkt-fwd | The total number of QCI9 uplink packets forwarded. | Counter / Int32
> qci9-dwlinkpkt-fwd | The total number of QCI9 downlink packets forwarded. | Counter / Int32
> qci9-uplinkbyte-fwd | The total number of QCI9 uplink bytes forwarded. | Counter / Int64
> qci9-dwlinkbyte-fwd | The total number of QCI9 downlink bytes forwarded. | Counter / Int64
> qci9-uplinkpkt-drop | The total number of QCI9 uplink packets dropped. | Counter / Int32
> qci9-dwlinkpkt-drop | The total number of QCI9 downlink packets dropped. | Counter / Int32
> qci9-uplinkbyte-drop | The total number of QCI9 uplink bytes dropped. | Counter / Int64
> qci9-dwlinkbyte-drop | The total number of QCI9 downlink bytes dropped. | Counter / Int64
> nonstdqci-nongbr-actbear | The total number of non-standard QCI, non-GBR active bearers. | Counter / Int32
> nonstdqci-nongbr-setupbear | The total number of non-standard QCI, non-GBR bearers setup. | Counter / Int32
> nonstdqci-nongbr-relbear | The total number of non-standard QCI, non-GBR released bearers. | Counter / Int32
> nonstdqci-nongbr-uplinkpkt-fwd | The total number of non-standard QCI, non-GBR uplink packets forwarded. | Counter / Int32
> nonstdqci-nongbr-dwlinkpkt-fwd | The total number of non-standard QCI, non-GBR downlink packets forwarded. | Counter / Int32
> nonstdqci-nongbr-uplinkbyte-fwd | The total number of non-standard QCI, non-GBR uplink bytes forwarded. | Counter / Int64
> nonstdqci-nongbr-dwlinkbyte-fwd | The total number of non-standard QCI, non-GBR downlink bytes forwarded. | Counter / Int64
> nonstdqci-nongbr-uplinkpkt-drop | The total number of non-standard QCI, non-GBR uplink packets dropped. | Counter / Int32
> nonstdqci-nongbr-dwlinkpkt-drop | The total number of non-standard QCI, non-GBR downlink packets dropped. | Counter / Int32
> nonstdqci-nongbr-uplinkbyte-drop | The total number of non-standard QCI, non-GBR uplink bytes dropped. | Counter / Int64
> nonstdqci-nongbr-dwlinkbyte-drop | The total number of non-standard QCI, non-GBR downlink bytes dropped. | Counter / Int64
> nonstdqci-gbr-actbear | The total number of non-standard QCI, GBR active bearers. | Counter / Int32
> nonstdqci-gbr-setupbear | The total number of non-standard QCI, GBR bearers setup. | Counter / Int32
> nonstdqci-gbr-relbear | The total number of non-standard QCI, GBR released bearers. | Counter / Int32
> nonstdqci-gbr-uplinkpkt-fwd | The total number of non-standard QCI, GBR uplink packets forwarded. | Counter / Int32
> nonstdqci-gbr-dwlinkpkt-fwd | The total number of non-standard QCI, GBR downlink packets forwarded. | Counter / Int32
> nonstdqci-gbr-uplinkbyte-fwd | The total number of non-standard QCI, GBR uplink bytes forwarded. | Counter / Int64
> nonstdqci-gbr-dwlinkbyte-fwd | The total number of non-standard QCI, GBR downlink bytes forwarded. | Counter / Int64
> nonstdqci-gbr-uplinkpkt-drop | The total number of non-standard QCI, GBR uplink packets dropped. | Counter / Int32
> nonstdqci-gbr-dwlinkpkt-drop | The total number of non-standard QCI, GBR downlink packets dropped. | Counter / Int32
> nonstdqci-gbr-uplinkbyte-drop | The total number of non-standard QCI, GBR uplink bytes dropped. | Counter / Int64
> nonstdqci-gbr-dwlinkbyte-drop | The total number of non-standard QCI, GBR downlink bytes dropped. | Counter / Int64
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883