> GT-Format3 Configuration Mode Commands
> The GT-Format3 configuration mode is a sub-mode for either the Global Title Translation Association configuration mode or the Global Title Translation Address-Map configuration mode. This sub-mode configures a set of rules used in the global title translation (GTT) process.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> encoding-scheme
> Configures the encoding-scheme to use during global title translation (GTT).
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> encoding scheme scheme_type
> scheme_type
> Select one of the following encoding scheme types to determine the encoding type to be used during GTT:

> • | bcd-even: BCD even encoding scheme

> • | bcd-odd: BCD odd encoding scheme

> • | nw-specfic: Network specific encoding scheme

> • | unknown: Unknown encoding scheme

> Usage
> Select BCD even encoding for GTT
> Example
> encoding scheme bcd-even
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> numbering-plan
> Configures the GTT process to apply one of the numbering-plans during the GT translation process.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> numbering-plan plan_type
> plan_type
> Select one of the following numbering plans be employed during GTT:

> • | data: Data numbering plan

> • | generic: Generic number plan

> • | isdn : ISDN tel numbering plan

> • | isdn-mobile: ISDN mobile numbering plan

> • | land-mobile: Land mobile numbering plan

> • | maritime-mobile: Maritime mobile numbering plan

> • | nw-specific : Private network / network-specific numbering plan

> • | telex: Telex numbering plan

> • | unknown: Unknown numbering plan

> Usage
> Select ISN telephone number plan for GTT process.
> Example
> The following command sets the numbering plan to use during GTT processing to isdn
> numbering-plan isdn
> translation-type
> Configures the global title translation (GTT) process to apply a specific number for translation during the GTT process.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> translation-type number
> number
> Must be an integer between 0 and 255.
> Default is 0
> Usage
> Use this command to define the translation-type to be used during the global title translation process.
> Example
> translation-type 233

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883