> CSCF Last Route Profile Criteria Configuration Mode Commands
> The CSCF Last Route Profile Criteria Configuration Mode is used to configure county names and assign them Last Routing Option (LRO) numbers to be used by the CSCF last route profile. The S-CSCF forwards emergency call packets to the correct Public Safety Answering Point (PSAP) based on this criteria, which it receives from a peer server.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> county-name
> Configure county names and assign them Last Routing Option (LRO) numbers to be used by the CSCF last route profile.
> Product
> SCM (S-CSCF)
> Privilege
> Administrator
> Syntax
> county-name county_name lro-number value
> [ no ] county-name county_name
> county_name
> Specifies the county name.
> county_name must be from 1 to 79 alpha and/or numeric characters in length.
> lro-number value
> Specifies an existing LRO number.
> value can be a maximum of ten digits in length.
> no county-name county_name
> Removes the specified county name.
> Usage
> Use this command to configure county names and assign them LRO numbers.
> Important: You may configure up to 100 county names.
> Example
> The following command creates a county name called norfolk and assigns it an LRO number of 8884384357:
> county-name norfolk lro-number 8884384357
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> lro-number
> Configure the Last Routing Option (LRO) numbers to be used by the CSCF last route profile.
> Product
> SCM (S-CSCF)
> Privilege
> Administrator
> Syntax
> lro-number value
> lro-number value
> Specifies the LRO number.
> value can be a maximum of ten digits in length.
> no
> Removes the specified LRO number.
> Usage
> Use this command to configure LRO numbers.
> Important: You may configure up to 100 LRO numbers.
> Example
> The following command creates an LRO number set at 8884384357:
> lro-number 8884384357

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883