> ACS Port Map Configuration Mode Commands
> The ACS Port Map Configuration Mode is used to define application-port map in the ACS Configuration Mode. The application-port map facilitates to associate a range of port to specific application/protocol within a rule definition (ruledef).
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> This command exits the current configuration mode and returns to the Executive mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to change to the Executive mode.
> exit
> This command exits the current configuration mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> port
> This command specifies a range of ports for application or protocol in ACS Port Map Configuration Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] port { port_num | range start_port to end_port }
> no
> Removes the specified port(s) / range of ports that were configured previously from this port map.
> port_num
> Specifies the port number to add to the port map.
> port_num must be an integer from 1 through 65535.
> range start_port to end_port
> Specifies the range of ports for an application/protocol to add to this port map.
> start_port must be an integer from 1 through 65535, and must be lesser than end_port.
> end_port must be an integer from 1 through 65535, and must be greater than start_port.
> Usage
> Use this command to specify mapping between application and range of ports. Up to 10 sets of ports can be configured in each port map.
> Example
> The following command adds all ports from 3112 through 5000 to the port map:
> port range 3112 to 5000

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883