> Network Service Virtual Connection Configuration Mode Commands
> The Network Service Virtual Connection (NSVC) configuration mode is a sub-mode of the Network Service Entity (NSE) - Frame Relay Peer NSEI (NSE-FR for short) configuration mode. This sub-mode provides the commands and parameters to define the management functionality for a specific NSVC of the Gb interface between a BSS and an SGSN in a 2.5G GPRS frame relay network connection.
> Upon accessing this mode, the prompt will appear similar to:
> [local]asr5000(nse-fr-peer-nsei-2344-nsvci-2)# where the numerics are user-defined ids for the configuration instances.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the previous configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the network service entity - frame relay configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883