> Network Service Entity- IP Local Configuration Mode Commands
> The Network Service Entity (NSE) - IP Local configuration mode is a sub-mode of the Global Configuration mode. This sub-mode configures the local endpoint for NS/IP with the commands and parameters to define the management functionality for the Gb interface between a BSS and an SGSN over a 2.5G GPRS IP network connection.
> Upon entering this mode, the prompt will appear in a manner similar to:
> [local]asr5000(nse-ip-local)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> all-nsvc-failure-action
> Configure how the SGSN handles the NSE when all NSVCs go down.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> all-nsvc-failure-action clear-nse
> default all-nsvc-failure-action
> default
> By default, the NSE is not cleared if all NSVCs go down.
> clear-nse
> Instructs the SGSN to SGSN to clear NSE if all NSVCs to the BSC are down.
> Usage
> Enable the SGSN to clear NSE information when all NSVCs go down.
> Example
> all-nsvc-failure-action clear-nse
> bssgp-timer
> This command has been deprecated.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the global configuration mode.
> max-ns-retransmissions
> This command configures the maximum number of transmission retries counter.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default ] max-ns-retransmissions { alive count| sns-proc count}
> default
> Resets the specified counter configuration to the default value.
> alive count
> Sets the maximum number of alive retries.
> count: Must be an integer between 0 and 10. Default is 3.
> sns-proc count
> Sets the maximum number of retries for the SNS procedure
> count: Must be an integer between 0 and 5. Default is 3.
> Usage
> Sets the maximum for NS transmission retries.
> Example
> max-ns-retransmission alive 4
> ns-timer
> This command sets the network service (NS) counters for the SNS procedure and testing.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ns-timer { sns-prov timeout_val| test timeout_val}
> default ns-timer { sns-prov | test }
> default
> Resets the selected timer configuration to its default value.
> sns-prov timeout_val
> Sets the SNS procedure timeout value in seconds.
> timeout_val: Enter an integer from 1 to 10. Default is 5.
> test timeout_val
> Sets the test procedure timeout value in seconds.
> timeout_val: Enter an integer from 1 to 60. Default is 30 seconds.
> Usage
> Set NS timers to help manage the NSE-IP connection.
> Example
> The following example sets the test timer to 4 seconds:
> ns-timer test 4
> nsvc-failure-action
> This command enables and disables the sending of an NS-STATUS message with cause ‘ip-test fail’ when NSVC goes down.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> nsvc-failure-action send-ns-status
> default nsvc-failure-action
> default
> Resets the command configuration to its default value. The default action is not to send an NS-STATUS message. This is applicable only to NSVCs that are auto-learned and not configured.
> send-ns-status
> Enables the sending of the NS-STATUS message.
> Usage
> Use this command to enable or disable sending an NS-STATUS messages when an NSVC goes down.
> Example
> Enable sending of the message:
> nsvc-failure-action send-ns-status
> nsvl
> This command creates and instance of a Network Service Virtual Link (NSVL) and enters the NSVL configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] nsvl instance nsvl_id
> no
> Removes the identified NSVL definition from the configuration.
> nsvl_id
> Identifies a specific NSVL. configuration instance.
> nsvl_id: Must be an integer from 0 to 3.
> Usage
> Access the NSVL configuration mode.
> Example
> nsvl instance 2
> peer-network-service-entity
> This command has been replaced by the Network Service Entity - Peer NSEI Frame Relay configuration mode.
> retry-count
> This command has been replaced by the max-ns-retransmissions command.
> timer
> This command has been replaced by the ns-timer command.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883