> Core MIB
> The following figure displays the hierarchical structure of the management information base (MIB) for the core platform.
> MIB Textual Conventions
> The following are the supported MIB Objects and Notifications. Not all entries are supported on all platforms. Some may return a different output than expected.

> Object: | StarentSlotType

> Object ID: | N/A

> Syntax: | Describes the type of a slot. Each slot in the chassis is build to contain specific type(s) of cards. Only a card of one of the appropriate types can be put into a specific slot.

> Enumeration: | unknown(1) pactac(2) spc(3) lc(4) rcc(5) spio(6)

> Object: | StarentCardType

> Object ID: | N/A

> Description: | Describes the type of a card. Each type represents a physically different card which would have a unique part number.

> Syntax: | Integer

> Enumeration: | none(1) unknown(2) spc(3) pac(4) spio(5) rcc(6) lceth(7) lcgeth(8) lcds3 tac(10) Icoc3(11) Icoc12(12) smc(13) psc(14) lcqgeth(15) lctgeth(16) vmc(17) vpc(18) vlceth1p(19)

> Object: | StarentVersionNum

> Object ID: | N/A

> Description: | Contains the system version identification string.

> Syntax: | Octet String (0.. 256)

> Object: | StarRelayState

> Object ID: | N/A

> Description: | The state of a Central Office (CO) relay.

> Syntax: | Integer

> Enumeration: | off(1) on(2) unknown(3)

> Object: | StarLongDurTimeoutAction

> Object ID: | N/A

> Description: | The action taken by the system upon detection of a long-duration session.

> Syntax: | INTEGER

> Enumeration: | unknown(0) detection(1) disconnection(2) notapplicable(3) dormantdisconnection(4) dormantdetection(5)

> Object: | StarShortName

> Object ID: | N/A

> Description: | short identification string. Follows the same conventions as the DisplayString TEXTUAL-CONVENTION.

> Syntax: | Octet String (1..32)

> Object: | StarShortID

> Object ID: | N/A

> Description: | An abbreviated form for identifying a service, composed of the first 8 characters of the context name, and the first 8 characters of a service name, separated by (:)

> Syntax: | OCTET STRING(1..17)

> Object: | StarMediumID

> Object ID: | N/A

> Description: | An abbreviated form for identifying a context-specific object, composed of the first 8 characters of the context name, and the first 16 characters of the object name, separated by (:)

> Syntax: | OCTET STRING (SIZE (1..25))

> Object: | StarQOSTPAction

> Object ID: | N/A

> Description: | Traffic Policing Action

> Syntax: | INTEGER

> Enumeration: | unknown(0) notapplicable(1) transmit(2) drop(3) loweripprecedence(4)

> Object: | StarOSPFNeighborState

> Object ID: | N/A

> Description: | OSPF Neighbor State

> Syntax: | INTEGER

> Enumeration: | unknown(0), down(1), attempt(2), init(3), twoway(4), exstart(5), exchange(6), loading(7), full(8)

> starentMIB(8164).starentMIBObjects(1).starentChassis(1)

> Object: | starChassisCriticalCO

> Object ID: | enterprises.8164.1.1.1

> Description: | The current state of the Critical Central Office (CO) relay.

> Syntax: | StarRelayState

> Access: | Read-only

> Object: | starChassisMajorCO

> Object ID: | enterprises.8164.1.1.2

> Description: | The current state of the Major Central Office (CO) relay.

> Syntax: | StarRelayState

> Access: | Read-only

> Object: | starChassisMinorCO

> Object ID: | enterprises.8164.1.1.3

> Description: | The current state of the Minor Central Office (CO) relay.

> Syntax: | StarRelayState

> Access: | Read-only

> Object: | starChassisAction

> Object ID: | enterprises.8164.1.1.5

> Description: | Trigger to perform certain system-wide operations. noaction (1) performs no operation. It is the normal value received when this attribute is read. testled (2) triggers a test of all of the LEDs in the system. aco (3) triggers the Alarm Cut-Off, which shuts off all of the Central Office (CO) audible/visual relays. reset (4) triggers a system-wide restart. It will completely disrupt service on the device.

> Syntax: | Integer

> Access: | Read-write

> Enumeration: | noaction(1) testled(2) aco(3) reset(4)

> Object: | starTimeTicks

> Object ID: | enterprises.8164.1.1.6

> Description: | The number of system clock ticks since the last system Epoch. One system clock tick is 10 milliseconds.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starChassisAudibleAlarm

> Object ID: | enterprises.8164.1.1.7

> Description: | The current state of the chassis Audible Alarm.

> Syntax: | StarRelayState

> Access: | Read-only

> Object: | starChassisUTCTime

> Object ID: | enterprises.8164.1.1.8

> Description: | The current time on the chassis, in UTC format

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starChassisLocalTime

> Object ID: | enterprises.8164.1.1.9

> Description: | The current time on the chassis, converted to the local time zone

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starChassisType

> Object ID: | enterprises.8164.1.1.10

> Description: | The physical chassis type

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(0) ST16(1) ST40(2) XT2(3) st20(4)

> Object: | starChassisDescription

> Object ID: | enterprises.8164.1.1.11

> Description: | Chassis description

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starChassisSWRevision

> Object ID: | enterprises.8164.1.1.12

> Description: | Software revision

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starChassisPeakMemoryUsage

> Object ID: | enterprises.8164.1.1.13

> Description: | The system level peak memory usage, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

> Syntax: | Integer32(1..2097152)

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentSlots(2)

> Object: | starSlotTable

> Object ID: | enterprises.8164.1.2.1

> Description: | A table containing information on all of the slots.

> Syntax: | Sequence of StarSlotEntry

> Access: | Not-accessible

> Object: | starSlotEntry

> Object ID: | enterprises.8164.1.2.1.1

> Description: | Information about a particular slot.

> Syntax: | StarSlotEntry

> Access: | Not-accessible

> Sequence: | starSlotNum starSlotType starCardType starCardOperState starCardAdminState starCardRevision starCardLastStateChange starCardMode starCardDesiredMode starCardPacStandbyPriority starCardLock starCardHaltIssued starCardRebootPending starCardUsable starCardSinglePOF starCardAttachment starCardTemperature starSlotVoltage1dot5 starSlotVoltage1dot5LowThresh starSlotVoltage1dot5HighThresh starSlotVoltage1dot8 starSlotVoltage1dot8LowThresh starSlotVoltage1dot8HighThresh starSlotVoltage2dot5 starSlotVoltage2dot5LowThresh starSlotVoltage2dot5HighThresh starSlotVoltage3dot3 starSlotVoltage3dot3LowThresh starSlotVoltage3dot3HighThresh starSlotVoltage5dot0 starSlotVoltage5dot0LowThresh starSlotVoltage5dot0HighThresh starSlotNumPorts starSlotVoltageState starSlotNumCpu starSlotNum

> Object ID: | enterprises.8164.1.2.1.1.1

> Description: | The slot number.

> Syntax: | Integer32(1..48)

> Access: | Not-accessible

> Object: | starSlotType

> Object ID: | enterprises.8164.1.2.1.1.2

> Description: | The type of the slot.

> Syntax: | StarentSlotType

> Access: | Read-only

> Object: | starCardType

> Object ID: | enterprises.8164.1.2.1.1.3

> Description: | The type of the card which is plugged into a slot.

> Syntax: | StarentCardType

> Access: | Read-only

> Object: | starCardOperState

> Object ID: | enterprises.8164.1.2.1.1.4

> Description: | The current operational state of the card.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) empty(2) offline(3) booting(4) ready(5) standby(6) active(7) migratefrom(8) migrateto(9)

> Object: | starCardAdminState

> Object ID: | enterprises.8164.1.2.1.1.5

> Description: | The current administrative state of the card.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) enabled(2) disabled(3)

> Object: | starCardRevision

> Object ID: | enterprises.8164.1.2.1.1.6

> Description: | The revision number of the card that is physically present in this slot.

> Syntax: | StarentVersionNum

> Access: | Read-only

> Object: | starCardLastStateChange

> Object ID: | enterprises.8164.1.2.1.1.7

> Description: | The time when the last state change occurred for this row. A manager could poll this variable to determine if information has changed.

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starCardMode

> Object ID: | enterprises.8164.1.2.1.1.8

> Description: | The desired mode of the card. This field is applicable only to slots which can contain PAC/PSC and TAC cards. The active(4) value is obsolete and has been replaces with activepac(5) and activetac(6).

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) notapplicable(2) standby(3) active(4) activepac(5) activetac(6) activepsc(7) activevpc(8)

> Object: | starCardPacStandbyPriority

> Object ID: | enterprises.8164.1.2.1.1.9

> Description: | Specifies the standby priority of the packet accelerator card.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starCardHaltIssued

> Object ID: | enterprises.8164.1.2.1.1.10

> Description: | Only applicable to SPC cards.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | notapplicable(1) yes(2) no(3)

> Object: | starCardLock

> Object ID: | enterprises.8164.1.2.1.1.11

> Description: | Identifies if the card lock is currently engaged. A value of locked(2) means that the lock is engaged, and thus the card could not be removed from the chassis. A value of unlocked(3) means that the lock is not engaged, and an operator could remove the card from the chassis. A value of unknown(1) should represent that there is no card physically in the slot.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) locked(2) unlocked(3)

> Object: | starCardRebootPending

> Object ID: | enterprises.8164.1.2.1.1.12

> Description: | Identifies if a reboot operation is currently pending for this card.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | no(1) yes(2)

> Object: | starCardUsable

> Object ID: | enterprises.8164.1.2.1.1.13

> Description: | Indicates if the card is currently usable.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | no(1) yes(2)

> Object: | starCardSinglePOF

> Object ID: | enterprises.8164.1.2.1.1.14

> Description: | Identifies if this card represents a single point of failure (POF). A value of no(1) indicates that this card is supported by a redundant card which can take over in the event of a failure. A value of yes(2) indicates that this card does not have a redundant partner, and that a failure of this card could result in service interruption.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | notapplicable(1) no(2) yes(3)

> Object: | starCardAttachment

> Object ID: | enterprises.8164.1.2.1.1.15

> Description: | Identifies if the card is currently attached to another card (a PAC/PSC attached to a line card, or visa versa, for example)

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | connected(1) unconnected(2)

> Object: | starCardTemperature

> Object ID: | enterprises.8164.1.2.1.1.16

> Description: | The temperature, in degrees Celsius, as measured on the card. A value of 0 indicates that the temperature cannot be read, or that the card is not present. The maximum measurable temperature is 70 C.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSlotVoltage1dot5

> Object ID: | enterprises.8164.1.2.1.1.20

> Description: | The current voltage, in millivolts, of the nominal 1.5V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot5LowThresh and starSlotVoltage1dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage1dot5LowThresh

> Object ID: | enterprises.8164.1.2.1.1.21

> Description: | The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage1dot5HighThresh

> Object ID: | enterprises.8164.1.2.1.1.22

> Description: | The voltage level, in millivolts, which is the highest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage1dot8

> Object ID: | enterprises.8164.1.2.1.1.23

> Description: | The current voltage, in millivolts, of the nominal 1.8V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot8LowThresh and starSlotVoltage1dot8HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage1dot8LowThresh

> Object ID: | enterprises.8164.1.2.1.1.24

> Description: | The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage1dot8HighThresh

> Object ID: | enterprises.8164.1.2.1.1.25

> Description: | The voltage level, in millivolts, which is the highest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage2dot5

> Object ID: | enterprises.8164.1.2.1.1.26

> Description: | The current voltage, in millivolts, of the nominal 2.5V power supply. The working range for this card is the range defined by variables starSlotVoltage2dot5LowThresh and starSlotVoltage2dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage2dot5LowThresh

> Object ID: | enterprises.8164.1.2.1.1.27

> Description: | The voltage level, in millivolts, which is the lowest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage2dot5HighThresh

> Object ID: | enterprises.8164.1.2.1.1.28

> Description: | The voltage level, in millivolts, which is the highest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage3dot3

> Object ID: | enterprises.8164.1.2.1.1.29

> Description: | The current voltage, in millivolts, of the nominal 3.3V power supply. The working range for this card is the range defined by variables starSlotVoltage3dot3LowThresh and starSlotVoltage3dot3HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage3dot3LowThresh

> Object ID: | enterprises.8164.1.2.1.1.30

> Description: | The voltage level, in millivolts, which is the lowest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage3dot3HighThresh

> Object ID: | enterprises.8164.1.2.1.1.31

> Description: | The voltage level, in millivolts, which is the highest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage5dot0

> Object ID: | enterprises.8164.1.2.1.1.32

> Description: | The current voltage, in millivolts, of the nominal 5.0V power supply. The working range for this card is the range defined by variables starSlotVoltage5dot0LowThresh and starSlotVoltage5dot0HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage5dot0LowThresh

> Object ID: | enterprises.8164.1.2.1.1.33

> Description: | The voltage level, in millivolts, which is the lowest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotVoltage5dot0HighThresh

> Object ID: | enterprises.8164.1.2.1.1.34

> Description: | The voltage level, in millivolts, which is the highest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

> Object: | starSlotNumPorts

> Object ID: | enterprises.8164.1.2.1.1.35

> Description: | Number of data ports on this card. This value will be 0 for cards that no not contain ports, such as SPC/PAC/TAC cards, or for slots which do not contain a card.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: This alarm is obsolete.

> Object: | starSlotAction

> Object ID: | enterprises.8164.1.2.1.1.36

> Description: | Trigger to perform certain slot operations. noaction(1) performs no operation. It is the normal value received when this attribute is read. reset(2) causes the slot to be reset.

> Syntax: | Integer

> Access: | Read-write

> Enumeration: | noaction(1) reset(2)

> Object: | starSlotVoltageState

> Object ID: | enterprises.8164.1.2.1.1.37

> Description: | The state of the voltage supplies on the card. A value of unknown(0) means that the state cannot be identified; normal(1) represents a properly functioning card; outofrange(2) indicates that one or more voltage sources are not within their specified operating range.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(0) normal(1) outfrange(2)

> Object: | starSlotNumCpu

> Object ID: | enterprises.8164.1.2.1.1.38

> Description: | The number of general purpose CPU on this card.

> Syntax: | Integer32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSlotMapping(3)

> Object: | starSlotMappingTable

> Object ID: | enterprises.8164.1.3.1

> Description: | A table identifying all of the slot mappings.

> Syntax: | Sequence of StarSlotMappingEntry

> Access: | Not-accessible

> Object: | starSlotMappingEntry

> Object ID: | enterprises.8164.1.3.1.1

> Description: | Information about a particular slot mapping.

> Syntax: | StarSlotMappingEntry

> Access: | Not-accessible

> Sequence: | starSlotMappingNum Index starSlotMappingType starSlotMappingRCCNum starSlotMappingToSlot

> Object: | starSlotMappingNum

> Object ID: | enterprises.8164.1.3.1.1.1

> Description: | The slot number. This always represents a slot in the back of the chassis.

> Syntax: | Integer32(17..48)

> Access: | Not-accessible

> Description: | The slot number. This always represents a slot in the back of the chassis.

> Object: | starSlotMappingType

> Object ID: | enterprises.8164.1.3.1.1.2

> Description: | The type of the slot mapping. The value none(1) represents that there is no mapping, which typically represents that there is no card present in this slot.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) none(2) direct(3) rcc(4) cross(5)

> Object: | starSlotMappingRCCNum

> Object ID: | enterprises.8164.1.3.1.1.3

> Description: | Identifies which RCC card is responsible for this mapping. This value is only valid if the value of starSlotMappingType is rcc(3).

> Syntax: | Integer32(0..2)

> Access: | Read-only

> Object: | starSlotMappingToSlot

> Object ID: | enterprises.8164.1.3.1.1.4

> Description: | The slot number this slot is mapped to. This always represents a slot in the front of the chassis.

> Syntax: | Integer32(1..16)

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentFans(4)

> Object: | starFanTable

> Object ID: | enterprises.8164.1.4.1

> Description: | A table containing information on all of the fan controllers.

> Syntax: | Sequence of StarFanEntry

> Access: | Not-accessible

> Object: | starFanEntry

> Object ID: | enterprises.8164.1.4.1.1

> Description: | Information about a particular fan controller.

> Syntax: | StarFanEntry

> Access: | Not-accessible

> Sequence: | starFanNum Index starFanLocation starFanStatus starFanSpeed

> Object: | starFanNum

> Object ID: | enterprises.8164.1.4.1.1.1

> Description: | The fan controller number.

> Syntax: | Integer32(1..2)

> Access: | Not-accessible

> Object: | starFanLocation

> Object ID: | enterprises.8164.1.4.1.1.2

> Description: | The physical location of the fan controller.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | upper(1) lower(2)

> Object: | starFanStatus

> Object ID: | enterprises.8164.1.4.1.1.3

> Description: | A bitmask representing the status of the fan tray. A normal, properly functioning fan tray would show 0x101 (257 decimal), meaning it is present (0x100) and all fans are working (0x1).

> Syntax: | Integer32

> Access: | Read-only

> Enumeration: | 0x01 All Fans Good 0x02 Multiple Fans Bad 0x04 Single Fan Bad 0x08 HB Error 0x10 COM A Error 0x20 COM B Error 0x40 COMM Error 0x80 Not Present 0x100 Present 0x200 Filter Clogged 0x400 State Unknown

> Object: | starFanSpeed

> Object ID: | enterprises.8164.1.4.1.1.4

> Description: | The speed of the fans controlled by this fan controller. The values represent the percentage that the speed is running relative to the maximum possible speed, speed100(12)

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(1) speed50(2) speed55(3) speed60(4) speed65(5) speed70(6) speed75(7) speed80(8) speed85(9) speed90(10) speed95(11) speed100(12)

> starentMIB(8164).starentMIBObjects(1).starentLogs(5)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starLogTable

> Object ID: | enterprises.8164.1.5.1

> Description: | A table containing information about all of the system logs.

> Syntax: | Sequence of StarLogEntry

> Access: | Not-accessible

> Object: | starLogEntry

> Object ID: | enterprises.8164.1.5.1.1

> Description: | Information about a particular system log.

> Syntax: | StarLogEntry

> Access: | Not-accessible

> Sequence: | starLogName Index starLogCurSize starLogMaxSize starLogText

> Object: | starLogName

> Object ID: | enterprises.8164.1.5.1.1.1

> Description: | The name of the system log.

> Syntax: | StarShortName

> Access: | Not-accessible

> Object: | starLogCurSize

> Object ID: | enterprises.8164.1.5.1.1.2

> Description: | The size, in bytes, of this log.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starLogMaxSize

> Object ID: | enterprises.8164.1.5.1.1.3

> Description: | The maximum size, in bytes, of this log.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starLogText

> Object ID: | enterprises.8164.1.5.1.1.4

> Description: | For use in LogMsg trap.

> Syntax: | Octet String (SIZE (1..512))

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentAlertMan(8)
> starentMIB(8164).starentMIBObjects(1).starentAlertMan(8).
> starentFeedback(1)

> Object: | starMaxAlertsPerTime

> Object ID: | enterprises.8164.1.8.1.1

> Description: | The maximum number of SNMP Traps which will be sent within the time period specified by starWindowTime.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starWindowTime

> Object ID: | enterprises.8164.1.8.1.2

> Description: | The amount of time, in seconds, within which no more than starMaxAlertsPerTime SNMP Traps will be sent.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starAlertSendingEnabled

> Object ID: | enterprises.8164.1.8.1.3

> Description: | Shows if SNMP traps are currently enabled or disabled. Traps are disabled when more than starMaxAlertsPerTime traps are sent within the starWindowTime time period. A value of true(1) indicates that traps will still be sent. A value of false(2) indicates that traps are no longer being generated

> Syntax: | TruthValue

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentPower(9)

> Object: | starPowerTable

> Object ID: | enterprises.8164.1.9.1

> Description: | A table containing information about all power filters.

> Syntax: | Sequence of StarPowerEntry

> Access: | Not-accessible

> Object: | starPowerEntry

> Object ID: | enterprises.8164.1.9.1.1

> Description: | Information about a particular power filter.

> Syntax: | StarPowerEntry

> Access: | Not-accessible

> Sequence: | starPowerNumber Index starPowerState

> Object: | starPowerNumber

> Object ID: | enterprises.8164.1.9.1.1.1

> Description: | The identifying number for this power filter.

> Syntax: | Integer

> Access: | Not-accessible

> Enumeration: | powerA(1) powerB(2)

> Object: | starPowerState

> Object ID: | enterprises.8164.1.9.1.1.2

> Description: | The state of the power filter. The value active(1) means that the power filter is present and operational. The value failed(2) means that the power filter is present, but not operational. The value not-present(3) means that the power filter is not physically present in the system.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | active(1) failed(2) notpresent(3)

> starentMIB(8164).starentMIBObjects(1).starentCPU(10)

> Object: | starCPUTable

> Object ID: | enterprises.8164.1.10.1

> Description: | A table containing information about all CPUs

> Syntax: | Sequence of StarCPUEntry

> Access: | Not-accessible

> Object: | starCPUEntry

> Object ID: | enterprises.8164.1.10.1.1

> Description: | Information about a particular CPU.

> Syntax: | StarCPUEntry

> Access: | Not-accessible

> Sequence: | starCPUSlot Index starCPUNumber Index starCPUUser starCPUSystem starCPUIdle starCPUIO starCPURQ starCPULoad1Min starCPULoad5Min starCPULoad15Min starCPUMemTotal starCPUMemUsed starCPUNumProcesses starCPUMemCached

> Object: | starCPUSlot

> Object ID: | enterprises.8164.1.10.1.1.1

> Description: | The slot number of the card holding this CPU.

> Syntax: | Integer32(1..16)

> Access: | Not-accessible

> Object: | starCPUNumber

> Object ID: | enterprises.8164.1.10.1.1.2

> Description: | The CPU number within this card. Numbers begin at 0.

> Syntax: | Integer32(0..3)

> Access: | Not-accessible

> Object: | starCPUUser

> Object ID: | enterprises.8164.1.10.1.1.3

> Description: | Percentage of the CPU spent running user processes. starCPUUser is the percentage value times 100; for example, 2.3% would be represented as 230

> Syntax: | Integer32(1..10000)

> Access: | Read-only

> Object: | starCPUSystem

> Object ID: | enterprises.8164.1.10.1.1.4

> Description: | Percentage of the CPU spent running system processes. starCPUSystem is the percentage value times 100; for example, 2.3% would be represented as 230.

> Syntax: | Integer32(1..10000)

> Access: | Read-only

> Object: | starCPUIdle

> Object ID: | enterprises.8164.1.10.1.1.6

> Description: | Percentage of the CPU spent idle. starCPUIdle is the percentage value times 100; for example, 2.3% would be represented as 230.

> Syntax: | Integer32(1..10000)

> Access: | Read-only

> Object: | starCPUIO

> Object ID: | enterprises.8164.1.10.1.1.7

> Description: | Percentage of the CPU spent running Input/Output processes. starCPUIO is the percentage value times 100; for example, 2.3% would be represented as 230.

> Syntax: | Integer32(1..10000)

> Access: | Read-only

> Object: | starCPURQ

> Object ID: | enterprises.8164.1.10.1.1.8

> Description: | Percentage of the CPU spent running IRQ processes. starCPURQ is the percentage value times 100; for example, 2.3% would be represented as 230.

> Syntax: | Integer32(1..10000)

> Access: | Read-only

> Object: | starCPULoad1Min

> Object ID: | enterprises.8164.1.10.1.1.11

> Description: | The average CPU load over the last minute. The CPU load is defined to be the number of processes who are ready to run. starCPULoad1Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

> Syntax: | Integer32(1..1000000000)

> Access: | Read-only

> Object: | starCPULoad5Min

> Object ID: | enterprises.8164.1.10.1.1.12

> Description: | The average CPU load over the last 5 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad5Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

> Syntax: | Integer32(1..1000000000)

> Access: | Read-only

> Object: | starCPULoad15Min

> Object ID: | enterprises.8164.1.10.1.1.13

> Description: | The average CPU load over the last 15 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad15Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

> Syntax: | Integer32(1..1000000000)

> Access: | Read-only

> Object: | starCPUMemTotal

> Object ID: | enterprises.8164.1.10.1.1.14

> Description: | The total amount of memory dedicated to this CPU, in kilobytes.

> Syntax: | Integer32(1..2097152)

> Access: | Read-only

> Object: | starCPUMemUsed

> Object ID: | enterprises.8164.1.10.1.1.15

> Description: | The total amount of memory consumed by this CPU, in kilobytes.

> Syntax: | Integer32(1..2097152)

> Access: | Read-only

> Object: | starCPUNumProcesses

> Object ID: | enterprises.8164.1.10.1.1.16

> Description: | The total number of processes which exist on this CPU.

> Syntax: | Integer32(1..4096)

> Access: | Read-only

> Object: | starCPUMemCached

> Object ID: | enterprises.8164.1.10.1.1.17

> Description: | The total amount of memory consumed by the (reusable) memory cache on this CPU, in kilobytes

> Syntax: | Integer32(1..2097152)

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentNPUMgr(11)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starNPUMgrTable

> Object ID: | enterprises.8164.1.11.1

> Description: | A table containing information about all NPU Managers.

> Syntax: | Sequence of StarNPUMgrEntry

> Access: | Not-accessible

> Object: | starNPUMgrEntry

> Object ID: | enterprises.8164.1.11.1.1

> Description: | Information about a particular NPU Manager.

> Syntax: | StarNPUMgrEntry

> Access: | Not-accessible

> Sequence: | starNPUMgrNumber

> Object: | starNPUMgrNumber

> Object ID: | enterprises.8164.1.11.1.1.1

> Description: | The identity of this NPU.

> Syntax: | Integer32(1..65535)

> Access: | Not-accessible

> starentMIB(8164).starentMIBObjects(1).starentSessInP(12)

> Object: | starSessInProgCalls

> Object ID: | enterprises.8164.1.12.1

> Description: | The number of sessions currently in progress.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgActiveCalls

> Object ID: | enterprises.8164.1.12.2

> Description: | The number of sessions with active calls.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgDormantCalls

> Object ID: | enterprises.8164.1.12.3

> Description: | The number of sessions associated with dormant calls.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgArrived

> Object ID: | enterprises.8164.1.12.4

> Description: | The number of sessions in the arrived state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgLCPNeg

> Object ID: | enterprises.8164.1.12.5

> Description: | The number of sessions in the link control protocol negotiation state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgLCPUp

> Object ID: | enterprises.8164.1.12.6

> Description: | The number of sessions in the link control protocol up state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgAuthenticating

> Object ID: | enterprises.8164.1.12.7

> Description: | The number of sessions in the authenticating state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgAuthenticated

> Object ID: | enterprises.8164.1.12.8

> Description: | The number of sessions in the authenticated state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgIPCPUp

> Object ID: | enterprises.8164.1.12.9

> Description: | The number of sessions in the IP control protocol up state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgSIPConn

> Object ID: | enterprises.8164.1.12.10

> Description: | The number of sessions in the Simple IP connected state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgMIPConn

> Object ID: | enterprises.8164.1.12.11

> Description: | The number of sessions in the Mobile IP connected state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessInProgDisc

> Object ID: | enterprises.8164.1.12.12

> Description: | The number of sessions in the disconnecting state.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSessMgr(13)

> Object: | starSessMgrCount

> Object ID: | enterprises.8164.1.13.1

> Description: | The total number of session manager instances.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlArrived

> Object ID: | enterprises.8164.1.13.2

> Description: | The total number of requested sessions.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlRejected

> Object ID: | enterprises.8164.1.13.3

> Description: | The total number of rejected sessions.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlConnected

> Object ID: | enterprises.8164.1.13.4

> Description: | The total number of sessions which were connected.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlAuthSucc

> Object ID: | enterprises.8164.1.13.5

> Description: | The total number of sessions where authentication was successful.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlAuthFail

> Object ID: | enterprises.8164.1.13.6

> Description: | The total number of sessions which failed authentication.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlLCPUp

> Object ID: | enterprises.8164.1.13.7

> Description: | The total number of sessions in the link control protocol in the up state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlIPCPUp

> Object ID: | enterprises.8164.1.13.8

> Description: | The total number of sessions in the IP control protocol up state.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlSrcViol

> Object ID: | enterprises.8164.1.13.9

> Description: | The total number of sessions which had an invalid source.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlKeepFail

> Object ID: | enterprises.8164.1.13.10

> Description: | The total number of sessions which had a keep alive failure.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessTtlOctForwarded

> Object ID: | enterprises.8164.1.13.11

> Description: | The total number of octets forwarded (data + control).

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlRPRegAccept

> Object ID: | enterprises.8164.1.13.12

> Description: | The total number of Initial RRQ Accepted.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessTtlRPRegAcceptInterPDSN

> Object ID: | enterprises.8164.1.13.13

> Description: | The total number of Inter PDSN Handoff RRQ Accepted.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPCurrSessions

> Object ID: | enterprises.8164.1.13.14

> Description: | The current number of PPP sessions

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessTtlTxBytes

> Object ID: | enterprises.8164.1.13.15

> Description: | The total number of bytes transmitted from mobiles

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlRxBytes

> Object ID: | enterprises.8164.1.13.16

> Description: | he total number of bytes received by mobiles

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlSIPTxBytes

> Object ID: | enterprises.8164.1.13.17

> Description: | The total number of bytes transmitted from mobiles using SIP

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlSIPRxBytes

> Object ID: | enterprises.8164.1.13.18

> Description: | The total number of bytes received by mobiles using SIP

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlMIPTxBytes

> Object ID: | enterprises.8164.1.13.19

> Description: | The total number of bytes transmitted from mobiles using MIP

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlMIPRxBytes

> Object ID: | enterprises.8164.1.13.20

> Description: | The total number of bytes received by mobiles using MIP

> Syntax: | Counter32

> Units: | Megabytes

> Access: | Read-only

> Object: | starSessTtlOctForwardedGB

> Object ID: | enterprises.8164.1.13.21

> Description: | The total number of octets forwarded (data + control)

> Syntax: | Counter32

> Units: | Gigabytes

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentAAAMgr(14)

> Object: | starAAAMgrCount

> Object ID: | enterprises.8164.1.14.1

> Description: | The total number of AAA manager instances.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlRequests

> Object ID: | enterprises.8164.1.14.2

> Description: | The total number of AAA requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlAuthRequests

> Object ID: | enterprises.8164.1.14.3

> Description: | The total number of AAA authentication requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlAcctRequests

> Object ID: | enterprises.8164.1.14.4

> Description: | The total number of AAA accounting requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAACurRequests

> Object ID: | enterprises.8164.1.14.5

> Description: | The current number of AAA requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAACurAuthRequests

> Object ID: | enterprises.8164.1.14.6

> Description: | The current number of AAA authentication requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAACurAcctRequests

> Object ID: | enterprises.8164.1.14.7

> Description: | The current number of AAA accounting requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlAcctSess

> Object ID: | enterprises.8164.1.14.8

> Description: | The total number of AAA accounting sessions.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAACurAcctSess

> Object ID: | enterprises.8164.1.14.9

> Description: | The current number of accounting sessions

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlAuthSuccess

> Object ID: | enterprises.8164.1.14.10

> Description: | The total number of AAA authentication successes.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starAAATtlAuthFailure

> Object ID: | enterprises.8164.1.14.11

> Description: | The total number of AAA authentication failures.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentA11Mgr(15)

> Object: | starA11MgrCount

> Object ID: | enterprises.8164.1.15.1

> Description: | The total number of A11 manager instances.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starA11TtlArrived

> Object ID: | enterprises.8164.1.15.2

> Description: | The total number of A11 session requests.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starA11TtlRejected

> Object ID: | enterprises.8164.1.15.3

> Description: | The total number of rejected A11 sessions.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starA11TtlDemultiplexed

> Object ID: | enterprises.8164.1.15.4

> Description: | The total number of demultiplexed A11 sessions.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starA11TtlDereg

> Object ID: | enterprises.8164.1.15.5

> Description: | The total number of A11 deregistrations.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starA11CurActive

> Object ID: | enterprises.8164.1.15.6

> Description: | The current number of active A11 sessions.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentHAMgr(16)

> Object: | starHAMgrCount

> Object ID: | enterprises.8164.1.16.1

> Description: | The total number of home agent manager instances.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starHATtlArrived

> Object ID: | enterprises.8164.1.16.2

> Description: | The total number of home agent session requests.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starHATtlRejected

> Object ID: | enterprises.8164.1.16.3

> Description: | The total number of rejected home agent sessions.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starHATtlDemultiplexed

> Object ID: | enterprises.8164.1.16.4

> Description: | The total number of demultiplexed home agent sessions.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starHATtlDereg

> Object ID: | enterprises.8164.1.16.5

> Description: | The total number of home agent deregistrations.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starHACurActive

> Object ID: | enterprises.8164.1.16.6

> Description: | The current number of active home agent sessions.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentFAMgr(17)

> Object: | starFAMgrCount

> Object ID: | enterprises.8164.1.17.1

> Description: | The total number of foreign agent manager instances.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starFATtlArrived

> Object ID: | enterprises.8164.1.17.2

> Description: | The total number of foreign agent session requests.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starFATtlRejected

> Object ID: | enterprises.8164.1.17.3

> Description: | The total number of rejected foreign agent sessions.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starFATtlDemultiplexed

> Object ID: | enterprises.8164.1.17.4

> Description: | The total number of demultiplexed foreign agent sessions.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starFATtlDereg

> Object ID: | enterprises.8164.1.17.5

> Description: | The total number of foreign agent deregistrations.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starFACurActive

> Object ID: | enterprises.8164.1.17.6

> Description: | The current number of active foreign agent sessions.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentService(18)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starServiceTable

> Object ID: | enterprises.8164.1.18.1

> Description: | A table containing information about all of the service managers.

> Syntax: | Sequence of StarSvcEntry

> Access: | Not-accessible

> Object: | starServiceEntry

> Object ID: | enterprises.8164.1.18.1.1

> Description: | Information about a particular service manager.

> Syntax: | StarSvcEntry

> Access: | Not-accessible

> Sequence: | starServiceVpnID Index starServiceSvcID Index starServiceVpnName starServiceServName starServiceSubLimit starServiceSubCurrent starServiceType starServiceFAIpAddr starServiceHAIpAddr

> Object: | starServiceVpnId

> Object ID: | enterprises.8164.1.18.1.1.1

> Description: | The internal identification of the VPN (context).

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starServiceSvcID

> Object ID: | enterprises.8164.1.18.1.1.2

> Description: | The internal identification of the service, unique to the associated context.

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starServiceVpnName

> Object ID: | enterprises.8164.1.18.1.1.3

> Description: | The name of the VPN (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starServiceServName

> Object ID: | enterprises.8164.1.18.1.1.4

> Description: | The name of the service.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starServiceSubLimit

> Object ID: | enterprises.8164.1.18.1.1.5

> Description: | The configured subscriber limit.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starServiceSubCurrent

> Object ID: | enterprises.8164.1.18.1.1.6

> Description: | Current subscriber limit.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starServiceType

> Object ID: | enterprises.8164.1.18.1.1.7

> Description: | Service type.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(1) pdsn(2) ggsn(3) ha(4) fa(5) l2tpserver(6) lac(7) lns(8) closedrp(9 ecs(10) cscf(11) ipsg(12) evdoreva(13) pdif(15) asnpc(16) mipv6ha(17) phsgw(18) phspc(19) sgsn(20) gprs(21) hsgw(22) pgw(23) sgw(24) pdg(25) standalonefa(26) imsue(27)

> Object: | starServiceFAIpAddr

> Object ID: | enterprises.8164.1.18.1.1.8

> Description: | The IP address for an FA service. Where unknown or not applicable this will contain all zeroes.

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starServiceHAIpAddr

> Object ID: | enterprises.8164.1.18.1.1.9

> Description: | The IP address for an HA service. Where unknown or not applicable this will contain all zeroes.

> Syntax: | IpAddress

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentCLIMgr(19)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starCLITable

> Object ID: | enterprises.8164.1.19.1

> Description: | A table containing information about all interactive CLI sessions.

> Syntax: | Sequence of StarSvcEntry

> Access: | Not-accessible

> Object: | starCLIEntry

> Object ID: | enterprises.8164.1.19.1.1

> Description: | Information about a particular CLI session.

> Syntax: | StarSvcEntry

> Access: | Not-accessible

> Sequence: | starCLIID starCLIUsername starCLITtyname starCLIPrivs starCLIType starCLIRemoteIpAddr starCLIContext

> Object: | starCLIID

> Object ID: | enterprises.8164.1.19.1.1.1

> Description: | The internal identify of the CLI session.

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starCLIUsername

> Object ID: | enterprises.8164.1.19.1.1.2

> Description: | The name of the user logged into the CLI sessions or ‘unknown’ if not known.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starCLITtyname

> Object ID: | enterprises.8164.1.19.1.1.3

> Description: | The name of the TTY device used for the CLI session.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starCLIPrivs

> Object ID: | enterprises.8164.1.19.1.1.4

> Description: | The CLI session privilege level.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starCLIType

> Object ID: | enterprises.8164.1.19.1.1.5

> Description: | The CLI type; commandline(1) represents the normal interactive command line; ftp(2) represents an incoming FTP session.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) commandline(1) ftp(2)

> Object: | starCLIRemoteIPAddr

> Object ID: | enterprises.8164.1.19.1.1.6

> Description: | The remote IP address used to access this CLI session. Where unknown or not applicable (such as access through a serial port) this will be 0.

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starCLIContext

> Object ID: | enterprises.8164.1.19.1.1.7

> Description: | The context (VPN) currently being viewed or managed by the CLI session.

> Syntax: | DisplayString

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentTaskMgr(20)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starTaskTable

> Object ID: | enterprises.8164.1.20.1

> Description: | A table containing information about all of the active tasks.

> Syntax: | Sequence of StarSvcEntry

> Access: | Not-accessible

> Object: | starTaskEntry

> Object ID: | enterprises.8164.1.20.1.1

> Description: | Information about a particular task.

> Syntax: | StarSvcEntry

> Access: | Not-accessible

> Sequence: | starTaskFacility Index starTaskInstance Index starTaskFacilityName starTaskCard starTaskCPU

> Object: | starTaskFacility

> Object ID: | enterprises.8164.1.20.1.1.1

> Description: | The internal identify of the facility.

> Syntax: | Unsigned32

> Access: | Not-accessible

> Object: | starTaskInstance

> Object ID: | enterprises.8164.1.20.1.1.2

> Description: | The unique internal instance identifier for the task without a given facility.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starTaskFacilityName

> Object ID: | enterprises.8164.1.20.1.1.3

> Description: | The name of the facility the task is associated with.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starTaskCard

> Object ID: | enterprises.8164.1.20.1.1.4

> Description: | The slot number of the card where the task is located.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starTaskCPU

> Object ID: | enterprises.8164.1.20.1.1.5

> Description: | The CPU number where the task is running.

> Syntax: | Unsigned32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentPPP(21)

> Object: | starPPPStatTable

> Object ID: | enterprises.8164.1.21.1

> Description: | A table containing PPP statistics.

> Syntax: | Sequence of StarPPPStatEntry

> Access: | Not-accessible

> Object: | starPPPStatEntry

> Object ID: | enterprises.8164.1.21.1.1

> Description: | The statistics for an individual entry for a PPP context and service.

> Syntax: | StarPPPStatEntry

> Access: | Not-accessible

> Sequence: | starPPPStatVpnID starPPPStatSvcID Index (Implied) starPPPStatVpnName starPPPStatServName starPPPStatInit starPPPStatReneg starPPPStatSuccess starPPPStatFailed starPPPStatReleased starPPPStatReleasedLocal starPPPStatReleasedRemote starPPPStatLcpFailMaxRetry starPPPStatLcpFailOption starPPPStatIpcpFailMaxRetry starPPPStatIpcpFailOption starPPPStatCcpFail starPPPStatAuthFail starPPPStatLcpEntered starPPPStatAuthEntered starPPPStatIpcpEntered starPPPStatRenegPdsn starPPPStatRenegMobil starPPPStatRenegAddrMismatch starPPPStatRenegOther starPPPStatChapAuthAttempt starPPPStatPapAuthAttempt starPPPStatMSChapAuthAttempt starPPPStatChapAuthFail starPPPStatPapAuthFail starPPPStatMSChapAuthFail starPPPStatStacComp starPPPStatMppcComp starPPPStatDeflComp starPPPStatFscErrs starPPPStatUnknProto starPPPStatBadAddr starPPPStatBadCtrl starPPPStatVjComp starPPPStatDiscLcpRemote starPPPStatDiscRpRemote starPPPStatDiscAdmin starPPPStatDiscIdleTimeout starPPPStatDiscAbsTimeout starPPPStatDiscPPPKeepalive starPPPStatDiscNoResource starPPPStatDiscMisc starPPPStatFailedReneg starPPPStatLcpFailUnknown starPPPStatIpcpFailUnknown starPPPStatAuthAbort starPPPStatLowerLayerDisc starPPPStatLcpSuccess starPPPStatAuthSuccess starPPPStatRenegLowerLayerHandoff starPPPStatRenegParamUpdate starPPPStatChapAuthSuccess starPPPStatPapAuthSuccess starPPPStatMSChapAuthSuccess starPPPStatChapAuthAbort starPPPStatPapAuthAbort starPPPStatMSChapAuthAbort starPPPStatSessSkipAuth starPPPStatNegComp starPPPStatCCPNegFailComp starPPPStatDiscLocalLowerLayer starPPPStatDiscAddFlowFail starPPPStatDiscMaxRetriesLCP starPPPStatDiscMaxRetriesIPCP starPPPStatDiscMaxSetupTimer starPPPStatDiscInvalidDestVpn starPPPStatDiscOptNegFailLCP starPPPStatDiscOptNegFailIPCP arPPPStatDiscNoRemoteIpAddr starPPPStatDiscCallTypeDetectFail starPPPStatDiscRemoteDiscUpLayer starPPPStatDiscLongDuraTimeout starPPPStatDiscAuthFail starPPPStatLCPEchoTotalReq starPPPStatLCPEchoReqResent starPPPStatLCPEchoRepRecved starPPPStatLCPEchoReqTimeout starPPPStatRecvErrBadCtrlField starPPPStatRecvErrBadPacketLen starPPPStatRemoteTerm starPPPStatMiscFail

> Object: | starPPPStatVpnID

> Object ID: | enterprises.8164.1.21.1.1.1

> Description: | The internal identification of the PPP VPN (context).

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starPPPStatSvcID

> Object ID: | enterprises.8164.1.21.1.1.2

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

> Syntax: | StarShortID

> Access: | Not-accessible

> Object: | starPPPStatVpnName

> Object ID: | enterprises.8164.1.21.1.1.3

> Description: | The name of the PPP VPN (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starPPPStatServName

> Object ID: | enterprises.8164.1.21.1.1.4

> Description: | The name of the PPP service.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starPPPStatInit

> Object ID: | enterprises.8164.1.21.1.1.5

> Description: | The number of initialized PPP sessions for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatReneg

> Object ID: | enterprises.8164.1.21.1.1.6

> Description: | The number of PPP session renegotiations for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatSuccess

> Object ID: | enterprises.8164.1.21.1.1.7

> Description: | The number of PPP session negotiation successes for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatFailed

> Object ID: | enterprises.8164.1.21.1.1.8

> Description: | The number of PPP session negotiation failures for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatReleased

> Object ID: | enterprises.8164.1.21.1.1.9

> Description: | The number of PPP sessions released for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatReleasedLocal

> Object ID: | enterprises.8164.1.21.1.1.10

> Description: | The number of PPP sessions where the release was initiated locally for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatReleasedRemote

> Object ID: | enterprises.8164.1.21.1.1.11

> Description: | The number of PPP session where the release was initiated remotely for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLcpFailMaxRetry

> Object ID: | enterprises.8164.1.21.1.1.12

> Description: | The number of PPP sessions which failed to bring up the link control protocol due to excessive retries for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLcpFailOption

> Object ID: | enterprises.8164.1.21.1.1.13

> Description: | The number of PPP sessions which failed to bring up the Link Control Protocol (LCP) due to an invalid option being received for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatIpcpFailMaxRetry

> Object ID: | enterprises.8164.1.21.1.1.14

> Description: | The number of PPP sessions which failed to start the IP Control Protocol (IPCP) due to excessive retries for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatIpcpFailOption

> Object ID: | enterprises.8164.1.21.1.1.15

> Description: | The number of PPP sessions which failed to start the IP Control Protocol due to an invalid option being received for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatCcpFail

> Object ID: | enterprises.8164.1.21.1.1.16

> Description: | The number of PPP sessions which failed to initialize the CCP.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatAuthFail

> Object ID: | enterprises.8164.1.21.1.1.17

> Description: | The number of PPP sessions which failed authentication for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLcpEntered

> Object ID: | enterprises.8164.1.21.1.1.18

> Description: | The number of PPP sessions which successfully initialized the Link Control Protocol.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatAuthEntered

> Object ID: | enterprises.8164.1.21.1.1.19

> Description: | The number of PPP sessions which were successfully authenticated.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatIpcpEntered

> Object ID: | enterprises.8164.1.21.1.1.20

> Description: | The number of PPP sessions which successfully initialized the IP Control Protocol.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegPdsn

> Object ID: | enterprises.8164.1.21.1.1.21

> Description: | The number of PPP sessions which re-negotiated the PDSN service access.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegMobil

> Object ID: | enterprises.8164.1.21.1.1.22

> Description: | The number of PPP sessions which re-negotiated the Mobile IP service access.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegAddrMismatch

> Object ID: | enterprises.8164.1.21.1.1.23

> Description: | The number of PPP sessions which had an IP address mismatch during re-negotiation.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegOther

> Object ID: | enterprises.8164.1.21.1.1.24

> Description: | The number of PPP sessions which failed renegotiation for reasons other than IP address mismatch.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatChapAuthAttempt

> Object ID: | enterprises.8164.1.21.1.1.25

> Description: | The number of PPP CHAP authentication attempts for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatPapAuthAttempt

> Object ID: | enterprises.8164.1.21.1.1.26

> Description: | The number of PPP PAP authentication attempts for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMSChapAuthAttempt

> Object ID: | enterprises.8164.1.21.1.1.27

> Description: | The number of PPP MSCHAP authentication attempts for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatChapAuthFail

> Object ID: | enterprises.8164.1.21.1.1.28

> Description: | The number of PPP CHAP authentication attempt failures for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatPapAuthFail

> Object ID: | enterprises.8164.1.21.1.1.29

> Description: | The number of PPP PAP authentication failures for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMSChapAuthFail

> Object ID: | enterprises.8164.1.21.1.1.30

> Description: | The number of PPP MSCHAP authentication failures for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatStacComp

> Object ID: | enterprises.8164.1.21.1.1.31

> Description: | The number of PPP sessions which had STAC compression enabled for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMppcComp

> Object ID: | enterprises.8164.1.21.1.1.32

> Description: | The number of PPP sessions which had MPPC compression enabled for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDeflComp

> Object ID: | enterprises.8164.1.21.1.1.33

> Description: | The number of PPP sessions which had DEFLATE compression enabled for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatFscErrs

> Object ID: | enterprises.8164.1.21.1.1.34

> Description: | The number of PPP forward sequence control errors in messaging.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatUnknProto

> Object ID: | enterprises.8164.1.21.1.1.35

> Description: | The number of PPP sessions which failed due to an unknown protocol received for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatBadAddr

> Object ID: | enterprises.8164.1.21.1.1.36

> Description: | The number of PPP sessions which failed due to a bad address being received for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatBadCtrl

> Object ID: | enterprises.8164.1.21.1.1.37

> Description: | The number of PPP sessions in which a bad control sequence was received.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatVjComp

> Object ID: | enterprises.8164.1.21.1.1.38

> Description: | The number of PPP sessions which had VJ header compression enabled for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscLcpRemote

> Object ID: | enterprises.8164.1.21.1.1.39

> Description: | The number of PPP sessions which were disconnected via the link control protocol from the remote end for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscRpRemote

> Object ID: | enterprises.8164.1.21.1.1.40

> Description: | The number of PPP sessions which were disconnected by the remote via the R-P interface for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscAdmin

> Object ID: | enterprises.8164.1.21.1.1.41

> Description: | The number of PPP sessions which were disconnected by a local administrator for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscIdleTimeout

> Object ID: | enterprises.8164.1.21.1.1.42

> Description: | The number of PPP sessions disconnected due to session idle timer expiration for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscAbsTimeout

> Object ID: | enterprises.8164.1.21.1.1.43

> Description: | The number of PPP sessions disconnected due to the session absolute timer expiration for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscPPPKeepalive

> Object ID: | enterprises.8164.1.21.1.1.44

> Description: | The number of PPP sessions disconnected due to PPP keep alive failure for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscNoResource

> Object ID: | enterprises.8164.1.21.1.1.45

> Description: | The number of PPP sessions disconnected due to local resource shortage for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscMisc

> Object ID: | enterprises.8164.1.21.1.1.46

> Description: | The number of PPP sessions disconnected due to any cause which does not match any other existing disconnect statistic for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatFailedReneg

> Object ID: | enterprises.8164.1.21.1.1.47

> Description: | The number of failed PPP renegotiations the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLcpFailUnknown

> Object ID: | enterprises.8164.1.21.1.1.48

> Description: | The number of failed PPP LCP that are due to unknown reasons for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatIpcpFailUnknown

> Object ID: | enterprises.8164.1.21.1.1.49

> Description: | The number of failed PPP IPCP that are due to unknown reasons for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatAuthAbort

> Object ID: | enterprises.8164.1.21.1.1.50

> Description: | The number of aborted PPP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLowerLayerDisc

> Object ID: | enterprises.8164.1.21.1.1.51

> Description: | The number of Failed PPP session due to RP disconnect for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLcpSuccess

> Object ID: | enterprises.8164.1.21.1.1.52

> Description: | The number of successful PPP LCPs for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatAuthSuccess

> Object ID: | enterprises.8164.1.21.1.1.53

> Description: | The number of successful PPP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegLowerLayerHandoff

> Object ID: | enterprises.8164.1.21.1.1.54

> Description: | The number of PPP renegotiations for RP handoff for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRenegParamUpdate

> Object ID: | enterprises.8164.1.21.1.1.55

> Description: | The number of PPP renegotiations for parameter update for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatChapAuthSuccess

> Object ID: | enterprises.8164.1.21.1.1.56

> Description: | The number of successful PPP CHAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatPapAuthSuccess

> Object ID: | enterprises.8164.1.21.1.1.57

> Description: | The number of successful PPP PAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMSChapAuthSuccess

> Object ID: | enterprises.8164.1.21.1.1.58

> Description: | The number of successful PPP MSCHAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatChapAuthAbort

> Object ID: | enterprises.8164.1.21.1.1.59

> Description: | The number of aborted PPP CHAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatPapAuthAbort

> Object ID: | enterprises.8164.1.21.1.1.60

> Description: | The number of aborted PPP PAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMSChapAuthAbort

> Object ID: | enterprises.8164.1.21.1.1.61

> Description: | The number of aborted PPP MSCHAP authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatSessSkipAuth

> Object ID: | enterprises.8164.1.21.1.1.62

> Description: | The number of PPP sessions that skipped authentications for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatNegComp

> Object ID: | enterprises.8164.1.21.1.1.63

> Description: | The number of PPP sessions that negotiated compressions for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatCCPNegFailComp

> Object ID: | enterprises.8164.1.21.1.1.64

> Description: | The number of PPP sessions that failed compression negotiation for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscLocalLowerLayer

> Object ID: | enterprises.8164.1.21.1.1.65

> Description: | The number of disconnected PPP sessions due to local RP disconnect for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscAddFlowFail

> Object ID: | enterprises.8164.1.21.1.1.66

> Description: | The number of disconnected PPP sessions due to failure in adding new flow for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscMaxRetriesLCP

> Object ID: | enterprises.8164.1.21.1.1.67

> Description: | The number of disconnected PPP sessions due to max retries for LCP for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscMaxRetriesIPCP

> Object ID: | enterprises.8164.1.21.1.1.68

> Description: | The number of disconnected PPP sessions due to max retries for IPCP for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscMaxSetupTimer

> Object ID: | enterprises.8164.1.21.1.1.69

> Description: | The number of disconnected PPP sessions due to max setup time out for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscInvalidDestVpn

> Object ID: | enterprises.8164.1.21.1.1.70

> Description: | The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscOptNegFailLCP

> Object ID: | enterprises.8164.1.21.1.1.71

> Description: | The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscOptNegFailIPCP

> Object ID: | enterprises.8164.1.21.1.1.72

> Description: | The number of disconnected PPP sessions due to failed IPCP option negotiation for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscNoRemoteIpAddr

> Object ID: | enterprises.8164.1.21.1.1.73

> Description: | The number of disconnected PPP sessions due to no remote IP address for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscCallTypeDetectFail

> Object ID: | enterprises.8164.1.21.1.1.74

> Description: | The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscRemoteDiscUpLayer

> Object ID: | enterprises.8164.1.21.1.1.75

> Description: | The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscLongDuraTimeout

> Object ID: | enterprises.8164.1.21.1.1.76

> Description: | The number of disconnected PPP sessions due to long duration time out for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatDiscAuthFail

> Object ID: | enterprises.8164.1.21.1.1.77

> Description: | The number of disconnected PPP sessions due to failed authentication for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLCPEchoTotalReq

> Object ID: | enterprises.8164.1.21.1.1.78

> Description: | The total number of PPP LCP echo requests for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLCPEchoReqResent

> Object ID: | enterprises.8164.1.21.1.1.79

> Description: | The total number of PPP LCP echo requests resent for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLCPEchoRepRecved

> Object ID: | enterprises.8164.1.21.1.1.80

> Description: | The total number of PPP LCP echo replies received for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatLCPEchoReqTimeout

> Object ID: | enterprises.8164.1.21.1.1.81

> Description: | The total number of PPP LCP echo requests time out for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRecvErrBadCtrlField

> Object ID: | enterprises.8164.1.21.1.1.82

> Description: | The total number of received PPP error due to bad control fields for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRecvErrBadPacketLen

> Object ID: | enterprises.8164.1.21.1.1.83

> Description: | The total number of received PPP error due to bad packet length for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatRemoteTerm

> Object ID: | enterprises.8164.1.21.1.1.84

> Description: | The total number of PPP remote terminations for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPPPStatMiscFail

> Object ID: | enterprises.8164.1.21.1.1.85

> Description: | The number of miscellaneous PPP failures for the associated VPN service.

> Syntax: | Counter32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentMIPHA(22)

> Object: | starMIPHAStatTable

> Object ID: | enterprises.8164.1.22.1

> Description: | A table containing MIP home agent statistics.

> Syntax: | Sequence of starMIPHAStatEntry

> Access: | Not-accessible

> Object: | starMIPHAStatEntry

> Object ID: | enterprises.8164.1.22.1.1

> Description: | The Mobile IP home agent statistics for a specific VPN (context) and service.

> Syntax: | starMIPHAStatEntry

> Access: | Not-accessible

> Sequence: | starMIPHAStatVpnID starMIPHAStatSvcID Index (Implied) starMIPHAStatVpnName starMIPHAStatServName starMIPHADisconnects starMIPHAExpiry starMIPHADereg starMIPHAAdminDrop starMIPHARegRecvTotal starMIPHARegRecvInitial starMIPHARegRecvRenew starMIPHARegRecvDereg starMIPHARegAcceptTotal starMIPHARegAcceptReg, starMIPHARegAcceptRenew starMIPHARegAcceptDereg starMIPHARegDeniedTotal starMIPHARegDeniedInitial starMIPHARegDeniedRenew starMIPHARegDeniedDereg starMIPHARegReplyTotal starMIPHARegReplyAcceptReg starMIPHARegReplyAcceptDereg starMIPHARegReplyDenied starMIPHARegReplyBadReq starMIPHARegReplyMismatchID starMIPHARegReplyAdminProhib starMIPHARegReplyUnspecErr, starMIPHARegReplyNoResource starMIPHARegReplyMnAuthFail starMIPHARegReplyFAAuthFail starMIPHARegReplySimulBind starMIPHARegReplyUnknownHA starMIPHARegReplyRevTunUnavail starMIPHARegReplyRevTunMand starMIPHARegReplyEncapUnavail starMIPHARegReplySendError starMIPHAStatFARevocations starMIPHAStatRegAcceptHO starMIPHAStatRegDeniedHO starMIPHAStatRegDiscardTotal

> Object: | starMIPHAStatVpnID

> Object ID: | enterprises.8164.1.22.1.1.1

> Description: | The internal identification of the home agent Mobile IP VPN (context).

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starMIPHAStatSvcID

> Object ID: | enterprises.8164.1.22.1.1.2

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

> Syntax: | StarShortID

> Access: | Not-accessible

> Object: | starMIPHAStatVpnName

> Object ID: | enterprises.8164.1.22.1.1.3

> Description: | The name of the VPN (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starMIPHAStatServName

> Object ID: | enterprises.8164.1.22.1.1.4

> Description: | The Mobile IP home agent service name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starMIPHAStatDisconnects

> Object ID: | enterprises.8164.1.22.1.1.5

> Description: | The number of session disconnects for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatExpiry

> Object ID: | enterprises.8164.1.22.1.1.6

> Description: | The number of session expirations for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatDereg

> Object ID: | enterprises.8164.1.22.1.1.7

> Description: | The number of session deregistrations for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatAdminDrop

> Object ID: | enterprises.8164.1.22.1.1.8

> Description: | The number of session disconnects due to administrator actions for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegRecvTotal

> Object ID: | enterprises.8164.1.22.1.1.9

> Description: | The number of session registrations received for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegRecvInitial

> Object ID: | enterprises.8164.1.22.1.1.10

> Description: | The number of initial session registrations received for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegRecvRenew

> Object ID: | enterprises.8164.1.22.1.1.11

> Description: | The number of session registration renewals received for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegRecvDereg

> Object ID: | enterprises.8164.1.22.1.1.12

> Description: | The number of session deregistrations received for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegAcceptTotal

> Object ID: | enterprises.8164.1.22.1.1.13

> Description: | The number of session registrations accepted for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegAcceptReg

> Object ID: | enterprises.8164.1.22.1.1.14

> Description: | The number of session registrations accepted for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegAcceptRenew

> Object ID: | enterprises.8164.1.22.1.1.15

> Description: | The number of session registration renewals accepted for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegAcceptDereg

> Object ID: | enterprises.8164.1.22.1.1.16

> Description: | The number of session deregistrations accepted for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDeniedTotal

> Object ID: | enterprises.8164.1.22.1.1.17

> Description: | The number of session registrations denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDeniedInitial

> Object ID: | enterprises.8164.1.22.1.1.18

> Description: | The number of session initial registrations denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDeniedRenew

> Object ID: | enterprises.8164.1.22.1.1.19

> Description: | The number of session registration renewals denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDeniedDereg

> Object ID: | enterprises.8164.1.22.1.1.20

> Description: | The number of session deregistrations denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyTotal

> Object ID: | enterprises.8164.1.22.1.1.21

> Description: | The total number of session registration replies for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyAcceptReg

> Object ID: | enterprises.8164.1.22.1.1.22

> Description: | The number of session registration replies accepted indicating registration for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyAcceptDereg

> Object ID: | enterprises.8164.1.22.1.1.23

> Description: | The number of session registration replies accepted indicating deregistration for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyDenied

> Object ID: | enterprises.8164.1.22.1.1.24

> Description: | The number of session registration replies which were denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyBadReq

> Object ID: | enterprises.8164.1.22.1.1.25

> Description: | The number of session registration replies indicating a bad request for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyMismatchID

> Object ID: | enterprises.8164.1.22.1.1.26

> Description: | The number of session registration replies indicating an ID mismatch for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyAdminProhib

> Object ID: | enterprises.8164.1.22.1.1.27

> Description: | The number of session registration replies indicating administrator prohibition for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyUnspecErr

> Object ID: | enterprises.8164.1.22.1.1.28

> Description: | The number of session registration replies with an unspecified error for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyNoResource

> Object ID: | enterprises.8164.1.22.1.1.29

> Description: | The number of session registration replies indicating no resources for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyMnAuthFail

> Object ID: | enterprises.8164.1.22.1.1.30

> Description: | The number of session registration replies indicating mobile number authentication failure for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyFAAuthFail

> Object ID: | enterprises.8164.1.22.1.1.31

> Description: | The number of session registration replies indicating a foreign agent authentication failure for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplySimulBind

> Object ID: | enterprises.8164.1.22.1.1.32

> Description: | The number of session registration replies indicating a simultaneous bind condition for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyUnknownHA

> Object ID: | enterprises.8164.1.22.1.1.33

> Description: | The number of session registration replies indicating unknown home agent for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyRevTunUnavail

> Object ID: | enterprises.8164.1.22.1.1.34

> Description: | The number of session registration replies indicating no reverse tunnel available for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyRevTunMand

> Object ID: | enterprises.8164.1.22.1.1.35

> Description: | The number of session registration replies indicating reverse tunneling is mandatory for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplyEncapUnavail

> Object ID: | enterprises.8164.1.22.1.1.36

> Description: | The number of session registration replies indicating IP encapsulation was not available for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegReplySendError

> Object ID: | enterprises.8164.1.22.1.1.37

> Description: | The number of session registration replies indicating a send error occurred for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatFARevocations

> Object ID: | enterprises.8164.1.22.1.1.38

> Description: | The number of FA revocations for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegAcceptHO

> Object ID: | enterprises.8164.1.22.1.1.39

> Description: | The number of hand over session registrations accepted for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDeniedHO

> Object ID: | enterprises.8164.1.22.1.1.40

> Description: | The number of hand over session registrations denied for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPHAStatRegDiscardTotal

> Object ID: | enterprises.8164.1.22.1.1.41

> Description: | The number of session registrations discarded for the associated Mobile IP home agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentMIPFA(23)

> Object: | starMIPFAStatTable

> Object ID: | enterprises.8164.1.23.1

> Description: | A table containing the Mobile IP Foreign Agent statistics.

> Syntax: | Sequence of starMIPFAStatEntry

> Access: | Not-accessible

> Description: | A table containing MIP FA statistics

> Object: | starMIPFAStatEntry

> Object ID: | enterprises.8164.1.23.1.1.

> Description: | The statistics for a specific foreign agent Mobile IP VPN (context) service.

> Syntax: | starMIPFAStatEntry

> Access: | Not-accessible

> Sequence: | starMIPFAStatVpnID starMIPFAStatSvcID Index (Implied) starMIPFAStatVpnName starMIPFAStatServName starMIPFAAdvertSend starMIPFADiscExpiry starMIPFADiscDereg starMIPFADiscAdmin starMIPFAAuthAttempt starMIPFAAuthSuccess starMIPFAAuthFailure starMIPFARegRecvTotal starMIPFARegRecvInitial starMIPFARegRecvRenewal starMIPFARegRecvDereg starMIPFARegAcceptTotal starMIPFARegAcceptInitial starMIPFARegAcceptRenewal starMIPFARegAcceptDereg starMIPFARegDenTotal starMIPFARegDenInitial starMIPFARegDenRenewal starMIPFARegDenDereg starMIPFARegDiscardTotal starMIPFARegDiscardInitial starMIPFARegDiscardRenewal starMIPFARegDiscardDereg starMIPFARegRelayedTotal starMIPFARegRelayedInitial starMIPFARegRelayedRenewal starMIPFARegRelayedDereg starMIPFARegAuthFailTotal starMIPFARegAuthFailInitial starMIPFARegAuthFailRenewal starMIPFARegAuthFailDereg starMIPFARegDenPDSNTotal starMIPFARegDenPDSNInitial starMIPFARegDenPDSNRenewal starMIPFARegDenPDSNDereg starMIPFARegDenHATotal starMIPFARegDenHAInitial starMIPFARegDenHARenewal starMIPFARegDenHADereg starMIPFARegDenPDSNUnspec starMIPFARegDenPDSNTimeout starMIPFARegDenPDSNAdmin starMIPFARegDenPDSNResources starMIPFARegDenPDSNMnAuth starMIPFARegDenPDSNHAAuth starMIPFARegDenPDSNTooLong starMIPFARegDenPDSNBadReq starMIPFARegDenPDSNEncapUnav starMIPFARegDenPDSNRevTunUnav starMIPFARegDenPDSNRevTunMand starMIPFARegDenHAFAAuth starMIPFARegDenHABadReq starMIPFARegDenHAMismatchID starMIPFARegDenHASimulBind starMIPFARegDenHAUnknownHA starMIPFARegDenHARevRunUnavail starMIPFARegRplRcvTotal starMIPFARegRplRcvTotalRly starMIPFARegRplRcvErrors starMIPFARegRplRcvInitial starMIPFARegRplRcvInitialRly starMIPFARegRplRcvRenewal starMIPFARegRplRcvRenewalRly starMIPFARegRplRcvDereg starMIPFARegRplRcvDeregRly starMIPFARegRplSentTotal starMIPFARegRplSentAcceptReg starMIPFARegRplSentAcceptDereg starMIPFARegRplSentBadReq starMIPFARegRplSentTooLong starMIPFARegRplSentMnAuthFail starMIPFARegRplSentHAAuthFail starMIPFARegRplSentAdminProhib starMIPFARegRplSentNoResources starMIPFARegRplSentRevTunUnavail starMIPFARegRplSentRevTunMand starMIPFARegRplSentSendErrors starMIPFAStatRegDenPDSNBadReply starMIPFAStatRegDenPDSNMissNAI starMIPFAStatRegDenPDSNMissHomeAgent starMIPFAStatRegDenPDSNMissHomeAddr starMIPFAStatRegDenPDSNUnknChallenge starMIPFAStatRegDenPDSNMissChallenge starMIPFAStatRegDenPDSNStaleChallenge starMIPFAStatRegDenPDSNMNTooDistant starMIPFAStatRegDenPDSNStyleUnavail starMIPFAStatRegDenPDSNHANetUnreach starMIPFAStatRegDenPDSNHAHostUnreach starMIPFAStatRegDenPDSNHAPortUnreach starMIPFAStatRegDenPDSNHAUnreach starMIPFAStatRegDenPDSNInvCOA starMIPFAStatRegReqSentInitTotal starMIPFAStatRegReqSentInitResend starMIPFAStatRegReqSentRenewTotal starMIPFAStatRegReqSentRenewResend starMIPFAStatRegReqSentDeregTotal starMIPFAStatRegReqSentDeregResend starMIPFAStatRegRplSentMNTooDistant starMIPFAStatRegRplSentInvCOA starMIPFAStatRegRplSentHANetUnreach starMIPFAStatRegRplSentHAHostUnreach starMIPFAStatRegRplSentHAPortUnreach starMIPFAStatRegRplSentHAUnreach starMIPFAStatRegRplSentRegTimeout starMIPFAStatRegRplSentMissNAI starMIPFAStatRegRplSentMissHomeAgent starMIPFAStatRegRplSentMissHomeAddr starMIPFAStatRegRplSentUnknChallenge starMIPFAStatRegRplSentMissChallenge starMIPFAStatRegRplSentStaleChallenge starMIPFAStatRegRplSentBadReply

> Object: | starMIPFAStatVpnID

> Object ID: | enterprises.8164.1.23.1.1.1

> Description: | Internal identification of the foreign agent Mobile IP VPN (context).

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starMIPFAStatSvcID

> Object ID: | enterprises.8164.1.23.1.1.2

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

> Syntax: | StarShortID

> Access: | Not-accessible

> Object: | starMIPFAStatVpnName

> Object ID: | enterprises.8164.1.23.1.1.3

> Description: | The foreign agent mobile IP VPN (context) name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starMIPFAStatServName

> Object ID: | enterprises.8164.1.23.1.1.4

> Description: | The Mobile IP foreign agent service name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starMIPFAStatAdvertSend

> Object ID: | enterprises.8164.1.23.1.1.5

> Description: | The number of advertisements sent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatDiscExpiry

> Object ID: | enterprises.8164.1.23.1.1.6

> Description: | The number of session disconnects due to expiration for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatDiscDereg

> Object ID: | enterprises.8164.1.23.1.1.7

> Description: | The number of session disconnects due to deregistration requests for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatDiscAdmin

> Object ID: | enterprises.8164.1.23.1.1.8

> Description: | The number of session disconnects due to administrator action for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatAuthAttempt

> Object ID: | enterprises.8164.1.23.1.1.9

> Description: | The number of session authentication attempts for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatAuthSuccess

> Object ID: | enterprises.8164.1.23.1.1.10

> Description: | The number of session authentication successes for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatAuthFailure

> Object ID: | enterprises.8164.1.23.1.1.11

> Description: | The number of session authentication failures for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRecvTotal

> Object ID: | enterprises.8164.1.23.1.1.12

> Description: | The total number of session registrations received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRecvInitial

> Object ID: | enterprises.8164.1.23.1.1.13

> Description: | The number of initial session registrations received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRecvRenewal

> Object ID: | enterprises.8164.1.23.1.1.14

> Description: | The number of session registration renewals for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRecvDereg

> Object ID: | enterprises.8164.1.23.1.1.15

> Description: | The number of session deregistrations for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAcceptTotal

> Object ID: | enterprises.8164.1.23.1.1.16

> Description: | The total number of session registrations accepted for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAcceptInitial

> Object ID: | enterprises.8164.1.23.1.1.17

> Description: | The number of initial session registrations accepted for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAcceptRenewal

> Object ID: | enterprises.8164.1.23.1.1.18

> Description: | The number of session registration renewals accepted for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAcceptDereg

> Object ID: | enterprises.8164.1.23.1.1.19

> Description: | The number of session deregistrations accepted for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenTotal

> Object ID: | enterprises.8164.1.23.1.1.20

> Description: | The total number of session registrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenInitial

> Object ID: | enterprises.8164.1.23.1.1.21

> Description: | The number of initial session registrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenRenewal

> Object ID: | enterprises.8164.1.23.1.1.22

> Description: | The number of session registration renewals denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenDereg

> Object ID: | enterprises.8164.1.23.1.1.23

> Description: | The number of session deregistrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDiscardTotal

> Object ID: | enterprises.8164.1.23.1.1.24

> Description: | The total number of session registrations discarded for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDiscardInitial

> Object ID: | enterprises.8164.1.23.1.1.25

> Description: | The number of initial session registrations discarded for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDiscardRenewal

> Object ID: | enterprises.8164.1.23.1.1.26

> Description: | The number of session registration renewals discarded for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDiscardDereg

> Object ID: | enterprises.8164.1.23.1.1.27

> Description: | The number of session deregistrations discarded for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRelayedTotal

> Object ID: | enterprises.8164.1.23.1.1.28

> Description: | The total number of session registrations relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRelayedInitial

> Object ID: | enterprises.8164.1.23.1.1.29

> Description: | The number of initial session registrations relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRelayedRenewal

> Object ID: | enterprises.8164.1.23.1.1.30

> Description: | The number of session registration renewals relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRelayedDereg

> Object ID: | enterprises.8164.1.23.1.1.31

> Description: | The number of session deregistrations relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAuthFailTotal

> Object ID: | enterprises.8164.1.23.1.1.32

> Description: | The total number of session registration authentication failures for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAuthFailInitial

> Object ID: | enterprises.8164.1.23.1.1.33

> Description: | The number of initial session registration failures for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAuthFailRenewal

> Object ID: | enterprises.8164.1.23.1.1.34

> Description: | The number of session registration renewal failures for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegAuthFailDereg

> Object ID: | enterprises.8164.1.23.1.1.35

> Description: | The number of session deregistration authentication failures for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNTotal

> Object ID: | enterprises.8164.1.23.1.1.36

> Description: | The total number of PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNInitial

> Object ID: | enterprises.8164.1.23.1.1.37

> Description: | The number of initial PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNRenewal

> Object ID: | enterprises.8164.1.23.1.1.38

> Description: | The number of PDSN session registration renewals denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNDereg

> Object ID: | enterprises.8164.1.23.1.1.39

> Description: | The number of PDSN session deregistrations denied for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHATotal

> Object ID: | enterprises.8164.1.23.1.1.40

> Description: | The total number of session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHAInitial

> Object ID: | enterprises.8164.1.23.1.1.41

> Description: | The number of initial session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHARenewal

> Object ID: | enterprises.8164.1.23.1.1.42

> Description: | The number of session registration renewals denied by the home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHADereg

> Object ID: | enterprises.8164.1.23.1.1.43

> Description: | The number of session deregistrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNUnspec

> Object ID: | enterprises.8164.1.23.1.1.44

> Description: | The number of PDSN session registrations denied for an unspecified reason for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNTimeout

> Object ID: | enterprises.8164.1.23.1.1.45

> Description: | The number of PDSN session registrations denied due to timer expiration for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNAdmin

> Object ID: | enterprises.8164.1.23.1.1.46

> Description: | The number of PDSN session registration denied due administrator prohibition for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNResources

> Object ID: | enterprises.8164.1.23.1.1.47

> Description: | The number of PDSN session registrations denied due to no resources for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMnAuth

> Object ID: | enterprises.8164.1.23.1.1.48

> Description: | The number of PDSN session registrations denied due to mobile number authentication failure for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNHAAuth

> Object ID: | enterprises.8164.1.23.1.1.49

> Description: | The number of PDSN session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNTooLong

> Object ID: | enterprises.8164.1.23.1.1.50

> Description: | The number of PDSN session registrations denied due to a life too lone indication for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNBadReq

> Object ID: | enterprises.8164.1.23.1.1.51

> Description: | The number of PDSN session registration denied due to a bad request indication for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNEncapUnav

> Object ID: | enterprises.8164.1.23.1.1.52

> Description: | The number of PDSN session registration denied due to no IP encapsulation available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDeniedPDSNRevTunUnav

> Object ID: | enterprises.8164.1.23.1.1.53

> Description: | The number of PDSN session registrations denied due to no reverse tunnel available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNRevTunMand

> Object ID: | enterprises.8164.1.23.1.1.54

> Description: | The number of PDSN session registration denied due to reverse tunneling being mandatory for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHAFAAuth

> Object ID: | enterprises.8164.1.23.1.1.55

> Description: | The number of session registrations denied by the home agent due to authentication failure for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHABadReq

> Object ID: | enterprises.8164.1.23.1.1.56

> Description: | The number of session registration denied by the home agent due to the request being invalid for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHAMismatchID

> Object ID: | enterprises.8164.1.23.1.1.57

> Description: | The number of session registrations denied by the home agent due to an ID mismatch for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHASimulBind

> Object ID: | enterprises.8164.1.23.1.1.58

> Description: | The number of session registrations denied by the home agent due to a simultaneous bind attempt for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHAUnknownHA

> Object ID: | enterprises.8164.1.23.1.1.59

> Description: | The number of session registrations denied by the home agent for an unknown reason for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenHARevRunUnavail

> Object ID: | enterprises.8164.1.23.1.1.60

> Description: | The number of session registrations denied by the home agent due to no reverse tunnel being available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvTotal

> Object ID: | enterprises.8164.1.23.1.1.61

> Description: | The total number of session registration replies received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvTotalRly

> Object ID: | enterprises.8164.1.23.1.1.62

> Description: | The total number of session registration replies relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvErrors

> Object ID: | enterprises.8164.1.23.1.1.63

> Description: | The number of session registration replies received indicating errors for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvInitial

> Object ID: | enterprises.8164.1.23.1.1.64

> Description: | The number of initial session registration replies received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvInitialRly

> Object ID: | enterprises.8164.1.23.1.1.65

> Description: | The number of initial session registration replies relayed for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvRenewal

> Object ID: | enterprises.8164.1.23.1.1.66

> Description: | The number of session registration renewal replies received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvRenewalRly

> Object ID: | enterprises.8164.1.23.1.1.67

> Description: | The number of session registration replies relayed received for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvDereg

> Object ID: | enterprises.8164.1.23.1.1.68

> Description: | The number of session registration replies received indicating deregistration for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplRcvDeregRly

> Object ID: | enterprises.8164.1.23.1.1.69

> Description: | The number of session registration replies relayed indicating deregistration for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentTotal

> Object ID: | enterprises.8164.1.23.1.1.70

> Description: | The total number of session registration replies sent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentAcceptReg

> Object ID: | enterprises.8164.1.23.1.1.71

> Description: | The number of session registration replies which were sent and accepted for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentAcceptDereg

> Object ID: | enterprises.8164.1.23.1.1.72

> Description: | The number of session registration replies which were sent and accepted indicating deregistration for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentBadReq

> Object ID: | enterprises.8164.1.23.1.1.73

> Description: | The number of session registration replies which were sent indicating the request was invalid for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentTooLong

> Object ID: | enterprises.8164.1.23.1.1.74

> Description: | The number of session registration replies which were sent indicating life too long for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMnAuthFail

> Object ID: | enterprises.8164.1.23.1.1.75

> Description: | The number of session registration replies which were sent indicating mobile number authentication failure for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentHAAuthFail

> Object ID: | enterprises.8164.1.23.1.1.76

> Description: | The number of session registration replies which were sent indicating for home agent authentication failure the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentAdminProhib

> Object ID: | enterprises.8164.1.23.1.1.77

> Description: | The number of session registration replies which were sent indicating prohibited by the administrator for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentNoResources

> Object ID: | enterprises.8164.1.23.1.1.78

> Description: | The number of session registration replies which were sent indicating no resources available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentRevTunUnavail

> Object ID: | enterprises.8164.1.23.1.1.79

> Description: | The number of session registration replies which were sent indicating no reverse tunnel available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentRevTunMand

> Object ID: | enterprises.8164.1.23.1.1.80

> Description: | The number of session registration replies which were sent indicating reverse tunneling was mandatory for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentSendErrors

> Object ID: | enterprises.8164.1.23.1.1.81

> Description: | The number of session registration replies which were sent indicating there were errors in transmission for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNBadReply

> Object ID: | enterprises.8164.1.23.1.1.82

> Description: | The number of session registrations denied by PDSN due to bad reply from HA for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMissNAI

> Object ID: | enterprises.8164.1.23.1.1.83

> Description: | The number of session registrations denied by PDSN due to missing NAI for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMissHomeAgent

> Object ID: | enterprises.8164.1.23.1.1.84

> Description: | The number of session registrations denied by PDSN due to missing home agent for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMissHomeAddr

> Object ID: | enterprises.8164.1.23.1.1.85

> Description: | The number of session registrations denied by PDSN due to missing home address for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNUnknChallenge

> Object ID: | enterprises.8164.1.23.1.1.86

> Description: | The number of session registrations denied by PDSN due to unknown challenge for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMissChallenge

> Object ID: | enterprises.8164.1.23.1.1.87

> Description: | The number of session registrations denied by PDSN due to missing challenge for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNStaleChallenge

> Object ID: | enterprises.8164.1.23.1.1.88

> Description: | The number of session registrations denied by PDSN due to stale challenge for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNMNTooDistant

> Object ID: | enterprises.8164.1.23.1.1.89

> Description: | The number of session registrations denied by PDSN due to MN too distant for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNStyleUnavail

> Object ID: | enterprises.8164.1.23.1.1.90

> Description: | The number of session registration denied by PDSN due to style not available for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNHANetUnreach

> Object ID: | enterprises.8164.1.23.1.1.91

> Description: | The number of session registrations denied by PDSN due to HA network unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNHAHostUnreach

> Object ID: | enterprises.8164.1.23.1.1.92

> Description: | The number of session registrations denied by PDSN due to HA host unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNHAPortUnreach

> Object ID: | enterprises.8164.1.23.1.1.93

> Description: | The number of session registrations denied by PDSN due to HA port unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNHAUnreach

> Object ID: | enterprises.8164.1.23.1.1.94

> Description: | The number of session registrations denied by PDSN due to HA unreachable for miscellaneous reasons for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegDenPDSNInvCOA

> Object ID: | enterprises.8164.1.23.1.1.95

> Description: | The number of session registrations denied by PDSN due to invalid COA for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentInitTotal

> Object ID: | enterprises.8164.1.23.1.1.96

> Description: | The number of initial session registrations for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentInitResend

> Object ID: | enterprises.8164.1.23.1.1.97

> Description: | The number of initial session registrations retried for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentRenewTotal

> Object ID: | enterprises.8164.1.23.1.1.98

> Description: | The number of renewal session registrations for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentRenewResend

> Object ID: | enterprises.8164.1.23.1.1.99

> Description: | The number of renewal session registrations retried for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentDeregTotal

> Object ID: | enterprises.8164.1.23.1.1.100

> Description: | The number of session deregistrations for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegReqSentDeregResend

> Object ID: | enterprises.8164.1.23.1.1.101

> Description: | The number of session deregistrations retried for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMNTooDistant

> Object ID: | enterprises.8164.1.23.1.1.102

> Description: | The number of session registration reply that indicate MN too distant for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentInvCOA

> Object ID: | enterprises.8164.1.23.1.1.103

> Description: | The number of session registration reply that indicate invalid COA for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentHANetUnreach

> Object ID: | enterprises.8164.1.23.1.1.104

> Description: | The number of session registration reply that indicate HA network unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentHAHostUnreach

> Object ID: | enterprises.8164.1.23.1.1.105

> Description: | The number of session registration reply that indicate HA host unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentHAPortUnreach

> Object ID: | enterprises.8164.1.23.1.1.106

> Description: | The number of session registration reply that indicate HA port unreachable for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentHAUnreach

> Object ID: | enterprises.8164.1.23.1.1.107

> Description: | The number of session registration reply that indicate HA unreachable due to miscellaneous reasons for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentRegTimeout

> Object ID: | enterprises.8164.1.23.1.1.108

> Description: | The number of session registration reply that indicate registration time out for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMissNAI

> Object ID: | enterprises.8164.1.23.1.1.109

> Description: | The number of session registration reply that indicate NAI missing for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMissHomeAgent

> Object ID: | enterprises.8164.1.23.1.1.110

> Description: | The number of session registration reply that indicate HA missing for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMissHomeAddr

> Object ID: | enterprises.8164.1.23.1.1.111

> Description: | The number of session registration reply that indicate home address missing for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentUnknChallenge

> Object ID: | enterprises.8164.1.23.1.1.112

> Description: | The number of session registration reply that indicate unknown challenge for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentMissChallenge

> Object ID: | enterprises.8164.1.23.1.1.113

> Description: | The number of session registration reply that indicate challenge missing for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentStaleChallenge

> Object ID: | enterprises.8164.1.23.1.1.114

> Description: | The number of session registration reply that indicate stale challenge for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starMIPFAStatRegRplSentBadReply

> Object ID: | enterprises.8164.1.23.1.1.115

> Description: | The number of session registration reply that indicate bad reply for the associated Mobile IP foreign agent VPN service.

> Syntax: | Counter32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentRP(24)

> Object: | starRPStatTable

> Object ID: | enterprises.8164.1.24.1

> Description: | A table containing the R-P interface statistics.

> Syntax: | Sequence of starMIPFAStatEntry

> Access: | Not-accessible

> Description: | A table containing MIP FA statistics

> Object: | starRPStatEntry

> Object ID: | enterprises.8164.1.24.1.1

> Description: | The statistics for a specific R-P VPN (context) service.

> Syntax: | starRPStatEntry

> Access: | Not-accessible

> Sequence: | starRPStatVpnID starRPStatSvcID Index (Implied) starRPStatVpnName starRPStatServName starRPRegRecvTotal starRPRegAcceptTotal starRPRegDeniedTotal starRPRegDiscardTotal starRPRegAcceptInitial starRPRegAcceptIntraPDSN starRPRegAcceptInterPDSN starRPRegDeniedInitial starRPRegAcceptRenew starRPRegDeniedRenew starRPRegAcceptDereg starRPRegDeniedDereg starRPRegSendError starRPRegHashError starRPRegDecodeError starRPRegUnhandled starRPRegAirlinkSeqError starRPRegDenyUnspec starRPRegDenyAdminProhib starRPRegDenyNoResource starRPRegDenyAuth starRPRegDenyMismatchID starRPRegDenyBadRequest starRPRegDenyUnknownPDSN starRPRegDenyRevTunUnav starRPRegDenyRevTunReq starRPRegDenyUnrecogVend starRPRegUpdTotal starRPRegUpdAccept starRPRegUpdDenied starRPRegUpdUnack starRPRegUpdTrans starRPRegUpdRetrans starRPRegUpdReceived starRPRegUpdDiscard starRPRegUpdSendError starRPRegUpdUplyrInit starRPRegUpdOther starRPRegUpdHandoff starRPRegUpdDenyUnspec starRPRegUpdDenyAdminProhib starRPRegUpdDenyAuth starRPRegUpdDenyMismatchID starRPRegUpdDenyBadRequest starRPSecViolations starRPSecBadAuth starRPSecBadID starRPSecBadSpi starRPSecMissingMnHAAuth starRPSecMissingRegUpdate starRPRegRecvInitial starRPRegAcceptActvStartIntraPDSN starRPRegAcceptActvStopIntraPDSN starRPRegRecvRenew starRPRegActvStartRenew starRPRegActvStopRenew starRPRegRecvDereg starRPRegAcceptActvStopDereg starRPDiscSessAbsent starRPDiscNoMemory starRPDiscMalformed starRPDiscAuthFail starRPDiscInternalBounce starRPDiscInpuQueueExceeded starRPDiscMismatchedId starRPDiscInvPacketLen starRPDiscMisc

> Object: | starRPStatVpnID

> Object ID: | enterprises.8164.1.24.1.1.1

> Description: | The internal identification of the R-P VPN (context).

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starRPStatSvcID

> Object ID: | enterprises.8164.1.24.1.1.2

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

> Syntax: | StarShortID

> Access: | Not-accessible

> Object: | starRPStatVpnName

> Object ID: | enterprises.8164.1.24.1.1.3

> Description: | The R-P VPN (context) name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starRPStatServName

> Object ID: | enterprises.8164.1.24.1.1.4

> Description: | The R-P service name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starRPRegRecvTotal

> Object ID: | enterprises.8164.1.24.1.1.5

> Description: | The total number of session registrations received for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptTotal

> Object ID: | enterprises.8164.1.24.1.1.6

> Description: | The total number of session registrations accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDeniedTotal

> Object ID: | enterprises.8164.1.24.1.1.7

> Description: | The total number of session registrations denied for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDiscardTotal

> Object ID: | enterprises.8164.1.24.1.1.8

> Description: | The total number of session registrations discarded for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptInitial

> Object ID: | enterprises.8164.1.24.1.1.9

> Description: | The total number of initial session registrations accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptIntraPDSN

> Object ID: | enterprises.8164.1.24.1.1.10

> Description: | The number of Intra-PDSN session registrations accepted for the associated R-P VPN service.

> Syntax: | Gauge32

> Access: | Read-only

> IMPORTANT: Status of this alarm is obsolete.

> Object: | starRPRegAcceptInterPDSN

> Object ID: | enterprises.8164.1.24.1.1.11

> Description: | The number of Inter-PDSN session registrations accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDeniedInitial

> Object ID: | enterprises.8164.1.24.1.1.12

> Description: | The number of initial session registrations denied for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptRenew

> Object ID: | enterprises.8164.1.24.1.1.13

> Description: | The number of session registration renewals accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDeniedRenew

> Object ID: | enterprises.8164.1.24.1.1.14

> Description: | The number of session registration renewals denied for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptDereg

> Object ID: | enterprises.8164.1.24.1.1.15

> Description: | The number of session deregistrations accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDeniedDereg

> Object ID: | enterprises.8164.1.24.1.1.16

> Description: | The number of session deregistrations denied accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegSendError

> Object ID: | enterprises.8164.1.24.1.1.17

> Description: | The number of session registrations with errors in transmission for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegHashError

> Object ID: | enterprises.8164.1.24.1.1.18

> Description: | The number of session registrations with hash errors for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDecodeError

> Object ID: | enterprises.8164.1.24.1.1.19

> Description: | The number of session registrations with decode errors for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUnhandled

> Object ID: | enterprises.8164.1.24.1.1.20

> Description: | The number of session registrations not processed for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAirlinkSeqError

> Object ID: | enterprises.8164.1.24.1.1.21

> Description: | The number of session registrations with air link sequence errors for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyUnspec

> Object ID: | enterprises.8164.1.24.1.1.22

> Description: | The number of session registrations denied for an unspecified reason for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyAdminProhib

> Object ID: | enterprises.8164.1.24.1.1.23

> Description: | The number of session registrations denied due to administrator prohibition for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyNoResource

> Object ID: | enterprises.8164.1.24.1.1.24

> Description: | The number of session registrations denied due to no resources available for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyAuth

> Object ID: | enterprises.8164.1.24.1.1.25

> Description: | The number of session registrations denied due to authentication failure for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyMismatchID

> Object ID: | enterprises.8164.1.24.1.1.26

> Description: | The number of session registrations denied due to an ID mismatch for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyBadRequest

> Object ID: | enterprises.8164.1.24.1.1.27

> Description: | The number of session registrations denied due to the request being invalid for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyUnknownPDSN

> Object ID: | enterprises.8164.1.24.1.1.28

> Description: | The number of session registrations denied due to the packet data service not being recognized for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyRevTunUnav

> Object ID: | enterprises.8164.1.24.1.1.29

> Description: | The number of session registrations denied due to no reverse tunnel being available for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyRevTunReq

> Object ID: | enterprises.8164.1.24.1.1.30

> Description: | The number of session registrations denied due to reverse tunneling being mandatory for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegDenyUnrecogVend

> Object ID: | enterprises.8164.1.24.1.1.31

> Description: | The number of session registrations denied due to the vendor not being recognized for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdTotal

> Object ID: | enterprises.8164.1.24.1.1.32

> Description: | The total number of session registration updates for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdAccept

> Object ID: | enterprises.8164.1.24.1.1.33

> Description: | The number of session registration updates which were accepted for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenied

> Object ID: | enterprises.8164.1.24.1.1.34

> Description: | The number of session registration updates denied for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdUnack

> Object ID: | enterprises.8164.1.24.1.1.35

> Description: | The number of session registration updates which were not acknowledged for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdTrans

> Object ID: | enterprises.8164.1.24.1.1.36

> Description: | The number of session registration updates sent for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdRetrans

> Object ID: | enterprises.8164.1.24.1.1.37

> Description: | The number of session registration updates resent for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdReceived

> Object ID: | enterprises.8164.1.24.1.1.38

> Description: | The number of session registration updates received for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDiscard

> Object ID: | enterprises.8164.1.24.1.1.39

> Description: | The number of session registration updates discarded for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdSendError

> Object ID: | enterprises.8164.1.24.1.1.40

> Description: | The number of session registration updates with errors in transmission for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdUplyrInit

> Object ID: | enterprises.8164.1.24.1.1.41

> Description: | The number of session registration updates with up-link re-initializations.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdOther

> Object ID: | enterprises.8164.1.24.1.1.42

> Description: | The number of session registration updates with a reason of ‘other’ for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdHandoff

> Object ID: | enterprises.8164.1.24.1.1.43

> Description: | The number of session registration updates due to a mobile hand-off for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenyUnspec

> Object ID: | enterprises.8164.1.24.1.1.44

> Description: | The number of session registration updates denied for an unspecified reason for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenyAdminProhib

> Object ID: | enterprises.8164.1.24.1.1.45

> Description: | The number of session registration updates denied due to administrator prohibition for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenyAuth

> Object ID: | enterprises.8164.1.24.1.1.46

> Description: | The number of session registration updates denied due to authentication failure for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenyMismatchID

> Object ID: | enterprises.8164.1.24.1.1.47

> Description: | The number of session registration updates denied due to an ID mismatch for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegUpdDenyBadRequest

> Object ID: | enterprises.8164.1.24.1.1.48

> Description: | The number of session registration updates denied due to the request being invalid for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecViolations

> Object ID: | enterprises.8164.1.24.1.1.49

> Description: | The total number of session security violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecBadAuth

> Object ID: | enterprises.8164.1.24.1.1.50

> Description: | The total number of session security authentication violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecBadID

> Object ID: | enterprises.8164.1.24.1.1.51

> Description: | The total number of session security ID violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecBadSpi

> Object ID: | enterprises.8164.1.24.1.1.52

> Description: | The total number of session security SPI violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecMissingMnHAAuth

> Object ID: | enterprises.8164.1.24.1.1.53

> Description: | The total number of session security missing mobile number home agent authentication violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPSecMissingRegUpdate

> Object ID: | enterprises.8164.1.24.1.1.54

> Description: | The total number of session missing registration update violations for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegRecvInitial

> Object ID: | enterprises.8164.1.24.1.1.55

> Description: | The total number of initial session registration for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptActvStartIntraPDSN

> Object ID: | enterprises.8164.1.24.1.1.56

> Description: | The number of accepted registration request during intra-PDSN handoffs which contains active start for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptActvStopIntraPDSN

> Object ID: | enterprises.8164.1.24.1.1.57

> Description: | The number of accepted registration request during intraPDSN handoff which contains active stop for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegRecvRenew

> Object ID: | enterprises.8164.1.24.1.1.58

> Description: | The number of received renew registration request for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegActvStartRenew

> Object ID: | enterprises.8164.1.24.1.1.59

> Description: | The number of received renew registration request that contains active start for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegActvStopRenew

> Object ID: | enterprises.8164.1.24.1.1.60

> Description: | The number of received renew registration request that contains active stop for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegRecvDereg

> Object ID: | enterprises.8164.1.24.1.1.61

> Description: | The number of received deregistration request for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPRegAcceptActvStopDereg

> Object ID: | enterprises.8164.1.24.1.1.62

> Description: | The number of accepted deregistration request that contains active stop for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscSessAbsent

> Object ID: | enterprises.8164.1.24.1.1.63

> Description: | The number of registration request discarded due to no session for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscNoMemory

> Object ID: | enterprises.8164.1.24.1.1.64

> Description: | The number of registration request discarded due to no memory for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscMalformed

> Object ID: | enterprises.8164.1.24.1.1.65

> Description: | The number of registration request discarded because malformed for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscAuthFail

> Object ID: | enterprises.8164.1.24.1.1.66

> Description: | The number of registration request discarded because authentication failed for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscInternalBounce

> Object ID: | enterprises.8164.1.24.1.1.67

> Description: | The number of registration request discarded because internal bounce for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscInpuQueueExceeded

> Object ID: | enterprises.8164.1.24.1.1.68

> Description: | The number of registration request discarded because internal queue exceeded for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscMismatchedId

> Object ID: | enterprises.8164.1.24.1.1.69

> Description: | The number of registration request discarded because mismatched ID for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscInvPacketLen

> Object ID: | enterprises.8164.1.24.1.1.70

> Description: | The number of registration request discarded because invalid packet length for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starRPDiscMisc

> Object ID: | enterprises.8164.1.24.1.1.71

> Description: | The number of registration request discarded due to misc. reasons for the associated R-P VPN service.

> Syntax: | Counter32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSubscriber(26)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starSubTable

> Object ID: | enterprises.8164.1.26.1

> Description: | A table containing subscriber information.

> Syntax: | SEQUENCE OF starSubEntry

> Access: | Not-accessible

> Object: | starSubEntry

> Object ID: | enterprises.8164.1.26.1.1

> Description: | Information for a specific Subscriber.

> Syntax: | starSubEntry

> Access: | Not-accessible

> Sequence: | starSubContext starSubMSID Index starSubName Index starSubTimerDuration starSubLongDurTimeoutAction starSubSetupTime starSubHomeAddr starSubHomeAddrv6

> Object: | starSubContext

> Object ID: | enterprises.8164.1.26.1.1.1

> Description: | The context the subscriber is in.

> Syntax: | DisplayString

> Access: | accessible-for-notify

> Object: | starSubMSID

> Object ID: | enterprises.8164.1.26.1.1.2

> Description: | The MSID of the subscriber.

> Syntax: | OCTET STRING (SIZE (1..16))

> Access: | Not-accessible

> Object: | starSubName

> Object ID: | enterprises.8164.1.26.1.1.3

> Description: | The name of the subscriber.

> Syntax: | OCTET STRING (SIZE (1..128))

> Access: | Not-accessible

> Object: | starSubTimerDuration

> Object ID: | enterprises.8164.1.26.1.1.4

> Description: | The length of the long-duration timer in seconds

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starSubLongDurTimeoutAction

> Object ID: | enterprises.8164.1.26.1.1.5

> Description: | he action taken by the system upon detection of a long-duration session.

> Syntax: | StarLongDurTimeoutAction

> Access: | Read-only

> Object: | starSubSetupTime

> Object ID: | enterprises.8164.1.26.1.1.6

> Description: | The time when the call was setup.

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starSubHomeAddr

> Object ID: | enterprises.8164.1.26.1.1.7

> Description: | The IPv4 home address.

> Syntax: | IPv4Address

> Access: | Read-only

> Object: | starSubHomeAddrv6

> Object ID: | enterprises.8164.1.26.1.1.8

> Description: | The IPv6 home address.

> Syntax: | IPv6Address

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentEISServer(27)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starEISServerTable

> Object ID: | enterprises.8164.1.27.1

> Description: | A table containing EIS Server information.

> Syntax: | SEQUENCE OF StarEISServerEntry

> Access: | Not-accessible

> Object: | starEISServerEntry

> Object ID: | enterprises.8164.1.27.1.1

> Description: | Information for a specific EIS Server.

> Syntax: | StarEISServerEntry

> Access: | Not-accessible

> Sequence: | starEISServerVPNID Index starEISServerAddr Index starEISServerVPNName

> Object: | starEISServerVPNID

> Object ID: | enterprises.8164.1.27.1.1.1

> Description: | The VPN ID for the EIS Server.

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starEISServerAddr

> Object ID: | enterprises.8164.1.27.1.1.2

> Description: | The IP Address for the EIS Server.

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starEISServerVPNName

> Object ID: | enterprises.8164.1.27.1.1.3

> Description: | The VPN Name for this EIS Server.

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentThresholds(28)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starThreshMeasuredPct

> Object ID: | enterprises.8164.1.28.1

> Description: | The measured value of a thresholded parameter.

> Syntax: | INTEGER32(0..100)

> Access: | Accessible-for-notify

> Object: | starThreshPct

> Object ID: | enterprises.8164.1.28.2

> Description: | The configured value of a thresholded parameter.

> Syntax: | INTEGER32(0..100)

> Access: | Accessible-for-notify

> Object: | starThreshMeasuredInt

> Object ID: | enterprises.8164.1.28.3

> Description: | The measured value of a thresholded parameter.

> Syntax: | Guage32

> Access: | Accessible-for-notify

> Object: | starThreshInt

> Object ID: | enterprises.8164.1.28.4

> Description: | The configured value of a thresholded parameter.

> Syntax: | Unsigned32

> Access: | Accessible-for-notify

> Object: | starThreshMeasuredMB

> Object ID: | enterprises.8164.1.28.5

> Description: | The measured value of a thresholded parameter.

> Syntax: | Guard32

> Units: | Megabytes

> Access: | Accessible-for-notify

> Object: | starThreshMB

> Object ID: | enterprises.8164.1.28.6

> Description: | The configured value of a thresholded parameter

> Syntax: | Unsigned32

> Units: | Megabytes

> Access: | Accessible-for-notify

> Object: | starThreshMeasuredGB

> Object ID: | enterprises.8164.1.28.7

> Description: | The configured value of a thresholded parameter.

> Syntax: | Gauge32

> Units: | Gigabytes

> Access: | Accessible-for-notify

> Object: | starThreshGB

> Object ID: | enterprises.8164.1.28.8

> Description: | The configured value of a thresholded parameter.

> Syntax: | Unsigned32

> Units: | Gigabytes

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentPort(29)

> Object: | starPortTable

> Object ID: | enterprises.8164.1.29.1

> Description: | A table containing Port information.

> Syntax: | SEQUENCE OF starPortEntry

> Access: | Not-accessible

> Object: | starPortEntry

> Object ID: | enterprises.8164.1.29.1.1

> Description: | Information for a specific Port

> Syntax: | starPortEntry

> Access: | Not-accessible

> Sequence: | starPortSlot Integer32 starPortNum integer32 starPortType INTEGER starPortTypeDescr DisplayString starPortAdminState INTEGER starPortOperState INTEGER starPortOperMode INTEGER starPortLinkState INTEGER starRedundantPortSlot integer32 starRedundantPortNum integer32 starPortRXByte Counter32 starPortTXByte Counter32 starPortRXFrames Counter32 starPortTXFrames Counter32 starPortRxDiscards Counter32 starPortTxDiscards Counter32 starPortRxErrors Counter32 starPortTxErrors Counter32

> Object: | starPortSlot

> Object ID: | enterprises.8164.1.29.1.1.1

> Description: | The Slot number for this port.

> Syntax: | Integer32(1..48)

> Access: | Not-accessible

> Object: | starPortNum

> Object ID: | enterprises.8164.1.29.1.1.2

> Description: | The Port number within this slot.

> Syntax: | Integer32(1..8)

> Access: | Not-accessible

> Object: | starPortType

> Object ID: | enterprises.8164.1.29.1.1.3

> Description: | The type of the port.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | none(0) ethernet10100(1) ethernet1000dualmedia(2) ethernet1000(3) ds3(4) oc3(5) oc3atm(6) ds3e(7) rs232(8) bits1e1(9) virtualEthernet(10)

> Object: | starPortTypeDescr

> Object ID: | enterprises.8164.1.29.1.1.4

> Description: | A textual representation of the starPortType attribute

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starPortAdminState

> Object ID: | enterprises.8164.1.29.1.1.5

> Description: | The administrative start of the port

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starPortOperState

> Object ID: | enterprises.8164.1.29.1.1.6

> Description: | The operation status of the port

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) up(1) down(2) notapplicable(3)

> Object: | starPortOperMode

> Object ID: | enterprises.8164.1.29.1.1.7

> Description: | The operation mode of the port

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) active(1) standby(2)

> Object: | starPortLinkState

> Object ID: | enterprises.8164.1.29.1.1.8

> Description: | The link status of the port

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) up(1) down(2)

> Object: | starRedundantPortSlot

> Object ID: | enterprises.8164.1.29.1.1.9

> Description: | The slot number of the redundant port for the current port.

> Syntax: | Integer32(1..48)

> Access: | Read-only

> Object: | starRedundantPortNum

> Object ID: | enterprises.8164.1.29.1.1.10

> Description: | The port number of the redundant port for the current port

> Syntax: | Integer32(1..8)

> Access: | Read-only

> Object: | starPortRXBytes

> Object ID: | enterprises.8164.1.29.1.1.11

> Description: | The number of bytes successfully received, in megabytes. For ports of type rs232(8) for bitst1e1(9) this value will always be zero.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPortTXBytes

> Object ID: | enterprises.8164.1.29.1.1.12

> Description: | The number of bytes successfully transmitted in megabytes. For ports of type rs232(8) for bitst1e1(9) this value will always be zero.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPortRXFrames

> Object ID: | enterprises.8164.1.29.1.1.13

> Description: | The number of frames successfully received, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received.

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPortTXFrames

> Object ID: | enterprises.8164.1.29.1.1.14

> Description: | The number of frames successfully transmitted, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received..

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPortRxDiscards

> Object ID: | enterprises.8164.1.29.1.1.15

> Description: | The number of inbound packets which were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol. One possible reason for discarding such a packet could be to free up buffer space.

> Syntax: | Counter32

> Access: | read-only

> Object: | starPortTxDiscards

> Object ID: | enterprises.8164.1.29.1.1.16

> Description: | The number of outbound packets which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a packet could be to free up buffer space.

> Syntax: | Counter32

> Access: | read-only

> Object: | starPortRxErrors

> Object ID: | enterprises.8164.1.29.1.1.17

> Description: | The number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.

> Syntax: | Counter32

> Access: | read-only

> Object: | starPortTxErrors

> Object ID: | enterprises.8164.1.29.1.1.18

> Description: | The number of outbound packets that could not be transmitted because of errors.

> Syntax: | Counter32

> Access: | read-only

> Units: | Thousands

> starentMIB(8164).starentMIBObjects(1).starentIPPool(30)

> Object: | starIPPoolTable

> Object ID: | enterprises.8164.1.30.1

> Description: | A table containing IP Pool information.

> Syntax: | SEQUENCE OF StarIPPoolEntry

> Access: | Not-accessible

> Object: | starIPPoolEntry

> Object ID: | enterprises.8164.1.30.1.1

> Description: | Information for a specific IP Pool

> Syntax: | StarIPPoolEntry

> Access: | Not-accessible

> Sequence: | starIPPoolVpnID Gauge32 starIPPoolID StarMediumID starIPPoolContext DisplayString starIPPoolGroup DisplayString starIPPoolName OCTET STRING starIPPoolType INTEGER starIPPoolState INTEGER starIPPoolStartAddr IpAddress starIPPoolMaskorEndAddr IpAddress starIPPoolPriority Integer32 starIPPoolUsed Gauge32 starIPPoolHold Gauge32 starIPPoolRelease Gauge32 starIPPoolFree Gauge32

> Object: | starIPPoolVpnID

> Object ID: | enterprises.8164.1.30.1.1.1

> Description: | The context ID for this pool.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starIPPoolID

> Object ID: | enterprises.8164.1.30.1.1.2

> Description: | The service identification is made up from first 16 chars of context name and first 8 chars of pool name separated by (:).

> Syntax: | StarMediumID

> Access: | Not-accessible

> Object: | starIPPoolContext

> Object ID: | enterprises.8164.1.30.1.1.3

> Description: | The context for this pool.

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starIPPoolGroup

> Object ID: | enterprises.8164.1.30.1.1.4

> Description: | The name of the group to which the IP pool belongs.

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starIPPoolName

> Object ID: | enterprises.8164.1.30.1.1.5

> Description: | The name of the IP pool.

> Syntax: | OCTET STRING (SIZE (1..32))

> Access: | Not-accessible

> Object: | starIPPoolType

> Object ID: | enterprises.8164.1.30.1.1.6

> Description: | The type of the pool.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) private(1) public(2) static(3) resource(4), nat(5)

> Object: | starIPPoolState

> Object ID: | enterprises.8164.1.30.1.1.7

> Description: | The state of the pool.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) good(1) pendingdelete(2) alarm(3) resize(4) inactive(5)

> Object: | starIPPoolStartAddr

> Object ID: | enterprises.8164.1.30.1.1.8

> Description: | The start IP address of the pool.

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starIPPoolMaskorEndAddr

> Object ID: | enterprises.8164.1.30.1.1.9

> Description: | The mask or end IP address of the pool.

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starIPPoolPriority

> Object ID: | enterprises.8164.1.30.1.1.10

> Description: | The priority of the pool.

> Syntax: | Integer32

> Access: | Read-only

> Object: | starIPPoolUsed

> Object ID: | enterprises.8164.1.30.1.1.11

> Description: | The number of IP addresses in USED state in the pool.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starIPPoolHold

> Object ID: | enterprises.8164.1.30.1.1.12

> Description: | The number of IP addresses in HOLD state in the pool.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starIPPoolRelease

> Object ID: | enterprises.8164.1.30.1.1.13

> Description: | The number of IP addresses in RELEASE state in the pool.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starIPPoolFree

> Object ID: | enterprises.8164.1.30.1.1.14

> Description: | The number of IP addresses in FREE state in the pool.

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentTrapData(31)

> Object: | starCongestionPolicy

> Object ID: | enterprises.8164.1.31.1

> Description: | The policy invoked for congestion events.

> Syntax: | INTEGER

> Access: | Not-accessible

> Objects: | reject(1) redirect(2) drop(3)

> Object: | starCongestionResourceType

> Object ID: | enterprises.8164.1.31.2

> Description: | The resource type for a congestion event.

> Syntax: | INTEGER

> Access: | Not-accessible

> Objects: | systemcpu(1) servicecpu(2) averagememory(3) queuesize(4) queuedelay(5) license(6) portutil(7) rxportutill(8) txportutil(9) rxperportutil(10) txperportutil(11) servicecapacity(12)

> Object: | starPTACConfig

> Object ID: | enterprises.8164.1.31.3

> Description: | The number of PACs/PSCs/TACs configured in the system.

> Syntax: | Integer32(0..14)

> Access: | Not-accessible

> Object: | starPTACActive

> Object ID: | enterprises.8164.1.31.4

> Description: | The number of PACs/PSCs/TACs active in the system.

> Syntax: | Integer32(0..14)

> Access: | Not-accessible

> Object: | starContextName

> Object ID: | enterprises.8164.1.31.5

> Description: | The name of a context configured on the system.

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starInterfaceName

> Object ID: | enterprises.8164.1.31.6

> Description: | The name of an interface.

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starPCFAddress

> Object ID: | enterprises.8164.1.31.7

> Description: | The IP address of a PCF.

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starPeerAddress

> Object ID: | enterprises.8164.1.31.8

> Description: | Peer Address

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starLicensedSessions

> Object ID: | enterprises.8164.1.31.9

> Description: | The number of sessions enabled by the software license.

> Syntax: | Unsigned32

> Access: | Accessible-for-notify

> Object: | starCurrentSessions

> Object ID: | enterprises.8164.1.31.10

> Description: | The number of current sessions in use against a software license.

> Syntax: | Gauge32

> Access: | Accessible-for-notify

> Object: | starL3Address

> Object ID: | enterprises.8164.1.31.11

> Description: | L3 Address

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starUDPPortNum

> Object ID: | enterprises.8164.1.31.12

> Description: | UDP Port Number

> Syntax: | Integer32(1..65535)

> Access: | Not-accessible

> Object: | starSRPIPAddress

> Object ID: | enterprises.8164.1.31.13

> Description: | SRP IP Address

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starBGPPeerIPAddress

> Object ID: | enterprises.8164.1.31.14

> Description: | BGP Peer IP Address

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starContFiltCFFilename

> Object ID: | enterprises.8164.1.31.15

> Description: | File name for the Optimized Content Rating Database (OPTCMDB)

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starContFiltCFErrorCode

> Object ID: | enterprises.8164.1.31.16

> Description: | Error code.

> Syntax: | Integer32

> Access: | Not-accessible

> Object: | starFetchedFromAAAMgr

> Object ID: | enterprises.8164.1.31.17

> Description: | The total number of calls fetched from AAA Manager

> Syntax: | Integer32

> Access: | Read-only

> Object: | starPriorToAudit

> Object ID: | enterprises.8164.1.31.18

> Description: | The number calls prior to audit

> Syntax: | Integer32

> Access: | Read-only

> Object: | starPassedAudit

> Object ID: | enterprises.8164.1.31.19

> Description: | The number calls prior to audit

> Syntax: | Integer32

> Access: | Read-only

> Object: | starCallsRecovered

> Object ID: | enterprises.8164.1.31.20

> Description: | The number calls recovered

> Syntax: | Integer32

> Access: | Read-only

> Object: | starA11CallLines

> Object ID: | enterprises.8164.1.31.21

> Description: | The number of A11 call lines

> Syntax: | Integer32

> Access: | Read-only

> Object: | starElapsedMs

> Object ID: | enterprises.8164.1.31.22

> Description: | The audit time elapsed in milli-seconds

> Syntax: | Integer32

> Access: | Read-only

> Object: | starCDRFilename

> Object ID: | enterprises.8164.1.31.23

> Description: | The name of a CDR (EDR/UDR) file.

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starDiameterVpnName

> Object ID: | enterprises.8164.1.31.24

> Description: | Diameter VPN (Context) Name

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starDiameterPeerAddr

> Object ID: | enterprises.8164.1.31.25

> Description: | Diameter Peer Address

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> Object: | starDiameterEndpointName

> Object ID: | enterprises.8164.1.31.26

> Description: | Diameter Endpoint Name

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starInterfaceIPAddress

> Object ID: | enterprises.8164.1.31.27

> Description: | Interface IP Address

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> Object: | starOSPFNeighborRouterID

> Object ID: | enterprises.8164.1.31.28

> Description: | Interface IP Address

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> Object: | starOSPFFromState

> Object ID: | enterprises.8164.1.31.29

> Description: | FROM state for OSPF Neighbor

> Syntax: | StarOSPFNeighborState

> Access: | Accessible-for-notify

> Object: | starOSPFToState

> Object ID: | enterprises.8164.1.31.30

> Description: | TO state for OSPF Neighbor

> Syntax: | StarOSPFNeighborState

> Access: | Accessible-for-notify

> Object: | starDiameterEncoderString

> Object ID: | enterprises.8164.1.31.31

> Description: | Diameter Cause Code String

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starDiameterECode

> Object ID: | enterprises.8164.1.31.33

> Description: | Diameter Cause code

> Syntax: | Integer

> Access: | Accessible-for-notify

> Enumeration: | notcomplete(1) hostnamemismatch(2) hostrealmismatch(3) securitymismatch(4) tlscertificateerror(5) tlshandshakeerror(6) authappidmismatch(7)

> Object: | starDiameterPeerAddrIpv6

> Object ID: | enterprises.8164.1.31.34

> Description: | Diameter Peer Address

> Syntax: | Ipv6Address

> Access: | accessible-for-notify

> Object: | starContFiltCFUpgradeFilename

> Object ID: | enterprises.8164.1.31.35

> Description: | File name for the Full or Incremental OPTCMDB

> Syntax: | DisplayString

> Access: | not-accessible

> Object: | starContFiltCFUpgradeErrorCode

> Object ID: | enterprises.8164.1.31.36

> Description: | Error code

> Syntax: | unknownerror(1) upgradefullfailure(2) upgradeincrfailure(3)

> Access: | not-accessible

> Object: | starBLUpgradeFilename

> Object ID: | enterprises.8164.1.31.37

> Description: | File name for the Full OPTBLDB

> Syntax: | DisplayString

> Access: | not-accessible

> Object: | starBLUpgradeErrorCode

> Object ID: | enterprises.8164.1.31.38

> Description: | Error code

> Syntax: | unknownerror(1) upgradefullfailure(2)

> Access: | not-accessible

> Object: | starDynPkgFilename

> Object ID: | enterprises.8164.1.31.39

> Description: | File name for the DynPkg

> Syntax: | DisplayString

> Access: | not-accessible

> Object: | starDynCFErrorCode

> Object ID: | enterprises.8164.1.31.40

> Description: | Error code

> Syntax: | unknownerror(1) notavailable(2) loadfailure(3)

> Access: | not-accessible

> Object: | starDynPkgUpgradeFilename

> Object ID: | enterprises.8164.1.31.41

> Description: | File name for the Full DynPkg

> Syntax: | DisplayString

> Access: | not-accessible

> Object: | starDynCFUpgradeErrorCode

> Object ID: | enterprises.8164.1.31.42

> Description: | Error code

> Syntax: | unknownerror(1) upgradefullfailure(2)

> Access: | not-accessible

> Object: | starEGTPVpnName

> Object ID: | enterprises.8164.1.31.45

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | accessible-for-notify

> Object: | starEGTPServName

> Object ID: | enterprises.8164.1.31.46

> Description: | The name of this service

> Syntax: | DisplayString

> Access: | accessible-for-notify

> Object: | starEGTPInterfaceType

> Object ID: | enterprises.8164.1.31.47

> Description: | Egtp interface type

> Syntax: | INTEGER

> Access: | accessible-for-notify

> Object: | starEGTPSelfPort

> Object ID: | enterprises.8164.1.31.48

> Description: | The Port number of the EGTP

> Syntax: | Gauge32

> Access: | accessible-for-notify

> Object: | starEGTPSelfAddr

> Object ID: | enterprises.8164.1.31.49

> Description: | The IP Address of the EGTP

> Syntax: | IpAddress

> Access: | accessible-for-notify

> Object: | starEGTPPeerPort

> Object ID: | enterprises.8164.1.31.50

> Description: | The Port number of the PeerNode

> Syntax: | Gauge32

> Access: | accessible-for-notify

> Object: | starEGTPPeerAddr

> Object ID: | enterprises.8164.1.31.51

> Description: | The IP Address of the PeerNode

> Syntax: | IpAddress

> Access: | accessible-for-notify

> Object: | starEGTPPeerOldRstCnt

> Object ID: | enterprises.8164.1.31.52

> Description: | EGTP peer old restart counter

> Syntax: | Gauge32

> Access: | accessible-for-notify

> Object: | starEGTPPeerNewRstCnt

> Object ID: | enterprises.8164.1.31.53

> Description: | EGTP peer new restart counter

> Syntax: | Gauge32

> Access: | accessible-for-notify

> Object: | starEGTPPeerSessCnt

> Object ID: | enterprises.8164.1.31.54

> Description: | EGTP peer session count

> Syntax: | Gauge32

> Access: | accessible-for-notify

> Object: | starEGTPFailureReason

> Object ID: | enterprises.8164.1.31.55

> Description: | Egtp path failure reason

> Syntax: | INTEGER

> Access: | accessible-for-notify

> Object: | starGSSCDRLossConfigured

> Object ID: | enterprises.8164.1.31.56

> Description: | The configured value of threshold CDR Loss at GSS

> Syntax: | Unsigned32

> Access: | accessible-for-notify

> Object: | starGSSCDRLossMeasured

> Object ID: | enterprises.8164.1.31.57

> Description: | The Measured value of CDR Loss at GSS

> Syntax: | Unsigned32

> Access: | accessible-for-notify

> Object: | starLicenseKey

> Object ID: | enterprises.8164.1.31.58

> Description: | The license key

> Syntax: | Unsigned32

> Access: | accessible-for-notify

> Object: | starLicenseExpiryDate

> Object ID: | enterprises.8164.1.31.59

> Description: | The license expiration date/time

> Syntax: | DateAndTime

> Access: | accessible-for-notify

> Object: | starLicenseDaysRemaining

> Object ID: | enterprises.8164.1.31.60

> Description: | The number of days remaining before the license expires

> Syntax: | Unsigned32

> Access: | accessible-for-notify

> Object: | starLicenseDaysafterExpiry

> Object ID: | enterprises.8164.1.31.61

> Description: | The number of days after the license has expired

> Syntax: | Unsigned32

> Access: | accessible-for-notify

> Object: | starNPUSlot

> Object ID: | enterprises.8164.1.31.62

> Description: | The NPU slot number

> Syntax: | Integer32(1..48)

> Access: | accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentGGSNService(32)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starGGSNSerTable

> Object ID: | enterprises.8164.1.32.1

> Description: | A table containing GGSN related information

> Syntax: | SEQUENCE OF StarGGSNSerEntry

> Access: | Not-accessible

> Object: | starGGSNSerEntry

> Object ID: | enterprises.8164.1.32.1.1

> Description: | The statistics for a specific GGSN service

> Syntax: | StarGGSNSerEntry

> Access: | Not-accessible

> Sequence: | starGGSNSerVpnID starGGSNSerSvcID starSessGGSNVpnName starSessGGSNServName starSessGGSNPeerPort starSessGGSNPeerAddr starSessGGSNImsi starSessGGSNSubsName starSessGGSNAPNName

> Object: | starGGSNSerVpnID

> Object ID: | enterprises.8164.1.32.1.1.1

> Description: | The internal identification of the VPN (context)

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starGGSNSerSvcID

> Object ID: | enterprises.8164.1.32.1.1.2

> Description: | The internal identification of this service; unique within a specific context

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starSessGGSNVpnName

> Object ID: | enterprises.8164.1.32.1.1.3

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessGGSNServName

> Object ID: | enterprises.8164.1.32.1.1.4

> Description: | The name of this service

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessGGSNPeerPort

> Object ID: | enterprises.8164.1.32.1.1.5

> Description: | The Peer Port for which PATH Failure has occurred

> Syntax: | Gauge32

> Access: | Accessible-for-notify

> Object: | starSessGGSNPeerAddr

> Object ID: | enterprises.8164.1.32.1.1.6

> Description: | The Peer Address for which PATH Failure has occurred

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessGGSNImsi

> Object ID: | enterprises.8164.1.32.1.1.7

> Description: | The IMSI of the subscriber.

> Syntax: | OCTET STRING (SIZE (1..8))

> Access: | Accessible-for-notify

> Object: | starSessGGSNSubsName

> Object ID: | enterprises.8164.1.32.1.1.8

> Description: | The name of the subscriber.

> Syntax: | OCTET STRING (SIZE (1..128))

> Access: | Accessible-for-notify

> Object: | starSessGGSNAPNName

> Object ID: | enterprises.8164.1.32.1.1.9

> Description: | The name of the APN.

> Syntax: | OCTET STRING (SIZE (1..64))

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentL2TP(33)

> Object: | starL2TPTable

> Object ID: | enterprises.8164.1.33.1

> Description: | A table containing L2TP related information

> Syntax: | SEQUENCE OF starL2TPEntry

> Access: | Not-accessible

> Object: | starL2TPEntry

> Object ID: | enterprises.8164.1.33.1.1

> Description: | The statistics for a L2TP entry

> Syntax: | starL2TPEntry

> Access: | Not-accessible

> Sequence: | starL2TPLocalTunnelID starL2TPPeerTunnelID starL2TPContextName starL2TPServiceName starL2TPServiceTypeName starL2TPLocalAddress starL2TPPeerAddress

> Object: | starL2TPLocalTunnelID

> Object ID: | enterprises.8164.1.33.1.1.1

> Description: | The internal identification of the L2TP local tunnel ID

> Syntax: | Unsigned32

> Access: | Not-accessible

> Object: | starL2TPPeerTunnelID

> Object ID: | enterprises.8164.1.33.1.1.2

> Description: | The internal identification of the L2TP peer tunnel ID

> Syntax: | Unsigned32

> Access: | Not-accessible

> Object: | starL2TPContextName

> Object ID: | enterprises.8164.1.33.1.1.3

> Description: | The name of the context

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starL2TPServiceName

> Object ID: | enterprises.8164.1.33.1.1.4

> Description: | The name of the service

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starL2TPServiceTypeName

> Object ID: | enterprises.8164.1.33.1.1.5

> Description: | The name of the service type

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starL2TPLocalAddress

> Object ID: | enterprises.8164.1.33.1.1.6

> Description: | The local address of the service

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> Object: | starL2TPPeerAddress

> Object ID: | enterprises.8164.1.33.1.1.7

> Description: | The peer address of the service

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starSessSub1(34)
> This is used to perform a lookup on information on a single subscriber. This is done in a two-step process:

> 1 | Use a SET pdu to provide the keys to lookup. Set one or more of the fields starSessSub1Context, starSessSub1NAI, starSessSub1MSID, starSessSub1IpAddr.

> The SET pdu returns once the query is complete. This query can takes some time especially on large systems, so do not use small retry timers.

> 2 | Use a GET pdu to retrieve the data.

> IMPORTANT: Note that in some cases, multiple subscribers might watch the given search criteria.
> The starSessSub1LastResult field identifies if zero, one or multiple matches were found.
> If multiple matches are found, data is returned for one of them.

> Object: | starSessSub1Context

> Object ID: | enterprises.8164.1.34.1

> Description: | The name of the context for this subscriber. If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

> Syntax: | DisplayString

> Access: | Read-write

> Object: | starSessSub1NAI

> Object ID: | enterprises.8164.1.34.2

> Description: | The NAI for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

> Syntax: | OCTET STRING (SIZE (1..128))

> Access: | Read-write

> Object: | starSessSub1MSID

> Object ID: | enterprises.8164.1.34.3

> Description: | The MSID for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

> Syntax: | OCTET STRING (SIZE (1..16))

> Access: | Read-write

> Object: | starSessSub1IpAddr

> Object ID: | enterprises.8164.1.34.4

> Description: | The remote IP address for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

> Syntax: | IpAddress

> Access: | Read-write

> Object: | starSessSub1LastResult

> Object ID: | enterprises.8164.1.34.5

> Description: | The result of the last search. A value of unknown(0) means that the query wasn't created properly, or that no query has been performed; error(1) indicates an internal error performing the query, this is an abnormal condition that shouldn't normally be seen; nomatch(2) means that the query did not find a matching subscriber; onematch(3) means that the query found exactly one subscriber; multimatch(4) means that more than one subscriber matched; the information for one (random) subscriber was fetched

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) error(1) nomatch(2) onematch(3) multimatch(4)

> Object: | starSessSub1ServiceName

> Object ID: | enterprises.8164.1.34.6

> Description: | The service name of the subscriber.

> Syntax: | OCTET STRING (SIZE (1..63))

> Access: | Read-only

> Object: | starSessSub1HAIpAddr

> Object ID: | enterprises.8164.1.34.7

> Description: | The HA IP address for FA MIP connections

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1PeerIpAddr

> Object ID: | enterprises.8164.1.34.8

> Description: | The remote IP address of the peer. The type of peer depends on the session type.

> Syntax: | IpAddress

> Access: | Read-only

> Session Type | Peer
> PDSN | PCF
> GGSN | SGSN
> HA Mobile IP/HA IPSEC | FA
> LAC | LNS
> LNS | LAC

> Object: | starSessSub1InPackets

> Object ID: | enterprises.8164.1.34.9

> Description: | The number of incoming packets for the subscriber

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1InPacketsDropped

> Object ID: | enterprises.8164.1.34.10

> Description: | The number of incoming packets dropped for the subscriber

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1InBytes

> Object ID: | enterprises.8164.1.34.11

> Description: | The count of incoming bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes

> Syntax: | Counter32

> Units: | KB

> Access: | Read-only

> Object: | starSessSub1OutPackets

> Object ID: | enterprises.8164.1.34.12

> Description: | The number of out going packets for the subscriber

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1OutPacketsDropped

> Object ID: | enterprises.8164.1.34.13

> Description: | The number of out going packets dropped for the subscriber

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1OutBytes

> Object ID: | enterprises.8164.1.34.14

> Description: | The count of outgoing bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes

> Syntax: | Counter32

> Units: | KB

> Access: | Read-only

> Object: | starSessSub1Activity

> Object ID: | enterprises.8164.1.34.15

> Description: | TBD

> Syntax: | Gauge32

> Units: | %

> Access: | Read-only

> Object: | starSessSub1State

> Object ID: | enterprises.8164.1.34.16

> Description: | The state of the subscriber

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | Unknown(0) Connecting(1) Connected(2) Disconnecting(3)

> Object: | starSessSub1CallID

> Object ID: | enterprises.8164.1.34.17

> Description: | The internal call ID of the subscriber

> Syntax: | Integer32

> Access: | Read-only

> Object: | starSessSub1ConnectTime

> Object ID: | enterprises.8164.1.34.18

> Description: | The connect time for the subscriber, in UTC. The UNIX epoch (Jan. 1, 1970) is used if no value is available

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starSessSub1CallDuration

> Object ID: | enterprises.8164.1.34.19

> Description: | The duration of the call, in seconds

> Syntax: | Counter32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1TimeIdle

> Object ID: | enterprises.8164.1.34.20

> Description: | The idle time of the call, in seconds

> Syntax: | Gauge32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1AccessType

> Object ID: | enterprises.8164.1.34.21

> Description: | The access type for the subscriber.

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) pdsnsimpleip(1) pdsnmobileip(2) hamobileip(3) ggsnpdptypeipv4(4) ggsnpdptypeppp(5) ggsnpdptypeipv6(6) lnsl2tp(7) haipsec(8) ipsg(9) pdsnsipmip(10) mipproxyfa(11) imsa(12) bcmcs(13) ggsnmip(14) ipprobe(15) ansgw(16)

> Object: | starSessSub1AccessTech

> Object ID: | enterprises.8164.1.34.22

> Description: | The access technology for the subscriber.

> Syntax: | INTEGER

> Access: | Read-only

> Sequence: | unknown(0) cdma1xrtt(1) cdmaevdo(2) cdmaother(3) wcdmautran(4) gprsgeran(5) gprsother(6) wirelesslan(7) ipsg(8) wimax(9) sip(10) other(11) cdmaevdoreva(12) pdif(13) phs(14) ehrpd(15) eutran(16) gan(17) hspa(18)

> Object: | starSessSub1LinkStatus

> Object ID: | enterprises.8164.1.34.23

> Description: | The link status for the subscriber.

> Syntax: | INTEGER

> Enumeration: | Read-only

> Sequence: | unknown(0) active(1) dormant(2)

> Object: | starSessSub1NetworkType

> Object ID: | enterprises.8164.1.34.24

> Description: | The network type for the subscriber.

> Syntax: | INTEGER

> Access: | Read-only

> Sequence: | unknown(0) ip(1) mobileip(2) l2tp(3) proxymobileip(4) ipinip(5) gre(6) ipv6inipv4(7)

> Object: | starSessSub1CarrierID

> Object ID: | enterprises.8164.1.34.25

> Description: | Carrier ID

> Syntax: | OCTET STRING (SIZE (0..6))

> Access: | Read-only

> Object: | starSessSub1ESN

> Object ID: | enterprises.8164.1.34.26

> Description: | Electronic Serial Number

> Syntax: | OCTET STRING (SIZE (0..15))

> Access: | Read-only

> Object: | starSessSub1GMTTimezoneOffset

> Object ID: | enterprises.8164.1.34.27

> Description: | Timezone offset from GMT, in seconds. This is a signed value

> Syntax: | Integer32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1SessMgr

> Object ID: | enterprises.8164.1.34.28

> Description: | The instance number of the session manager for this subscriber.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starSessSub1RemoteIPAddr

> Object ID: | enterprises.8164.1.34.29

> Description: | Remote IP Address

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1Card

> Object ID: | enterprises.8164.1.34.30

> Description: | The card holding the session manager for this session. Use in combination with starSessSub1CPU.

> Syntax: | Integer32(1..16)

> Access: | Read-only

> Object: | starSessSub1CPU

> Object ID: | enterprises.8164.1.34.31

> Description: | The CPU holding the session manager for this session. Use in combination with starSessSub1Card

> Syntax: | Integer32(0..3)

> Access: | Read-only

> Object: | starSessSub1TimeIdleLeft

> Object ID: | enterprises.8164.1.34.32

> Description: | The remaining idle time of the call, in seconds. A value of 0xffffffff is used if the call does not have an idle timeout

> Syntax: | Gauge32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1TimeLeft

> Object ID: | enterprises.8164.1.34.33

> Description: | The remaining session time of the call, in seconds. A value of 0xffffffff is used if the call does not have a session timeout

> Syntax: | Gauge32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1TimeLongDurLeft

> Object ID: | enterprises.8164.1.34.34

> Description: | The remaining long duration time of the call, in seconds. A value of 0xffffffff is used if the call does not have a long duration timer

> Syntax: | Gauge32

> Units: | Seconds

> Access: | Read-only

> Object: | starSessSub1LongDurAction

> Object ID: | enterprises.8164.1.34.35

> Description: | The action to take when the long duration timer is reached

> Syntax: | StarLongDurTimeoutAction

> Access: | Read-only

> Object: | starSessSub1AlwaysOn

> Object ID: | enterprises.8164.1.34.36

> Description: |

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starSessSub1IPPoolName

> Object ID: | enterprises.8164.1.34.37

> Description: |

> Syntax: | OCTET STRING (SIZE(0..31))

> Access: | Read-only

> Object: | starSessSub1VLANID

> Object ID: | enterprises.8164.1.34.38

> Description: | 0 is returned if this is not applicable

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starSessSub1LNSIPAddr

> Object ID: | enterprises.8164.1.34.39

> Description: | Only valid if starSessSub1NetworkType is l2tp(3), otherwise 0.0.0.0

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1ProxyMIP

> Object ID: | enterprises.8164.1.34.40

> Description: |

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starSessSub1GGSNMIP

> Object ID: | enterprises.8164.1.34.41

> Description: |

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starSessSub1HomeAgentIpAddr

> Object ID: | enterprises.8164.1.34.42

> Description: | The IP address of the Home Agent. This value is applicable only if one of the following is true: 1. The value of starSessSub1AccessType is pdsnmobileip(2) 2. The value of starSessSub1ProxyMIP is enabled(1) 3. The value of starSessSub1GGSNMIP is enabled(1) If not applicable, a value of 0.0.0.0 will be returned

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1LocalIPAddr

> Object ID: | enterprises.8164.1.34.43

> Description: | The Local IP address of the Home Agent. This value is applicable only if one of the following is true: 1. The value of starSessSub1AccessType is pdsnsimpleip(1) 2. The value of starSessSub1AccessType is ggsnpdptypeppp(5) 3. The value of starSessSub1AccessType is lnsl2tp(7) If not applicable, a value of 0.0.0.0 will be returned

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1FAServiceName

> Object ID: | enterprises.8164.1.34.44

> Description: | The FA service name for the subscriber. This value is applicable only if one of the following is true: 1. The value of starSessSub1AccessType is pdsnmobileip(2) 2. The value of starSessSub1ProxyMIP is enabled(1) 3. The value of starSessSub1GGSNMIP is enabled(1)

> Syntax: | OCTET STRING (SIZE (1..63))

> Access: | Read-only

> Object: | starSessSub1FAVPNName

> Object ID: | enterprises.8164.1.34.45

> Description: | The FA VPN (Context) name. This value is applicable only if one of the following is true: 1. The value of starSessSub1AccessType is pdsnmobileip(2) 2. The value of starSessSub1ProxyMIP is enabled(1) 3. The value of starSessSub1GGSNMIP is enabled(1)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1SourceVPN

> Object ID: | enterprises.8164.1.34.46

> Description: | The Source VPN (Context) name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1DestVPN

> Object ID: | enterprises.8164.1.34.47

> Description: | The Destination VPN (Context) name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1AAAVPN

> Object ID: | enterprises.8164.1.34.48

> Description: |

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1AAADomain

> Object ID: | enterprises.8164.1.34.49

> Description: |

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1AAAStart

> Object ID: | enterprises.8164.1.34.50

> Description: |

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1AAAStop

> Object ID: | enterprises.8164.1.34.51

> Description: |

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1AAAInterim

> Object ID: | enterprises.8164.1.34.52

> Description: |

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1AcctSessionID

> Object ID: | enterprises.8164.1.34.53

> Description: |

> Syntax: | OCTET STRING (SIZE(0..23))

> Access: | Read-only

> Object: | starSessSub1AAARadiusGroup

> Object ID: | enterprises.8164.1.34.54

> Description: |

> Syntax: | OCTET STRING (SIZE(0..63))

> Access: | Read-only

> Object: | starSessSub1AAARadiusAuthServerIPAddr

> Object ID: | enterprises.8164.1.34.55

> Description: |

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1AAARadiusAcctServerIPAddr

> Object ID: | enterprises.8164.1.34.56

> Description: |

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1NASIPAddr

> Object ID: | enterprises.8164.1.34.57

> Description: |

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1NexthopIPAddr

> Object ID: | enterprises.8164.1.34.58

> Description: |

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1ActiveInACL

> Object ID: | enterprises.8164.1.34.59

> Description: |

> Syntax: | OCTET STRING (SIZE(0..79))

> Access: | Read-only

> Object: | starSessSub1ActiveOutACL

> Object ID: | enterprises.8164.1.34.60

> Description: |

> Syntax: | OCTET STRING (SIZE(0..79))

> Access: | Read-only

> Object: | starSessSub1ECSRulebase

> Object ID: | enterprises.8164.1.34.61

> Description: |

> Syntax: | OCTET STRING (SIZE(0..63))

> Access: | Read-only

> Object: | starSessSub1InPlcyGrp

> Object ID: | enterprises.8164.1.34.62

> Description: |

> Syntax: | OCTET STRING (SIZE(0..15))

> Access: | Read-only

> Object: | starSessSub1OutPlcyGrp

> Object ID: | enterprises.8164.1.34.63

> Description: |

> Syntax: | OCTET STRING (SIZE(0..15))

> Access: | Read-only

> Object: | starSessSub1DownTrafPolState

> Object ID: | enterprises.8164.1.34.64

> Description: |

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starSessSub1DownCommDataRate

> Object ID: | enterprises.8164.1.34.65

> Description: | Downlink committed data rate, in bps. This value is only valid if starSessSub1DownTrafPolState is enabled(1)

> Syntax: | Unsigned32

> Units: | bps

> Access: | Read-only

> Object: | starSessSub1DownPeakDataRate

> Object ID: | enterprises.8164.1.34.66

> Description: | Downlink peak data rate, in bps. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

> Syntax: | Unsigned32

> Units: | bps

> Access: | Read-only

> Object: | starSessSub1DownBurstSize

> Object ID: | enterprises.8164.1.34.67

> Description: | Downlink burst size, in bytes. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

> Syntax: | Unsigned32

> Units: | bytes

> Access: | Read-only

> Object: | starSessSub1DownExceedAction

> Object ID: | enterprises.8164.1.34.68

> Description: | Downlink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

> Syntax: | StarQOSTPAction

> Access: | Read-only

> Object: | starSessSub1DownViolateAction

> Object ID: | enterprises.8164.1.34.69

> Description: | Downlink Violate Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

> Syntax: | StarQOSTPAction

> Access: | Read-only

> Object: | starSessSub1DownExceed

> Object ID: | enterprises.8164.1.34.70

> Description: | Downlink packets exceeded bandwidth parameters

> Syntax: | Counter32

> Units: | packets

> Access: | Read-only

> Object: | starSessSub1DownViolate

> Object ID: | enterprises.8164.1.34.71

> Description: | Downlink packets violated bandwidth parameters

> Syntax: | Counter32

> Units: | packets

> Access: | Read-only

> Object: | starSessSub1UpTrafPolState

> Object ID: | enterprises.8164.1.34.72

> Description: | Uplink traffic policing state

> Syntax: | INTEGER

> Access: | Read-only

> Enumeration: | unknown(0) enabled(1) disabled(2)

> Object: | starSessSub1UpCommDataRate

> Object ID: | enterprises.8164.1.34.73

> Description: | Uplink committed data rate, in bps. This value is only valid if starSessSub1UpTrafPolState is enabled(1)

> Syntax: | Unsigned32

> Units: | bps

> Access: | Read-only

> Object: | starSessSub1UpPeakDataRate

> Object ID: | enterprises.8164.1.34.74

> Description: | Uplink peak data rate, in bps. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

> Syntax: | Unsigned32

> Units: | bps

> Access: | Read-only

> Object: | starSessSub1UpBurstSize

> Object ID: | enterprises.8164.1.34.75

> Description: | Uplink burst size, in bytes. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1

> Syntax: | Unsigned32

> Units: | bytes

> Access: | Read-only

> Object: | starSessSub1UpExceedAction

> Object ID: | enterprises.8164.1.34.76

> Description: | Uplink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

> Syntax: | StarQOSTPAction

> Access: | Read-only

> Object: | starSessSub1UpViolateAction

> Object ID: | enterprises.8164.1.34.77

> Description: | Uplink Violate Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

> Syntax: | StarQOSTPAction

> Access: | Read-only

> Object: | starSessSub1UpExceed

> Object ID: | enterprises.8164.1.34.78

> Description: | Uplink packets exceeded bandwidth parameters

> Syntax: | Counter32

> Units: | packets

> Access: | Read-only

> Object: | starSessSub1UpViolate

> Object ID: | enterprises.8164.1.34.79

> Description: | Uplink packets violated bandwidth parameters

> Syntax: | Counter32

> Units: | packets

> Access: | Read-only

> Object: | starSessSub1L3TunnelingState

> Object ID: | enterprises.8164.1.34.80

> Description: | Identifies if L3 tunneling is enabled. This value should be enabled(1) if starSessSub1NetworkType is ipinip(5) or gre(6).

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1L3TunLocalIPAddr

> Object ID: | enterprises.8164.1.34.81

> Description: | L3 tunnel local address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0.

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1L3TunRemoteIPAddr

> Object ID: | enterprises.8164.1.34.82

> Description: | L3 tunnel remote address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1AddrViaDHCP

> Object ID: | enterprises.8164.1.34.83

> Description: |

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1DHCPServName

> Object ID: | enterprises.8164.1.34.84

> Description: | DHCP service name. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1)

> Syntax: | Octet string

> Access: | Read-only

> Object: | starSessSub1DHCPServIPAddr

> Object ID: | enterprises.8164.1.34.85

> Description: | DHCP service IP address. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1), otherwise it will be 0.0.0.0

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1AccessLinkIPFrag

> Object ID: | enterprises.8164.1.34.86

> Description: |

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1IgnoreDFBit

> Object ID: | enterprises.8164.1.34.87

> Description: | Ignore DF-bit data-tunnel

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1MIPGratARPMode

> Object ID: | enterprises.8164.1.34.88

> Description: | This field is only applicable if starSessSub1AccessType is hamobileip(3) or haipsec(8)

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrProc

> Object ID: | enterprises.8164.1.34.89

> Description: | The state of external inline server processing

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrIngrIPAddr

> Object ID: | enterprises.8164.1.34.90

> Description: | The external inline server ingress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | IP Address

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrIngrVLANTag

> Object ID: | enterprises.8164.1.34.91

> Description: | The external inline server ingress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrEgrIPAddr

> Object ID: | enterprises.8164.1.34.92

> Description: | The external inline server egress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrEgrVLANTag

> Object ID: | enterprises.8164.1.34.93

> Description: | The external inline server egress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrVPNName

> Object ID: | enterprises.8164.1.34.94

> Description: | The external inline server context (VPN). This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSessSub1RadAcctMode

> Object ID: | enterprises.8164.1.34.95

> Description: | Radius Accounting Mode

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1InBytesDropped

> Object ID: | enterprises.8164.1.34.96

> Description: | The count of incoming bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1OutBytesDropped

> Object ID: | enterprises.8164.1.34.97

> Description: | The count of outgoing bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1PeakBPSTx

> Object ID: | enterprises.8164.1.34.98

> Description: | Peak rate from user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1PeakBPSRx

> Object ID: | enterprises.8164.1.34.99

> Description: | Peak rate to user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1AveBPSTx

> Object ID: | enterprises.8164.1.34.100

> Description: | Average rate from user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1AveBPSRx

> Object ID: | enterprises.8164.1.34.101

> Description: | Average rate to user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1SustBPSTx

> Object ID: | enterprises.8164.1.34.102

> Description: | Sustained rate from user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1SustBPSRx

> Object ID: | enterprises.8164.1.34.103

> Description: | Sustained rate to user, in bytes per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1PeakPPSTx

> Object ID: | enterprises.8164.1.34.104

> Description: | Peak rate from user, in packets per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1PeakPPSRx

> Object ID: | enterprises.8164.1.34.105

> Description: | Peak rate to user, in packets per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1AvePPSTx

> Object ID: | enterprises.8164.1.34.106

> Description: | Average rate from user, in packets per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1AvePPSRx

> Object ID: | enterprises.8164.1.34.107

> Description: | Average rate to user, in packets per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1SustPPSTx

> Object ID: | enterprises.8164.1.34.108

> Description: | Sustained rate from user, in packets per second.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1SustPPSRx

> Object ID: | enterprises.8164.1.34.109

> Description: | Sustained rate to user, in packets per second

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1ActivePct

> Object ID: | enterprises.8164.1.34.110

> Description: | Link online/active percentage.

> Syntax: | Integer32(0..100)

> Access: | Read-only

> Object: | starSessSub1IPv4BadHdr

> Object ID: | enterprises.8164.1.34.111

> Description: | IPv4 Bad Headers

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4TtlExceeded

> Object ID: | enterprises.8164.1.34.112

> Description: | IPv4 Total Exceeded

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4FragSent

> Object ID: | enterprises.8164.1.34.113

> Description: | IPv4 Fragments sent

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4FragFail

> Object ID: | enterprises.8164.1.34.114

> Description: | IPv4 Could Not Fragment errors

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4InACLDrop

> Object ID: | enterprises.8164.1.34.115

> Description: | IPv4 Input ACL Drops

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4OutACLDrop

> Object ID: | enterprises.8164.1.34.116

> Description: | IPv5 Output ACL Drops

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4InCSSDownDrop

> Object ID: | enterprises.8164.1.34.117

> Description: | IPv4 Input CSS Down Drops

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4OutCSSDownDrop

> Object ID: | enterprises.8164.1.34.118

> Description: | IPv4 Output CSS Down Drops

> Syntax: | Counter-32

> Access: | Read-only

> Object: | starSessSub1IPv4OutXOFFDropPkt

> Object ID: | enterprises.8164.1.34.119

> Description: | IPv4 Output XOFF Packets Drop

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4OutXOFFDropByte

> Object ID: | enterprises.8164.1.34.120

> Description: | IPv4 Output XOFF Bytes Drop

> Syntax: | Counter-32

> Access: | Read-only

> Object: | starSessSub1IPv4SrcViol

> Object ID: | enterprises.8164.1.34.121

> Description: | IPv4 Source Violations

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4ProxyDNSRedir

> Object ID: | enterprises.8164.1.34.122

> Description: | IPv4 Proxy-DNS Redirect

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4SrcProxyDNSPThru

> Object ID: | enterprises.8164.1.34.123

> Description: | IPv4 Proxy-DNS Pass-Thru

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4ProxyDNSDrop

> Object ID: | enterprises.8164.1.34.124

> Description: | IPv4 Proxy-DNS Drop

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4SrcViolNoAcct

> Object ID: | enterprises.8164.1.34.125

> Description: | IPv4 Source Violations No Account

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4SrcViolIgnored

> Object ID: | enterprises.8164.1.34.126

> Description: | IPv4 Source Violations Ignored

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrTxPkt

> Object ID: | enterprises.8164.1.34.127

> Description: | Packets transmitted to inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1ExtInlSrvrRxPkt

> Object ID: | enterprises.8164.1.34.128

> Description: | Packets received from inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPv4ICMPDropPkt

> Object ID: | enterprises.8164.1.34.129

> Description: | IPv4 ICMP Packets dropped

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1TunnelType

> Object ID: | enterprises.8164.1.34.130

> Description: | Tunnel Type

> Syntax: | Integer

> Access: | Read-only

> Object: | starSessSub1IPSECTunDownDropPkt

> Object ID: | enterprises.8164.1.34.131

> Description: | Pool IPSEC tunnel down packets dropped. This value is only valid if the value of starSessSub1TunnelType is esp(6)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1IPSECFlowID

> Object ID: | enterprises.8164.1.34.132

> Description: | IP Pool IPSEC flow id. This value is only valid if the value of starSessSub1TunnelType is esp(6)

> Syntax: | Integer32

> Access: | Read-only

> Object: | starSessSub1DormancyTotal

> Object ID: | enterprises.8164.1.34.133

> Description: | Dormancy total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1HandoffTotal

> Object ID: | enterprises.8164.1.34.134

> Description: | Handoff total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)

> Syntax: | Counter32

> Access: | Read-only

> Object: | starSessSub1AccessFlows

> Object ID: | enterprises.8164.1.34.135

> Description: | Access flows

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1TFT

> Object ID: | enterprises.8164.1.34.136

> Description: | Number of TFTs

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSub1NASPort

> Object ID: | enterprises.8164.1.34.137

> Description: | NAS port

> Syntax: | Integer32

> Access: | Read-only

> Object: | starSessSub1CorrID

> Object ID: | enterprises.8164.1.34.139

> Description: | ThreeGPP2-correlation-id (C2)

> Syntax: | Octet String

> Access: | Read-only

> Object: | starSessSub1L2TPPeerIPAddr

> Object ID: | enterprises.8164.1.34.140

> Description: | L2TP Peer address. This value is only valid if the value of starSessSub1NetworkType is l2tp(3)

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSessSub1IPv4EarlyPDURecv

> Object ID: | enterprises.8164.1.34.141

> Description: | IPv4 early PDU received

> Syntax: | Counter32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentNwReachServer(35)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starNwReachTable

> Object ID: | enterprises.8164.1.35.1

> Description: | A table containing Network Reachable Server information

> Syntax: | SEQUENCE OF StarNwReachEntry

> Access: | Not-accessible

> Object: | starNwReachEntry

> Object ID: | enterprises.8164.1.35.1.1

> Description: | Information for a specific Ntw Reachable Server

> Syntax: | StarNwReachEntry

> Access: | Not-accessible

> Sequence: | starNwReachName starNwReachSrvrAddr

> Object: | starNwReachName

> Object ID: | enterprises.8164.1.35.1.1.1

> Description: | The Name for this Network Reachable Server

> Syntax: | OCTET STRING (SIZE (1..16))

> Access: | Not-accessible

> Object: | starNwReachSrvrAddr

> Object ID: | enterprises.8164.1.35.1.1.2

> Description: | The IP Address for the Network Reachable Server

> Syntax: | IpAddress

> Access: | Not-accessible

> starentMIB(8164).starentMIBObjects(1).starentIPSEC(36)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starIPSECContextName

> Object ID: | enterprises.8164.1.36.1

> Description: | The name of a context

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starIPSECGroupName

> Object ID: | enterprises.8164.1.36.2

> Description: | The name of a crypto map

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starIPSECTunLocalIPAddr

> Object ID: | enterprises.8164.1.36.3

> Description: | The local IP Address for an IPSEC tunnel

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starIPSECTunRemoteIPAddr

> Object ID: | enterprises.8164.1.36.4

> Description: | The local IP Address for an IPSEC tunnel

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starIPSECPolicyName

> Object ID: | enterprises.8164.1.36.5

> Description: | An IPSEC policy name

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starIPSECDynPolicyType

> Object ID: | enterprises.8164.1.36.6

> Description: | An IPSEC dynamic policy type. Note that the value test(5) is used only for internal testing

> Syntax: | Integer

> Access: | Accessible-for-notify

> Enumeration: | unknown(0) manual(1) isakmp(2) subscribertemplate(3) subscribertunnel(4) test(5) dynamic(6)

> Object: | starIPSECDynPolicyPayloadType

> Object ID: | enterprises.8164.1.36.7

> Description: | An IPSEC dynamic policy payload type

> Syntax: | Integer

> Access: | Accessible-for-notify

> Object: | starIPSECLocalGateway

> Object ID: | enterprises.8164.1.36.8

> Description: | IP address of IPSec local gateway

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> Object: | starIPSECRemoteGateway

> Object ID: | enterprises.8164.1.36.9

> Description: | IP address of IPSec remote gateway

> Syntax: | IpAddress

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentSIPRoute(37)

> Object: | starSIPRouteTable

> Object ID: | enterprises.8164.1.37.1

> Description: | A table containing SIPRoute related information

> Syntax: | SEQUENCE OF StarSIPRouteEntry

> Access: | Not-accessible

> Object: | starSIPRouteEntry

> Object ID: | enterprises.8164.1.37.1.1

> Description: | The statistics for a specific SIPRoute service

> Syntax: | StarSIPRouteEntry

> Access: | Not-accessible

> Sequence: | starSIPRouteVpnID Index starSIPRouteVpnName Index starSIPRouteVmgName starSIPRouteAsName starSIPRouteDestPartyNum starSIPRouteReqNum

> Object: | starSIPRouteVpnID

> Object ID: | enterprises.8164.1.37.1.1.1

> Description: | The internal identification of the VPN (context)

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starSIPRouteVpnName

> Object ID: | enterprises.8164.1.37.1.1.2

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteVmgName

> Object ID: | enterprises.8164.1.37.1.1.3

> Description: | The name of this VMG (context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteAsName

> Object ID: | enterprises.8164.1.37.1.1.4

> Description: | The name of this AS (context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteDestPartyNum

> Object ID: | enterprises.8164.1.37.1.1.5

> Description: | The dest. party number

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteReqNum

> Object ID: | enterprises.8164.1.37.1.1.6

> Description: | The request number

> Syntax: | DisplayString

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentRPServiceOption(38)

> Object: | starRPServiceOptionTable

> Object ID: | enterprises.8164.1.38.1

> Description: |

> Syntax: | SEQUENCE OF StarRPServiceOptionEntry

> Access: | Not-accessible

> Object: | starRPServiceOptionEntry

> Object ID: | enterprises.8164.1.38.1.1

> Description: |

> Syntax: | StarRPServiceOptionEntry

> Access: | Not-accessible

> Sequence: | starRPServiceOptionNum starRPServiceOptionCalls

> Object: | starRPServiceOptionNum

> Object ID: | enterprises.8164.1.38.1.1.1

> Description: |

> Syntax: | Integer32(1..255)

> Access: | Not-accessible

> Object: | starRPServiceOptionCalls

> Object ID: | enterprises.8164.1.38.1.1.2

> Description: |

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentPCFStats(39)

> Object: | starPCFStatTable

> Object ID: | enterprises.8164.1.39.1

> Description: | A table containing per-PCF statistics.

> Syntax: | SEQUENCE OF StarPCFStatEntry

> Access: | Not-accessible

> Object: | starPCFStatEntry

> Object ID: | enterprises.8164.1.39.1.1

> Description: | The statistics for a specific PCF.

> Syntax: | StarPCFStatsEntry

> Access: | Not-accessible

> Sequence: | starPCFStatVpnID Index starPCFStatIpAddr starPCFStatVpnName starPCFStatRxPkts starPCFStatTxPkts starPCFStatRxBytes starPCFStatTxBytes starPCFStatTotalSessions starPCFStatCurrentSessions starPCFStatCurrentActiveSessions starPCFStatCurrentDormantSessions starPCFStatCurrentSIPConnected starPCFStatCurrentMIPConnected starPCFStatCurrentPMIPConnected starPCFStatCurrentL2TPLACConnected starPCFStatCurrentOtherConnected

> Object: | starPCFStatVpnID

> Object ID: | enterprises.8164.1.39.1.1.1

> Description: | The internal identification of the VPN (context).

> Syntax: | Guage32

> Access: | Not-accessible

> Object: | starPCFStatIpAddr

> Object ID: | enterprises.8164.1.39.1.1.2

> Description: | The IP address of the specific PCF.

> Syntax: | IpAddress

> Object ID: | Not-accessible

> Object: | starPCFStatVpnName

> Object ID: | enterprises.8164.1.39.1.1.3

> Description: | The name of the VPN (context).

> Syntax: | DisplayString

> Object ID: | Read-only

> Object: | starPCFStatRxPkts

> Object ID: | enterprises.8164.1.39.1.1.4

> Description: | Total packets received.

> Syntax: | Counter32

> Units: | Millions

> Access: | Read-only

> Object: | starPCFStatTxPkts

> Object ID: | enterprises.8164.1.39.1.1.5

> Description: | total packets transferred.

> Syntax: | Counter32

> Units: | Millions

> Object ID: | Read-only

> Object: | starPCFStatRxBytes

> Object ID: | enterprises.8164.1.39.1.1.6

> Description: | Total bytes received.

> Syntax: | Counter32

> Units: | Megabytes

> Object ID: | Read-only

> Object: | starPCFStatTxBytes

> Object ID: | enterprises.8164.1.39.1.1.7

> Description: | Total bytes send.

> Syntax: | Counter32

> Units: | Megabytes

> Object ID: | Read-only

> Object: | starPCFStatTotalSessions

> Object ID: | enterprises.8164.1.39.1.1.8

> Description: | Total number of sessions.

> Syntax: | Counter32

> Object ID: | Read-only

> Object: | starPCFStatCurrentSessions

> Object ID: | enterprises.8164.1.39.1.1.9

> Description: | Total current sessions.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPCFStatCurrentActiveSessions

> Object ID: | enterprises.8164.1.39.1.1.10

> Description: | Total number of current active sessions.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentDormantSessions

> Object ID: | enterprises.8164.1.39.1.1.11

> Description: | Total Numbers of current dormant sessions.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentSIPConnected

> Object ID: | enterprises.8164.1.39.1.1.12

> Description: | Total number of Simple IP sessions connected.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentMIPConnected

> Object ID: | enterprises.8164.1.39.1.1.13

> Description: | Total number of Mobile IP sessions connected.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentPMIPConnected

> Object ID: | enterprises.8164.1.39.1.1.14

> Description: | Total number of Proxy Mobile IP sessions connected.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentL2TPLACConnected

> Object ID: | enterprises.8164.1.39.1.1.15

> Description: | Total number of current L2TP LAC connected.

> Syntax: | Gauge32

> Object ID: | Read-only

> Object: | starPCFStatCurrentOtherConnected

> Object ID: | enterprises.8164.1.39.1.1.16

> Description: | Total number of other connections.

> Syntax: | Gauge32

> Object ID: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSIPRouteServer(40)

> Object: | starSIPRouteServerTable

> Object ID: | enterprises.8164.1.40.1

> Description: | A table containing SIPRouteServer related information

> Syntax: | SEQUENCE OF StarSIPRouteServerEntry

> Access: | Not-accessible

> Object: | starSIPRouteServerEntry

> Object ID: | enterprises.8164.1.40.1.1

> Description: | The statistics for a specific SIPRouteServer.

> Syntax: | StarSIPRouteServerEntry

> Access: | Not-accessible

> Sequence: | starSIPRouteServerVpnID Index starSIPRouteServerVpnName starSIPRouteServerVmgName starSIPRouteServerAsName starSIPRouteServerIpAddr

> Object: | starSIPRouteServerVpnID

> Object ID: | enterprises.8164.1.40.1.1.1

> Description: | The internal identification of the VPN (context).

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starSIPRouteServerVpnName

> Object ID: | enterprises.8164.1.40.1.1.2

> Description: | The name of the VPN (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteServerVmgName

> Object ID: | enterprises.8164.1.40.1.1.3

> Description: | The name of the VMG (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteServerAsName

> Object ID: | enterprises.8164.1.40.1.1.4

> Description: | The name of the AS (context).

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSIPRouteServerIpAddr

> Object ID: | enterprises.8164.1.40.1.1.5

> Description: | The SIP Route Server IP address.

> Syntax: | IP Address in dotted decimal notation

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentVIMService(41)

> Object: | starVIMServiceTable

> Object ID: | enterprises.8164.1.41.1

> Description: | A table containing VIM's Service related information

> Syntax: | SEQUENCE OF StarVIMServiceEntry

> Access: | Not-accessible

> Object: | starVIMServiceEntry

> Object ID: | enterprises.8164.1.41.1.1

> Description: | The statistics for a specific VIM's Service

> Syntax: | StarVIMServiceEntry

> Access: | Not-accessible

> Sequence: | starVIMServiceVpnID starVIMServiceVpnName starVIMServiceInstanceId starVIMServiceFMDMaxCallRate starVIMServiceFMDContinuousLoadCount

> Object: | starVIMServiceVpnID

> Object ID: | enterprises.8164.1.41.1.1.1

> Description: | The internal identification of the VPN (context)

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starVIMServiceVpnName

> Object ID: | enterprises.8164.1.41.1.1.2

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starVIMServiceInstanceId

> Object ID: | enterprises.8164.1.41.1.1.3

> Description: | The VIM Instance ID

> Syntax: | Unsigned32

> Access: | Not-accessible

> Object: | starVIMServiceFMDMaxCallRate

> Object ID: | enterprises.8164.1.41.1.1.4

> Description: | Configured FMD max call rate

> Syntax: | Unsigned32

> Units: | Calls per Minute

> Access: | Read-only

> Object: | starVIMServiceFMDContinuousLoadCount

> Object ID: | enterprises.8164.1.41.1.1.5

> Description: | Configured FMD continuous load count

> Syntax: | Unsigned32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentGSS(42)
> IMPORTANT: The GTPP Storage Server is an external entity, but the ST16/ST40 reports notifications on its behalf. The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starGSSClusterName

> Object ID: | enterprises.8164.1.42.1

> Description: | The name of the Storage Server Cluster

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterNodeName

> Object ID: | enterprises.8164.1.42.2

> Description: | The name of a node within a Storage Server Cluster

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterRgName

> Object ID: | enterprises.8164.1.42.3

> Description: | The name of the Storage Server Cluster Resource Group

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterRsName

> Object ID: | enterprises.8164.1.42.4

> Description: | The name of the Storage Server Cluster Resource

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterNodeState

> Object ID: | enterprises.8164.1.42.5

> Description: | Status of the Storage Server Cluster node

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterPrevOnlineNode

> Object ID: | enterprises.8164.1.42.6

> Description: | Name of the previous node of the Storage Server Cluster which was online/active

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterFromNode

> Object ID: | enterprises.8164.1.42.7

> Description: | Information from Storage Server Cluster to node

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSClusterToNode

> Object ID: | enterprises.8164.1.42.8

> Description: | Information from node to Storage Server Cluster

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSDiskPath

> Object ID: | enterprises.8164.1.42.9

> Description: | Path information of Storage Server disk

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSTransportPath

> Object ID: | enterprises.8164.1.42.10

> Description: | Path information of Storage Server for data transportation

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSIPMPGroup

> Object ID: | enterprises.8164.1.42.11

> Description: | Name of the IPMP group for GSS

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> Object: | starGSSInterfaceName

> Object ID: | enterprises.8164.1.42.12

> Description: | Name of the GSS interface

> Syntax: | DisplayString

> Access: | Accessible-for-notify

> starentMIB(8164).starentMIBObjects(1).starentPDIFSys(43)

> Object: | starPDIFSysStatus

> Object ID: | enterprises.8164.1.43.1

> Description: | The overall status of the chassis as a PDIF service. A value of noservice(1) means that the chassis is not configured/licensed for PDIF; active(2) indicates that at least one PDIF service is available for processing sessions; temporary(3) indicates that PDIF is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDIF service is currently active, but one or more PDIF services are configured

> Syntax: | INTEGER unknown(0) noservice(1) active(2) temporary(3) outofservice(4)

> Access: | Read-only

> Object: | starPDIFSysNumService

> Object ID: | enterprises.8164.1.43.2

> Description: | The number of PDIF services configured

> Syntax: | Unsigned32

> Units: | Services

> Access: | Read-only

> Object: | starPDIFSysSessCurrent

> Object ID: | enterprises.8164.1.43.3

> Description: | The number of current PDIF sessions for this chassis

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSysSessCurrActive

> Object ID: | enterprises.8164.1.43.4

> Description: | The number of currently active PDIF sessions for this chassis

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSysSessCurrDormant

> Object ID: | enterprises.8164.1.43.5

> Description: | The number of currently dormant PDIF sessions for this chassis

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSysSessTtlSetup

> Object ID: | enterprises.8164.1.43.6

> Description: | The cumulative total number of PDIF sessions that has been setup

> Syntax: | Counter32

> Access: | Read-only

> Object: | starPDIFSysChildSACurrent

> Object ID: | enterprises.8164.1.43.7

> Description: | Number of current PDIF child SAs for the chassis

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentPDIFService(44)

> Object: | starPDIFTable

> Object ID: | enterprises.8164.1.44.1

> Description: | A table of per-service PDIF information

> Syntax: | SEQUENCE OF StarPDIFEntry

> Access: | Not-accessible

> Object: | starPDIFEntry

> Object ID: | enterprises.8164.1.44.1.1

> Description: | The information for a PDIF service

> Syntax: | StarPDIFEntry

> Access: | Not-accessible

> Sequence: | starPDIFSvcID StarShortID starPDIFVpnID Gauge32 starPDIFVpnName DisplayString starPDIFServName DisplayString starPDIFStatus INTEGER starPDIFSessCurrent Gauge32 starPDIFSessRemain Gauge32 starPDIFSessCurrentActive Gauge32 starPDIFSessCurrentDormant Gauge32 starPDIFSessCurrentIpv6Active Gauge32 starPDIFSessCurrentIpv6Dormant Gauge32 starPDIFSessCurrentIpv4Active Gauge32 starPDIFSessCurrentIpv4Dormant Gauge32 starPDIFBindIpAddress IpAddress starPDIFBindIpPort Integer32 starPDIFBindSlot Integer32 starPDIFBindPort Integer32

> Object: | starPDIFSvcID

> Object ID: | enterprises.8164.1.44.1.1.1

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

> Syntax: | StarShortID

> Access: | Not-accessible

> Object: | starPDIFVpnID

> Object ID: | enterprises.8164.1.44.1.1.2

> Description: | The internal VPN (context) ID.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFVpnName

> Object ID: | enterprises.8164.1.44.1.1.3

> Description: | The VPN (context) name.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starPDIFServName

> Object ID: | enterprises.8164.1.44.11.1.4

> Description: | The name of this service

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starPDIFStatus

> Object ID: | enterprises.8164.1.44.1.1.5

> Description: | The state of this PDIF service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.

> Syntax: | INTEGER unknown(0) inservice(1) outofservice(2)

> Access: | Read-only

> Object: | starPDIFSessCurrent

> Object ID: | enterprises.8164.1.44.1.1.6

> Description: | The number of current sessions for this PDIF service.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessRemain

> Object ID: | enterprises.8164.1.44.1.1.7

> Description: | A count of the remaining capacity for this PDIF service, in terms of sessions. If a session limit is configured for this PDIF service, starPDIFSessRemain will identify the difference between this limit and starPDIFSessCurrent. If no individual limit has been configured for this service, starPDIFSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDIFSessRemain cannot be summed across multiple services.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentActive

> Object ID: | enterprises.8164.1.44.1.1.8

> Description: | The number of currently active sessions for this PDIF service

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentDormant

> Object ID: | enterprises.8164.1.44.1.1.9

> Description: | The number of currently dormant sessions for this PDIF service

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentIpv6Active

> Object ID: | enterprises.8164.1.44.1.1.10

> Description: | The number of currently active IPv6 sessions for this PDIF service

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentIpv6Dormant

> Object ID: | enterprises.8164.1.44.1.1.11

> Description: | The number of currently dormant IPv6 sessions for this PDIF service.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentIpv4Active

> Object ID: | enterprises.8164.1.44.1.1.12

> Description: | The number of currently active IPv4 sessions for this PDIF service.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFSessCurrentIpv4Dormant

> Object ID: | enterprises.8164.1.44.1.1.13

> Description: | The number of currently dormant IPv4 sessions for this PDIF service.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starPDIFBindIpAddress

> Object ID: | enterprises.8164.1.44.1.1.14

> Description: | The bind IP address for this PDIF service

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starPDIFBindIpPort

> Object ID: | enterprises.8164.1.44.1.1.15

> Description: | The bind IP port for this PDIF service

> Syntax: | Integer32

> Access: | Read-only

> Object: | starPDIFBindSlot

> Object ID: | enterprises.8164.1.44.1.1.16

> Description: | The physical slot number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.

> Syntax: | Integer32

> Access: | Read-only

> Object: | starPDIFBindPort

> Object ID: | enterprises.8164.1.44.1.1.17

> Description: | The physical port number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.

> Syntax: | SYNTAX Integer32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSGSNService(45)

> Object: | starSGSNSerTable

> Object ID: | enterprises.8164.1.45.1

> Description: | A table containing SGSN related information.

> Syntax: | SEQUENCE OF StarSGSNSerEntry

> Access: | Not-accessible

> Object: | starSGSNSerEntry

> Object ID: | enterprises.8164.1.45.1.1

> Description: | The statistics for a specific SGSN service.

> Syntax: | StarSGSNSerEntry

> Access: | Not-accessible

> Sequence: | starSGSNSerVpnID Gauge32 starSGSNSerSvcID Gauge32 starSessSGSNVpnName DisplayString starSessSGSNServName DisplayString starLinkM3UASs7rdId Gauge32 starSS7Pc Gauge32 starLinkM3UAPsId Gauge32

> Object: | starSGSNSerVpnID

> Object ID: | enterprises.8164.1.45.1.1.1

> Description: | The internal identification of the VPN (context).

> Syntax: | Gauge32

> Access: | not-accessible

> Object: | starSGSNSerSvcID

> Object ID: | enterprises.8164.1.45.1.1.2

> Description: | The internal identification of this service; unique within a specific context.

> Syntax: | Gauge32

> Access: | not-accessible

> Object: | starSessSGSNVpnName

> Object ID: | enterprises.8164.1.45.1.1.3

> Description: | The name of this VPN (context).

> Syntax: | DisplayString

> Access: | read-only

> Object: | starSessSGSNServName

> Object ID: | enterprises.8164.1.45.1.1.4

> Description: | The name of this service.

> Syntax: | DisplayString

> Access: | read-only

> Object: | starSessSGSNMcc

> Object ID: | enterprises.8164.1.45.1.1.5

> Description: | Mobile country code

> Syntax: | Octet String (size1..3))

> Access: | Read-only

> Object: | starSessSGSNMnc

> Object ID: | enterprises.8164.1.45.1.1.6

> Description: | Mobile network code

> Syntax: | Octet String (size1..3))

> Access: | Read-only

> Object: | starSessSGSNRncid

> Object ID: | enterprises.8164.1.45.1.1.7

> Description: | The RNC id

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSessSGSNHlrNum

> Object ID: | enterprises.8164.1.45.1.1.8

> Description: | The HLR id

> Syntax: | Octet String (Size(1..16))

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSS7Rd(46)

> Object: | starSS7RdTable

> Object ID: | enterprises.8164.1.46.1

> Description: | Table containing SS7Rd-related information

> Syntax: | Sequence of StarSS7RdEntry

> Access: | Not-Accessible

> Object: | starSS7RdEntry

> Object ID: | enterprises.8164.1.46.1.1

> Description: | The statistics for a specific ss7rd

> Syntax: | StarSS7RdEntry

> Access: | Not-Accessible

> Sequence: | starSS7rdId Index starSS7Pc starSS7M3UAPsId starSS7M3UAPspId starSS7MTP3LinkSetId starSS7MTP3LinkId starSS7SCTPSelfAddr starSS7SCTPPeerAddr starSS7SCTPSelfPort starSS7SCTPPeerPort

> Object: | starSS7rdid

> Object ID: | enterprises.8164.1.46.1.1.1

> Description: | SS7 Routing Domain identification.

> Syntax: | Gauge32

> Access: | Not accessible

> Object: | starSS7Pc

> Object ID: | enterprises.8164.1.46.1.1.2

> Description: | Point Code.

> Syntax: | Gauge32

> Access: | not-accessible

> Object: | starSS7M3UAPsId

> Object ID: | enterprises.8164.1.46.1.1.3

> Description: | Peer Server identification.

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSS7M3UAPspid

> Object ID: | enterprises.8164.1.46.1.1.4

> Description: | Peer Server Process Identification

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSS7MTP3LinkSetId

> Object ID: | enterprises.8164.1.46.1.1.5

> Description: | MTP3 LinkSet Identifier

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSS7MTP3LinkId

> Object ID: | enterprises.8164.1.46.1.1.6

> Description: | MTP3 Link Identifier

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSS7SCTPSelfAddr

> Object ID: | enterprises.8164.1.46.1.1.7

> Description: | Self-End-Point IP Address

> Syntax: | IpAddress

> Access: | Read-only

> Object: | starSS7SCTPPeerAddr

> Object ID: | enterprises.8164.1.46.1.1.8

> Description: | Peer Node IP Address

> Syntax: | IpAddress

> Access: | Read-Only

> Object: | starSS7SCTPSelfPort

> Object ID: | enterprises.8164.1.46.1.1.9

> Description: | Self end-point sctp port

> Syntax: | Gauge32

> Access: | Read-Only

> Object: | starSS7SCTPPeerPort

> Object ID: | enterprises.8164.1.46.1.1.10

> Description: | Peer end-point SCTP Port

> Syntax: | Gauge32

> Access: | Read-Only

> starentMIB(8164).starentMIBObjects(1).starentSccpNw(47)

> Object: | starSccpNwTable

> Object ID: | enterprises.8164.1.47.1

> Description: | Table containing Sccp Network-related information

> Syntax: | Sequence of StarSccpNwEntry

> Access: | Not-accessible

> Object: | starSccpNwEntry

> Object ID: | enterprises.8164.1.47.1.1

> Description: | Statistics for a specific Sccp Network

> Syntax: | StarSccpNwEntry

> Access: | Not-accessible

> Sequence: | starSccpNwld Gauge32 starSccpSsn Gauge32

> Object: | starSccpNwId

> Object ID: | enterprises.8164.1.47.1.1.1

> Description: | SCCP Network ID

> Syntax: | Gauge32

> Access: | Not accessible

> Object: | starSccpSsn

> Object ID: | enterprises.8164.1.47.1.1.2

> Description: | Sub-system number

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentSGTPService(48)

> Object: | starSGTPSerTable

> Object ID: | enterprises.8164.1.48.1

> Description: | Table containing SGTP Service-related info

> Syntax: | Sequence of StarSGTPSerEntry

> Access: | Not-accessible

> Object: | starSGTPSerEntry

> Object ID: | enterprises.8164.1.48.1.1

> Description: | Statistics for a specific SGTP Service

> Syntax: | StarSGTPSerEntry

> Access: | Not-accessible

> Sequence: | starSGTPSerVpnID Gauge32 starSGTPSerSvcID Gauge32 starSGTPVpnName Display String starSGTPServName Display String starSGTPSelfAddr IpAddress starSGTPPeerAddr IpAddress starSGTPSelfPort Gauge32 starSGTPPeerPort Gauge32

> Object: | starSGTPSerVpnID

> Object ID: | enterprises.8164.1.48.1.1.1

> Description: | Internal ID of the VPN (Context)

> Syntax: | Gauge32

> Access: | Not accessible

> Object: | starSGTPSerSvcID

> Object ID: | enterprises.8164.1.48.1.1.2

> Description: | Internal service ID unique within this context

> Syntax: | Gauge32

> Access: | Not-accessible

> Object: | starSGTPVpnName

> Object ID: | enterprises.8164.1.48.1.1.3

> Description: | Name of this VPN (Context)

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSGTPServName

> Object ID: | enterprises.8164.1.48.1.1.4

> Description: | Name of this service

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starSGTPSelfAddr

> Object ID: | enterprises.8164.1.48.1.1.5

> Description: | SGSN IP Address

> Syntax: | IP Address

> Access: | Read-only

> Object: | starSGTPPeerAddr

> Object ID: | enterprises.8164.1.48.1.1.6

> Description: | IP Address for the PeerNode

> Syntax: | IPAddress

> Access: | Read-only

> Object: | starSGTPSelfPort

> Object ID: | enterprises.8164.1.48.1.1.7

> Description: | The self end point SGTP port

> Syntax: | Gauge32

> Access: | Read-only

> Object: | starSGTPPeerPort

> Object ID: | enterprises.8164.1.48.1.1.8

> Description: | The peer end point SGTP port

> Syntax: | Gauge32

> Access: | Read-only

> starentMIB(8164).starentMIBObjects(1).starentIPMSServer(49)

> Object: | starIPMSServerTable

> Object ID: | enterprises.8164.1.49.1

> Description: | Table containing information on IPMS servers

> Syntax: | Sequence of StarIPMSServerEntry

> Access: | Not-accessible

> Object: | starIPMSServerEntry

> Object ID: | enterprises.8164.1.49.1.1

> Description: | Information about a particular IPMS Server

> Syntax: | StarIPMSServerEntry

> Access: | not-accessible

> Sequence: | starIPMSServerVpnID Gauge32, starIPMSServerAddr IpAddress, starIPMSServerVpnName DisplayString

> Object: | starIPMSServerVpnID

> Object ID: | enterprises.8164.1.49.1.1.1

> Description: | The internal identification of the VPN (context)

> Syntax: | Gauge32

> Access: | not-accessible

> Object: | starIPMSServerAddr

> Object ID: | enterprises.8164.1.49.1.1.2

> Description: | The IP address of the IPMS server within this VPN (context)

> Syntax: | IpAddress

> Access: | not-accessible

> Object: | starIPMSServerVpnName

> Object ID: | enterprises.8164.1.49.1.1.3

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentCert(50)

> Object: | starCertTable

> Object ID: | enterprises.8164.1.50.1

> Description: | Table containing information on X.509 certificates

> Syntax: | Sequence of StarCertEntry

> Access: | Not-accessible

> Object: | starCertEntry

> Object ID: | enterprises.8164.1.50.1.1

> Description: | Information on a particular X.509 Certificate

> Syntax: | StarCertEntry

> Access: | Not-accessible

> Sequence: | starCertSerialNumber Display-String starCertExpiryTime DateAndTime starCertIssuer Display-String

> Object: | starCertSerialNumber

> Object ID: | enterprises.8164.1.50.1.1.1

> Description: | Certificate serial number

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starCertExpiryTime

> Object ID: | enterprises.8164.1.50.1.1.2

> Description: | Certificate expiration date and time

> Syntax: | DateAndTime

> Access: | Read-only

> Object: | starCertIssuer

> Object ID: | enterprises.8164.1.50.1.1.3

> Description: | The certificate issuing agency

> Syntax: | DisplayString

> Access: | Read-0nly

> starentMIB(8164).starentMIBObjects(1).starentFile(51)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starFileTable

> Object ID: | enterprises.8164.1.51.1

> Description: | A table of files stored on a mass storage device

> Syntax: | SEQUENCE OF StarFileEntry

> Access: | Not-accessible

> Object: | starFileEntry

> Object ID: | enterprises.8164.1.51.1.1

> Description: | Information about a particular file on a mass storage device

> Syntax: | StarFileEntry

> Access: | Not-accessible

> Sequence: | starFileName DisplayString, starFileApplication INTEGER

> Object: | starFileName

> Object ID: | enterprises.8164.1.51.1.1.1

> Description: | The name (full path) of the file

> Syntax: | DisplayString

> Access: | Not-accessible

> Object: | starFileApplication

> Object ID: | enterprises.8164.1.51.1.1.2

> Description: | The application that owns this file

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | unknown(0) systemfile(1) cdrmod(2)

> starentMIB(8164).starentMIBObjects(1).starentFTPServ(52)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starFTPServTable

> Object ID: | enterprises.8164.1.52.1

> Description: | A table of FTP servers configured

> Syntax: | SEQUENCE OF StarFTPServEntry

> Access: | Not-accessible

> Object: | starFTPServEntry

> Object ID: | enterprises.8164.1.52.1.1

> Description: | Information about a particular FTP Server

> Syntax: | StarFTPServEntry

> Access: | Not-accessible

> Sequence: | starFTPServVpnID Unsigned32, starFTPServIpAddr IpAddress, starFTPServVpnName DisplayString

> Object: | starFTPServVpnID

> Object ID: | enterprises.8164.1.52.1.1.1

> Description: | The internal identification of the VPN (context) used to reach this FTP server

> Syntax: | Unsigned32

> Access: | Not-accessible

> Object: | starFTPServIpAddr

> Object ID: | enterprises.8164.1.52.1.1.2

> Description: | The IP address of the FTP server

> Syntax: | IpAddress

> Access: | Not-accessible

> Object: | starFTPServVpnName

> Object ID: | enterprises.8164.1.52.1.1.3

> Description: | The name of the VPN (context)

> Syntax: | DisplayString

> Access: | Not-accessible

> starentMIB(8164).starentMIBObjects(1).starentCSCFPeerServer(53)

> Object: | starCSCFPeerServerTable

> Object ID: | enterprises.8164.1.53.1

> Description: | A table containing PeerServer related information

> Syntax: | SEQUENCE OF StarCSCFPeerServerEntry

> Access: | Not Accessible

> Object: | starCSCFPeerServerEntry

> Object ID: | enterprises.8164.1.53.1.1

> Description: | The statistics for a specific CSCF service

> Syntax: | StarCSCFPeerServerEntry

> Access: | Not Accessible

> Sequence: | starCSCFPeerServerVpnID Gauge32, starCSCFPeerServerSvcID Gauge32, starCSCFPeerServerVpnName DisplayString, starCSCFPeerServerSvcName DisplayString, starCSCFPeerServerListName DisplayString

> Object: | starCSCFPeerServerVpnID

> Object ID: | enterprises.8164.1.53.1.1.1

> Description: | The internal identification of the VPN (context)

> Syntax: | Gauge32

> Access: | Not Accessible

> Object: | starCSCFPeerServerSvcID

> Object ID: | enterprises.8164.1.53.1.1.2

> Description: | The internal identification of this CSCF service; unique

> Syntax: | Gauge32

> Access: | Not Accessible

> Object: | starCSCFPeerServerVpnName

> Object ID: | enterprises.8164.1.53.1.1.3

> Description: | The name of this VPN (context)

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starCSCFPeerServerSvcName

> Object ID: | enterprises.8164.1.53.1.1.4

> Description: | The name of this CSCF-service

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starCSCFPeerServerListName

> Object ID: | enterprises.8164.1.53.1.1.5

> Description: | The name of the cscf-peer-server

> Syntax: | DisplayString

> Object: | starThreshGPRSSessions

> Object ID: | enterprises.8164.1.53.1.1.6

> Description: | The total number of GPRS sessions is above the configured threshold value.

> Objects: | starThreshInt, starThreshMeasuredInt

> Object: | starThreshClearGPRSSessions

> Object ID: | enterprises.8164.1.53.1.1.7

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt, starThreshMeasuredInt

> Object: | starThreshPerServiceGPRSSessions

> Object ID: | enterprises.8164.1.53.1.1.8

> Description: | The total number of GPRS sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName, starServiceServName, starThreshInt, starThreshMeasuredInt

> Object: | starThreshClearPerServiceGPRSSessions

> Object ID: | enterprises.8164.1.53.1.1.9

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName, starServiceServName, starThreshInt, starThreshMeasuredInt

> Object: | starThreshGPRSPdpSessions

> Object ID: | enterprises.8164.1.53.1.1.10

> Description: | The total number of GPRS PDP sessions is above the configured threshold value.

> Objects: | starThreshInt, starThreshMeasuredInt

> Object: | starThreshClearGPRSPdpSessions

> Object ID: | enterprises.8164.1.53.1.1.11

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt, starThreshMeasuredInt

> Object: | starThreshPerServiceGPRSPdpSessions

> Object ID: | enterprises.8164.1.53.1.1.12

> Description: | The total number of GPRS PDP sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName, starServiceServName, starThreshInt, starThreshMeasuredInt

> Object: | starThreshClearPerServiceGPRSPdpSessions

> Object ID: | enterprises.8164.1.53.1.1.13

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName, starServiceServName, starThreshInt, starThreshMeasuredInt

> starentMIB(8164).starentMIBObjects(1).starentSDH(54)

> Object: | starSDHTable

> Object ID: | enterprises.8164.1.54.1

> Description: | Table containing SDH information

> Syntax: | SEQUENCE OF StarSDHEntry

> Access: | Not Accessible

> Object: | starSDHEntry

> Object ID: | enterprises.8164.1.54.1.1

> Description: | Statistical data

> Syntax: | StarSDHEntry

> Access: | Not Accessible

> Sequence: | starSDHSlot Index starSDHPort Index starSDHOperState

> Object: | starSDHSlot

> Object ID: | enterprises.8164.1.54.1.1.1

> Description: | The slot number for this port

> Syntax: | Integer32(17..48)

> Access: | Not Accessible

> Object: | starSDHPort

> Object ID: | enterprises.8164.1.54.1.1.2

> Description: | The port number within this slot

> Syntax: | Integer32(1..8)

> Access: | Not Accessible

> Object: | starSDHOperState

> Object ID: | enterprises.8164.1.54.1.1.3

> Description: | A bitmask indicating the state of SDH layer SCT. 0x0000 Good 0x0001 lais 0x0002 linesd 0x0004 linesf 0x0010 lof 0x0020 los 0x0040 msrdi

> Syntax: | Integer32

> Access: | Read-Only

> starentMIB(8164).starentMIBObjects(1).starentSDHPath(55)

> Object: | starSDHPathTable

> Object ID: | enterprises.8164.1.55.1

> Description: | Table for SDH Path data

> Syntax: | SEQUENCE OF starSDHPathEntry

> Access: | Not Accessible

> Object: | starSDHPathEntry

> Object ID: | enterprises.8164.1.55.1.1

> Description: | Table statistical data

> Syntax: | starSDHPathEntry

> Access: | Not Accessible

> Sequence: | starSDHPathSlot Integer32 starSDHPathPort Integer32 starSDHPathNum Integer32 starSDHPathOperState Integer32

> Object: | starSDHPathSlot

> Object ID: | enterprises.8164.1.55.1.1.1

> Description: | Slot number for this port

> Syntax: | Integer32(17..48)

> Access: | Not Accessible

> Object: | starSDHPathPort

> Object ID: | enterprises.8164.1.55.1.1.2

> Description: | Port number within this slot

> Syntax: | Integer32(1..8)

> Access: | Not Accessible

> Object: | starSDHPathNum

> Object ID: | enterprises.8164.1.55.1.1.3

> Description: | Path number

> Syntax: | Integer32(1..3)

> Access: | Not Accessible

> Object: | starSDHPathOperState

> Object ID: | enterprises.8164.1.55.1.1.4

> Description: | A bitmask indicating the state of SDH Path HOP 0x0000 Good 0x0001 hopathsd 0x0002 hopathsf 0x0020ppdi 0x0040 prdi 0x0080 perdi 0x0100 perdival 0x0200 perdivaloff

> Syntax: | Integer32

> Access: | Read-Only

> starentMIB(8164).starentMIBObjects(1).starentE1Trib(56)

> Object: | starE1TribTable

> Object ID: | enterprises.8164.1.56.1

> Description: | Table for E1Trib data

> Syntax: | SEQUENCE OF StarE1TribEntry

> Access: | Not Accessible

> Object: | starE1TribEntry

> Object ID: | enterprises.8164.1.56.1.1

> Description: | Statistical data for table

> Syntax: | StarE1TribEntry

> Access: | Not Accessible

> Sequence: | starE1TribSlot Index starE1TribPort Index starE1TribPath Index starE1TribTug2 Integer32 starE1TribTu12 Integer32 starE1TribOperStateLOP Integer32 starE1TribOperState Integer32

> Object: | starE1TribSlot

> Object ID: | enterprises.8164.1.56.1.1.1

> Description: | The slot number for this port

> Syntax: | Integer32(17..48)

> Access: | Not Accessible

> Object: | starE1TribPort

> Object ID: | enterprises.8164.1.56.1.1.2

> Description: | The port number within this slot

> Syntax: | Integer32(1..8)

> Access: | Not Accessible

> Object: | starE1TribPath

> Object ID: | enterprises.8164.1.56.1.1.3

> Description: | Not shown

> Syntax: | Integer32(1..3)

> Access: | Not Accessible

> Object: | starE1TribTug2

> Object ID: | enterprises.8164.1.56.1.1.4

> Description: | Not shown

> Syntax: | Integer32(1..7)

> Access: | Not Accessible

> Object: | starE1TribTu12

> Object ID: | enterprises.8164.1.56.1.1.5

> Description: | Not shown

> Syntax: | Integer32(1..3)

> Access: | Not Accessible

> Object: | starE1TribOperStateLOP

> Object ID: | enterprises.8164.1.56.1.1.6

> Description: | A bitmask indicating the stare of SDH layer LOP 0x0000 Good 0x0001 lopathsd 0x0002 lopathsf 0x0100 erdi 0x0200 rdi 0x0400 lop 0x0800 ais 0x1000 lom

> Syntax: | Integer32

> Access: | Read Only

> Object: | starE1TribOperState

> Object ID: | enterprises.8164.1.56.1.1.7

> Description: | A bitmask indicating the state of the E1 Tributary 0x0000 Good 0x0001 inf0x0002 insmf 0x0004 incmf 0x0008 ooof 0x0010 raiccrc 0x0020 cfebe 0x0040 rai 0x0080 rmai 0x0100 aisd 0x0200 red 0x0400 ais 0x0800 ts16aisd

> Syntax: | Integer32

> Access: | Read Only

> starentMIB(8164).starentMIBObjects(1).starentGPRSLink(57)

> Object: | starGPRSLinkTable

> Object ID: | enterprises.8164.1.57.1

> Description: | A table containing GPRS Service Link related information.

> Syntax: | SEQUENCE of StarGPRSLinkEntry

> Access: | Not Accessible

> Object: | starGPRSLinkEntry

> Object ID: | enterprises.8164.1.57.1.1

> Description: | The link statistics for a specific GPRS service.

> Syntax: | StarGPRSLinkEntry

> Sequence: | starGPRSNsei Gauge32, starGPRSNsvci Gauge32, starGPRSBvci Gauge32,

> Object: | starGPRSNsei

> Object ID: | enterprises.8164.1.57.1.1.1

> Description: | Network Service Entity Identifier

> Syntax: | Gauge32

> Access: | Read-Only

> Object: | starGPRSNsvci

> Object ID: | enterprises.8164.1.57.1.1.2

> Description: | Network Service Virtual Circuit Identifier

> Syntax: | Gauge32

> Access: | Read-Only

> Object: | starGPRSBvci

> Object ID: | enterprises.8164.1.57.1.1.3

> Description: | Base Station System GPRS (General Packet Radio Service) Protocol Virtual Circuit Identifier.

> Syntax: | Gauge32

> Access: | Read-Only

> starentMIB(8164).starentMIBObjects(1).starentFractE1Trib(58)

> Object: | starFractE1TribTable

> Object ID: | enterprises.8164.1.58.1

> Description: | A table ...

> Syntax: | SEQUENCE of StarFractTribEntry

> Access: | Not Accessible

> Object: | starFractE1TribEntry

> Object ID: | enterprises.8164.1.58.1.1

> Description: | Information about a specific Entry

> Syntax: | starFractE1TribEntry

> Sequence: | starFractE1TribSlot Integer32, starFractE1TribPort I Integer32, starFractE1TribPath Integer32, starFractE1TribTug2 Integer32, starFractE1TribTu12 Integer32 starFractE1TribBundNum Integer32, starFractE1TribTimeslots DisplayString

> Object: | starFractE1TribSlot

> Object ID: | enterprises.8164.1.58.1.1.1

> Description: | Slot number for this port

> Syntax: | Integer32(17..48)

> Access: | Not Accessible

> Object: | starFractE1TribPort

> Object ID: | enterprises.8164.1.58.1.1.2

> Description: | Port number within slot

> Syntax: | Integer32(1..8)

> Access: | Not Accessible

> Object: | starFractE1TribPath

> Object ID: | enterprises.8164.1.58.1.1.3

> Description: | Not shown

> Syntax: | Integer32(1..3)

> Object: | starFractE1TribTug2

> Object ID: | enterprises.8164.1.58.1.1.4

> Description: | Not shown

> Syntax: | Integer32(1..84)

> Access: | Not Accessible

> Object: | starFractE1TribTu12

> Object ID: | enterprises.8164.1.58.1.1.5

> Description: |

> Syntax: | Integer32(1..3)

> Access: | not-accessible

> Object: | starFractE1TribBundNum

> Object ID: | enterprises.8164.1.58.1.1.6

> Description: | Not Given

> Syntax: | Integer32(0..31)

> Access: | Not Accessible

> Object: | starFractE1TribTimeslots

> Object ID: | enterprises.8164.1.58.1.1.7

> Description: | Not Given

> Syntax: | Display/String

> Access: | Read-Only

> starentMIB(8164).starentMIBObjects(1).starentStorage(59)
> IMPORTANT: The objects in this table are not accessible via SNMP. They are intended for use within traps.

> Object: | starStorageTable

> Object ID: | enterprises.8164.1.59.1

> Description: | A table of mass storage devices

> Syntax: | SEQUENCE OF StarStorageEntry

> Access: | Not Accessible

> Object: | starStorageEntry

> Object ID: | enterprises.8164.1.59.1.1

> Description: | Information about a particular file on a mass storage device

> Syntax: | StarStorageEntry

> Access: | Not Accessible

> Sequence: | starStorageSlot Integer32, starStorageName DisplayString, starStorageDeviceType INTEGER

> Object: | starStorageSlot

> Object ID: | enterprises.8164.1.59.1.1.1

> Description: | The slot number of the card holding this storage device

> Syntax: | Integer32(1..16)

> Access: | Not Accessible

> Object: | starStorageName

> Object ID: | enterprises.8164.1.59.1.1.2

> Description: | The name of the storage device

> Syntax: | DisplayString

> Access: | Not Accessible

> Object: | starStorageDeviceType

> Object ID: | enterprises.8164.1.59.1.1.3

> Description: | The storage device type. A value of independent(1) means that the device can be accessed as a standalone device, and is not part of a raid array. A value of raid(2) means that this device is a raid array. A value of raidmember(3) means the device is part of a raid array, and thus cannot be read/written to outside of the raid array

> Syntax: | INTEGER

> Access: | Not Accessible

> Enumeration: | unknown(0), independent(1), raid(2), raidmember(3)

> starentMIB(8164).starentMIBObjects(1).starentPDGSys(60)

> Object: | starFNGSysStatus

> Object ID: | 8164.1.60.1

> Description: | The overall status of the chassis as a FNG service. A value of noservice(1) means that the chassis is not configured/licensed for FNG; active(2) indicates that at least one FNG service is available for processing sessions; temporary(3) indicates that FNG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no FNG service is currently active, but one or more FNG services are configured

> Syntax: | INTEGER { unknown(0), noservice(1), active(2), temporary(3), outofservice(4)}

> Access: | read-only

> Object: | starFNGSysNumService

> Object ID: | 8164.1.60.2

> Description: | The number of FNG services configured

> Syntax: | Unsigned32

> Access: | read-only

> Units: | Services

> Object: | starFNGSysSessCurrent

> Object ID: | 8164.1.60.3

> Description: | The number of current FNG sessions for this chassis

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSysSessCurrActive

> Object ID: | 8164.1.60.4

> Description: | The number of FNG services configured

> Syntax: | Unsigned32

> Access: | read-only

> Object: | starFNGSysSessCurrent

> Object ID: | 8164.1.60.5

> Description: | The number of currently dormant FNG sessions for this chassis

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSysSessTtlSetup

> Object ID: | 8164.1.60.6

> Description: | The cumulative total number of FNG sessions that has been setup

> Syntax: | Counter32

> Access: | read-only

> Object: | starFNGSysChildSACurrent

> Object ID: | 8164.1.60.7

> Description: | The number of current FNG child SAs for this chassis

> Syntax: | Gauge32

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentPDGSys(61)

> Object: | starFNGTable

> Object ID: | 8164.1.61.1

> Description: | A table of per-service FNG information

> Syntax: | SEQUENCE OF StarFNGEntry

> Access: | not-accessible

> Object: | starFNGEntry

> Object ID: | 8164.1.61.1.1

> Description: | The information for a FNG service

> Syntax: | StarFNGEntry

> Access: | not-accessible

> Sequence: | starFNGSvcID StarShortID starFNGVpnID Gauge32, starFNGVpnName DisplayString, starFNGServName DisplayString, starFNGStatus INTEGER, starFNGSessCurrent Gauge32, starFNGSessRemain Gauge32, starFNGSessCurrentActive Gauge32, starFNGSessCurrentDormant Gauge32, starFNGSessCurrentIpv6Active Gauge32, starFNGSessCurrentIpv6Dormant Gauge32, starFNGSessCurrentIpv4Active Gauge32, starFNGSessCurrentIpv4Dormant Gauge32, starFNGBindIpAddress IpAddress, starFNGBindIpPort Integer32, starFNGBindSlot Integer32, starFNGBindPort Integer32

> Object: | starFNGSvcID

> Object ID: | 8164.1.61.1.1.1

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)

> Syntax: | StarShortID

> Access: | not-accessible

> Object: | starFNGVpnID

> Object ID: | 8164.1.61.1.1.2

> Description: | The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the FNG device; in general tarFNGVpnName should be used to identify the VPN (context)

> Syntax: | StarShortID

> Access: | not-accessible

> Object: | starFNGVpnID

> Object ID: | 8164.1.61.1.1.3

> Description: | The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the FNG device; in general starFNGVpnName should be used to identify the VPN (context)

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGServName

> Object ID: | 8164.1.61.1.1.4

> Description: | The name of this service

> Syntax: | DisplayString

> Access: | read-only

> Object: | starFNGStatus

> Object ID: | 8164.1.61.1.1.5

> Description: | The state of this FNG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault

> Syntax: | INTEGER

> Access: | read-only

> Object: | starFNGSessCurrent

> Object ID: | 8164.1.61.1.1.6

> Description: | The number of current sessions for this FNG service

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSessRemain

> Object ID: | 8164.1.61.1.1.7

> Description: | A count of the remaining capacity for this FNG service, in terms of sessions. If a session limit is configured for this FNG service, starFNGSessRemain will identify the difference between this limit and starFNGSessCurrent. If no individual limit has been configured for this service, starFNGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starFNGSessRemain cannot be summed across multiple services

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSessCurrentActive

> Object ID: | 8164.1.61.1.1.8

> Description: | The number of currently active sessions for this FNG service

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSessCurrentDormant

> Object ID: | 8164.1.61.1.1.9

> Description: | The number of currently dormant sessions for this FNG service

> Syntax: | Gauge32

> Access: | read-only

> Object: | starFNGSessCurrentIpv6Active

> Object ID: | 8164.1.61.1.1.10

> Description: | The number of currently active IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv6Dormant

> Object ID: | 8164.1.61.1.1.11

> Description: | The number of currently dormant IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv4Active

> Object ID: | 8164.1.61.1.1.12

> Description: | The number of currently active IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', and the value for starPDGSessCurrentIPv4Dormant will always be zero

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv4Dormant

> Object ID: | 8164.1.61.1.1.13

> Description: | The number of currently dormant IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', so the value for starPDGSessCurrentIPv4Dormant will always be zero

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGBindIpAddress

> Object ID: | 8164.1.61.1.1.14

> Description: | The bind IP address for this PDG service

> Syntax: | IpAddress

> Access: | read-only

> Object: | starPDGBindIpPort

> Object ID: | 8164.1.61.1.1.15

> Description: | The bind IP port for this PDG service

> Syntax: | Integer32

> Access: | read-only

> Object: | starPDGBindSlot

> Object ID: | 8164.1.61.1.1.16

> Description: | The physical slot number for the physical port which holds the interface bound to the starPDGBindIpAddress address

> Syntax: | Integer32

> Access: | read-only

> Object: | starPDGBindPort

> Object ID: | 8164.1.61.1.1.17

> Description: | The physical port number for the physical port which holds the interface bound to the starPDGBindIpAddress address

> Syntax: | Integer32

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentPDGSys(62)

> Object: | starPDGSysStatus

> Object ID: | 8164.1.62.1

> Description: | The overall status of the chassis as a PDG service. A value of noservice(1) means that the chassis is not configured/licensed for PDG; active(2) indicates that at least one PDG service is available for processing sessions; temporary(3) indicates that PDG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDG service is currently active, but one or more PDG services are configured.

> Syntax: | unknown(0) noservice(1) active(2) temporary(3) outofservice(4)

> Access: | read-only

> Object: | starPDGSysNumService

> Object ID: | 8164.1.62.2

> Description: | The number of PDG services configured

> Syntax: | Unsigned32

> Access: | read-only

> Units: | Services

> Object: | starPDGSysSessCurrent

> Object ID: | 8164.1.62.3

> Description: | The number of current PDG sessions for this chassis

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSysSessCurrActive

> Object ID: | 8164.1.62.4

> Description: | he number of currently active PDG sessions for this chassis.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSysSessCurrDormant

> Object ID: | 8164.1.62.5

> Description: | The number of currently dormant PDG sessions for this chassis

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSysSessTtlSetup

> Object ID: | 8164.1.62.6

> Description: | The cumulative total number of PDG sessions that has been setup

> Syntax: | Counter32

> Access: | read-only

> Object: | starPDGSysChildSACurrent

> Object ID: | 8164.1.62.7

> Description: | The number of current PDG child SAs for this chassis

> Syntax: | Gauge32

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentPDGSys(63)

> Object: | starPDGTable

> Object ID: | 8164.1.63.1

> Description: | A table of per-service PDG information

> Syntax: | SEQUENCE OF StarPDGEntry

> Access: | not-accessible

> Object: | starPDGEntry

> Object ID: | 8164.1.63.1.1

> Description: | The information for a PDG service

> Syntax: | StarPDGEntry

> Access: | not-accessible

> Sequence: | starPDGSvcID starPDGVpnID starPDGVpnName starPDGServName starPDGStatus starPDGSessCurrent starPDGSessRemain starPDGSessCurrentActive starPDGSessCurrentDormant starPDGSessCurrentIpv6Active starPDGSessCurrentIpv6Dormant starPDGSessCurrentIpv4Active starPDGSessCurrentIpv4Dormant starPDGBindIpAddress starPDGBindIpPort

> Object: | starPDGSvcID

> Object ID: | 8164.1.63.1.1.1

> Description: | The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)

> Syntax: | StarShortID

> Access: | not-accessible

> Object: | starPDGVpnID

> Object ID: | 8164.1.63.1.1.2

> Description: | The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the PDG device; in general starPDGVpnName should be used to identify the VPN (context)

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGVpnName

> Object ID: | 8164.1.63.1.1.3

> Description: | The VPN (context) name

> Syntax: | DisplayString

> Access: | read-only

> Object: | starPDGServName

> Object ID: | 8164.1.63.1.1.4

> Description: | The name of this service

> Syntax: | DisplayString

> Access: | read-only

> Object: | starPDGStatus

> Object ID: | 8164.1.63.1.1.5

> Description: | The state of this PDG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.

> Syntax: | unknown(0) inservice(1) outofservice(2)

> Access: | read-only

> Object: | starPDGSessCurrent

> Object ID: | 8164.1.63.1.1.6

> Description: | The number of current sessions for this PDG service.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessRemain

> Object ID: | 8164.1.63.1.1.7

> Description: | A count of the remaining capacity for this PDG service, in terms of sessions. If a session limit is configured for this PDG service, starPDGSessRemain will identify the difference between this limit and starPDGSessCurrent. If no individual limit has been configured for this service, starPDGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDGSessRemain cannot be summed across multiple services.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentActive

> Object ID: | 8164.1.63.1.1.8

> Description: | The number of currently active sessions for this PDG service

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentDormant

> Object ID: | 8164.1.63.1.1.9

> Description: | The number of currently dormant sessions for this PDG service

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv6Active

> Object ID: | 8164.1.63.1.1.10

> Description: | The number of currently active IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv6Dormant

> Object ID: | 8164.1.63.1.1.11

> Description: | The number of currently dormant IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv4Active

> Object ID: | 8164.1.63.1.1.12

> Description: | The number of currently active IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', and the value for tarPDGSessCurrentIPv4Dormant will always be zero.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGSessCurrentIpv4Dormant

> Object ID: | 8164.1.63.1.1.13

> Description: | The number of currently dormant IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', so the value for starPDGSessCurrentIPv4Dormant will always be zero.

> Syntax: | Gauge32

> Access: | read-only

> Object: | starPDGBindIpAddress

> Object ID: | 8164.1.63.1.1.14

> Description: | The bind IP address for this PDG service

> Syntax: | IpAddress

> Access: | read-only

> Object: | starPDGBindIpPort

> Object ID: | 8164.1.63.1.1.15

> Description: | The bind IP port for this PDG service

> Syntax: | Integer32

> Access: | read-only

> Object: | starPDGBindSlot

> Object ID: | 8164.1.63.1.1.16

> Description: | The bind IP port for this PDG service

> Syntax: | Integer32

> Access: | read-only

> Object: | starPDGBindPort

> Object ID: | 8164.1.63.1.1.17

> Description: | The physical port number for the physical port which holds the interface bound to the starPDGBindIpAddress address.

> Syntax: | Integer32

> Access: | read-only

> starentMIB(8164).starentTraps(2)

> Object: | starCardTempOverheat

> Object ID: | enterprises.8164.2.1

> Description: | The card has reached a temperature beyond its safe operating range. Probable Cause: External temperature is too high; One or more fan failures; blockages the prevent fan air inflow/outflow. Action to be Taken: Inspect chassis for any item that may be blocking chassis air flow. Verify adjacent equipment is not obstructing air flow. Verify that the fans are running via the CLI/Web Element Manager. Check air filters. Check chassis maintenance schedule to see if chassis needs routine air filter replacement. Verify room temperature is within acceptable operating conditions. Clear Condition: This condition is cleared when the card reaches its operating temperature range or is removed from the system. Condition Clear Alarm: This condition is cleared by a starCardTempOK notification.

> Objects: | starSlotNum starCardTemperature

> Object: | starCardTempOK

> Object ID: | enterprises.8164.2.2

> Description: | The temperature of the card is now within its safe operating range. This notification is only generated if the card has previously generated a starCardTempOverheat notification. Action to be Taken: No action required. The cause for the card overheat condition should be investigated.

> Objects: | starSlotNum starCardTemperature

> Object: | starCardReset

> Object ID: | enterprises.8164.2.3

> Description: | A reset operation has been invoked on the card.

> IMPORTANT: This trap is obsolete.

> Objects: | starSlotNum starCardType

> Object: | starCardRebootRequest

> Object ID: | enterprises.8164.2.4

> Description: | A Reboot operation has been invoked on this card by an administrator. If successful, a subsequent CardDown trap is typically generated. Action to be Taken: No action required. If the reboot was not scheduled the admin logs can be examined to determine who invoked the reboot operation.

> Objects: | starSlotNum starCardType

> Object: | starCardUp

> Object ID: | enterprises.8164.2.5

> Description: | The card is up (operational).

> Objects: | starSlotNum starCardType

> Object: | starCardVoltageFailure

> Object ID: | enterprises.8164.2.6

> Description: | A voltage regulation failure has been detected this card. Probable Cause: Problem with incoming power; failure of power filters; hardware issue with card. Note that this is an extremely abnormal condition. Action To Be Taken: Verify that the power supplied to the chassis is operating correctly; use the CLI/Web Element Manager to check the state of the chassis power filters; replace the card. Clear Condition: This is not a recoverable error except via restarting the card, so the condition is only cleared via a starCardUp or starCardActive notification.

> Objects: | starSlotNum starCardType

> Object: | starCardRemoved

> Object ID: | enterprises.8164.2.7

> Description: | A card has been removed from the chassis. Probable Cause: An operator has physically unlocked and removed a card from the chassis Action to be Taken: No action is required. If the card removal was unplanned, the admin logs can identify the time when the card was initially unlocked.

> Objects: | starSlotNum starCardType

> Object: | starCardInserted

> Object ID: | enterprises.8164.2.8

> Description: | A card has been inserted into the chassis.

> Objects: | starSlotNum starCardType

> Object: | starCardBootFailed

> Object ID: | enterprises.8164.2.9

> Description: | A card has failed to startup properly. The card is not operational. Probable Cause: The system logs should contain additional information about the cause of the boot failure.

> Objects: | starSlotNum starCardType

> Object: | starCardFailed

> Object ID: | enterprises.8164.2.10

> Description: | The card has failed and is no longer operational. This trap is obsolete and has been replaced with more specific traps to identify specific failures.

> Objects: | starSlotNum starCardType

> Object: | starCardSWFailed

> Object ID: | enterprises.8164.2.11

> Description: | An unrecoverable software error has occurred on the card. This trap is obsolete and has been replaced with more specific traps to identify specific failures.

> Objects: | starSlotNum

> IMPORTANT: This trap is obsolete.

> Object: | starCardRCCFailed

> Object ID: | enterprises.8164.2.12

> Description: | The RCC has failed. Probable Cause: A hardware failure on the RCC card.

> IMPORTANT: This trap is obsolete.

> Objects: | starSlotNum

> Object: | starCardMismatch

> Object ID: | enterprises.8164.2.13

> Description: | The card does not match its configuration, or the card does not match the slot it was inserted into, or the card is of an unsupported type. Probable Cause: A card was inserted into a slot which was configured for a different type of card. For example, a Gigabit Ethernet card was inserted into a slot configured for a Fast Ethernet card. Clear Condition: A starCardUp or starCardActive notification would indicate that this condition has been cleared.

> Objects: | starSlotNum starCardType

> Object: | starCardFailureLEDOn

> Object ID: | enterprises.8164.2.14

> Description: | The failure LED is illuminated on the card. This trap is obsolete and has been replaced with more specific traps for specific failures.

> Objects: | starSlotNum starCardType

> IMPORTANT: This object is obsolete.

> Object: | starCardFailureLEDOff

> Object ID: | enterprises.8164.2.15

> Description: | The failure LED is no longer illuminated on the card. This notification is only generated if the card has previously generated a starCardFailureLEDOn notification. This trap is obsolete and has been replaced with more specific traps for specific failures.

> Objects: | starSlotNum starCardType

> Object: | starCardPACMigrateStart

> Object ID: | enterprises.8164.2.16

> Description: | A PAC/PSC Migration operation has begun. The first varbind identifies the PAC/PSC being migrated away from; the second varbind identifies the PAC being migrated to. Probable Cause: This is typically caused by an operator action; it can also represent the system recovering from a software or hardware fault. Clear Condition: A starCardPACMigrateComplete is generated when the migration is completed.

> Objects: | starSlotNum starSlotNum

> Object: | starCardPACMigrateComplete

> Object ID: | enterprises.8164.2.17

> Description: | A PAC/PSC Migration operation has successfully completed. The first varbind identifies the PAC/PSC that was migrated away from; the second varbind identifies the PAC/PSC that was migrated to.

> Objects: | starSlotNum starSlotNum

> Object: | starCardPACMigrateFailed

> Object ID: | enterprises.8164.2.18

> Description: | A PAC/PSC Migration operation has failed. The first varbind identifies the PAC/PSC that was attempted to be migrated away from; the second varbind identifies the PAC/PSC that was attempted to be migrated to. Probable Cause: The PAC/PSC being migrated to was removed or reset before the migration completed; the migration operation was terminated by an operator; or a software or hardware failure on either PAC/PSC involved in the migration operation. Clear Condition: The PAC/PSC in question will be reset; a starCardUp notification will be generated when the card is operational again.

> Objects: | starSlotNum starSlotNum

> Object: | starCardSPCSwitchoverStart

> Object ID: | enterprises.8164.2.19

> Description: | An SPC switchover operation has begun. The first varbind identifies the SPC being switched away from; the second varbind identifies the SPC being switched to. Note that since an SPC switchover can cause a momentary loss of communication through the management (SPIO) interface, it is possible that this trap will not be successfully delivered. Probable Cause: This is typically caused by an operator action; it can also represent the system recovering from a software or hardware fault. Action to be Taken: If the SPC switchover was unplanned, the admin logs should be examined for the cause of the switchover. If the cause was a software failure, the system crash logs should be examined. Clear Condition: Verify the SPC switchover completes successfully. Clear Condition Alarm: A starCardSPCSwitchoverComplete is generated when the switchover operation has completed.

> Objects: | starSlotNum starSlotNum

> Object: | starCardSPCSwitchoverComplete

> Object ID: | enterprises.8164.2.20

> Description: | An SPC Switchover has completed successfully. The starSlotNum varbind identifies the new primary SPC. Action to be Taken: If the SPC switchover was unplanned, the admin logs should be examined for the cause of the switchover. If the cause was a software failure, the system crash logs should be examined.

> Objects: | starSlotNum

> Object: | starCardSPCSwitchoverFailed

> Object ID: | enterprises.8164.2.21

> Description: | An SPC switchover operation has failed. The first varbind identifies the SPC that was attempted to be switched away from; the second varbind identifies the SPC that was attempted to be switched to. Probable Cause: The SPC being migrated to was removed or reset before the migration completed; the migration operation was terminated by an operator; or a software or hardware failure on either SPC. Action to be Taken: Verify that both SPCs have the card locks in the locked position; examine the admin logs for the cause of the failure. If the cause was a software failure, the system crash logs should be examined. Clear Condition: The SPC in question will be reset; a starCardUp notification will be generated when the card is operational again.

> Objects: | starSlotNum starSlotNum

> Object: | starFanFailed

> Object ID: | enterprises.8164.2.22

> Description: | One of more fans have failed on the indicated fan controller. Probable Cause: A hardware failure on the fan tray. The fan tray should be replaced. Action to be Taken: Verify there is no physical obstruction to the fans; Replace the fan tray. Clear Condition: Verify the fans are running Condition Clear Alarm: A starFanInserted notification will be generated when the fan tray is replaced.

> Objects: | starFanNum starFanStatus

> Object: | starFanRemoved

> Object ID: | enterprises.8164.2.23

> Description: | A fan tray has been removed. Action to be Taken: Replace the fan tray. Clear Condition: Verify both fan trays are present and operational. Condition Clear Alarm: A starFanInserted notification will be generated when the fan tray is replaced.

> Objects: | starFanNum

> Object: | starFanInserted

> Object ID: | enterprises.8164.2.24

> Description: | A fan tray has been inserted.

> Objects: | starFanNum

> Object: | starLogThreshold

> Object ID: | enterprises.8164.2.25

> Description: | A system log has reached its maximum size. This trap is obsolete.

> Objects: | starLogName starLogCurSize starLogMaxSize

> IMPORTANT: This object is obsolete.

> Object: | starCPUBusy

> Object ID: | enterprises.8164.2.26

> Description: | The CPU is experiencing very high usage. Probable Cause: For SPC/SMC CPUs this typically represents an abnormal amount of management (CLI, SNMP, CORBA) requests. For PAC/PSC cards this indicates that the system is reaching its capacity. Action to be Taken: For SPC/SMC cards, this may be a transient condition because of a burst of management activity. Monitor the CPU usage and if it is persistently high, examine the CPU table to determine which management activity is causing the excessive usage. For PAC/PSC cards, this indicates the system is nearing its overall capacity. Monitor CPU usage and if it is persistently high, the system may need additional PACs/PSCs to keep up with the system load. Clear Condition: Verify that CPU usage returned to a normal load. This can represent a transient condition; the trap will be periodically repeated if the condition persists.

> Objects: | starCPUSlot starCPUNumber

> Object: | starCPUMemoryLow

> Object ID: | enterprises.8164.2.27

> Description: | The CPU is experiencing a low memory condition. Probable Cause: For SPC/SMC CPUs this typically represents an abnormal number of management sessions, in particular CLI sessions. For PAC/PSC cards this indicates that the system is reaching its capacity. Action to be Taken: For SPC/SMC cards, this may be a transient condition because of a burst of management activity. Monitor memory usage and if it is persistently high, examine the CPU table to determine which management activity is causing the excessive usage. Verify that large numbers of CLI sessions are not being generated and, if needed, terminate extra sessions. For PAC/PSC cards, this indicated the system is nearing its overall capacity. Monitor memory usage and if it is persistently high, the system may need additional PACs/PSCs or additional PAC/PSC memory to keep up with the system load. Clear Condition: Verify that memory usage returned to a normal load. This can represent a transient condition; the trap will be periodically repeated if the condition persists.

> Objects: | starCPUSlot starCPUNumber

> Object: | starCPUMemoryFailed

> Object ID: | enterprises.8164.2.28

> Description: | The memory on this CPU has failed. Probable Cause: This indicates a hardware problem. Action to be Taken: Replace the failing card. Clear Condition: The card will be reset; a starCardUp will be generated if the card is restored to an operational state.

> Objects: | starCPUSlot starCPUNumber

> Object: | starCPUFailed

> Object ID: | enterprises.8164.2.29

> Description: | The CPU has failed. Probable Cause: This indicates a hardware problem. Action to be Taken: Replace the failing card. Clear Condition: The card will be reset; a starCardUp will be generated if the card is restored to an operational state.

> Objects: | starCPUSlot starCPUNumber

> Object: | starCPUWatchDogExpired

> Object ID: | enterprises.8164.2.30

> Description: | The watch dog timer has failed on this CPU. Probable Cause: This could indicate an extremely busy CPU, a software problem, or a hardware issue. Action to be Taken: Check the admin logs for an indication of the problem. Check the system crash logs for an indication of software problems. If the problem persists, replace the card. Clear Condition: Verify that an SPC/SMC switchover or PAC/PSC migration completes successfully to recover from the failure condition. Condition Clear Alarm: A starCardUp will be generated if the card is restored to an operational state.

> Objects: | starCPUSlot starCPUNumber

> Object: | starNPUARPPoolExhausted

> Object ID: | enterprises.8164.2.31

> Description: | The ARP pool on this NPU manager is exhausted. When this occurs, the ARP entry isn't added and traffic to the local device is forwarded through a slower path. Action To Be Taken: Reduce the total number of directly connected devices or clear ARP entries.

> Objects: | starNPUMgrNumber

> Object: | starPowerFilterUnitFailed

> Object ID: | enterprises.8164.2.32

> Description: | A Power Filter Unit (PFU) failed. Probable Cause: The external power source has failed or has been disconnected, or a hardware failure on the PFU. Action to be Taken: Verify that the input power to the power filter is operational and repair if needed. Verify that the connections to the power filter are intact and that the power filter is properly inserted into the chassis. Replace the power filter if required. Clear Condition: Verify that both power filters are operating. Condition Clear Alarm: A starPowerFilterAvail will be generated when the power filter is replaced.

> Objects: | starPowerNumber

> Object: | starPowerFilterUnitUnavail

> Object ID: | enterprises.8164.2.33

> Description: | A Power Filter Unit (PFU) is unavailable. Probable Cause: The power filter has been removed from the chassis, or no power is being provided to the PFU. Action to be Taken: If the power filter removal wasn't planned, Verify that the input power to the power filter is operational and repair if needed. Verify that the connections to the power filter are intact and that the power filter is properly inserted into the chassis. Replace the power filter if required. Clear Condition: Verify that both power filters are operating. Condition Clear Alarm: A starPowerFilterUnitAvail will be generated when the power filter is replaced.

> Objects: | starPowerNumber

> Object: | starPowerFilterUnitAvail

> Object ID: | enterprises.8164.2.34

> Description: | A Power Filter Unit (PFU) is available. This typically means that a PFU has been inserted into the chassis or has its power source restored. Action to be Taken: No action required.

> Objects: | starPowerNumber

> Object: | starAlertsDisabled

> Object ID: | enterprises.8164.2.37

> Description: | The sending of SNMP Traps has been disabled because too many alerts were generated within the defined window type. Probable Cause: Either a large number of SNMP notifications are being generated, or the configured threshold which limits the number of notifications is set too aggressively. Actions to be Taken: Examine the admin logs and the SNMP trap logs to determine the source of the large number of traps and take appropriate actions; verify that the configured limit for the rate at which traps will be sent is appropriate for your environment. Clear Condition Alarm: Clear Condition Alarm: When the rate of SNMP notifications goes down a starAlertsEnabled notification is generated.

> Objects: | starMaxAlertsPerTime starWindowTime

> Object: | starAlertsEnabled

> Object ID: | enterprises.8164.2.38

> Description: | The sending of SNMP Traps has been re-enabled.

> Object: | starAAAAuthServerUnreachable

> Object ID: | enterprises.8164.2.39

> Description: | The Authentication, Authorization and Accounting (AAA) server cannot be reached. Probable Cause: The AAA server is down, or there is a network issue preventing communication with the AAA server. Actions to be Taken: Restore the AAA server to an operational status; Verify that the AAA server is reachable by performing a 'ping' operation from the CLI in the appropriate context. Check the admin logs for notification of communication problems. Clear Condition: Verify that communication to the AAA authentication server has been restored. Condition Clear Alarm: When this condition clears a starAAAAuthServerReachable notification will be generated. Note that if in a AAA group all the configured RADIUS servers are detected as Down, their state is brought back to Active before the deadtime expiry period so that call setup signaling with AAA can proceed for subsequent requests. Therefore, when the last Active authentication server in the group is detected as Down, starAAAAuthServerUnreachable is generated, and immediately later when the server state changes to Active, starAAAAuthServerReachable is generated. This behavior is the same when there is only one RADIUS server configured.

> Objects: | radiusAuthServerIndex radiusAuthServerAddress

> Object: | starAAAAuthServerReachable

> Object ID: | enterprises.8164.2.40

> Description: | The Authentication, Authorization and Accounting (AAA) server is now reachable. This can be the result of a system startup, the configuration of a new server, or a previously unreachable server becoming reachable. Action to be Taken: No Action Required.

> Objects: | radiusAuthServerIndex radiusAuthServerAddress

> Object: | starAAAAuthServerMisconfigured

> Object ID: | enterprises.8164.2.41

> Description: | The Authentication, Authorization and Accounting (AAA) server has been misconfigured. This server is not usable until this condition is repaired. Action to be Taken: Examine the system configuration and correct the misconfiguration. See the user documentation for details on AAA configuration. Clear Condition: Verify that communication to the AAA authentication server has been restored. Condition Clear Alarm: When this condition clears a starAAAAuthServerReachable notification will be generated.

> Objects: | radiusAuthServerIndex radiusAuthServerAddress

> Object: | starAAAAccServerUnreachable

> Object ID: | enterprises.8164.2.42

> Description: | The Authentication, Authorization and Accounting (AAA) server cannot be reached. Probable Cause: The AAA server is down, or there is a network issue preventing communication with the AAA server. Actions to be Taken: Restore the AAA server to an operational status; Verify that the AAA server is reachable by performing a 'ping' operation from the CLI in the appropriate context. Check the admin logs for notification of communication problems. Clear Condition: Verify that communication to the AAA accounting server has been restored. Condition Clear Alarm: When this condition clears a starAAAAccServerReachable notification will be generated. Note that if in a AAA group all the configured RADIUS servers are detected as Down, their state is brought back to Active before the deadtime expiry period so that call setup signaling with AAA can proceed for subsequent requests. Therefore, when the last Active Accounting server in the group is detected as Down, starAAAAccServerUnreachable is generated, and immediately later when the server state changes to Active, starAAAAccServerReachable is generated. This behavior is the same when there is only one RADIUS server configured.

> Objects: | radiusAccServerIndex radiusAccServerAddress

> Object: | starAAAAccServerReachable

> Object ID: | enterprises.8164.2.43

> Description: | The Authentication, Authorization and Accounting (AAA) server is now reachable. This can be the result of a system startup, the configuration of a new server, or a previously unreachable server becoming reachable. Note that since Accounting servers are not responding to 'hello'-type messages, it is not always possible to accurately determine when an accounting server is reachable. A server may be declared 'reachable' when the ST-16 is ready to start using the server, but before any acknowledgement is actually received from the server. Once accounting information actually is sent to the server a starAAAAccServerUnreachable will be generated if the server does not properly respond. Action to be Taken: No Action Required.

> Objects: | radiusAccServerIndex radiusAccServerAddress

> Object: | starAAAAccServerMisconfigured

> Object ID: | enterprises.8164.2.44

> Description: | The Authentication, Authorization and Accounting (AAA) server has been misconfigured. This server is not usable until this condition is repaired. Action to be Taken: Examine the system configuration and correct the misconfiguration. See the user documentation for details on AAA configuration. Clear Condition: Verify that communication to the AAA authentication server has been restored. Condition Clear Alarm: When this condition clears a starAAAAccServerReachable notification will be generated.

> Objects: | radiusAccServerIndex radiusAccServerAddress

> Object: | starLogMsg

> Object ID: | enterprises.8164.2.45

> Description: | A log message. This trap is used only for debugging.

> Objects: | starLogText

> Object: | starPDSNServiceStart

> Object ID: | enterprises.8164.2.46

> Description: | A PDSN service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starPDSNServiceStop

> Object ID: | enterprises.8164.2.47

> Description: | A PDSN service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the PDSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the PDSN service is operational. Condition Clear Alarm: A starPDSNServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starHAServiceStart

> Object ID: | enterprises.8164.2.48

> Description: | An HA service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starHAServiceStop

> Object ID: | enterprises.8164.2.49

> Description: | An HA service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the PDSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the PDSN service is operational. Condition Clear Alarm: A starHAServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starFAServiceStart

> Object ID: | enterprises.8164.2.50

> Description: | An FA service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starFAServiceStop

> Object ID: | enterprises.8164.2.51

> Description: | An FA service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the FA service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the FA service is operational. Condition Clear Alarm: A starFAServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starCLISessionStart

> Object ID: | enterprises.8164.2.52

> Description: | An interactive CLI session has started. Condition Clear Alarm: A starCLISessionEnd notification will be sent when the CLI session is terminated.

> Objects: | starCLIUsername starCLIPrivs starCLITtyname

> Object: | starCLISessionEnd

> Object ID: | enterprises.8164.2.53

> Description: | An interactive CLI session has ended. The CLI session may have been terminated by the CLI user; the session may have expired due to an idle timeout, or a session timeout; or the session may have been terminated by operator intervention.

> Objects: | starCLIUsername starCLIPrivs starCLITtyname

> Object: | starCritTaskFailed

> Object ID: | enterprises.8164.2.54

> Description: | A critical task has failed and the appropriate recovery steps begun. The card containing the failed task will be restarted; migration/recovery operations will proceed. Probable Cause: Software error. Actions to be Taken: Examine the admin logs for an indication of the source of the failure. Clear Condition: Verify that an SPC/SMC switchover or PAC migration completes to recover from this condition. Condition Clear Alarm: A starCardUp will be generated when the card has successfully restarted.

> Objects: | starTaskFacilityName starTaskInstance starTaskCard starTaskCPU

> Object: | starCardActive

> Object ID: | enterprises.8164.2.55

> Description: | The card is now active.

> Objects: | starSlotNum starCardType

> Object: | starLACServiceStart

> Object ID: | enterprises.8164.2.56

> Description: | A LAC service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starLACServiceStop

> Object ID: | enterprises.8164.2.57

> Description: | A LAC service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the LAC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the LAC service is operational. Condition Clear Alarm: A starLACServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starLNSServiceStart

> Object ID: | enterprises.8164.2.58

> Description: | A LNS service has started. Action to be Taken: No Action Required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starLNSServiceStop

> Object ID: | enterprises.8164.2.59

> Description: | A LNS service has stopped. Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the LNS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the LNS service is operational. Condition Clear Alarm: A starLNSServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starCardDown

> Object ID: | enterprises.8164.2.60

> Description: | The card is now down. Probable Cause: The card was shut down by an operator; the card was removed by an operator; or a hardware or software fault caused the card to shut down. In the latter case an additional notification is generated with the specific failure. Action to be Taken: If the card shutdown was not planned, verify that the card is present in the system and its card lock is in the locked position. Check the admin logs for the cause of the card shutdown. Clear Condition: Verify that an SPC switchover/card migration completes to recover from the card shutdown. Condition Clear Alarm: A starCardUp notification is generated when the card is restarted.

> Objects: | starSlotNum starCardType

> Object: | dsx3LineStatusChange

> Object ID: | enterprises.8164.2.61

> Description: | As defined by RFC2496, this trap (mib-2.10.30.15.0 1) is sent when there is a change in the value of an dsx3LineStatus instance. If the line status change is the result of a line status change at a lower level (i.e. ds1), then no traps for the ds3 are sent.

> Objects: | dsx3LineStatus dsx3LineStatusLastChange

> Object: | dsx1LineStatusChange

> Object ID: | enterprises.8164.2.62

> Description: | As defined by RFC2496, this trap (mib-2.10.18.15.0 1) is sent when there is a change in the value of an dsx1LineStatus instance. If the line status change is the result of a line status change at a higher level (i.e. ds3), then no traps for the ds1 are sent.

> Objects: | dsx1LineStatus dsx1LineStatusLastChange

> Object: | starGGSNServiceStart

> Object ID: | enterprises.8164.2.63

> Description: | A GGSN Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starGGSNServiceStop

> Object ID: | enterprises.8164.2.64

> Description: | A GGSN Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the GGSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the GGSN service is operational. Condition Clear Alarm: A starGGSNServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starLicenseExceeded

> Object ID: | enterprises.8164.2.65

> Description: | The licenses session limit has been exceeded; note that a small number of sessions are permitted beyond the licensed limit. Probable Cause: The usage of the system has exceeded the capacity of the license installed; The license installed does not match the identification of the system; No license is installed. Action to be Taken: Verify that the proper license is installed on the system; verify that the SPCs present in the system match those identified in the software license. If required, install an additional higher-capacity license. Clear Condition: This condition is cleared when usage goes under the licensed limit. Condition Clear Alarm: This condition is cleared by a starLicenseUnderLimit notification.

> Objects: | starLicensedSessions starCurrentSessions starServiceType

> Object: | starSubscriberLimit

> Object ID: | enterprises.8164.2.66

> Description: | The specified service has reached its configured limit for number of subscribers. Action to be Taken: Verify that the configured subscriber limit is correct. Configure additional services, or configure the existing service to permit a larger number of subscribers.

> Objects: | starServiceVpnName starServiceServName starServiceSubLimit starServiceSubCurrent starServiceType

> Object: | starSessionRejectNoResource

> Object ID: | enterprises.8164.2.67

> Description: | A session setup was rejected because of a lack of available resources. Probable Cause: The system has reached its maximum capacity based on the number of available PACs/PSCs/CPUs/memory. Actions to be Taken: Examine the system CPU table to determine if there is abnormal system usage or if the system is reaching its capacity. If this condition persists, additional PACs/PSCs or PAC/PSC memory may be required. Note that there is a configuration threshold which can be setup to monitor the number of NORESOURCE rejects.

> Objects: | starServiceVpnID starServiceType

> Object: | starLongDurTimerExpiry

> Object ID: | enterprises.8164.2.68

> Description: | The long duration timer has expired for the identified subscriber. Action to be Taken: No action is typically required. If an abnormal number of expiries occur, verify that the configuration expiry time is correct.

> Objects: | starSubContext starSubMSID starSubName starSubTimerDuration starSubLongDurTimeoutAction starSubSetupTime starSubHomeAddr starSubHomeAddrv6

> Object: | starClosedRPServiceStart

> Object ID: | enterprises.8164.2.69

> Description: | Closed RP Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starClosedRPServiceStop

> Object ID: | enterprises.8164.2.70

> Description: | Closed RP Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the Closed RP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the Closed RP service is operational. Condition Clear Alarm: A starClosedRPServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starGtpcPathFailure

> Object ID: | enterprises.8164.2.71

> Description: | GTP Control Path Failure.

> Objects: | starSessGGSNVpnName starSessGGSNServName starSessGGSNPeerAddr

> Object: | starGtpuPathFailure

> Object ID: | enterprises.8164.2.72

> Description: | GTP Data Path Failure.

> Objects: | starSessGGSNVpnName starSessGGSNServName starSessGGSNPeerAddr

> Object: | starManagerFailure

> Object ID: | enterprises.8164.2.73

> Description: | Software manager Failure. Probable Cause: A software failure. The failing manager will be restarted. Action to be Taken: Examine the admin and crash logs for more information about the failure.

> Objects: | starTaskFacilityName starTaskInstance starTaskCard starTaskCPU

> Object: | starEISServerAlive

> Object ID: | enterprises.8164.2.74

> Description: | EIS Server alive.

> Objects: | starEISServerVPNID starEISServerAddr

> Object: | starEISServerDead

> Object ID: | enterprises.8164.2.75

> Description: | EIS Server down. Probable Cause: The remote EIS server is down or there is a network error making it unreachable. Condition Clear Alarm: A starEISServerAlive notification will be generated when this condition is cleared

> Objects: | starEISServerVPNID starEISServerAddr

> Object: | starCgfAlive

> Object ID: | enterprises.8164.2.76

> Description: | GTPP CGF Server Alive.

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starCgfDead

> Object ID: | enterprises.8164.2.77

> Description: | GTPP CGF Server Dead. Probable Cause: The remote CGF server is down or there is a network error making it unreachable. Action to be Taken: Verify that the CGF server is functioning properly; verify network connectivity to the CGF server. Clear Condition: This condition is cleared when the CGF server becomes reachable. Condition Clear Alarm: A starCgfServerAlive notification will be generated when this condition is cleared

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starStorageServerAlive

> Object ID: | enterprises.8164.2.78

> Description: | GTPP Storage Server is Alive.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr

> Object: | starStorageServerDead

> Object ID: | enterprises.8164.2.79

> Description: | GTPP Storage Server is Dead. Probable Cause: The remote storage server is down. There is a network error making it unreachable. Action to be Taken: Verify that the storage server is functioning properly; verify network connectivity to the storage server. Clear Condition: This condition is cleared when the Storage server becomes reachable. Condition Clear Alarm: A starStorageServerAlive notification is generated when this condition is cleared.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr

> Object: | starGgsnInitiatedUpdtFailed

> Object ID: | enterprises.8164.2.80

> Description: | GGSN Initiated Update PDP Context Response Failed. Probable Cause: This can happen if there is an inter-SGSN handoff and the new SGSN is not listed in GGSN service and its PLMN policy is set to reject unknown SGSNs. Action to be Taken: List the SGSN address in the GGSN service. Condition Clear Alarm: N/A

> Objects: | starSessGGSNVpnName starSessGGSNServName starSessGGSNSubsName starSessGGSNAPNName starSessGGSNImsi starSessGGSNPeerAddr

> Object: | starCongestion

> Object ID: | enterprises.8164.2.81

> Description: | A congestion condition has occurred. Probable Cause: This is the result of an operator-configured congestion threshold being reached. This can be due to high usage of the resource being monitored which indicates that the system is reaching its peak capacity, or could be caused by the incorrect configuration of the congestion thresholds. Actions to be Taken: Verify that the congestion thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online. Clear Condition: This system is cleared when the use of the specific resource falls below the configured limit. Condition Clear Alarm: A starCongestionClear notification is sent when there are no congestion conditions for a service type

> Objects: | starServiceType starCongestionPolicy starCongestionResourceType

> Object: | starCongestionClear

> Object ID: | enterprises.8164.2.82

> Description: | A congestion condition has cleared.

> Objects: | starServiceType

> Object: | starServiceLossPTACs

> Object ID: | enterprises.8164.2.83

> Description: | A service loss condition has occurred due to PAC/PSC/TAC failure or removal. Probable cause: Multiple PAC/PSC/TAC cards are no longer available, due to failure, removal, or operator action -- or configuration changes have been made which eliminated the availability of redundant cards. Action to be Taken: Bring additional PAC/PSC/TAC cards online to match the number of configured cards, or update the configuration to require fewer active PAC/PSC/TAC cards. Clear Condition: This condition is cleared when the number of active PAC/PSC/TAC cards reaches or exceeds the configured number.

> Objects: | starCardMode starPTACConfig starPTACActive

> Object: | starServiceLossLC

> Object ID: | enterprises.8164.2.84

> Description: | A service loss condition has occurred due to LC failure or removal. Probable Cause: Multiple Line Cards (LCs) are no longer available, due to failure, removal, or operator action. Action to be Taken: Bring additional LCs online to match the number of configured cards, or update the configuration to require fewer active LCs. Clear Condition: This condition is cleared when the number of active line cards reaches or exceeds the configured number.

> Objects: | starCardType starSlotNum starSlotNum

> Object: | starServiceLossSPIO

> Object ID: | enterprises.8164.2.85

> Description: | A service loss condition has occurred due to SPIO failure or removal. Since the SPIO contains the ports used for SNMP access, this notification cannot normally be delivered as an SNMP trap. The notification will be logged and stored in the historical trap list, and if the system is configured to send INFORM PDUs the notification might be delivered at a later time. Probable Cause: Both SPIOs are no longer available, due to failure, removal, or operator action. Action to be Taken: Bring at least one SPIO online. Clear Condition: This condition is cleared when a SPIO is made active

> Object: | starIPSPAllAddrsFree

> Object ID: | enterprises.8164.2.86

> Description: | All IP addresses are now free on the IP Pool Sharing Protocol (IPSP) primary HA. Probable Cause: IP Pool Sharing Protocol (IPSP) is running between two HAs (a primary and a secondary). The primary HA has now released the last address that was in use. This presumably is done in preparation for taking the primary HA out of server. Action to be Taken: Perform the desired maintenance on the primary HA that required taking the device out of service.

> Objects: | starContextName starInterfaceName

> Object: | starPCFUnreachable

> Object ID: | enterprises.8164.2.87

> Description: | A PCF that the system communicates with is no longer reachable. Probable Cause: The PCF has failed or is otherwise unavailable, or a network connectivity problem makes it unreachable. Action to be Taken: If the PCF outage was unplanned, restart/reset the PCF; verify network connectivity

> Objects: | starContextName starPCFAddress

> Object: | starDhcpAlive

> Object ID: | enterprises.8164.2.88

> Description: | DHCP Server Alive.

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starDhcpDead

> Object ID: | enterprises.8164.2.89

> Description: | DHCP Server Dead. Probable Cause: The remote DHCP server is down or there is a network error making it unreachable. Action to be Taken: Verify that the DHCP server is functioning properly; verify network connectivity to the DHCP server. Clear Condition: The condition is cleared when the DHCP server becomes reachable, or if the configuration is changes to not use this server. Condition Clear Alarm: A starDhcpAlive notification is generated when the server becomes reachable.

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starNTPPeerUnreachable

> Object ID: | enterprises.8164.2.90

> Description: | NTP Peer Unreachable. Probable Cause: The NTP server is down or unavailable, or there is a network connectivity issue that prevents access to the NTP server. Action to be Taken: Action to be Taken: Verify that the NTP server is running properly; verify that the connection to the NTP server is functioning. Clear Condition: This condition is cleared when the NTP server becomes reachable. Condition Clear Alarm: This condition is cleared by a starNTPPeerReachable notification.

> Objects: | starPeerAddress

> Object: | starNTPSyncLost

> Object ID: | enterprises.8164.2.91

> Description: | NTP Synchronization Lost. Probable Cause: All configured NTP server are no longer available, or some/all NTP servers have been un-configured by an operator. Action to be Taken: Action to be Taken: Verify that the NTP server(s) are running properly and that the network connections to the NTP servers are available. Check the configured of the NTP servers for correctness. If needed, configure additional NTP servers. Clear Condition: This condition is cleared when any (one) NTP server becomes reachable. Condition Clear Alarm: This condition is cleared by a starNTPSyncEstablished notification.

> Object: | starL2TPTunnelDownPeerUnreachable

> Object ID: | enterprises.8164.2.92

> Description: | L2TP tunnel down due to peer unreachable. Probable Cause: Misconfiguration of the peer router address or inability to route to the peer. Action to be Taken: Verify the peer address is correct; verify that the peer is operational; verify network connectivity to the peer.

> Objects: | starL2TPLocalTunnelID starL2TPPeerTunnelID starL2TPContextName starL2TPServiceName starL2TPServiceTypeName starL2TPLocalAddress starL2TPPeerAddress

> Object: | starCardStandby

> Object ID: | enterprises.8164.2.93

> Description: | The card is now standby.

> Objects: | starSlotNum starCardType

> Object: | starLicenseUnderLimit

> Object ID: | enterprises.8164.2.94

> Description: | Usage is now under the licensed session limit.

> Objects: | starLicensedSessions starCurrentSessions starServiceType

> Object: | starIPSECPriTunDown

> Object ID: | enterprises.8164.2.95

> Description: | IPSEC Primary Tunnel Down

> Objects: | starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr

> Object: | starIPSECPriTunUp

> Object ID: | enterprises.8164.2.96

> Description: | IPSEC Primary Tunnel Up

> Objects: | starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr

> Object: | starIPSECSecTunDown

> Object ID: | enterprises.8164.2.97

> Description: | IPSEC Secondary Tunnel Down

> Objects: | starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr

> Object: | starIPSECSecTunUp

> Object ID: | enterprises.8164.2.98

> Description: | IPSEC Secondary Tunnel Up

> Objects: | starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr

> Object Group: | starIPSECTunSwitchFail

> Object ID: | enterprises.8164.2.99

> Description: | IPSEC Tunnel Switchover failed or unable to be attempted

> Objects: | starIPSECContextName starIPSECGroupName

> Object: | starIPSECTunSwitchComplete

> Object ID: | enterprises.8164.2.100

> Description: | IPSEC Tunnel Switchover complete

> Objects: | starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr

> Object: | starNwReachServerAlive

> Object ID: | enterprises.8164.2.101

> Description: | Nw Reachable Server alive

> Objects: | starNwReachName starNwReachSrvrAddr

> Object: | starNwReachServerDead

> Object ID: | enterprises.8164.2.102

> Description: | Nw Reachable Server Dead. Probable Cause: The remote server is down or there is a network error making it unreachable. A starNwReachServerAlive notification will be generated when this condition is cleared

> Objects: | starNwReachName starNwReachSrvrAddr

> Object: | starStorageServerUnackedGcdrVolPurge

> Object ID: | enterprises.8164.2.103

> Description: | GTPP storage server has performed un-acked GCDRs volume purge. Probable Cause: GTPP storage server has purged un-acked GCDRs after hitting the max allowed configured limit on un-acked GCDR in the backup database. Action to be Taken: Check for the unacked file generated for these GCDRs. Clear Condition: There is no clear condition for this notification. Condition Clear Alarm: There is no clear alarm for this notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr

> Object: | starStorageServerUnackedGcdrFileGen

> Object ID: | enterprises.8164.2.104

> Description: | GTPP storage server has exported the unacked GCDRs to file from backup db. Probable Cause: GTPP storage server has generated and saved all the unacked GCDRs to file. Action to be Taken: Operator needs to FTP the generated file. Clear Condition: There is no clear condition for this notification. Condition Clear Alarm: There is no clear alarm for this notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr

> Object: | starNTPPeerReachable

> Object ID: | enterprises.8164.2.105

> Description: | NTP Peer Reachable. Probable Cause: The NTP server is reachable. This could indicate a newly configured NTP server (including an initial configuration on system startup) or could indicate a previously unreachable server has become reachable. Action to be Taken: No action required.

> Objects: | starPeerAddress

> Object: | starNTPSyncEstablished

> Object ID: | enterprises.8164.2.106

> Description: | NTP Synchronization Established. Probable Cause: An NTP server is available when previously no server was available. This could indicate a newly configured NTP server (including an initial configuration on system startup) or could indicate that one or more previously unreachable server(s) has become reachable. Action to be Taken: No action required.

> Object: | starSIPServiceStart

> Object ID: | enterprises.8164.2.107

> Description: | A SIP service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starSIPServiceStop

> Object ID: | enterprises.8164.2.108

> Description: | A SIP service has stopped Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starVIMServiceStart

> Object ID: | enterprises.8164.2.109

> Description: | A VIM service has started Action to be taken: No action required

> Syntax: | starServiceVpnName starServiceServName

> Object: | starVIMServiceStop

> Object ID: | enterprises.8164.2.110

> Description: | A VIM service has stopped. This is because of application out-of-service or if vim is down or no app. server Action to be taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starCHATCONFServiceStart

> Object ID: | enterprises.8164.2.111

> Description: | A CHAT/CONF service has started Action to be taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starCHATCONFServiceStop

> Object ID: | enterprises.8164.2.112

> Description: | A CHAT/CONF service has stopped. This is because of application out-of-service or if chatconf is down or no app. server Action to be taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starSIPRouteNomatch

> Object ID: | enterprises.8164.2.113

> Description: | SIP session has failed since there is no match in the routing table with matching prefix Action to be taken: Operator has to configure with matching prefix if required

> Objects: | starSIPRouteVpnName starSIPRouteVmgName starSIPRouteAsName starSIPRouteDestPartyNum starSIPRouteReqNum

> Object: | starL3AddrUnreachable

> Object ID: | enterprises.8164.2.114

> Description: | A L3 Address is unreachable through the specific slot and port. Action to be taken: No action required

> Objects: | starL3Address starPortSlot starPortNum

> Object: | starSWUpgradeStart

> Object ID: | enterprises.8164.2.115

> Description: | An operator has begun to upgrade the software on the ST-16.

> Object: | starSWUpgradeComplete

> Object ID: | enterprises.8164.2.116

> Description: | An operator-initiated software upgrade has been completed.

> Object: | starSWUpgradeAborted

> Object ID: | enterprises.8164.2.117

> Description: | An operator-initiated software upgrade has been aborted.

> Object: | starBGPPeerSessionUp

> Object ID: | enterprises.8164.2.118

> Description: | The BGP peer session to the specified IP address is operational. This may indicate the initial configuration of a new peer, the initial connectivity after a system restart, or the restoration of connectivity after a starBGNPeerSessionDown event. Action to be Taken: No action required.

> Objects: | starContextName starBGPPeerIPAddress

> Object: | starBGPPeerSessionDown

> Object ID: | enterprises.8164.2.119

> Description: | The BGP peer session to the specified IP address is no longer operational. Probable Cause: The BGP peer is not-operational; the network between the ST-16 and the BGP peer is experiencing an outage; LC failure(s) on the ST-16. Action to be Taken: Verify the BGP peer is operational; verify network connectivity to the BGP peer. Clear Condition Alarm: A starBGPPeerSessionUp is generated when connectivity is reestablished

> Objects: | starContextName starBGPPeerIPAddress

> Object: | starSRPActive

> Object ID: | enterprises.8164.2.120

> Description: | The SRP Chassis Status is now Active. Action to be Taken: No action is required.

> Objects: | starContextName starSRPIPAddress

> Object: | starSRPStandby

> Object ID: | enterprises.8164.2.121

> Description: | The SRP Chassis Status is now Standby. Action to be Taken: No action is required.

> Objects: | starContextName starSRPIPAddress

> Object: | starBGPPeerReachable

> Object ID: | enterprises.8164.2.122

> Description: | The monitored BGP peer is now Reachable. This notification can represent the initial detection of the peer's state, or the re-connection to a peer after a starBGPPeerDown notification. Action to be Taken: No action is required.

> Objects: | starContextName starSRPIPAddress starUDPPortNum starBGPPeerIPAddress

> Object: | starBGPPeerUnreachable

> Object ID: | enterprises.8164.2.123

> Description: | The monitored BGP peer is now Unreachable. Action to be Taken: Verify that the BGP Peer is running and is properly configured. Verify the network link to the BGP Peer. Clear Condition: This condition is cleared when communication with the BGP peer is reestablished. Condition Clear Alarm: This condition is cleared by a starBGPPeerReachable notification.

> Objects: | starContextName starSRPIPAddress starUDPPortNum starBGPPeerIPAddress

> Object: | starSRPAAAReachable

> Object ID: | enterprises.8164.2.124

> Description: | The SRP AAA monitor has found a reachable AAA server. This notification can represent the initial detection of an AAA server, or the restoration of reachability after a starSRPAAAUnreachable notification. This notification is only generated if there was previously no reachable AAA server. Action to be Taken: No action required.

> Objects: | starContextName starSRPIPAddress starUDPPortNum

> Object: | starSRPAAAUnreachable

> Object ID: | enterprises.8164.2.125

> Description: | The SRP AAA monitor has determined that all AAA servers are unreachable. Action to be Taken: Verify the state of the configured AAA server(s) and restart them if required. Verify the network link to the AAA Server(s). Configure additional AAA servers if required. Clear Condition: This condition is cleared when communication with any single AAA service is (re)established. Condition Clear Alarm: This condition is cleared by a starSRPAAAReachable notification.

> Objects: | starContextName starSRPIPAddress starUDPPortNum

> Object: | starHASwitchoverInitiated

> Object ID: | enterprises.8164.2.126

> Description: | An HA Switchover operation has been initiated by an operator. Action to be Taken: Verify that the switchover was a planned operator action.

> Objects: | starContextName starSRPIPAddress

> Object: | starSRPCheckpointFailure

> Object ID: | enterprises.8164.2.127

> Description: | The system has detected that a checkpoint messaged failed to be sent successfully to the standby HA. If the active HA were to fail, this information will be lost. Action to be Taken: Verify the communication path to the Standby HA.

> Objects: | starContextName starSRPIPAddress

> Object: | starSRPConfigOutOfSync

> Object ID: | enterprises.8164.2.128

> Description: | The system has detected that the standby HA has a different configuration than the active HA. In the event of a failure of the active HA, it is possible that the standby HA is not configured properly to be able to take over. Action to be Taken: Update the configuration of the standby HA to match the active HA. Clear Condition: This condition is cleared when the active HA confirms that the standby HA has an identify configuration. Condition Clear Alarm: This condition is cleared by a starSRPConfigInSync notification.

> Objects: | starContextName starSRPIPAddress

> Object: | starSRPConfigInSync

> Object ID: | enterprises.8164.2.129

> Description: | The system has detected that the standby HA has a matching configuration as the active HA. This notification is generated only after a starSRPConfigOutOfSync notification. Action to be Taken: No action required.

> Objects: | starContextName starSRPIPAddress

> Object: | starGESwitchFailure

> Object ID: | enterprises.8164.2.130

> Description: | A failure of an internal Gigabit Ethernet switch has been detected. If it is possible to determine the slow containing the failed switch it is identified in starSlotNum, otherwise starSlotNum is 0. Action to be Taken: If this condition persists, the identified card needs to be replaced.

> Objects: | starSlotNum

> Object: | starSIPRouteServerAvailable

> Object ID: | enterprises.8164.2.131

> Description: | SIP route server is available. Action to be Taken: No action required.

> Objects: | starSIPRouteServerVpnName starSIPRouteServerVmgName starSIPRouteServerAsName starSIPRouteServerIpAddr

> Object: | starSIPRouteServerUnavailable

> Object ID: | enterprises.8164.2.132

> Description: | SIPsession has failed since the route server is unavailable. Action to be Taken: Operator has to check the reason for the unavailability of the server an act accordingly.

> Objects: | starSIPRouteServerVpnName starSIPRouteServerVmgName starSIPRouteServerAsName starSIPRouteServerIpAddr

> Object: | starFMDMaxCallRateReached

> Object ID: | enterprises.8164.2.133

> Description: | FMD max call rate reached Action to be Taken: Increase the value of fmd-max-call-rate or set no fmd-max-call-rate. Condition Clear Alarm: This condition is cleared by a starFMDCallRateUnderControl notification

> Objects: | starVIMServiceVpnName starVIMServiceInstanceId starVIMServiceFMDMaxCallRate starVIMServiceFMDContinuousLoadCount

> Object: | starFMDCallRateUnderControl

> Object ID: | enterprises.8164.2.134

> Description: | FMD call rate is under control. Action to be Taken: No action required.

> Objects: | starVIMServiceVpnName starVIMServiceInstanceId starVIMServiceFMDMaxCallRate starVIMServiceFMDContinuousLoadCount

> Object: | starStorageServerCPUBusy

> Object ID: | enterprises.8164.2.135

> Notifications: | GTPP Storage Server is experiencing high CPU usage. The usage has exceeded an operator-configure value.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Description: | Probable Cause: The amount of information being sent to the Storage Server is approaching the server's capacity; the Storage Server has other tasks running on it which are taking CPU time; a problem with the Storage Server is causing the CPU to be abnormally busy Condition Clear Alarm: This condition is cleared by a starStorageServerCPUNormal notification

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshPct starThreshMeasuredPct starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerCPUNormal

> Object ID: | enterprises.8164.2.136

> Description: | GTPP Storage Server CPU usage has returned to a normal range.

> IMPORTANT: Note that this is an external server, not part of the chassis.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshPct starThreshMeasuredPct starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerDiskSpaceLow

> Object ID: | enterprises.8164.2.137

> Description: | GTPP Storage Server is experiencing low available disk space. The available disk space has gone below an operator-configure value.

> IMPORTANT: Note that this is an external server, not part of the chassis.

> Description: | Probable Cause: This can be caused by an improper configuration, or by the failure or removal of other cards in the system. Condition Clear Alarm: This condition is cleared by a starStorageServerDiskSpaceOK notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshGB starThreshMeasuredGB starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerDiskSpaceOK

> Object ID: | enterprises.8164.2.138

> Description: | Available disk space for GTPP Storage Server is now in a normal range.

> IMPORTANT: Note that this is an external server, not part of the chassis.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshPct starThreshMeasuredPct starGSSClusterName starGSSClusterNodeName

> Object: | starCardSPOFAlarm

> Object ID: | enterprises.8164.2.139

> Description: | The identified card is a Single Point of Failure (SPOF). There is no redundant card available to take over in the event of a failure. Probable Cause: This can be caused by an improper configuration, or by the failure or removal of other cards in the system. Action to be Taken: Install or configure additional redundant cards. Condition Clear Alarm: A starCardSPOFClear notification will be generated is a redundant card becomes available. Notifications like starCardDown could also obsolete this notification.

> Objects: | starSlotNum starCardType

> Object: | starCardSPOFClear

> Object ID: | enterprises.8164.2.140

> Description: | The identified card is no longer a Single Point of Failure (SPOF).

> Objects: | starSlotNum starCardType

> Object: | starStorageServerOldGcdrPending

> Object ID: | enterprises.8164.2.141

> Description: | GCDR files on the Storage Server have been unprocessed since the configured threshold value of time period.

> IMPORTANT: Note that this is an external server, not part of the ST-16.

> Description: | Probable Cause: No action has been taken long for the GCDR files generated by Storage Server. Condition Clear Alarm: This condition is cleared by a starStorageServerOldGcdrCleared notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshInt starThreshMeasuredInt starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerOldGcdrCleared

> Object ID: | enterprises.8164.2.142

> Description: | GCDR files on the Storage Server have been processed on the Storage Server. The threshold condition is now clear.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshInt starGSSClusterName starGSSClusterNodeName

> Object: | starLoginFailure

> Object ID: | enterprises.8164.2.143

> Description: | A login failure occurred attempting to establish a CLI or FTP session.

> Objects: | starCLITtyname starCLIRemoteIPAddr starCLIType

> Object Group: | starIPSGServiceStart

> Object ID: | enterprises.8164.2.144

> Description: | A IP Services Gateway (IPSG) Service has started.

> Objects: | starServiceVpnName starServiceServName

> Object: | starIPSGServiceStop

> Object ID: | enterprises.8164.2.145

> Description: | A IP Services Gateway (IPSG) Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the IPSG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the IPSG service is operational. Condition Clear Alarm: A starIPSGServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starHAUnreachable

> Object ID: | enterprises.8164.2.146

> Description: | A monitored HA is unreachable from the identified FA Service. Condition Clear Alarm: A starHAReachable notification will be generated when the HA becomes reachable

> Objects: | starServiceVPNName starServiceServName starServiceFAIpAddr starServiceHAIpAddr

> Object: | starHAReachable

> Object ID: | enterprises.8164.2.147

> Description: | A monitored HA is now reachable. A starHAReachable notification is only generated for monitored HA's which previously were marked unreachable.

> Objects: | starServiceVPNName starServiceServName starServiceFAIpAddr starServiceHAIpAddr

> Object: | starASNGWServiceStart

> Object ID: | enterprises.8164.2.148

> Description: | A WiMAX ASN Gateway (ASNGW) Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starASNGWServiceStop

> Object ID: | enterprises.8164.2.149

> Description: | A WiMAX ASN Gateway (ASNGW) Service has stopped. Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the ASNGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the ASNGW service is operational. Condition Clear Alarm: A starASNGWServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starTaskFailed

> Object ID: | enterprises.8164.2.150

> Description: | A non-critical task has failed and the appropriate recovery steps begun. The failing task will be restarted. Probable Cause: Software error. Actions to be Taken: Examine the admin logs for an indication of the source of the failure. Clear Condition: Verify that the task has been restarted. Condition Clear Alarm: A starTaskRestart notification will be generated when task has successfully restarted.

> Objects: | starTaskFacilityName starTaskInstance starTaskCard starTaskCPU

> Object: | starTaskRestart

> Object ID: | enterprises.8164.2.151

> Description: | A non-critical task has restarted after an earlier failure. Actions to be Taken: None.

> Objects: | starTaskFacilityName starTaskInstance starTaskCard starTaskCPU

> Object: | starCSCFServiceStart

> Object ID: | enterprises.8164.2.152

> Description: | A CSCF Service has started Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starCSCFServiceStop

> Object ID: | enterprises.8164.2.153

> Description: | A CSCF Service has stopped. Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the CSCF service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the CSCF service is operational. Condition Clear Alarm: A starCSCFServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starDhcpServiceStarted

> Object ID: | enterprises.8164.2.154

> Description: | A DHCP Service has started. Action to be Taken: No action required.

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starDhcpServiceStopped

> Object ID: | enterprises.8164.2.155

> Description: | A DHCP Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the DHCP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the DHCP service is operational. Condition Clear Alarm: A starDHCPServiceStart notification will be generated when the service is restarted.

> Objects: | starSessGGSNVpnName starSessGGSNPeerPort starSessGGSNPeerAddr

> Object: | starContFiltDBError

> Object ID: | enterprises.8164.2.156

> Description: | The Content Filtering OPTCMDB file error displayed with an error code. Action to be Taken: If no OPTCMDB file is there in the specified directory then Place a OPTCMDB-FULL file in the directory and give an upgrade command. If the error is related to merge/loading failure then give an upgrade command with a new inc/full database file. Condition Clear Alarm: This condition is cleared by a starContFiltDBErrorClear notification.

> Objects: | starContFiltCFFilename starContFiltCFErrorCode

> Object: | starContFiltDBErrorClear

> Object ID: | enterprises.8164.2.157

> Description: | The Content Filtering OPTCMDB file error removed. Action to be Taken: No action required.

> Objects: | starContFiltCFFilename starContFiltCFErrorCode

> Object: | starBLDBError

> Object ID: | enterprises.8164.2.158

> Description: | The Blacklisting OPTBLDB file error displayed with an error code Action to be Taken: If no or invalid OPTBLDB file is there in the specified directory then Place a OPTBLDB_FULL file in the directory and give an upgrade command Condition Clear Alarm: This condition is cleared by a starBLDBErrorClear notification

> Objects: | starBLFilename starBLErrorCode

> Object: | starBLDBErrorClear

> Object ID: | enterprises.8164.2.159

> Description: | The Blacklisting OPTBLDB file error removed Action to be Taken: No action required

> Objects: | starBLFilename starBLErrorCode

> Object: | starContFiltDBUpgradeError

> Object ID: | enterprises.8164.2.160

> Description: | The Content Filtering OPTCMDB file error displayed with an error code Action to be Taken: Place a valid OPTCMDB-FULL file or OPTCMDB_INCR file in the directory and give an upgrade command Condition Clear Alarm: This condition is cleared by a starContFiltDBUpgradeErrorClear notification

> Objects: | starContFiltCFUpgradeFilename starContFiltCFUpgradeErrorCode

> Object: | starContFiltDBUpgradeErrorClear

> Object ID: | enterprises.8164.2.161

> Description: | The Content Filtering OPTCMDB file error removed Action to be Taken: No action required

> Objects: | starContFiltCFUpgradeFilename starContFiltCFUpgradeErrorCode

> Object: | starBLDBUpgradeError

> Object ID: | enterprises.8164.2.162

> Description: | The Blacklisting OPTBLDB file error displayed with an error code Action to be Taken: Place a valid OPTBLDB-FULL file file in the directory and give an upgrade command Condition Clear Alarm: This condition is cleared by a starBLDBUpgradeErrorClear

> Objects: | starBLUpgradeFilename starBLUpgradeErrorCode

> Object: | starBLDBUpgradeErrorClear

> Object ID: | enterprises.8164.2.163

> Description: | The Blacklisting OPTBLDB file error removed Action to be Taken: No action required

> Objects: | starBLUpgradeFilename starBLUpgradeErrorCode

> Object: | starIPSECDynTunUp

> Object ID: | enterprises.8164.2.164

> Description: | IPSEC Dynamic Tunnel Up. Action to be Taken: No action required.

> Objects: | starIPSECContextName starIPSECPolicyName starIPSECDynPolicyType starIPSECPolicyPayloadType starIPSECLocalGateway starIPSECRemoteGateway

> Object: | starIPSECDynTunDown

> Object ID: | enterprises.8164.2.165

> Description: | IPSEC Dynamic Tunnel Down.

> Objects: | starIPSECContextName starIPSECPolicyName starIPSECDynPolicyType starIPSECDynPolicyPayloadType starIPSECLocalGateway starIPSECRemoteGateway

> Object: | starHeartbeat

> Object ID: | enterprises.8164.2.166

> Description: | Periodic SNMP heartbeat. A starHeartbeat notification can be generated periodically if the system is configured to do so. These notifications serve only to validate that there is communication to external entities which sink SNMP notifications

> Object: | starOverloadSystem

> Object ID: | enterprises.8164.2.167

> Description: | A system-wide congestion overload condition has occurred. Probable Cause: This is the result of an operator-configured congestion overload value reached. This notification indicated a chassis-wide overload condition, typically overall system usage reaching some fraction of capacity. Once this limit is reached, the configured behavior is taken. This will cause certain older and/or dormant calls to be dropped in favor of newer calls. Note that this is similar to, but different than, the starCongestion notification. Typically the 'overload' condition will be configured to trigger at an earlier point. Actions to be Taken: Verify that the congestion overload thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online. Clear Condition: This system is cleared when the use of the specific resource falls below the configured limit. Condition Clear Alarm: A starOverloadSystemClear notification is sent when the system overload condition is clear

> Objects: | starCongestionResourceType

> Object: | starOverloadSystemClear

> Object ID: | enterprises.8164.2.168

> Description: | A system-wide congestion overload condition has cleared

> Object: | starOverloadService

> Object ID: | enterprises.8164.2.169

> Description: | A service-specific congestion overload condition has occurred. Probable Cause: This is the result of an operator-configured congestion overload value reached. This notification indicated a service-specific overload condition, typically the use of the service reaching some fraction of capacity. Once this limit is reached, the configured behavior is taken. This will cause certain older and/or dormant calls to be dropped in favor of newer calls. Note that this is similar to, but different than, the starCongestion notification. Typically the 'overload' condition will be configured to trigger at an earlier point. Since this is a service-specific notification, it is possible to receive multiple notifications for different services. Each Action to be Taken: Verify that the congestion overload thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online. Clear Condition: This system is cleared when the use of the specific resource falls below the configured limit. Condition Clear Alarm: A starOverloadServiceClear notification is sent when the service-specific overload condition is clear.

> Objects: | starCongestionResourceType starServiceVpnName starServiceServName

> Object: | starOverloadServiceClear

> Object ID: | enterprises.8164.2.170

> Description: | A service-specific congestion overload condition has cleared

> Objects: | starServiceVpnName starServiceServName

> Object: | starStorageServerClusterStateChange

> Object ID: | enterprises.8164.2.171

> Description: | GTPP Storage Server cluster state has been changed. GTPP Storage Server may have gone offline from all the nodes or switchover has been occurred.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Description: | Probable Cause: GTPP Storage Server cluster hardware/software component failure or maintenance of GTPP Storage Server is in progress.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSClusterName starGSSClusterRgName starGSSClusterRsName starGSSClusterNodeState starGSSClusterPrevOnlineNode

> Object: | starStorageServerCluswitchOver

> Object ID: | enterprises.8164.2.172

> Description: | GTPP Storage Server switchover from current online node to next available node in cluster.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Description: | Probable Cause: GTPP storage server cluster hardware/software component failure or maintenance of GTPP storage server is in progress.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSClusterName starGSSClusterRgName starGSSClusterFromNode starGSSClusterToNode

> Object: | starStorageServerClusPathFail

> Object ID: | enterprises.8164.2.173

> Description: | GTPP Storage Server cluster disk path failure has been occurred.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Description: | Probable Cause: Fibre cable may have been damaged, fibre cable may have been pulled out or disk fault may have been occurred. Condition Clear Alarm: This condition is cleared by a starStorageServerClusPathOK notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSDiskPath starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerClusPathOK

> Object ID: | enterprises.8164.2.174

> Description: | GTPP Storage Server cluster disk path failure has been restored to ok state.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSDiskPath starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerClusInterCFail

> Object ID: | enterprises.8164.2.175

> Description: | GTPP Storage Server cluster transport path (Interconnect) failure has been occurred.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Description: | Probable Cause: Interconnect interface may have been failed, Interconnect interface cable may have been pulled out. Condition Clear Alarm: This condition is cleared by a starStorageServerClusInterCOK notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSTransportPath starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerClusInterCOK

> Object ID: | enterprises.8164.2.176

> Description: | GTPP Storage Server cluster transport path (Interconnect) failure has been restored to an operational state.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSTransportPath starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerClusIntfFail

> Object ID: | enterprises.8164.2.177

> Description: | GTPP Storage Server cluster disk path failure has been occurred.

> IMPORTANT: Note that this is an external server, not part of the ST-series hardware

> Description: | Probable Cause: Interface may have been failed, interface cable may have been pulled out. Condition Clear Alarm: This condition is cleared by a starStorageServerClusIntfOK notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSIPMPGroupName starGSSInterfaceName starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerClusIntfOK

> Object ID: | enterprises.8164.2.178

> Description: | GTPP Storage Server cluster GE Interface failure has been restored to ok state.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSIPMPGroupName starGSSInterfaceName starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerMemLow

> Object ID: | enterprises.8164.2.179

> Description: | GTPP Storage Server is experiencing a low memory condition.

> Description: | Probable Cause: The amount of free memory used by Storage Server is approaching the server's capacity. Condition Clear Alarm: This condition is cleared by a starStorageServerMemNormal notification.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshMB starThreshMeasuredMB starGSSClusterName starGSSClusterNodeName

> Object: | starStorageServerMemNormal

> Object ID: | enterprises.8164.2.180

> Description: | GTPP Storage Server Memory usage has returned to a normal range.

> IMPORTANT: Note that this is an external server, not part of the ST16.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starThreshMB starThreshMeasuredMB starGSSClusterName starGSSClusterNodeName

> Object: | starPDIFServiceStart

> Object ID: | enterprises.8164.2.181

> Description: | A PDIF Service has started. Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starPDIFServiceStop

> Object ID: | enterprises.8164.2.182

> Description: | A PDIF Service has stopped. Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs) to support the running configuration. Action to be Taken: If the PDIF service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the PDIF service is operational. Condition Clear Alarm: A starPDIFServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | -starSessMgrRecoveryComplete

> Object ID: | enterprises.8164.2.183

> Description: | The overall CPU utilization for the identified processor has exceeded for configured threshold value for the current monitoring period. Probable Cause: This is typically caused by session manager task fails and successfully completed recovery. Action to be Taken: None.

> Objects: | starCPUSlot starCPUNumber

> Object: | starDiameterPeerDown

> Object ID: | enterprises.8164.2.184

> Description: | A diameter peer is down. Problem Cause: The diameter peer has failed, or a network connectivity prevents reaching the peer. Condition Clear Alarm: A starDiameterPeerUp notification will be generated when the peer is up.

> Objects: | starDiameterVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starDiameterPeerUp

> Object ID: | enterprises.8164.2.185

> Description: | A diameter peer is up. This notification is only generated for peers which have previously been declared down.

> Objects: | starDiameterVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starDiameterServerUnreachable

> Object ID: | enterprises.8164.2.186

> Description: | A diameter server is down. Problem Cause: The diameter server has failed, or a network connectivity prevents reaching the server. Condition Clear Alarm: A starDiameterServerReachable notification will be generated when the server is reachable.

> Objects: | starServiceVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starDiameterServerReachable

> Object ID: | enterprises.8164.2.187

> Description: | A diameter server is up. This notification is only generated for servers which have previously been declared unreachable.

> Objects: | starServiceVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starCDRFileRemoved

> Object ID: | enterprises.8164.2.188

> Description: | A Charging Data Record (CDR) file has been deleted from the system due to a lack of available storage space. When required, the system deletes old files to make space for new files. This notification is only generated when specifically enabled on the system. Probable Cause: CDR files are not being moved off the system, or these files are not being deleted after they have been transferred.

> Objects: | starCDRFilename

> Object: | starCSCFPeerServerReachable

> Object ID: | enterprises.8164.2.189

> Description: | A peer server is reachable

> Objects: | starServiceVPNName starServiceServName starServicePeerServerName

> Object: | starCSCFPeerServerUnreachable

> Object ID: | enterprises.8164.2.190

> Description: | A peer server is reachable

> Objects: | starServiceVPNName starServiceServName starServicePeerServerName

> Object: | starCLIConfigMode

> Object ID: | enterprises.8164.2.192

> Description: | An interactive CLI session has an “enter configuration” mode for the specified context. Thus the CLI user can potentially start entering configuration commands that could impact the entire system. Note that this notification is not enabled by default; it is only generated if the system is specifically configured to enable it.

> Objects: | starCLIUsername starCLIContext

> Object: | starSGSNServiceStart

> Object ID: | enterprises.8164.2.194

> Description: | A SGSN Service has started.

> Objects: | starServiceVpnName starServiceServName

> Object: | starSGSNServiceStop

> Object ID: | enterprises.8164.2.195

> Description: | A SGSN Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the SGSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the SGSN service is operational. Condition Clear Alarm: A starSGSNServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName, starServiceServName

> Object: | starM3UAPCUnavailable

> Object ID: | enterprises.8164.2.196

> Description: | M3UA route to the Point code becomes unavailable. Probable Cause: Received destination unavailable (DUNA) message SCTP association is down Remote peer server is down. Action to be taken: Verify that the peer server is UP.

> Objects: | starSS7rdId starSS7Pc starSS7M3UAPsId

> Object: | starM3UAPCAvailable

> Object ID: | enterprises.8164.2.197

> Description: | M3UA route to the Point code becomes available. Probable Cause: Received destination available (DAVA) message. SCTP Association is up. Remote peer server is up. Condition Clear Alarm: A starM3UAPCAvailable message is generated only after a starM3UAPCUnavailable message was generated.

> Objects: | starSS7M3UAPsId starSS7Pc starSS7rdId

> Object: | starDynPkgLoadError

> Object ID: | enterprises.8164.2.1103

> Description: | The Dynamic rater package error displayed with an error code. Condition Clear Alarm: This condition is cleared by a starDynPkgLoadErrorClear notification

> Objects: | starDynPkgFilename starDynCFErrorCode

> Object: | starDynPkgLoadErrorClear

> Object ID: | enterprises.8164.2.1104

> Description: | The Dynamic rater package error removed.

> Objects: | starDynPkgFilename starDynCFErrorCode

> Object: | starDynPkgUpgradeError

> Object ID: | enterprises.8164.2.1105

> Description: | The Dynamic rater package error displayed with an error code. This condition is cleared by a starDynPkgUpgradeErrorClear

> Description: | The Dynamic rater package error displayed with an error code.

> Objects: | starDynPkgUpgradeFilename starDynCFUpgradeErrorCode

> Object: | starDynPkgUpgradeErrorClear

> Object ID: | enterprises.8164.2.1106

> Description: | The Dynamic Rater package error removed.

> Objects: | starDynPkgUpgradeFilename starDynCFUpgradeErrorCode

> Object: | starCSCFPeerServerUnavailable

> Object ID: | enterprises.8164.2.1107

> Description: | Peer server is unavailable

> Objects: | starCSCFPeerServerVpnName starCSCFPeerServerSvcName starCSCFPeerServerName

> Object: | starCSCFPeerServerOutofService

> Object ID: | enterprises.8164.2.1108

> Description: | Peer server is out-of-service

> Objects: | starCSCFPeerServerVpnName starCSCFPeerServerSvcName starCSCFPeerServerName

> Object: | starCSCFPeerServerInService

> Object ID: | enterprises.8164.2.1109

> Description: | Peer server unavailable and/or out of service condition cleared

> Objects: | starCSCFPeerServerVpnName starCSCFPeerServerSvcName starCSCFPeerServerName

> Object: | starThreshCPUUtilization

> Object ID: | enterprises.8164.2.200

> Description: | The overall CPU utilization for the identified processor has exceeded for configured threshold value for the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCPUUtilization notification will be generated when the measured value falls below the threshold.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCPUUtilization

> Object ID: | enterprises.8164.2.201

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshCPUMemory

> Object ID: | enterprises.8164.2.202

> Description: | The amount of available memory for the identified processor has fallen below the configured threshold value. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCPUMemory notification will be generated when the measured value falls below the threshold.

> Objects: | starCPUSlot starCPUNumber starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCPUMemory

> Object ID: | enterprises.8164.2.203

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshInt starThreshMeasuredInt

> Object: | starThreshLicense

> Object ID: | enterprises.8164.2.204

> Description: | The percentage available, licensed subscribers has fallen below the configured threshold value. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearLicense notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct starServiceType

> Object: | starThreshClearLicense

> Object ID: | enterprises.8164.2.205

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt starServiceType

> Object: | starThreshSubscriberTotal

> Object ID: | enterprises.8164.2.206

> Description: | The total number of subscribers is above the configured threshold value. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSubscriberTotal notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearSubscriberTotal

> Object ID: | enterprises.8164.2.207

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshSubscriberActive

> Object ID: | enterprises.8164.2.208

> Description: | The total number of active subscribers is above the configured threshold value. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSubscriberActive notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearSubscriberActive

> Object ID: | enterprises.8164.2.209

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPortRxUtil

> Object ID: | enterprises.8164.2.210

> Description: | The Rx utilization of the port has exceeded the configured threshold value during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortRxUtil notification will be generated when the measured value falls below the threshold.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshClearPortRxUtil

> Object ID: | enterprises.8164.2.211

> Description: | The threshold condition is now clear.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshPortTxUtil

> Object ID: | enterprises.8164.2.212

> Description: | The Tx utilization of the port has exceeded the configured threshold value during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortTxUtil notification will be generated when the measured value falls below the threshold.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshClearPortTxUtil

> Object ID: | enterprises.8164.2.213

> Description: | The threshold condition is now clear.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshPortHighActivity

> Object ID: | enterprises.8164.2.214

> Description: | The number of seconds of 'high activity' time on the port has exceeded the configured threshold value during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortHighActivity notification is generated when the measured value falls below the threshold.

> Objects: | starPortSlot starPortNum starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPortHighActivity

> Object ID: | enterprises.8164.2.215

> Description: | The threshold condition is now clear.

> Objects: | starPortSlot starPortNum starThreshInt starThreshMeasuredInt

> Object: | starThreshAAAAuthFail

> Object ID: | enterprises.8164.2.216

> Description: | The number of AAA authentication failures has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAuthFail notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearAAAAuthFail

> Object ID: | enterprises.8164.2.217

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshAAAAuthFailRate

> Object ID: | enterprises.8164.2.218

> Description: | The percentage of AAA authentication requests which failed has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAuthFailRate notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearAAAAuthFailRate

> Object ID: | enterprises.8164.2.219

> Description: | The threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshAAAAcctFail

> Object ID: | enterprises.8164.2.220

> Description: | The number of AAA accounting failures has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctFail notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearAAAAcctFail

> Object ID: | enterprises.8164.2.221

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshAAAAcctFailRate

> Object ID: | enterprises.8164.2.222

> Description: | The percentage of AAA accounting requests which failed has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctFailRate notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearAAAAcctFailRate

> Object ID: | enterprises.8164.2.223

> Description: | The threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshAAARetryRate

> Object ID: | enterprises.8164.2.224

> Description: | The percentage of AAA requests which has to be retried has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAARetryRate notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearAAARetryRate

> Object ID: | enterprises.8164.2.225

> Description: | The threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshCallSetup

> Object ID: | enterprises.8164.2.226

> Description: | The number of call setup operations has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallSetup notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCallSetup

> Object ID: | enterprises.8164.2.227

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshCallSetupFailure

> Object ID: | enterprises.8164.2.228

> Description: | The number of call setup operations which failed has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallSetupFailure notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCallSetupFailure

> Object ID: | enterprises.8164.2.229

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshCallRejectNoResource

> Object ID: | enterprises.8164.2.230

> Description: | The number of call setup operations which were rejected due to a no resource condition has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallRejectNoResource notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCallRejectNoResource

> Object ID: | enterprises.8164.2.231

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPacketsFilteredDropped

> Object ID: | enterprises.8164.2.232

> Description: | The number of user data packets filtered has exceeded the configured threshold for the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearPacketsFilteredDropped notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPacketsFilteredDropped

> Object ID: | enterprises.8164.2.233

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPacketsForwarded

> Object ID: | enterprises.8164.2.234

> Description: | The number of user data packets forwarded has exceeded the configured threshold for the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPacketsForwarded notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPacketsForwarded

> Object ID: | enterprises.8164.2.235

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshSessCPUThroughput

> Object ID: | enterprises.8164.2.236

> Description: | The total session throughout for the specified processor has exceeded the configured threshold for the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSessCPUThroughput notification will be generated when the measured value falls below the threshold.

> Objects: | starCPUSlot starCPUNumber starThreshMB starThreshMeasuredMB

> Object: | starThreshClearSessCPUThroughput

> Object ID: | enterprises.8164.2.237

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshMB starThreshMeasuredMB

> Object: | starThreshIPPoolAvail

> Object ID: | enterprises.8164.2.238

> Description: | The available IP pool addresses in a context has fallen below the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPPoolAvail notification will be generated when the measured value falls below the threshold.

> Objects: | starIPPoolContext starIPPoolGroup starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPPoolAvail

> Object ID: | enterprises.8164.2.239

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolGroup starThreshInt starThreshMeasuredInt

> Object: | starThreshCPUUtilization10Sec

> Object ID: | enterprises.8164.2.240

> Description: | The CPU utilization of 10 second measurement for the identified processor has exceeded for configured threshold value for the current monitoring period.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCPUUtilization10Sec

> Object ID: | enterprises.8164.2.241

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshCPULoad

> Object ID: | enterprises.8164.2.242

> Description: | The CPU load for the identified processor has exceeded for configured threshold value for the current monitoring period.

> Objects: | starCPUSlot starCPUNumber starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCPULoad

> Object ID: | enterprises.8164.2.243

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshInt starThreshMeasuredInt

> Object: | starThreshCPUMemUsage

> Object ID: | enterprises.8164.2.244

> Description: | The CPU mem usage for the identified processor has exceeded for configured threshold value for the current monitoring period.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCPUMemUsage

> Object ID: | enterprises.8164.2.245

> Description: | The threshold condition is now clear.

> Objects: | starCPUSlot starCPUNumber starThreshPct starThreshMeasuredPct

> Object: | starThreshPDSNSessions

> Object ID: | enterprises.8164.2.246

> Description: | The total number of PDSN sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSessions

> Object ID: | enterprises.8164.2.247

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshGGSNSessions

> Object ID: | enterprises.8164.2.248

> Description: | The total number of GGSN sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearGGSNSessions

> Object ID: | enterprises.8164.2.249

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshHASessions

> Object ID: | enterprises.8164.2.250

> Description: | The total number of HA sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHASessions

> Object ID: | enterprises.8164.2.251

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshLNSSessions

> Object ID: | enterprises.8164.2.252

> Description: | The total number of L2TP LNS sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearLNSSessions

> Object ID: | enterprises.8164.2.253

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServicePDSNSessions

> Object ID: | enterprises.8164.2.254

> Description: | The total number of PDSN sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServicePDSNSessions

> Object ID: | enterprises.8164.2.255

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceGGSNSessions

> Object ID: | enterprises.8164.2.256

> Description: | The total number of GGSN sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceGGSNSessions

> Object ID: | enterprises.8164.2.257

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceHASessions

> Object ID: | enterprises.8164.2.258

> Description: | The total number of HA sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceHASessions

> Object ID: | enterprises.8164.2.259

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceLNSSessions

> Object ID: | enterprises.8164.2.260

> Description: | The total number of L2TP LNS sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceLNSSessions

> Object ID: | enterprises.8164.2.261

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPPoolHold

> Object ID: | enterprises.8164.2.262

> Description: | The percentage IP pool addresses in HOLD state in a context has gone above the configured threshold.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPPoolHold

> Object ID: | enterprises.8164.2.263

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPPoolUsed

> Object ID: | enterprises.8164.2.264

> Description: | The percentage IP pool addresses in USED state in a context has gone above the configured threshold.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPPoolUsed

> Object ID: | enterprises.8164.2.265

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPPoolRelease

> Object ID: | enterprises.8164.2.266

> Description: | The percentage IP pool addresses in RELEASE state in a context has gone above the configured threshold.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPPoolRelease

> Object ID: | enterprises.8164.2.267

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPPoolFree

> Object ID: | enterprises.8164.2.268

> Description: | The percentage IP pool addresses in HOLD state in a context has gone below the configured threshold.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPPoolFree

> Object ID: | enterprises.8164.2.269

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshAAAAcctArchive

> Object ID: | enterprises.8164.2.270

> Description: | The AAA accounting archive size has gone above the configured threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearAAAAcctArchive

> Object ID: | enterprises.8164.2.271

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPortSpecRxUtil

> Object ID: | enterprises.8164.2.272

> Description: | The Rx utilization of the port has exceeded the configured threshold value during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortSpecRxUtil notification will be generated when the measured value falls below the threshold.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshClearPortSpecRxUtil

> Object ID: | enterprises.8164.2.273

> Description: | The threshold condition is now clear.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshPortSpecTxUtil

> Object ID: | enterprises.8164.2.274

> Description: | The Tx utilization of the port has exceeded the configured threshold value during the current monitoring period. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortSpecTxUtil notification will be generated when the measured value falls below the threshold.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshClearPortSpecTxUtil

> Object ID: | enterprises.8164.2.275

> Description: | The threshold condition is now clear.

> Objects: | starPortSlot starPortNum starThreshPct starThreshMeasuredPct

> Object: | starThreshHACallSetupRate

> Object ID: | enterprises.8164.2.276

> Description: | The per-context HA call setup rate (calls per second) has gone above the configured threshold Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in 'alarm' mode, a starThreshClearHACallSetupRate notification will be generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHACallSetupRate

> Object ID: | enterprises.8164.2.277

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starThreshInt starThreshMeasuredInt

> Object: | starThreshHASvcCallSetupRate

> Object ID: | enterprises.8164.2.278

> Description: | The per-service HA Call setup rate (calls per second) has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcCallSetupRate notification will be generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHASvcCallSetupRate

> Object ID: | enterprises.8164.2.279

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshHASvcRegReplyError

> Object ID: | enterprises.8164.2.280

> Description: | The per-service HA Reg Reply Error count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcRegReplyError notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHASvcRegReplyError

> Object ID: | enterprises.8164.2.281

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshHASvcReregReplyError

> Object ID: | enterprises.8164.2.282

> Description: | The per-service HA Rereg Reply Error count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcReregReplyError notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHASvcReregReplyError

> Object ID: | enterprises.8164.2.283

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshHASvcDeregReplyError

> Object ID: | enterprises.8164.2.284

> Description: | The per-service HA Dereg Reply Error count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcDeregReplyError notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHASvcDeregReplyError

> Object ID: | enterprises.8164.2.285

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshFASvcRegReplyError

> Object ID: | enterprises.8164.2.286

> Description: | The Per-Service FA Reg Reply Error count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearFASvcRegReplyError notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFASvcRegReplyError

> Object ID: | enterprises.8164.2.287

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNCallSetupRate

> Object ID: | enterprises.8164.2.288

> Description: | The Per-Context PDSN Call Setup Rate (calls per second) has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNCallSetupRate notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNCallSetupRate

> Object ID: | enterprises.8164.2.289

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNSvcCallSetupRate

> Object ID: | enterprises.8164.2.290

> Description: | The Per-Service PDSN Call Setup Rate (calls per second) has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcCallSetupRate notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSvcCallSetupRate

> Object ID: | enterprises.8164.2.291

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNSvcA11RRPFailure

> Object ID: | enterprises.8164.2.292

> Description: | The Per-Service PDSN A11 RRP Failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcA11RRPFailure notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSvcA11RRPFailure

> Object ID: | enterprises.8164.2.293

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNSvcA11RRQMsgDiscard

> Object ID: | enterprises.8164.2.294

> Description: | The Per-Service PDSN A11 RRQ Msg Discard count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode a starThreshClearPDSNSvcA11RRQMsgDiscard notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSvcA11RRQMsgDiscard

> Object ID: | enterprises.8164.2.295

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNSvcA11RACMsgDiscard

> Object ID: | enterprises.8164.2.296

> Description: | The Per-Service PDSN A11 RAC Msg Discard count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode a starThreshClearPDSNSvcA11RACMsgDiscard notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSvcA11RACMsgDiscard

> Object ID: | enterprises.8164.2.297

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPDSNSvcA11PPPSendDiscard

> Object ID: | enterprises.8164.2.298

> Description: | he Per-Service PDSN A11 PPP Send Discard count has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcA11PPPSendDiscard notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDSNSvcA11PPPSendDiscard

> Object ID: | enterprises.8164.2.299

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshAAAMgrQueue

> Object ID: | enterprises.8164.2.300

> Description: | The Per-AAA Manager internal request queue usage has gone above the configured threshold Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAMgrQueue is generated when the measured value falls below the threshold.

> Objects: | starTaskInstance starThreshPct starThreshMeasuredPct

> Object: | starThreshClearAAAMgrQueue

> Object ID: | enterprises.8164.2.301

> Description: | The threshold condition is now clear.

> Objects: | starTaskInstance starThreshPct starThreshMeasuredPct

> Object: | starThreshCPUOrbsWarn

> Object ID: | enterprises.8164.2.302

> Description: | The ORBs task has exceeding the CPU usage configured as a warning

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCPUOrbsWarn

> Object ID: | enterprises.8164.2.303

> Description: | The threshold condition is now clear

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshCPUOrbsCritical

> Object ID: | enterprises.8164.2.304

> Description: | The ORBs task has exceeded the CPU usage configured as a critical error

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCPUOrbsCritical

> Object ID: | enterprises.8164.2.305

> Description: | The threshold condition is now clear

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshRPSetupFailRate

> Object ID: | enterprises.8164.2.306

> Description: | The RP call setup failure rate has exceeded the configured threshold

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearRPSetupFailRate

> Object ID: | enterprises.8164.2.307

> Description: | The threshold condition is now clear

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshPPPSetupFailRate

> Object ID: | enterprises.8164.2.308

> Description: | The PPP call setup failure rate has exceeded the configured threshold

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearPPPSetupFailRate

> Object ID: | enterprises.8164.2.309

> Description: | The threshold condition is now clear

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshStorageUtilization

> Object ID: | enterprises.8164.2.310

> Description: | The utilization of a mass storage device has exceeded the configured threshold.

> Objects: | starStorageSlot starStorageName starThreshPct starThreshMeasuredPct

> Object: | starThreshClearStorageUtilization

> Object ID: | enterprises.8164.2.311

> Description: | The threshold condition is now clear.

> Objects: | starStorageSlot starStorageName starThreshPct starThreshMeasuredPct

> Object: | starThreshDCCAProtocolErrors

> Object ID: | enterprises.8164.2.312

> Description: | The number of DCCA Protocol Errors has exceeded the configured threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearDCCAProtocolErrors

> Object ID: | enterprises.8164.2.313

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshDCCABadAnswers

> Object ID: | enterprises.8164.2.314

> Description: | The number of DCCA BadAnswers has exceeded the configured threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearDCCABadAnswers

> Object ID: | enterprises.8164.2.315

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshDCCAUnknownRatingGroup

> Object ID: | enterprises.8164.2.316

> Description: | The number of DCCA UnknownRatingGroup has exceeded the configured threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearDCCAUnknownRatingGroup

> Object ID: | enterprises.8164.2.317

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshDCCARatingFailed

> Object ID: | enterprises.8164.2.318

> Description: | The number of DCCA RatingFailed has exceeded the configured threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearDCCARatingFailed

> Object ID: | enterprises.8164.2.319

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshIPSECIKERequests

> Object ID: | enterprises.8164.2.320

> Description: | The number of IPSEC IKE requests seen for this HA service has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearIPSECIKERequests notification will be generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPSECIKERequests

> Object ID: | enterprises.8164.2.321

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPSECIKEFailures

> Object ID: | enterprises.8164.2.322

> Description: | The number of IPSEC IKE failures seen for this HA service has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECIKEFailures notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPSECIKEFailures

> Object ID: | enterprises.8164.2.323

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPSECIKEFailRate

> Object ID: | enterprises.8164.2.324

> Description: | The rate of IPSEC IKE failures (as a percentage of total requests) seen for this HA service has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECIKEFailRate notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshPct starThreshMeasuredPct

> Object: | starThreshClearIPSECIKEFailRate

> Object ID: | enterprises.8164.2.325

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshPct starThreshMeasuredPct

> Object: | starThreshIPSECTunSetup

> Object ID: | enterprises.8164.2.326

> Description: | The number of IPSEC tunnels setup over the last measurement period for this HA service has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunSetup notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPSECTunSetup

> Object ID: | enterprises.8164.2.327

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPSECTunEstabl

> Object ID: | enterprises.8164.2.328

> Description: | The current number of IPSEC tunnels established for this HA service has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunEstabl notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPSECTunEstabl

> Object ID: | enterprises.8164.2.329

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshIPSECCallReqRej

> Object ID: | enterprises.8164.2.330

> Description: | The number of IPSEC Rejected Call Requests has exceeded the configured threshold. Probable Cause: This is a user configurable threshold. Reject Call Requests indicate that an IPSEC Manager has reached its maximum allowable number of IPSEC tunnels. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunnelsTotal notification is generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearIPSECCallReqRej

> Object ID: | enterprises.8164.2.331

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcRouteFailure

> Object ID: | enterprises.8164.2.332

> Description: | The Per-Service CSCF Route failure count has gone above the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCSCFSvcRouteFailure notification will be generated when the measured value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcRouteFailure

> Object ID: | enterprises.8164.2.333

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshContFiltRating

> Object ID: | enterprises.8164.2.334

> Description: | The number of Content Filtering Rating operations performed has gone above the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearContFiltRating notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearContFiltRating

> Object ID: | enterprises.8164.2.335

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshContFiltBlock

> Object ID: | enterprises.8164.2.336

> Description: | The number of Content Filtering Block operations performed has gone above the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearContFiltBlock notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearContFiltBlock

> Object ID: | enterprises.8164.2.337

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshCDRFileSpace

> Object ID: | enterprises.8164.2.338

> Description: | The CDR file space usage is above the configured threshold percentage. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearCDRFileSpaceOverLimit notification is generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearCDRFileSpace

> Object ID: | enterprises.8164.2.339

> Description: | This information indicates that the threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshEDRFileSpace

> Object ID: | enterprises.8164.2.340

> Description: | The EDR file space usage is above the configured threshold percentage. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearEDRFileSpaceOverLimit notification generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearEDRFileSpace

> Object ID: | enterprises.8164.2.341

> Description: | This information indicates that the threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshPDIFCurrSess

> Object ID: | enterprises.8164.2.342

> Description: | The chassis-wide count of current PDIF sessions has gone above the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in 'alarm' mode, a starThreshClearPDIFCurrSess notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDIFCurrSess

> Object ID: | enterprises.8164.2.343

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPDIFCurrActSess

> Object ID: | enterprises.8164.2.344

> Description: | The chassis-wide count of current PDIF active sessions has gone above the configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: If thresholding is configured to run in ‘alarm’ mode, a starThreshClearPDIFCurrActSess notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDIFCurrActSess

> Object ID: | enterprises.8164.2.345

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshCDRFlowControl

> Object ID: | enterprises.8164.2.346

> Description: | The number of Charging Data Record (CDR) records which have been discarded at an ACSMGR due to flow control has gone above the configured threshold. Probable Cause: This is a user configurable threshold. This threshold potentially indicates an overload condition due which prevents processes CDR messages at the same rate as the incoming packets. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearCDRFlowControl notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCDRFlowControl

> Object ID: | enterprises.8164.2.347

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWSessTimeout

> Object ID: | enterprises.8164.2.348

> Description: | ASNGW session timeout has exceeded the configured threshold. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in ‘alarm’ mode, a starThreshClearASNGWSessTimeout notification is generated when the value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWSessTimeout

> Object ID: | enterprises.8164.2.349

> Description: | Threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWSessSetupTimeout

> Object ID: | enterprises.8164.2.350

> Description: | ASNGW session setup timeout has exceeded the configured threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWSessSetupTimeout notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWSessSetupTimeout

> Object ID: | enterprises.8164.2.351

> Description: | Threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWAuthFail

> Object ID: | enterprises.8164.2.352

> Description: | Number of ASNGW authentication failures has exceeded the configured threshold in the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearASNGWAuthFail notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWAuthFail

> Object ID: | enterprises.8164.2.353

> Description: | Threshold conditrion is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWR6InvNai

> Object ID: | enterprises.8164.2.354

> Description: | Number of ASNGW Invalid NAI has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWR6InvNai notification is generated when the value falls below the threshold.

> IMPORTANT: This object is obsolete.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWR6InvNai

> Object ID: | enterprises.8164.2.355

> Description: | Threshold condition is now clear

> IMPORTANT: This object is obsolete.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWMaxEAPRetry

> Object ID: | enterprises.8164.2.356

> Description: | Number of ASNGW EAP retries has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearASNGWMaxEAPRetry notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWMaxEAPRetry

> Object ID: | enterprises.8164.2.357

> Description: | Threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWNWEntryDenial

> Object ID: | enterprises.8164.2.358

> Description: | Number of ASNGW network entry denials has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWNWEntryDenial notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWNWEntryDenial

> Object ID: | enterprises.8164.2.359

> Description: | Threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWHandoffDenial

> Object ID: | enterprises.8164.2.360

> Description: | Number of ASNGW handoff denials has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGW Handoff Denial notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWHandoffDenial

> Object ID: | enterprises.8164.2.361

> Description: | Threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshSGSNSessions

> Object ID: | enterprises.8164.2.362

> Description: | The total number of SGSN sessions is above the configured threshold value. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearSGSNSessions notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearSGSNSessions

> Object ID: | enterprises.8164.2.363

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceSGSNSessions

> Object ID: | enterprises.8164.2.364

> Description: | The total number of SGSN sessions in a service is above the configured threshold value. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearPerServiceSGSNSessions notification is generated when the value falls below the threshold.

> Description: |

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceSGSNSessions

> Object ID: | enterprises.8164.2.365

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshSGSNPdpSessions

> Object ID: | enterprises.8164.2.366

> Description: | The total number of SGSN PDP sessions is above the configured threshold value. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearSGSNPdpSessions notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearSGSNPdpSessions

> Object ID: | enterprises.8164.2.367

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceSGSNPdpSessions

> Object ID: | enterprises.8164.2.368

> Description: | The total number of SGSN PDP sessions in a service is above the configured threshold value. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearPerServiceSGSNPdpSessions notification is generated when the value falls below the threshold.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceSGSNPdpSessions

> Object ID: | enterprises.8164.2.369

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshFWDosAttack

> Object ID: | enterprises.8164.2.370

> Description: | The cumulative number of FW DoS Attacks has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDoSAttack notification is generated when the value falls below the threshold.

> Description: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFWDosAttack

> Object ID: | enterprises.8164.2.371

> Description: | Threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshFWDropPacket

> Object ID: | enterprises.8164.2.372

> Description: | The cumulative number of FW dropped packets has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDropPacket notification is generated when the value falls below the threshold.

> Description: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFWDropPacket

> Object ID: | enterprises.8164.2.373

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshFWDenyRule

> Object ID: | enterprises.8164.2.374

> Description: | The cumulative number of FW Deny-Rules has exceeded the user-configurable threshold. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDenyRule notification is generated when the value falls below the threshold.

> Description: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFWDenyRule

> Object ID: | enterprises.8164.2.375

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshFWNoRule

> Object ID: | enterprises.8164.2.376

> Description: | The cumulative number of FW No Rules has exceeded the configured threshold in the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDenyRule notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFWNoRule

> Object ID: | enterprises.8164.2.377

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWSessTimeout

> Object ID: | enterprises.8164.2.378

> Description: | The PHSGW session timeout has gone above the configured threshold. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWSessTimeout

> Object ID: | enterprises.8164.2.379

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWSessSetupTimeout

> Object ID: | enterprises.8164.2.380

> Description: | The PHSGW session setup timeout has gone above the configured threshold. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWSessSetupTimeout

> Object ID: | enterprises.8164.2.381

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWAuthFail

> Object ID: | enterprises.8164.2.382

> Description: | The number of PHSGW authentication failures has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWAuthFail

> Object ID: | enterprises.8164.2.383

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWMaxEAPRetry

> Object ID: | enterprises.8164.2.384

> Description: | The number of PHSGW Maximum EAP Retry has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWMaxEAPRetry

> Object ID: | enterprises.8164.2.385

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWNWEntryDenial

> Object ID: | enterprises.8164.2.386

> Description: | The number of PHSGW Network Entry Denial has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWNWEntryDenial

> Object ID: | enterprises.8164.2.387

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWHandoffDenial

> Object ID: | enterprises.8164.2.388

> Description: | The number of PHSGW Handoff Denial has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWHandoffDenial

> Object ID: | enterprises.8164.2.389

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshASNGWSessions

> Object ID: | enterprises.8164.2.390

> Description: | The total number of ASNGW sessions is above the configured threshold value. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: a starThreshClearASNGWSessions notification is generated when the value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearASNGWSessions

> Object ID: | enterprises.8164.2.391

> Description: | Threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceASNGWSessions

> Object ID: | enterprises.8164.2.392

> Description: | The total number of PDSN sessions in a service is above the configured threshold value. Possible Cause: This is a user-configurable threshold. Condition Clear Alarm: a starThreshClearPerServiceASNGWSessions notification is generated when the value falls below the threshold.

> Objects: | starServiceVPNName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceASNGWSessions

> Object ID: | enterprises.8164.2.393

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSPCSessSetupTimeout

> Object ID: | enterprises.8164.2.394

> Description: | The PHSPC session setup timeout has gone above the configured threshold Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSPCSessSetupTimeout

> Object ID: | enterprises.8164.2.395

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSPCSleepModeTimeout

> Object ID: | enterprises.8164.2.396

> Description: | The PHSPC idle mode timeout has gone above the configured threshold. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSPCSleepModeTimeout

> Object ID: | enterprises.8164.2.397

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSPCSmEntryDenial

> Object ID: | enterprises.8164.2.398

> Description: | The number of PHSPC sm entry denial has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSPCSmEntryDenial

> Object ID: | enterprises.8164.2.399

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshSGWSessions

> Object ID: | enterprises.8164.2.408

> Description: | The total number of SGW sessions is above the configured threshold value Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearSGWSessions notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearSGWSessions

> Object ID: | enterprises.8164.2.409

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPGWSessions

> Object ID: | enterprises.8164.2.410

> Description: | The total number of PGW sessions is above the configured threshold valu Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearSGWSessions notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPGWSessions

> Object ID: | enterprises.8164.2.411

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshMeasuredInt

> Object ID: | enterprises.8164.2.412

> Description: | The total number of LMA sessions is above the configured threshold value Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearLMASessions notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearLMASessions

> Object ID: | enterprises.8164.2.413

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshMAGSessions

> Object ID: | enterprises.8164.2.414

> Description: | The total number of MAG sessions is above the configured threshold value Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearMAGSessions notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearMAGSessions

> Object ID: | enterprises.8164.2.415

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshFNGCurrSess

> Object ID: | enterprises.8164.2.416

> Description: | The chassis-wide count of current FNG sessions has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearFNGCurrSess notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFNGCurrSess

> Object ID: | enterprises.8164.2.417

> Description: | he threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshFNGCurrActSess

> Object ID: | enterprises.8164.2.418

> Description: | The chassis-wide count of current FNG active sessions has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearFNGCurrActiveSess notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearFNGCurrActSess

> Object ID: | enterprises.8164.2.419

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWEAPOLAuthFailure

> Object ID: | enterprises.8164.2.420

> Description: | The number of PHSGW EAPOL Auth Failure has exceeded the configured threshold during the current monitoring period Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshPHSGWEAPOLAuthFailure notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWEAPOLAuthFailure

> Object ID: | enterprises.8164.2.421

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPHSGWMaxEAPOLRetry

> Object ID: | enterprises.8164.2.422

> Description: | The number of PHSGW max EAPOL retry has exceeded the configured threshold during the current monitoring period Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshPHSGWMaxEAPOLRetry notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPHSGWMaxEAPOLRetry

> Object ID: | enterprises.8164.2.423

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshHSGWSessions

> Object ID: | enterprises.8164.2.424

> Description: | The total number of HSGW sessions is above the configured threshold value Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearHSGWSessions notification will be generated when the measured value falls below the threshold

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearHSGWSessions

> Object ID: | enterprises.8164.2.425

> Description: | The threshold condition is now clear

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPDGCurrSess

> Object ID: | enterprises.8164.2.426

> Description: | The chassis-wide count of current PDG sessions has gone above the configured threshold. Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearPDGCurrSess notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDGCurrSess

> Object ID: | enterprises.8164.2.427

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPDGCurrActSess

> Object ID: | enterprises.8164.2.428

> Description: | The chassis-wide count of current PDG active sessions has gone above the configured threshold Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearPDGCurrActiveSess notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPDGCurrActSess

> Object ID: | enterprises.8164.2.429

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshNAPTPortChunks

> Object ID: | enterprises.8164.2.430

> Description: | The NAT port chunks utilization of NAT pool is above the configured threshold value. Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearNAPTPortChunks notification will be generated when the measured value exceeds the threshold.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearNAPTPortChunks

> Object ID: | enterprises.8164.2.431

> Description: | The threshold condition is now clear.

> Objects: | starIPPoolContext starIPPoolName starThreshInt starThreshMeasuredInt

> Object: | starThreshGPRSSessions

> Object ID: | enterprises.8164.2.432

> Description: | The total number of GPRS sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearGPRSSessions

> Object ID: | enterprises.8164.2.433

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceGPRSSessions

> Object ID: | enterprises.8164.2.434

> Description: | The total number of GPRS sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceGPRSSessions

> Object ID: | enterprises.8164.2.435

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshGPRSPdpSessions

> Object ID: | enterprises.8164.2.436

> Description: | The total number of GPRS PDP sessions is above the configured threshold value.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshClearGPRSPdpSessions

> Object ID: | enterprises.8164.2.437

> Description: | The threshold condition is now clear.

> Objects: | starThreshInt starThreshMeasuredInt

> Object: | starThreshPerServiceGPRSPdpSessions

> Object ID: | enterprises.8164.2.438

> Description: | The total number of GPRS PDP sessions in a service is above the configured threshold value.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearPerServiceGPRSPdpSessions

> Object ID: | enterprises.8164.2.439

> Description: | The threshold condition is now clear.

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcRegRcvdRate

> Object ID: | enterprises.8164.2.446

> Description: | The Per-Service CSCF Registration Per Interval count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcRegRcvdRate notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcRegRcvdRate

> Object ID: | enterprises.8164.2.447

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcTotalActiveReg

> Object ID: | enterprises.8164.2.448

> Description: | The Per-Service CSCF Total Active Registrations count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcTotalActiveReg notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcTotalActiveReg

> Object ID: | enterprises.8164.2.449

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcInviteRcvdRate

> Object ID: | enterprises.8164.2.450

> Description: | The Per-Service CSCF Calls Per Interval count has gone above the configured threshold Probable Cause: This is a user configurable threshold If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcInviteRcvdRate notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcInviteRcvdRate

> Object ID: | enterprises.8164.2.451

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcTotalActiveCalls

> Object ID: | enterprises.8164.2.452

> Description: | The Per-Service CSCF Total Active Calls count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcTotalActiveCalls notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcTotalActiveCalls

> Object ID: | enterprises.8164.2.453

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcTotalCallFailure

> Object ID: | enterprises.8164.2.454

> Description: | The Per-Service CSCF Total Call Failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcTotalCallFailure notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcTotalCallFailure

> Object ID: | enterprises.8164.2.455

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcErrorNoResource

> Object ID: | enterprises.8164.2.456

> Description: | The Per-Service CSCF No resource failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcErrorNoResource notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcErrorNoResource

> Object ID: | enterprises.8164.2.457

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcErrorTcp

> Object ID: | enterprises.8164.2.458

> Description: | The Per-Service CSCF Tcp failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcErrorTcp notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcErrorTcp

> Object ID: | enterprises.8164.2.459

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcErrorPresence

> Object ID: | enterprises.8164.2.460

> Description: | The Per-Service CSCF Presence failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcErrorPresence notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcErrorPresence

> Object ID: | enterprises.8164.2.461

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshCSCFSvcErrorRegAuth

> Object ID: | enterprises.8164.2.462

> Description: | The Per-Service CSCF Reg-Auth failure count has gone above the configured threshold Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearCSCFSvcErrorRegAuth notification will be generated when the measured value falls below the threshold

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearCSCFSvcErrorRegAuth

> Object ID: | enterprises.8164.2.463

> Description: | The threshold condition is now clear

> Objects: | starServiceVpnName starServiceServName starThreshInt starThreshMeasuredInt

> Object: | starThreshBGPRoutes

> Object ID: | enterprises.8164.2.464

> Description: | The Total number of BGP routes is above the configured threshold value Probable Cause: This is a user configurable threshold, If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearBGPRoutes notification will be generated when the measured value falls below the threshold

> Objects: | starContextName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearBGPRoutes

> Object ID: | enterprises.8164.2.465

> Description: | The threshold condition is now clear

> Objects: | starContextName starThreshInt starThreshMeasuredInt

> Object: | starThreshNPUUtilization

> Object ID: | enterprises.8164.2.478

> Description: | The overall NPU utilization for the identified processor has exceeded for configured threshold value for the current monitoring period. Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearNPUUtilization notification will be generated when the measured value falls below the threshold.

> Objects: | starNPUSlot starThreshPct starThreshMeasuredPct

> Object: | starThreshClearNPUUtilization

> Object ID: | enterprises.8164.2.479

> Description: | The threshold condition is now clear.

> Objects: | starNPUSlot starThreshPct starThreshMeasuredPct

> Object: | starThreshDnsLookupFailure

> Object ID: | enterprises.8164.2.480

> Description: | The Total number of DNS lookup failures is above the configured threshold value. Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearDnsLookupFailure notification will be generated when the measured value falls below the threshold.

> Objects: | starContextName starThreshInt starThreshMeasuredInt

> Object: | starThreshClearDnsLookupFailure

> Object ID: | enterprises.8164.2.481

> Description: | The threshold condition is now clear.

> Objects: | starContextName starThreshInt starThreshMeasuredInt

> Object: | starThreshDiameterRetryRate

> Object ID: | enterprises.8164.2.482

> Description: | The percentage of Diameter requests which has to be retried has exceeded the configured threshold during the current monitoring period. Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearDiameterRetryRate notification will be generated when the measured value falls below the threshold.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starThreshClearDiameterRetryRate

> Object ID: | enterprises.8164.2.483

> Description: | The threshold condition is now clear.

> Objects: | starThreshPct starThreshMeasuredPct

> Object: | starOSPFNeighborDown

> Object ID: | enterprises.8164.2.1001

> Description: | An OSPF neighbor is down. Probable Cause: Problems with network connectivity. Condition Clear Alarm: A starOSPFNeighborFull notification is generated when the neighbor is restored.

> Objects: | starContextName starInterfaceName starInterfaceIPAddress starOSPFNeighborRouterID starOSPFFromState starOSPFToState

> Object: | starOSPFNeighborFull

> Object ID: | enterprises.8164.2.1002

> Description: | A starOSPFNeighborFull notification is only sent for neighbors which had previously been declared down via a starOSPFNeighborDown notification.

> Objects: | starContextName starInterfaceName starInterfaceIPAddress starOSPFNeighborRouterID

> Object: | starM3UAPSDown

> Object ID: | enterprises.8164.2.1004

> Description: | M3UA Peer Server is unavailable Probable Cause: All related Peer Server Processes are in the ASP Down state for this server. Condition Clear Alarm: A starM3UAPSActive notification will be generated when the App Server becomes reachable.

> Objects: | starSS7Rdid starSS7M3UAPsid

> Object: | starM3UAPSActive

> Object ID: | enterprises.8164.2.1005

> Description: | Peer server is available and passing traffic. At least one ASP is in the ASP_ACTIVE state. This condition is only generated for Peer Services previously declared unavailable.

> Objects: | starSS7rdId starSS7M3UAPsId

> Object: | starM3UAPSPDown

> Object ID: | enterprises.8164.2.1006

> Description: | ASP Down message received from the remote M3UA peer indicates the adaptation layer at the remote peer is not ready to receive DATA, SSNM, RKM or ASPTM messages. Probable Cause: SCTP association down or Remote peer server down. Condition Clear Alarm: A starM3UAPSPUp notification will be generated when remote ASP is available

> Objects: | starSS7rdId starSS7M3UAPspID

> Object: | starM3UAPSPUp

> Object ID: | enterprises.8164.2.1007

> Description: | ASP Up message from remote M3UA Peer indicates the adaptation layer at the remote per is ready to receive ASPSM/ASPTM messages for all routing keys the ASP is configured to serve. Up message is only generated after a previous Down message.

> Objects: | starSS7rdId starSS7M3UAPspId starSS7M3UAPsId

> Object: | starSCCPSspRcvd

> Object ID: | enterprises.8164.2.1008

> Description: | Subsystem Prohibited message was received from a peer. Probable Cause: This is sent by the peer SCCP layer when one of its apps (subsystems), such as the HLR, is out of commission. Action to be Taken: Receiving node needs to update the translation tables so that traffic can be directed to a backup system if available. Condition Clear Alarm: A starSCCPSspClear notification is generated when this condition is cleared.

> Objects: | starSccpNwId starSS7Pc starSccpSsn

> Object: | starSCCPSspClear

> Object ID: | enterprises.8164.2.1009

> Description: | Subsystem Available received from a peer This indicates a previously prohibited node is now available.

> Objects: | starSccpNwId starSS7Pc starSccpSsn

> Object: | starSGSNRNCReset

> Object ID: | enterprises.8164.2.1010

> Description: | SGSN has received a Radio Network Controller reset event. SGSN will clean up all the lu connections.

> IMPORTANT: This event is not generated for RNC Reset the first time the system boots up.

> Objects: | starSessSGSNVpnName starSessSGSNServName starSessSGSNMcc starSessSGSNMnc starSessSGSNRncId

> Object: | starSGSNHLRReset

> Object ID: | enterprises.8164.2.1011

> Description: | Home Location Register (HLR) reset event received. SGSN will mark all subscribers served by this HLR so the subscription record can be fetched again on subsequent activity.

> Objects: | starSessSGSNVpnName starSessSGSNServName starSessSGSNhlrNum

> Object: | starSGSNGtpcPathFailure

> Object ID: | enterprises.8164.2.1012

> Description: | No response received from peer GSN as several messages have timed out. The control path to the GSN is down Probable Cause: Remote GSN is down. Condition Clear Alarm: A starSGSNGtpcPathFailureClear alarm is generated when the GSN becomes reachable.

> Objects: | starSGTPVpnName starSGTPServName starSGTPPeerAdd starSGTPPeerPort starSGSNSelfAddr starSGSNSelfPort

> Object: | starSGSNFtpcPathFailureClear

> Object ID: | enterprises.8164.2.1013

> Description: | The path to the peer GSN which was down is now available. Generated only for GSNs which had previously been down.

> Objects: | starSGTPVpnName starSGTPServName starSGTPPeerAddr

> Object: | starSGSNGtpuPathFailure

> Object ID: | enterprises.8164.2.1014

> Description: | No Response received for Echo Request sent from SGSN. Data path failure detected toward GSN or RNC. Probable Cause: Remote GSN is down. Action to be Taken: Check if peer RNC or GSN is up. Condition Clear Alarm: A starSGSNGtpuPathFailureClear message is generated when the remote GSN becomes available again.

> Objects: | starSGTPVpnName starSGTPNServName starSGTPPeerAddr tarSGTPPeerPort starSGSNSelfAddr starSGSNSelfPort

> Object: | starSGSNGtpuPathFailureClear

> Object ID: | enterprises.8164.2.1015

> Description: | The data path toward the peer GSN or RNC is now available. A path failure clear notification will only be sent for peers which had previously generated a path failure notification.

> Objects: | starSGTPVpnName, starSGTPServName starSGTPPeerAddr starSGTPPeerPort starSGSNSelfAddr starSGSNSelfPor

> Object: | starMTP3LinkOutofService

> Object ID: | enterprises.8164.2.1016

> Description: | Message Transfer Part (MTP3) Link out of service. Probable Cause: Physical link is down, Layer 2 SSCOP/MTP2 is down or link deactivated by operator. Condition Clear Alarm: A starMTP3LinkInService message is generated when the link is restored.

> Objects: | starSS7rdId starSS7MTP3LinkSetId starSS7MTP3LinkId

> Object: | starMTP3LinkinService

> Object ID: | enterprises.8164.2.1017

> Description: | MTP3 link is now in service.

> Objects: | starSS7rdId starSS7MTP3LinkSetId starSS7MP3LinkId

> Object: | starMTP3LinkSetUnAvailable

> Object ID: | enterprises.8164.2.1018

> Description: | MTP3 Linkset Unavailable message. Probable Cause: All links in linkset are down. Linkset deactivated by operator. Condition Clear Alarm: A starMTP3LinkSetAvailable message is generated when the previously down linkset is restored.

> Objects: | starSS7rdId starSS7MTP3LinkSetId

> Object: | starMTP3LinkSetAvailable

> Object ID: | enterprises.8164.2.1019

> Description: | MTP3 linkset is now available

> Objects: | starSS7rdId starSS7MTP3LinkSetId

> Object: | starSCTPAssociationFail

> Object ID: | enterprises.8164.2.1020

> Description: | M3UA SCTP association establishment failure. Probable Cause: Peer is down. Network is down. The endpoint configuration is incorrect at our end. Condition Clear Alarm: A starSCTPAssociationEstablished message is sent when a previously failed association is restored.

> Objects: | starSS7rdId starSS7M3UAPspId starSS7M3UAPsId

> Object: | starSCTPAssociationEstablished

> Object ID: | enterprises.8164.2.1021

> Description: | M3UA SCTP association established successfully. This message is only generated for peers which previously generated an Association Fail message.

> Objects: | starSS7rdId starSS7M3UAPspId starSS7M3UAPsId

> Object: | starSCTPPathDown

> Object ID: | enterprises.8164.2.1022

> Description: | SCTP path is down. Probable Cause: Peer is down. Network to the remote server is down. The endpoint configuration is incorrect at our end. Condition Clear Alarm: A starSCTPPathUp notification is generated when the path is restored.

> Objects: | starSS7rdId starSS7M3UAPspId starSS7M3UAPsId starSS7SCTPPeerAddr starSS7SCTPSelfAddr starSS7SCTPPeerPort starSS7SCTPSelfPort

> Object: | starSCTPPathUp

> Object ID: | enterprises.8164.2.1023

> Description: | SCTP path up. This notification is only generated for peers which had previously generated an SCTP path down notification.

> Objects: | starSS7rdId starSS7M3UAPspId starSS7M3UAPsId starSS7SCTPPeerAddr starSS7SCTPPeerPort starSS7SCTPSelfPort starSS7SCTPSelfAddr

> Object: | starPortDown

> Object ID: | enterprises.8164.2.1024

> Description: | Physical port status is down. Probable Cause: Network is down. Port disconnected. Condition Clear Alarm: A starPortUp notification is generated when the port is restored.

> Objects: | starPortSlot starPortNum starPortType

> Object: | starPortUp

> Object ID: | enterprises.8164.2.1025

> Description: | Physical port is up. This notification is only generated for a physical port with a previous starPortDown notification.

> Objects: | starPortSlot starPortNum starPortType

> Object: | starBSReachable

> Object ID: | enterprises.8164.2.1026

> Description: | The base station that the IMG communicates with is now reachable.

> Objects: | starContextName starASNGWServiceName starBSAddress

> Object: | starBSUnreachable

> Object ID: | enterprises.8164.2.1027

> Description: | The Base Station that the IMG communicates with is not reachable. Probable Cause: The Base Station has failed. Network has connectivity problems. Action to be Taken: If the outage was unplanned, reboot the base station and verify network connectivity. Condition Clear Alarm: A starBSReachable notification is generated when the base station is reconnected.

> Objects: | starContextName starASNGWServiceName starBSAddress

> Object: | starSystemStartup

> Object ID: | enterprises.8164.2.1028

> Description: | The system has completed a reboot/startup

> Objects: | starChassisType starChassisDescription starChassisSWRevision

> Object: | starMTP3PCUnavailable

> Object ID: | enterprises.8164.2.1029

> Description: | MTP3 route to the point code is unavailable. Probable Cause: All links within the linkset become unavailable. Remote peer is down. Condition Clear Alarm: A starMTP3PCAvailable message is generated when the route to the point code is reestablished.

> Objects: | starSS7rdId starSS7Pc starSS7MTP3LinkSetId

> Object: | starMTP3PCAvailable

> Object ID: | enterprises.8164.2.1030

> Description: | MTP3 route to the point code available

> Objects: | starSS7rdId starSS7Pc starSS7MTP3LinkSetId

> Object: | starSS7PCUnavailable

> Object ID: | enterprises.8164.2.1031

> Description: | SS7 point code unavailable. Probable Cause: All MTP3 and M3UA routes to the point code become unavailable. Condition Clear Alarm: A starSS7PCAvailable message is generated when the route is reestablished.

> Objects: | starSS7rdId starSS7Pc

> Object: | starSS7PCAvailable

> Object ID: | enterprises.8164.2.1032

> Description: | SS7 point code available. Probable Cause: one of the M3UA or MTP3 routes is back up. Action to be Taken: No action required.

> Objects: | starSS7rdId starSS7Pc

> Object: | starASNPCServiceStart

> Object ID: | enterprises.8164.2.1033

> Description: | A WiMAX ASN Paging Controller (ASNPC) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starASNPCServiceStop

> Object ID: | enterprises.8164.2.1034

> Description: | A WiMAX ASN Paging Controller (ASNPC) Service has stopped Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration Action to be Taken: If the ASNPC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the ASNPC service is operational Condition Clear Alarm: A starASNPCServiceStart notification will be generated when the service is restarted

> Object: | starDiameterCapabilitiesExchangeFailure

> Object ID: | enterprises.8164.2.1035

> Description: | Capability negotiations have failed and connections are down. Probable cause: Connections have been torn down due to an error in the Capability Exchange Answer received from the peer

> Objects: | starDiameterVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starDiameterCapabilitiesExchangeSuccess

> Object ID: | enterprises.8164.2.1036

> Description: | Diameter server is up. This notification is only generated for a server that has been previously declared unreachable

> Objects: | starDiameterVpnName starDiameterPeerAddr starDiameterEndpointName

> Object: | starSRPConnDown

> Object ID: | enterprises.8164.2.1037

> Objects: | SRP system connection is down and active system is now without a standby and therefore unable to perform an SRP switchover. Probable Cause: Network connectivity problem. Action to be Taken: Verify standby system is operational and check the network connections are up. Clear Condition: A starSRPConnUp notification s generated when condition is cleared.

> Objects: | starContextName starSRPIpAddress

> Object: | starSRPConnUP

> Object ID: | enterprises.8164.2.1038

> Description: | SRP connection is restored. This notification is only generated after a previous connection loss was reported.

> Objects: | starContextName starSRPIpAddress

> Object: | starDiameterIpv6PeerDown

> Object ID: | enterprises.8164.2.1039

> Description: | A diameter peer is down. This diameter peer is reached using an IPv6 address For IPv4-connected diameter peers, a starDiameterPeerDown notification would be generated Problem Cause: The diameter peer has failed, or a network connectivity prevents reaching the peer Condition Clear Alarm: A starDiameterPeerUp notification will be generated when the peer is up

> Objects: | starDiameterVpnName starDiameterPeerAddrIpv6 starDiameterEndpointName

> Object: | starDiameterIpv6PeerUp

> Object ID: | enterprises.8164.2.1040

> Description: | A diameter peer is up. This diameter peer is reached using an IPv6 address. This notification is only generated for peers which have previously been declared down For IPv4-connected diameter peers, a starDiameterPeerUp notification would be generated

> Objects: | starDiameterVpnName starDiameterPeerAddrIpv6 starDiameterEndpointName

> Object: | starIPMSServerUnreachable

> Object ID: | enterprises.8164.2.1041

> Description: | An IPMS server is unreachable Probable Cause: The IPMS server has failed, or a network connectivity issue prevents reaching the server Condition Clear Alarm: A starIPMSServerReachable notification will be generated when the server becomes reachable

> Objects: | starIPMSServerVpnName starIPMSServerAddr

> Object: | starIPMSServerReachable

> Object ID: | enterprises.8164.2.1042

> Description: | An IPMS server is reachable. A starIPMSServerReachable notification is only generated for servers which had previously been declared unreachable

> Objects: | starIPMSServerVpnName starIPMSServerAddr

> Object Group: | starCertShortLifetime

> Object ID: | enterprises.8164.2.1043

> Description: | A certificate is approaching its expiration. The certificate is still valid, but should be updated with a new certificate Action to be Taken: A new certificate should be created and configured on the system

> Object: | starCertExpired

> Object ID: | enterprises.8164.2.1044

> Description: | A certificate has expired. The certificate is no longer valid.

> Objects: | starCertSerialNumber, starCertIssuer, starCertExpiryTime

> Object: | starCertValid

> Object ID: | enterprises.8164.2.1045

> Description: | A valid certificate has been configured. This notification is only generated if a starCertExpired had been previously generated.

> Objects: | starCertSerialNumber, starCertIssuer, starCertExpiryTime

> Object: | starFTPPushFail

> Object ID: | enterprises.8164.2.1046

> Description: | An FTP push operation has failed for the specified file to the specified server.

> Objects: | starFTPServVpnName, starFTPServIpAddr, starFileName, starFileApplication

> Object: | starFTPServSwitch

> Object ID: | enterprises.8164.2.1047

> Description: | An FTP server switchover has been performed; that is, the system has determined that an external FTP server is unreachable, and is not using an alternate FTP server.

> Objects: | starFTPServVpnName, starFTPServIpAddr, starFTPServIpAddr, starFileApplication

> Object: | starSDHSectionDown

> Object ID: | enterprises.8164.2.1048

> Description: | SDH interface on this port is down.starSDHOperState identifies the cause. Probable Cause: Not shown Action to be taken: Not shown Clear Alarm: Cleared by a starSDHUp notification

> Objects: | starSDHslot starSDHport starSDHOperState

> Object: | starSDHSectionUp

> Object ID: | enterprises.8164.2.1049

> Description: | SDH interface on this port is now up. This notification is only generated after starSDHSectionDown was previously generated.

> Objects: | starSDHSlot starSDHPort

> Object: | starSDHPathHopDown

> Object ID: | enterprises.8164.2.1050

> Description: | The identified SDH Path is down. The value of starSDHPathOperState identifies the specific failure bits Probable Cause: None given. Action to be Taken: None given. Condition Clear Alarm: This condition is cleared by a starSDHPathUp notification.

> Objects: | starSDHPathSlot starSDHPathPort starSDHPathNum starSDHPathOperState

> Object: | starSDHPathHopUp

> Object ID: | enterprises.8164.2.1051

> Description: | The identified SDH path on this port is now up. Notification is only generated if a previous SDHPathHop down message was generated

> Objects: | starE1TribSlot starE1TribPort starE1TribPath starE1TribNum

> Object: | starSDHLopDown

> Object ID: | enterprises.8164.2.1052

> Description: | The identified E1 tributary on this port is down.The value of starE1TribOperStateLOP identifies the specific failure bits. Probable Cause: Not known Condition CLear Alarm: A starSDHLopUp notification is generated

> Objects: | starE1TribSlot starE1TribPort starE1TribPath starE1TribTug2 starE1TribTu12 starE1TribOperStateLOP

> Object: | starSDHLopUp

> Object ID: | enterprises.8164.2.1053

> Description: | The identified E1tributary on this port is up. An SDHLopUpnotification is only generated in response to a previous SDHLopDown notification.

> Objects: | startE1TribSlot starE1TribPort starE1TribPath starE1TribTug2 starE1TribTu12

> Object: | starSS7PCCongested

> Object ID: | enterprises.8164.2.1056

> Description: | SS7 Point code is congested, all the routes to this point-code is congested. Possible reason: All the routes (both M3UA and MTP3) to this Point Code have become congested. Condition Clear Alarm: A starSS7PCCongestionCleared notification will be generated when the congestion gets cleared for any one of the routes.

> Objects: | starSS7rdId starSS7Pc

> Object: | starSS7PCCongestionCleared

> Object ID: | enterprises.8164.2.1057

> Description: | SS7 Point code Congestion gets cleared, one of the routes to this point-code is cleared from congestion. Possible reason: One of the routes (either M3UA or MTP3) to this Point Code has resumed from congestion. starSS7PCCongestionCleared is generated only when a previous starSS7PCCongested is generated.

> Objects: | starSS7rdId starSS7Pc

> Object: | starPHSGWServiceStart

> Object ID: | enterprises.8164.2.1058

> Description: | A PHS-GW Service has started. Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starPHSGWServiceStop

> Object ID: | enterprises.8164.2.1059

> Description: | A PHS-GW Service has stopped. Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the PHS-GW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure.

> Objects: | starServiceVpnName starServiceServName

> Object: | starGPRSServiceStart

> Object ID: | enterprises.8164.2.1060

> Description: | A GPRS Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starGPRSServiceStop

> Object ID: | enterprises.8164.2.1061

> Description: | A GPRS Service has stopped. Probable Cause: In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration.This can also happen due to some misconfiguration of the service parameters. Action to be Taken: If the GPRS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the GPRS service is operational. Condition Clear Alarm: A starGPRSServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starGPRSNseDown

> Object ID: | enterprises.8164.2.1062

> Description: | Network Service Entity (NSE) is down. Probable Cause: The Last NSVC (Network Service virtual circuit) in the NSE is down. Condition Clear Alarm: A starGPRSNseUp will be generated when at least one NSVC in the NSE comes up.

> Objects: | starGPRSNsei

> Object: | starGPRSNseUp

> Object ID: | enterprises.8164.2.1063

> Description: | Network Service Entity (NSE) is up. Probable Cause: The First NSVC (Network Service virtual circuit) in the NSE is up. starGPRSNseUp is generated only when a previous starGPRSNseDown has been generated.

> Objects: | starGPRSNsei

> Object Group: | starGPRSNsvcDown

> Object ID: | enterprises.8164.2.1064

> Description: | Network Service Entity Virtual Circuit (NSVC) is down. Probable Cause: NS_ALIVE heartbeat messages sent from the Serving GPRS support Node (SGSN) were not acknowledged by the Base Station Subsystem (BSS) for a configured number of maximum retries. This trap is generated only when an NSVC goes down due to reasons other than physical port failure. A separate trap is generated for a physical port failure event. Condition Clear Alarm: A starGPRSNsvcUp will be generated when the NSVC comes up.

> Objects: | starGPRSNsei starGPRSNsvci

> Object Group: | starGPRSNsvcUp

> Object ID: | enterprises.8164.2.1065

> Description: | An Network Service Entity Virtual Circuit (NSVC) comes up. An starGPRSNsvcUp trap is generated only when a previous starGPRSNsvcDown was generated.

> Objects: | starGPRSNsei starGPRSNsvci

> Object Group: | starGPRSBvcDown

> Object ID: | enterprises.8164.2.1066

> Description: | Base Station Subsystem (BSS) GPRS (General Packet Radio Service) Protocol (BSSGP) Virtual Circuit (BVC) is Down. Probable Cause: ALL Network Service Entity Virtual Circuit (NSVC) associated with this BVC are down Condition Clear Alarm: A starGPRSBvcUp will be generated when the BVC is available.

> Objects: | starGPRSNsei starGPRSBvci

> Object Group: | starGPRSBvcUp

> Object ID: | enterprises.8164.2.1067

> Description: | Base Station Subsystem (BSS) GPRS ((General Packet Radio Service) Protocol (BSSGP) Virtual Circuit (BVC) is Up. Probable Cause: At least one NSVC associated with the BVC becomes available. starGPRSBvcUp is generated only when a previous starGPRSBvcDown has been generated.

> Objects: | starGPRSNsei starGPRSBvci

> Object: | starSDHE1TribDown

> Object ID: | enterprises.8164.2.1068

> Description: | The identified E1 tributary on this port is down. Possible Cause: None given Condition Clear Alarm: The condition is cleared when a starSDHE1TribUp message is generated.

> Objects: | starE1TribSlot starE1TribPort starE1TribPath startE1TribTug2 starE1TribTu12 starE1TribOperState

> Object: | starSDHE1TribUp

> Object ID: | enterprises.8164.2.1069

> Description: | The identified E1 tributary on this port is up.

> Objects: | starE1TribSlot starE1TribPort starE1TribPath startE1TribTug2 starE1TribTu12

> Object: | starSDHFractE1LMIDown

> Object ID: | enterprises.8164.2.1070

> Description: | The identified fractional E1 tributary on this port is down. Possible Cause: None given. Condition Clear Alarm: The condition is cleared when a starSDHFractE1LMIUp message is generated.

> Objects: | starFractE1TribSlot starFractE1TribPort starFractE1TribPath starFractE1TribTug2 starFractE1TribTu12 starFractE1TribTimeslots

> Object: | starSDHFractE1LMIUp

> Object ID: | enterprises.8164.2.1071

> Description: | The identified fractional E1 tributary on this port is up.

> Objects: | starFractE1TribSlot starFractE1TribPort starFractE1TribPath starFractE1TribTug2 starFractE1TribTu12

> Object: | starPHSPCServiceStart

> Object ID: | enterprises.8164.2.1072

> Description: | A PHS-PC Service has started. Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starPHSPCServiceStop

> Object ID: | enterprises.8164.2.1073

> Description: | A PHS-PC Service has stopped. Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the PHS-PC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure.

> Objects: | starServiceVpnName starServiceServName

> Object: | starM3UAPSPCongested

> Object ID: | enterprises.8164.2.1074

> Description: | Peer Server Process (PSP) link is congested when the queue size rises above the threshold limit. Possible Cause: No SCTP acknowledgement from peer because of packet loss, or the acknoledgement has zero window size. Condition Clear Alarm: The condition is cleared when a starM3UAPSPCongestionCleared message is generated.

> Objects: | starSS7rdId starSS7M3UAPsId starSS7M3UAPsId starSS7M3UAPspId starSS7Pc

> Object: | starM3UAPSPCongestionCleared

> Object ID: | enterprises.8164.2.1075

> Description: | Peer Server Process (PSP) link congestion gets cleared when the congestion queue size goes below the threshold limit.

> Objects: | starSS7rdId starSS7M3UAPsId starSS7M3UAPsId starSS7M3UAPspId starSS7Pc

> Object: | starStorageFailed

> Object ID: | enterprises.8164.2.1076

> Description: | The specified storage device has failed. This storage device is now out of service and cannot be used to store additional data. This notification is currently only generated for failures on the hard drive attached to the SMC card. Probable Cause: A hardware failure on the device; a hardware failure on the card to which the device is attached. Action to be Taken: Replace the card Condition Clear Alarm: A starCardRemoved notification will be generated when the card is removed from the chassis.

> Objects: | starStorageSlot starStorageName

> Object: | starRaidFailed

> Object ID: | enterprises.8164.2.1077

> Description: | The specified raid array has failed. The raid array can no longer be used to store data. Probable Cause: Hardware failure(s) on the devices within the raid array; Hardware failure(s) on the card(s) to which the devices are attached; the removal of the cards containing devices in the array; operator action which disabled the raid array. Condition Clear Alarm: a starRaidStarted notification will be generated when the raid array is online.

> Objects: | starStorageName

> Object: | starRaidStarted

> Object ID: | enterprises.8164.2.1078

> Description: | The specific raid array has resumed operation. This notification is only generated if a starRaidFailed notification was previously generated for this array.

> Objects: | starStorageName

> Object: | starRaidDegraded

> Object ID: | enterprises.8164.2.1079

> Description: | The specified raid array is running in a degraded state. This typically means one of the member devices has failed or become unavailable. The raid array continues to function and can read/store data, but may not be operating in a redundant manner. Probable Cause: Hardware failure(s) on the devices within the raid array; Hardware failure(s) on the card(s) to which the devices are attached; the removal of the cards containing devices in the array; operator action which disabled the raid array. Condition Clear Alarm: a starRaidRecovered notification will be generated when the raid array is fully recovered.

> Objects: | starStorageName starStorageSlot starStorageName

> Object: | starRaidRecovered

> Object ID: | enterprises.8164.2.1080

> Description: | The specific raid array has been recovered and is running in its normal, redundant state. This notification is only generated if a starRaidDegraded notification was previously generated for this array.

> Objects: | starStorageName starStorageSlot starStorageName

> Object: | starPDGServiceStart

> Object ID: | enterprises.8164.2.1101

> Description: | A PDG Service has started Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starPDGServiceStop

> Object ID: | enterprises.8164.2.1102

> Description: | A PDG Service has stopped. Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs) to support the running configuration. Action to be Taken: If the PDG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the PDG service is operational. Condition Clear Alarm: A starPDGServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starASNPCServiceStart

> Object ID: | enterprises.8164.2.1103

> Description: | A WiMAX ASN Paging Controller (ASNPC) Service has started

> Objects: | starServiceVpnName, starServiceServName

> Object: | starPDGServiceStop

> Object ID: | enterprises.8164.2.1104

> Description: | A PDG Service has stopped.

> Objects: | starServiceVpnName, starServiceServName

> Object: | starDiameterIpv6PeerDown

> Object ID: | enterprises.8164.2.1105

> Description: | A diameter peer is down.

> Objects: | starDiameterVpnName, starDiameterPeerAddrIpv6, starDiameterEndpointName

> Object: | starDiameterIpv6PeerUp

> Object ID: | enterprises.8164.2.1106

> Description: | A diameter peer is up.

> Objects: | starDiameterVpnName, starDiameterPeerAddrIpv6, starDiameterEndpointName

> Object: | starIPMSServerUnreachable

> Object ID: | enterprises.8164.2.1107

> Description: | An IPMS server is unreachable.

> Objects: | starIPMSServerVpnName, starIPMSServerAddr

> Object: | starIPMSServerReachable

> Object ID: | enterprises.8164.2.1108

> Description: | An IPMS server is reachable. A starIPMSServerReachable notification is only generated for servers which had previously been declared unreachable.

> Objects: | starIPMSServerVpnName, starIPMSServerAddr

> Object: | starCertShortLifetime

> Object ID: | enterprises.8164.2.1109

> Description: | A certificate is approaching its expiration. The certificate is still valid, but should be updated with a new certificate.

> Objects: | starCertSerialNumber, starCertIssuer, starCertExpiryTime

> Object: | starServiceLossPTACsClear

> Object ID: | enterprises.8164.2.1110

> Description: | Service Loss condition is no longer valid for PAC/PSC/TACs

> Objects: | starCardMode

> Object: | starServiceLossLCClear

> Object ID: | enterprises.8164.2.1111

> Description: | Service Loss condition is no longer valid for LC

> Objects: | starCardMode

> Object: | starCscfSessResourceCongestion

> Object ID: | enterprises.8164.2.1114

> Description: | A congestion condition has occurred at Session Manager for Cscf Service Probable Cause: This is the result of an operator-configured congestion threshold being reached for Cscf Service at Session Manager. This can be due to high usage of the resource being monitored which indicates that the IMG is reaching its peak capacity, or could be caused by the incorrect configuration of the congestion thresholds Actions to be Taken:Verify that the congestion thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online. This system is cleared when the use of the specific resource falls below the configured limit. Condition Clear Alarm: A starCscfSessResourceCongestionClear notification is sent when there are no congestion conditions for cscf service in that Session Manager Instance

> Objects: | starSmgrId starCongestionPolicy starCscfSessCongestionResourceType

> Object: | starCscfSessResourceCongestionClear

> Object ID: | enterprises.8164.2.1115

> Description: | A congestion condition has cleared at Session Manager for Cscf service

> Objects: | starSmgrId

> Object: | starOSPFv3NeighborDown

> Object ID: | enterprises.8164.2.1116

> Description: | An OSPFv3 neighbor is down

> Objects: | starContextName starInterfaceName starInterfaceIPAddress starOSPFNeighborRouterID starOSPFFromState starOSPFToState

> Object: | starOSPFv3NeighborFull

> Object ID: | enterprises.8164.2.1117

> Description: | An OSPFv3 neighbor is full. A starOSPFv3NeighborFull notification is only sent for neighbors which had previous been declared down via a starOSPFv3NeighborDown notification

> Objects: | starContextName starInterfaceName starInterfaceIPAddress starOSPFNeighborRouterID

> Object: | starServiceLossSPIOClear

> Object ID: | enterprises.8164.2.1118

> Description: | Service Loss condition is no longer valid for SPIO

> Objects: | starCardMode

> Object: | starCertExpired

> Object ID: | enterprises.8164.2.1044

> Description: | A certificate has expired. The certificate is no longer valid.

> Objects: | starCertSerialNumber, starCertIssuer, starCertExpiryTime

> Object: | starCertValid

> Object ID: | enterprises.8164.2.1045

> Description: | A valid certificate has been configured. This notification is only generated if a starCertExpired had been previously generated.

> Objects: | starCertSerialNumber, starCertIssuer, starCertExpiryTime

> Object: | starFTPPushFail

> Object ID: | enterprises.8164.2.1046

> Description: | An FTP push operation has failed for the specified file to the specified server.

> Objects: | starFTPServVpnName, starFTPServIpAddr, starFileName, starFileApplication

> Object: | starFTPServSwitch

> Object ID: | enterprises.8164.2.1047

> Description: | An FTP server switchover has been performed; that is, the system has determined that an external FTP server is unreachable, and is not using an alternate FTP server.

> Objects: | starFTPServVpnName, starFTPServIpAddr, starFTPServIpAddr, starFileApplication

> Object: | starPGWServiceStart

> Object ID: | enterprises.8164.2.1081

> Description: | A Packet Data Network Gateway (PGW) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starPGWServiceStop

> Object ID: | enterprises.8164.2.1082

> Description: | A Packet Data Network Gateway (PGN) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the PGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the PGW service is operational Condition Clear Alarm: A starPGWServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starSGWServiceStart

> Object ID: | enterprises.8164.2.1083

> Description: | A Serving Gateway (SGW) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starSGWServiceStop

> Object ID: | enterprises.8164.2.1084

> Description: | A Serving Gateway (SGW) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the SGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the SGW service is operational Condition Clear Alarm: A starSGWServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starEGTPServiceStart

> Object ID: | enterprises.8164.2.1085

> Description: | An Evolved GPRS Tunneling Protocol (EGTP) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starEGTPServiceStop

> Object ID: | enterprises.8164.2.1086

> Description: | An Evolved GPRS Tunneling Protocol (EGTP) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the EGTP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the EGTP service is operational Condition Clear Alarm: A starEGTPServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starLMAServiceStart

> Object ID: | enterprises.8164.2.1087

> Description: | A Local Mobility Anchor (LMA) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object Group: | starLMAServiceStop

> Object ID: | enterprises.8164.2.1088

> Description: | A Local Mobility Anchor (LMA) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the LMA service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the LMA service is operational Condition Clear Alarm: A starLMAServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starMAGServiceStart

> Object ID: | enterprises.8164.2.1089

> Description: | A Mobile Access Gateway (MAG) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starMAGServiceStop

> Object ID: | enterprises.8164.2.1090

> Description: | A MAG Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the MAG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the MAG service is operational Condition Clear Alarm: A starMAGServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starMMEServiceStart

> Object ID: | enterprises.8164.2.1091

> Description: | A Mobility Management Entity (MME) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starMMEServiceStop

> Object ID: | enterprises.8164.2.1092

> Description: | A Mobility Management Entity (MME) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the MME service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the MME service is operational Condition Clear Alarm: A starMMEServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starHSGWServiceStart

> Object ID: | enterprises.8164.2.1093

> Description: | A HRPD Serving Gateway (HSGW) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starHSGWServiceStop

> Object ID: | enterprises.8164.2.1094

> Description: | A HRPD Serving Gateway (HSGW) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the HSGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the HSGW service is operational Condition Clear Alarm: A starHSGWServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starCPUBusyClear

> Object ID: | enterprises.8164.2.1095

> Description: | The CPU is no longer busy

> Objects: | starCPUSlot starCPUNumber

> Object: | starCPUMemoryLowClear

> Object ID: | enterprises.8164.2.1096

> Description: | The CPU is no longer experiencing a low memory condition

> Objects: | starCPUSlot starCPUNumber

> Object: | starFNGServiceStart

> Object ID: | enterprises.8164.2.1097

> Description: | A FNG Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starFNGServiceStop

> Object ID: | enterprises.8164.2.1098

> Description: | A FNG Service has stopped Probable Cause: This is typically caused by operator invention. In rare cases it can be caused by the loss of resources (PACs) to support the running configuration Action to be Taken: If the FNG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the FNG service is operational Condition Clear Alarm: A starFNGServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starManagerRestart

> Object ID: | enterprises.8164.2.1099

> Description: | The identified manager task has been restarted

> Objects: | starTaskFacilityName starTaskInstance starTaskCard starTaskCPU

> Object: | starConfigurationUpdate

> Object ID: | enterprises.8164.2.1100

> Description: | The configuration of the chassis has been changed. This notification is generated based on a periodic polling of the chassis, it is not real-time generated based on individual changes. The configuration change could have been made via CLI sessions, CORBA management operations, or other methods This notification is not generated by default; it is only generated if the configuration polling mechanism is specifically enabled

> Object Group: | starEgtpcPathFailure

> Object ID: | enterprises.8164.2.1112

> Description: | EGTP Control Path Failure. No response received for GTPV2 request sent from MME or SGW or PGW Possibe reason: Remote peer MME or SGW or PGW is down Condition Clear Alarm: A StarEgtpcPathFailureClear notification will be generated when the control path to the remote peer MME or SGW or PGW becomes available

> Objects: | starEGTPVpnName starEGTPServName starEGTPInterfaceType starEGTPSelfAddr starEGTPPeerAddr starEGTPPeerOldRstCnt starEGTPPeerNewRstCnt starEGTPPeerSessCnt starEGTPFailureReason

> Object: | starEgtpcPathFailureClear

> Object ID: | enterprises.8164.2.1113

> Description: | EGTP Control Path Failure condition is no longer valid

> Objects: | starEGTPVpnName starEGTPServName starEGTPInterfaceType starEGTPSelfAddr starEGTPPeerAddr

> Object: | starServiceLossSPIOClear

> Object ID: | enterprises.8164.2.1118

> Description: | Service Loss condition is no longer valid for SPIO

> Objects: | starCardMode

> Object: | starEgtpuPathFailure

> Object ID: | enterprises.8164.2.1119

> Description: | No response received for GTP-U ECHO requests. Data path failure detected towards peer EPC Node Check if the peer RNC or GSN is up Possible reason: Remote EPC node is down Condition Clear Alarm: A starEgtpuPathFailureClear notification will be generated when the data path towards the peer node is available

> Objects: | starEGTPVpnName starEGTPServName starEGTPSelfAddr starEGTPPeerAddr starEGTPSelfPort starEGTPPeerPort starEGTPPeerSessCnt

> Object: | starEgtpuPathFailureClear

> Object ID: | enterprises.8164.2.1120

> Description: | The data path to the peer EPC node which was down is now available A starEgtpuPathFailureClear notification is only generated for nodes which had previously generated a starEgtpuPathFailure notification

> Objects: | starEGTPVpnName starEGTPServName starEGTPSelfAddr starEGTPPeerAddr starEGTPSelfPort starEGTPPeerPort

> Object: | starStorageServerCDRLoss

> Object ID: | enterprises.8164.2.1121

> Description: | GTPP Storage Server is experiencing CDR Loss greater than the configured threshold value at the GSS.

> Objects: | starSessGGSNVpnName starSessGGSNPeerAddr starGSSCDRLossConfigured starGSSCDRLossMeasured starGSSClusterName starGSSClusterNodeName

> Object: | starHNBGWServiceStart

> Object ID: | enterprises.8164.2.1122

> Description: | A Home Node B Gateway (HNB GW) Service has started Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object Group: | starHNBGWServiceStop

> Object ID: | enterprises.8164.2.1123

> Description: | A Home Node B Gateway (PGN) Service has stopped Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (PSCs) to support the running configuration Action to be Taken: If the HNB GW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PSCs are present and running in the system. Check the crash logs for an indication of a software failure Clear Condition: Verify that the HNB GW service is operational Condition Clear Alarm: A starHNBGWServiceStart notification will be generated when the service is restarted

> Objects: | starServiceVpnName starServiceServName

> Object: | starSystemReboot

> Object ID: | enterprises.8164.2.1124

> Description: | The system has rebooted by the operator. If successful, a subsequent starSystemStartup trap is typically generated Action to be Taken: No action required. If the reboot was not scheduled the admin logs can be examined to determine who invoked the reboot operation

> Objects: | starChassisType starChassisDescription starChassisSWRevision

> Object: | starLicenseAboutToExpire

> Object ID: | enterprises.8164.2.1125

> Description: | A license is about to expire Action to be Taken: A new license should be created and configured on the system before the grace period is over

> Objects: | starLicenseKey starLicenseExpiryDate starLicenseDaysRemaining

> Object: | starLicenseExpired

> Object ID: | enterprises.8164.2.1126

> Description: | A license is in the grace period and should be updated with a new license Action to be Taken: A new license should be created and configured on the system

> Objects: | starLicenseKey starLicenseExpiryDate starLicenseDaysafterexpiry

> Object: | starGSServiceStart

> Object ID: | enterprises.8164.2.1135

> Description: | A GS Service has started. Action to be Taken: No action required

> Objects: | starServiceVpnName starServiceServName

> Object: | starGSServiceStop

> Object ID: | enterprises.8164.2.1136

> Description: | A GS Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the GS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the GS service is operational. Condition Clear Alarm: A starGSServiceStart notification will be generated when the service is restarted"

> Objects: | starServiceVpnName starServiceServName

> Object: | starMAPServiceStart

> Object ID: | enterprises.8164.2.1137

> Description: | A MAP Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starMAPServiceStop

> Object ID: | enterprises.8164.2.1138

> Description: | A MAP Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the MAP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the MAP service is operational. Condition Clear Alarm: A starMAPServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starIUPSServiceStart

> Object ID: | enterprises.8164.2.1139

> Description: | An IUPS Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starIUPSServiceStop

> Object ID: | enterprises.8164.2.1140

> Description: | An IUPS Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the IUPS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the IUPS service is operational. Condition Clear Alarm: A starIUPSServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> Object: | starSGTPServiceStart

> Object ID: | enterprises.8164.2.1141

> Description: | A SGTP Service has started. Action to be Taken: No action required.

> Objects: | starServiceVpnName starServiceServName

> Object: | starSGTPServiceStop

> Object ID: | enterprises.8164.2.1142

> Description: | A SGTP Service has stopped. Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of resources (PACs/PSCs) to support the running configuration. Action to be Taken: If the SGTP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure. Clear Condition: Verify that the SGTP service is operational. Condition Clear Alarm: A starSGTPServiceStart notification will be generated when the service is restarted.

> Objects: | starServiceVpnName starServiceServName

> starentMIB(8164).starentMIBConformance(3)
> starentMIB(8164).starentMIBConformance(3).starentMIBGroups(1)

> Object Group: | starChassisGroup

> Object ID: | enterprises.8164.3.1.1

> Description: | A collection of objects providing information about a chassis.

> Description: | starChassisCriticalCO starChassisMajorCO starChassisMinorCO starChassisAudibleAlarm starChassisUTCTime starChassisLocalTime starChassisType starChassisAction starTimeTicks starChassisDescription starChassisSWRevision starChassisPeakMemoryUsage starSlotType starCardType starCardOperState starCardAdminState starCardRevision starCardLastStateChange starCardMode starCardPacStandbyPriority starCardLock starCardHaltIssued starCardRebootPending starCardUsable starCardSinglePOF starCardAttachment starCardTemperature starSlotNumPorts starSlotAction starSlotVoltageState starSlotNumCPU starSlotMappingType starSlotMappingRCCNum starSlotMappingToSlot starFanLocation starFanStatus starFanSpeed starLogCurSize starLogMaxSize starLogText starPowerState starCPUUser starCPUSystem starCPUIdle starCPUIO starCPUIRQ starCPULoad1Min starCPULoad5Min starCPULoad15Min starCPUMemTotal starCPUMemUsed starCPUNumProcesses starCPUMemCached starSessInProgCalls starSessInProgActiveCalls starSessInProgDormantCalls starSessInProgArrived starSessInProgLCPNeg starSessInProgLCPUp starSessInProgAuthenticating starSessInProgAuthenticated starSessInProgIPCPUp starSessInProgSIPConn starSessInProgMIPConn starSessInProgDisc starSessMgrCount starSessTtlArrived starSessTtlRejected starSessTtlConnected starSessTtlAuthSucc starSessTtlAuthFail starSessTtlLCPUp starSessTtlIPCPUp starSessTtlSrcViol starSessTtlKeepFail starSessTtlOctForwarded starSessTtlRPRegAccept starSessTtlRPRegAcceptInterPDSN starPPPCurrSessions starSessTtlTxBytes starSessTtlRxBytes starSessTtlSIPTxBytes starSessTtlSIPRxBytes starSessTtlMIPTxBytes starSessTtlMIPRxBytes starSessTtlOctForwardedGB starAAAMgrCount starAAATtlRequests starAAATtlAuthRequests starAAATtlAcctRequests starAAACurRequests starAAACurAuthRequests starAAACurAcctRequests starAAATtlAcctSess starAAACurAcctSess starAAATtlAuthSuccess starAAATtlAuthFailure starA11MgrCount starA11TtlArrived starA11TtlRejected starA11TtlDemultiplexed starA11TtlDereg starA11CurActive starHAMgrCount starHATtlArrived starHATtlRejected starHATtlDemultiplexed starHATtlDereg starHACurActive starFAMgrCount starFATtlArrived starFATtlRejected starFATtlDemultiplexed starFATtlDereg starFACurActive starServiceVpnName starServiceServName starServiceSubLimit starServiceSubCurrent starServiceType starServiceFAIpAddr starServiceHAIpAddr starCLITtyname starCLIPrivs starCLIType starCLIRemoteIPAddr starCLIContext starTaskFacilityName starTaskCard starTaskCPU starPPPStatVpnName starPPPStatServName starPPPStatInit starPPPStatReneg starPPPStatSuccess starPPPStatFailed starPPPStatReleased starPPPStatReleasedLocal starPPPStatReleasedRemote starPPPStatLcpFailMaxRetry starPPPStatLcpFailOption starPPPStatIpcpFailMaxRetry starPPPStatIpcpFailOption starPPPStatCcpFail starPPPStatAuthFail starPPPStatLcpEntered starPPPStatAuthEntered starPPPStatIpcpEntered starPPPStatRenegPdsn starPPPStatRenegMobil starPPPStatRenegAddrMismatch starPPPStatRenegOther starPPPStatChapAuthAttempt starPPPStatPapAuthAttempt starPPPStatMSChapAuthAttempt starPPPStatChapAuthFail starPPPStatPapAuthFail starPPPStatMSChapAuthFail starPPPStatStacComp starPPPStatMppcComp starPPPStatDeflComp starPPPStatFscErrs starPPPStatUnknProto starPPPStatBadAddr starPPPStatBadCtrl starPPPStatVjComp starPPPStatDiscLcpRemote starPPPStatDiscRpRemote starPPPStatDiscAdmin starPPPStatDiscIdleTimeout starPPPStatDiscAbsTimeout starPPPStatDiscPPPKeepalive starPPPStatDiscNoResource starPPPStatDiscMisc starPPPStatFailedReneg starPPPStatLcpFailUnknown starPPPStatIpcpFailUnknown starPPPStatAuthAbort starPPPStatLowerLayerDisc starPPPStatLcpSuccess starPPPStatAuthSuccess starPPPStatRenegLowerLayerHandoff starPPPStatRenegParamUpdate starPPPStatChapAuthSuccess starPPPStatPapAuthSuccess starPPPStatMSChapAuthSuccess starPPPStatChapAuthAbort starPPPStatPapAuthAbort starPPPStatMSChapAuthAbort starPPPStatSessSkipAuth starPPPStatNegComp starPPPStatCCPNegFailComp starPPPStatDiscLocalLowerLayer starPPPStatDiscAddFlowFail starPPPStatDiscMaxRetriesLCP starPPPStatDiscMaxRetriesIPCP starPPPStatDiscMaxSetupTimer starPPPStatDiscInvalidDestVpn starPPPStatDiscOptNegFailLCP starPPPStatDiscOptNegFailIPCP starPPPStatDiscNoRemoteIpAddr starPPPStatDiscCallTypeDetectFail starPPPStatDiscRemoteDiscUpLayer starPPPStatDiscLongDuraTimeout starPPPStatDiscAuthFail starPPPStatLCPEchoTotalReq starPPPStatLCPEchoReqResent starPPPStatLCPEchoRepRecved starPPPStatLCPEchoReqTimeout starPPPStatRecvErrBadCtrlField starPPPStatRecvErrBadPacketLen starPPPStatRemoteTerm starPPPStatMiscFail starMIPHAStatVpnID starMIPHAStatVpnName starMIPHAStatServName starMIPHAStatDisconnects starMIPHAStatExpiry starMIPHAStatDereg starMIPHAStatAdminDrop starMIPHAStatRegRecvTotal starMIPHAStatRegRecvInitial starMIPHAStatRegRecvRenew starMIPHAStatRegRecvDereg starMIPHAStatRegAcceptTotal starMIPHAStatRegAcceptReg starMIPHAStatRegAcceptRenew starMIPHAStatRegAcceptDereg starMIPHAStatRegDeniedTotal starMIPHAStatRegDeniedInitial starMIPHAStatRegDeniedRenew starMIPHAStatRegDeniedDereg starMIPHAStatRegReplyTotal starMIPHAStatRegReplyAcceptReg starMIPHAStatRegReplyAcceptDereg starMIPHAStatRegReplyDenied starMIPHAStatRegReplyBadReq starMIPHAStatRegReplyMismatchID starMIPHAStatRegReplyAdminProhib starMIPHAStatRegReplyUnspecErr starMIPHAStatRegReplyNoResource starMIPHAStatRegReplyMnAuthFail starMIPHAStatRegReplyFAAuthFail starMIPHAStatRegReplySimulBind starMIPHAStatRegReplyUnknownHA starMIPHAStatRegReplyRevTunUnav starMIPHAStatRegReplyRevTunMand starMIPHAStatRegReplyEncapUnav starMIPHAStatRegReplySendError starMIPHAStatFARevocations starMIPHAStatRegAcceptHO starMIPHAStatRegDeniedHO starMIPHAStatRegDiscardTotal starMIPFAStatVpnID starMIPFAStatVpnName starMIPFAStatServName starMIPFAStatAdvertSend starMIPFAStatDiscExpiry starMIPFAStatDiscDereg starMIPFAStatDiscAdmin starMIPFAStatAuthAttempt starMIPFAStatAuthSuccess starMIPFAStatAuthFailure starMIPFAStatRegRecvTotal starMIPFAStatRegRecvInitial starMIPFAStatRegRecvRenewal starMIPFAStatRegRecvDereg starMIPFAStatRegAcceptTotal starMIPFAStatRegAcceptInitial starMIPFAStatRegAcceptRenewal starMIPFAStatRegAcceptDereg starMIPFAStatRegDenTotal starMIPFAStatRegDenInitial starMIPFAStatRegDenRenewal starMIPFAStatRegDenDereg starMIPFAStatRegDiscardTotal starMIPFAStatRegDiscInitial starMIPFAStatRegDiscardRenewal starMIPFAStatRegDiscardDereg starMIPFAStatRegRelayedTotal starMIPFAStatRegRelayedInitial starMIPFAStatRegRelayedRenewal starMIPFAStatRegRelayedDereg starMIPFAStatRegAuthFailTotal starMIPFAStatRegAuthFailInitial starMIPFAStatRegAuthFailRenewal starMIPFAStatRegAuthFailDereg starMIPFAStatRegDenPDSNTotal starMIPFAStatRegDenPDSNInitial starMIPFAStatRegDenPDSNRenewal starMIPFAStatRegDenPDSNDereg starMIPFAStatRegDenHATotal starMIPFAStatRegDenHAInitial starMIPFAStatRegDenHARenewal starMIPFAStatRegDenHADereg starMIPFAStatRegDenPDSNUnspec starMIPFAStatRegDenPDSNTimeout starMIPFAStatRegDenPDSNAdmin starMIPFAStatRegDenPDSNResources starMIPFAStatRegDenPDSNMnAuth starMIPFAStatRegDenPDSNHAAuth starMIPFAStatRegDenDSNTooLong starMIPFAStatRegDenPDSNBadReq starMIPFAStatRegDenPDSNEncapUnav starMIPFAStatRegDenPDSNRevTunUnav starMIPFAStatRegDenPDSNRevTunMand starMIPFAStatRegDenHAFAAuth starMIPFAStatRegDenHABadReq starMIPFAStatRegDenHAMismatchID starMIPFAStatRegDenHASimulBind starMIPFAStatRegDenHAUnknownHA starMIPFAStatRegDenHARevRunUnavail starMIPFAStatRegRplRcvTotal starMIPFAStatRegRplRcvTotalRly starMIPFAStatRegRplRcvErrors starMIPFAStatRegRplRcvInitial starMIPFAStatRegRplRcvInitialRly starMIPFAStatRegRplRcvRenewal starMIPFAStatRegRplRcvRenewalRly starMIPFAStatRegRplRcvDereg starMIPFAStatRegRplRcvDeregRly starMIPFAStatRegRplSentTotal starMIPFAStatRegRplSentAcceptReg starMIPFAStatRegRplSentAcceptDereg starMIPFAStatRegRplSentBadReq starMIPFAStatRegRplSentTooLong starMIPFAStatRegRplSentMnAuthFail starMIPFAStatRegRplSentHAAuthFail starMIPFAStatRegRplSentAdminProhib starMIPFAStatRegRplSentNoResources starMIPFAStatRegRplSentRevTunUnav starMIPFAStatRegRplSentRevTunMand starMIPFAStatRegRplSentSendErrors starMIPFAStatRegDenPDSNBadReply starMIPFAStatRegDenPDSNMissNAI starMIPFAStatRegDenPDSNMissHomeAgent starMIPFAStatRegDenPDSNMissHomeAddr starMIPFAStatRegDenPDSNUnknChallenge starMIPFAStatRegDenPDSNMissChallenge starMIPFAStatRegDenPDSNStaleChallenge starMIPFAStatRegDenPDSNMNTooDistant starMIPFAStatRegDenPDSNStyleUnavail starMIPFAStatRegDenPDSNHANetUnreach starMIPFAStatRegDenPDSNHAHostUnreach starMIPFAStatRegDenPDSNHAPortUnreach starMIPFAStatRegDenPDSNHAUnreach starMIPFAStatRegDenPDSNInvCOA starMIPFAStatRegReqSentInitTotal starMIPFAStatRegReqSentInitResend starMIPFAStatRegReqSentRenewTotal starMIPFAStatRegReqSentRenewResend starMIPFAStatRegReqSentDeregTotal starMIPFAStatRegReqSentDeregResend starMIPFAStatRegRplSentMNTooDistant starMIPFAStatRegRplSentInvCOA starMIPFAStatRegRplSentHANetUnreach starMIPFAStatRegRplSentHAHostUnreach starMIPFAStatRegRplSentHAPortUnreach starMIPFAStatRegRplSentHAUnreach starMIPFAStatRegRplSentRegTimeout starMIPFAStatRegRplSentMissNAI starMIPFAStatRegRplSentMissHomeAgent starMIPFAStatRegRplSentMissHomeAddr starMIPFAStatRegRplSentUnknChallenge starMIPFAStatRegRplSentMissChallenge starMIPFAStatRegRplSentStaleChallenge starMIPFAStatRegRplSentBadReply starRPStatVpnID starRPStatVpnName starRPStatServName starRPRegRecvTotal starRPRegAcceptTotal starRPRegDeniedTotal starRPRegDiscardTotal starRPRegAcceptInitial starRPRegAcceptIntraPDSN starRPRegAcceptInterPDSN starRPRegDeniedInitial starRPRegAcceptRenew starRPRegDeniedRenew starRPRegAcceptDereg starRPRegDeniedDereg starRPRegSendError starRPRegHashError starRPRegDecodeError starRPRegUnhandled starRPRegAirlinkSeqError starRPRegDenyUnspec starRPRegDenyAdminProhib starRPRegDenyNoResource starRPRegDenyAuth starRPRegDenyMismatchID starRPRegDenyBadRequest starRPRegDenyUnknownPDSN starRPRegDenyRevTunUnav starRPRegDenyRevTunReq starRPRegDenyUnrecogVend starRPRegUpdTotal starRPRegUpdAccept starRPRegUpdDenied starRPRegUpdUnack starRPRegUpdTrans starRPRegUpdRetrans starRPRegUpdReceived starRPRegUpdDiscard starRPRegUpdSendError starRPRegUpdUplyrInit starRPRegUpdOther starRPRegUpdHandoff starRPRegUpdDenyUnspec starRPRegUpdDenyAdminProhib starRPRegUpdDenyAuth starRPRegUpdDenyMismatchID starRPRegUpdDenyBadRequest starRPSecViolations starRPSecBadAuth starRPSecBadID starRPSecBadSpi starRPSecMissingMnHAAuth starRPSecMissingRegUpdate starRPRegRecvInitial starRPRegAcceptActvStartIntraPDSN starRPRegAcceptActvStopIntraPDSN starRPRegRecvRenew starRPRegActvStartRenew starRPRegActvStopRenew starRPRegRecvDereg starRPRegAcceptActvStopDereg starRPDiscSessAbsent starRPDiscNoMemory starRPDiscMalformed starRPDiscAuthFail starRPDiscInternalBounce starRPDiscInpuQueueExceeded starRPDiscMismatchedId starRPDiscInvPacketLen starRPDiscMisc starSubContext starSubMSID starSubName starSubTimerDuration starSubLongDurTimeoutAction starSubSetupTime starSubHomeAddr starSubHomeAddrv6 starEISServerVPNName starThreshMeasuredPct starThreshPct starThreshMeasuredInt starThreshInt starThreshMeasuredMB starThreshMB starThreshMeasuredGB starThreshGB starPortType starPortTypeDescr starPortAdminState starPortOperState starPortOperMode starPortLinkState starRedundantPortSlot starRedundantPortNum starPortRXBytes starPortTXBytes starPortRXFrames starPortTXFrames starPortRxDiscards starPortTxDiscards starPortRxErrors starPortTxErrors starIPPoolVpnID starIPPoolContext starIPPoolGroup starIPPoolName starIPPoolType starIPPoolState starIPPoolStartAddr starIPPoolMaskorEndAddr starIPPoolPriority starIPPoolUsed starIPPoolHold starIPPoolRelease starIPPoolFree starLicensedSessions starCurrentSessions starDiameterVpnName starDiameterPeerAddr starDiameterEndpointName starInterfaceIPaddress starOSPFNeighborRouterID starOSPFFromState starOSPFToState starDiameterEncoderString starDiameterECode starDiameterPeerAddrIpv6 starContFiltCFUpgradeFilename starContFiltCFUpgradeErrorCode starBLUpgradeFilename starBLUpgradeErrorCode starDynPkgFilename starDynCFErrorCode starDynPkgUpgradeFilename starDynCFUpgradeErrorCode starEGTPVpnName starEGTPServName starEGTPInterfaceType starEGTPSelfPort starEGTPSelfAddr starEGTPPeerPort starEGTPPeerAddr starEGTPPeerOldRstCnt starEGTPPeerNewRstCnt starEGTPPeerSessCnt starEGTPFailureReason starGSSCDRLossConfigured starGSSCDRLossMeasured starLicenseKey starLicenseExpiryDate starLicenseDaysRemaining starLicenseDaysafterExpiry starSessGGSNVpnName starSessGGSNServName starSessGGSNPeerPort starSessGGSNPeerAddr starSessGGSNImsi starSessGGSNSubsName starSessGGSNAPNName starL2TPLocalTunnelID starL2TPPeerTunnelID starL2TPContextName starL2TPServiceName starL2TPServiceTypeName starL2TPLocalAddress starL2TPPeerAddress starSessSub1Context starSessSub1NAI starSessSub1MSID starSessSub1IpAddr starSessSub1LastResult starSessSub1ServiceName starSessSub1HAIpAddr starSessSub1PeerIpAddr starSessSub1InPackets starSessSub1InPacketsDropped starSessSub1InBytes starSessSub1OutPackets starSessSub1OutPacketsDropped starSessSub1OutBytes starSessSub1Activity starSessSub1State starSessSub1CallID starSessSub1ConnectTime starSessSub1CallDuration starSessSub1TimeIdle starSessSub1AccessType starSessSub1AccessTech starSessSub1LinkStatus starSessSub1NetworkType starSessSub1CarrierID starSessSub1ESN starSessSub1GMTTimezoneOffset starSessSub1SessMgr starSessSub1RemoteIPAddr starSessSub1Card starSessSub1CPU starSessSub1TimeIdleLeft starSessSub1TimeLeft starSessSub1TimeLongDurLeft starSessSub1LongDurAction starSessSub1AlwaysOn starSessSub1IPPoolName starSessSub1VLANID starSessSub1LNSIPAddr starSessSub1ProxyMIP starSessSub1GGSNMIP starSessSub1HomeAgentIpAddr starSessSub1LocalIPAddr starSessSub1FAServiceName starSessSub1FAVPNName starSessSub1SourceVPN starSessSub1DestVPN starSessSub1AAAVPN starSessSub1AAADomain starSessSub1AAAStart starSessSub1AAAStop starSessSub1AAAInterim starSessSub1AcctSessionID starSessSub1AAARadiusGroup starSessSub1AAARadiusAuthServerIPAddr starSessSub1AAARadiusAcctServerIPAddr starSessSub1NASIPAddr starSessSub1NexthopIPAddr starSessSub1ActiveInACL starSessSub1ActiveOutACL starSessSub1ECSRulebase starSessSub1InPlcyGrp starSessSub1OutPlcyGrp starSessSub1DownTrafPolState starSessSub1DownCommDataRate starSessSub1DownPeakDataRate starSessSub1DownBurstSize starSessSub1DownExceedAction starSessSub1DownViolateAction starSessSub1DownExceed starSessSub1DownViolate starSessSub1UpTrafPolState starSessSub1UpCommDataRate starSessSub1UpPeakDataRate starSessSub1UpBurstSize starSessSub1UpExceedAction starSessSub1UpViolateAction starSessSub1UpExceed starSessSub1UpViolate starSessSub1L3TunnelingState starSessSub1L3TunLocalIPAddr starSessSub1L3TunRemoteIPAddr starSessSub1AddrViaDHCP starSessSub1DHCPServName starSessSub1DHCPServIPAddr starSessSub1AccessLinkIPFrag starSessSub1IgnoreDFBit starSessSub1MIPGratARPMode starSessSub1ExtInlSrvrProc starSessSub1ExtInlSrvrIngrIPAddr starSessSub1ExtInlSrvrIngrVLANTag starSessSub1ExtInlSrvrEgrIPAddr starSessSub1ExtInlSrvrEgrVLANTag starSessSub1ExtInlSrvrVPNName starSessSub1RadAcctMode starSessSub1InBytesDropped starSessSub1OutBytesDropped starSessSub1PeakBPSTx starSessSub1PeakBPSRx starSessSub1AveBPSTx starSessSub1AveBPSRx starSessSub1SustBPSTx starSessSub1SustBPSRx starSessSub1PeakPPSTx starSessSub1PeakPPSRx starSessSub1AvePPSTx starSessSub1AvePPSRx starSessSub1SustPPSTx starSessSub1SustPPSRx starSessSub1ActivePctstarSessSub1IPv4BadHdr starSessSub1IPv4TtlExceeded starSessSub1IPv4FragSent starSessSub1IPv4FragFail starSessSub1IPv4InACLDrop starSessSub1IPv4OutACLDrop starSessSub1IPv4InCSSDownDrop starSessSub1IPv4OutCSSDownDrop starSessSub1IPv4OutXOFFDropPkt starSessSub1IPv4OutXOFFDropByte starSessSub1IPv4SrcViolstarSessSub1IPv4ProxyDNSRedir starSessSub1IPv4SrcProxyDNSPThru starSessSub1IPv4ProxyDNSDrop starSessSub1IPv4SrcViolNoAcct starSessSub1IPv4SrcViolIgnored starSessSub1ExtInlSrvrTxPkt starSessSub1ExtInlSrvrRxPkt starSessSub1IPv4ICMPDropPkt starSessSub1TunnelType starSessSub1IPSECTunDownDropPkt starSessSub1IPSECFlowID starSessSub1DormancyTotal starSessSub1HandoffTotal starSessSub1AccessFlows starSessSub1TFT starSessSub1NASPort starSessSub1AcctSessionID starSessSub1CorrID starSessSub1L2TPPeerIPAddr starSessSub1IPv4EarlyPDURecv starIPSECContextName starIPSECGroupName starIPSECTunLocalIPAddr starIPSECTunRemoteIPAddr starIPSECPolicyName starIPSECDynPolicyType starIPSECDynPolicyPayloadType starIPSECLocalGateway starIPSECRemoteGateway starSIPRouteVpnName starSIPRouteVmgName starSIPRouteAsName starSIPRouteDestPartyNum starSIPRouteReqNum starSIPRouteServerVpnName starSIPRouteServerVmgName starSIPRouteServerAsName starSIPRouteServerIpAddr starVIMServiceVpnName starVIMServiceFMDMaxCallRate starVIMServiceFMDContinuousLoadCount starGSSClusterName starGSSClusterNodeName starGSSClusterRgName starGSSClusterRsName starGSSClusterNodeState starGSSClusterPrevOnlineNode starGSSClusterFromNode starGSSClusterToNode starGSSDiskPath starGSSTransportPath starGSSIPMPGroupName starGSSInterfaceName starRPServiceOptionCalls starPCFStatVpnName starPCFStatRxPkts starPCFStatTxPkts starPCFStatRxBytes starPCFStatTxBytes starPCFStatTotalSessions starPCFStatCurrentSessions starPCFStatCurrentActiveSessions starPCFStatCurrentDormantSessions starPCFStatCurrentSIPConnected starPCFStatCurrentMIPConnected starPCFStatCurrentPMIPConnected starPCFStatCurrentL2TPLACConnected starPCFStatCurrentOtherConnected starPDIFSysStatus starPDIFSysNumService starPDIFSysSessCurrent, starPDIFSysSessCurrActive starPDIFSysSessCurrDormant starPDIFSysSessTtlSetup starPDIFSysChildSACurrent starPDIFVpnID starPDIFVpnName starPDIFServName starPDIFStatus starPDIFSessCurrent starPDIFSessRemain starPDIFSessCurrentActive starPDIFSessCurrentDormant starPDIFSessCurrentIpv6Active starPDIFSessCurrentIpv6Dormant starPDIFSessCurrentIpv4Active starPDIFSessCurrentIpv4Dormant starPDIFBindIpAddress starPDIFBindIpPort starPDIFBindSlot starPDIFBindPort starSessSGSNVpnNam starSessSGSNServName starSessSGSNMcc, starSessSGSNMnc, starSessSGSNRncId, starSessSGSNHlrNum, starSS7Pc, starSS7M3UAPsId, starSS7M3UAPspId, starSS7MTP3LinkSetId, starSS7MTP3LinkId, starSS7SCTPSelfAddr, starSS7SCTPPeerAddr starSS7SCCTPSelfPort starSCTPPeerPort starSccpSsn, starSGTPVpnName, starSGTPServName, starSGTPSelfAddr, starSGTPPeerAddr starSGTPPeerPort starIPMSServerVpnName starCertExpiryTime starCertissuer starFileApplication starFTPServVpnName starCSCFPeerServerVpnName, starCSCFPeerServerSvcName, starCSCFPeerServerListName, starSDHOperState starSDHPathOperState starE1TribOperStateLOP starE1TribOperState starFractE1TribTimeslots starGPRSNsvci starGPRSBvci starStorageDeviceType

> Object Group: | starAlertGroup

> Object ID: | enterprises.8164.3.1.3

> Description: | A collection of objects to control the rate at which traps can be generated.

> Objects: | starMaxAlertsPerTime starWindowTime starAlertSendingEnabled

> Object Group: | starAlertTrapGroup

> Object ID: | enterprises.8164.3.1.4

> Description: | A collection of traps related to trap thresholding.

> Notifications: | starAlertsDisabled starAlertsEnabled

> Object Group: | starTrapGroup

> Object ID: | enterprises.8164.3.1.5

> Description: | A collection of objects which represent required notifications.

> Objects: | starCardTempOverheat starCardTempOK starCardReset starCardRebootRequest starCardUp starCardVoltageFailure starCardInserted starCardRemoved starCardBootFailed starCardFailed starCardSWFailed starCardRCCFailed starCardMismatch starCardFailureLEDOn starCardFailureLEDOff starCardPACMigrateStart starCardPACMigrateComplete starCardPACMigrateFailed starCardSPCSwitchoverStart starCardSPCSwitchoverComplete starCardSPCSwitchoverFailed starFanFailed starFanRemoved starFanInserted starLogThreshold starCPUBusy starCPUMemoryLow starCPUMemoryFailed starCPUFailed starCPUWatchDogExpired starNPUARPPoolExhausted starPowerFilterUnitFailed starPowerFilterUnitUnavail starPowerFilterUnitAvail starAAAAuthServerUnreachable starAAAAuthServerReachable starAAAAuthServerMisconfigured starAAAAccServerUnreachable starAAAAccServerReachable starAAAAccServerMisconfigured starLogMsg starAlertsDisabled starAlertsEnabled starPDSNServiceStart starPDSNServiceStop starHAServiceStart starHAServiceStop starFAServiceStart starFAServiceStop starCLISessionStart starCLISessionEnd starCritTaskFailed starCardActive starLACServiceStart starLACServiceStop starLNSServiceStart starLNSServiceStop starCardDown starGGSNServiceStart starGGSNServiceStop starLicenseExceeded starSubscriberLimit starSessionRejectNoResource starSIPServiceStart starSIPServiceStop starVIMServiceStart starVIMServiceStop starCHATCONFServiceStart starCHATCONFServiceStop starSIPRouteNomatch starl3addrunreachable starSWUpgradeStart starSWUpgradeComplete starSWUpgradeAborted starBGPPeerSessionUp starBGPPeerSessionDown starSRPActive starSRPStandby starBGPPeerReachable starBGPPeerUnreachable starSRPAAAReachable starSRPAAAUnreachable starHASwitchoverInitiated starSRPCheckpointFailure starSRPConfigOutOfSync starSRPConfigInSync starGESwitchFailure starSIPRouteServerAvailable starSIPRouteServerUnavailable starFMDMaxCallRateReached starFMDCallRateUnderControl starStorageServerCPUBusy starStorageServerCPUNormal starStorageServerDiskSpaceLow starStorageServerDiskSpaceOK starCardSPOFAlarm starCardSPOFClear starStorageServerOldGcdrPending starStorageServerOldGcdrCleared starLoginFailure starIPSGServiceStart starIPSGServiceStop starHAUnreachable starHAReachable starASNGWServiceStart starASNGWServiceStop starTaskFailed starTaskRestart starCSCFServiceStart starCSCFServiceStop starIPSECDynTunUp starIPSECDynTunDown starHeartbeat starOverloadSystem starOverloadSystemClear starOverloadService starOverloadServiceClear starStorageServerClusterStateChange starStorageServerClusSwitchOver starStorageServerClusPathFail starStorageServerClusPathOK starStorageServerClusInterCFail starStorageServerClusInterCOK starStorageServerClusIntfFail starStorageServerClusIntfOK starStorageServerMemLow starStorageServerMemNormal sstarLongDurTimerExpiry starClosedRPServiceStart starClosedRPServiceStop starGtpcPathFailure starGtpuPathFailure starManagerFailure starEISServerAlive starEISServerDead starCgfAlive starCgfDead starBkupServerAlive starBkupServerDead starGgsnInitiatedUpdtFailed starGgsnInitiatedUpdtFailed starCongestion starCongestionClear starServiceLossPTACs starServiceLossLC starServiceLossSPIO starIPSPAllAddrsFree starPCFUnreachable starDhcpAlive starDhcpDead starDhcpServiceStarted starDhcpServiceStopped starNTPPeerUnreachable starNTPSyncLost starL2TPTunnelDownPeerUnreachable starCardStandby starLicenseUnderLimit starIPSECPriTunDown starIPSECPriTunUp starIPSECSecTunDown starIPSECSecTunUp starIPSECTunSwitchFail starIPSECTunSwitchComplete starNwReachServerAlive starNwReachServerDead starStorageServerUnackedGcdrVolPurge starStorageServerUnackedGcdrFileGen starNTPPeerReachable starNTPSyncEstablished starContFiltDBError starContFiltDBErrorClear starBLDBError starBLDBErrorClear starContFiltDBUpgradeError starContFiltDBUpgradeErrorClear starBLDBUpgradeErrorClear starPDIFServiceStart starBLDBError starBLDBErrorClear starContFiltDBUpgradeError starContFiltDBUpgradeErrorClear starBLDBUpgradeError starBLDBUpgradeErrorClear starPDIFServiceStart starPDIFServiceStop starSessMgrRecoveryComplete starDiameterPeerDown starDiameterPeerUp starDiameterServerUnreachable starDiameterServerReachable starDiameterCapabilitiesExchangeSuccess starDiameterCapabilitiesExchangeFailure starCDRFileRemoved starCSCFPeerServerReachable starCSCFPeerServerUnreachable starCLIConfigMode starSGSNServiceStart starSGSNServiceStop starM3UAPCUnavailable starM3UAPCAvailable starM3UAPSDown, starM3UAPSActive starM3UAPSPDown starM3UAPSPUp starSCCPSspRcvd starSCCPSspClear starSGSNRNCReset starSGSNHLRReset starSGSNGtpcPathFailure starSGSNGtpcPathFailureClear starSGSNGtpuPathFailure starSGSNGtpuPathFailureClear starMTP3LinkOutOfService starMTP3LinkInService starMTP3LinkSetUnAvailable starMTP3LinkSetAvailable starSCTPAssociationFail starSCTPAssociationEstablished starSCTPPathDown starSCTPPathUp, starMTP3PCUnavailable starMTP3PCAvailable starSS7PcUnavailable starSS7PCAvailable starASNPCServiceStart starASNPCServiceStop starSS7PCCongested starSS7PCCongestionCleared starPHSGWServiceStart starPHSGWServiceStop starM3UAPSPCongested starM3UAPSPCongestionCleared starStorageFailed starRaidFailed starRaidStarted starRaidDegraded starRaidRecovered starASNPCServiceStart starPDGServiceStart starPDGServiceStop starDiameterIpv6PeerDown starDiameterIpv6PeerUp starIPMSServerUnreachable starIPMSServerReachable starCertShortLifetime starServiceLossPTACsClear starServiceLossLCClear starCscfSessResourceCongestion starCscfSessResourceCongestionClear starOSPFv3NeighborDown starOSPFv3NeighborFull starServiceLossSPIOClear starStorageServerCDRLoss starCertExpired starCertValid starFTPPushFail starFTPServSwitch starPGWServiceStart starPGWServiceStop starSGWServiceStart starSGWServiceStop starEGTPServiceStart starEGTPServiceStop starEGTPServiceStop starLMAServiceStart starLMAServiceStop starMAGServiceStart starMAGServiceStop starMMEServiceStart starMMEServiceStop starHSGWServiceStart starHSGWServiceStop starCPUBusyClear starCPUMemoryLowClear starFNGServiceStart starFNGServiceStop starManagerRestart starConfigurationUpdate starEgtpcPathFailure starEgtpcPathFailureClear starServiceLossSPIOClear starEgtpuPathFailure starEgtpuPathFailureClear starHNBGWServiceStart starHNBGWServiceStop starSystemReboot starLicenseAboutToExpire starLicenseExpired starThreshCPUUtilization starThreshClearCPUUtilization starThreshCPUMemory starThreshClearCPUMemory starThreshLicence starThreshClearLicence starThreshSubscriberTotal starThreshClearSubscriberTotal starThreshSubscriberActive starThreshClearSubscriberActive starThreshPortRxUtil starThreshClearPortRxUtil starThreshPortTxUtil starThreshClearPortTxUtil starThreshPortHighActivity starThreshClearPortHighActivity starThreshAAAAuthFail starThreshClearAAAAuthFail starThreshAAAAuthFailRate starThreshClearAAAAuthFailRate starThreshAAAAcctFail starThreshClearAAAAcctFail starThreshAAAAcctFailRate starThreshClearAAAAcctFailRate starThreshAAARetryRate starThreshClearAAARetryRate starThreshCallSetup starThreshClearCallSetup starThreshCallSetupFailure starThreshClearCallSetupFailure starThreshCallRejectNoResource starThreshClearCallRejectNoResource starThreshPacketsFilteredDropped starThreshClearPacketsFilteredDropped starThreshPacketsForwarded starThreshClearPacketsForwarded starThreshSessCPUThroughput starThreshClearSessCPUThroughput starThreshIPPoolAvail starThreshClearIPPoolAvail starThreshCPUUtilization10Sec starThreshClearCPUUtilization10Sec starThreshCPULoad starThreshClearCPULoad starThreshCPUMemUsage starThreshClearCPUMemUsage starThreshPDSNSessions starThreshClearPDSNSessions starThreshGGSNSessions starThreshClearGGSNSessions starThreshHASessions starThreshClearHASessions starThreshLNSSessions starThreshClearLNSSessions starThreshPerServicePDSNSessions starThreshClearPerServicePDSNSessions starThreshPerServiceGGSNSessions starThreshClearPerServiceGGSNSessions starThreshPerServiceHASessions starThreshClearPerServiceHASessions starThreshPerServiceLNSSessions starThreshClearPerServiceLNSSessions starThreshIPPoolHold starThreshClearIPPoolHold starThreshIPPoolUsed starThreshClearIPPoolUsed starThreshIPPoolRelease starThreshClearIPPoolRelease starThreshIPPoolFree starThreshClearIPPoolFree starThreshAAAAcctArchive starThreshClearAAAAcctArchive starThreshPortSpecRxUtil starThreshClearPortSpecRxUtil starThreshPortSpecTxUtil starThreshClearPortSpecTxUtil starThreshHACallSetupRate starThreshClearHACallSetupRate starThreshHASvcCallSetupRate starThreshClearHASvcCallSetupRate starThreshHASvcRegReplyError starThreshClearHASvcRegReplyError starThreshHASvcReregReplyError starThreshClearHASvcReregReplyError starThreshHASvcDeregReplyError starThreshClearHASvcDeregReplyError starThreshFASvcRegReplyError starThreshClearFASvcRegReplyError starThreshPDSNCallSetupRate starThreshClearPDSNCallSetupRate starThreshPDSNSvcCallSetupRate starThreshClearPDSNSvcCallSetupRate starThreshPDSNSvcA11RRPFailure starThreshClearPDSNSvcA11RRPFailure starThreshPDSNSvcA11RRQMsgDiscard starThreshClearPDSNSvcA11RRQMsgDiscard starThreshPDSNSvcA11RACMsgDiscard starThreshClearPDSNSvcA11RACMsgDiscard starThreshPDSNSvcA11PPPSendDiscard starThreshClearPDSNSvcA11PPPSendDiscard starThreshAAAMgrQueue starThreshClearAAAMgrQueue starThreshCPUOrbsWarn starThreshClearCPUOrbsWarn starThreshCPUOrbsCritical starThreshClearCPUOrbsCritical starThreshRPSetupFailRate starThreshClearRPSetupFailRate starThreshPPPSetupFailRate starThreshClearPPPSetupFailRate starThreshStorageUtilization starThreshClearStorageUtilization starThreshClearStorageUtilization starThreshDCCAProtocolErrors starThreshClearDCCAProtocolErrors starThreshDCCABadAnswers starThreshClearDCCABadAnswers starThreshDCCAUnknownRatingGroup starThreshClearDCCAUnknownRatingGroup starThreshDCCARatingFailed starThreshClearDCCARatingFailed starThreshIPSECIKERequests starThreshClearIPSECIKERequests starThreshIPSECIKEFailures starThreshClearIPSECIKEFailures starThreshIPSECIKEFailRate starThreshClearIPSECIKEFailRate starThreshIPSECTunSetup starThreshClearIPSECTunSetup starThreshIPSECTunEstabl starThreshClearIPSECTunEstabl starThreshIPSECCallReqRej starThreshClearIPSECCallReqRej starThreshCSCFSvcRouteFailure starThreshClearCSCFSvcRouteFailure starThreshContFiltRating starThreshClearContFiltRating starThreshContFiltBlock starThreshClearContFiltBlock starThreshCDRFileSpace starThreshClearCDRFileSpace starThreshEDRFileSpace starThreshClearEDRFileSpace starThreshPDIFCurrSess starThreshClearPDIFCurrSess starThreshPDIFCurrActSess starThreshClearPDIFCurrActSess starThreshCDRFlowControl starThreshSGSNSessions starThreshClearSGSNSessions starThreshPerServiceSGSNSessions starThreshClearPerServiceSGSNSessions starThreshSGSNPdpSessions starThreshClearSGSNPdpSessions starThreshPerServiceSGSNPdpSessions starThreshClearPerServiceSGSNPdpSessions starThreshClearCDRFlowControl starThreshASNGWSessTimeout starThreshClearASNGWSessTimeout starThreshASNGWSessSetupTimeout starThreshClearASNGWSessSetupTimeout starThreshASNGWAuthFail starThreshClearASNGWAuthFail starThreshASNGWR6InvNai starThreshClearASNGWR6InvNai starThreshASNGWMaxEAPRetry starThreshClearASNGWMaxEAPRetry starThreshASNGWEntryDenial starThreshClearASNGWEntryDenial starThreshASNGWHandoffDenial starThreshClearASNGWHandoffDenial starThreshASNGWSessions starThreshClearASNGWSessions starThreshPerServiceASNGWSessions starThreshClearPerServiceASNGWSessions starThreshPHSPCSessSetupTimeout starThreshClearPHSPCSessSetupTimeout starThreshPHSPCSleepModeTimeout starThreshClearPHSPCSleepModeTimeout starThreshPHSPCSmEntryDenial starThreshClearPHSPCSmEntryDenial starThreshSGWSessions starThreshClearSGWSessions starThreshPGWSessions starThreshClearPGWSessions starThreshMeasuredInt starThreshClearLMASessions starThreshMAGSessions starThreshClearMAGSessions starThreshFNGCurrSess starThreshClearFNGCurrSess starThreshFNGCurrActSess starThreshClearFNGCurrActSess starThreshPHSGWEAPOLAuthFailure starThreshClearPHSGWEAPOLAuthFailure starThreshPHSGWMaxEAPOLRetry starThreshClearPHSGWMaxEAPOLRetry starThreshHSGWSessions starThreshClearHSGWSessions starThreshFWDosAttack starThreshClearFWDosAttack starThreshFWDropPacket starThreshClearFWDropPacket starThreshFWDenyRule starThreshClearFWDenyRule starThreshFWNoRule starThreshClearFWNoRule starThreshPHSGWSessTimeout starThreshClearPHSGWSessTimeout starThreshPHSGWSessSetupTimeout starThreshClearPHSGWSessSetupTimeout starThreshPHSGWAuthFail starThreshClearPHSGWAuthFail starThreshPHSGWMaxEAPRetry starThreshClearPHSGWMaxEAPRetry starThreshPHSGWNWEntryDenial starThreshClearPHSGWNWEntryDenial starThreshPHSGWHandoffDenial starThreshMeasuredInt starSRPConnDown starSRPConnUp starDiameterIpv6PeerDown starDiameterIpv6PeerUp starIPMSServerUnreachable starIPMSServerReachable starCertShortLifetime starSDHSectionDown starSDHSectionUp starSDHPathHopDown starSDHPathHopUp starSDHLopDown starSDHLopUp starThreshNAPTPortChunks, starThreshClearNAPTPortChunks starThreshGPRSSessions starThreshClearGPRSSessions starThreshPerServiceGPRSSessions starThreshClearPerServiceGPRSSessions starThreshGPRSPdpSessions starThreshClearGPRSPdpSessions starThreshPerServiceGPRSPdpSessions starThreshClearPerServiceGPRSPdpSessions starThreshCSCFSvcRegRcvdRate starThreshClearCSCFSvcRegRcvdRate starThreshCSCFSvcTotalActiveReg starThreshClearCSCFSvcTotalActiveReg starThreshCSCFSvcInviteRcvdRate starThreshClearCSCFSvcInviteRcvdRate starThreshCSCFSvcTotalActiveCalls starThreshClearCSCFSvcTotalActiveCalls starThreshCSCFSvcTotalCallFailure starThreshClearCSCFSvcTotalCallFailure starThreshCSCFSvcErrorNoResource starThreshClearCSCFSvcErrorNoResource starThreshCSCFSvcErrorTcp starThreshClearCSCFSvcErrorTcp starThreshCSCFSvcErrorPresence starThreshClearCSCFSvcErrorPresence starThreshCSCFSvcErrorRegAuth starThreshClearCSCFSvcErrorRegAuth starThreshBGPRoutes--enterprises starThreshBGPRoutes--enterprises starThreshClearBGPRoutes starPortDown starPortUp starOSPFNeighborDown starOSPFNeighborFull starBSReachable starBSUnreachable starSystemStartup starASNPCserviceStart starASNPCServiceStop starDiameterIPv6PeerDown starDiameterIPv6PeerUp starIPMSServerUnreachable starIPMSServerReachable starCertShortLifetime starCertExpired starCertValid starFTPPushFail starFTPServSwitch starSDHSectionDown, starSDHSectionUp starSDHPathHopDown starSDHPathHopUp starSDHLopDown starSDHLopUp starSDHE1TribDown starSDHE1TribUp starSDHFractE1LMIDown starSDHFractE1LMIUp starGPRSServiceStart starGPRSServiceStop starGPRSNseUp starGPRSNsvcDown starGPRSNsvcUp starGPRSBvcDown starGPRSBvcUp starSDHE1TribUp starSDHFractE1LMIDown starSDHFractE1LMIUp starPHSPCServiceStart starPHSPCServiceStop starPDGServiceStart, starPDGServiceStop starThreshPDGCurrSess starThreshClearPDGCurrSess, starThreshPDGCurrActSess, starThreshClearPDGCurrActSess starGPRSServiceStart starGPRSServiceStop starGPRSNseDown starGPRSNseUp starGPRSNsvcDown starGPRSNsvcUp starGPRSBvcDown starGPRSBvcUp

> Object: | starTrapObsoleteGroup

> Object ID: | enterprises.8164.3.1.6

> Description: | A collection of objects which represent obsolete notifications.

> Notifications: | starCardReset starCardFailed starCardRCCFailed starCardSWFailed starCardFailureLEDOn starCardFailureLEDOff starLogThreshold starThreshASNGWR6InvNai starThreshClearASNGWR6InvNai

> Object: | starChassisObsoleteGroup

> Object ID: | enterprises.8164.3.1.7

> Description: | A collection of objects which are obsolete.

> Objects: | starRPRegAcceptIntraPDSN starSlotVoltage1dot5 starSlotVoltage1dot5LowThresh starSlotVoltage1dot5HighThresh starSlotVoltage1dot8 starSlotVoltage1dot8LowThresh starSlotVoltage1dot8HighThresh starSlotVoltage2dot5 starSlotVoltage2dot5LowThresh starSlotVoltage2dot5HighThresh starSlotVoltage3dot3 starSlotVoltage3dot3LowThresh starSlotVoltage3dot3HighThresh starSlotVoltage5dot0 starSlotVoltage5dot0LowThresh starSlotVoltage5dot0HighThresh

> starentMIB(8164).starentMIBConformance(3).starentMIBCompliances(2)

> Object: | MIBCompliance2

> Object ID: | enterprises.8164.3.2.2

> Description: | The statement listing compliant mandatory groups.

> Required Groups: | starChassisGroup starAlertGroup starAlertTrapGroup starTrapGroup starTrapObsoleteGroup

> Standards-based Traps
> The following traps are defined in RFC 1157, Simple Network Management Protocol (SNMP) and are supported by the system:

> l | linkDown The Interface Index for this trap is the IfIndex for the physical port, not the logical interface.

> l | linkUp The Interface Index for this trap is the IfIndex for the physical port, not the logical interface.

> l | authenticationFailure

> l | enterpriseSpecific

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883