> show sgw
> This chapter describes the output of the show sgw command.
> show sgw-service all
> Displays configuration information for all S-GW services configured on the system.
> show sgw-service all Command Output Descriptions

> Field | Description
> Service name | The name of the S-GW service.
> Service-ID | The system generated identification number of the service.
> Context | The context name where the service is located.
> Accounting Context | The context where the accounting configuration and or interfaces are configured.
> Status | The status of the service.
> Egress Protocol | The egress protocol
> Ingress EGTP Service | The ingress eGTP service configured for this S-GW service.
> Egress Context | The egress context configured for this service.
> Egress MAG Service | The egress MAG service configured for this service.
> Newcall Policy | The newcall policy configured for this service.
> Ims auth Service | The IMS authorization service used by this service for IMS subscribers.
> Charging Characteristics(CC) Profiles
> QCI-QOS Mapping Table Name | The QoS Class Index to QoS mapping table configured for use with this service.

> ‌
> show sgw-service statistics all
> show sgw-service statistics all Command Output Descriptions

> Field | Description
> SGW Node Level Statistics
> VPN Name | The name of the context configured on the system that is currently facilitating the S-GW service.
> Session Level Statistics
> Current
> UE
> Idle | The total number of UE sessions currently idle.
> Active | The total number of UE sessions currently active.
> PDN | The total number of current PDN sessions.
> Bearers | The total number of current Bearers.
> Setup
> UE | The total number of UE session set up.
> PDN | The total number of PDN sessions set up.
> Bearers | The total number of bearers set up.
> PDNs Setup Per PDN-type
> IPv4 | The total number of PDN sessions set up using IPv4.
> IPv6 | The total number of PDN sessions set up using IPv6.
> IPv4v6 | The total number of PDN sessions set up using IPv4 in IPv6.
> PDNs Setup Per Interface
> S11 | The total number of PDN sessions set up on an S11 interface.
> S4 | The total number of PDN sessions set up on an S4 interface.
> PDNs Setup Per S5 Proto
> GTP | The total number of PDN sessions set up using GTP tunneling.
> PMIP | The total number of PDN sessions set up using PMIP tunneling.
> PDNs Released
> IPv4 | The total number of PDN sessions released using IPv4.
> IPv6 | The total number of PDN sessions released using IPv6.
> IPv4v6 | The total number of PDN sessions released using IPv4 in IPv6.
> PDNs Released Reason
> MME Ini | The total number of PDN sessions released - initiated by the MME.
> PGW Ini | The total number of PDN sessions released - initiated by the P-GW.
> PCRF Ini | The total number of PDN sessions released - initiated by the PCRF.
> Local | The total number of PDN sessions released - initiated locally.
> S1 Error Ind | The total number of PDN sessions released due to an S1 interface error.
> S5 Error Ind | The total number of PDN sessions released due to an S5 interface error.
> Path Failure S11 | The total number of PDN sessions released due to an S11 path failure.
> Path Failure S1-U | The total number of PDN sessions released due to an S1-U path failure.
> Path Failure S5 | The total number of PDN sessions released due to an S5 path failure.
> Path Failure S5-U | The total number of PDN sessions released due to an S5-U path failure.
> Other | The total number of PDN sessions released due to other reasons.
> PDNs Rejected
> IPv4 | The total number of PDN sessions rejected using IPv4.
> IPv6 | The total number of PDN sessions rejected using IPv6.
> IPv4v6 | The total number of PDN sessions rejected using IPv4 in IPv6.
> PDNs Rejected Reason
> PGW Ini | The total number of PDN sessions rejected - initiated by the P-GW.
> License | The total number of PDN sessions rejected due to license reasons.
> Newcall | The total number of PDN sessions rejected due to newcall reasons.
> Overload | The total number of PDN sessions rejected due to overload reasons.
> Congestion | The total number of PDN sessions rejected due to congestion reasons.
> Other | The total number of PDN sessions rejected due to other reasons.
> Bearer Level Statistics
> Total EPS Bearers Setup
> QCI 1 - 9 | The total number of EPS bearers set up, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers set up, with a non-standard QoS Class Index.
> Total EPS Bearers Released
> QCI 1 - 9 | The total number of EPS bearers released, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers released, with a non-standard QoS Class Index.
> Total EPS Bearers Modified |
> QCI 1 - 9 | The total number of EPS bearers modified, with a QoS Class Index.
> Non-Std QCI | The total number of EPS bearers modified, with a non-standard QoS Class Index.
> Dedicated Bearers Released Reason
> PGW Ini | The total number of dedicated bearers released - initiated by the P-GW.
> PCRF Ini | The total number of dedicated bearers released - initiated by the PCRF.
> S1 Error Ind | The total number of dedicated bearers released due to an S1 interface error.
> S5 Error Ind | The total number of dedicated bearers released due to an S5 interface error.
> Local | The total number of dedicated bearers released - initiated locally.
> PDN Down | The total number of dedicated bearers released due to an inaccessible PDN.
> Path Failure S1-U | The total number of dedicated bearers released due to an S1-U path failure.
> Path Failure S5-U | The total number of dedicated bearers released due to an S5-U path failure.
> Other | The total number of dedicated bearers released due to other reasons.
> Data Statistics
> Total Uplink Packets Forwarded
> QCI 1 - 9 | The total number of uplink packets forwarded with a QoS Class Index.
> Non-Std QCI | The total number of uplink packets forwarded with a non-standard QoS Class Index.
> Total Uplink Bytes Forwarded
> QCI 1 - 9 | The total number of uplink bytes forwarded with a QoS Class Index.
> Non-Std QCI | The total number of uplink bytes forwarded with a non-standard QoS Class Index.
> Total Uplink Packets Dropped
> QCI 1 - 9 | The total number of uplink packets dropped with a QoS Class Index.
> Non-Std QCI | The total number of uplink packets dropped with a non-standard QoS Class Index.
> Total Uplink Bytes Dropped
> QCI 1 - 9 | The total number of uplink bytes dropped with a QoS Class Index.
> Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
> Total Downlink Packets Forwarded
> QCI 1 - 9 | The total number of downlink packets forwarded with a QoS Class Index.
> Non-Std QCI | The total number of downlink packets forwarded with a non-standard QoS Class Index.
> Total Downlink Bytes Forwarded
> QCI 1 - 9 | The total number of downlink bytes forwarded with a QoS Class Index.
> Non-Std QCI | The total number of downlink bytes forwarded with a non-standard QoS Class Index.
> Total Downlink Packets Dropped
> QCI 1 - 9 | The total number of downlink packets dropped with a QoS Class Index.
> Non-Std QCI | The total number of downlink packets dropped with a non-standard QoS Class Index.
> Total Downlink Bytes Dropped
> QCI 1 - 9 | The total number of downlink bytes dropped with a QoS Class Index.
> Non-Std QCI | The total number of downlink bytes dropped with a non-standard QoS Class Index.
> Inter-SGW Handover Statistics
> PDNs Incoming
> X2 based | The total number of incoming X2-based PDNs.
> Idle-mode TAU | The total number of incoming PDNs Incoming - Idle-mode TAU
> S1 Based | The total number of incoming S1-based PDNs.
> PDNs Outgoing | The total number of outgoing PDNs.
> Intra-SGW Handover Statistics
> Intra-MME | Intra-MME
> Inter-MME | Inter-MME
> Paging Statistics
> Requests | The total number of paging requests.
> Success | The total number of paging successes.
> Rejects | The total number of paging rejects.
> Failures | The total number of paging failures.
> Active-Idle UE Transitions | The total number of Active-Idle UE transitions
> Idle-Active UE Transitions | The total number of Idle-Active UE transitions
> Paging Related Data Statistics
> Total Bytes Buffered | The total number of buffered paging bytes.
> Total Pkts Buffered | The total number of buffered paging packets.
> Total Discarded Bytes | The total number of discarded paging bytes.
> Total Discarded Pkts | The total number of discarded paging packets.
> Idle Mode ACL Statistics
> Total Dropped Bytes | The total number of dropped paging bytes.
> Total Dropped Pkts | The total number of dropped paging packets.
> Miscellaneous
> Uplink Data Before MBReq | Uplink data before MBreq
> CBReq Rcvd Before CSRsp | CBReq Rcvd before CSRsp

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883