> Accounting Management
> This section contains additions and changes made to the accounting-related parameters available in Release 10.0. Topics covered in this chapter are:

> l | Bulk Statistic Enhancements in Release 10.0

> l | CDR Enhancements

> l | Command Enhancements

> l | New Commands

> l | RADIUS Attributes in Release 10.0

> l | Diameter Attributes in Release 10.0

> l | Web Element Manager Enhancements

> Bulk Statistic Enhancements in Release 10.0
> This section lists bulk statistic additions and changes in Release 10.0. Detailed information on bulk statistics is located in both the System Administration Guide and in the Statistics and Counters Reference. Bulk statistic changes in this version are divided into the following sections:

> l | New Bulk Statistics

> l | Modified Bulk Statistics

> l | Obsoleted Bulk Statistics

> New Bulk Statistics
> Support for the following bulk statistics were added in Release 10.0.
> CSCF Schema

> l | emerg-priv-calls

> l | msrp-sent

> l | msrp-recv

> l | fhloerrrx

> l | fhloerrtx

> l | calldur-lt-01sec

> l | calldur-01to10sec

> l | calldur-10to30sec

> l | calldur-30to60sec

> l | calldur-60to90sec

> l | calldur-90to120sec

> l | calldur-120to150sec

> l | calldur-150to180sec

> l | calldur-03to04min

> l | calldur-04to05min

> l | calldur-05to06min

> l | calldur-06to07min

> l | calldur-07to08min

> l | calldur-08to09min

> l | calldur-09to11min

> l | calldur-11to13min

> l | calldur-13to15min

> l | calldur-15to17min

> l | calldur-17to19min

> l | calldur-19to21min

> l | calldur-21to23min

> l | calldur-23to25min

> l | calldur-25to27min

> l | calldur-27to29min

> l | calldur-29to60min

> l | calldur-gt-60min

> ECS Schema

> l | p2p-freenet-uplnk-bytes

> l | p2p-freenet-dwlnk-bytes

> l | p2p-freenet-uplnk-pkts

> l | p2p-freenet-dwlnk-pkts

> l | p2p-aimini-uplnk-bytes

> l | p2p-aimini-dwlnk-bytes

> l | p2p-aimini-uplnk-pkts

> l | p2p-aimini-dwlnk-pkts

> l | p2p-battlefld-uplnk-bytes

> l | p2p-battlefld-dwlnk-bytes

> l | p2p-battlefld-uplnk-pkts

> l | p2p-battlefld-dwlnk-pkts

> l | p2p-openft-uplnk-bytes

> l | p2p-openft-dwlnk-bytes

> l | p2p-openft-uplnk-pkts

> l | p2p-openft-dwlnk-pkts

> l | p2p-qqgame-uplnk-bytes

> l | p2p-qqgame-dwlnk-bytes

> l | p2p-qqgame-uplnk-pkts

> l | p2p-qqgame-dwlnk-pkts

> l | p2p-quake-uplnk-bytes

> l | p2p-quake-dwlnk-bytes

> l | p2p-quake-uplnk-pkts

> l | p2p-quake-dwlnk-pkts

> l | p2p-secondlife-uplnk-bytes

> l | p2p-secondlife-dwlnk-bytes

> l | p2p-secondlife-uplnk-pkts

> l | p2p-secondlife-dwlnk-pkts

> l | p2p-actsync-uplnk-bytes

> l | p2p-actsync-dwlnk-bytes

> l | p2p-actsync-uplnk-pkts

> l | p2p-actsync-dwlnk-pkts

> l | p2p-nimbuzz-uplnk-bytes

> l | p2p-nimbuzz-dwlnk-bytes

> l | p2p-nimbuzz-uplnk-pkts

> l | p2p-nimbuzz-dwlnk-pkts

> l | p2p-iax-uplnk-bytes

> l | p2p-iax-dwlnk-bytes

> l | p2p-iax-uplnk-pkts

> l | p2p-iax-dwlnk-pkts

> l | p2p-paltalk-uplnk-bytes

> l | p2p-paltalk-dwlnk-bytes

> l | p2p-paltalk-uplnk-pkts

> l | p2p-paltalk-dwlnk-pkts

> l | p2p-warcft3-uplnk-bytes

> l | p2p-warcft3-dwlnk-bytes

> l | p2p-warcft3-uplnk-pkts

> l | p2p-warcft3-dwlnk-pkts

> l | p2p-rdp-uplnk-bytes

> l | p2p-rdp-dwlnk-bytes

> l | p2p-rdp-uplnk-pkts

> l | p2p-rdp-dwlnk-pkts

> l | p2p-iptv-uplnk-bytes

> l | p2p-iptv-dwlnk-bytes

> l | p2p-iptv-uplnk-pkts

> l | p2p-iptv-dwlnk-pkts

> l | p2p-pandora-uplnk-bytes

> l | p2p-pandora-dwlnk-bytes

> l | p2p-pandora-uplnk-pkts

> l | p2p-pandora-dwlnk-pkts

> Diameter Accounting Schema

> l | vpnid

> l | vpnname

> l | ipaddr

> l | port

> l | servertype

> l | group

> l | req-sent

> l | req-retried

> l | rsp-rcvd

> l | req-timeout

> l | rsp-bad-resp

> l | rsp-malformed

> l | rsp-dropped

> l | start-sent

> l | stop-sent

> l | interim-sent

> l | start-retries

> l | stop-retries

> l | interim-retries

> Diameter Authentication Schema

> l | vpnid

> l | vpnname

> l | ipaddr

> l | port

> l | servertype

> l | group

> l | der-req-id-sent

> l | der-req-aka-chal-sent

> l | der-req-retried

> l | dea-chal-rcvd

> l | dea-acpt-rcvd

> l | dea-timeout

> l | dea-badauth

> l | dea-malformed

> l | dea-malformed-avp

> l | dea-dropped

> l | rar-req-rcvd

> l | raa-ans-accpt-sent

> l | aar-req-sent

> l | str-req-sent

> l | str-req-retried

> l | sta-ans-accpt-rcvd

> l | asr-req-rcvd

> l | asa-rsp-accpt-sent

> l | asa-rsp-rej-sent

> l | req-sock-write-err

> l | rsp-sock-write-err

> l | any-sock-read-err

> l | rem-disconnect

> l | loc-disconnect

> IMSA Schema

> l | dpca-fail-connfh-totmsgtmo

> l | dpca-fail-connfh-totmsgsenderr

> l | dpca-fail-rescodefh-confrescode

> l | dpca-fail-rescodefh-unhunkrescode

> NAT Realm Schema

> l | nat-rlm-port-chunk-size

> l | nat-rlm-port-chunk-average-usage-tcp

> l | nat-rlm-port-chunk-average-usage-udp

> l | nat-rlm-port-chunk-average-usage-others

> l | nat-rlm-max-port-chunk-subs

> l | nat-rlm-max-port-chunk-used

> l | nat-rlm-max-cur-port-chunk-subs

> l | nat-rlm-max-cur-port-chunk-used

> Modified Bulk Statistics
> The following bulk statistics were modified in Release 10.0.
> P-GW Node Level Schema
> The following statistics were added to this schema:

> l | sessstat-bearact-def

> l | sessstat-bearact-ue-init-ded

> l | sessstat-bearact-nw-init-ded

> l | sessstat-bearrel-nwdedadmin

> l | sessstat-bearrel-nwdedgtp

> l | sessstat-bearrel-nwdedmme

> l | sessstat-bearrel-nwdeddefbear

> l | sessstat-bearrel-nwdedgxdisc

> l | sessstat-bearrej-uereq-nores

> l | sessstat-bearrej-nwreq-nores

> l | sessstat-bearrej-nwreq-nomem

> l | sessstat-bearrej-nwreq-sysfail

> l | sessstat-bearmodfail-ueinit

> l | sessstat-bearmodfail-nwinit

> l | sessstat-bearmodfail-nwnores

> l | sessstat-bearmodfail-nwnomem

> l | sessstat-bearmodfail-nwsysfail

> l | sessstat-bearmodfail-nwsemtft

> l | sessstat-bearmodfail-nwsyntft

> l | sessstat-bearmodfail-nwsempkt

> l | sessstat-bearmodfail-nwsynpkt

> l | sessstat-bearrel-nwdefadmin

> l | sessstat-bearrel-nwdefgtp

> l | sessstat-bearrel-nwdefsgw

> l | sessstat-bearrel-nwdefmme

> l | sessstat-bearrel-nwdedadmin

> l | sessstat-bearrel-nwdedgtp

> l | sessstat-bearrel-nwdedmme

> l | sessstat-bearrel-nwdeddefbear

> l | sessstat-bearrel-nwdedgxdisc

> l | subdatastat-uppktfwd-stdqcinongbr

> l | subdatastat-uppktfwd-stdqcigbr

> l | subdatastat-uppktfwd-totgbr

> l | subdatastat-uppktfwd-totnongbr

> l | subdatastat-upbytefwd-stdqcinongbr

> l | subdatastat-upbytefwd-stdqcigbr

> l | subdatastat-upbytefwd-totgbr

> l | subdatastat-upbytefwd-totnongbr

> l | subdatastat-downpktfwd-stdqcinongbr

> l | subdatastat-downpktfwd-stdqcigbr

> l | subdatastat-downpktfwd-totgbr

> l | subdatastat-downpktfwd-totnongbr

> l | subdatastat-downbytefwd-stdqcinongbr

> l | subdatastat-downbytefwd-stdqcigbr

> l | subdatastat-downbytefwd-totgbr

> l | subdatastat-downbytefwd-totnongbr

> l | subdatastat-uppktdrop-stdqcinongbr

> l | subdatastat-uppktdrop-stdqcigbr

> l | subdatastat-uppktdrop-totgbr

> l | subdatastat-uppktdrop-totnongbr

> l | subdatastat-upbytedrop-stdqcinongbr

> l | subdatastat-upbytedrop- stdqcigbr

> l | subdatastat-upbytedrop-totgbr

> l | subdatastat-upbytedrop-totnongbr

> l | subdatastat-downpktdrop-stdqcinongbr

> l | subdatastat-downpktdrop-stdqcigbr

> l | subdatastat-downpktdrop-totgbr

> l | subdatastat-downpktdrop-totnongbr

> l | subdatastat-downbytedrop-stdqcinongbr

> l | subdatastat-downbytedrop-stdqcigbr

> l | subdatastat-downbytedrop-totgbr

> l | subdatastat-downbytedrop-totnongbr

> l | subdatastat-totuppktdropmbrexc

> l | subdatastat-uppktdropmbrexc-qci1

> l | subdatastat-uppktdropmbrexc-qci2

> l | subdatastat-uppktdropmbrexc-qci3

> l | subdatastat-uppktdropmbrexc-qci4

> l | subdatastat-uppktdropmbrexc-qci5

> l | subdatastat-uppktdropmbrexc-qci6

> l | subdatastat-uppktdropmbrexc-qci7

> l | subdatastat-uppktdropmbrexc-qci8

> l | subdatastat-uppktdropmbrexc-qci9

> l | subdatastat-uppktdropmbrexc-stdqcinongbr

> l | subdatastat-uppktdropmbrexc-stdqcigbr

> l | subdatastat-uppktdropmbrexc-qcinongbr

> l | subdatastat-uppktdropmbrexc-qcigbr

> l | subdatastat-uppktdropmbrexc-totgbr

> l | subdatastat-uppktdropmbrexc-totnongbr

> l | subdatastat-totupbytedropmbrexc

> l | subdatastat-upbytedropmbrexc-qci1

> l | subdatastat-upbytedropmbrexc-qci2

> l | subdatastat-upbytedropmbrexc-qci3

> l | subdatastat-upbytedropmbrexc-qci4

> l | subdatastat-upbytedropmbrexc-qci5

> l | subdatastat-upbytedropmbrexc-qci6

> l | subdatastat-upbytedropmbrexc-qci7

> l | subdatastat-upbytedropmbrexc-qci8

> l | subdatastat-upbytedropmbrexc-qci9

> l | subdatastat-upbytedropmbrexc-stdqcinongbr

> l | subdatastat-upbytedropmbrexc-stdqcigbr

> l | subdatastat-upbytedropmbrexc-qcinongbr

> l | subdatastat-upbytedropmbrexc-qcigbr

> l | subdatastat-upbytedropmbrexc-totgbr

> l | subdatastat-upbytedropmbrexc-totnongbr

> S-GW Node Level Schema Statistics
> The following statistics were added to this schema:

> l | sessstat-pdnrelrsn-pathfail-S11

> l | sessstat-pdnrelrsn-pathfail-S5

> l | sessstat-pdnrelrsn-pathfail-S5-u

> l | sessstat-pdnrelrsn-pathfail-S1-u

> l | sessstat-pdnrejrsn-license

> l | sessstat-pdnrejrsn-newcall-policy

> l | sessstat-pdnrejrsn-overload

> l | sessstat-pdnrejrsn-cong

> Obsoleted Bulk Statistics
> The following bulk statistics were obsoleted in Release 10.0.
> None for this release.
> Web Element Manager Path
> Click Accounting | Bulk Statistics Configuration.
> CDR Enhancements
> This section lists new custom GTPP dictionaries in Release 10.0. Refer to the AAA Interface Configuration and Reference for details.
> Command Enhancements
> None for this release.
> New Commands
> None for this release.
> RADIUS Attributes in Release 10.0
> This section lists additions and changes to RADIUS AVPs in Release 10.0. Refer to the AAA Interface Configuration and Reference for details.
> New Attributes
> The following RADIUS attributes are new in Release 10.0.

> l | SN-TrafficSelector-Class

> l | SN1-NAT-IP-Address-Old

> l | WiMAX-Prepaid-Tariff-Switch

> Modified Attributes
> The following RADIUS attributes were modified in Release 10.0.

> l | 3GPP2-Service-Option

> l | SN-Disconnect-Reason

> l | SN1-Disconnect-Reason

> l | WiMAX-Capability

> l | WiMAX-NSP-ID

> l | WiMAX-Packet-Flow-Descriptor

> l | WiMAX-QoS-Descriptor

> Removed Attributes
> None for this release.
> Diameter Attributes in Release 10.0
> This section lists additions and changes to Diameter attributes in Release 10.0. Refer to the AAA Interface Reference for details.
> New Attributes
> The following Diameter attributes are new in Release 10.0:

> l | 3GPP-WLAN-APN-Id

> l | Associated-Registered-Identities

> l | Call-ID-SIP-Header

> l | Charging-Characteristics

> l | Charging-Data

> l | Contact

> l | From-SIP-Header

> l | Loose-Route-Indication

> l | Multiple-Registration-Indication

> l | Path

> l | Record-Route

> l | Restoration-Info

> l | SCSCF-Restoration-Info

> l | Session-Priority

> l | Session-Request-Type

> l | SN-Phase0-PSAPName

> l | Subscription-Info

> l | To-SIP-Header

> l | Usage-Monitoring-Information

> l | Usage-Monitoring-Level

> l | Usage-Monitoring-Report

> l | Usage-Monitoring-Support

> l | Wildcarded-IMPU

> Modified Attributes
> The following Diameter attributes were modified in Release 10.0:

> l | Event-Trigger

> l | SIP-Auth-Data-Item

> Removed Attributes
> The following Diameter attributes were removed in Release 10.0:
> None for this release.
> Web Element Manager Enhancements
> None for this release.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883