> P-GW Service Configuration Mode Commands
> The P-GW (PDN Gateway) Service Configuration Mode is used to create and manage the relationship between specified services used for either GTP or PMIP network traffic.
> associate
> Associates the P-GW service with specific pre-configured services and/or policies configured in the same context.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> associate { egtp-service name [ lma-service name ] | lma-service name [ egtp-service name ] | qci-qos-mapping name }
> no associate { egtp-service | lma-service | qci-qos-mapping }
> no
> Removes the selected association from this service.
> { egtp-service name [ lma-service name ] | lma-service name [ egtp-service name ] }
> egtp-service name [ lma-service name ]: Specifies that the P-GW service is to be associated with an existing eGTP service within this context. name must be from 1 to 63 alpha and/or numeric characters and be an existing eGTP service.
> Configure an associated LMA service name to support handoffs between PMIPv6 and GTP. name must be from 1 to 63 alpha and/or numeric characters and be an existing LMA service.
> lma-service name [ egtp-service name ]: Specifies that the P-GW service is to be associated with an existing LMA service within this context. name must be from 1 to 63 alpha and/or numeric characters and be an existing LMA service.
> Configure an associated eGTP service name to support handoffs between PMIPv6 and GTP. name must be from 1 to 63 alpha and/or numeric characters and be an existing eGTP service.
> qci-qos-mapping name
> Specifies that the P-GW service is to be associated with an existing QCI-QoS mapping configuration within this context. name must be from 1 to 63 alpha and/or numeric characters and be an existing QCI-QoS mapping configuration.
> QCI-Qos mapping is typically configured in a AAA context. Refer to the QCI-QoS Mapping Configuration Mode Commands chapter for more information.
> Usage
> Use this command to associate the P-GW service with other pre-configured services and/or policies configured in the same context.
> Example
> The following command associates this service with an eGTP service called egtp1:
> associate egtp-service egtp1
> authorize-with-hss
> Identifies the function to use for subscriber authorization.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> [ default | no ] authorize-with-hss
> [ default | no ]
> Resets the command to the default setting of “authorize locally” from an internal APN authorization configuration.
> Usage
> Use this command to specify that the system will use the S6b interface to acquire subscriber authorization from a 3GPP AAA server and the HSS.
> dns-client context
> Specifies the context to use where the DNS client resides to send DNS queries.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> dns-client context name
> [ default | no ] dns-client context
> default
> Returns the command to the default setting of targeting the DNS client in the context where the P-GW service resides.
> no
> DNS query is disabled.
> name
> Specifies the name of the context where the DNS client is used for the resolution of PCSCF-FQDN received from S6b interface. name must be an existing context and be from 1 to 79 alpha and/or numeric characters.
> Usage
> Use this command to specify the context where the DNS client resides to perform P-CSCF-FQDN resolution from the S6b interface.
> Example
> The following command identifies the egress1 context as the context where the DNS client resides:
> dns-client context egress1
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> fqdn
> Configures a Fully Qualified Domain Name for this P-GW service used in messages between the P-GW and a 3GPP AAA server over the S6b interface.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> fqdn host domain_name realm realm_name
> [ default | no ] fqdn
> default
> Returns the command to the default setting of “null”.
> no
> Remove the configured FQDN from this services configuration.
> host domain_name
> Specifies the domain name of the P-GW service. domain_name must be from 1 to 255 alpha and/or numeric characters.
> realm realm_name
> Specifies the realm name of the P-GW service. realm_name must be from 1 to 255 alpha and/or numeric characters.
> Usage
> Use this command to identify the P-GW service using an FQDN required when sending messages over the S6b interface to a 3GPP AAA server.
> Example
> The following command configures the FQDN for this P-GW service as 123abc.com with a realm name of all.com:
> fqdn host 123abc realm all.com
> gx-li context
> Configures the name of the context where lawful intercept packets are delivered to the lawful intercept server.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> gx-li context name
> default gx-li context
> default
> Return the command to the default setting of the P-GW context (where this service resides).
> name
> Specifies the name of the context where the LI interface is configured for transmitting LI packets to an LI server. name must be from 1 to 79 alpha and/or numeric characters.
> Usage
> Use this command to specify the name of the context where the LI source address is configured to send packets to a LI server. By default, the P-GW context will be used.
> Important: A LI source IP address and interface must be configured in the context specified by this command.
> Example
> The following command identifies the context to use for LI server traffic as aaa3:
> gx-li context aaa3
> newcall
> Configures the P-GW to accept or reject requests for a static IP address if the address is already in use by another session.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> newcall duplicate-subscriber-requested-address { accept | reject }
> no newcall duplicate-subscriber-requested-address
> no
> Returns the command to the default setting of “reject”.
> duplicate-subscriber-requested-address { accept | reject }
> Default: reject
> accept: Specifies that the old session with the requested address will be ended to accept the new session with the same address.
> reject: Specifies that the new session requesting the same address will be rejected.
> Usage
> Use this command to configure the behavior of the P-GW service when receiving requests for static IP address already in use by other sessions.
> Important: This command is only applicable to sessions using services supporting duplicate address abort. These services include HA, GGSN, and P-GW.
> Example
> The following command allows for the acceptance of requests for static IP addresses already in use by other sessions:
> newcall duplicate-subscriber-requested-address accept
> plmn id
> Configures Public Land Mobile Network identifiers used to determine if a mobile station is visiting, roaming, or belongs to this network.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> plmn id mcc number mnc number [ primary ]
> mcc number mnc number
> mcc number: Specifies the mobile country code (MCC) portion of the PLMN’s identifier. number is the PLMN MCC identifier and must be an integer value between 100 and 999.
> mnc number: Specifies the mobile network code (MNC) portion of the PLMN’s identifier. number is the PLMN MNC identifier and can be configured to any 2 or 3 digit integer value between 00 and 999.
> primary
> When multiple PLMN IDs are configured, the primary keyword can be used to designate one of the PLMN IDs to be used for the AAA attribute.
> Usage
> The PLMN identifier is used to aid the P-GW service in the determination of whether or not a mobile station is visiting, roaming, or home. Multiple P-GW services can be configured with the same PLMN identifier. Up to five PLMN IDs can be configured for each P-GW Service.
> Example
> The following command configures the PLMN identifier with an MCC of 462 and MNC of 02:
> plmn id mcc 462 mnc 02
> session-delete-delay
> Configures a delay in terminating a session.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> session-delete-delay timeout [ msec ]
> [ default | no ] session-delete-delay timeout
> default
> Resets the command to the default setting of 10000 msecs.
> no
> Disables the feature.
> timeout msec
> Default: 10000
> Specifies the time to retain the session before terminating it. msec must be an integer from 1000 to 60000.
> Usage
> Use this command to set a delay to provide session continuity in case of break-before-make scenario.
> Example
> The following command sets the session delete delay to the default setting of 10,000 msecs:
> session-delete-delay timeout

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883