> Adding Application and Line Cards to an Existing Installation
> This chapter provides instructions for installing additional application and line cards in an installed chassis that is processing calls.
> Important: Note that all application and line cards are hot swappable. This means that you can install or remove cards from the chassis without powering the chassis down. However, it is strongly recommended that you add system components during a maintenance window.
> Chassis Slot Numbering and Assignments
> The following figure shows the front and rear chassis slots.
> Chassis Slot Numbering (Front)
> Chassis Slot Numbering (Back)
> Important: In ASR 5000 systems, the System Management Cards (SMCs) must be installed in slots 8 and 9. Their associated line cards are the Switch Processor Input Output card (SPIO) and the Redundant Crossbar Card (RCC). Assure that the SPIOs are installed in slots 24 and 25, and the RCCs are installed in slots 40 and 41 to prevent damage to the cards or the chassis midplane.
> Important: In ASR 5000 systems, the 10 Gigabit Ethernet Line Card is a full-height line card that takes up the upper and lower slots in the back of the chassis. Use the upper slot number only when referring to installed XGLCs. Slot numbering for other installed half-height cards is maintained: 17 to 32 and 33 to 48, regardless of the number of installed XGLCs
> Adding Application Cards
> The installation procedure is identical for all application cards. This section provides the instructions for adding application cards to the chassis.
> Important: If you are adding PSCs, PSC2s, or PPCs to a live system, it is recommended that you add them two at a time. This evenly distributes software tasks between the CPUs on the cards for optimal performance. You can add single packet processing cards to a production system. However, you must reboot the system to ensure optimal operation and capacity. For this reason Cisco Systems suggests that you perform the installation during a maintenance window when a reboot will have minimal impact.
> ESD Caution: During installation, maintenance, and/or removal, wear grounding wrist straps to avoid ESD damage to the components. Failure to do so could result in damage to electrical components and could potentially void your warranty.

> Step 1 | Determine the type of application card you are installing. Each application card is identified by the text near the bottom of its front panel.

> Step 2 | Determine which chassis slot to install the card in based on the information in the Chassis Slot Numbering and Assignments section in this guide.

> Important: To achieve optimal airflow performance in minimal system deployments, populate packet processing cards from the middle of the chassis outward, leaving an empty slot between them. For example, with four packet processing cards use slots 3, 5, 12, and 14. For two packet processing cards, place them in slots 5 and 12.

> Step 3 | Remove the blanking panel, if one is installed, covering the slot.

> Step a | Use a #2 Phillips screwdriver to loosen the screw at the top of the blanking panel.

> Step b | Use a #2 Phillips screwdriver to loosen the screw at the bottom of the blanking panel.

> Step c | Holding the screws on the blanking panel, pull the blanking panel away from the chassis to expose the chassis slot.

> Caution: Do not leave chassis slots uncovered for extended periods of time. This reduces airflow through the chassis and could cause it to overheat. Make sure there is a card or blanking panel in every chassis slot at all times.

> Step 4 | Properly support the weight of the card and align it with the upper and lower card guides of the chassis slot. Gently slide the card into the slot until the levers touch the chassis frame.

> Caution: To avoid damaging the card’s interlock switch, ensure that it is completely down prior to proceeding. For additional information, refer to the Product Overview Guide. In addition, take extra care when you install packet processing cards. These cards contain heat sinks that could become loose or damaged if they come into contact with another card while the packet processing card is being inserted in the chassis slot.

> Step 5 | Push the ejector levers inward firmly and straight until the card is seated in the chassis midplane and you cannot push the ejector levers in any further. Press firmly on the card’s faceplate to ensure that it is fully seated. The card’s front panel should be flush against the chassis’ upper and lower card mounts for the slot.

> Step 6 | Raise the interlock switch on the front panel of the application card to lock the ejector tab in place. The flange on the left-side of the interlock switch prevents movement of the ejector tab when raised completely.

> Important: Make sure the interlock switch is fully raised in order to properly secure the application card’s top screw to the chassis.

> Step 7 | Use a #2 Phillips screwdriver to tighten the screws at the top and bottom of the application card’s front panel to secure the card to the chassis.

> Step 8 | Repeat step 1 through step 7 for every application card you are installing.

> Step 9 | Install blanking panels over any unused chassis slots.

> Warning: To reduce the risk of electric shock and ensure proper ventilation, blanking panels must be used to cover any chassis slot not occupied by an application card. Leere Steckplaetze muessen mit der dafuer vorgesehenen Abdeckplatte geschlossen werden, um die Luftzirkulation innerhalb des Geraets zu gewaehrleisten und um einen elektrischen Schlag zu vermeiden.

> Step a | Position the blanking panel over the unused chassis slot(s).

> Step b | Position the blanking panel over the unused chassis slot.

> Step c | Use a #2 Phillips screwdriver to tighten the screw at the top of the blanking panel to secure the panel to the chassis.

> Step d | Use a #2 Phillips screwdriver to tighten the screw at the bottom of the blanking panel to secure the panel to the chassis.

> Step e | Repeat step a through step d for any additional unused chassis slots.

> Step 10 | Proceed to the next section of this chapter for instructions on adding the respective line card(s) for every application card just installed.

> Adding Half-Height Line Cards
> This section provides instructions for adding half-height line cards to the chassis. For instructions on adding full-height 10 Gigabit Ethernet Line Cards (XGLCs), see the next section.
> ESD Caution: During installation, maintenance, and/or removal, wear grounding wrist straps to avoid ESD damage to the components. Failure to do so could result in damage to electrical components and could potentially void your warranty.

> Step 1 | Determine the type of line card you are installing. Each line card is identified by the label near the bottom of its front panel.

> Step 2 | Determine which chassis slot to install the card in based on the information in the Chassis Slot Numbering and Assignments section of this guide.

> Step 3 | Remove the blanking panel covering the slot:

> Step a | Use a #2 Phillips screwdriver to loosen the screw at the top of the blanking panel.

> Step b | Use a #2 Phillips screwdriver to loosen the screw at the bottom of the blanking panel.

> Step c | Hold the screws on the blanking panel, and pull the blanking panel away from the chassis to expose the chassis slot.

> Caution: Do not leave chassis slots uncovered for extended periods of time. This reduces airflow through the chassis, which could cause it to overheat. Install a card or a blanking panel s in every chassis slot.

> Step 4 | Hold the card by its ejector levers and align the card with the upper and lower card guides of the chassis slot. Gently slide it into the slot until the levers touch the chassis frame.

> Caution: To avoid damaging the card’s interlock switch, ensure that it is completely down prior to proceeding. For additional information, refer to the Product Overview Guide.

> Step 5 | Push the ejector levers inward firmly until the card is firmly seated in the chassis midplane and the ejector levers can be pushed in no further. Press firmly on the card’s faceplate to ensure that it is fully seated. The card’s from panel should be flush against the chassis’ upper and lower card mounts for the slot.

> Step 6 | Raise the interlock switch on the front panel of the line card to lock the ejector tab in place. The flange on the left-side of the interlock switch prevents movement of the ejector tab when raised completely.

> Step 7 | Use a #2 Phillips screwdriver to tighten the screws at the top and bottom of the line card’s front panel to secure the card to the chassis.

> Step 8 | Repeat step 1 through step 7 for every other line card that to be installed.

> Step 9 | Install blanking panels over any unused chassis slots.

> Warning: To reduce the risk of electric shock and to ensure proper ventilation, blanking panels must be used to cover any chassis slot that is not occupied by an application card. Leere Steckplaetze muessen mit der dafuer vorgesehenen Abdeckplatte geschlossen werden, um die Luftzirkulation innerhalb des Geraets zu gewaehrleisten und um einen elektrischen Schlag zu vermeiden.

> Step a | Position the blanking panel over the unused chassis slot(s).

> Step b | Use a #2 Phillips screwdriver to tighten the screw at the top of the blanking panel to secure the panel to the chassis.

> Step c | Use a #2 Phillips screwdriver to tighten the screw at the bottom of the blanking panel to secure the panel to the chassis.

> Step 10 | Refer to one of the following chapters in this guide for information on cabling the line cards you just installed.

> Line Card | Chapter
> Switch Processor Input/Output | Cabling the Switch Processor Input/Output Line Card
> Ethernet 10/100 | Cabling the Ethernet 10/100 Line Card
> Ethernet 1000 | Cabling the Gigabit Ethernet Line Cards
> Quad Gigabit Ethernet Line Card (QGLC)
> 10 Gigabit Ethernet Line Cards
> Optical (ATM) | Cabling the Optical (ATM) Line Card
> Channelized Line Card Interfaces | Cabling the Channelized Line Card

> ‌
> Adding the 10 Gigabit Ethernet Line Card
> The 10 Gigabit Ethernet Line Card (XGLC) is a full-height line card that gets installed in the rear slots of the ASR 5000 chassis. It provides a single Small Form-factor Pluggable+ (SFP+) 10 Gigabit Ethernet interface for network connectivity.
> There are two versions of the XGLC:

> • | XGLC SR: 10GBase-SR modules have a center wavelength of 850nm with an LC optical connector. They can drive up to 300 meters using 50/125um fiber (MMF), and up to 33 meters using 62.5/125um fiber (MMF).

> • | XGLC LR: 10GBase-LR modules have a center wavelength of 1310nm with an LC optical connector. They can drive up to 10 kilometers using 50/125um fiber (SMF).

> Install XGLCs behind PSCs, PSC2s, or PPCs. You can install a maximum of six XGLCs in the chassis.
> Installing the XGLC
> Since the XGLC is a full-height card, it requires two line card slots: an upper chassis slot and the lower chassis slot directly beneath it. For example, if a PSC2 is installed in slot 1, its corresponding XGLC would be installed in slots 17 and 33.
> Note that when you refer to and XGLC or entering its slot location in a command, use the upper slot number only.
> ESD Caution: During installation, maintenance, and/or removal, wear grounding wrist straps to avoid ESD damage to the components. Failure to do so could result in damage to electrical components and could potentially void your warranty.

> Step 1 | Power down the chassis if it is currently in operation.

> Step 2 | Verify that the card you are installing is an XGLC. Each line card is identified by the text near the bottom of its front panel. The XGLC’s label displays either Ethernet 10G SR or Ethernet 10G LR.

> Step 3 | Determine the chassis slot in which the line card will be installed.

> Step 4 | Remove the half-height blanking panel covering the upper chassis slot, if one is installed.

> Step a | Use a #2 Phillips screwdriver to loosen the screw at the top of the blanking panel.

> Step b | Use a #2 Phillips screwdriver to loosen the screw at the bottom of the blanking panel.

> Step c | Hold the screws on the blanking panel, and pull the blanking panel away from the chassis to expose the chassis slot.

> Step 5 | Repeat step 3 to remove the half-height blanking panel covering the chassis slot directly below the slot exposed in the previous step.

> Caution: Do not leave chassis slots uncovered for extended periods of time. This reduces airflow through the chassis, which could cause it to overheat. Install a card or a blanking panel s in every chassis slot.

> Step 6 | Remove the half-height card guide separating the exposed upper and lower chassis slots.

> Important: Save all of the items you remove in this step in the event that you wish to re-populate these slots with half-height cards at a later time.

> Step a | Remove the two gasket strips to allow access to the screws beneath. Save the gasket strips.

> Step b | Using a Philips 4-40 (#1) screwdriver, loosen the two screws that secure the half-height card guide ejector rail/cap. Save the screws for later use.

> Step c | Remove the half-height card guide ejector rail/cap.

> Step d | Using only the screwdriver provided with the XGLC, loosen the screw that secures the half-height card guide to the chassis mid-plane.

> Step e | Gently pull the half-height card guide out of the chassis.

> Important: You may need to slightly angle the guide when you slide it out of the chassis to unlatch it.

> Step 7 | Properly support the weight of the card and align it with the upper and lower card guides of the chassis slot. Gently slide the card into the slot until the levers touch the chassis frame.

> Caution: To avoid damaging the card’s interlock switch, ensure that it is completely down prior to proceeding. For additional information, refer to the Product Overview Guide.

> Step 8 | Push the ejector levers inward firmly until the card is firmly seated in the chassis midplane and the ejector levers can be pushed in no further. Press firmly on the card’s faceplate to ensure that it is fully seated. The card’s front panel should be flush against the chassis’ upper and lower card mounts for the slot.

> Step 9 | Raise the interlock switch on the front panel of the line card to lock the ejector tab in place. The flange on the left-side of the interlock switch prevents movement of the ejector tab when raised completely.

> Important: The interlock switch must be fully raised in order to properly secure the line card’s top screw to the chassis.

> Step 10 | Use a #2 Phillips screwdriver to tighten the screws at the top and bottom of the line card’s front panel to secure the card to the chassis.

> Step 11 | Repeat step 1 through step 10 for every other line card that to be installed.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883