> Global Title Translation Address-Map Configuration Mode Commands
> The Global Title Translation (GTT) Address-Map configuration mode provides the commands to create, configure, and manage a specific GTT address map database.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> associate
> This command associates (links) the global title translation (GTT) address-map with a specific GTT association, which includes the translation action rules.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> associate gtt-association assoc_num action id id
> no association
> no
> Removes the association definition from the GTT address-map configuration.
> gtt-association assoc_num
> Identifies a specific GTT association to link (associate) with the GTT address-map.
> assoc_num: Must be an integer from 1 to 16.
> action id id
> Identifies a specific action defined in the GTT association database configuration.
> id: Must be an integer from 1 to 8.
> Usage
> Create an association between a specific translation action rule in a specific GTT association and this GTT address-map.
> Example
> associate gtt-association 1 action id 1
> description
> This command defines a descriptive string to facilitate identification of this particular global title translation (GTT) address-map. This is used for operator reference only.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> description string
> no description
> no
> Removes the description string from the current global title translation address-map configuration.
> string
> Specifies the alphanumeric string that is stored. must be from 1 through 127 alphanumeric characters. Strings with spaces must be enclosed in double-quotes. See the example below.
> Usage
> Use this command to set a description for reference by operators.
> Example
> description “GTT for Finnish national carrier.”
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> gt-address
> Configures the SCCP global title address.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gt-address gt_address
> no gt-address
> no
> Removes the GT address from the GTT address-map configuration.
> gt_address
> Up to 15 digits.
> Usage
> Define the SCCP short address.
> Example
> gt-address 01040552873424
> mode
> Configures the mode of operation of the SCCP entities.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> mode [ dominant | loadshare ]
> dominant
> This instructs the system to maintain the associated entity as the primary traffic pipe.
> loadshare
> This instructs the system to distribute the traffic load.
> Usage
> This command configure load balance for the system.
> Example
> mode loadshare
> out-address
> Identifies the out-going address of the SCCP entity. After this command is completed, the system enters the Out-Address configuration mode. Refer to the Out-Address Configuration Mode chapter for information about commands to define the out-address.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> out-address name
> no out-address
> no
> Removes the out-address definition from the GSS address-map configuration.
> name
> Defines a unique string to identify the out-going address using 1 to 63 alphanumeric characters.
> Usage
> Use this command to identify the address of the SCCP in the GTT configuration. This command also provides access to the Out-Address configuration mode so that the parameters for the out-going SCCP can be configured and maintained.
> Example
> out-address SCCP_London

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883