> show egtp
> This chapter includes the show egtp command output tables.
> show egtpc peers interface
> show egtpc peers interface Command Output Descriptions

> Field | Description
> Status | The status of the GTPC session. A: Online/Active I: Offline/Inactive
> GTPC Echo | Displays whether GTPC echo is enable or not. D: Disabled E: Enabled
> Restart Counter | Displays whether restart counter messages have been sent or not. S: Sent N: Not Sent
> Peer Restart Counter | Displays the status of the peer restart counter. K: Known U: Unknown
> Type of Node | Indicates the type of node with which the interface communicates. S: SGW P: PGW M: MME G: SGSN
> Service ID | The Service ID for the eGTP service
> Peer Address | Indicates the IP address of peer service (MME/P-GW/S-GW) etc.
> Restart Counter | Indicates the restart counter value.
> No. of restarts | Indicates the number of restarts of the peer node (MME/S-GW/P-GW).
> Current sessions | Indicates the number of sessions currently active on eGTP service.
> Max sessions | Indicates the total number of sessions allowed on this eGTP service.

> ‌
> show egtpc statistics
> show egtpc statistics Command Output Descriptions

> Field | Description
> Tunnel Management Messages
> Create Session Request
> Total TX | The total number of tunnel - create session request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - create session request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted create session request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted create session request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted create session request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted create session request messages received by this system, the specified service, or the specified interface.
> Create Session Response
> Total TX | The total number of tunnel - create session response messages sent by this system, a specified service, or a specified interface.
> Total RX | The total number of tunnel - create session response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted create session response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create session response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted create session request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create session response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - create session response - denied messages sent by this system, the specified service, or the specified interface.
> Modify Bearer Request
> Total TX | The total number of tunnel - modify bearer request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - modify bearer request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted modify bearer request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted modify bearer request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted modify bearer request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted modify bearer request messages received by this system, the specified service, or the specified interface.
> Modify Bearer Response
> Total TX | The total number of tunnel - modify bearer response messages sent by this system, a specified service, or a specified interface.
> Total RX | The total number of tunnel - modify bearer response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted modify bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted modify bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted modify bearer request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted modify bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - modify bearer response - denied messages sent by this system, the specified service, or the specified interface.
> Delete Session Request
> Total TX | The total number of tunnel - delete session request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - delete session request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted delete session request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted delete session request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted delete session request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted delete session request messages received by this system, the specified service, or the specified interface.
> Delete Session Response
> Total TX Accepted Denied | The total number of tunnel - initially transmitted delete session response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted delete session response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Total RX Accepted Denied | The total number of tunnel - initially transmitted delete session request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted delete session response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Downlink Data Notification Request
> Total TX | The total number of tunnel - downlink data notification request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - downlink data notification request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted downlink data notification request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted downlink data notification request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted downlink data notification request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted downlink data notification request messages received by this system, the specified service, or the specified interface.
> Downlink Data Notification Response
> Total TX | The total number of tunnel - downlink data notification response messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - downlink data notification response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted downlink data notification response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted downlink data notification response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted downlink data notification response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted downlink data notification response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted downlink data notification response messages sent by the system, the specified service, or the specified interface.
> Downlink Data Failure Indication
> Initial TX | The total number of tunnel - initial downlink data failure indication messages sent by this system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initial downlink data failure indication messages received by this system, the specified service, or the specified interface.
> Update User Plane Request
> Total TX | The total number of tunnel - update user plane request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - update user plane request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted update user plane request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted update user plane request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted update user plane request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted update user plane request messages received by this system, the specified service, or the specified interface.
> Update User Plane Response
> Total TX | The total number of tunnel - update user plane response messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - update user plane response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted update user plane response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update user plane response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted update user plane response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update user plane response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted update user plane response messages sent by the system, the specified service, or the specified interface.
> Create Bearer Request
> Total TX | The total number of tunnel - create bearer request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - create bearer request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted create bearer request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted create bearer request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted create bearer request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted create bearer request messages received by this system, the specified service, or the specified interface.
> Create Bearer Response
> Total TX | The total number of tunnel - create bearer response messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - create bearer response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted create bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted create bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted create bearer response messages sent by the system, the specified service, or the specified interface.
> Update Bearer Request
> Total TX | The total number of tunnel - update bearer request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - update bearer request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted update bearer request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted update bearer request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted update bearer request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted update bearer request messages received by this system, the specified service, or the specified interface.
> Update Bearer Response
> Total TX | The total number of tunnel - update bearer response messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - update bearer response messages received by this system, the specified service, or the specified interface.
> Initial TX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Initial RX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Delete Bearer Request
> Total TX | The total number of tunnel - delete bearer request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - delete bearer request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted delete bearer request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted delete bearer request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted delete bearer request messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted delete bearer request messages received by this system, the specified service, or the specified interface.
> Delete Bearer Response
> Total TX Accepted Denied | The total number of tunnel - delete bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
> Total RX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
> Delete Bearer Command
> Total TX | The total number of tunnel - delete bearer command messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - delete bearer command messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted delete bearer command messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted delete bearer command messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted delete bearer command messages sent by the system, the specified service, or the specified interface.
> Retrans RX | The total number of tunnel - retransmitted delete bearer command messages received by this system, the specified service, or the specified interface.
> Delete Bearer Failure Indication
> Total TX | The total number of tunnel - delete bearer failure indication messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of tunnel - delete bearer failure indication messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of tunnel - initially transmitted delete bearer failure indication messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of tunnel - initially transmitted delete bearer failure indication messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of tunnel - retransmitted delete bearer failure indication messages sent by the system, the specified service, or the specified interface.
> Path Management Messages
> Echo Request
> Total TX | The total number of path - echo request messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of path - echo request messages received by this system, the specified service, or the specified interface.
> Initial TX | The total number of path - initially transmitted echo request messages sent by the system, the specified service, or the specified interface.
> Initial RX | The total number of path - initially transmitted echo request messages received by the system, the specified service, or the specified interface.
> Retrans TX | The total number of path - retransmitted echo request messages sent by the system, the specified service, or the specified interface.
> Echo Response
> Total TX | The total number of path - echo response messages sent by this system, the specified service, or the specified interface.
> Total RX | The total number of path - echo response messages received by this system, the specified service, or the specified interface.

> ‌
> show egtp-service all
> show egtp service all Command Output Descriptions

> Field | Description
> Service name | The name of the service configured in the named context.
> Service-ID | A system generated ID number applied to the service.
> Context | The name of the context where the service is configured.
> Interface Type | The type of LTE interface this service is supporting.
> Status | The status of the service, i.e., “STARTED”.
> Restart Counter |
> Message Validation Mode | The type of IE validation to be performed on messages received by this service.
> GTPC Retransmission Timeout | The number of seconds between the re-sending of GTP-C echo messages.
> GTPC Maximum Request Retransmissions | The number of control packet request message retransmissions that can be sent before an error condition is established.
> GTPC IP QOS DSCP value | The IP QoS DSCP per-hop behavior to be marked on the outer header of signalling packets originating from the LTE component.
> GTPC Echo | Identifies if GTP-C echo messages will be sent.
> GTPC Echo Interval | The duration between the sending of GTP-C echo messages.
> GTPU Retransmission Timeout | The number of seconds between the re-sending of GTP-U echo messages
> GTPU Maximum Request Retransmissions | The number of user data packet request message retransmissions that can be sent before an error condition is established.
> GTPU Echo | Identifies if GTP-U echo messages will be sent.
> GTP-C Bind Address | The IP address of the interface to which this service is bound.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883