> BCMCS Schema Statistics
> The BCMCS schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> BCMCS Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the BCMCS configuration. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the BCMCS configuration. This is an internal reference number. | Int32
> servname | The name of the BCMCS service for which the statistics are displayed. | String
> srsp-recv-total | The total number of service requests received. | Int32
> srsp-accept-total | The total number of service requests accepted. | Int32
> srsp-denied-total | The total number of service requests that were denied. | Int32
> srsp-reply-total | The total number of service replies sent. | Int32
> srsp-discard-total | The total number of service requests that were discarded. | Int32
> srsp-accept-initial | The total number of initial service requests received and accepted. | Int32
> srsp-recv-initial | The total number of initial service requests received. | Int32
> srsp-denied-initial | The total number of initial service requests received and rejected. | Int32
> srsp-discard-initial | The total number of initial service requests discarded. | Int32
> srsp-accept-renew | The total number of service registration requests accepted. | Int32
> srsp-denied-renew | The total number of renewal service requests denied. | Int32
> srsp-recv-renew | The total number of service registration requests received. | Int32
> srsp-discard-renew | The total number of service request renewals received and discarded. | Int32
> srsp-send-error | The total number of service replies for which errors were experienced during transmission. | Int32
> srsp-decode-error | The total number of service requests that had decode errors. | Int32
> srsp-unhandled | The total number of service requests that had unhandled errors. | Int32
> srsp-deny-unspec | The total number of service requests that were denied for an unspecified reason. | Int32
> srsp-deny-auth | The total number of service requests that were denied because the mobile node failed authentication. | Int32
> srsp-deny-idmismatch | The total number of denied service updates that were sent due to identification mismatch. | Int32
> srsp-deny-unknownbsn | The total number of service requests that were denied due to an unknown BSN address. | Int32
> srsp-deny-noresource-nosessmgr | The total number of service requests denied due to insufficient resource, no session manager reported per service. | Int32
> srsp-deny-noresource-nomem | The total number of service requests denied due to Insufficient resource, no memory reported per service. | Int32
> srsp-deny-noresource-sessmgrretried | The total number of service requests denied due to Insufficient resource, session managers retried reported per service. | Int32
> srsp-deny-noresource-inputq | The total number of service requests denied due to Insufficient resource, input queue exceeded reported per service. | Int32
> srsp-deny-badrequest-alrdorm | The total number of service requests denied due to poorly formed request, session already dormant reported per service. | Int32
> srsp-deny-badrequest-alractive | The total number of service requests denied due to poorly formed request, already active reported per service. | Int32
> srsp-deny-badrequest-other | The total number of service requests denied due to poorly formed request, other reason reported per service. | Int32
> srsp-deny-cong-adminprohib | The total number of denied service replies that were denied due to administrative prohibition due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> srsp-deny-cong-unknownbsn | The total number of denied service replies that were denied due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> num-sessions | The current total number of BCMCS sessions. | Int32
> recv-total | The total number of registration requests received. | Int32
> accept-total | The total number of registration requests accepted. | Int32
> denied-total | The total number of registration requests denied. | Int32
> reply-total | The total number of registration replies sent. | Int32
> discard-total | The total number of registration requests that were discarded. | Int32
> accept-initial | The total number of initial registration requests received and accepted. | Int32
> recv-initial | The total number of initial registration requests received. | Int32
> denied-initial | The total number of initial registration requests received and rejected. | Int32
> discard-initial | The total number of initial registration requests discarded. | Int32
> accept-renew | The total number of renewal registration requests accepted. | Int32
> denied-renew | The total number of renewal registration requests denied. | Int32
> discard-renew | The total number of registration request renewals received and discarded. | Int32
> recv-renew | The total number of renewal registration requests received. | Int32
> active-start-renew | The total number of ACTIVE START registration request renewals received. | Int32
> active-stop-renew | The total number of ACTIVE STOP registration request renewals received. | Int32
> accept-dereg | The total number of requests for de-registration accepted. | Int32
> denied-dereg | The total number of requests for de-registration denied. | Int32
> discard-dereg | The total number of requests for de-registration discarded. | Int32
> recv-dereg | The total number of de-registration request renewals received. | Int32
> active-stop-dereg | The total number of ACTIVE STOP de-registration request renewals received and accepted. | Int32
> send-error | The total number of registration replies for which errors were experienced during transmission. | Int32
> hash-error | The total number of registration requests that had internal hash lookup errors. | Int32
> decode-error | The total number of registration requests that had decode errors. | Int32
> unhandled | The total number of registration requests that had unhandled errors. | Int32
> seqerror | The total number of registration requests that had sequence numbers that were not acceptable. | Int32
> deny-unspec | The total number of registration requests that were denied using reply code of 80H (Registration Denied - reason unspecified) | Int32
> deny-adminprohib | The total number of registration requests that were denied using reply code of 81H (Registration Denied - administratively prohibited). | Int32
> deny-noresource | The total number of registration requests that were denied using reply code of 82H (Registration Denied - insufficient resources). | Int32
> deny-auth | The total number of registration requests that were denied using reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
> deny-idmismatch | The total number of registration requests that were denied using reply code of 85H (Registration Denied - identification mismatch). | Int32
> deny-badrequest | The total number of registration requests that were denied using reply code of 86H (Registration Denied - poorly formed request). | Int32
> deny-unknownbsn | The total number of registration requests that were denied due to an unknown BSN address. | Int32
> deny-revtununavail | The total number of registration requests that were denied using reply code of 89H (Registration Denied - requested reverse tunnel unavailable). | Int32
> deny-revtunreq | The total number of registration requests that were denied using reply code of 8AH (Registration Denied - reverse tunnel is mandatory and “T”-bit not set). | Int32
> deny-unrecogvend | The total number of registration requests that were denied using reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE). | Int32
> deny-sessclosed | The total number of registration requests that were denied using an error code 0x8E for absent RP sessions | Int32
> deny-bsninfo | The total number of registration requests that were denied because BSN information was unavailable. | Int32
> deny-noresource-nosessmgr | The total number of requests denied due to Insufficient resource, no session manager reported per service. | Int32
> deny-noresource-nomem | The total number of requests denied due to Insufficient resource, no memory reported per service. | Int32
> deny-noresource-sessmgrretried | The total number of requests denied due to Insufficient resource, session managers retried reported per service. | Int32
> deny-noresource-inputq | The total number of requests denied due to Insufficient resource, input queue exceeded reported per service. | Int32
> deny-badrequest-alrdorm | The total number of requests denied due to poorly formed request, session already dormant reported per service. | Int32
> deny-badrequest-alractive | The total number of requests denied due to poorly formed request, already active reported per service. | Int32
> deny-badrequest-other | The total number of requests denied due to poorly formed request, other reason reported per service. | Int32
> deny-cong-drop | The total number of denied registration replies discarded due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> deny-cong-adminprohib | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> deny-cong-unknownbsn | The total number of denied registration replies due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> upd-total | The total number of registration updates that were transmitted. | Int32
> upd-accept | The total number of registration updates that were accepted by the PCF. | Int32
> upd-denied | The total number of registration updates that were denied. | Int32
> upd-unack | The total number of registration updates that were not acknowledged. | Int32
> upd-trans | The total number of initial registration updates that were transmitted. | Int32
> upd-ttlnoretrans | The total number of registration updates that were not re-transmitted due to TTL expiration. | Int32
> upd-retrans | The total number of registration updates that were re-transmitted. | Int32
> upd-received | The total number of registration updates that were received | Int32
> upd-ack-received | The total number of registration acknowledgements that were received. | Int32
> upd-discard | The total number of registration acknowledgements that were discarded. | Int32
> upd-senderror | The total number of registration updates for which errors were experienced during transmission. | Int32
> upd-lifetime | The total number of registration updates that the send reason was Lifetime Expiry reported per service. | Int32
> upd-uplyrinit | The total number of registration updates that were initiated by upper processing layers. | Int32
> upd-other | The total number of registration updates that were sent due to reasons other than those listed here. | Int32
> upd-smgrexit | The total number of registration updates that the send reason was that the session manager exited reported per service. | Int32
> upddeny-unspec | The total number of denied registration updates that were sent with a reply code of 80H (Registration Denied - reason unspecified). | Int32
> upddeny-adminprohib | The total number of denied registration updates that were sent with a reply code of 81H (Registration Denied - administratively prohibited). | Int32
> upddeny-auth | The total number of denied registration updates that were sent with a reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
> upddeny-idmismatch | The total number of denied registration updates that were sent with a reply code of 85H (Registration Denied - identification mismatch). | Int32
> upddeny-badrequest | The total number of denied registration updates that were sent with a reply code of 86H (Registration Denied - poorly formed request). | Int32
> sec-violations | The total number of security violations that occurred. | Int32
> sec-badauth | The total number of security violations that occurred due to a mis-computed authentication field. | Int32
> sec-badid | The total number of security violations that occurred due to a bad ID. | Int32
> sec-badspi | The total number of security violations that occurred due to the receipt of a Security Parameter Index (SPI) that was in the reserved range (0 through 255). | Int32
> sec-mnhaauth | The total number of security violations that occurred due to missing mobile node-home agent authentication extensions. | Int32
> sec-regupdate | The total number of security violations that occurred due to missing registration update authentication extensions. | Int32
> disc-absent | The total number of registration acknowledgements that were discarded due to the session having been already ended because the acknowledgement was late. | Int32
> disc-nomem | The total number of registration acknowledgements that were discarded due to insufficient memory. | Int32
> disc-malform | The total number of registration acknowledgements that were discarded due to being poorly formed. | Int32
> disc-authfail | The total number of registration acknowledgements that were discarded due to the mobile node failing authentication. | Int32
> disc-bounce | The total number of internal communication messages between an A11 Manager task and a Session Manager task that bounced (were not successfully sent). | Int32
> disc-inputq | The number of times that the queue in which incoming calls are kept prior to being processed exceeded its capacity. | Int32
> disc-mismatchid | The total number of discarded registration acknowledgements due to reply code 85H (Registration Denied - identification mismatch). | Int32
> disc-invpktlen | The total number of registration acknowledgements that were discarded due to having an invalid packet length. | Int32
> disc-misc | The number of registration acknowledgements that were discarded due to reasons other than those listed above. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883