> RADIUS Attribute Definitions
> This chapter presents RADIUS attribute definitions.
> Dictionary Types
> The CLI command to specify the dictionary is:
> radius dictionary [ 3gpp | 3gpp2 | 3gpp2-835 | custom X | standard | starent | starent-835 | starent-vsa1 | starent-vsa1-835 ]

> Keyword | Description
> custom XX | These dictionaries can be customized. Customization information can be obtained by contacting your local service representative. XX is the integer value of the custom dictionary. Important: RADIUS dictionary custom23 should be used in conjunction with Enhanced Charging Service (ECS). Refer to the Enhanced Charging Service Configuration and Reference Guide for more information.
> standard | This dictionary consists only of the attributes specified in RFC 2865, RFC 2866, and RFC 2869. It also supports 3GPP release 4 and 3GPP Release 5 - extended QoS format.
> 3gpp | This dictionary consists not only of all of the attributes in the standard dictionary, but also all of the attributes specified in 3GPP 32.015.
> 3gpp2 | This dictionary consists of all of the attributes in the standard dictionary, and all of the attributes specified in IS-835-A.
> 3gpp2-835 | This dictionary consists of all of the attributes in the standard dictionary, and all of the attributes specified in IS-835.
> starent-vsa1 | This dictionary consists of the 3GPP2 dictionary, and includes the vendor-specific attributes (VSAs) as well. The VSAs in this dictionary support a one-byte wide VSA Type field in order to support certain RADIUS applications. The one-byte limit allows support for only 256 VSAs (0 - 255) as shown in the following figure. This is the default dictionary.
> starent-vsa1-835 | This dictionary consists of the 3GPP2-835 dictionary, and includes the vendor-specific attributes (VSAs) as well. The VSAs in this dictionary support a one-byte wide VSA Type field in order to support certain RADIUS applications. The one-byte limit allows support for only 256 VSAs (0 - 255) as shown in the following figure.
> starent | This dictionary consists of all of the attributes in the starent-vsa1 dictionary and incorporates additional VSAs by using a two-byte VSA Type field as shown in the following figure. This dictionary is the master-set of all of the attributes in all of the dictionaries supported by the system.
> starent-835 | This dictionary consists of all of the attributes in the starent-vsa1-835 dictionary and incorporates additional VSAs by using a two-byte VSA Type field. This dictionary is the master-set of all of the attributes in all of the -835 dictionaries supported by the system.

> ‌
> Difference in VSA Value Lengths per Dictionary
> Important: Customer-specific attributes are not documented in this reference. For information on customer-specific attributes, please contact your local service representative.
> Important: The length documented for each attribute is the length of the attribute’s Value field (data portion) and not length of the attribute (Type + Length + Value fields).
> Attributes
> Important: RADIUS attributes received by the system from the RADIUS server always take precedence over local-subscriber attributes and parameters configured on the system.
> 3GPP-CAMEL-Charging-Info
> This attribute contains the received CAMEL charging information. CAMEL charging information is applicable to GGSN.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 24
> Length
> 1–255
> Value
> String
> 3GPP-CG-Address
> This attribute identifies the charging gateway address.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 4
> Length
> 4
> Value
> IPv4 address
> 3GPP-Charging-ID
> This attribute contains the charging ID for the PDP Context. This together with the GGSN-Address constitutes a unique identifier for the PDP context.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 2
> Length
> 4
> Value
> Unsigned integer
> 3GPP-Chrg-Char
> This attribute contains the charging characteristics for this PDP Context received in the Create PDP Context Request Message (only available in R99 and later releases).
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 13
> Length
> 4
> Value
> Opaque value
> 3GPP-GGSN-Address
> This attribute contains IP address of the GGSN.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 7
> Length
> 4
> Value
> IPv4 address
> 3GPP-GGSN-Mcc-Mnc
> This attribute contains the MCC-MNC of the network the GGSN belongs to.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 9
> Length
> 1–6
> Value
> Opaque value
> 3GPP-IMEISV
> This attribute identifies the International Mobile Equipment Identity and Software Version (IMEISV) number received from the mobile node (MN). It is sent in RADIUS authentication and accounting messages by GGSN.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 20
> Length
> 16
> Value
> Opaque value
> 3GPP-IMSI
> This attribute contains the IMSI identifying the mobile unit.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 1
> Length
> 1–15
> Value
> Opaque value
> 3GPP-IMSI-Mcc-Mnc
> This attribute contains the MCC and MNC extracted from the user's IMSI (first 5 or 6 digits, as applicable from the presented IMSI).
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 8
> Length
> 1–6
> Value
> Opaque value
> 3GPP-MS-TimeZone
> This attribute indicates the offset between universal time and local time in steps of 15 minutes of where the MS currently resides.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 23
> Length
> 2
> Value
> Opaque value
> 3GPP-Negotiated-DSCP
> This attribute is used to mark IP packets of PDP context on the Gi interface.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 26
> Length
> 1
> Value
> Unsigned integer
> 3GPP-Negotiated-QoS-Profile
> This attribute specifies the QoS profile to be used for the subscriber.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 5
> Length
> 1–35
> Value
> Opaque value
> 3GPP-NSAPI
> This attribute specifies the value of the NSAPI of the PDP context that the RADIUS message is related to. It is encoded as its hexadecimal representation, using 1 UTF-8 encoded digit.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 10
> Length
> 1
> Value
> Opaque value
> 3GPP-Packet-Filter
> This compound attribute specifies the Packet Filter used for the PDP context.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 25
> Length
> 65
> Value
> Contains the following four subattributes:
> Identifier
> Identifier of the packet filter.
> Type
> 1
> Length
> 1
> Value
> Unsigned integer
> Eval-Precedence
> Evaluation precedence of the packet filter.
> Type
> 2
> Length
> 1
> Value
> Unsigned integer
> Length
> Length of the packet filter.
> Type
> 3
> Length
> 1
> Value
> Unsigned integer
> Direction
> Direction of the packet filter.
> Type
> 4
> Length
> 1
> Value
> Unsigned integer
> IPv4-Address-Type
> This is a compound attribute and specifies the IPv4 Source Address and Netmask if the direction is Downlink or Destination Address & Netmask if the direction is Downlink or Destination Address & Netmask if the direction is Uplink.
> Type
> 5
> Length
> 8
> Value
> Contains the following two subattributes:
> Address
> Contains source address if direction value is set to Downlink, and destination address if direction value is set to Uplink.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> Netmask
> Contains netmask of the IPv4 address
> Type
> 2
> Length
> 4
> Value
> IPv4 address
> IPv6-Address-Type
> This is a compound attribute and specifies the IPv6 Source Address and Netmask if the direction is Downlink, or Destination Address and Netmask if the direction is Downlink, or Destination Address and Netmask if the direction is Uplink.
> Type
> 6
> Length
> 32
> Value
> Contains the following two subattributes:
> Address
> Contains source address if direction value is set to Downlink, and destination address if direction value is set to Uplink.
> Type
> 1
> Length
> 16
> Value
> Opaque value
> Netmask
> Contains the Netmask of the IPv6 address.
> Type
> 2
> Length
> 16
> Value
> Opaque value
> Protocol-Identifier-Or-Next-Header
> Specifies the IPv4 Protocol Identifier or IPv6 Next Header
> Type
> 7
> Length
> 1
> Value
> Unsigned integer
> Destination-Port
> Specifies the Destination Port number of the Packet Filter
> Type
> 8
> Length
> 2
> Value
> An integer in network byte order
> Destination-Port-Range
> This is a compound attribute and specifies the destination port range.
> Type
> 9
> Length
> 4
> Value
> Contains the following two subattributes:
> Lower
> Specifies the Lower range of the destination port of the packet filter
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> Higher
> Specifies the Higher range of the destination port of the packet filter
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> Source-Port
> Specifies the Source Port number of the packet filter
> Type
> 10
> Length
> 2
> Value
> Unsigned integer
> Source-Port-Range
> Specifies the Source Port Range
> Type
> 11
> Length
> 4
> Value
> Contains the following two subattributes:
> Lower
> Specifies Lower range of the source port of the packet filter
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> Higher
> Specifies Higher range of the source port of the packet filter
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> Security-Parameter-Index
> Specifies the IPSec Security Parameter Index(IPv6).
> Type
> 12
> Length
> 4
> Value
> Unsigned integer
> Type-Of-Service
> This is a compound attribute and specifies the Type of Service/ Traffic Class.
> Type
> 13
> Length
> 2
> Value
> Contains the following two subattributes:
> Value
> Specifies the Type of Service/Traffic Class Value.
> Type
> 1
> Length
> 1
> Value
> Unsigned integer
> Mask
> Specifies the Type of Service/Traffic Class Mask.
> Type
> 2
> Length
> 1
> Value
> Unsigned integer
> Flow-Label
> Specifies the IPv6 Flow Label.
> Type
> 14
> Length
> 3
> Value
> Opaque value
> 3GPP-PDP-Type
> This attribute identifies the PDP Context type.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 3
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | ipv4 = 0

> • | ppp = 1

> • | ipv6 = 2

> • | ipv4-or-ipv6 = 3

> 3GPP-RAT-Type
> This attribute indicates which Radio Access Technology is currently serving the UE.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 21
> Length
> 1
> Value
> Opaque value
> 3GPP-Selection-Mode
> This attribute contains the selection mode for this PDP Context received in the Create PDP Context Request message as an UTF-8 encoded character.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 12
> Length
> 1
> Value
> Opaque value
> 3GPP-Session-Stop-Ind
> The presence of this attribute indicates to the AAA server that the last PDP context of a session is released and that the PDP session has been terminated.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 11
> Length
> 1
> Value
> Opaque value
> 3GPP-SGSN-Address
> This attribute contains IP address of the SGSN.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 6
> Length
> 4
> Value
> IPv4 address
> 3GPP-SGSN-Mcc-Mnc
> For GPRS the MCC and the MNC of the SGSN.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 18
> Length
> 1–6
> Value
> String
> 3GPP-Teardown-Indicator
> If this value is set to 1 in disconnect-request, the whole correlated sessions would be disconnected.
> Type
> 16
> Vendor ID
> 10415
> VSA Type
> 19
> Length
> 1
> Value
> Opaque value
> 3GPP-User-Location-Info
> GTP user location information attribute for the subscriber session.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 22
> Length
> 8
> Value
> Opaque value
> 3GPP2-835-Release-Indicator
> 3GPP2-895- Standard Release-Indicator, reason/cause for session release.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Unknown = 0

> • | PPP-Timeout = 1

> • | Handoff = 2

> • | PPP-Termination = 3

> • | Mobile-IP-Registration-Failure = 4

> • | Active-To-Dormant = 5

> 3GPP2-Acct-Session-Time
> The total amount of time spent in the Active state, in seconds. This attribute has the same type as Acct-Session-Time, and thus conforms to IS-835.
> Type
> 46
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Active-Time
> The total amount of time spent in the Active state, in seconds.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 49
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Active-Time-Corrected
> 3GPP2 Active session time value.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 49
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Airlink-Record-Type
> This attribute indicates the most recent type of Airlink Record to be received for this subscriber's connection.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 40
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Connection-Setup = 1

> • | Active-Start = 2

> • | Active-Stop = 3

> • | SDB = 4

> • | BCMCS-Connection-Setup = 5

> • | BCMCS-Active-Start = 6

> • | BCMCS-Active-Stop = 7

> 3GPP2-Airlink-Sequence-Number
> This represents the sequence number of an Airlink Record and is incremented (modulo 256) by the PCF for each Airlink Record. The sequence number is unique for a given RP Session ID, PCF ID, and MSID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 42
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Air-QOS
> This attribute identifies airlink QOS associated with the user data. The least significant 4 bits hold the QOS priority as defined in C.S0001-A in the subscriber profile.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 39
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Allowed-Diffserv
> This attribute specifies if the user is able to mark packets with AF and/or EF. The Max Class specifies that the user may mark packets with a Class Selector Code Point that is less then or equal to Max Class.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 73
> Length
> 24
> Value
> Contains the following three subattributes:
> Flags
> Allowed DSCP flag.
> Type
> 1
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Allow_AF_EF_Exp = 0xE000

> • | Allow_AF_EF = 0xC000

> • | Allow_AF_Exp = 0xA000

> • | Allow_EF_Exp = 0x6000

> • | Allow_AF = 0x8000

> • | Allow_EF = 0x4000

> • | Allow_Exp = 0x2000

> • | Allow_None = 0x0

> Max-Class
> Allowed max dscp.
> Type
> 2
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0x0

> • | AF11 = 0x2800

> • | AF12 = 0x3000

> • | AF13 = 0x3800

> • | AF21 = 0x4800

> • | AF22 = 0x5000

> • | AF23 = 0x5800

> • | AF31 = 0x6800

> • | AF32 = 0x7000

> • | AF33 = 0x7800

> • | AF41 = 0x8800

> • | AF42 = 0x9000

> • | AF43 = 0x9800

> • | EF = 0xb800

> • | Class1 = 0x2000

> • | Class2 = 0x4000

> • | Class3 = 0x6000

> • | Class4 = 0x8000

> • | Class5 = 0xa000

> • | Class6 = 0xc000

> • | Class7 = 0xe000

> RT-Marking
> Allowed max dscp rev. tun.
> Type
> 3
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0x0

> • | AF11 = 0x2800

> • | AF12 = 0x3000

> • | AF13 = 0x3800

> • | AF21 = 0x4800

> • | AF22 = 0x5000

> • | AF23 = 0x5800

> • | AF31 = 0x6800

> • | AF32 = 0x7000

> • | AF33 = 0x7800

> • | AF41 = 0x8800

> • | AF42 = 0x9000

> • | AF43 = 0x9800

> • | EF = 0xb800

> • | Class1 = 0x2000

> • | Class2 = 0x4000

> • | Class3 = 0x6000

> • | Class4 = 0x8000

> • | Class5 = 0xa000

> • | Class6 = 0xc000

> • | Class7 = 0xe000

> 3GPP2-Allowed-Persistent-TFTs
> This attribute displays the 3GPP2 Allowed Persistent Traffic Flow Templates.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 89
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Alternate-Billing-ID
> This attribute is currently not supported.
> 3GPP2-Always-On
> This attribute, when set to Active, indicates that the subscriber's session should be kept up regardless of the idle time as long as the subscriber is reachable. Reachability is ascertained using LCP keepalive messages.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 78
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Inactive = 0

> • | Active = 1

> 3GPP2-Auth-Flow-Profile-Id
> This compound attribute is a list of flow profile IDs.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 131
> Length
> 6
> Value
> Contains the following three subattributes:
> Profile-Id-Forward
> This attribute specifies a list of Forward Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> Profile-Id-Reverse
> This attribute specifies a list of Reverse Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> Profile-Id-Bi-Direction
> This attribute specifies the list of Bi-Direction Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> 3GPP2-Auth-QoS-Profile-Id
> This attribute specifies the authorized QOS profile ID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 131
> Length
> 1
> Value
> 1
> 3GPP2-Bad-PPP-Frame-Count
> The total number of PPP frames from the MS dropped by the PDSN due to uncorrectable errors.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 25
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-BCMCS-Auth-Parameters
> This is a grouped AVP with Authentication signature, Sequence number, and timestamp required to validate each flow in a BCMCS flow registration request. Each flow is validated using the procedure described in 3GPP2 standard C.S0054-0_v1.0. This information is configured on a per subscriber basis.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 99
> Length
> 38
> Value
> Contains the following three subattributes:
> BAK-Sequence-Number
> Type
> 1
> Length
> 1
> Value
> Opaque value
> Timestamp
> Type
> 2
> Length
> 33
> Value
> Opaque value
> Auth-Signature
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-BCMCS-BSN-Session-Info
> This is a grouped AVP containing information about the established flows. This includes the multicast address, port, compression status of the flow, and the content server address.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 103
> Length
> 46
> Value
> Contains the following 11 subattributes:
> Flow-ID
> Type
> 1
> Length
> 2-4
> Value
> Opaque value
> Mcast-IP-Addr
> Type
> 2
> Length
> 4
> Value
> IPv4 address
> Mcast-Port
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> Header-Compression-Algorithm
> Type
> 4
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No_header_compression = 0

> • | ROHC_U_Mode = 1

> CID-Type-Attribute
> Type
> 5
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Small_CID = 0

> • | Large_CID = 1

> MAX-CID
> Type
> 6
> Length
> 2
> Value
> Unsigned integer
> Compression-Profile
> Type
> 7
> Length
> 2
> Value
> Unsigned integer
> MAX-Header-Size
> Type
> 8
> Length
> 2
> Value
> Unsigned integer
> MRRU
> Type
> 9
> Length
> 2
> Value
> Unsigned integer
> Content-Server-Source-IP-Address
> Type
> 10
> Length
> 4
> Value
> IPv4 address
> Content-Server-Source-IPv6-Address
> Type
> 11
> Length
> 16
> Value
> Opaque value
> 3GPP2-BCMCS-Capability
> This AVP defines the specific BCMCS protocol revision the PDSN supports.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 101
> Length
> 4
> Value
> Contains the following subattribute:
> BCMCS-Protocol-Revision
> Type
> 1
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Release_0 = 1

> 3GPP2-BCMCS-Common-Session-Info
> This is a grouped AVP which specifies the program start time, end time and the allowed registration time on a per flow basis.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 102
> Length
> 18
> Value
> Contains the following five subattributes:
> Flow-ID
> Type
> 1
> Length
> 2–4
> Value
> Opaque value
> Program-Start-Time
> Type
> 2
> Length
> 4
> Value
> Unsigned integer
> Program-End-Time
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> Program-Allowed-Registration-Time
> Type
> 4
> Length
> 4
> Value
> Unsigned integer
> Auth-Required-Flag
> Type
> 5
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Authorization_not_required = 0

> • | Authorization_required = 1

> 3GPP2-BCMCS-Flow-ID
> This attribute specifies the BCMCS_FLOW_ID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 100
> Length
> 2–4
> Value
> String
> 3GPP2-BCMCS-Flow-Transmit-Time
> The total BCMCS flow transmission time in seconds.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 107
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-BCMCS-Mcast-IP-Addr
> Contains the multicast IP address of the BCMCS flow as it would appear in the source or destination field of an IP header.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 109
> Length
> 4
> Value
> IPv4 address
> 3GPP2-BCMCS-Mcast-Port
> The multicast port for the BCMCS flow.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 110
> Length
> 2
> Value
> Unsigned integer
> 3GPP2-BCMCS-Reason-Code
> This attribute specifies the reason to send the RADIUS Access-Accept message.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 105
> Length
> 1
> Value
> Opaque value
> 3GPP2-BCMCS-RN-Session-Info
> This is a grouped AVP which contains the encryption mechanism, BAK (Broadcast access key), BAK_ID, BAK expire time and authorization required flag. This attribute specifies the session information that needs to be known only by the RN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 104
> Length
> 31
> Value
> Contains the following six subattributes:
> Flow-ID
> Type
> 1
> Length
> 2-4
> Value
> Opaque value
> BCMCS-Encryption-Mechanism-Attribute
> Type
> 2
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | High_layer_encryption_in_CS = 0

> • | Link_layer_encryption_in_RN = 1

> BCMCS-BAK-ID-Attribute
> Type
> 3
> Length
> 1
> Value
> Unsigned integer
> BCMCS-BAK
> Type
> 4
> Length
> 16
> Value
> Opaque value
> BCMCS-BAK-Expire-Time
> Type
> 5
> Length
> 4
> Value
> Unsigned integer
> BCMCS-Session-Bandwidth-attribute
> Type
> 6
> Length
> 2
> Value
> Unsigned integer
> 3GPP2-BCMCS-Subnet-VSA-Format
> This attribute is deprecated.
> 3GPP2-Beginning-Session
> 3GPP2 Beginning Session will be TRUE or FALSE depending on if this is a new session.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 51
> Length
> 4
> Value
> Enumerated integer. Supported values:

> • | False = 0

> • | True = 1

> 3GPP2-BSID
> The base station ID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 10
> Length
> 6–12
> Value
> Opaque value
> 3GPP2-Carrier-ID
> A 5 or 6-byte identifier of the visited PDSN comprising of a 3 byte Mobile Country Code (MCC) followed by a 2 or 3 byte Mobile Network Code (MNC) of the visited carrier. This value is configured locally in the visited carrier's PDSN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 142
> Length
> 5–6
> Value
> Opaque value
> 3GPP2-Comp-Tunnel-Indicator
> This attribute indicates the invocation of a compulsory tunnel established on behalf of the MS for providing private network and/or ISP access during a single packet data connection. Normal PPP sessions will show No Tunnel. L2TP, IPinIP, and IP-GRE tunnels will show Non-Secure-Tunnel. IPSEC support will show Secure-Tunnel.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 23
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No Tunnel = 0

> • | Non-Secure-Tunnel = 1

> • | Secure-Tunnel = 2

> 3GPP2-Container
> A compound attribute that encapsulates the User Data Record for an Airlink Event.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 6
> Length
> Varies
> Value
> Embedded attributes as defined in “Wireless IP Network Standard – 3GPP2.P.S0001-A-1” [6].
> Format of the 3GPP2-Container attribute:
> Embedded attributes will contain 0 or 1 of the following attributes:

> • | 3GPP2-User-Zone

> • | 3GPP2-Air-QOS

> • | NAS-IP-Address

> • | 3GPP2-Serving-PCF

> • | 3GPP2-BSID

> • | Acct-Output-Octets

> • | Acct-Output-Gigawords

> • | Acct-Input-Octets

> • | Acct-Input-Gigawords

> • | SNA1-PPP-Unfr-data-In-Oct

> • | SNA1-PPP-Unfr-data-Out-Oct

> • | 3GPP2-Bad-PPP-Frame-Count

> • | 3GPP2-Active-Time

> • | 3GPP2-Number-Active-Transitions

> • | 3GPP2-SDB-Input-Octets

> • | 3GPP2-SDB-Output-Octets

> • | 3GPP2-Num-SDB-Input

> • | 3GPP2-Num-SDB-Output

> • | 3GPP2-Num-Bytes-Received-Total

> • | 3GPP2-MIP-Sig-Octet-Count-In

> • | 3GPP2-MIP-Sig-Octet-Count-Out

> Embedded attributes inside the 3GPP2-Container attribute have the same format as those outside the 3GPP2-Container attribute.
> 3GPP2-Correlation-Id
> This attribute contains an ID that correlates all accounting sessions authorized for this NAI by this access request.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 44
> Length
> 1–253
> Value
> String
> 3GPP2-Correlation-Id-Old
> Custom-11 style correlation ID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 40
> Length
> 1–251
> Value
> Opaque value
> 3GPP2-DCCH-Frame-Size
> Specifies the DCCH frame size.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 50
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | 5s = 1

> • | 20ms = 2

> 3GPP2-Diff-Service-Class-Option
> This is the DSCP (Differentiated Service Code Point) value as defined in the 3GPP2 standard. The DSCP values are assigned for different classes of traffic so that each traffic class can be Given different priorities (QoS).
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 5
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Disconnect-Reason
> This attribute indicates the reason for disconnecting the user. This attribute may be present in the RADIUS Disconnect-request Message from Home RADIUS server to the PDSN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 96
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | MS_Mobility_Detection = 1

> • | All other values are reserved.

> 3GPP2-DNS-Server-IP-Address
> DNS server IP address. Used in custom dictionary.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 117
> Value
> Contains the following four subattributes:
> Primary-DNS-Server-IP
> Primary DNS Server IP address.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> Secondary-DNS-Server-IP
> Secondary DNS Server IP address.
> Type
> 2
> Length
> 4
> Value
> IPv4 address
> Flag
> M bit set to 1 indicates to the PDSN that Primary and Secondary IP addresses provided by the Home RADIUS server should override the Primary and Secondary IP addresses provided also by the visited RADIUS server.
> Type
> 3
> Length
> 1
> Value
> Unsigned integer
> Entity-Type
> Network Entity that inserted in the DNS server ID address. Currently the Following types are defined. HAAA = 1, VAAA = 1.
> Type
> 4
> Length
> 1
> Value
> Unsigned integer
> 3GPP2-DNS-Update-Required
> This attribute indicates whether the HA needs to send the DNS update to the DNS server.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 75
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0 — HA does not need to send DSN update

> • | Yes = 1 — HA needs to send DNS update

> 3GPP2-ESN
> Contains the Electronic Serial Number (ESN) of the Mobile Station.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 52
> Length
> 1–15
> Value
> Opaque value
> 3GPP2-FA-Address
> This attribute indicates if compulsory tunneling is to be employed on behalf of a subscriber. Usually compulsory tunneling is employed when a subscriber cannot initiate a tunnel itself, usually because the subscriber's device does not support tunneling. Contains an IP address as it would appear in the IP header.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 79
> Length
> 4
> Value
> IPv4 address
> 3GPP2-Flow-Id
> This attribute displays the 3GPP2-Flow-Id-parameter.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 144
> Value
> Contains the following two subattributes:
> Direction
> This attribute identifies the IP flow id direction.
> Type
> 1
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Forward = 0

> • | Reverse = 1

> • | Both = 2

> Flow-Id
> This attribute identifies the IP flow.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> 3GPP2-Flow-Status
> This attribute displays the 3GPP2 Flow Status.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 145
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Active = 0

> • | Inactive = 1

> 3GPP2-Forward-Fundamental-Rate
> As defined in “Wireless IP Network Standard – 3GPP2.P.S0001-A-1”.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 14
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Forward-Fundamental-RC
> The format and structure of the RADIUS channel in the forward direction. A set of forward transmission formats that are characterized by data rates, modulation characterized, and spreading rates.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 20
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Forward-Mux-Option
> Forward direction multiplexer option.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 12
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Forward-Traffic-Type
> Specifies the forward traffic type.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 17
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Primary = 0

> • | Secondary = 1

> 3GPP2-Fundamental-Frame-Size
> This attribute indicates the fundamental frame size. The fundamental channel has the choice of 5 or 20 ms size. The 5 ms frame size allows fast response for short signaling messages (short frame can be decoded quickly). However, depending on configuration, the fundamental may not be present.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 19
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | 5ms = 1

> • | 20ms = 2

> 3GPP2-Fwd-Dcch-Mux-Option
> This attribute specifies Forward DCCH Mux option.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 84
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Fwd-Dcch-Rc
> This attribute specifies Radio Configuration of the Forward Packet Data Channel.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 86
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Fwd-Pdch-Rc
> This attribute specifies Radio Configuration of the Forward Packet Data Channel.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 83
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-GMT-Timezone-Offset
> GMT- Time-Zone-Offset is 4-octet string that is interpreted as a 4-byte signed integer that indicates the current offset in seconds from GMT at the visited carrier's PDSN. The offset should be adjusted to reflect standard time or daylight saving time.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 143
> Length
> 4
> Value
> Integer
> 3GPP2-Granted-QoS
> This attribute displays the 3GPP2-Granted-QoS-Parameter.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 132
> Value
> Contains the following subattributes:
> Direction
> This attribute specifies the Granted QoS parameters received from the RAN for the flow identified by direction.
> Type
> 1
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Forward = 0

> • | Reverse = 1

> • | Both = 2

> Flow-Id
> This attribute specifies the Granted QoS parameters received from the RAN for the flow identified by FLOW_ID.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> Attribute-Set-Id
> This attribute specifies the Granted QoS parameters received from the RAN for flow verbose or non-verbose.
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> Flow-Profile-Id
> This attribute specifies the Granted QoS parameters received from the RAN for the flow profile ID.
> Type
> 4
> Length
> 2
> Value
> Unsigned integer
> Traffic-Class
> This attribute specifies the Granted QoS parameters received from the RAN for the flow traffic class.
> Type
> 5
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Unknown = 0

> • | Conversational = 1

> • | Streaming = 2

> • | Interactive = 3

> • | Background = 4

> Peak-Rate
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Peak Rate.
> Type
> 6
> Length
> 2
> Value
> Unsigned integer
> Bucket-Rate
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Bucket Rate.
> Type
> 7
> Length
> 2
> Value
> Unsigned integer
> Token-Rate
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Token Rate.
> Type
> 8
> Length
> 2
> Value
> Unsigned integer
> Max-Latency
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Max Latency.
> Type
> 9
> Length
> 2
> Value
> Unsigned integer
> Max-IP-Packet-Loss-Rate
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Packet Loss Rate.
> Type
> 10
> Length
> 2
> Value
> Unsigned integer
> Packet-Size
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Packet Size.
> Type
> 11
> Length
> 2
> Value
> Unsigned integer
> Delay-Var-Sensitive
> This attribute specifies the Granted QoS parameters received from the RAN for the flow Delay Var Sensitive.
> Type
> 12
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Not-Specified = 0

> • | Sensitive = 1

> 3GPP2-IKE-Secret
> This attribute contains the FA/HA shared secret for the IKE protocol. This attribute is salt-encrypted.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 3
> Length
> 1-247
> Value
> Opaque value
> 3GPP2-IKE-Secret-Request
> This attribute indicates if the IKE secret for the FA/HA pair is to be returned for the subscriber.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 1
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> 3GPP2-IKE-Secret-Unencrypted
> IKE Secret key from RADIUS server in Access Accept Message
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 3
> Length
> 1–247
> Value
> Opaque value
> 3GPP2-IMSI
> This is the calling Station-ID attribute. IMSI value of the mobile is being filled in. This is sent when Custom11 dictionary is selected.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 1
> Length
> 1–253
> Value
> Opaque value
> 3GPP2-Interconnect-IP
> This attribute is currently not supported.
> 3GPP2-Interconnect-QOS
> This attribute is currently not supported.
> 3GPP2-Inter-User-Priority
> This attribute displays the 3GPP2-Inter-User-Priority.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 139
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-IP-QOS
> This attribute defines the differentiated Services code points associated with the user data.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 36
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> 3GPP2-IP-Technology
> This attribute identifies whether we are using Simple IP, Mobile IP, or another technology.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 22
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Simple IP = 1

> • | Mobile IP = 2

> 3GPP2-KeyID
> This attribute contains the opaque IKE Key Identifier for the FA/HA shared IKE secret. The first eight bytes is the network-order FA IP address in hexadecimal characters. The next eight bytes is the network-order HA IP address in hexadecimal characters. The final four bytes is a timestamp in network order, indicating when the key was created, and is the number of seconds since January 1, 1970, UTC.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 8
> Length
> 20
> Value
> Opaque value
> 3GPP2-Last-Activity
> This attribute contains timestamp of the last user activity. This attribute is same as the 3GPP2-Last-User-Activity-Time standard attribute.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 80
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Max-Auth-Aggr-Bw-BET
> This attribute contains the maximum authorized aggregate bandwidth for Best Effort Traffic.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 130
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Max-Per-Fl-Pri-ForTheUser
> The maximum per flow priority for the user.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 133
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-MEID
> Mobile Equipment Identifier (MEID) uniquely identifies the mobile equipment and is the future replacement for ESN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 116
> Length
> 0–14
> Value
> Opaque value
> 3GPP2-MIP-HA-Address
> The IP address of the MIP Home Agent.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 7
> Length
> 4
> Value
> IPv4 address
> 3GPP2-MIP-Lifetime
> This VSA should be included in the RADIUS Access-Request message from the HA to the Home RADIUS/PPS if the HA is PrePaid capable. It may be included in the RADIUS Access-Accept message from the Home RADIUS/PPS to HA, in which case, the HA should include the received value in the MIP RRP sent to the PDSN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 92
> Length
> Variable, greater than 8
> Value
> Contains the following two subattributes:
> RRQ-Lifetime
> Should be included in the initial RADIUS Access-Request message and subsequent on-line RADIUS Access-Request if duration based PrePaid is provided for the session. It contains the MIP RRQ integer value lifetime received in the MIP RRQ message. In the RADIUS Access-Accept message, it contains the MIP RRQ integer value lifetime that should be used in the MIP RRP.
> Type
> 1
> Length
> 4
> Value
> Unsigned integer
> Used-Lifetime
> Should be included in the RADIUS Access-Request message at re-registration and updated RRQ (new CoA) if duration based PrePaid is provided for the session, it contains the used MIP RRQ lifetime value from an existing MIP session with the same NAI and Home Address.
> Type
> 1
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-MIP-Reverse-Tunnel-Required
> Indicates to the PDSN if MIP Reverse Tunneling is Required
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 4
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Not Required = 0

> • | Required = 1

> 3GPP2-MIP-Rev-Tunnel-Required
> Indicates to the PDSN if MIP Reverse Tunneling is required.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 4
> Length
> 4
> Value
> Enumerated integer. Supported Values are:

> • | NotRequired = 0

> • | Required = 1

> 3GPP2-MIP-Sig-Octet-Count-In
> The total number of octets in registration requests and solicitations sent by the mobile.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 46
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-MIP-Sig-Octet-Count-Out
> The total number of octets in registration replies and agent advertisements, sent to the mobile.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 47
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-MIP6-Authenticator
> The MN-AAA authenticator obtained from the MN-AAA authentication mobility option in the BU.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 134
> Length
> 12
> Value
> Opaque value
> 3GPP2-MIP6-CoA
> MIPv6 CoA received in binding update.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 119
> Length
> 16
> Value
> Opaque value
> 3GPP2-MIP6-HA
> MIPv6 Home Agent address received in binding update.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 118
> Length
> 16
> Value
> Opaque value
> 3GPP2-MIP6-HoA
> MIPv6 HoA received in binding update.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 141
> Length
> 16
> Value
> Opaque value
> 3GPP2-MIP6-HoA-Not-Authorized
> Value of 1 indicates to the HA that the HoA is not authorized to be used by HA.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 120
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | UnAuthorized = 1

> 3GPP2-MIP6-Home-Address
> Carries the assigned Home Address during MIP6 bootstrapping.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 129
> Length
> 18
> Value
> Opaque value
> 3GPP2-MIP6-Home-Agent
> Carries the assigned MIPv6 Home Agent address received during MIPv6 bootstrapping.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 140
> Length
> 18
> Value
> Opaque value
> 3GPP2-MIP6-Home-Link-Prefix
> Carries the assigned Home Link Prefix during MIP6 bootstrapping.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 128
> Length
> 2–18
> Value
> Opaque value
> 3GPP2-MIP6-MAC-Mobility-Data
> The hashed Mobility Data from the HA to the Home RADIUS server so that the Home RADIUS server can validate the MN-AAA authenticator.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 138
> Length
> 20
> Value
> Opaque value
> 3GPP2-MIP6-Mesg-ID
> Value of Message ID from Mobility message replay protection option in Binding Update.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 123
> Length
> 8
> Value
> Opaque value
> 3GPP2-MIP6-Session-Key
> This VSA carries the Integrity Key (IK) in its encrypted form, from the Home RADIUS server to the HA.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 121
> Length
> 16–64
> Value
> Opaque value
> 3GPP2-MN-AAA-Removal-Indication
> This attribute, when set to “Not Required”, indicates that the system, when acting as a Mobile-IP Foreign Agent, should remove the MN-FA challenge and the MN-AAA Authentication Extensions, when present, from the RRQ before relaying the RRQ to the Mobile-IP Home Agent.
> Vendor ID
> 26
> VSA Type
> 5535
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Allowed = 0

> • | Not-Required = 1

> 3GPP2-MN-HA-Shared-Key
> A shared key for MN-HA authentication. The MN-HA shared key is encrypted using a method based on MD5.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 58
> Length
> 1–251
> Value
> Opaque value
> 3GPP2-MN-HA-Shared-Key-No-Enc
> Contains the MN-HA shared key in plain format.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 58
> Length
> 1–251
> Value
> Opaque value
> 3GPP2-MN-HA-SPI
> The SPI for the MN-HA authentication shared key.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 57
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Mobile-Term-Orig-Ind
> Tells whether the call is mobile originated (Call initiated from mobile side) or mobile terminated (Call initiated from external towards mobile).
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 45
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Mobile-Originated = 0

> • | Mobile-Terminated = 1

> 3GPP2-Number-Active-Transitions
> This attribute counts the total number of non-active to active transitions by the user.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 30
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Num-Bytes-Received-Total
> This attribute counts all bytes received in the reverse direction by the HDLC layer in the PDSN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 43
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Num-SDB-Input
> This attribute counts the total number of Short Data Burst transactions to the user.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 33
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Num-SDB-Output
> This attribute counts the total number of Short Data Burst transactions from the user.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 34
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Pre-Paid-Accounting-Quota
> This attribute specifies the characteristics for PrePaid accounting of the volume and/or duration of a packet data session. It should be present in all on-line RADIUS Access-Request and on-line RADIUS Access-Accept messages and may be included in other RADIUS Access-Accept messages. Non-used Sub-Types by the PPC and PPS should be omitted.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 90
> Length
> Variable, greater than 8.
> Value
> Contains the following nine subattributes:
> Quota-Identifier
> The Quota-IDentifier Sub-Type is generated by the PrePaid server at allocation of a Volume and/or Duration Quota. The on-line quota update RADIUS Access-Request message sent from the PPC to the PPS should include a previously received Quota-Identifier.
> Type
> 1
> Length
> 8
> Value
> Unsigned integer
> Volume-Quota
> The optional Volume-Quota Sub-Type is only present if Volume Based charging is used. In RADIUS Access-Accept message (PPS to PPC direction), it indicates the Volume (in octets) allocated for the session by the PrePaid server. In on-line RADIUS Access-Request message (PPC to PPS direction), it indicates the total used volume (in octets) for both forward and reverse traffic applicable to PrePaid accounting13. If a Tariff Switch condition was reached during the session, this Sub-Type contains the complete (before and after) volume used, while the VolumeUsedAfterTariffSwitch attribute contains the volume used after the tariff switch condition.
> Type
> 2
> Length
> 4
> Value
> Unsigned integer
> Volume-Quota-Overflow
> The optional Volume-Quota-Overflow Sub-Type is used to indicate how many times the VolumeQuota counter has wrapped around 2^32 over the course of the service being provided.
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> Volume-Threshold
> The Volume-Threshold Sub-Type should always be present if VolumeQuota is present in a RADIUS Access-Accept message (PPS to PPC direction). It is generated by the PrePaid server and indicates the volume (in octets) that should be used before requesting quota update. This threshold should not be larger than the VolumeQuota.
> Type
> 4
> Length
> 4
> Value
> Unsigned integer
> Volume-Threshold-Overflow
> The optional Volume-Threshold-Overflow Sub-Type is used to indicate how many times the VolumeThreshold counter has wrapped around 2^32 over the course of the service being provided.
> Type
> 5
> Length
> 2
> Value
> Unsigned integer
> Duration-Quota
> The optional Duration-Quota Sub-Type is only present if Duration Based charging is used. In RADIUS Access-Accept message (PPS to PPC direction), it indicates the Duration (in seconds) allocated for the session by the PrePaid server. In on-line RADIUS Access-Accept message (PPC to PPS direction), it indicates the total Duration (in seconds) since the start of the accounting session related to the QuotaID.
> Type
> 6
> Length
> 4
> Value
> Unsigned integer
> Duration-Threshold
> The Duration-Threshold Sub-Type should always be present if DurationQuota is present in a RADIUS Access-Accept message (PPS to PPC direction). It represents the duration (in seconds) that should be used by the session before requesting quota update. This threshold should not be larger than the DurationQuota and should always be sent with the DurationQuota.
> Type
> 7
> Length
> 4
> Value
> Unsigned integer
> Update-Reason
> The Update-Reason Sub-Type should be present in the on-line RADIUS Access-Request message (PPC to PPS direction). It indicates the reason for initiating the on-line quota update operation. Update reasons 4, 5, 6, 7 and 8 indicate that the associated resources are released at the client side, and therefore the PPS should not allocate a new quota in the RADIUS Access-Accept message.
> Type
> 8
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Pre-Initialization = 1

> • | Initial-Request = 2

> • | Threshold-Reached = 3

> • | Quota-Reached = 4

> • | Remote-Forced-Disconnect = 5

> • | Client-Service-Termination = 6

> • | Main-SI-Released = 7

> • | Service-Instance-Not-Established = 8

> • | Tariff-Switch-Update = 9

> • | Incorrect-Quota-Type-Received = 10

> • | Poorly-Formed-Quota-Attribute = 11

> Pre-Paid-Server
> The optional, multi-value Pre-Paid-Server indicates the address of the serving PrePaid System. If present, the Home RADIUS server uses this address to route the message to the serving PrePaid Server. The attribute may be sent by the Home RADIUS server. If present in the incoming RADIUS Access-Accept message, the PDSN should send this attribute back without modifying it in the subsequent RADIUS Access-Request message, except for the first one. If multiple values are present, the PDSN should not change the order of the attributes.
> Type
> 9
> Length
> 4
> Value
> IPv4 address
> 3GPP2-Pre-Paid-Acct-Capability
> This attribute specifies the capability for PrePaid accounting for a packet data session. It contains the possible capabilities of the PrePaid client and the selected (by the PrePaid server) capability for the session. The absence of this VSA indicates that the client is not capable of PrePaid Accounting and the session should not use PrePaid accounting.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 91
> Length
> Variable, greater than 8
> Value
> Contains the following two subattributes:
> Available-In-Client
> The optional Available-In-Client Sub-Type, generated by the PrePaid client, indicates the PrePaid Accounting capabilities of the client in the PDSN or HA and should be bitmap encoded.
> Type
> 1
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Supported_None = 0

> • | Supported_Volume = 1 — PrePaid Accounting for Volume supported

> • | Supported_Duration = 2 — PrePaid Accounting for Duration supported

> • | Supported_Volume_And_Duration = 3 — PrePaid Accounting for Volume and Duration supported (non concurrently)

> Selected-For-Session
> The optional Selected-For-Session Sub-Type, generated by the PrePaid server, indicates the PrePaid Accounting capability to be used for a given session.
> Type
> 2
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Usage_None = 0 — PrePaid Accounting not used

> • | Usage_Volume = 1 — Usage of PrePaid Accounting for Volume (only possible if the AvailableInClient supports PrePaid Accounting for Volume).

> • | Usage_Duration = 2 — Usage of PrePaid Accounting for Duration (only possible if the AvailableInClient supports PrePaid Accounting for Duration).

> • | Usage_Volume_And_Duration = 3 — Usage of PrePaid Accounting for Volume and Duration (non concurrent) (only possible if the AvailableInClient supports PrePaid Accounting for Volume and duration).

> 3GPP2-Pre-Paid-TariffSwitch
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 98
> Length
> Compound
> Value
> Contains the following subattributes:
> Quota-Identifier
> Quota-Identifier
> Type
> 1
> Length
> 4
> Value
> Unsigned integer.
> Volume-Used-After-Tariff-Switch
> Volume Quota used after Tariff Switch happened.
> Type
> 2
> Length
> 4
> Value
> Unsigned integer.
> Volume-Used-ATS-Overflow
> Indicates how many times the VUATS counter has wrapped around 2^32 over the course of the service being provided.
> Type
> 3
> Length
> 2
> Value
> Unsigned integer.
> Tariff-Switch-Interval
> Indicates Tariff Switch Interval in seconds.
> Type
> 4
> Length
> 4
> Value
> Unsigned integer.
> Time-Interval-After-Tariff-Switch-Update
> Duration after TSI where an on-line RADIUS Access-Request is sent by PrePaid client to report VUATS before the next TS condition is triggered.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer.
> 3GPP2-QoS-Service-Opt-Profile
> The attribute specifies the unauthorized packet data service options, the maximum number of simultaneous service instances of the given service option number and the total maximum number of simultaneous service instances.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 74
> Length
> 8-247
> Value
> Opaque value
> 3GPP2-Release-Indicator
> This attribute specifies reasons for sending a stop record. The enumeration of this attribute conforms to IS-835-1.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Unknown = 0

> • | PPP-Timeout = 1

> • | Handoff = 2

> • | PPP-Termination = 3

> • | Mobile-IP-Registration-Failure = 4

> • | Abnormal-Terminations = 5

> • | Termation-Dueto-Resource-Mgmt = 6

> • | Service-Instance-Released = 7

> • | VolumeQuota-Reached = 8

> • | DurationQuota-Reached = 9

> • | Incompatible-Prepaid = 10

> • | Airlink-Parameter-Change = 11

> • | TOD-Timer-Expiry = 12

> • | Active-To-Dormant = 13

> • | Flow-Deactivated = 15

> • | PPP-Renegotiation = 1001

> • | MIP-Lifetime-Expired = 1002

> • | A11-Lifetime-Expired = 1003

> • | MIP-Remote-Dereg = 1004

> • | Tarrif-Boundary = 1006

> • | PPP-Renegotiation-Handoff = 1007

> • | MIP-Registration-Revocation = 1008

> 3GPP2-Release-Indicator-custom9
> 3GPP2 Release Indicator for custom9, reason/cause for session release.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Unknown = 0

> • | PPP-Timeout = 1

> • | Handoff = 2

> • | PPP-Termination = 3

> • | Mobile-IP-Registration-Failure = 4

> • | PPP-Renegotiation = 5

> • | MIP-Registration-Revocation = 6

> • | VolumeQuota-Reached = 8

> • | DurationQuota-Reached = 9

> • | Incompatible-Prepaid = 10

> 3GPP2-Release-Indicator-Old
> 3GPP2 old Standard Release Indicator, reason/cause for session release.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Unknown = 0

> • | PPP-Timeout = 1

> • | Handoff = 2

> • | PPP-Protocol-Failure = 3

> • | PPP-Abnormal-Release = 4

> • | PPP-Termination = 5

> • | Mobile-IP-Registration-Failure = 6

> • | Active-To-Dormant = 7

> 3GPP2-Remote-Addr-Table-Index
> This attribute contains the Remote Address Table Index used to generate remote address accounting records. Supported range is 1–65535. Only one 3GPP2-Remote-Addr-Table-Index can be associated with a session.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 71
> Length
> 4
> Value
> Contains the following two subattributes:
> Table-Index
> Table-Index
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> Qualifier
> Qualifier
> Type
> 2
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Exempt-From-Prepaid = 1

> • | Summarize-Octet-Count = 2

> • | Both = 3

> 3GPP2-Remote-IPv4-Address
> This attribute allows the HA or PDSN to identify any IP address to be used for remote address-based accounting for the user. Up to 20 instances of the attribute are supported in the access response.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 59
> Length
> 12
> Value
> Contains the following three subattributes:
> Address
> Contains an IPv4 address to be used for remote address based accounting for the user. The address is used in conjunction with the Remote-Address-Mask subattribute to define the range of addresses to be monitored.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> Netmask
> Contains an IPv4 address mask that defines the set of remote addresses to be used for remote address based accounting.
> Type
> 2
> Length
> 4
> Value
> IPv4 address
> Qualifier
> Qualifier
> Type
> 3
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Exempt-From-Prepaid = 1

> • | Summarize-Octet-Count = 2

> • | Both = 3

> 3GPP2-Remote-IPv4-Addr-Octets
> This attribute allows the HA or PDSN to identify any IP address to be used for remote address based accounting for the user. Up to 10 instances of the attribute are supported.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 72
> Length
> 26
> Value
> Contains the following subattributes:
> Address
> Contains an IPv4 address to be used for remote address based accounting for the user. The address is used in conjunction with the Netmask subattribute to define the range of addresses to be monitored.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> Netmask
> Contains an IPv4 address mask that defines the set of remote addresses to be used for remote address based accounting.
> Type
> 2
> Length
> 4
> Value
> An IP Netmask specified in IP address format.
> Octets-Out
> Indicates how many bytes have been sent to the remote address specification (corresponds to forward traffic direction).
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> Octets-In
> Indicates how many bytes have been received from the remote address specification (corresponds to reverse traffic direction).
> Type
> 4
> Length
> 4
> Value
> Unsigned integer
> Table-Index
> Table-Index
> Type
> 5
> Length
> 2
> Value
> Unsigned integer
> Octets-Overflow-Out
> Indicates how many times the forward octet overflow counter has wrapped around 2^32 over the course of the service being provided.
> Type
> 6
> Length
> 2
> Value
> Unsigned integer
> Octets-Overflow-In
> Indicates how many times the reverse octets overflow counter has wrapped around 2^32 over the course of the service being provided.
> Type
> 7
> Length
> 2
> Value
> Unsigned integer
> 3GPP2-Rev-Dcch-Mux-Option
> This attribute specifies Reverse DCCH Mux option.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 85
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Rev-Dcch-Rc
> This attribute specifies the Radio Configuration of the Reverse Packet Data Channel.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 87
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Reverse-Fundamental-Rate
> As defined in “Wireless IP Network Standard - 3GPP2.P.S0001-A-1[4]”.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 15
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Reverse-Fundamental-RC
> The format and structure of the RADIUS channel in the reverse direction. A set of forward transmission formats that are characterized by data rates, modulation characterized, and spreading rates.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 21
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Reverse-Mux-Option
> Forward direction multiplexer option.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 13
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Reverse-Traffic-Type
> Specifies the reverse traffic type.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 18
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Primary = 0

> • | Secondary = 1

> 3GPP2-Rev-Pdch-Rc
> This attribute displays the 3GPP2-Rev-Pdch-Rc.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 114
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-RP-Session-ID
> This represents the GRE key selected by the PCF that identifies the A10 traffic for a user session.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 41
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Rsvp-Signal-In-Count
> This attribute specifies the RSVP signaling octets sent by the MS.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 162
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Rsvp-Signal-In-Packets
> This attribute specifies the Number of RSVP signaling packets sent by the MS.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 164
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Rsvp-Signal-Out-Count
> This attribute specifies the RSVP signaling octets sent to the MS.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 163
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Rsvp-Signal-Out-Packets
> This attribute specifies the Number of RSVP signaling packets sent to the MS.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 165
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-S
> This attribute contains the 'S' secret parameter used to make the IKE pre-shared secret.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 54
> Length
> 1–247
> Value
> A binary string of the value of 'S'.
> 3GPP2-SDB-Input-Octets
> This attribute counts the total number of octets sent to the user via Short Data Bursts.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 31
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-SDB-Output-Octets
> This attribute counts the total number of octets sent by the user via Short Data Bursts.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 32
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-Security-Level
> This attribute indicates the type of security that the home network mandates on the visited network.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 2
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | IPSec = 3—IPSec for tunnels and registration messages

> • | None = 4

> 3GPP2-Service-Option
> This attribute indicates the service option used for CDMA air interface.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 16
> Length
> 4
> Value
> Enumerated integer. Possible values are:

> • | HSPD = 0x21

> • | HRPD = 0x3b

> • | LLAROHC = 0x3d

> • | HRPD-AUX = 0x40

> • | HRPD-AUX-IP = 0x43

> • | eHRPD = 0x252

> • | LTE = 0x253

> • | UTRAN = 0x254

> • | GERAN = 0x255

> 3GPP2-Service-Option-Profile
> This attribute specifies the authorized packet data service options, the maximum number of simultaneous service instances of the given service option number (n), and the total maximum number of simultaneous service instances. This attribute may appear in a RADIUS Access-Accept message.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 74
> Length
> 4
> Value
> Unsigned integer. Supported values are:

> • | Maximum Service Instances total: The maximum number of service instances the user is allowed to establish regardless of the service option numbers. '1' represents one service instance, i.e., the main service instance. '0' is not an allowed value.

> • | Sub-Type ( = 1): Sub-Type for service option length for service option attribute in octets (4 octets)Service Option n: Service Option number: Maximum Number of Service instances of service option n. Sub-Type 1 may be repeated, once for each authorized service option.

> 3GPP2-Service-Reference-ID
> Specifies the reference ID of the service instance as received in the A11 Registration Request. If the service instance is the main service instance, the main SI Indicator Sub-Type should be included.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 94
> Length
> 4
> Value
> Contains two subattributes:
> SR-ID
> The SR_ID value received in the A11 Registration-Request message.
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> Main-SI-Indicator
> Only included for the main service instance.
> Type
> 2
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Main-SI = 1

> 3GPP2-Serving-PCF
> IP address of the serving PCF.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 9
> Length
> 4
> Value
> IPv4 address
> 3GPP2-Session-Continue
> This attribute when set to True means it is not the end of a session, and an Accounting Stop is immediately followed by an Account Start Record. False means end of a session.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 48
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> 3GPP2-Session-Term-Capability
> This attribute should be included in a RADIUS Access-request message to the Home RADIUS server and should contain the value 3 to indicate that the PDSN and HA support both Dynamic authorization with RADIUS and Registration Revocation for Mobile Ipv4. The attribute should also be included in the RADIUS Access-Accept message and should contain the preferred resource management mechanism by the home network, which should be used for the session and may include values 1 to 3.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 88
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Only_Dynamic_Auth_Extn_to_Radius = 0x00000001 = 1

> • | Only_Reg_Revocation_in_MIP = 0x00000002 = 2

> • | Both_Dynamic_Auth_And_Reg_Revocation_in_MIP = 0x00000003 = 3

> 3GPP2-S-Key
> Contains the HA IKE key in encrypted format.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 54
> Length
> 1–247
> Value
> Opaque value
> 3GPP2-S-Lifetime
> This attribute contains the lifetime of the 'S' secret parameter used to make the IKE pre-shared secret. indicating the time in seconds since January 1, 1970 00:00 UTC. Note that this is equivalent to the UNIX operating system expression of time.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 55
> Length
> 4
> Value
> Unsigned integer
> 3GPP2-S-Request
> This attribute indicates whether the HA requests a shared secret 'S'.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 55
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1 — 'S' secret requested for IKE

> 3GPP2-Subnet
> This attribute specifies the Subnet information of the HRPD RAN.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 108
> Value
> Contains the following subattributes:
> Rev-A-Subnet
> This attribute specifies the Subnet information of the HRPD RAN.
> Type
> 1
> Length
> In StarOS 8.1 and earlier: 118; In StarOS 9.0 and later: 119
> Value
> Opaque value
> Rev-A-Sector-Id
> This attribute specifies the Sector ID information of the HRPD RAN.
> Type
> 2
> Length
> In StarOS 8.1 and earlier: 119; In StarOS 9.0 and later: 118
> Value
> Opaque value
> 3GPP2-S-Unencrypted
> Contains the HA IKE key in plain format.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 54
> Length
> 1–247
> Value
> Opaque value
> 3GPP2-User-Zone
> This attribute describes the Tiered Services user zone. The least significant 16 bits are the user zone ID, the next significant 15 bits are the user zone system ID, and the most significant bit is zero.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 11
> Length
> 4
> Value
> Unsigned integer
> AAA-Session-ID
> A unique per realm identifier assigned to WiMAX session by the Home network during network entry.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 4
> Length
> 1–246
> Value
> Opaque value
> Access-In-Subs
> This attribute is used in a custom dictionary, and the VSA type is not standard. Opaque 1 byte value received in Access Accept. This will be included in accounting messages for this session.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 224
> Length
> 1
> Value
> Opaque value
> Acct-Authentic
> This attribute is included in Accounting-Request packets to indicate how the session was authenticated (RADIUS or locally).
> Type
> 45
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0 — Authentication was not required for the session

> • | RADIUS = 1 — The session was authenticated via RADIUS

> • | Local = 2 — The session was authenticated locally

> • | Remote = 3

> • | Diameter = 4

> Acct-Delay-Time
> This attribute indicates how many seconds the chassis has been trying to send this record for.
> Type
> 41
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Input-Gigawords
> This attribute indicates how many times the Acct-Input-Octets attribute has wrapped within its 32-bit field length. In effect, the number of octets received is a 64-bit integer, with this attribute representing the high 32 bits, and the Acct-Input-Octets attribute representing the low 32 bits. This attribute is not included unless it has a non-zero value.
> Type
> 52
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Input-Octets
> This attribute indicates how many octets have been received in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the Acct-Input-Gigawords attribute will be incremented. In effect, the number of octets received is a 64-bit integer, with the Acct-Input-Gigawords attribute representing the high 32 bits, and this attribute representing the low 32 bits.
> Important: RADIUS reports what is going through the air interface. For uplink traffic, it reports all packets including those dropped/filtered by ACS. For downlink traffic, it reports what is going to the MS after ACS filtering. When DCCA is enabled, packets may be dropped due to unavailability of quota. Therefore, for pre-paid calls, accounting attributes “Acct-Input-Octets” and “Acct-Output-Octets” will not match totals of “dataVolumeGPRSUplink” and “dataVolumeGPRSDownlink” respectively from generated eG-CDRs.
> Type
> 42
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Input-Packets
> This attribute indicates how many PPP packets have been received during the session.
> Type
> 47
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Interim-Interval
> Indicates the time (in seconds) between updates to session counters (log file on RADIUS or AAA event log) during the session. Note that the setting for this attribute always takes precedence over interim interval settings configured on the system.
> Caution: To avoid increasing network traffic unnecessarily and potentially reducing network and system performance, do not set this parameter to a value less than 50.
> Type
> 85
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Multi-Session-Id
> This attribute is a unique Accounting ID to make it easy to link together multiple related sessions in a log file. Each session linked together would have a unique Acct-Session-Id but the same Acct-Multi-Session-Id. It is strongly recommended that the Acct-Multi-Session-Id contain UTF-8 encoded characters.
> Type
> 50
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> Acct-Output-Gigawords
> This attribute indicates how many times the Acct-Output-Octets attribute has wrapped within its 32-bit field length. In effect, the number of octets received is a 64-bit integer, with this attribute representing the high 32 bits, and the Acct-Output-Octets attribute representing the low 32 bits. This attribute is not included unless it has a non-zero value.
> Type
> 53
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Output-Octets
> This attribute indicates how many octets have been sent in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the Acct-Output-Gigawords attribute will be incremented. In effect, the number of octets received is a 64-bit integer, with the Acct-Output-Gigawords attribute representing the high 32 bits, and this attribute representing the low 32 bits.
> Important: RADIUS reports what is going through the air interface. For uplink traffic, it reports all packets including those dropped/filtered by ACS. For downlink traffic, it reports what is going to the MS after ACS filtering. When DCCA is enabled, packets may be dropped due to unavailability of quota. Therefore, for pre-paid calls, accounting attributes “Acct-Input-Octets” and “Acct-Output-Octets” will not match totals of “dataVolumeGPRSUplink” and “dataVolumeGPRSDownlink” respectively from generated eG-CDRs.
> Type
> 43
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Output-Packets
> This attribute indicates how many PPP packets have been sent during the session.
> Type
> 48
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Acct-Session-Id
> This attribute is a session ID. Combined with the identification of the chassis (NAS-IP-Address or NAS-Identifier), this uniquely describes a session. For a given chassis, there will never be another session (even across boots) with this same session ID. The Acct-Session-ID AVP is sent on both Gx and Gy messages.
> Type
> 44
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> Acct-Session-Id-Long
> This attribute contains long format account session ID. This is supported only for custom2 dictionary.
> Type
> 44
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> Acct-Session-Time
> This attribute indicates the duration of the session in seconds.
> Type
> 46
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Integer
> Acct-Status-Type
> This attribute indicates the event for the session.
> Type
> 40
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Start = 1 — The session has started, or the service has been delivered

> • | Stop = 2 — The session has completed, or the user has released service

> • | Interim-Update = 3 — The session or service is still ongoing. Usage details are given in other RADIUS attributes.

> • | Accounting-On = 7 — The chassis sends this message to the RADIUS server upon boot.

> • | Accounting-Off = 8 — The chassis sends this message to the RADIUS server when it shuts down in a normal fashion.

> • | Tunnel-Start = 9

> • | Tunnel-Stop = 10

> • | Tunnel-Reject = 11

> • | Tunnel-Link-Start = 12

> • | Tunnel-Link-Stop = 13

> • | Tunnel-Link-Reject = 14

> • | Failed = 15

> Acct-Termination-Cause
> This attribute indicates why the session was terminated.
> Type
> 49
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | User_Request = 1 — The user requested termination

> • | Lost_Carrier = 2

> • | Lost_Service = 3 — The chassis session terminated abnormally

> • | Idle_Timeout = 4 — The session idle timeout expired

> • | Session_Timeout = 5 — The session timeout expired

> • | Admin_Reset = 6 — The Service Provisioning system terminated the session

> • | Admin_Reboot = 7 — The Service Provisioning system rebooted the chassis

> • | Port_Error = 8 — PAC error, requiring the session to be terminated

> • | NAS_Error = 9 — Error other than PAC error, requiring session to be terminated

> • | NAS_Request = 10 — Session terminated for any other non error reason by PDSN

> • | NAS_Reboot = 11 — The chassis rebooted abnormally.

> • | Port_Unneeded = 12

> • | Port_Preempted = 13 — Duplicate Home Address Requested. Call aborted.

> • | Port_Suspended = 14 — PPP restart or RP-A11 disconnect without active Stop conditions

> • | Service_Unavailable = 15 — The chassis could not provide the service requested

> • | Callback = 16

> • | User_Error = 17 — A non-compliant PPP client required the chassis to terminate the session

> • | Host_Request = 18 — Inter-PDSN handoff, Active->Dormant transition, PPP re-nego-tiation, Active Start Parameter change, Accounting Tariff Boundary

> • | Supplicant_Restart = 19

> • | Reauthentication_Failure = 20

> • | Port_Reinitialized = 21

> • | Port_Administratively_Disabled = 22

> • | Inter-PDSN-Handoff = 99 — Customer-specific implementation

> • | Long-Duration-Timeout = 1001

> • | Invalid-Source-Address = 1002

> • | Duplicate-IMSI = 1003

> • | Interim-Update = 1004

> BU-CoA-Ipv6
> CoA from the BU message.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 51
> Length
> 16
> Value
> Opaque value
> Called-Station-ID
> For PDSN, the value of this attribute is a single zero byte for custom6/7/8 dictionaries. For other dictionaries, this attribute will not be present for PDSN calls.
> Type
> 30
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> For GGSN, a UTF-8 encoded string identifying the target network. For PDSN, a single zero byte.
> Calling-Station-Id
> This attribute indicates the Mobile Station Identifier in PDSN, and MSISDN in GGSN.
> Type
> 31
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–15
> Value
> ASCII string
> Calling-Subscriber-Type
> Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 218
> Length
> 1
> Value
> The system does not interpret this value, it is only copied in accounting messages.
> CHAP-Challenge
> This attribute contains the CHAP Challenge that was sent by the chassis to the other end of the PPP link, when CHAP authentication is being used.
> Type
> 60
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1-253
> Value
> Opaque value
> CHAP-Password
> This attribute contains the CHAP ID and the CHAP Response when CHAP authentication is used.
> Type
> 3
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 17
> Value
> Bit string. First byte is the CHAP ID. Next 16 bytes is the CHAP Response.
> Charging-Id
> Same as 3GPP-Charging-ID standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 225
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Class
> This attribute may be sent by the RADIUS server to the chassis in an Access-Accept packet. The chassis will include this attribute in all subsequent Accounting-Request messages sent to the RADIUS Accounting server for this user’s session. This attribute is included to support the RADIUS protocol and should not be human-interpreted.
> Type
> 25
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> The format of the value is server-dependent. The chassis will interpret it as simply a bit string to be reflected in Accounting-Request messages.
> CUI
> Chargeable User Identity is a unique temporary handle to the user responsible for paying bill. Set to NULL in Initial Access request and set to value sent by AAA in subsequent messages.
> Type
> 89
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> Opaque value
> DHCP-RK
> DHCP-RK is a 160-bit randomly generated for every DHCP server, the DHCP Key is derived from this.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 40
> Length
> 1–250
> Value
> Opaque value
> DHCP-RK-Key-ID
> An integer uniquely identifying the DHCP-RK within the scope of a single DHCP server.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 41
> Length
> 4
> Value
> Unsigned Integer
> DHCP-RK-Lifetime
> Lifetime of the DHCP-RK and derived keys.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 42
> Length
> 4
> Value
> Unsigned Integer
> DHCPMSG-Server-IP
> The IPv4 address of the DHCP server.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 43
> Length
> 4
> Value
> IPv4 address
> Digest-AKA-Auts
> This attribute holds the auts parameter that is used in the Digest AKA calculation.
> Type
> 118
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Algorithm
> This parameter holds the algorithm parameter that influences the HTTP Digest calculation.
> Type
> 111
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0–253
> Value
> Opaque value
> Digest-Auth-Param
> This attribute is a placeholder for future extensions.
> Type
> 117
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0–253
> Value
> Opaque value
> Digest-CNonce
> This attribute holds the client nonce that is used in the digest calculation.
> Type
> 113
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0–253
> Value
> Opaque value
> Digest-Domain
> This attribute consists of single URI that defines a protection space component.
> Type
> 119
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-256
> Value
> Opaque value
> Digest-Entity-Body-Hash
> This attribute holds the hexadecimal representation of H(entity-body). This hash is required when quality of protection is set to “auth-int”.
> Type
> 112
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> Hexadecimal string
> Digest-HA1
> This attribute contains the hexadecimal representation on H(A1) as described in RFC 2617.
> Type
> 121
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Method
> This attribute holds the method value to be used in the HTTP digest calculation.
> Type
> 108
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Nextnonce
> This attribute holds a nonce to be used in the HTTP digest calculation.
> Type
> 107
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> Hexadecimal string
> Digest-Nonce-Count
> This attribute holds the nonce count parameter that is used to detect replay attacks.
> Type
> 114
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Opaque
> This attribute holds the opaque parameter that is passed to the SIP client.
> Type
> 116
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Qop
> This attribute holds the quality of protection parameter that influences the HTTP digest calculation.
> Type
> 110
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Realm
> This attribute describes a protection space component of the RADIUS server.
> Type
> 104
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Response-Auth
> This enables the RADIUS server to prove possession of the password.
> Type
> 106
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> Hexadecimal string.
> Digest-Stale
> This attribute is sent by RADIUS server in order to notify the RADIUS client whether it has accepted a nonce.
> Type
> 120
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string. The following are valid values for this attribute:

> • | False = 0

> • | True = 1

> Digest-URI
> This attribute is used to transport the contents of the URI of the SIP request.
> Type
> 109
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> Digest-Username
> This attribute holds the user name used in the HTTP Digest calculation.
> Type
> 115
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> ASCII string
> DNS
> IPv4/IPv6 address of the DNS server to be conveyed to the MS via DHCP.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 52
> Length
> 4–16
> Value
> Opaque value
> EAP-Message
> The EAP exchanged transported over RADIUS.
> Type
> 79
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0-253
> Value
> Opaque value
> Error-Cause
> It is possible that the NAS cannot honor Disconnect-Request or CoA-Request messages for some reason. The Error-Cause Attribute provides more detail on the cause of the problem. It MAY be included within Disconnect-ACK, Disconnect-NAK, and CoA-NAK messages.
> Type
> 101
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Residual-Session-Context-Remove = 201

> • | Invalid-EAP-Packet = 202

> • | Unsupported-Attribute = 401

> • | Missing-Attribute = 402

> • | NAS-Identification-Mismatch = 403

> • | Invalid-Request = 404

> • | Unsupported-Service = 405

> • | Unsupported-Extension = 406

> • | Administratively-Prohibited = 501

> • | Request-Not-Routable = 502

> • | Session-Context-Not-Found = 503

> • | Session-Context-Not-Removable = 504

> • | Other-Proxy-Processing-Error = 505

> • | Resources-Unavailable = 506

> • | Request-Initiated = 507

> • | Session-Context-Not-Removable-Dormant = 599

> Event-Timestamp
> This attribute is a timestamp of when the event being logged occurred, indicating the time in seconds since January 1, 1970 00:00 UTC. Note that this is equivalent to the UNIX operating system expression of time.
> Type
> 55
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> FA-RK-KEY
> Contains the encrypted FA-RK-KEY. The FA-RK determined during EAP authentication by the RADIUS server and passed on to the NAS upon successful EAP authentication. It is used by the NAS to generate MN-FA keys.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 14
> Length
> 1–244
> Value
> Opaque value
> FA-RK-SPI
> SPI associated with FA-RK.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 61
> Length
> 4
> Value
> Unsigned integer
> Filter-Id
> This attribute identifies the IP access-list/filter by name. By default, a Filter-Id is applied in both directions. To apply a filter in a single direction, add the prefix “in:” or “out:” to the access-list name in the Filter-Id. Syntax: in:<filter_name>This assigns an input filter identified by filter_name out:<filter_name> This assigns an output filter identified by filter_name <filter_name>
> Type
> 11
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–32
> Value
> ASCII string
> Framed-Compression
> This attribute indicates the compression protocol to be used.
> Type
> 13
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0 — Do not use compression

> • | VJ_TCP_IP_header_compression = 1 — Use VJ TCP/IP header compression

> • | IPX_header_compression = 2

> • | Stac_LZS_compressions = 3 — Use Stac-LZS compression

> Framed-Interface-Id
> This attribute contains the value of IPv6 Interface ID.
> Type
> 96
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 8
> Value
> Opaque value
> Framed-IP-Address
> This attribute indicates the IP address to be configured for the user.
> Type
> 8
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> An IP address as it would appear in the source or destination field of an IP header. Special values are:

> • | 255.255.255.255 – User selected address

> • | 255.255.255.254 – Assign address from a pool (see Framed-Pool and SN-IP-Pool-Name )

> Framed-IP-Netmask
> This attribute indicates the IP netmask to be configured for the session when the PPP connection is to a router servicing a network.
> Type
> 9
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> An IP netmask specified in IPv4 address format.
> Framed-IPv6-Pool
> This attribute contains the value of IPv6 pool name.
> Type
> 100
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> Framed-IPv6-Prefix
> This attribute contains IPv6 prefix.
> Type
> 97
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 2–18
> Value
> Opaque value
> Framed-MTU
> This attribute indicates the Maximum Transmission Unit that was configured for the PPP session.
> Type
> 12
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Integer. Supported values are from 64 through 4096.
> Framed-Pool
> This standard attribute indicates the name of the IP pool from which an IP address should be allocated to the subscriber. Also, see SN-IP-Pool-Name, which is a vendor-specific attribute accomplishing the same.
> Type
> 88
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> Framed-Protocol
> This attribute describes the framed protocol that the user is granted to use (Access-Accept), when Service-Type = Framed. Note that PPP is the only framed protocol supported.
> Type
> 7
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | PPP = 1

> • | SLIP = 2

> • | ARAP = 3

> • | Gandalf_proprietary___ = 4

> • | Xylogics_proprietary_IPX_SLIP = 5

> • | X_75_Synchronous = 6

> • | GPRS_PDP_Context = 7

> Framed-Route
> This attribute contains the IP route to be installed specific to this session.
> Type
> 61
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> In StarOS 8.x and earlier: 16; in StarOS 9.0 and later: 1–64
> Value
> Opaque value
> GGSN-GTP-IP-Address
> Same as 3GPP-GGSN-Address standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 230
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> IPv4 address
> HA-IP-MIP4
> IPv4 address of the HA.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 6
> Length
> 4
> Value
> IPv4 address
> HA-IP-MIP6
> IPv6 address of the HA for CMIP4.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 7
> Length
> 4–16
> Value
> Opaque value
> HA-RK-KEY
> The HA-RK-KEY determined during EAP authentication by the RADIUS server and passed to the NAS upon successful EAP authentication. It is used by the NAS to generate FA-HA keys.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 15
> Length
> 1–244
> Value
> Opaque value
> HA-RK-Lifetime
> Lifetime of the HA-RK and derived keys.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 17
> Length
> 4
> Value
> Unsigned integer.
> HA-RK-SPI
> SPI associated with HA-RK.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 16
> Length
> 4
> Value
> Unsigned integer.
> hLMA-IPv6-PMIP6
> MIPv6 Home Agent address received in binding update.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 127
> Length
> 2
> Value
> Opaque value
> Hotline-Profile-ID
> A unique identifier of a hotline profile to be applied to the session.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 53
> Length
> 1–246
> Value
> Opaque value
> Hotline-Session-Timer
> The time period, in seconds, the session can remain hotlined.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 56
> Length
> 4
> Value
> Unsigned Integer
> HTTP-Redirection-Rule
> An HTTP redirection rule.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 54
> Length
> 1–246
> Value
> Opaque value
> Idle-Timeout
> This attribute sets the maximum idle session time, in seconds. A session is idle when there is no IP traffic on the link. After the connection has been idle for the indicated amount of time, the chassis will tear down the session.
> Type
> 28
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Integer
> IMSI
> Same as 3GPP-IMSI standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 224
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–6
> Value
> ASCII string
> IMSI-MCC-MNC
> Same as 3GPP-IMSI-Mcc-Mnc standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 226
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–6
> Value
> String.
> In-Packet-Period
> Opaque 4 byte value received in Access Accept. This will be included in accounting messages for this session. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 247
> Length
> Unsigned integer.
> IP-Redirection-Rule
> An IP redirection rule.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 55
> Length
> 1–246
> Value
> Opaque value
> MN-HA-MIP4-KEY
> MN-HA key for SPI value in the Access request if present.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 10
> Length
> 1–244
> Value
> Opaque value
> MN-HA-MIP4-SPI
> SPI associated with the MN-HA-MIP4 key. This attribute needs to be sent in the Access Request to fetch the corresponding MN-HA keys.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 11
> Length
> 4
> Value
> Unsigned integer
> MN-HA-MIP6-KEY
> Used to calculate AUTH for MIP6 BU during PMIP6 on ASN and to validate and compute AUTH for MIP6 Binding Answer on HA.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 12
> Length
> 1–244
> Value
> Opaque value
> MN-HA-MIP6-SPI
> SPI associated with the MN-HA-MIP6-KEY.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 12
> Length
> 4
> Value
> Unsigned integer.
> MSISDN
> MSIDSN of the call. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 222
> Length
> 1-256
> Value
> String
> MSK
> The Master Session Key determined during EAP authentication by the RADIUS server and passed to the NAS upon successful EAP authentication.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 5
> Length
> 1–246
> Value
> Opaque value
> NAS-Filter-Rule
> Indicates filter rules to be applied for the user.
> Type
> 92
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–246
> Value
> Opaque value
> NAS-Identifier
> This attribute identifies the NAS generating the record.
> Type
> 32
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> ASCII string
> NAS-IP-Address
> This attribute identifies the serving NAS.
> Type
> 4
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> An IP address as it would appear in the source or destination field of an IP header.
> NAS-Port
> This attribute describes the assigned resource number to the user session. It is guaranteed to be unique at a particular instance in time for a particular chassis.
> Type
> 5
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> NAS-Port-Type
> This attribute indicates the physical layer that the session is using.
> Type
> 61
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Async = 0

> • | Sync = 1

> • | ISDN_Sync = 2

> • | ISDN_Async_V_120 = 3

> • | ISDN_Async_V_110 = 4

> • | Virtual = 5 – MGMT

> • | PIAFS = 6

> • | HDLC_Clear_Channel = 7

> • | X_25 = 8

> • | X_75 = 9

> • | G_3_Fax = 10

> • | SDSL_Symmetric_DSL = 11

> • | ADSL_CAP = 12

> • | ADSL_DMT = 13

> • | IDSL = 14

> • | Ethernet = 15

> • | xDSL = 16

> • | Cable = 17

> • | Wireless_Other = 18 – Other wireless

> • | Wireless_IEEE_802_11 = 19 – Wireless IEEE 802.11

> • | Token_Ring = 20

> • | FDDI = 21

> • | Wireless_CDMA2000 = 22

> • | Wireless_UMTS = 23

> • | HRPD = 24 – High Rate Packet Data. HRPD is only available if included in the custom dictionary. None of the standard dictionaries include it.

> • | IAPP = 25

> • | FTTP = 26

> • | Wireless_IEEE_802_16 = 27

> • | Wireless_IEEE_802_20 = 28

> • | Wireless_IEEE_802_22 = 29

> • | Wireless_XGP=36

> PMIP-Authenticated-Nwk-Id
> The real user identifier returned by hAAA after successful authentication.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 58
> Length
> 1–246
> Value
> Opaque value
> PMIP6-RK-KEY
> PMIP6-RK-KEY
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 131
> Length
> 1–251
> Value
> Opaque value
> PMIP6-RK-SPI
> PMIP6-RK-SPI
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 132
> Length
> 1–251
> Value
> Opaque value
> PMIP6-Service-Info
> Indicates which PMIPv6 features are supported and enabled on ASN/LMA.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 126
> Length
> 2
> Value
> Unsigned Integer
> Price-Plan
> Opaque 1 byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 196
> Length
> 1
> Value
> The system does not interpret this value, but it is copied in accounting messages.
> Primary-DNS-Server
> Same as SN1-Primary-DNS-Server standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 135
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> IPv4 address
> Prohibit-Payload-Compression
> Flag to prohibit SGSN from compressing user data on per APN basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 237
> Length
> 2
> Value
> Enumerated integer. Possible values are:

> • | Allowed = 0

> • | Prohibited = 1

> Prohibit-Payload-Compression1
> Flag to prohibit SGSN from compressing user data on per APN basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 237
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Allowed = 0

> • | Prohibited = 1

> Reply-Message
> This attribute indicates the text to be displayed to a user upon completion of authentication, whether successful or not.
> Type
> 18
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–2048
> Value
> An ASCII string to be displayed to the user. This attribute may appear more than once, in which case the string displayed to the user is a concatenation of the Reply-Message attributes in the order in which they appear in the RADIUS response message.
> RRQ-MN-HA-KEY
> MN-HA key computed using RRQ-HA-IP if sent in Access request.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 19
> Length
> 1–244
> Value
> Opaque value
> Secondary-DNS-Server
> Same as SN1-Secondary-DNS-Server standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 136
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> IPv4 address
> Selection-Mode
> Same as 3GPP-Selection-Mode standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 229
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1
> Value
> Opaque value
> Service-Type
> This attribute identifies the service that the user is attempting to use (Access-Request), or is granted to use (Access-Accept).
> Type
> 6
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer.

> • | Supported values are:

> • | Framed = 2—PPP or HA session

> • | Administrative = 6—Configuration administration CLI session

> • | Authenticate_Only = 8

> • | Inspector = 19650516—Configuration/statistics read-only CLI session

> • | Security_Admin = 19660618—Security administration CLI session

> • | The following values are not supported, used only for display/decoding purposes:

> • | Login = 1

> • | Callback_Login = 3

> • | Callback_Framed = 4

> • | Outbound = 5

> • | NAS_Prompt = 7—CLI session

> • | Callback_NAS_Prompt = 9

> • | Call_Check = 10

> • | Callback_Administrative = 11

> • | Voice = 12

> • | Fax = 13

> • | Modem_Relay = 14

> • | IAPP_Register = 15

> • | IAPP_AP_Check = 16

> • | Authorize_Only = 17—RADIUS Change of Authorize/Disconnect/Prepaid Access Requests

> Session-Timeout
> This attribute sets the maximum session time in seconds. After this session time expires the chassis will tear down the session.
> Type
> 27
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> SGSN-IP-Address
> Same as 3GPP-SGSN-Address standard attribute; non-standard behavior for use in custom dictionary.
> Type
> 228
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> IPv4 address
> SIP-AOR
> This attribute identifies the URI, the use of which must be authenticated and authorized.
> Type
> 122
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 0–253
> Value
> ASCII string
> SN-Access-link-IP-Frag
> This attribute specifies what to do when data received for the subscriber on the Access link that needs to be fragmented and the DF bit is either set or unset. The default is Normal.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 63
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0 — Data to be fragmented is not fragmented if the DF bit is set

> • | DF-Ignore = 1 — Fragment regardless

> • | DF-Fragment-ICMP-Notify = 2 — Fragment regardless, and ICMP Notify if DF bit is set

> SN-Acct-Input-Giga-Dropped
> Contains the number of input gigawords dropped if the number of input bytes is greater than 2^32 - 1.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 230
> Length
> 4
> Value
> Unsigned integer
> SN-Acct-Input-Octets-Dropped
> This attribute indicates how many octets received have been dropped in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the SN-Acct-Input-Giga-Dropped attribute will be incremented.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 228
> Length
> 8
> Value
> Unsigned integer
> SN-Acct-Input-Packets-Dropped
> This attribute indicates how many PPP packets received have been dropped during the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 226
> Length
> 4
> Value
> Unsigned integer
> SN-Acct-Output-Giga-Dropped
> Contains the number of output gigawords dropped if the number of output bytes is greater than 2^32 - 1.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 231
> Length
> 4
> Value
> Unsigned integer
> SN-Acct-Output-Octets-Dropped
> This attribute indicates how many octets have been dropped in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the SN-Acct-Output-Giga-Dropped attribute will be incremented.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 229
> Length
> 8
> Value
> Unsigned integer
> SN-Acct-Output-Packets-Dropped
> This attribute indicates how many output PPP packets have been dropped during the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 227
> Length
> 4
> Value
> Unsigned integer
> SN-Acs-Credit-Control-Group
> This attribute contains the Diameter Credit Control Group name. It is used to send the Credit Control Group name from APN config to the ACS module.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 301
> Length
> 1–63
> Value
> String
> SN-Admin-Expiry
> This attribute contains the date/time the administrative user account expires. It is an integer value specifying the number of seconds since the UNIX epoch at which time the account will expire.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 204
> Length
> 4
> Value
> Integer
> SN-Admin-Permission
> This attribute indicates the services allowed to be delivered to the administrative user. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 21
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | CLI = 1

> • | FTP = 2

> • | CLI-FTP = 3

> • | Intercept = 4

> • | CLI-Intercept = 5

> • | CLI-Intercept-FTP = 7

> • | ECS = 8

> • | CLI-ECS = 9

> • | CLI-FTP-ECS = 11

> • | CLI-Intercept-ECS = 13

> • | CLI-Intercept-FTP-ECS = 15

> SN-ANID
> This attribute contains the Access Network ID.
> Type
> 26
> Vendor ID
> 5535
> VSA Type
> 178
> Length
> 10
> Value
> Opaque value
> SN-Assigned-VLAN-ID
> This attribute contains the Assigned VLAN ID.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 152
> Length
> 2
> Value
> Unsigned integer
> SN-Authorised-Qos
> This attribute contains the authorized QoS.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 266
> Length
> 4
> Value
> ASCII string
> SN-Bandwidth-Policy
> This attribute contains the Traffic Policy value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 300
> Length
> 1–63
> Value
> String
> SN-Call-Id
> This attribute contains the Call ID.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 251
> Length
> 4
> Value
> Unsigned integer
> SN-Cause-Code
> This attribute includes the termination cause code value from IMS node.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 267
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal_End_Of_Session = 0

> • | Successful_Transaction = 1

> • | End_Of_Subscriber_Dialog = 2

> • | 3XX_Redirection = 3

> • | 4XX_Request_Failure = 4

> • | 5XX_Server_Failure = 5

> • | 6XX_Global_Failure = 6

> • | Unspecified_Error = 7

> • | Unsuccessful_Session_Setup = 8

> • | Internal_Error = 9

> SN-Cause-For-Rec-Closing
> This attribute contains the GGSN Specific Record Closing Reason Value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 139
> Length
> 4
> Value
> Unsigned integer
> SN-CBB-Policy
> This attribute contains the CBB policy value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 302
> Length
> 1–63
> Value
> String
> SN-CF-Call-International
> This attribute contains enable/disable config for CF call restriction and dialing permission for international calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 293
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-Local
> This attribute contains enable/disable config for CF call restriction and dialing permission for local calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 291
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-LongDistance
> This attribute contains enable/disable config for CF call restriction and dialing permission for long distance calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 292
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-Premium
> This attribute contains enable/disable config for CF call restriction and dialing permission for premium calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 294
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-RoamingInternatnl
> This attribute contains enable/disable config for CSCF call restriction and dialing permission - Roaming International call.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 298
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-Transfer
> This attribute contains enable/disable config for CSCF call feature - call transfer.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 285
> Length
> 4
> Value
> Enumerated integer. Supported values are.

> • | Disable = 0

> • | Enable = 1

> SN-CF-Call-Waiting
> This attribute contains enable/disable config for CSCF call feature - call waiting.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 284
> Length
> 4
> Value
> Enumerated integer. Supported values are.

> • | Disable = 0

> • | Enable = 1

> SN-CF-CId-Display
> This attribute contains enable/disable config for CSCF call feature - caller ID display.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 282
> Length
> 4
> Value
> Enumerated integer. Supported values are.

> • | Disable = 0

> • | Enable = 1

> SN-CF-CId-Display-Blocked
> This attribute contains enable/disable config for CSCF call feature - caller ID display blocked.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 283
> Length
> 4
> Value
> Enumerated integer. Supported values are.

> • | Disable = 0

> • | Enable = 1

> SN-CF-Follow-Me
> This attribute contains URIs for CSCF call feature - follow me.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 281
> Length
> 0–255
> Value
> ASCII string
> SN-CF-Forward-Busy-Line
> This attribute contains URI for CSCF call feature - forward busy line.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 279
> Length
> 0–255
> Value
> ASCII string
> SN-CF-Forward-No-Answer
> This attribute contains URI for CSCF call feature - forward no answer.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 278
> Length
> 0–255
> Value
> ASCII string
> SN-CF-Forward-Not-Regd
> This attribute contains URI for CSCF call feature - forward not registered.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 280
> Length
> 0–255
> Value
> ASCII string
> SN-CF-Forward-Unconditional
> This attribute contains URI for CSCF call feature - forward unconditional.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 277
> Length
> 0–255
> Value
> ASCII string
> SN-CFPolicy-ID
> Content Filtering policy ID.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 220
> Length
> 4
> Value
> Unsigned integer
> SN-Change-Condition
> The change condition that triggered this record for a GGSN session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 140
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | QOSCHANGE = 0

> • | TARIFFTIMECHANGE = 1

> • | SGSNCHANGE = 500

> SN-Charging-VPN-Name
> The Charging Context Name for GGSN sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 137
> Length
> 1–252
> Value
> ASCII string
> SN-Chrg-Char-Selection-Mode
> SN-Chrg-Char-Selection-Mode
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 138
> Length
> 4
> Value
> Unsigned integer
> SN-Content-Disposition
> This attribute indicates how the SIP message body or a message body part is to be interpreted.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 272
> Length
> 4
> Value
> ASCII string
> SN-Content-Length
> This attribute holds size of the SIP message body.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 271
> Length
> 4
> Value
> ASCII string
> SN-Content-Type
> This attribute contains the media type of the SIP message body.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 270
> Length
> 4
> Value
> ASCII string
> SN-CR-International-Cid
> Carrier ID for routing international calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 295
> Length
> 4
> Value
> Unsigned integer
> SN-CR-LongDistance-Cid
> Carrier ID for routing long distance calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 296
> Length
> 4
> Value
> Unsigned integer
> SN-CSCF-App-Server-Info
> This is a compound attribute and contains information about application servers.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 275
> Length
> 4
> Value
> Contains the following two subattributes:
> App-Server
> Holds URL of the application server.
> Type
> 1
> Length
> 4
> Value
> ASCII string
> AS-Called-Party-Address
> Holds the called party addresses determined by the application server.
> Type
> 2
> Length
> 4
> Value
> ASCII string
> SN-CSCF-Rf-SDP-Media-Components
> This is a compound attribute for IMS SDP media components.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 273
> Value
> Contains the following subattributes:
> Media-Name
> Name of the media as available in the SDP data.
> Type
> 1
> Length
> 0–128
> Value
> String
> Media-Description
> Holds the attributes of the media as available in the SDP data.
> Type
> 2
> Length
> 0–128
> Value
> String
> Authorised-QoS
> Holds the 3GPP Authorised QoS string.
> Type
> 3
> Length
> 0–128
> Value
> String
> 3GPP-Charging-Id
> Holds the 3GPP charging ID.
> Type
> 4
> Length
> 0–253
> Value
> String
> Access-Network-Charging-Identifier-Value
> Holds the access network charging identifier value.
> Type
> 5
> Length
> 1–256
> Value
> Opaque value
> SN-Cscf-Subscriber-Ip-Address
> This attribute contains the IP address of subscriber, used for early IMS authentication procedures.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 287
> Length
> 4
> Value
> IPv4 address
> SN-Data-Tunnel-Ignore-DF-Bit
> This attribute specifies if the PDSN/FA or HA should ignore the DF bit in the IPv4 header when encapsulating the IPv4 packet in MIP, and therefore fragmenting the resulting tunneled packet if necessary. The default is not to ignore the DF bit.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 49
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not ignore DF bit

> • | Enabled = 1 — Ignore DF bit

> SN-DHCP-Lease-Expiry-Policy
> This attribute specifies whether to renew or disconnect on expiry of IP address lease time.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 157
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | auto-renew = 0

> • | disconnect = 1

> SN-Direction
> ROHC protocol control that specifies in which direction to enable Robust Header Compression (ROHC).
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 153
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Any = 0

> • | Uplink = 1

> • | Downlink = 2

> SN-Disconnect-Reason
> This attribute indicates the reason the user was disconnected from service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 3
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Not-Defined = 0

> • | Admin-Disconnect = 1

> • | Remote-Disconnect = 2

> • | Local-Disconnect = 3

> • | Disc-No-Resource = 4

> • | Disc-Excd-Service-Limit = 5

> • | PPP-LCP-Neg-Failed = 6

> • | PPP-LCP-No-Response = 7

> • | PPP-LCP-Loopback = 8

> • | PPP-LCP-Max-Retry = 9

> • | PPP-Echo-Failed = 10

> • | PPP-Auth-Failed = 11

> • | PPP-Auth-Failed-No-AAA-Resp = 12

> • | PPP-Auth-No-Response = 13

> • | PPP-Auth-Max-Retry = 14

> • | Invalid-AAA-Attr = 15

> • | Failed-User-Filter = 16

> • | Failed-Provide-Service = 17

> • | Invalid-IP-Address-AAA = 18

> • | Invalid-IP-Pool-AAA = 19

> • | PPP-IPCP-Neg-Failed = 20

> • | PPP-IPCP-No-Response = 21

> • | PPP-IPCP-Max-Retry = 22

> • | PPP-No-Rem-IP-Address = 23

> • | Inactivity-Timeout = 24

> • | Session-Timeout = 25

> • | Max-Data-Excd = 26

> • | Invalid-IP-Source-Address = 27

> • | MSID-Auth-Failed = 28

> • | MSID-Auth-Failed-No-AAA-Resp = 29

> • | A11-Max-Retry = 30

> • | A11-Lifetime-Expired = 31

> • | A11-Message-Integrity-Failure = 32

> • | PPP-lcp-remote-disc = 33

> • | Session-setup-timeout = 34

> • | PPP-keepalive-failure = 35

> • | Flow-add-failed = 36

> • | Call-type-detection-failed = 37

> • | Wrong-ipcp-params = 38

> • | MIP-remote-dereg = 39

> • | MIP-lifetime-expiry = 40

> • | MIP-proto-error = 41

> • | MIP-auth-failure = 42

> • | MIP-reg-timeout = 43

> • | Invalid-dest-context = 44

> • | Source-context-removed = 45

> • | Destination-context-removed = 46

> • | Req-service-addr-unavailable = 47

> • | Demux-mgr-failed = 48

> • | Internal-error = 49

> • | AAA-context-removed = 50

> • | invalid-service-type = 51

> • | mip-relay-req-failed = 52

> • | mip-rcvd-relay-failure = 53

> • | ppp-restart-inter-pdsn-handoff = 54

> • | gre-key-mismatch = 55

> • | invalid_tunnel_context = 56

> • | no_peer_lns_address = 57

> • | failed_tunnel_connect = 58

> • | l2tp-tunnel-disconnect-remote = 59

> • | l2tp-tunnel-timeout = 60

> • | l2tp-protocol-error-remote = 61

> • | l2tp-protocol-error-local = 62

> • | l2tp-auth-failed-remote = 63

> • | l2tp-auth-failed-local = 64

> • | l2tp-try-another-lns-from-remote = 65

> • | l2tp-no-resource-local = 66

> • | l2tp-no-resource-remote = 67

> • | l2tp-tunnel-disconnect-local = 68

> • | l2tp-admin-disconnect_remote = 69

> • | l2tpmgr-reached-max-capacity = 70

> • | MIP-reg-revocation = 71

> • | path-failure = 72

> • | dhcp-relay-ip-validation-failed = 73

> • | gtp-unknown-pdp-addr-or-pdp-type = 74

> • | gtp-all-dynamic-pdp-addr-occupied = 75

> • | gtp-no-memory-is-available = 76

> • | dhcp-relay-static-ip-addr-not-allowed = 77

> • | dhcp-no-ip-addr-allocated = 78

> • | dhcp-ip-addr-allocation-tmr-exp = 79

> • | dhcp-ip-validation-failed = 80

> • | dhcp-static-addr-not-allowed = 81

> • | dhcp-ip-addr-not-available-at-present = 82

> • | dhcp-lease-expired = 83

> • | lpool-ip-validation-failed = 84

> • | lpool-static-ip-addr-not-allowed = 85

> • | static-ip-validation-failed = 86

> • | static-ip-addr-not-present = 87

> • | static-ip-addr-not-allowed = 88

> • | radius-ip-validation-failed = 89

> • | radius-ip-addr-not-provided = 90

> • | invalid-ip-addr-from-sgsn = 91

> • | no-more-sessions-in-aaa = 92

> • | ggsn-aaa-auth-req-failed = 93

> • | conflict-in-ip-addr-assignment = 94

> • | apn-removed = 95

> • | credits-used-bytes-in = 96

> • | credits-used-bytes-out = 97

> • | credits-used-bytes-total = 98

> • | prepaid-failed = 99

> • | l2tp-ipsec-tunnel-failure = 100

> • | l2tp-ipsec-tunnel-disconnected = 101

> • | mip-ipsec-sa-inactive = 102

> • | Long-Duration-Timeout = 103

> • | proxy-mip-registration-failure = 104

> • | proxy-mip-binding-update = 105

> • | proxy-mip-inter-pdsn-handoff-require-ip-address = 106

> • | proxy-mip-inter-pdsn-handoff-mismatched-address = 107

> • | Local-purge = 108

> • | failed-update-handoff = 109

> • | closed_rp-handoff-complete = 110

> • | closed_rp-duplicate-session = 111

> • | closed_rp-handoff-session-not-found = 112

> • | closed_rp-handoff-failed = 113

> • | pcf-monitor-keep-alive-failed = 114

> • | call-internal-reject = 115

> • | call-restarted = 116

> • | a11-mn-ha-auth-failure = 117

> • | a11-badly-formed = 118

> • | a11-t-bit-not-set = 119

> • | a11-unsupported-vendor-id = 120

> • | a11-mismatched-id = 121

> • | mipha-dup-home-addr-req = 122

> • | mipha-dup-imsi-session = 123

> • | ha-unreachable = 124

> • | IPSP-addr-in-use = 125

> • | mipfa-dup-home-addr-req = 126

> • | mipha-ip-pool-busyout = 127

> • | inter-pdsn-handoff = 128

> • | active-to-dormant = 129

> • | ppp-renegotiation = 130

> • | active-start-param-change = 131

> • | tarrif-boundary = 132

> • | a11-disconnect-no-active-stop = 133

> • | nw-reachability-failed-reject = 134

> • | nw-reachability-failed-redirect = 135

> • | container-max-exceeded = 136

> • | static-addr-not-allowed-in-apn = 137

> • | static-addr-required-by-radius = 138

> • | static-addr-not-allowed-by-radius = 139

> • | mip-registration-dropped = 140

> • | counter-rollover = 141

> • | constructed-nai-auth-fail = 142

> • | inter-pdsn-service-optimize-handoff-disabled = 143

> • | gre-key-collision = 144

> • | inter-pdsn-service-optimize-handoff-triggered = 145

> • | intra-pdsn-handoff-triggered = 146

> • | delayed-abort-timer-expired = 147

> • | Admin-AAA-disconnect = 148

> • | Admin-AAA-disconnect-handoff = 149

> • | PPP-IPV6CP-Neg-Failed = 150

> • | PPP-IPV6CP-No-Response = 151

> • | PPP-IPV6CP-Max-Retry = 152

> • | PPP-Restart-Invalid-source-IPV4-address = 153

> • | a11-disconnect-handoff-no-active-stop = 154

> • | call-restarted-inter-pdsn-handoff = 155

> • | call-restarted-ppp-termination = 156

> • | mipfa-resource-conflict = 157

> • | failed-auth-with-charging-svc = 158

> • | mipha-dup-imsi-session-purge = 159

> • | mipha-rev-pending-newcall = 160

> • | volume-quota-reached = 161

> • | duration-quota-reached = 162

> • | gtp-user-authentication-failed = 163

> • | MIP-reg-revocation-no-lcp-term = 164

> • | MIP-private-ip-no-rev-tunnel = 165

> • | Invalid-Prepaid-AAA-attr-in-auth-response = 166

> • | mipha-prepaid-reset-dynamic-newcall = 167

> • | gre-flow-control-timeout = 168

> • | mip-paaa-bc-query-not-found = 169

> • | mipha-dynamic-ip-addr-not-available = 170

> • | a11-mismatched-id-on-handoff = 171

> • | a11-badly-formed-on-handoff = 172

> • | a11-unsupported-vendor-id-on-handoff = 173

> • | a11-t-bit-not-set-on-handoff = 174

> • | MIP-reg-revocation-i-bit-on = 175

> • | A11-RRQ-Deny-Max-Count = 176

> • | Dormant-Transition-During-Session-Setup = 177

> • | PPP-Rem-Reneg-Disc-Always-Cfg = 178

> • | PPP-Rem-Reneg-Disc-NAI-MSID-Mismatch = 179

> • | mipha-subscriber-ipsec-tunnel-down = 180

> • | mipha-subscriber-ipsec-tunnel-failed = 181

> • | mipha-subscriber-ipsecmgr-death = 182

> • | flow-is-deactivated = 183

> • | ecsv2-license-exceeded = 184

> • | IPSG-Auth-Failed = 185

> • | driver-initiated = 186

> • | ims-authorization-failed = 187

> • | service-instance-released = 188

> • | flow-released = 189

> • | ppp-renego-no-ha-addr = 190

> • | intra-pdsn-handoff = 191

> • | overload-disconnect = 192

> • | css-service-not-found = 193

> • | Auth-Failed = 194

> • | dhcp-client-sent-release = 195

> • | dhcp-client-sent-nak = 196

> • | msid-dhcp-chaddr-mismatch = 197

> • | link-broken = 198

> • | prog-end-timeout = 199

> • | qos-update-wait-timeout = 200

> • | css-synch-cause = 201

> • | Gtp-context-replacement = 202

> • | PDIF-Auth-failed = 203

> • | l2tp-unknown-apn = 204

> • | ms-unexpected-network-reentry = 205

> • | r6-invalid-nai = 206

> • | eap-max-retry-reached = 207

> • | vbm-hoa-session-disconnected = 208

> • | vbm-voa-session-disconnected = 209

> • | in-acl-disconnect-on-violation = 210

> • | eap-msk-lifetime-expiry = 211

> • | eap-msk-lifetime-too-low = 212

> • | mipfa-inter-tech-handoff = 213

> • | r6-max-retry-reached = 214

> • | r6-nwexit-recd = 215

> • | r6-dereg-req-recd = 216

> • | r6-remote-failure = 217

> • | r6r4-protocol-errors = 218

> • | wimax-qos-invalid-aaa-attr = 219

> • | npu-gre-flows-not-available = 220

> • | r4-max-retry-reached = 221

> • | r4-nwexit-recd = 222

> • | r4-dereg-req-recd = 223

> • | r4-remote-failure = 224

> • | ims-authorization-revoked = 225

> • | ims-authorization-released = 226

> • | ims-auth-decision-invalid = 227

> • | mac-addr-validation-failed = 228

> • | excessive-wimax-pd-flows-cfgd = 229

> • | sgsn-canc-loc-sub = 230

> • | sgsn-canc-loc-upd = 231

> • | sgsn-mnr-exp = 232

> • | sgsn-ident-fail = 233

> • | sgsn-sec-fail = 234

> • | sgsn-auth-fail = 235

> • | sgsn-glu-fail = 236

> • | sgsn-imp-det = 237

> • | sgsn-smgr-purge = 238

> • | sgsn-subs-handed-to-peer = 239

> • | sgsn-dns-fail-inter-rau = 240

> • | sgsn-cont-rsp-fail = 241

> • | sgsn-hlr-not-found-for-imsi = 242

> • | sgsn-ms-init-det = 243

> • | sgsn-opr-policy-fail = 244

> • | sgsn-duplicate-context = 245

> • | hss-profile-update-failed = 246

> • | sgsn-no-pdp-activated = 247

> • | asnpc-idle-mode-timeout = 248

> • | asnpc-idle-mode-exit = 249

> • | asnpc-idle-mode-auth-failed = 250

> • | asngw-invalid-qos-configuration = 251

> • | sgsn-dsd-allgprswithdrawn = 252

> • | r6-pmk-key-change-failure = 253

> • | sgsn-illegal-me = 254

> • | sess-termination-timeout = 255

> • | sgsn-sai-fail = 256

> • | sgsn-rnc-removal = 257

> • | sgsn-rai-removal = 258

> • | sgsn-init-deact = 259

> • | ggsn-init-deact = 260

> • | hlr-init-deact = 261

> • | ms-init-deact = 262

> • | sgsn-detach-init-deact = 263

> • | sgsn-rab-rel-init-deact = 264

> • | sgsn-iu-rel-init-deact = 265

> • | sgsn-gtpu-path-failure = 266

> • | sgsn-gtpc-path-failure = 267

> • | sgsn-local-handoff-init-deact = 268

> • | sgsn-remote-handoff-init-deact = 269

> • | sgsn-gtp-no-resource = 270

> • | sgsn-rnc-no-resource = 271

> • | sgsn-odb-init-deact = 272

> • | sgsn-invalid-ti = 273

> • | sgsn-ggsn-ctxt-non-existent = 274

> • | sgsn-apn-restrict-vio = 275

> • | sgsn-regular-deact = 276

> • | sgsn-abnormal-deact = 277

> • | sgsn-actv-rejected-by-peer = 278

> • | sgsn-err-ind = 279

> • | asngw-non-anchor-prohibited = 280

> • | asngw-im-entry-prohibited = 281

> • | session-idle-mode-entry-timeout = 282

> • | session-idle-mode-exit-timeout = 283

> • | asnpc-ms-power-down-nwexit = 284

> • | asnpc-r4-nwexit-recd = 285

> • | sgsn-iu-rel-before-call-est = 286

> • | ikev2-subscriber-ipsecmgr-death = 287

> • | All-dynamic-pool-addr-occupied = 288

> • | mip6ha-ip-addr-not-available = 289

> • | bs-monitor-keep-alive-failed = 290

> • | sgsn-att-in-reg-state = 291

> • | sgsn-inbound-srns-in-reg-state = 292

> • | dt-ggsn-tun-reestablish-failed = 293

> • | sgsn-unknown-pdp = 294

> • | sgsn-pdp-auth-failure = 295

> • | sgsn-duplicate-pdp-context = 296

> • | sgsn-no-rsp-from-ggsn = 297

> • | sgsn-failure-rsp-from-ggsn = 298

> • | sgsn-apn-unknown = 299

> • | sgsn-serv-req-init-deact = 300

> • | sgsn-attach-on-attch-init-abort = 301

> • | sgsn-iu-rel-in-israu-init-abort = 302

> • | sgsn-smgr-init-abort = 303

> • | sgsn-mm-ctx-cleanup-init-abort = 304

> • | sgsn-unknown-abort = 305

> • | sgsn-guard-timeout-abort = 306

> • | vpn-bounce-dhcpip-validate-req = 307

> • | mipv6-id-mismatch = 308

> • | aaa-session-id-not-found = 309

> • | x1-max-retry-reached = 310

> • | x1-nwexit-recd = 311

> • | x1-dereg-req-recd = 312

> • | x1-remote-failure = 313

> • | x1x2-protocol-errors = 314

> • | x2-max-retry-reached = 315

> • | x2-nwexit-recd = 316

> • | x2-dereg-req-recd = 317

> • | x2-remote-failure = 318

> • | x1-pmk-key-change-failure = 319

> • | sa-rekeying-failure = 320

> • | sess-sleep-mode-entry-timeout = 321

> • | phsgw-non-anchor-prohibited = 322

> • | asnpc-pc-relocation-failed = 323

> • | asnpc-pc-relocation = 324

> • | auth_policy_mismatch = 325

> • | sa-lifetime-expiry = 326

> • | asnpc-del-ms-entry-recd = 327

> • | phspc-sleep-mode-timeout = 328

> • | phspc-sleep-mode-exit = 329

> • | phspc-sleep-mode-auth-failed = 330

> • | phspc-ms-power-down-nwexit = 331

> • | phspc-x2-nwexit-recd = 332

> • | invalid-nat-config = 333

> • | asngw-tid-entry-not-found = 334

> • | No-NAT-IP-Address = 335

> • | excessive-phs-pd-flows-cfgd = 336

> • | phsgw-invalid-qos-configuration = 337

> • | Interim-Update = 338

> • | sgsn-attach-abrt-rad-lost = 339

> • | sgsn-inbnd-irau-abrt-rad-lost = 340

> • | ike-keepalive-failed = 341

> • | sgsn-attach-abrt-ms-suspend = 342

> • | sgsn-inbnd-irau-abrt-ms-suspend = 343

> • | duplicate-session-detected = 344

> • | sgsn-xid-response-failure = 345

> • | sgsn-nse-cleanup = 346

> • | sgsn-gtp-req-failure = 347

> • | sgsn-imsi-mismatch = 348

> • | sgsn-bvc-blocked = 349

> • | sgsn-attach-on-inbound-irau = 350

> • | sgsn-attach-on-outbound-irau = 351

> • | sgsn-incorrect-state = 352

> • | sgsn-t3350-expiry = 353

> • | sgsn-page-timer-expiry = 354

> • | phsgw-tid-entry-not-found = 355

> • | phspc-del-ms-entry-recd = 356

> • | sgsn-pdp-local-purge = 357

> • | phs-invalid-nai = 358

> • | session-sleep-mode-exit-timeout = 359

> • | sgsn-offload-phase2 = 360

> • | phs-thirdparty-auth-fail = 361

> • | remote-error-notify = 362

> • | no-response = 363

> • | PDG-Auth-failed = 364

> • | mme-s1AP-send-failed=365

> • | mme-egtpc-connection-failed=366

> • | mme-egtpc-create-session-failed=367

> • | mme-authentication-failure=368

> • | mme-ue-detach=369

> • | mme-mme-detach=370

> • | mme-hss-detach=371

> • | mme-pgw-detach=372

> • | mme-sub-validation-failure=373

> • | mme-hss-connection-failure=374

> • | mme-hss-user-unknown=375

> • | dhcp-lease-mismatch-detected=376

> • | nemo-link-layer-down=377

> • | eapol-max-retry-reached = 378

> • | sgsn-offload-phase3 = 379

> • | mbms-bearer-service-disconnect = 380

> • | disconnect-on-violation-odb = 381

> • | disconn-on-violation-focs-odb = 382

> • | CSCF-REG-Admin-disconnect = 383

> • | CSCF-REG-User-disconnect = 384

> • | CSCF-REG-Inactivity-timeout = 385

> • | CSCF-REG-Network-disconnect = 386

> • | CSCF-Call-Admin-disconnect = 387

> • | CSCF-CAll-User-disconnect = 388

> • | CSCF-CALL-Local-disconnect = 389

> • | CSCF-CALL-No-Resource = 390

> • | CSCF-CALL-No-Respone = 391

> • | CSCF-CALL-Inactivity-timeout = 392

> • | CSCF-CALL-Media-Auth-Failure = 393

> • | CSCF-REG-No-Resource = 394

> • | ms-unexpected-idle-mode-entry = 395

> • | re-auth-failed = 396

> • | sgsn-pdp-nse-cleanup = 397

> • | sgsn-mm-ctxt-gtp-no-resource = 398

> • | unknown-apn = 399

> • | gtpc-path-failure = 400

> • | gtpu-path-failure = 401

> • | actv-rejected-by-sgsn = 402

> • | sgsn-pdp-gprs-camel-release = 403

> • | sgsn-check-imei-failure = 404

> • | sgsn-sndcp-init-deact = 405

> • | sgsn-pdp-inactivity-timeout = 406

> • | fw-and-nat-policy-removed = 407

> • | FNG-Auth-failed = 408

> • | ha-stale-key-disconnect = 409

> • | No-IPV6-address-for-subscriber = 410

> • | prefix-registration-failure = 411

> • | disconnect-from-policy-server = 412

> • | s6b-auth-failed = 413

> • | gtpc-err-ind = 414

> • | gtpu-err-ind = 415

> • | invalid-pdn-type = 416

> • | aaa-auth-req-failed = 417

> • | apn-denied-no-subscription = 418

> • | Sgw-context-replacement = 419

> • | dup-static-ip-addr-req = 420

> • | apn-restrict-violation = 421

> • | invalid-wapn = 422

> • | ttg-nsapi-allocation-failed = 423

> • | mandatory-gtp-ie-missing = 424

> • | aaa-unreachable = 425

> SN-DNS-Proxy-Intercept-List
> DNS proxy list.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 214
> Length
> 1–253
> Value
> ASCII string
> SN-DNS-Proxy-Use-Subscr-Addr
> This attribute is used to convey whether to use the subscriber's address as the source address for DNS Proxy.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 25
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-Dynamic-Addr-Alloc-Ind-Flag
> SN-Dynamic-Addr-Alloc-Ind-Flag.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 141
> Length
> 1
> Value
> Opaque value
> SN-Ecs-Data-Volume
> Compound attribute indicating downlink and uplink octet usage for a PDP context per rating group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 176
> Length
> 12
> Value
> Contains the following subattributes:
> Rating-Group-Id
> Rating Group Id in a PDP context.
> Type
> 1
> Length
> 4
> Value
> Unsigned integer
> GPRS-Uplink
> Uplink octet usage for a PDP context per rating group.
> Type
> 2
> Length
> 4
> Value
> Unsigned integer
> GPRS-Downlink
> Downlink octet usage for a PDP context per rating group.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> SN-Enable-QoS-Renegotiation
> This attribute configures the enabling of dynamic QoS renegotiation.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 144
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-Event
> This attribute contains the type of SIP event for which the accounting-request message is generated.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 255
> Length
> 4
> Value
> ASCII string
> SN-Ext-Inline-Srvr-Context
> This attribute configures the context name in which the External In-line server resides.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 41
> Length
> 1–247
> Value
> String
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Ext-Inline-Srvr-Down-Addr
> This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 56
> Length
> 4
> Value
> IPv4 address
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Ext-Inline-Srvr-Down-VLAN
> This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 59
> Length
> 4
> Value
> The VLAN tag to apply.
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Ext-Inline-Srvr-Preference
> This attribute configures the preference for the tagged group of External In-line Servers. This attribute is required, although it doesn't actually assign a preference right now. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 57
> Length
> 4
> Value
> Unsigned integer
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Ext-Inline-Srvr-Up-Addr
> This attribute configures the IP address of the Upstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 55
> Length
> 4
> Value
> IPv4 address
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Ext-Inline-Srvr-Up-VLAN
> This attribute configures the VLAN tag to be applied to Upstream packets and forwarded to the External In-line server. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 58
> Length
> 4
> Value
> The VLAN tag to apply.
> Important: This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
> SN-Fast-Reauth-Username
> Fast re-authentication user name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 304
> Length
> 1–128
> Value
> Opaque value
> SN-Firewall-Enabled
> Firewall for subscriber enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 198
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> SN-Firewall-Policy
> This attribute contains the firewall policy value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 239
> Length
> 1–63
> Value
> String
> SN-FMC-Location
> MAC address and CDMA location information.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 171
> Length
> 1–247
> Value
> String
> SN-GGSN-Address
> The control plane IP address of the GGSN that handles one or more media component(s) of an IMS session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 264
> Length
> 4
> Value
> IPv4 address
> SN-GGSN-MIP-Required
> This attribute specifies if MIP is required for the GGSN subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 68
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-Gratuitous-ARP-Aggressive
> This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 54
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not send Gratuitous ARP

> • | Enabled = 1 — Send Gratuitous ARP in Aggressive mode

> SN-GTP-Version
> This attribute indicates the version of GTP the subscriber is using.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 62
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | GTP_VERSION_0 = 0

> • | GTP_VERSION_1 = 1

> SN-HA-Send-DNS-ADDRESS
> This attribute specifies if the HA should send the DNS address in the Mobile IP RRP message. The default is not to send the DNS address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 47
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not send

> • | Enabled = 1 — Send

> SN-Home-Behavior
> Configuration for the behavior bits settings for a home subscriber in an APN
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 119
> Length
> 4
> Value
> Unsigned integer
> SN-Home-Profile
> Configuration for the profile bits settings for a subscriber in an APN
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 109
> Length
> 4
> Value
> Unsigned integer
> SN-Home-Sub-Use-GGSN
> Configures GGSN to accept GGSN's charging characteristics for home subscribers defined for the APN, if the subscriber is home.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 106
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN-IMS-AM-Address
> IMS application manager address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 167
> Length
> 4
> Value
> IPv4 address
> SN-IMS-AM-Domain-Name
> IMS application manager domain name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 168
> Length
> 1–64
> Value
> String
> SN-IMS-Charging-Identifier
> This attribute holds the IMS Charging Identifier (ICID) as generated by an IMS node for a SIP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 260
> Length
> 4
> Value
> ASCII string
> SN-IMSI
> SN-IMSI
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 252
> Length
> 1–8
> Value
> Opaque value
> SN-Inactivity-Time
> This attribute contains the inactivity time duration for a subscriber session under long time duration timer configuration.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 275
> Length
> 4
> Value
> Integer
> SN-Internal-SM-Index
> SN-Internal-SM-Index
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 122
> Length
> 4
> Value
> Unsigned integer
> SN-IP-Alloc-Method
> This attribute specifies the method for allocating an IP address. This feature only applies to the GGSN service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 53
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Alloc_Local_Pool = 0

> • | Alloc_Dhcp_Client = 1

> • | Alloc_Radius = 2

> • | Alloc_No_Alloc = 3

> • | Alloc_Static_Alloc = 4

> • | Alloc_Dhcp_Relay = 5

> SN-IP-Filter-In
> IP input filter rules.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 10
> Length
> 1–253
> Value
> String
> SN-IP-Filter-Out
> IP output filter.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 11
> Length
> 1–253
> Value
> String
> SN-IP-Header-Compression
> Specifies the IP header compression method to use.
> Type
> Type 26
> Vendor ID
> 8164
> VSA Type
> 150
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | VJ = 1

> • | ROHC = 2

> • | VJ_ROHC = 3

> SN-IP-Hide-Service-Address
> This attribute prevents subscribers from using traceroute to discover the public domain network addresses configured on HA and other services on the system.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 60
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0 — Disabled

> • | Yes = 1 — Enabled

> SN-IP-In-ACL
> This attribute contains a definition for one Input IP Access Control List, which is used to filter the IP packets coming from the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 17
> Length
> 1–253
> Value
> ASCII string
> SN-IP-In-Plcy-Grp
> This attribute specifies the name of the policy group configuration applied in the uplink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 193
> Length
> 1–15
> Value
> String
> SN-IP-Out-ACL
> This attribute contains a definition for one Output IP Access Control List, which is used to filter the IP packets sent to the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 18
> Length
> 1–253
> Value
> ASCII string
> SN-IP-Out-Plcy-Grp
> This attribute specifies the name of the policy group configuration applied in the downlink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 194
> Length
> 1–15
> Value
> String
> SN-IP-Pool-Name
> This vendor-specific attribute indicates the name of the IP pool from which an IP address should be allocated to the subscriber. Also, see Framed-Pool, which is the standard attribute accomplishing the same.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 8
> Length
> 1–253
> Value
> ASCII string
> SN-IP-Source-Validation
> This attribute indicates if the source IP address should be validated before forwarding the IP packet.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 14
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0 — No Validation

> • | Yes = 1 — Validated

> SN-IP-Source-Violate-No-Acct
> When enabled, This attribute excludes the Source Violated IP packets and byte counts when reporting the Octet and Packet count in an accounting message.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 196
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-IP-Src-Validation-Drop-Limit
> Maximum number of packet drops entertained before disconnecting the session for source violated packets for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 110
> Length
> 4
> Value
> Unsigned integer
> SN-IPv6-DNS-Proxy
> IPV6 DNS Proxy Enabled or Disabled Setting for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 126
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-IPv6-Egress-Filtering
> This attribute enables egress filtering to make sure that packets being sent to the mobile device have an interface ID that matches that of the mobile device. This feature is meant to protect the Mobile from receiving unwanted packets from the Internet.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 103
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-IPv6-Min-Link-MTU
> IPV6 MTU size.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 136
> Length
> 4
> Value
> Unsigned integer
> SN-IPv6-num-rtr-advt
> This attribute indicates the IPv6 number of Initial Router Advertisements. The default value is 3.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 97
> Length
> 4
> Value
> Unsigned integer
> SN-IPv6-Primary-DNS
> This attribute specifies a Primary DNS server address that the Router Advertisement message sent by the PDSN will include.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 101
> Length
> 2
> Value
> IPv6 address
> SN-IPv6-rtr-advt-interval
> This attribute indicates the IPv6 Initial Router Advertisement Interval specified in milliseconds. The default value is 3000.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 96
> Length
> 4
> Value
> Unsigned integer
> SN-IPv6-Secondary-DNS
> This attribute specifies a Secondary DNS server address that the Router Advertisement message sent by the PDSN will include.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 102
> Length
> 16
> Value
> Opaque value
> SN-IPv6-Sec-Pool
> IPv6 secondary pool names.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 124
> Length
> 1–253
> Value
> String
> SN-IPv6-Sec-Prefix
> IPv6 Secondary Pool name prefix.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 125
> Length
> 2–18
> Value
> Opaque value
> SN-ISC-Template-Name
> This attribute contains name of the CSCF ISC template to be used for a subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 276
> Length
> 0-255
> Value
> ASCII string
> SN-Is-Unregistered-Subscriber
> This attribute specifies if a subscriber is registered or not.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 269
> Length
> 4
> Value
> ASCII string
> SN-L3-to-L2-Tun-Addr-Policy
> This attribute specifies the address allocation policy.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 43
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | no-local-alloc-validate = 0 — Do not locally allocate, do not validate

> • | local-alloc = 1 — Locally allocate

> • | local-alloc-validate = 2 — Locally allocate and validate

> SN-Local-IP-Address
> This attribute indicates the IP address of the local interface on the chassis for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 13
> Length
> 4
> Value
> IPv4 address
> SN-Long-Duration-Action
> This attribute specifies the action to take place when the long duration timeout expires for a subscriber session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 45
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Detection = 1 — Detect the session and alert the administrator

> • | Disconnection = 2 — Disconnect the session

> • | Dormant-Only-Disconnection = 3

> • | Dormant-Only-Detection = 4

> SN-Long-Duration-Notification
> SN-Long-Duration-Notification.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 253
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Suppress = 0

> • | Send = 1

> SN-Long-Duration-Timeout
> This attribute is used to detect and if necessary disconnect sessions connected to the PDSN. This attribute configures the time period, in seconds, before either alerting the administrator or disconnecting the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 44
> Length
> 4
> Value
> Integer
> SN-Max-Sec-Contexts-Per-Subs
> Maximum secondary PDP contexts per subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 290
> Length
> 2
> Value
> Unsigned integer
> SN-Mediation-Acct-Rsp-Action
> When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the Mediation Accounting server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the Mediation Accounting server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the Mediation Accounting server.
> Type
> Type 26
> Vendor ID
> Vendor-ID 8164
> VSA Type
> 105
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | No_Early_PDUs = 1

> • | Delay_GTP_Response = 2

> SN-Mediation-Enabled
> Mediation Accounting Enabled or Disabled settings for GGSN
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 123
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-Mediation-No-Interims
> Disable or Enable mediation Interim records for this session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 146
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-Mediation-VPN-Name
> Mediation context name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 104
> Length
> 1–128
> Value
> String
> SN-Min-Compress-Size
> This attribute indicates the minimum size (in octets) a data packet can have in order to be compressed.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 23
> Length
> 4
> Value
> Unsigned integer
> SN-MIP-AAA-Assign-Addr
> This attribute specifies if the PDSN/FA will allow AAA to assign the home address. The default is to not allow AAA to assign the home address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 50
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not allow AAA to assign home address

> • | Enabled = 1 — Allow AAA to assign home address

> SN-MIP-ANCID
> Accounting correlation ID created by IPGW, received by VBM and HBM.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 166
> Length
> 12
> Value
> Opaque value
> SN-MIP-Dual-Anchor
> Enable/disable dual-anchor service for a subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 165
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-MIP-HA-Assignment-Table
> MIP-HA Assignment Table name. When this is received in an Access Accept message, the system uses this local table to get the HA Address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 154
> Length
> 1–253
> Value
> ASCII string
> SN-MIP-Match-AAA-Assign-Addr
> This attribute specifies if the PDSN/FA will enforce that a non-zero AAA-specified home address must match the home address present in the MIP RRQ from the mobile node, and disconnect the subscriber session if a match is not present. The default is not to force the addresses to match.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 51
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not force the AAA-specified home address to match RRQ

> • | Enabled = 1 — Force the AAA-specified home address to match RRQ

> SN-MIP-Reg-Lifetime-Realm
> Configure the maximum MIP registration lifetime for a subscriber/realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 175
> Length
> 2
> Value
> Unsigned integer
> SN-MIP-Send-Ancid
> AAA attribute to enable/disable sending ANCID from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 163
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-MIP-Send-Correlation-Info
> AAA Attribute to enable/disable sending of correlation-id from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 188
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | Disabled = 0

> • | Enabled = 1

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0

> • | NVSE_Starent = 1

> • | NVSE_CUstom1 = 2

> • | NVSE_Custom2 = 3

> SN-MIP-Send-Imsi
> AAA attribute to enable/disable sending IMSI from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 164
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS and 8.1 and earlier, supported values are:

> • | None = 0

> • | Starent_NVSE = 1

> • | Custom1_NVSE = 2

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0

> • | NVSE_Starent = 1

> • | NVSE_Custom1 = 2

> • | NVSE_Custom2 = 3

> SN-MIP-Send-Term-Verification
> This attribute specifies whether the PDSN/FA should send the Terminal Verification Normal Vendor/Organization Specific Extension (NVSE) in the Mobile IP RRQ message to the HA. The default is not to send the Terminal Verification NVSE.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 48
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | Disabled = 0 — Do not send

> • | Enabled = 1 — Send

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0

> • | NVSE_Custom1 = 1 — Send custom NVSE

> • | NVSE_Custom2 = 2 — Send custom NVSE

> • | NVSE_Starent = 3 — Send custom NVSE

> SN-MN-HA-Hash-Algorithm
> This attribute contains the hash algorithm to use for MN-HA authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 99
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | MD5 = 1

> • | MD5-RFC2002 = 2

> • | HMAC-MD5 = 3

> SN-MN-HA-Timestamp-Tolerance
> This attribute indicates the duration of timestamp tolerance, in seconds, to use for MN-HA authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 30
> Length
> 4
> Value
> Unsigned integer
> SN-Mode
> Robust Header Compression (ROHC) Mode. Reliable mode means each ROHC control needs to be Acknowledged. Optimistic mode is a modified version to reduce the number of control messages and bandwidth consumption. Unidirectional assumes a one way link without any Feedback from the decompressor.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 151
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Reliable = 0

> • | Optimistic = 1

> • | Unidirectional = 2

> SN-MS-ISDN
> SN-MS-ISDN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 248
> Length
> 1–9
> Value
> Opaque value
> SN-MSK-Lifetime
> This attribute is currently not supported.
> SN-NAI-Construction-Domain
> This attribute specifies the domain name to use when constructing the NAI.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 37
> Length
> 1–247
> Value
> String
> SN-NAT-IP-Address
> This attribute includes the NAT (public) IP address used for the call.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 297
> Length
> 4
> Value
> IPv4 address
> SN-Node-Functionality
> This attribute includes the functionality identifier of the IMS node where the cause code was generated.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 268
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | S-CSCF = 0

> • | P-CSCF = 1

> • | I-CSCF = 2

> SN-NPU-Qos-Priority
> This attribute configures Inter-Subscriber priority Queueing based on class of service offered. Gold has highest priority and Best_effort lowest priority. From DSCP, means the priority queueing will be done based on the DSCP marking the incoming subscriber packet carries.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 98
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best_Effort = 0

> • | Bronze = 1

> • | Silver = 2

> • | Gold = 3

> • | From_DSCP = 4

> SN-Ntk-Initiated-Ctx-Ind-Flag
> Indicates whether the GGSN call is a network initiated PDP Context.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 142
> Length
> 1
> Value
> Opaque value
> SN-Ntk-Session-Disconnect-Flag
> SN-Ntk-Session-Disconnect-Flag.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 143
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Session-Disconnect = 1

> SN-Nw-Reachability-Server-Name
> This attribute Specifies the name of the Network Reachability Detection Server.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 65
> Length
> 1–16
> Value
> String
> SN-Originating-IOI
> This attribute holds the Inter Operator Identifier for the originating network in the home network of the originating end user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 261
> Length
> 1–253
> Value
> ASCII string
> SN-Overload-Disc-Connect-Time
> This attribute provides inactivity time for session to become candidate for disconnection during overload.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 233
> Length
> 4
> Value
> Unsigned integer
> SN-Overload-Disc-Inact-Time
> This attribute provides inactivity time for session to become candidate for disconnection during overload.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 234
> Length
> 4
> Value
> Unsigned integer
> SN-Overload-Disconnect
> This attribute enables (if one) and disables the overload-disconnect feature for a subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 235
> Length
> 4
> Value
> Unsigned integer
> SN-PDG-TTG-Required
> TTG mode of operation Required for PDG.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 299
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-PDIF-MIP-Release-TIA
> PDIF mobile IP release TIA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 172
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-PDIF-MIP-Required
> PDIF mobile IP required.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 170
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-PDIF-MIP-Simple-IP-Fallback
> PDIF mobile IP simple IP fallback.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 173
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-PDSN-Correlation-Id
> Correlation ID received from PDSN to HA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 189
> Length
> 8
> Value
> Opaque value
> SN-PDSN-Handoff-Req-IP-Addr
> This attribute specifies if the PDSN should reject and terminate the subscriber session when the proposed address in IPCP by the mobile does not match the existing address in the PDSN. The default (Disabled) is not to reject these sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 46
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not reject

> • | Enabled = 1 — Reject

> SN-PDSN-NAS-Id
> NAS Identifier received from PDSN to HA
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 190
> Length
> 1–253
> Value
> String
> SN-PDSN-NAS-IP-Address
> NAS IP Address received from PDSN to HA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 191
> Length
> 4
> Value
> IPv4 address
> SN-Permit-User-Mcast-PDUs
> Specifies whether or not to let the subscriber discard multicast PDUs.
> Type
> 26
> Vendor ID
> 8164
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | disabled = 0

> • | enabled = 1

> SN-PPP-Accept-Peer-v6Ifid
> This attribute indicates the acceptance of the interface ID provided by peer during PPP IPv6CP if the ID is valid. The default is disabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 95
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not accept interface ID

> • | Enabled = 1 — Accept interface ID

> SN-PPP-Always-On-Vse
> SN-PPP-Always-On-Vse.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 130
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-PPP-Data-Compression
> This attribute indicates the PPP data compression algorithm to use for the PPP session. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 9
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Stac-LZS = 1

> • | MPPC = 2

> • | Deflate = 4

> SN-PPP-Data-Compression-Mode
> This attribute indicates the PPP data compression mode to use for the PPP session when PPP data compression is used.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 19
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Stateless = 1

> SN-PPP-Keepalive
> This attribute indicates the interval for the PPP keepalive, in seconds.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 16
> Length
> 4
> Value
> Unsigned integer
> SN-PPP-NW-Layer-IPv4
> This attribute indicates the PPP IPCP negotiation for IPv4. The default is enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 92
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — IPCP negotiation for IPv4 is disabled.

> • | Enabled = 1 — IPCP negotiation for IPv4 is enabled.

> • | Passive = 2 — Start the negotiation only if peer initiates it.

> SN-PPP-NW-Layer-IPv6
> This attribute indicates the PPP IPv6CP negotiation for IPv6. The default is enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 93
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — IPCP negotiation for IPv6 is disabled.

> • | Enabled = 1 — IPCP negotiation for IPv6 is enabled.

> • | Passive = 2 — Start the negotiation only if peer initiates it.

> SN-PPP-Outbound-Password
> This attribute indicates the password to be used when the user side of the PPP connection requires authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 15
> Length
> 1–247
> Value
> ASCII string
> SN-PPP-Outbound-Username
> This attribute indicates the username to be used when the user side of the PPP connection requires authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 61
> Length
> 1–247
> Value
> ASCII string
> SN-PPP-Progress-Code
> This attribute provides information about the “state” of the PPP connection, when the connection was terminated.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 4
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Not-Defined = 0

> • | Call-Lcp-Down = 10

> • | Call-Disconnecting = 20

> • | Call-Ppp-Renegotiating = 30

> • | Call-Arrived = 40

> • | Call-Pdg-Tcp-Connecting = 45

> • | Call-Pdg-Ssl-Connecting = 46

> • | Call-Lcp-Up = 50

> • | Call-Authenticating = 60

> • | Call-Bcmcs-Authenticating = 70

> • | Call-Authenticated = 80

> • | Call-Tunnel-Connecting = 85

> • | Call-Ipcp-Up = 90

> • | Call-Imsa-Authorizing = 95

> • | Call-Imsa-Authorized = 97

> • | Call-MBMS-UE-Authorizing = 98

> • | Call-MBMS-Bearer-Authorizing = 99

> • | Call-Simple-IP-Connected = 100

> • | Call-Mobile-IP-Connected = 110

> • | Call-Tunnel-Connected = 115

> • | Call-Pdp-Type-IP-Connected = 120

> • | Call-Pdp-Type-IPv6-Connected = 125

> • | Call-Pdp-Type-PPP-Connected = 130

> • | Call-Proxy-Mobile-IP-Connected = 140

> • | Call-Pdg-Connected = 142

> • | Call-Pdg-Ssl-Connected = 141

> • | Call-Pdg-Connected = 142

> • | Call-Pdg-Connected = 142

> • | Call-Ipsg-Connected = 145

> • | Call-Bcmcs-Connected = 150

> • | Call-MBMS-UE-Connected = 155

> • | Call-MBMS-Bearer-Connected = 156

> • | Call-Pending-Addr-From-DHCP = 160

> • | Call-Got-Addr-From-DHCP = 170

> • | Call-HA-IPSEC-Tunnel-Connecting = 180

> • | Call-HA-IPSEC-Connected = 190

> • | Call-ASN-Non-Anchor-Connected = 200

> • | Call-ASNPC-Connected = 210

> • | Call-Mobile-IPv6-Connected = 220

> • | Call-PMIPv6-Connected = 221

> • | Call-PHSPC-Connected = 230

> • | Call-GTP-IPv4-Connected = 235

> • | Call-GTP-IPv6-Connected = 236

> • | Call-GTP-IPv4-IPv6-Connected = 237

> • | Call-SGW-Connected = 245

> • | Call-MME-Attached = 246

> • | Call-Auth-Only-Connected = 247

> SN-PPP-Reneg-Disc
> PPP remote reneg disconnect policy
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 187
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Never = 0

> • | Always = 1

> • | NAI_Prefix_MSID_Mismatch = 2

> SN-Prepaid
> Prepaid
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 128
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | no_prepaid = 0

> • | custom_prepaid = 1

> • | standard_prepaid = 2

> • | wimax_prepaid = 4

> SN-Prepaid-Compressed-Count
> This attribute indicates if a Pre-paid subscriber's byte usage should be counted on the basis of compressed or uncompressed byte data over the subscriber's PPP connection to the system. If not present, the default is to count uncompressed byte data.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 31
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Uncompressed = 0

> • | Compressed = 1

> SN-Prepaid-Final-Duration-Alg
> For prepaid, final duration is calculated based on the algorithm specified by the value of this attribute.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 135
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | current_time = 0

> • | last-user-layer3-activity-time = 1

> • | last-airlink-activity-time = 2

> • | last-airlink-activity-time-last-reported = 3

> SN-Prepaid-Inbound-Octets
> In an Access-Accept, this indicates how many additional inbound (bytes delivered to the subscriber) byte credits should be granted to the subscriber. In an Accounting- Request, this indicates how many total inbound byte credits have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on an inbound octet basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 32
> Length
> 4
> Value
> Unsigned integer
> SN-Prepaid-Outbound-Octets
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 33
> Length
> 4
> Value
> Unsigned integer
> SN-Prepaid-Preference
> This attribute specifies whether prepaid is volume based or duration based.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 129
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | prepaid_duration = 0

> • | prepaid_volume = 1

> SN-Prepaid-Timeout
> This attribute indicates how much time may elapse before a new request for more pre-paid credits is issued. If the specified time has elapsed since the prior grant of credits was received from the RADIUS server, then a new request for credits is issued. This attribute is primarily used to periodically update the subscriber of new credits issued since the subscriber was connected. Note that credit requests will still be made on behalf of the subscriber when the subscriber drops down to the low watermark of credits (or zero if there is no low watermark). The presence or absence of this attribute does not affect that mechanism in any way. However, this timer is re-set whenever any grant of credits is received on behalf of the subscriber, regardless of why the grant of credits was requested.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 35
> Length
> 4
> SN-Prepaid-Total-Octets
> In an Access-Accept, this attribute indicates how many additional byte credits (combining both inbound and outbound counts) should be granted to the subscriber. In an Accounting- Request, this indicates how many total bytes credits (combined inbound and outbound) have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on a combined inbound and outbound octet-count basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 34
> Length
> 4
> Value
> Unsigned integer
> SN-Prepaid-Watermark
> This attribute Indicates the percentage of remaining granted credits that will trigger a new request to grant credits from the RADIUS server. For example, if 1GB of credits was granted to a user, and the value of SN-Prepaid-Watermark was 10, then when 100 MB of credits are remaining (900 MB have been used) to the subscriber, a new request for any new byte credits is issued on behalf of the subscriber. Note that when calculating the pre-paid low watermark, the total credits granted for the subscriber's entire session is used.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 36
> Length
> 4
> SN-Primary-DCCA-Peer
> This attribute indicates the name of the primary DCCA peer and primary DCCA realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 223
> Length
> 2
> Value
> A colon separated string, like “primary_peer : primary_realm”
> SN-Primary-DNS-Server
> This attribute indicates the IP address of the primary DNS server that should be used for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 5
> Length
> 4
> Value
> IPv4 address
> SN-Primary-NBNS-Server
> Primary NBNS Server IP address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 148
> Length
> 4
> Value
> IPv4 address
> SN-Proxy-MIP
> This attribute specifies if the PDSN/FA will perform compulsory Proxy-MIP tunneling for a Simple-IP PDSN subscriber. This feature is licensed. The default is not to perform compulsory Proxy-MIP.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 52
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not perform compulsory Proxy-MIP

> • | Enabled = 1 — Perform compulsory Proxy-MIP

> SN-Pseudonym-Username
> This attribute contains the pseudonym user name generated by AAA server.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 305
> Length
> 1-256
> Value
> Opaque value
> SN-QoS-Background-Class
> This attribute defines the QOS Background Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 91
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QoS-Class-Background-PHB
> Quality of Service DSCP classification value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 113
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Class-Conversational-PHB
> Quality of Service DSCP classification value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 111
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Class-Interactive-1-PHB
> Interactive-1 class PHB value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 114
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Class-Interactive-2-PHB
> Interactive-2 class PHB.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 115
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Class-Interactive-3-PHB
> Interactive-3 class PHB.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 115
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Class-Streaming-PHB
> Quality of Service DSCP classification value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 112
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN-QoS-Conversation-Class
> This attribute defines the QOS Conversation Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 86
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QOS-HLR-Profile
> QoS with Allocation Retention bit. QoS structured as per 29.002.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 303
> Length
> 1–35
> Value
> Opaque
> SN-QoS-Interactive1-Class
> This attribute defines the QOS Interactive TrafficClass.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 88
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QoS-Interactive2-Class
> This attribute defines the QOS Interactive2 Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 89
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QoS-Interactive3-Class
> This attribute defines the QOS Interactive3 Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 90
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QoS-Negotiated
> Negotiated QoS for GGSN sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 147
> Length
> 4-17
> Value
> ASCII string
> SN-QoS-Renegotiation-Timeout
> This attribute configures the timeout duration of dampening time for dynamic QoS renegotiation.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 145
> Length
> 4
> Value
> Unsigned integer
> SN-QoS-Streaming-Class
> This attribute defines the QOS Streaming Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 87
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN-QoS-Tp-Dnlk
> This attribute enables/disables Traffic Policing/Shaping in downlink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 73
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Policing = 1

> • | Shaping = 2

> SN-QoS-Tp-Uplk
> This attribute enables/disables Traffic Policing/Shaping in uplink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 79
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Policing = 1

> • | Shaping = 2

> SN-QoS-Traffic-Policy
> This compound attribute simplifies sending QoS values for Traffic Class, Direction, Burst-Size, Committed-Data-Rate, Peak-Data-Rate, Exceed-Action, and Violate-Action from the RADIUS server. When the SN-QoS-Traffic-Policy attribute is sent along with Acct-Session-ID attribute, the system matches the particular PDP context, and applies the new policy and retains the policy with the subscriber profile for future use. The next time the system sends a CoA request with a new policy and a different Acct-Session-ID for the same subscriber, the previously received policy is also applied to the matching PDP context along with the new policy.
> Important: This attribute is specific to the GGSN service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 177
> Value
> Contains the following subattributes:
> Direction
> Direction of traffic.
> Type
> 1
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Downlink = 0

> • | Uplink = 1

> Class
> Traffic class.
> Type
> 2
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Undefined = 0

> • | Conversational = 1

> • | Streaming = 2

> • | Interactive TP 1 = 4

> • | Interactive TP 2 = 5

> • | Interactive TP 3 = 6

> • | Background = 7

> Burst-Size
> Peak burst size.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer.
> Committed-Data-Rate
> Committed data rate.
> Type
> 4
> Length
> 4
> Value
> Unsigned integer.
> Peak-Data-Rate
> Peak data rate.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer.
> Exceed-Action
> Action to take on packets that exceed the Committed-Data-Rate but do not violate the Peak-Data-Rate.
> Type
> 6
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower IP Precedence = 2

> Violate-Action
> Violate action.
> Type
> 7
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower IP Precedence = 2

> • | Buffer = 3

> • | Buffer-Transmit-On-Full = 4

> Auto-Readjust-Enabled
> Available only in StarOS 8.1 and later. Auto-readjust enabled.
> Type
> 8
> Length
> 1
> Value
> Unsigned integer.
> Auto-Readjust-Duration
> Available only in StarOS 8.1 and later. Auto-readjust duration.
> Type
> 9
> Length
> 4
> Value
> Unsigned integer.
> SN-Rad-APN-Name
> RADIUS returned APN name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 162
> Length
> 1–64
> Value
> Opaque value
> SN-Radius-Returned-Username
> This attribute is used to prefer RADIUS returned username over constructed username in the accounting messages.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 236
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN-Re-CHAP-Interval
> The Periodic CHAP authentication interval for PPP, in seconds.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 7
> Length
> 4
> Value
> Unsigned integer
> SN-Roaming-Behavior
> Configuration for the behavior bits settings for a roaming subscriber in an APN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 121
> Length
> 4
> Value
> Unsigned integer
> SN-Roaming-Profile
> Configuration for the profile bits settings for a roaming subscriber in an APN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 118
> Length
> 4
> Value
> Unsigned integer
> SN-Roaming-Sub-Use-GGSN
> Configures GGSN to accept GGSN's charging characteristics for roaming subscribers defined for the APN, if the subscriber is roaming.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 108
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN-ROHC-Flow-Marking-Mode
> Configure ROHC compression for marked flows only.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 274
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> SN-ROHC-Mode
> ROHC Mode.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 151
> Length
> 4
> Value
> An integer in network order. Supported values are:

> • | Reliable = 0

> • | Optimistic = 1

> • | Unidirectional = 2

> SN-ROHC-Profile-Name
> Specifies the ROHC profile to use for the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 238
> Length
> 1–64
> Value
> ASCII string
> SN-Role-Of-Node
> This attribute denotes the role of the CSCF.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 256
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | ORIGINATING_ROLE = 0

> • | TERMINATING_ROLE = 1

> SN-Routing-Area-Id
> For GGSN calls this indicates the Routing Area ID of the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 249
> Length
> 3
> Value
> String
> SN-Rulebase
> When the session is active charging enabled, Rulebase name will specify one of the pre configured ECSv2 rulebases in active charging subsystem.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 250
> Length
> 1–64
> Value
> String
> SN-SDP-Media-Components
> This attribute is currently not supported. See SN-CSCF-Rf-SDP-Media-Components.
> SN-SDP-Session-Description
> This attribute contains the Session portion of the SDP data exchanged between the User Agents in the SIP transaction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 263
> Length
> 4
> Value
> ASCII string
> SN-Sec-IP-Pool-Name
> Available only in StarOS 8.1 and later. This attribute contains the secondary IP pool name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 265
> Length
> 1–253
> Value
> String
> SN-Secondary-DCCA-Peer
> This attribute indicates the name of the Secondary DCCA peer and Secondary DCCA realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 224
> Length
> 1–192
> Value
> A colon separated string, like “secondary_peer : secondary_realm”.
> SN-Secondary-DNS-Server
> This attribute indicates the IP address of the secondary DNS server that should be used for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 6
> Length
> 4
> Value
> IPv4 address
> SN-Secondary-NBNS-Server
> Secondary NBNS Server IP Address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 149
> Length
> 4
> Value
> IPv4 address
> SN-Served-Party-Address
> This attribute is currently not supported.
> SN-Service-Address
> Used to send the bind IP address of the service in RADIUS messages.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 169
> Length
> 4
> Value
> IPv4 address
> SN-Service-Type
> This attribute indicates the service type that the user is accessing.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | PDSN = 1

> • | Management = 2

> • | HA = 3

> • | GGSN = 4

> • | LNS = 5

> • | IPSG = 6

> • | CSCF = 7

> • | ASNGW = 8

> • | PDIF = 9

> • | STANDALONE_FA = 10

> • | SGSN = 11

> • | PHSGW = 12

> • | PDG = 13

> • | MIPV6HA = 14

> • | PGW = 15

> • | SGW = 16

> • | FNG=17

> SN-Session-Id
> This attribute contains Call-ID of the SIP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 257
> Length
> 4
> Value
> ASCII string
> SN-Simultaneous-SIP-MIP
> This attribute indicates if a PDSN Subscriber can simultaneously be given Simple IP and Mobile IP service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 22
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-SIP-Method
> This attribute identifies the SIP-method for which acct request is sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 254
> Length
> 4
> Value
> ASCII string
> SN-SIP-Request-Time-Stamp
> This attribute specifies the time of initial SIP request.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 258
> Length
> 4
> Value
> ASCII string
> SN-SIP-Response-Time-Stamp
> This attribute specifies the time of response to initial SIP request.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 259
> Length
> 4
> Value
> ASCII string
> SN-Software-Version
> Provides the Software version. This contains the major version number, minor version number and build number.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 288
> Length
> 1–32
> Value
> ASCII string
> SN-Subs-Acc-Flow-Traffic-Valid
> This attribute indicates the subscriber account flow traffic is valid.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 225
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN-Subscriber-Accounting
> This attribute indicates the accounting method to be used for subscriber sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 64
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Radius = 1

> • | GTPP = 2

> SN-Subscriber-Acct-Interim
> This attribute specifies if accounting INTERIM messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context (along with a specific INTERIM interval), if accounting INTERIM messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 70
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN-Subscriber-Acct-Mode
> This attribute displays the SN Subscriber Accounting Mode.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 192
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | flow-based-auxilliary = 0

> • | flow-based-all = 1

> • | flow-based-none = 2

> • | session-based = 3

> • | main-a10-only = 4

> SN-Subscriber-Acct-Rsp-Action
> When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the RADIUS server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the RADIUS server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the RADIUS server.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 100
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | No_Early_PDUs = 1

> • | Delay_GTP_Response = 2

> SN-Subscriber-Acct-Start
> This attribute specifies if accounting START messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting START messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 69
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN-Subscriber-Acct-Stop
> This attribute specifies if accounting STOP messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting STOP messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 71
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN-Subscriber-Class
> Customer-requested attribute for supporting specific behavior for their subscriber billing.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 219
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal_Subscriber = 0

> • | Ting_100 = 1

> • | Ting_500 = 2

> • | Ting_Buddy = 3

> • | Ting_Star = 4

> • | Ting_Nolimit_SMS = 5

> • | Kids_Locator = 6

> • | Ting_2000 = 7

> • | Handicapped_Welfare = 8

> • | Reserved = 9

> SN-Subscriber-Dormant-Activity
> This attribute specifies whether to treat dormant packets routed to the mobile as activity for idle timeout purposes. The default is Enabled. Disabled means dormant packets routed to the mobile is not treated as activity for idle timeout purposes.
> Type
> 26
> Vendor ID
> 8164
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-Subscriber-IP-Hdr-Neg-Mode
> This attribute specifies whether to wait (detect) for IP header compression to be requested by the mobile before responding, or not to wait (force). Force is the default.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 67
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Force = 0

> • | Detect = 1

> SN-Subscriber-IP-TOS-Copy
> This attribute controls the copying of the IP TOS octet value from IPv4 datagrams to the IP header in tunnel encapsulation.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 85
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Access-Tunnel = 1

> • | Data-Tunnel = 2

> • | Both = 3

> SN-Subscriber-Nexthop-Address
> This attribute specifies the nexthop gateway address to be returned by AAA on a per subscriber basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 127
> Length
> 4
> Value
> IPv4 address
> SN-Subscriber-No-Interims
> This is a GGSN specific attribute. When set to 0 (disabled) interim accounting is generated. When set to 1 (enabled) interim accounting generation is disabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 133
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Enabled = 0

> • | Disabled = 1

> SN-Subscriber-Permission
> This attribute indicates the services allowed to be delivered to the subscriber. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 20
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | None = 0

> • | Simple-IP = 1

> • | Mobile-IP = 2

> • | Simple-IP-Mobile-IP = 3

> • | HA-Mobile-IP = 4

> • | Simple-IP-HA-Mobile-IP = 5

> • | Mobile-IP-HA-Mobile-IP = 6

> • | All = 7

> • | In StarOS 8.3 and later, supported values are:

> • | None = 0

> • | Simple-IP = 1

> • | Mobile-IP = 2

> • | Simple-IP-Mobile-IP = 3

> • | HA-Mobile-IP = 4

> • | Simple-IP-HA-Mobile-IP = 5

> • | Mobile-IP-HA-Mobile-IP = 6

> • | SIP-MIP-HA-MIP = 7

> • | GGSN-PDP-TYPE-IP = 0x08, # see SessSubscriberPermission in sess_common.x

> • | GGSN-PDP-TYPE-PPP = 0x10, # see SessSubscriberPermission in sess_common.x

> • | Network-Mobility = 0x20

> • | FA-HA-NEMO = 0x26

> • | All = 0x3F

> SN-Subscriber-Template-Name
> RADIUS returned Subscriber Template
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 158
> Length
> 1–127
> Value
> String
> SN-Subs-IMSA-Service-Name
> IMS Authorization Service name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 159
> Length
> 1–128
> Value
> String
> SN-Subs-VJ-Slotid-Cmp-Neg-Mode
> Enable/Disable slotid compression in either direction when using VJ compression.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 221
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Receive = 1

> • | Transmit = 2

> • | Both = 3

> SN-Transparent-Data
> This AVP is used by RADIUS to provide Global Title information for the GGSN to use in CDRs and Quota Auth.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 247
> Length
> In StarOS 8.1 and later: 1–247
> In StarOS 8.0: 1–237
> Value
> Opaque value
> SN-Terminating-IOI
> This attribute holds the Inter Operator Identifier for the originating network in the home network of the terminating end user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 262
> Length
> 4
> Value
> ASCII string
> SN-Tp-Dnlk-Burst-Size
> This attribute specifies the Traffic Policing downlink burst size in bytes.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 76
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Dnlk-Committed-Data-Rate
> This attribute specifies the Traffic Policing downlink committed data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 74
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Dnlk-Exceed-Action
> This attribute specifies the action to take on Traffic Policing downlink packets that exceed the committed-data-rate but do not violate the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 77
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN-Tp-Dnlk-Peak-Data-Rate
> This attribute specifies the Traffic Policing downlink peak data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 75
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Dnlk-Violate-Action
> This attribute specifies the action to take on Traffic Policing downlink packets that exceed both the committed-data-rate and the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 78
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN-Tp-Uplk-Burst-Size
> This attribute specifies the Traffic Policing uplink burst size in bytes.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 82
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Uplk-Committed-Data-Rate
> This attribute specifies the Traffic Policing uplink committed data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 80
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Uplk-Exceed-Action
> This attribute specifies the action to take on Traffic Policing uplink packets that exceed the committed-data-rate but do not violate the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 83
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN-Tp-Uplk-Peak-Data-Rate
> This attribute specifies the Traffic Policing Uplink Peak Data Rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 81
> Length
> 4
> Value
> Unsigned integer
> SN-Tp-Uplk-Violate-Action
> This attribute specifies the action to take on Traffic Policing uplink packets that exceed both the committed-data-rate and the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 84
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN-Traffic-Group
> This attribute is used to assign a tag to a FA or a group of FAs, so that traffic policy can be enforced based on the tag value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 161
> Length
> 2
> Value
> Unsigned integer
> SN-TrafficSelector-Class
> Identify the ipsec traffic selector class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 307
> Length
> 4
> Value
> Unsigned integer
> SN-Tun-Addr-Policy
> Describes IP address validation policy for non L2TP tunneled calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 156
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | no-local-alloc-validate = 0

> • | local-alloc = 1

> • | local-alloc-validate = 2

> SN-Tunnel-Gn
> Used to enable/disable Gn interface from PDG/TTG to GGSN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 174
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN-Tunnel-ISAKMP-Crypto-Map
> This attribute specifies the system-defined crypto map to use for the subscriber's Mobile-IP connection, when IPSec is used to protect the Mobile-IP connection. This attribute is salt-encrypted.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 38
> Length
> 1–128
> Value
> String
> SN-Tunnel-ISAKMP-Secret
> This attribute specifies the secret to use for IKE.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 39
> Length
> 1–128
> Value
> String
> SN-Tunnel-Load-Balancing
> This attribute specifies the load-balancing algorithm to use when tunneling is employed.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 27
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | random = 1

> • | balanced = 2

> • | prioritized = 3

> SN-Tunnel-Password
> This attribute contains a secret for tunneling usage. Currently this is only used for L2TP. It is recommended that you use the Tunnel-Password attribute if your RADIUS server supports salt-encryption of attributes.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 26
> Length
> 1–240
> Value
> Opaque value
> SN-Unclassify-List-Name
> Unclassify List Name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 132
> Length
> 1–32
> Value
> An ASCII string
> SN-Virtual-APN-Name
> This attribute indicates the virtual APN name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 94
> Length
> 1–64
> Value
> ASCII string
> SN-Visiting-Behavior
> Configuration for the behavior bits settings for a visiting subscriber in an APN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 120
> Length
> 4
> Value
> Unsigned integer
> SN-Visiting-Profile
> Configuration for the profile bits settings for a visiting subscriber in an APN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 117
> Length
> 4
> Value
> Unsigned integer
> SN-Visiting-Sub-Use-GGSN
> Configures GGSN to accept GGSN's charging characteristics for visiting subscribers defined for the APN, if the subscriber is visiting.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 107
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN-Voice-Push-List-Name
> SN-Voice-Push-List-Name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 131
> Length
> 1–32
> Value
> ASCII string
> SN-VPN-ID
> This attribute indicates the Destination VPN of the user, specified by a 32-bit identifier.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1
> Length
> 4
> Value
> Unsigned integer
> SN-VPN-Name
> This attribute indicates the name of the user’s Destination VPN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 2
> Length
> 1–253
> Value
> ASCII string
> SN-WiMAX-Auth-Only
> Specifies whether the call is established for Authentication Mode Only.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 306
> Length
> 1
> Value
> Enumerated integer. Supported values are:
> Disabled = 0
> Enabled = 1
> SN1-Access-link-IP-Frag
> This attribute specifies what to do when data received for the subscriber on the Access link that needs to be fragmented and the DF bit is either set or unset. The default is Normal.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 63
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0 — Data to be fragmented is not fragmented if the DF bit is set

> • | DF-Ignore = 1 — Fragment regardless

> • | DF-Fragment-ICMP-Notify = 2 — Fragment regardless, and ICMP Notify if DF bit is set

> SN1-Acct-Input-Giga-Dropped
> Contains the number of input gigawords dropped if the number of input bytes is greater than 2^32 - 1
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 230
> Length
> 4
> Value
> Unsigned integer
> SN1-Acct-Input-Octets-Dropped
> Contains the number of input bytes dropped.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 228
> Length
> 4
> Value
> Unsigned integer
> SN1-Acct-Input-Packets-Dropped
> Contains the number of input packets dropped.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 226
> Length
> 4
> Value
> Unsigned integer
> SN1-Acct-Output-Giga-Dropped
> Contains the number of output gigawords dropped if the number of output bytes is greater than 2^32 - 1.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 231
> Length
> 4
> Value
> integer
> SN1-Acct-Output-Octets-Dropped
> Contains the number of output bytes dropped.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 229
> Length
> 4
> Value
> Integer
> SN1-Acct-Output-Packets-Dropped
> Contains the number of output packets dropped.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 227
> Length
> 4
> Value
> Integer
> SN1-Admin-Expiry
> This attribute contains the date/time the administrative user account expires. It is an integer value specifying the number of seconds since the UNIX epoch at which time the account will expire.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 72
> Length
> 4
> Value
> Integer
> SN1-Admin-Permission
> This attribute indicates the services allowed to be delivered to the administrative user. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 21
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | CLI = 1

> • | FTP = 2

> • | CLI-FTP = 3

> • | Intercept = 4

> • | CLI-Intercept = 5

> • | CLI-Intercept-FTP = 7

> • | ECS = 8

> • | CLI-ECS = 9

> • | CLI-FTP-ECS = 11

> • | CLI-Intercept-ECS = 13

> • | CLI-Intercept-FTP-ECS = 15

> SN1-Assigned-VLAN-ID
> The VLAN ID assigned to the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 152
> Length
> 4
> Value
> Unsigned integer
> SN1-Call-Id
> Internal system generated call ID number for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 251
> Length
> 4
> Value
> Unsigned integer
> SN1-Cause-For-Rec-Closing
> This attribute contains a reason for the release of the CDR.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 139
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | normalRelease = 0

> • | abnormalRelease = 4

> • | volumeLimit = 16

> • | timeLimit = 17

> • | SGSNChange = 18

> • | maxChangeCond = 19

> • | managementIntervention = 20

> SN1-CFPolicy-ID
> Content Filtering policy ID.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 220
> Length
> 4
> Value
> Unsigned integer
> SN1-Change-Condition
> This attribute defines the reason for closing the container.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 140
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | QOSCHANGE = 0

> • | TARIFFTIMECHANGE = 1

> • | SGSNCHANGE = 500

> SN1-Charging-VPN-Name
> Charging VPN Name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 137
> Length
> 1–252
> Value
> String
> SN1-Chrg-Char-Selection-Mode
> This attribute indicates the charging characteristics type that the GSNs applied to the CDR.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 138
> Length
> 4
> Value
> Integer. Supported values are:

> • | SGSN = 0

> • | HOME = 3

> • | ROAMING = 4

> • | VISITING = 5

> SN1-Data-Tunnel-Ignore-DF-Bit
> This attribute specifies if the PDSN/FA or HA should ignore the DF bit in the IPv4 header when encapsulating the IPv4 packet in MIP, and therefore fragmenting the resulting tunneled packet if necessary. The default is not to ignore the DF bit.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 49
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not ignore DF bit

> • | Enabled = 1 — Ignore DF bit

> SN1-DHCP-Lease-Expiry-Policy
> This attribute specifies whether to renew or disconnect on expiry of IP address lease time.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 157
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | auto-renew = 0

> • | disconnect = 1

> SN1-Disconnect-Reason
> This attribute indicates the reason the user was disconnected from service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 3
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Not-Defined = 0

> • | Admin-Disconnect = 1

> • | Remote-Disconnect = 2

> • | Local-Disconnect = 3

> • | Disc-No-Resource = 4

> • | Disc-Excd-Service-Limit = 5

> • | PPP-LCP-Neg-Failed = 6

> • | PPP-LCP-No-Response = 7

> • | PPP-LCP-Loopback = 8

> • | PPP-LCP-Max-Retry = 9

> • | PPP-Echo-Failed = 10

> • | PPP-Auth-Failed = 11

> • | PPP-Auth-Failed-No-AAA-Resp = 12

> • | PPP-Auth-No-Response = 13

> • | PPP-Auth-Max-Retry = 14

> • | Invalid-AAA-Attr = 15

> • | Failed-User-Filter = 16

> • | Failed-Provide-Service = 17

> • | Invalid-IP-Address-AAA = 18

> • | Invalid-IP-Pool-AAA = 19

> • | PPP-IPCP-Neg-Failed = 20

> • | PPP-IPCP-No-Response = 21

> • | PPP-IPCP-Max-Retry = 22

> • | PPP-No-Rem-IP-Address = 23

> • | Inactivity-Timeout = 24

> • | Session-Timeout = 25

> • | Max-Data-Excd = 26

> • | Invalid-IP-Source-Address = 27

> • | MSID-Auth-Failed = 28

> • | MSID-Auth-Failed-No-AAA-Resp = 29

> • | A11-Max-Retry = 30

> • | A11-Lifetime-Expired = 31

> • | A11-Message-Integrity-Failure = 32

> • | PPP-lcp-remote-disc = 33

> • | Session-setup-timeout = 34

> • | PPP-keepalive-failure = 35

> • | Flow-add-failed = 36

> • | Call-type-detection-failed = 37

> • | Wrong-ipcp-params = 38

> • | MIP-remote-dereg = 39

> • | MIP-lifetime-expiry = 40

> • | MIP-proto-error = 41

> • | MIP-auth-failure = 42

> • | MIP-reg-timeout = 43

> • | Invalid-dest-context = 44

> • | Source-context-removed = 45

> • | Destination-context-removed = 46

> • | Req-service-addr-unavailable = 47

> • | Demux-mgr-failed = 48

> • | Internal-error = 49

> • | AAA-context-removed = 50

> • | invalid-service-type = 51

> • | mip-relay-req-failed = 52

> • | mip-rcvd-relay-failure = 53

> • | ppp-restart-inter-pdsn-handoff = 54

> • | gre-key-mismatch = 55

> • | invalid_tunnel_context = 56

> • | no_peer_lns_address = 57

> • | failed_tunnel_connect = 58

> • | l2tp-tunnel-disconnect-remote = 59

> • | l2tp-tunnel-timeout = 60

> • | l2tp-protocol-error-remote = 61

> • | l2tp-protocol-error-local = 62

> • | l2tp-auth-failed-remote = 63

> • | l2tp-auth-failed-local = 64

> • | l2tp-try-another-lns-from-remote = 65

> • | l2tp-no-resource-local = 66

> • | l2tp-no-resource-remote = 67

> • | l2tp-tunnel-disconnect-local = 68

> • | l2tp-admin-disconnect_remote = 69

> • | l2tpmgr-reached-max-capacity = 70

> • | MIP-reg-revocation = 71

> • | path-failure = 72

> • | dhcp-relay-ip-validation-failed = 73

> • | gtp-unknown-pdp-addr-or-pdp-type = 74

> • | gtp-all-dynamic-pdp-addr-occupied = 75

> • | gtp-no-memory-is-available = 76

> • | dhcp-relay-static-ip-addr-not-allowed = 77

> • | dhcp-no-ip-addr-allocated = 78

> • | dhcp-ip-addr-allocation-tmr-exp = 79

> • | dhcp-ip-validation-failed = 80

> • | dhcp-static-addr-not-allowed = 81

> • | dhcp-ip-addr-not-available-at-present = 82

> • | dhcp-lease-expired = 83

> • | lpool-ip-validation-failed = 84

> • | lpool-static-ip-addr-not-allowed = 85

> • | static-ip-validation-failed = 86

> • | static-ip-addr-not-present = 87

> • | static-ip-addr-not-allowed = 88

> • | radius-ip-validation-failed = 89

> • | radius-ip-addr-not-provided = 90

> • | invalid-ip-addr-from-sgsn = 91

> • | no-more-sessions-in-aaa = 92

> • | ggsn-aaa-auth-req-failed = 93

> • | conflict-in-ip-addr-assignment = 94

> • | apn-removed = 95

> • | credits-used-bytes-in = 96

> • | credits-used-bytes-out = 97

> • | credits-used-bytes-total = 98

> • | prepaid-failed = 99

> • | l2tp-ipsec-tunnel-failure = 100

> • | l2tp-ipsec-tunnel-disconnected = 101

> • | mip-ipsec-sa-inactive = 102

> • | Long-Duration-Timeout = 103

> • | proxy-mip-registration-failure = 104

> • | proxy-mip-binding-update = 105

> • | proxy-mip-inter-pdsn-handoff-require-ip-address = 106

> • | proxy-mip-inter-pdsn-handoff-mismatched-address = 107

> • | Local-purge = 108

> • | failed-update-handoff = 109

> • | closed_rp-handoff-complete = 110

> • | closed_rp-duplicate-session = 111

> • | closed_rp-handoff-session-not-found = 112

> • | closed_rp-handoff-failed = 113

> • | pcf-monitor-keep-alive-failed = 114

> • | call-internal-reject = 115

> • | call-restarted = 116

> • | a11-mn-ha-auth-failure = 117

> • | a11-badly-formed = 118

> • | a11-t-bit-not-set = 119

> • | a11-unsupported-vendor-id = 120

> • | a11-mismatched-id = 121

> • | mipha-dup-home-addr-req = 122

> • | mipha-dup-imsi-session = 123

> • | ha-unreachable = 124

> • | IPSP-addr-in-use = 125

> • | mipfa-dup-home-addr-req = 126

> • | mipha-ip-pool-busyout = 127

> • | inter-pdsn-handoff = 128

> • | active-to-dormant = 129

> • | ppp-renegotiation = 130

> • | active-start-param-change = 131

> • | tarrif-boundary = 132

> • | a11-disconnect-no-active-stop = 133

> • | nw-reachability-failed-reject = 134

> • | nw-reachability-failed-redirect = 135

> • | container-max-exceeded = 136

> • | static-addr-not-allowed-in-apn = 137

> • | static-addr-required-by-radius = 138

> • | static-addr-not-allowed-by-radius = 139

> • | mip-registration-dropped = 140

> • | counter-rollover = 141

> • | constructed-nai-auth-fail = 142

> • | inter-pdsn-service-optimize-handoff-disabled = 143

> • | gre-key-collision = 144

> • | inter-pdsn-service-optimize-handoff-triggered = 145

> • | intra-pdsn-handoff-triggered = 146

> • | delayed-abort-timer-expired = 147

> • | Admin-AAA-disconnect = 148

> • | Admin-AAA-disconnect-handoff = 149

> • | PPP-IPV6CP-Neg-Failed = 150

> • | PPP-IPV6CP-No-Response = 151

> • | PPP-IPV6CP-Max-Retry = 152

> • | PPP-Restart-Invalid-source-IPV4-address = 153

> • | a11-disconnect-handoff-no-active-stop = 154

> • | call-restarted-inter-pdsn-handoff = 155

> • | call-restarted-ppp-termination = 156

> • | mipfa-resource-conflict = 157

> • | failed-auth-with-charging-svc = 158

> • | mipha-dup-imsi-session-purge = 159

> • | mipha-rev-pending-newcall = 160

> • | volume-quota-reached = 161

> • | duration-quota-reached = 162

> • | gtp-user-authentication-failed = 163

> • | MIP-reg-revocation-no-lcp-term = 164

> • | MIP-private-ip-no-rev-tunnel = 165

> • | Invalid-Prepaid-AAA-attr-in-auth-response = 166

> • | mipha-prepaid-reset-dynamic-newcall = 167

> • | gre-flow-control-timeout = 168

> • | mip-paaa-bc-query-not-found = 169

> • | mipha-dynamic-ip-addr-not-available = 170

> • | a11-mismatched-id-on-handoff = 171

> • | a11-badly-formed-on-handoff = 172

> • | a11-unsupported-vendor-id-on-handoff = 173

> • | a11-t-bit-not-set-on-handoff = 174

> • | MIP-reg-revocation-i-bit-on = 175

> • | A11-RRQ-Deny-Max-Count = 176

> • | Dormant-Transition-During-Session-Setup = 177

> • | PPP-Rem-Reneg-Disc-Always-Cfg = 178

> • | PPP-Rem-Reneg-Disc-NAI-MSID-Mismatch = 179

> • | mipha-subscriber-ipsec-tunnel-down = 180

> • | mipha-subscriber-ipsec-tunnel-failed = 181

> • | mipha-subscriber-ipsecmgr-death = 182

> • | flow-is-deactivated = 183

> • | ecsv2-license-exceeded = 184

> • | IPSG-Auth-Failed = 185

> • | driver-initiated = 186

> • | ims-authorization-failed = 187

> • | service-instance-released = 188

> • | flow-released = 189

> • | ppp-renego-no-ha-addr = 190

> • | intra-pdsn-handoff = 191

> • | overload-disconnect = 192

> • | css-service-not-found = 193

> • | Auth-Failed = 194

> • | dhcp-client-sent-release = 195

> • | dhcp-client-sent-nak = 196

> • | msid-dhcp-chaddr-mismatch = 197

> • | link-broken = 198

> • | prog-end-timeout = 199

> • | qos-update-wait-timeout = 200

> • | css-synch-cause = 201

> • | Gtp-context-replacement = 202

> • | PDIF-Auth-failed = 203

> • | l2tp-unknown-apn = 204

> • | ms-unexpected-network-reentry = 205

> • | r6-invalid-nai = 206

> • | eap-max-retry-reached = 207

> • | vbm-hoa-session-disconnected = 208

> • | vbm-voa-session-disconnected = 209

> • | in-acl-disconnect-on-violation = 210

> • | eap-msk-lifetime-expiry = 211

> • | eap-msk-lifetime-too-low = 212

> • | mipfa-inter-tech-handoff = 213

> • | r6-max-retry-reached = 214

> • | r6-nwexit-recd = 215

> • | r6-dereg-req-recd = 216

> • | r6-remote-failure = 217

> • | r6r4-protocol-errors = 218

> • | wimax-qos-invalid-aaa-attr = 219

> • | npu-gre-flows-not-available = 220

> • | r4-max-retry-reached = 221

> • | r4-nwexit-recd = 222

> • | r4-dereg-req-recd = 223

> • | r4-remote-failure = 224

> • | ims-authorization-revoked = 225

> • | ims-authorization-released = 226

> • | ims-auth-decision-invalid = 227

> • | mac-addr-validation-failed = 228

> • | excessive-wimax-pd-flows-cfgd = 229

> • | sgsn-canc-loc-sub = 230

> • | sgsn-canc-loc-upd = 231

> • | sgsn-mnr-exp = 232

> • | sgsn-ident-fail = 233

> • | sgsn-sec-fail = 234

> • | sgsn-auth-fail = 235

> • | sgsn-glu-fail = 236

> • | sgsn-imp-det = 237

> • | sgsn-smgr-purge = 238

> • | sgsn-subs-handed-to-peer = 239

> • | sgsn-dns-fail-inter-rau = 240

> • | sgsn-cont-rsp-fail = 241

> • | sgsn-hlr-not-found-for-imsi = 242

> • | sgsn-ms-init-det = 243

> • | sgsn-opr-policy-fail = 244

> • | sgsn-duplicate-context = 245

> • | hss-profile-update-failed = 246

> • | sgsn-no-pdp-activated = 247

> • | asnpc-idle-mode-timeout = 248

> • | asnpc-idle-mode-exit = 249

> • | asnpc-idle-mode-auth-failed = 250

> • | asngw-invalid-qos-configuration = 251

> • | sgsn-dsd-allgprswithdrawn = 252

> • | r6-pmk-key-change-failure = 253

> • | sgsn-illegal-me = 254

> • | sess-termination-timeout = 255

> • | sgsn-sai-fail = 256

> • | sgsn-rnc-removal = 257

> • | sgsn-rai-removal = 258

> • | sgsn-init-deact = 259

> • | ggsn-init-deact = 260

> • | hlr-init-deact = 261

> • | ms-init-deact = 262

> • | sgsn-detach-init-deact = 263

> • | sgsn-rab-rel-init-deact = 264

> • | sgsn-iu-rel-init-deact = 265

> • | sgsn-gtpu-path-failure = 266

> • | sgsn-gtpc-path-failure = 267

> • | sgsn-local-handoff-init-deact = 268

> • | sgsn-remote-handoff-init-deact = 269

> • | sgsn-gtp-no-resource = 270

> • | sgsn-rnc-no-resource = 271

> • | sgsn-odb-init-deact = 272

> • | sgsn-invalid-ti = 273

> • | sgsn-ggsn-ctxt-non-existent = 274

> • | sgsn-apn-restrict-vio = 275

> • | sgsn-regular-deact = 276

> • | sgsn-abnormal-deact = 277

> • | sgsn-actv-rejected-by-peer = 278

> • | sgsn-err-ind = 279

> • | asngw-non-anchor-prohibited = 280

> • | asngw-im-entry-prohibited = 281

> • | session-idle-mode-entry-timeout = 282

> • | session-idle-mode-exit-timeout = 283

> • | asnpc-ms-power-down-nwexit = 284

> • | asnpc-r4-nwexit-recd = 285

> • | sgsn-iu-rel-before-call-est = 286

> • | ikev2-subscriber-ipsecmgr-death = 287

> • | All-dynamic-pool-addr-occupied = 288

> • | mip6ha-ip-addr-not-available = 289

> • | bs-monitor-keep-alive-failed = 290

> • | sgsn-att-in-reg-state = 291

> • | sgsn-inbound-srns-in-reg-state = 292

> • | dt-ggsn-tun-reestablish-failed = 293

> • | sgsn-unknown-pdp = 294

> • | sgsn-pdp-auth-failure = 295

> • | sgsn-duplicate-pdp-context = 296

> • | sgsn-no-rsp-from-ggsn = 297

> • | sgsn-failure-rsp-from-ggsn = 298

> • | sgsn-apn-unknown = 299

> • | sgsn-serv-req-init-deact = 300

> • | sgsn-attach-on-attch-init-abort = 301

> • | sgsn-iu-rel-in-israu-init-abort = 302

> • | sgsn-smgr-init-abort = 303

> • | sgsn-mm-ctx-cleanup-init-abort = 304

> • | sgsn-unknown-abort = 305

> • | sgsn-guard-timeout-abort = 306

> • | vpn-bounce-dhcpip-validate-req = 307

> • | mipv6-id-mismatch = 308

> • | aaa-session-id-not-found = 309

> • | x1-max-retry-reached = 310

> • | x1-nwexit-recd = 311

> • | x1-dereg-req-recd = 312

> • | x1-remote-failure = 313

> • | x1x2-protocol-errors = 314

> • | x2-max-retry-reached = 315

> • | x2-nwexit-recd = 316

> • | x2-dereg-req-recd = 317

> • | x2-remote-failure = 318

> • | x1-pmk-key-change-failure = 319

> • | sa-rekeying-failure = 320

> • | sess-sleep-mode-entry-timeout = 321

> • | phsgw-non-anchor-prohibited = 322

> • | asnpc-pc-relocation-failed = 323

> • | asnpc-pc-relocation = 324

> • | auth_policy_mismatch = 325

> • | sa-lifetime-expiry = 326

> • | asnpc-del-ms-entry-recd = 327

> • | phspc-sleep-mode-timeout = 328

> • | phspc-sleep-mode-exit = 329

> • | phspc-sleep-mode-auth-failed = 330

> • | phspc-ms-power-down-nwexit = 331

> • | phspc-x2-nwexit-recd = 332

> • | invalid-nat-config = 333

> • | asngw-tid-entry-not-found = 334

> • | No-NAT-IP-Address = 335

> • | excessive-phs-pd-flows-cfgd = 336

> • | phsgw-invalid-qos-configuration = 337

> • | Interim-Update = 338

> • | sgsn-attach-abrt-rad-lost = 339

> • | sgsn-inbnd-irau-abrt-rad-lost = 340

> • | ike-keepalive-failed = 341

> • | sgsn-attach-abrt-ms-suspend = 342

> • | sgsn-inbnd-irau-abrt-ms-suspend = 343

> • | duplicate-session-detected = 344

> • | sgsn-xid-response-failure = 345

> • | sgsn-nse-cleanup = 346

> • | sgsn-gtp-req-failure = 347

> • | sgsn-imsi-mismatch = 348

> • | sgsn-bvc-blocked = 349

> • | sgsn-attach-on-inbound-irau = 350

> • | sgsn-attach-on-outbound-irau = 351

> • | sgsn-incorrect-state = 352

> • | sgsn-t3350-expiry = 353

> • | sgsn-page-timer-expiry = 354

> • | phsgw-tid-entry-not-found = 355

> • | phspc-del-ms-entry-recd = 356

> • | sgsn-pdp-local-purge = 357

> • | phs-invalid-nai = 358

> • | session-sleep-mode-exit-timeout = 359

> • | sgsn-offload-phase2 = 360

> • | phs-thirdparty-auth-fail = 361

> • | remote-error-notify = 362

> • | no-response = 363

> • | PDG-Auth-failed = 364

> • | mme-s1AP-send-failed=365

> • | mme-egtpc-connection-failed=366

> • | mme-egtpc-create-session-failed=367

> • | mme-authentication-failure=368

> • | mme-ue-detach=369

> • | mme-mme-detach=370

> • | mme-hss-detach=371

> • | mme-pgw-detach=372

> • | mme-sub-validation-failure=373

> • | mme-hss-connection-failure=374

> • | mme-hss-user-unknown=375

> • | dhcp-lease-mismatch-detected=376

> • | nemo-link-layer-down=377

> • | eapol-max-retry-reached = 378

> • | sgsn-offload-phase3 = 379

> • | mbms-bearer-service-disconnect = 380

> • | disconnect-on-violation-odb = 381

> • | disconn-on-violation-focs-odb = 382

> • | CSCF-REG-Admin-disconnect = 383

> • | CSCF-REG-User-disconnect = 384

> • | CSCF-REG-Inactivity-timeout = 385

> • | CSCF-REG-Network-disconnect = 386

> • | CSCF-Call-Admin-disconnect = 387

> • | CSCF-CAll-User-disconnect = 388

> • | CSCF-CALL-Local-disconnect = 389

> • | CSCF-CALL-No-Resource = 390

> • | CSCF-CALL-No-Respone = 391

> • | CSCF-CALL-Inactivity-timeout = 392

> • | CSCF-CALL-Media-Auth-Failure = 393

> • | CSCF-REG-No-Resource = 394

> • | ms-unexpected-idle-mode-entry = 395

> • | re-auth-failed = 396

> • | sgsn-pdp-nse-cleanup = 397

> • | sgsn-mm-ctxt-gtp-no-resource = 398

> • | unknown-apn = 399

> • | gtpc-path-failure = 400

> • | gtpu-path-failure = 401

> • | actv-rejected-by-sgsn = 402

> • | sgsn-pdp-gprs-camel-release = 403

> • | sgsn-check-imei-failure = 404

> • | sgsn-sndcp-init-deact = 405

> • | sgsn-pdp-inactivity-timeout = 406

> • | fw-and-nat-policy-removed = 407

> • | FNG-Auth-failed = 408

> • | ha-stale-key-disconnect = 409

> • | No-IPV6-address-for-subscriber = 410

> • | prefix-registration-failure = 411

> • | disconnect-from-policy-server = 412

> • | s6b-auth-failed = 413

> • | gtpc-err-ind = 414

> • | gtpu-err-ind = 415

> • | invalid-pdn-type = 416

> • | aaa-auth-req-failed = 417

> • | apn-denied-no-subscription = 418

> • | Sgw-context-replacement = 419

> • | dup-static-ip-addr-req = 420

> • | apn-restrict-violation = 421

> • | invalid-wapn = 422

> • | ttg-nsapi-allocation-failed = 423

> • | mandatory-gtp-ie-missing = 424

> • | aaa-unreachable = 425

> SN1-DNS-Proxy-Intercept-List
> DNS proxy list.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 214
> Length
> 1–253
> Value
> String
> SN1-DNS-Proxy-Use-Subscr-Addr
> This attribute is used to convey whether to use the subscriber's address as the source address for DNS Proxy.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 25
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN1-Dynamic-Addr-Alloc-Ind-Flag
> This attribute indicates that the PDP address has been dramatically allocated for that particular PDP context. This field is missing if the address is static (e.g., part of the PDP context subscription). Dynamic address allocation might be relevant for charging (e.g., the duration of PDP context as one resource offered and possibly owned by the network operator).
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 141
> Length
> 1
> Value
> Integer.
> Dynamic address allocation = 1
> SN1-Ecs-Data-Volume
> Compound attribute indicating downlink and uplink octet usage for a PDP context per rating group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 176
> Length
> 12
> Value
> Contains the following subattributes:
> Rating-Group-Id
> Rating Group Id in a PDP context.
> Type
> 1
> Length
> 4
> Value
> Unsigned integer
> GPRS-Uplink
> Uplink octet usage for a PDP context per rating group.
> Type
> 2
> Length
> 4
> Value
> Unsigned integer
> GPRS-Downlink
> Downlink octet usage for a PDP context per rating group.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> SN1-Enable-QoS-Renegotiation
> This attribute configures the enabling of dynamic QoS renegotiation.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 144
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-Ext-Inline-Srvr-Context
> This attribute configures the context name in which the External In-line server resides. The value is an ASCII string naming the In-line Server Context.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 41
> Length
> 1–247
> Value
> ASCII string
> SN1-Ext-Inline-Srvr-Down-Addr
> This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 56
> Length
> 4
> Value
> IPv4 address
> SN1-Ext-Inline-Srvr-Down-VLAN
> This attribute configures the IP address of the downstream external in-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 59
> Length
> 4
> Value
> Unsigned integer
> SN1-Ext-Inline-Srvr-Preference
> This attribute configures the preference for the tagged group of External In-line Servers. This attribute is required, although it doesn't actually assign a preference right now. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 57
> Length
> 4
> Value
> Unsigned integer
> SN1-Ext-Inline-Srvr-Up-Addr
> This attribute configures the IP address of the Upstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 55
> Length
> 4
> Value
> IPv4 address
> SN1-Ext-Inline-Srvr-Up-VLAN
> This attribute configures the VLAN tag to be applied to Upstream packets and forwarded to the External In-line server. It can be tagged, in which case it is treated as part of an external in-line server group.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 58
> Length
> 4
> Value
> The VLAN tag to apply.
> SN1-Firewall-Enabled
> Firewall for subscriber enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 198
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> SN1-Firewall-Policy
> This attribute is obsoleted.
> SN1-FMC-Location
> MAC address and CDMA location information.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 171
> Length
> 1–247
> Value
> String
> SN1-GGSN-MIP-Required
> This attribute specifies if MIP is required for the GGSN subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 68
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Gratuitous-ARP-Aggressive
> This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 54
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Gratuitous-ARP-Mode
> This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 54
> Length
> 4
> Value
> An integer in network order. Supported values are:

> • | Disabled = 0 — Do not send Gratuitous ARP

> • | Aggressive = 1 — Send Gratuitous ARP in Aggressive mode

> SN1-GTP-Version
> This attribute indicates the version of GTP the subscriber is using.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 62
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | GTP_VERSION_0 = 0

> • | GTP_VERSION_1 = 1

> SN1-HA-Send-DNS-Address
> This attribute specifies if the HA should send the DNS address in the Mobile IP RRP message. The default is not to send the DSN Address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 47
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not send

> • | Enabled = 1 — Send

> SN1-Home-Behavior
> SN1-Home-Behavior
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 119
> Length
> 4
> Value
> Unsigned integer
> SN1-Home-Profile
> SN1-Home-Profile
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 109
> Length
> 4
> Value
> Unsigned integer
> SN1-Home-Sub-Use-GGSN
> GGSN
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 106
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN1-Ignore-Unknown-HA-Addr-Err
> Value of 1 enables HA to ignore unknown HA address error for incoming RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 160
> Length
> 1
> Value
> Unsigned integer
> SN1-IMSI
> This is the IMSI that identifies the mobile subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 252
> Length
> 1–8
> Value
> ASCII string
> SN1-IMS-AM-Address
> IMS application manager address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 167
> Length
> 4
> Value
> IPv4 address
> SN1-IMS-AM-Domain-Name
> IMS application manager domain name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 168
> Length
> 1 - 64
> Value
> String
> SN1-Internal-SM-Index
> GGSN charging service, internally used.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 122
> Length
> 4
> Value
> Unsigned integer
> SN1-Inactivity-Time
> This attribute contains the inactivity time duration for a subscriber session under long time duration timer configuration.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 275
> Length
> 1
> Value
> 1
> SN1-IP-Alloc-Method
> This attribute specifies the method for allocating an IP address. This feature only applies to the GGSN Service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 53
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Alloc_Local_Pool = 0

> • | Alloc_Dhcp_Client = 1

> • | Alloc_Radius = 2

> • | Alloc_No_Alloc = 3

> • | Alloc_Static_Alloc = 4

> • | Alloc_Dhcp_Relay = 5

> SN1-IP-Filter-In
> This attribute is deprecated. To select an IP access list that is already defined in the destination context, use the IETF standard Filter-Id attribute. The filter ID is used to identify the IP access list by name.
> SN1-IP-Filter-Out
> This attribute is deprecated. To select an IP access list that is already defined in the destination context, use the IETF standard Filter-Id attribute. The filter ID is used to identify the IP access list by name.
> SN1-IP-Header-Compression
> Specifies the IP header compression method to use.
> Type
> Type 26
> Vendor ID
> 8164
> VSA Type
> 150
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | VJ = 1

> • | ROHC = 2

> • | VJ_ROHC = 3

> SN1-IP-Hide-Service-Address
> This attribute prevents the IP address bound to a call service from responding to ping and IMCP error packets.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 60
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-IP-In-ACL
> This attribute contains a definition for one Input IP Access Control List, which is used to filter the IP packets coming from the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 17
> Length
> 1–253
> Value
> ASCII string
> SN1-IP-In-Plcy-Grp
> This attribute specifies the name of the policy group config applied in the uplink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 193
> Length
> 1–16
> Value
> String.
> SN1-IP-Out-ACL
> This attribute contains a definition for one Output IP Access Control List, which is used to filter the IP packets sent to the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 18
> Length
> 1–253
> Value
> ASCII string
> SN1-IP-Out-Plcy-Grp
> This attribute specifies the name of the policy group config applied in the downlink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 194
> Length
> 1–16
> Value
> String.
> SN1-IP-Pool-Name
> This attribute indicates the name of the IP Pool, configured on the chassis, from which an IP address should be chosen for the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 8
> Length
> 1–253
> Value
> ASCII string
> SN1-IP-Source-Validation
> This attribute indicates if the source IP address should be validated before forwarding the IP packet.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 14
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0 — No Validation

> • | Yes = 1 — Validated

> • | VSA1 vendor specific.

> SN1-IP-Source-Violate-No-Acct
> When enabled, This attribute excludes the Source Violated IP packets and byte counts when reporting the Octet and Packet count in an accounting message.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 196
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-IP-Src-Valid-Drop-Limit
> Maximum number of packet drops entertained before disconnecting the session for source violated packets for the session
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 110
> Length
> 1
> Value
> Unsigned integer
> SN1-IPv6-DNS-Proxy
> IPV6 DNS Proxy Enabled or Disabled Setting for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 126
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-IPv6-Egress-Filtering
> This attribute enables egress filtering to make sure that packets being sent to the mobile device have an interface ID that matches that of the mobile device. This feature is meant to protect the Mobile from receiving unwanted packets from the Internet.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 103
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-IPv6-Min-Link-MTU
> SN1-IPv6-Min-Link-MTU
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 136
> Length
> 2
> Value
> Unsigned integer
> SN1-IPv6-num-rtr-advt
> This attribute indicates the IPv6 number of Initial Router Advertisements. Default value is 3
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 97
> Length
> 4
> Value
> Unsigned integer
> SN1-IPv6-Primary-DNS
> This attribute specifies a Primary DNS server address that the Router Advertisement message sent by the PDSN will include.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 101
> Length
> 4
> Value
> IPv6 address
> SN1-IPv6-rtr-advt-interval
> This attribute indicates the IPv6 Initial Router Advertisement Interval specified in milliseconds. The default value is 3000.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 96
> Length
> 4
> Value
> Unsigned integer
> SN1-IPv6-Sec-Pool
> IPv6 Secondary Pool name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 124
> Length
> 1–253
> Value
> String
> SN1-IPv6-Sec-Prefix
> IPv6 Secondary Pool name prefix.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 125
> Length
> 2–18
> Value
> Opaque value
> SN1-IPv6-Secondary-DNS
> This attribute specifies a Secondary DNS server address that the Router Advertisement message sent by the PDSN will include.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 102
> Length
> 4
> Value
> IPv6 address
> SN1-L3-to-L2-Tun-Addr-Policy
> This attribute specifies the address allocation policy.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 43
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | no-local-alloc-validate = 0 — Do not locally allocate, do not validate

> • | local-alloc = 1 — Locally allocate

> • | local-alloc-validate = 2 — Locally allocate and validate

> SN1-Local-IP-Address
> This attribute indicates the IP address of the local interface on the chassis for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 13
> Length
> 4
> Value
> IPv4 address
> SN1-Long-Duration-Action
> This attribute specifies the action to take place when the long duration timeout expires for a subscriber session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 45
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Detection = 1 — Detect the session and alert the administrator

> • | Disconnection = 2 — Disconnect the session

> • | Dormant-Only-Disconnection = 3

> • | Dormant-Only-Detection = 4

> SN1-Long-Duration-Notification
> Long Duration Notification.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 253
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Suppress = 0

> • | Send = 1

> SN1-Long-Duration-Timeout
> This attribute is used to detect and if necessary disconnect sessions connected to the PDSN. This attribute configures the time period before either alerting the administrator or disconnecting the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 44
> Length
> 4
> Value
> An integer in network order which is the number of seconds for the long duration timer.
> SN1-Mediation-Acct-Rsp-Action
> When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the Mediation Accounting server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the Mediation Accounting server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the Mediation Accounting server.
> Type
> Type 26
> Vendor ID
> Vendor-ID 8164
> VSA Type
> 105
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | No_Early_PDUs = 1

> • | Delay_GTP_Response = 2

> SN1-Mediation-Enabled
> Mediation Accounting Enabled or Disabled settings for GGSN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 123
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Mediation-No-Interims
> Mediation no interims.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 146
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Mediation-VPN-Name
> Mediation context name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 104
> Length
> 1–128
> Value
> String
> SN1-Min-Compress-Size
> This attribute indicates the minimum size (in octets) a data packet can have in order to be compressed.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 23
> Length
> 4
> Value
> Unsigned integer
> SN1-MIP-AAA-Assign-Addr
> This attribute specifies if the PDSN/FA will allow AAA to assign the home address. The default is to not allow AAA to assign the home address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 50
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not allow AAA to assign home address

> • | Enabled = 1 — Allow AAA to assign home address

> SN1-MIP-ANCID
> Accounting correlation ID created by IPGW, received by VBM and HBM.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 166
> Length
> 12
> Value
> Opaque value
> SN1-MIP-Dual-Anchor
> Enable/disable dual-anchor service for a subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 165
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-MIP-HA-Assignment-Table
> MIP-HA Assignment Table name. When this is received in an Access Accept message, the system uses this local table to get the HA Address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 154
> Length
> 1–253
> Value
> ASCII string
> SN1-MIP-Match-AAA-Assign-Addr
> This attribute specifies if the PDSN/FA will enforce that a non-zero AAA-specified home address must match the home address present in the MIP RRQ from the mobile node, and disconnect the subscriber session if a match is not present. The default is not to force the addresses to match.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 51
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not force the AAA-specified home address to match RRQ

> • | Enabled = 1 — Force the AAA-specified home address to match RRQ

> SN1-MIP-Reg-Lifetime-Realm
> Configure the maximum MIP registration lifetime for a subscriber/realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 175
> Length
> 2
> Value
> Unsigned integer
> SN1-MIP-Send-Ancid
> AAA attribute to enable/disable sending ANCID from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 163
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-MIP-Send-Correlation-Info
> AAA Attribute to enable/disable sending of correlation-id from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 188
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | Disabled = 0

> • | Enabled = 1

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0

> • | NVSE_Starent = 1

> • | NVSE_CUstom1 = 2

> • | NVSE_Custom2 = 3

> SN1-MIP-Send-Imsi
> Attribute to enable/disable sending IMSI from FA to HA in MIP RRQ.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 164
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | None = 0

> • | Starent_NVSE = 1

> • | Custom1_NVSE = 2

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0,

> • | NVSE_Starent = 1,

> • | NVSE_Custom1 = 2,

> • | NVSE_Custom2 = 3

> SN1-MIP-Send-Term-Verification
> This attribute specifies whether the PDSN/FA should send the Terminal Verification Normal Vendor/Organization Specific Extension (NVSE) in the Mobile IP RRQ message to the HA. The default is not to send the Terminal Verification NVSE.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 48
> Length
> 4
> Value
> Enumerated integer.

> • | In StarOS 8.1 and earlier, supported values are:

> • | Disabled = 0 — Do not send

> • | Enabled = 1 — Send

> • | In StarOS 8.3 and later, supported values are:

> • | Disabled = 0

> • | NVSE_Custom1 = 1 — Send custom NVSE

> • | NVSE_Custom2 = 2 — Send custom NVSE

> • | NVSE_Starent = 3 — Send custom NVSE

> SN1-MN-HA-Hash-Algorithm
> This attribute contains the hash algorithm to use for MN-HA authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 28
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | MD5 = 1

> • | MD5-RFC2002 = 2

> • | HMAC-MD5 = 3

> SN1-MN-HA-Timestamp-Tolerance
> This attribute indicates the duration of timestamp tolerance, in seconds, to use for MN-HA authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 30
> Length
> 4
> Value
> Unsigned integer
> SN1-MS-ISDN
> SN1-MS-ISDN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 248
> Length
> 1–9
> Value
> Opaque value
> SN1-MSK-Lifetime
> This attribute is currently not supported.
> SN1-NAI-Construction-Domain
> This attribute specifies the domain name to use when constructing the NAI.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 37
> Length
> 1–247
> Value
> An ASCII string specifying the domain to use when constructed NAI is used.
> SN1-NAT-Bind-Record
> Contains the NAT Binding Record.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 216
> Length
> Compound
> Value
> Contains the following subattributes:
> NAT-IP-Address
> NAT IP Address.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> NAT-Port-Block-Start
> Start port of the port chunk.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> NAT-Port-Block-End
> End port of the port chunk.
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> Alloc-Flag
> Port chunk status. Accepted Values are 0(De-Allocated) and 1(Allocated).
> Type
> 4
> Length
> 1
> Value
> Unsigned integer
> Correlation-Id
> Correlation ID.
> Type
> 5
> Length
> 1–253
> Value
> String
> Loading-Factor
> Indicates maximum number of users per NAT IP address.
> Type
> 6
> Length
> 2
> Value
> Unsigned integer
> Binding-Timer
> Port chunk hold timer.
> Type
> 7
> Length
> 4
> Value
> Unsigned integer
> SN1-NAT-Info-Record
> NAT-Record-Info.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 246
> Length
> Compound
> Value
> Contains the following subattributes:
> Framed-IP-Address
> Framed IP address.
> Type
> 1
> Length
> 4
> Value
> IPv4 address
> NAT-IP-Address
> NAT IP address.
> Type
> 2
> Length
> 4
> Value
> IPv4 address
> NAT-Port-Block-Start
> Start port of the port chunk
> Type
> 3
> Length
> 2
> Value
> Unsigned integer
> NAT-Port-Block-End
> End port of the port chunk.
> Type
> 4
> Length
> 2
> Value
> Unsigned integer
> Acct-Session-Id
> Accounting Session ID.
> Type
> 5
> Length
> 1–17
> Value
> String
> User-Name
> User name.
> Type
> 6
> Length
> 1–128
> Value
> String
> Correlation-Id
> Correlation ID.
> Type
> 7
> Length
> 1–17
> Value
> String
> SN1-NAT-IP-Address
> This attribute includes the NAT (public) IP address used for the call.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 217
> Length
> 4
> Value
> IPv4 address
> SN1-NAT-IP-Address-Old
> Public IP address used for the call
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 0
> Length
> 4
> Value
> IPv4 address
> SN1-NPU-Qos-Priority
> This attribute configures Inter-Subscriber priority Queueing based on class of service offered. Gold has highest priority and Best_effort lowest priority. From DSCP, means the priority queueing will be done based on the DSCP marking the incoming subscriber packet carries.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 98
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best_Effort = 0

> • | Bronze = 1

> • | Silver = 2

> • | Gold = 3

> • | From_DSCP = 4

> SN1-Ntk-Initiated-Ctx-Ind-Flag
> This attribute indicates that the PDP context is network initiated. The attribute is missing for a mobile activated PDP context.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 142
> Length
> 1
> Value
> Opaque value
> SN1-Ntk-Session-Disconnect-Flag
> SN1-Ntk-Session-Disconnect-Flag.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 143
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Session-Disconnect = 1

> SN1-Ntk-Session-Disconnect-Reason
> SN1-Ntk-Session-Disconnect-Reason.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 143
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Session-Disconnect = 1

> SN1-Nw-Reachability-Server-Name
> This attribute specifies the name of a network reachability server (defined in the destination context of the subscriber) that must respond as reachable, or the user is be redirected.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 65
> Length
> 1–247
> Value
> An ASCII string representing the name of the Network Reachability Detection Server.
> SN1-Overload-Disconnect
> Enables/disables the overload-disconnect feature (if 1) and disables if 0
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 235
> Length
> 4
> Value
> Unsigned Integer
> SN1-Overload-Disc-Connect-Time
> Provides the connect time for a session. When this time expires, the session may become a candidate for disconnection.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 233
> Length
> 1
> Value
> Integer
> SN1-Overload-Disc-Inact-Time
> Provides inactivity time for a session after which it may become candidate for disconnection.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 234
> Length
> 1
> Value
> Integer
> SN1-PDIF-MIP-Release-TIA
> PDIF mobile IP release TIA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 172
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-PDIF-MIP-Required
> PDIF mobile IP required.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 170
> Length
> 4
> Value
> Enumerated Integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-PDIF-MIP-Simple-IP-Fallback
> PDIF mobile IP simple IP fallback.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 173
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-PDSN-Correlation-Id
> Correlation ID received from PDSN to HA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 189
> Length
> 8
> Value
> Opaque value
> SN1-PDSN-Handoff-Req-IP-Addr
> This attribute specifies if the PDSN should reject and terminate the subscriber session when the proposed address in IPCP by the mobile does not match the existing address in the PDSN. The default (Disabled) is not to reject these sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 46
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not reject

> • | Enabled = 1 — Reject

> SN1-PDSN-NAS-Id
> NAS Identifier received from PDSN to HA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 190
> Length
> 1–253
> Value
> String
> SN1-PDSN-NAS-IP-Address
> NAS IP address received from PDSN to HA.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 191
> Length
> 4
> Value
> IPv4 address
> SN1-Permit-User-Mcast-PDUs
> Specifies whether or not to let the subscriber discard multicast PDUs.
> Type
> 26
> Vendor ID
> 8164
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-PPP-Accept-Peer-v6Ifid
> This attribute indicates the acceptance of the interface ID provided by peer during PPP IPv6CP if the ID is valid. The default is disabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 95
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not accept interface ID

> • | Enabled = 1 — Accept interface ID

> SN1-PPP-Always-On-Vse
> SN1-PPP-Always-On-Vse.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 130
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-PPP-Data-Compression
> This attribute indicates the PPP data compression algorithm to use for the PPP session. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 9
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Stac-LZS = 1

> • | MPPC = 2

> • | Deflate = 4

> SN1-PPP-Data-Compression-Mode
> This attribute indicates the PPP data compression mode to use for the PPP session when PPP data compression is used.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 19
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Stateless = 1

> SN1-PPP-Keepalive
> This attribute indicates the interval for the PPP keepalive, in seconds.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 16
> Length
> 4
> Value
> Unsigned integer
> SN1-PPP-NW-Layer-IPv4
> This attribute indicates the PPP IPCP negotiation for IPv4. The default is enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 92
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — IPCP negotiation for IPv4 is disabled.

> • | Enabled = 1 — IPCP negotiation for IPv4 is enabled.

> • | Passive = 2 — Start the negotiation only if peer initiates it.

> SN1-PPP-NW-Layer-IPv6
> This attribute indicates the PPP IPv6CP negotiation for IPv6. The default is enabled.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 93
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — IPCP negotiation for IPv6 is disabled.

> • | Enabled = 1 — IPCP negotiation for IPv6 is enabled.

> • | Passive = 2 — Start the negotiation only if peer initiates it.

> SN1-PPP-Outbound-Password
> This attribute indicates the password to be used when the user side of the PPP connection requires authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 15
> Length
> 1–253
> Value
> ASCII string
> SN1-PPP-Outbound-Username
> This attribute indicates the username to be used when the user side of the PPP connection requires authentication.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 61
> Length
> 1–253
> Value
> ASCII string
> SN1-PPP-Progress-Code
> This attribute provides information about the “state” of the PPP connection, when the connection was terminated.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 4
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Not-Defined = 0

> • | Call-Lcp-Down = 10

> • | Call-Disconnecting = 20

> • | Call-Ppp-Renegotiating = 30

> • | Call-Arrived = 40

> • | Call-Pdg-Tcp-Connecting = 45

> • | Call-Pdg-Ssl-Connecting = 46

> • | Call-Lcp-Up = 50

> • | Call-Authenticating = 60

> • | Call-Bcmcs-Authenticating = 70

> • | Call-Authenticated = 80

> • | Call-Tunnel-Connecting = 85

> • | Call-Ipcp-Up = 90

> • | Call-Imsa-Authorizing = 95

> • | Call-Imsa-Authorized = 97

> • | Call-MBMS-UE-Authorizing = 98

> • | Call-MBMS-Bearer-Authorizing = 99

> • | Call-Simple-IP-Connected = 100

> • | Call-Mobile-IP-Connected = 110

> • | Call-Tunnel-Connected = 115

> • | Call-Pdp-Type-IP-Connected = 120

> • | Call-Pdp-Type-IPv6-Connected = 125

> • | Call-Pdp-Type-PPP-Connected = 130

> • | Call-Proxy-Mobile-IP-Connected = 140

> • | Call-Pdg-Connected = 142

> • | Call-Pdg-Ssl-Connected = 141

> • | Call-Pdg-Connected = 142

> • | Call-Pdg-Connected = 142

> • | Call-Ipsg-Connected = 145

> • | Call-Bcmcs-Connected = 150

> • | Call-MBMS-UE-Connected = 155

> • | Call-MBMS-Bearer-Connected = 156

> • | Call-Pending-Addr-From-DHCP = 160

> • | Call-Got-Addr-From-DHCP = 170

> • | Call-HA-IPSEC-Tunnel-Connecting = 180

> • | Call-HA-IPSEC-Connected = 190

> • | Call-ASN-Non-Anchor-Connected = 200

> • | Call-ASNPC-Connected = 210

> • | Call-Mobile-IPv6-Connected = 220

> • | Call-PMIPv6-Connected = 221

> • | Call-PHSPC-Connected = 230

> • | Call-GTP-IPv4-Connected = 235

> • | Call-GTP-IPv6-Connected = 236

> • | Call-GTP-IPv4-IPv6-Connected = 237

> • | Call-SGW-Connected = 245

> • | Call-MME-Attached = 246

> • | Call-Auth-Only-Connected = 247

> SN1-PPP-Reneg-Disc
> PPP remote reneg disconnect policy.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 187
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Disc_no = 0

> • | Always = 1

> • | NAI_Prefix_MSID_Mismatch = 2

> SN1-Prepaid
> Prepaid.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 128
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | no_prepaid = 0

> • | custom_prepaid = 1

> • | standard_prepaid = 2

> • | wimax_prepaid = 4

> SN1-Prepaid-Compressed-Count
> This attribute indicates if a Pre-paid subscriber's byte usage should be counted on the basis of compressed or uncompressed byte data over the subscriber's PPP connection to the system. If not present, the default is to count uncompressed byte data.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 31
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Uncompressed = 0

> • | Compressed = 1

> SN1-Prepaid-Final-Duration-Alg
> For prepaid, final duration is calculated based on the algorithm specified by the value of this attribute.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 135
> Length
> 2
> Value
> Enumerated integer. Supported values are:

> • | current_time = 0

> • | last-user-layer3-activity-time = 1

> • | last-airlink-activity-time = 2

> • | last-airlink-activity-time-last-reported = 3

> SN1-Prepaid-Inbound-Octets
> In an Access-Accept, this indicates how many additional inbound (bytes delivered to the subscriber) byte credits should be granted to the subscriber. In an Accounting- Request, this indicates how many total inbound byte credits have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on an inbound octet basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 32
> Length
> 4
> Value
> Unsigned integer
> SN1-Prepaid-Outbound-Octets
> SN1-Prepaid-Outbound-Octets.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 33
> Length
> 4
> Value
> Unsigned integer
> SN1-Prepaid-Preference
> This attribute specifies whether prepaid is volume based or duration based.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 129
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | prepaid_duration = 0

> • | prepaid_volume = 1

> SN1-Prepaid-Profile
> Do not do prepaid, regardless of the Rulebase configuration.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 155
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Use-Rulebase-Config = 0

> • | Prohibit = 1

> SN1-Prepaid-Total-Octets
> In an Access-Accept, this attribute indicates how many additional byte credits (combining both inbound and outbound counts) should be granted to the subscriber. In an Accounting- Request, this indicates how many total bytes credits (combined inbound and outbound) have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on a combined inbound and outbound octet-count basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 34
> Length
> 4
> Value
> Unsigned integer
> SN1-Prepaid-Timeout
> This attribute indicates how much time may elapse before a new request for more pre-paid credits is issued. If the specified time has elapsed since the prior grant of credits was received from the RADIUS server, then a new request for credits is issued. This attribute is primarily used to periodically update the subscriber of new credits issued since the subscriber was connected. Note that credit requests will still be made on behalf of the subscriber when the subscriber drops down to the low watermark of credits (or zero if there is no low watermark). The presence or absence of this attribute does not affect that mechanism in any way. However, this timer is re-set whenever any grant of credits is received on behalf of the subscriber, regardless of why the grant of credits was requested.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 35
> Length
> 4
> Value
> Unsigned integer
> SN1-Prepaid-Watermark
> This attribute Indicates the percentage of remaining granted credits that will trigger a new request to grant credits from the RADIUS server. For example, if 1GB of credits was granted to a user, and the value of SN-Prepaid-Watermark was 10, then when 100 MB of credits are remaining (900 MB have been used) to the subscriber, a new request for any new byte credits is issued on behalf of the subscriber. Note that when calculating the pre-paid low watermark, the total credits granted for the subscriber's entire session is used.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 36
> Length
> 4
> Value
> Unsigned integer
> SN1-Primary-DCCA-Peer
> This attribute indicates the name of the primary DCCA peer and primary DCCA realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 223
> Length
> 1
> Value
> A colon separated string, like “primary_peer : primary_realm”
> SN1-Primary-DNS-Server
> This attribute indicates the IP address of the primary DNS server that should be used for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 5
> Length
> 4
> Value
> IPv4 address
> SN1-Primary-NBNS-Server
> Primary NBNS Server IP address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 148
> Length
> 4
> Value
> IPv4 address
> SN1-Proxy-MIP
> This attribute specifies if the PDSN/FA will perform compulsory Proxy-MIP tunneling for a Simple-IP PDSN subscriber. This feature is licensed. The default is not to perform compulsory Proxy-MIP.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 52
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0 — Do not perform compulsory Proxy-MIP

> • | Enabled = 1 — Perform compulsory Proxy-MIP

> SN1-QoS-Background-Class
> This attribute defines the QOS Background Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 91
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Class-Background-PHB
> SN1-QoS-Class-Background-PHB
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 113
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Class-Converstional-PHB
> SN1-QoS-Class-Converstional-PHB.
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 111
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Class-Interactive-1-PHB
> SN1-QoS-Class-Interactive-1-PHB
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 114
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Class-Interactive-2-PHB
> SN1-QoS-Class-Interactive-2-PHB
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 115
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Class-Interactive-3-PHB
> SN1-QoS-Class-Interactive-3-PHB
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 116
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Class-Streaming-PHB
> SN1-QoS-Class-Streaming-PHB
> Type
> 26
> Vendor ID
> 10415
> VSA Type
> 112
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 0

> • | Pass-Through = 1

> • | AF11 = 10

> • | AF12 = 12

> • | AF13 = 14

> • | AF21 = 18

> • | AF22 = 20

> • | AF23 = 22

> • | AF31 = 26

> • | AF32 = 28

> • | AF33 = 30

> • | AF41 = 34

> • | AF42 = 36

> • | AF43 = 38

> • | EF = 46

> SN1-QoS-Conversation-Class
> This attribute defines the QOS Conversation Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 86
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Interactive1-Class
> This attribute defines the QOS Interactive Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 88
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Interactive2-Class
> This attribute defines the QOS Interactive2 Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 89
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Interactive3-Class
> This attribute defines the QOS Interactive3 Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 90
> Length
> 28 bytes
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Negotiated
> Negotiated QoS for GGSN sessions.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 147
> Length
> 4-17
> Value
> String
> SN1-QoS-Renegotiation-Timeout
> This attribute configures the timeout duration of dampening time for dynamic QoS renegotiation.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 145
> Length
> 1
> Value
> 1
> SN1-QoS-Streaming-Class
> This attribute defines the QOS Streaming Traffic Class.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 87
> Length
> 28 byte
> Value
> Opaque value encoded in the following format:

> • | Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable

> • | Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable

> • | Byte 16 Bits 3,4 - Uplink Exceed Action

> • | Byte 16 Bits 5,6 - Downlink Exceed Action

> • | Byte 16 Bits 7,8 - Uplink Violate Action

> • | Byte 15 Bits 1,2 - Downlink Violate Action

> • | Byte 15 Bit 3 - Downlink Ext Peak Data Rate

> • | Byte 15 Bit 4 - Downlink Ext Committed Data Rate

> • | Byte 14 - Uplink Peak Data Rate

> • | Byte 13 - Downlink Peak Data Rate

> • | Byte 12 - Uplink Committed Data Rate

> • | Byte 11 - Downlink Committed Data Rate

> • | Byte 5-8 - Uplink Burst Size (in Network Byte Order)

> • | Byte 1-4 - Downlink Burst Size (in Network Byte Order)

> SN1-QoS-Tp-Dnlk
> This attribute enables/disables Traffic Policing/Shaping in downlink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 73
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Policing = 1

> • | Shaping = 2

> SN1-QoS-Tp-Uplk
> This attribute enables/disables Traffic Policing/Shaping in uplink direction.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 79
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Policing = 1

> • | Shaping = 2

> SN1-QoS-Traffic-Policy
> This compound attribute simplifies sending QoS values for Traffic Class, Direction, Burst-Size, Committed-Data-Rate, Peak-Data-Rate, Exceed-Action, and Violate-Action from the RADIUS server. When the SN1-QoS-Traffic-Policy attribute is sent along with the Acct-Session-ID attribute, the system matches the particular PtDP context, and applies the new policy and retains the policy with the subscriber profile for future use. The next time the system sends a CoA request with a new policy and a different Acct-Session-ID for the same subscriber, the previously received policy is also applied to the matching PDP context along with the new policy.
> Important: This attribute is specific to the GGSN service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 177
> Value
> Contains the following subattributes:
> Direction
> Direction of traffic.
> Type
> 1
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Downlink = 0

> • | Uplink = 1

> Class
> Traffic class.
> Type
> 2
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Undefined = 0

> • | Conversational = 1

> • | Streaming = 2

> • | Interactive TP 1 = 4

> • | Interactive TP 2 = 5

> • | Interactive TP 3 = 6

> • | Background = 7

> Burst-Size
> Peak burst size.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer.
> Committed-Data-Rate
> Committed data rate.
> Type
> 4
> Length
> 4
> Value
> Unsigned integer.
> Peak-Data-Rate
> Peak data rate.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer.
> Exceed-Action
> Action to take on packets that exceed the Committed-Data-Rate but do not violate the Peak-Data-Rate.
> Type
> 6
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower IP Precedence = 2

> Violate-Action
> Violate action.
> Type
> 7
> Length
> 1
> Value
> Unsigned integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower IP Precedence = 2

> • | Buffer = 3

> • | Buffer-Transmit-On-Full = 4

> Auto-Readjust-Enabled
> Available only in StarOS 8.1 and later. Auto-readjust enabled.
> Type
> 8
> Length
> 1
> Value
> Unsigned integer.
> Auto-Readjust-Duration
> Available only in StarOS 8.1 and later. Auto-readjust duration.
> Type
> 9
> Length
> 4
> Value
> Unsigned integer.
> SN1-Rad-APN-Name
> RADIUS returned APN name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 162
> Length
> 1 - 64
> Value
> Opaque value
> SN1-Radius-Returned-Username
> This attribute is used to prefer RADIUS returned user name over constructed username in the accounting messages.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 236
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | No = 0

> • | Yes = 1

> SN1-Re-CHAP-Interval
> The Periodic CHAP authentication interval for PPP, in seconds.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 7
> Length
> 4
> Value
> Integer.
> SN1-Roaming-Profile
> SN1-Roaming-Profile
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 118
> Length
> 4
> Value
> Unsigned integer
> SN1-Roaming-Behavior
> SN1-Roaming-Behavior
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 121
> Length
> 4
> Value
> Unsigned integer
> SN1-Roaming-Sub-Use-GGSN
> SN1-Roaming-Sub-Use-GGSN
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 108
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN1-ROHC-Direction
> Specifies in which direction to apply Robust Header Compression (ROHC).
> Type
> Type 26
> Vendor ID
> Vendor-ID 8164
> VSA Type
> VSA-Type 153
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Any = 0

> • | Uplink = 1

> • | Downlink = 2

> SN1-ROHC-Flow-Marking-Mode
> Configure ROHC compression for marked flows only.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 216
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> SN1-ROHC-Mode
> Sets the mode of operation for Robust Header Compression for IP.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 151
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Reliable = 0

> • | Optimistic = 1

> • | Unidirectional = 2

> SN1-ROHC-Profile-Name
> Specifies the ROHC profile name to use for the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 238
> Length
> 1–64
> Value
> ASCII string
> SN1-Routing-Area-Id
> For GGSN calls this indicates the Routing Area ID of the subscriber.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 249
> Length
> 3
> Value
> Opaque value
> SN1-Rulebase
> When the session is active charging enabled, Rulebase name will specify one of the pre configured ECSv2 rulebases in active charging subsystem.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 249
> Length
> 1–64
> Value
> ASCII string
> SN1-Secondary-DCCA-Peer
> This attribute indicates the name of the Secondary DCCA peer and Secondary DCCA realm.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 224
> Length
> 1–192
> Value
> A colon separated string, like “secondary_peer : secondary_realm”.
> SN1-Secondary-DNS-Server
> This attribute indicates the IP address of the secondary DNS server that should be used for the session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 6
> Length
> 4
> Value
> IPv4 address
> SN1-Secondary-NBNS-Server
> Secondary NBNS Server IP Address.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 149
> Length
> 4
> Value
> IPv4 address
> SN1-Service-Address
> Used to send the bind IP address of the service in RADIUS messages.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 169
> Length
> 4
> Value
> IPv4 address
> SN1-Service-Type
> This attribute signifies the type that the user is accessing.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 24
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | PDSN = 1

> • | Management = 2

> • | HA = 3

> • | GGSN = 4

> • | LNS = 5

> • | IPSG = 6

> • | CSCF = 7

> • | ASNGW = 8

> • | PDIF = 9

> • | STANDALONE_FA = 10

> • | SGSN = 11

> • | PHSGW = 12

> • | PDG = 13

> • | MIPV6HA = 14

> • | PGW = 15

> • | SGW = 16

> • | FNG=17

> SN1-Simultaneous-SIP-MIP
> This attribute indicates if a PDSN Subscriber can simultaneously be given Simple IP and Mobile IP service.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 22
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Subscriber-Acct-Mode
> SN1-Subscriber-Acct-Mode
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 192
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | flow-based-auxilliary = 0

> • | flow-based-all = 1

> • | flow-based-none = 2

> • | session-based = 3

> • | main-a10-only = 4

> SN1-Subscriber-Accounting
> This attribute specifically enables or disables subscriber accounting. Note that if enabled, subscriber accounting still needs to be enabled in the subscriber's AAA context for accounting to be performed.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 64
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Radius = 1

> • | GTPP = 2

> SN1-Subscriber-Acct-Interim
> This attribute specifies if accounting INTERIM messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context (along with a specific INTERIM interval), if accounting INTERIM messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 70
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN1-Subscriber-Acct-Rsp-Action
> When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the RADIUS server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the RADIUS server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the RADIUS server.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 100
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | No_Early_PDUs = 1

> • | Delay_GTP_Response = 2

> SN1-Subscriber-Acct-Start
> This attribute specifies if accounting START messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting START messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 69
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN1-Subscriber-Acct-Stop
> This attribute specifies if accounting STOP messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting STOP messages are to be sent.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 71
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal = 0

> • | Suppress = 1

> SN1-Subscriber-Class
> Customer-requested attribute for supporting specific behavior for their subscriber billing.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 219
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Normal_Subscriber = 0

> • | Ting_100 = 1

> • | Ting_500 = 2

> • | Ting_Buddy = 3

> • | Ting_Star = 4

> • | Ting_Nolimit_SMS = 5

> • | Kids_Locator = 6

> • | Ting_2000 = 7

> • | Handicapped_Welfare = 8

> • | Reserved = 9

> SN1-Subscriber-Dormant-Activity
> This attribute specifies whether to treat dormant packets routed to the mobile as activity for idle timeout purposes. The default is Enabled. Disabled means dormant packets routed to the mobile are not treated as activity for idle timeout purposes.
> Type
> 26
> Vendor ID
> 8164
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Subscriber-IP-Hdr-Neg-Mode
> This attribute specifies whether to wait for (detect) IP header compression to be requested by the mobile before responding, or not to wait (force). Force is the default.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 67
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Force = 0

> • | Detect = 1

> SN1-Subscriber-IP-TOS-Copy
> This attribute enables copying of TOS bits from outer IP headers into inner tunneled IP headers. The default is Both.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 85
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Access-Tunnel = 1

> • | Data-Tunnel = 2

> • | Both = 3

> SN1-Subscriber-Nexthop-Address
> This attribute specifies the nexthop gateway address to be returned by AAA on a per subscriber basis.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 127
> Length
> 6
> Value
> IPv4 address
> SN1-Subscriber-No-Interims
> Subscriber No Interims.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 133
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Enabled = 0

> • | Disabled = 1

> SN1-Subscriber-Permission
> This attribute indicates the services allowed to be delivered to the subscriber. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 20
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Simple-IP = 1

> • | Mobile-IP = 2

> • | Simple-IP-Mobile-IP = 3

> • | HA-Mobile-IP = 4

> • | Simple-IP-HA-Mobile-IP = 5

> • | Mobile-IP-HA-Mobile-IP = 6

> • | All = 7

> • | In StarOS 8.3 and later, supported values are:

> • | None = 0

> • | Simple-IP = 1

> • | Mobile-IP = 2

> • | Simple-IP-Mobile-IP = 3

> • | HA-Mobile-IP = 4

> • | Simple-IP-HA-Mobile-IP = 5

> • | Mobile-IP-HA-Mobile-IP = 6

> • | SIP-MIP-HA-MIP = 7

> • | GGSN-PDP-TYPE-IP = 0x08, # see SessSubscriberPermission in sess_common.x

> • | GGSN-PDP-TYPE-PPP = 0x10, # see SessSubscriberPermission in sess_common.x

> • | Network-Mobility = 0x20

> • | FA-HA-NEMO = 0x26

> • | All = 0x3F

> SN1-Subscriber-Template-Name
> RADIUS returned subscriber template.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 158
> Length
> 1–127
> Value
> String
> SN1-Subs-Acc-Flow-Traffic-Valid
> This attribute indicates the subscriber account flow traffic is valid.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 225
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disable = 0

> • | Enable = 1

> SN1-Subs-IMSA-Service-Name
> IMS Authorization Service name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 159
> Length
> 1–128
> Value
> ASCII string
> SN1-Subs-VJ-Slotid-Cmp-Neg-Mode
> Enable/Disable slotid compression in either direction when using VJ compression.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 221
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | None = 0

> • | Receive = 1

> • | Transmit = 2

> • | Both = 3

> SN1-Tp-Dnlk-Burst-Size
> This attribute specifies the Traffic Policing downlink burst size in bytes.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 76
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Dnlk-Committed-Data-Rate
> This attribute specifies the Traffic Policing downlink committed data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 74
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Dnlk-Exceed-Action
> This attribute specifies the action to take on Traffic Policing downlink packets that exceed the committed-data-rate but do not violate the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 77
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN1-Tp-Dnlk-Peak-Data-Rate
> This attribute specifies the Traffic Policing downlink peak data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 75
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Dnlk-Violate-Action
> This attribute specifies the action to take on Traffic Policing downlink packets that exceed both the committed-data-rate and the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 78
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN1-Tp-Uplk-Burst-Size
> This attribute specifies the Traffic Policing uplink burst size in bytes.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 82
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Uplk-Committed-Data-Rate
> This attribute specifies the Traffic Policing uplink committed data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 80
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Uplk-Exceed-Action
> This attribute specifies the action to take on Traffic Policing uplink packets that exceed the committed-data-rate but do not violate the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 83
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN1-Tp-Uplk-Peak-Data-Rate
> This attribute specifies the Traffic Policing uplink peak data rate in bps.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 81
> Length
> 4
> Value
> Unsigned integer
> SN1-Tp-Uplk-Violate-Action
> This attribute specifies the action to take on Traffic Policing uplink packets that exceed both the committed-data-rate and the peak-data-rate.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 84
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Transmit = 0

> • | Drop = 1

> • | Lower-IP-Precedence = 2

> • | Buffer = 3

> • | Transmit-On-Buffer-Full = 4

> SN1-Traffic-Group
> This attribute is used to assign a tag to a FA or a group of FAs, so that traffic policy can be enforced based on the tag value.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 161
> Length
> 2
> Value
> Unsigned integer
> SN1-Transparent-Data
> This AVP is used by RADIUS to provide Global Title information for the GGSN to use in CDRs and Quota Auth.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 247
> Length
> In StarOS 8.1 and later: 1–247 In StarOS 8.0: 1–237
> Value
> Opaque value
> SN1-Tun-Addr-Policy
> Describes IP address validation policy for non L2TP tunneled calls.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 156
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | no-local-alloc-validate = 0

> • | local-alloc = 1

> • | local-alloc-validate = 2

> SN1-Tunnel-Gn
> Used to enable/disable Gn interface from PDG/TTG to GGSN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 174
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Disabled = 0

> • | Enabled = 1

> SN1-Tunnel-ISAKMP-Crypto-Map
> This attribute specifies the system-defined crypto map to use for the subscriber's Mobile-IP connection, when IPSec is used to protect the Mobile-IP connection. This attribute is salt-encrypted.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 38
> Length
> 1–128
> Value
> String
> SN1-Tunnel-ISAKMP-Secret
> This attribute specifies the secret to use for IKE.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 39
> Length
> 1–128
> Value
> String
> SN1-Tunnel-Load-Balancing
> Specifies the load-balancing algorithm to use when tunneling is employed.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 27
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | random = 1

> • | balanced = 2

> • | prioritized = 3

> SN1-Tunnel-Password
> Contains a secret for tunneling usage. Currently this is only used for L2TP. It is recommended that if your RADIUS server supports salt-encryption of attributes, that you use the Tunnel-Password attribute instead.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 26
> Length
> 1–247
> Value
> A bitstring which is the tunnel secret.
> SN1-Unclassify-List-Name
> SN1-Unclassify-List-Name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 132
> Length
> 1–132
> Value
> String
> SN1-Virtual-APN-Name
> This attribute indicates the virtual APN name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 94
> Length
> 1–64
> Value
> Opaque value
> SN1-Visiting-Behavior
> SN1-Visiting-Behavior
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 120
> Length
> 4
> Value
> Unsigned integer
> SN1-Visiting-Profile
> Visiting Profile.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 117
> Length
> 4
> Value
> Unsigned integer
> SN1-Visiting-Sub-Use-GGSN
> Accept Visiting.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 107
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Deny = 0

> • | Accept = 1

> SN1-Voice-Push-List-Name
> SN1-Voice-Push-List-Name.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 131
> Length
> 1–32
> Value
> String
> SN1-VPN-ID
> This attribute indicates the Destination VPN of the user, specified by a 32-bit identifier.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1
> Length
> 4
> Value
> Unsigned integer
> SN1-VPN-Name
> This attribute indicates the name of the user’s destination VPN.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 2
> Length
> 1–253
> Value
> ASCII string
> SNA-Input-Gigawords
> This attribute contains the total number of input gigawords.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 206
> Length
> 4
> Value
> Unsigned integer
> SNA-Output-Gigawords
> This attribute contains the total number of output gigawords.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 207
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Bad-Addr
> This attribute contains the total number of frames received with bad address field in the HDLC header field, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1011
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Bad-Ctrl
> This attribute contains the total number of frames received with bad control field in the HDLC header field, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1012
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Bad-FCS
> This attribute contains the number of frames received, for the user’s PPP session, with bad FCS.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1014
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Ctrl-Input-Octets
> This attribute contains the number of PPP Control Octets received for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1001
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Ctrl-Input-Packets
> This attribute contains the number of PPP Control packets received for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1003
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Ctrl-Output-Octets
> This attribute contains the number of PPP Control Octets sent to the user during the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1002
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Ctrl-Output-Packets
> This attribute contains the number of PPP Control packets sent to the user during the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1004
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Discards-Input
> This attribute contains the number of PPP input frames that were discarded during the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1007
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Discards-Output
> This attribute contains the number of PPP output frames that were discarded during the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1008
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Echo-Req-Input
> This attribute contains the number of LCP echo packets received, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1015
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Echo-Req-Output
> This attribute contains the number of LCP echo packets sent, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1016
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Echo-Rsp-Input
> This attribute contains the number of LCP echo response packets received, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1017
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Echo-Rsp-Output
> This attribute contains the number of LCP echo response packets sent, for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1018
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Errors-Input
> This attribute contains the number of PPP input de-framing errors for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1009
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Errors-Output
> This attribute contains the number of PPP output framing errors for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1010
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Framed-Input-Octets
> This attribute contains the number of PPP octets received (without framing overhead) for the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1005
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Framed-Output-Octets
> This attribute contains the number of PPP octets sent (without framing overhead) to the user during the user’s PPP session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1006
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Packet-Too-Long
> This attribute contains the total number of frames received, for the user’s PPP session, that exceeds the MTU of the interface.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1013
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Unfr-Data-In-Gig
> This attribute contains the total number of PPP gigawords without framing sent for the subscriber's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing send for the subscriber's session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 202
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Unfr-Data-Out-Gig
> This attribute contains the total number of PPP octets without framing received for the user's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing received for the subscriber's session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 203
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Unfr-data-In-Oct
> This attribute contains the total number of PPP octets without framing sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 200
> Length
> 4
> Value
> Unsigned integer
> SNA-PPP-Unfr-data-Out-Oct
> This attribute contains the total number of PPP octets without framing received for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 201
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRAK-Rcvd-Acc-Ack
> This attribute contains the total number of A11 registration ACK accepted for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1028
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRAK-Rcvd-Mis-ID
> This attribute contains the total number of A11 registration ACK messages received with ID-mismatch for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1030
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRAK-Rcvd-Msg-Auth-Fail
> This attribute contains the total number of message auth failures for A11 registration ACK messages for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1029
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRAK-Rcvd-Total
> This attribute contains the total number of A11 registration ACK received for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1027
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Acc-Dereg
> This attribute contains the number of Accept A11 registration reply sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1033
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Acc-Reg
> This attribute contains the number of Accept A11 registration reply sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1032
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Bad-Req
> This attribute contains the number of A11 registration reply sent for bad requests for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1034
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Denied
> This attribute contains the number of denied A11 registration reply sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1035
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Mis-ID
> This attribute contains the number of A11 registration reply sent for mismatched ID for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1036
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Send-Err
> This attribute contains the number of A11 registration reply sent with send errors for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1037
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Reply-Sent-Total
> This attribute contains the total number A11 registration reply sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1031
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Upd-Re-Sent
> This attribute contains the total number of A11 registration update re-sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1039
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Upd-Send-Err
> This attribute contains the total number of A11 registration update send errors for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1040
> Length
> 4
> Value
> Unsigned integer
> SNA-RP-Reg-Upd-Sent
> This attribute contains the total number of A11 registration update sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1038
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Acc-Dereg
> This attribute contains the number of A11 De-registration Requests accepted for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1021
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Acc-Reg
> This attribute contains the number of A11 Registration Requests accepted for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1020
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Badly-Formed
> This attribute contains the number of badly formed A11 registration requests received for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1024
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Mis-ID
> This attribute contains the number of A11 registration requests received with ID-mismatch for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1023
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Msg-Auth-Fail
> This attribute contains the number of message authentication failures for A11 registration requests for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1022
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-T-Bit-Not-Set
> This attribute contains the number of A11 registration requests received with T-Bit not set for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1026
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-Total
> This attribute contains the number of A11 Registration Requests received for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1019
> Length
> 4
> Value
> Unsigned integer
> SNA-RPRRQ-Rcvd-VID-Unsupported
> This attribute contains the number of A11 registration requests received with an unsupported Vendor ID for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 1025
> Length
> 4
> Value
> Unsigned integer
> SNA1-PPP-Unfr-data-In-Gig
> This attribute contains the total number of PPP gigawords without framing sent for the subscriber's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing send for the subscriber's session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 202
> Length
> 4
> Value
> Unsigned integer
> SNA1-PPP-Unfr-data-Out-Gig
> This attribute contains the total number of PPP octets without framing received for the user's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing received for the subscriber's session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 203
> Length
> 4
> Value
> Unsigned integer
> SNA1-PPP-Unfr-data-In-Oct
> This attribute contains the total number of PPP octets without framing sent for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 200
> Length
> 4
> Value
> Unsigned integer
> SNA1-PPP-Unfr-data-Out-Oct
> This attribute contains the total number of PPP octets without framing received for the user’s session.
> Type
> 26
> Vendor ID
> 8164
> VSA Type
> 201
> Length
> 4
> Value
> Unsigned integer
> Terminal-Capability
> Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 219
> Length
> 1
> Value
> The system does not interpret this value, but it is copied in accounting messages.
> Termination-Action
> Indicates what action the NAS should take when the service is completed. AAAmgr passes this attribute to Sessmgr only for ASN-GW calls. The combination of Session-Timeout and Termination-Action attributes received in Access-Accept or Access-Challenge determines how NAS should interpret it.
> Type
> 29
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 6
> Value
> Enumerated integer. Supported values are:

> • | Default = 0 — Indicates that the session should terminate.

> • | RADIUS-Request = 1 — Indicates that re-authentication should occur on expiration of the Session-Time. Upon termination of the specified service the NAS MAY send a new Access-Request to the RADIUS server, including the State attribute if any.

> Tunnel-Assignment-ID
> This attribute indicates the tunnel to which the session is to be assigned.
> Type
> 82
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–247
> Value
> ASCII string. It can be tagged.
> Tunnel-Client-Auth-ID
> This attribute contains the name of the client for the purposes of tunnel authentication.
> Type
> 90
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–247
> Value
> ASCII string. It can be tagged.
> Tunnel-Client-Endpoint
> This attribute is an identifier of the Tunnel client. When Tunnel-Medium-Type = IPv4, then this attribute is in the form of an IP address string in “dotted-decimal” notation.
> Type
> 66
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–250
> Value
> Opaque value. It can be tagged.
> Tunnel-Medium-Type
> This attribute indicates the protocol medium over which the tunneling protocol runs. It is used to describe the format of the attributes Tunnel-Client-Endpoint and Tunnel-Server-Endpoint.
> Type
> 65
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. It can be tagged. Supported values are:

> • | IPv4 = 1

> • | IPv6 = 2

> • | NSAP = 3

> • | HDLC = 4

> • | BBN-1822 = 5

> • | IEEE-802 = 6

> • | E-163 = 7

> • | E-164 = 8

> • | F-69 = 9

> • | X-121 = 10

> • | IPX = 11

> • | Appletalk = 12

> • | Decnet-IV = 13

> • | Banyan-Vines = 14

> • | E-164-NSAP-Subaddress = 15

> Tunnel-Password
> This attribute contains a shared secret for the Tunnel connection. It is salt-encrypted.
> Type
> 69
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–240
> Value
> Opaque value
> Tunnel-Preference
> This attribute indicates the priority given to the tunnel group. The tunnel group is defined as those tunnel attributes that have the same tag.
> Type
> 82
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Unsigned integer
> Tunnel-Private-Group-ID
> This attribute contains the context of the tunnel.
> Type
> 81
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–252
> Value
> ASCII string. It can be tagged.
> Tunnel-Server-Auth-ID
> This attribute contains the name of the server for the purposes of tunnel authentication.
> Type
> 91
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–252
> Value
> Opaque value
> Tunnel-Server-Endpoint
> This attribute is an identifier of the Tunnel server. When Tunnel-Medium-Type = IPv4, then this attribute is in the form of an IP address string in “dotted-decimal” notation.
> Type
> 67
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–250
> Value
> A string identifying the Tunnel server. It can be tagged.
> Important: This attribute is used in conjunction with L2TP functionality. Please refer to the RFC 2868 Tunneling Attributes section for additional information on this and other attributes added in support of this functionality.
> Tunnel-Type
> This attribute indicates the type of tunnel used by the subscriber.
> Type
> 64
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 4
> Value
> Enumerated integer. It can be tagged. Supported values are:

> • | PPTP = 1

> • | L2F = 2

> • | L2TP = 3

> • | ATMP = 4

> • | VTP = 5

> • | AH = 6

> • | IP-IP = 7

> • | MIN-IP-IP = 8

> • | ESP = 9

> • | GRE = 10

> • | DVS = 11

> • | MIP = 12

> • | VLAN = 13

> User-Name
> This attribute indicates the name of the user to be authenticated. This field can contain a stand-alone user name, or a user name and domain name. The format of this field is variable and configurable on a per-context basis. Separation of user and domain names is delineated by a special character, which can be %, -, @, \, #, and /. The user name may appear before the domain name or after. If this attribute is included in the Access-Accept, then the value of that attribute will be the value of the User-Name attribute in subsequent Accounting-Request messages for that particular session.
> Type
> 1
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–253
> Value
> String
> User-Password
> This attribute contains the encrypted password of the user, when simple password authentication is being used.
> Type
> 2
> Vendor ID
> N/A
> VSA Type
> N/A
> Length
> 1–128
> Value
> String
> WiMAX-Acct-Input-Packets-Giga
> Number of packets incremented each time Acct-Input-Packets(47) overflows.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 48
> Length
> 4
> Value
> Unsigned integer
> WiMAX-Acct-Output-Packets-Giga
> Number of packets incremented each time Acct-Output-Packets(48) overflows.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 49
> Length
> 4
> Value
> Unsigned integer.
> WiMAX-Active-Time
> The amount of time the session was not in idle state.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 39
> Length
> 4
> Value
> Unsigned integer.
> WiMAX-Beginning-Of-Session
> WiMAX beginning of session.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 22
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> WiMAX-BS-ID
> Uniquely identifies an NAP and a Base Station within that NAP. The first three octets representing the NAP operator identifier, and the next three the Base Station ID.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 46
> Length
> 6–12
> Value
> Opaque value
> WiMAX-Capability
> This compound attribute identifies the supported WiMAX capabilities.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 1
> Length
> 1–246
> Value
> Contains the following subattributes:
> WiMAX-Release
> Specifies WiMAX release of the sender.
> Type
> 1
> Length
> 4
> Value
> ASCII string
> Accounting-Capabilities
> Describes accounting capabilities supported for the session.
> Type
> 2
> Length
> 1
> Value
> 0x00 = No accounting. Only valid at the HA.

> • | 0x01 = IP-Session-based accounting. Default value for the ASN.

> • | 0x02 = Flow-based accounting

> Hotlining-Capabilities
> Describes hotline capabilities supported.
> Type
> 3
> Length
> 1
> Value
> 0x00 = Hot lining is not Supported

> • | 0x01 = Profile-based Hot lining is supported (using Hotline-Profile-ID VSA)

> • | 0x02 = Rule-based Hot lining is supported using NAS-Filter-Rule

> • | 0x04 = Hot lining HTTP Redirection is supported.

> • | 0x08 = Rule-based Hot lining is supported using IP-Redirection rule.

> Idle-Mode-Notification-Capabilities
> Describes idle mode notification capabilities.
> Type
> 4
> Length
> 1
> Value
> 0x00 = Idle Mode notification is not supported or is not required.

> • | 0x01 = Idle Mode notification is supported or is required.

> ROHC-Support
> Describes ROHC capability support for the session
> Type
> 5
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Not-Supported = 0x00

> • | Supported = 0x01

> WiMAX-Control-Octets-In
> Octet counts for incoming Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 4
> Length
> 13
> Value
> Unsigned integer
> WiMAX-Control-Octets-Out
> Octet counts for outgoing Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 34
> Length
> 4
> Value
> Unsigned integer
> WiMAX-Control-Packets-In
> Packet counts for incoming Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 4
> Length
> 13
> Value
> Unsigned integer
> WiMAX-Control-Packets-Out
> Packet counts for outgoing Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 33
> Length
> 4
> Value
> Unsigned Integer
> WiMAX-Count-Type
> Indicates if the record represents compressed counts over-the-air.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 59
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Uncompressed = 0

> • | Compressed = 1

> WiMAX-Device-Auth-Indicator
> Indicates whether NAS performed device authentication successfully or not.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 2
> Length
> 1
> Value
> Unsigned octet.
> WiMAX-Flow-Description
> Describes a flow classifier.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 50
> Length
> 1–240
> Value
> String
> WiMAX GMT-Time-Zone-Offset
> The current offset in seconds of the local time at the NAS with respect to GMT time.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 3
> Length
> 4
> Value
> Unsigned integer.
> WiMAX-Home-HNP-PMIP6
> WiMAX-Home-HNP-PMIP6
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 133
> Length
> 2–18
> Value
> Opaque value
> WiMAX-Home-IPv4-HoA-PMIP6
> WiMAX-Home-IPv4-HoA-PMIP6
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 135
> Length
> 4
> Value
> IPv4 Address
> WiMAX-Hotline-Indicator
> WiMAX-Hotline-Indicator
> Type
> This attribute in a RADIUS Accounting-Request message indicates to back-office systems (billing audit systems) that the session has been Hot-Lined.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 24
> Length
> 1–246
> Value
> Opaque value
> WiMAX-Idle-Mode-Transition
> A flag indicating whether the mobile node is in idle mode or not. When the mobile node enters or exits idle mode, an interim accounting message that includes WiMAX-Idle-Mode-Transition(26/44) attribute is generated instantly. The value of this attribute is 1 when mobile enters idle mode, and 0 when mobile exits idle mode. If accounting mode is flow based, then the asynchronous interim message is generated only for an ISF and not for all the flows in the session. Regular interim accounting if enabled, is not affected by idle mode entry. Also, the regular interim messages will not include WiMAX-Idle-Mode-Transition attribute.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 44
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | In idle mode = 0x01

> • | Not in idle mode = 0x00

> WiMAX-IP-Technology
> Indicates the type of WiMAX session being used.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 23
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | SIP = 1

> • | PMIP4 = 2

> • | CMIP4 = 3

> • | CMIP6 = 4

> • | Ethernet-CS = 5

> • | PMIP6 = 6

> WiMAX-NAP-ID
> Uniquely identifies the Network Access Provider.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 45
> Length
> 3
> Value
> String
> WiMAX-NSP-ID
> Uniquely identifies the Network Service Provider.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 57
> Length
> 3
> Value
> Opaque value
> WiMAX-Packet-Flow-Descriptor
> This compound attribute describes a packet flow. A packet flow may describe uni-directional flow and bi-directional flow. The packet flow descriptor may be pre-provisioned. A packet flow descriptor references one or two QoS specifications.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 28
> Length
> 4–1400
> Value
> Contains the following subattributes:
> PDF-ID
> Used to match all records from the same Packet Data Flow.
> Type
> 1
> Length
> 2
> Value
> Unsigned integer
> SDF-ID
> Used to match all PDFs from the same Service Data Flow.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer
> Service-Profile-ID
> Identifies a pre configured Flow Descriptor at the NAS.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> Direction
> Direction of the PDF.
> Type
> 4
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Uplink = 1

> • | Downlink = 2

> • | Bi-Directional = 3

> Activation-Trigger
> Specifies the trigger to be used for the activation of Service Flow.
> Type
> 5
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Provisioned = 0x01

> • | Admit = 0x02

> • | Provisioned-Admit = 0x03

> • | Activate = 0x04

> • | Provisioned-Activate = 0x05

> • | Admit-Activate = 0x06

> • | Provisioned-Admit-Activate = 0x07

> • | Dynamic = 0x08

> • | Dynamic-Admit = 0x0a

> • | Dynamic-Activate = 0x0c

> • | Dynamic-Admit-Activate = 0x0e

> Transport-Type
> Type of transport (IP, Ethernet).
> Type
> 6
> Length
> 1
> Value
> Enumerated integer
> Uplink-QoS-ID
> Identifier of the QoS Descriptor for Uplink or Bidirection.
> Type
> 7
> Length
> 1
> Value
> Unsigned integer
> Downlink-QoS-ID
> Identifier of the QoS Descriptor for Downlink.
> Type
> 8
> Length
> 1
> Value
> Unsigned integer
> Uplink-Classifier
> Classifier to match for traffic flowing in Uplink Direction.
> Type
> 9
> Length
> 1–240
> Value
> String
> Downlink-Classifier
> Classifier to match for traffic flowing in Downlink Direction.
> Type
> 10
> Length
> 1–240
> Value
> String
> WiMAX-Packet-Flow-Descriptor-V2
> Describes a Unidirectional or Bidirectional Packet Flow Descriptor Version 2.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 84
> Length
> 4–1400
> Value
> Contains the following subattributes:
> PDF-ID
> Used to match all records from the same Packet Data Flow.
> Type
> 1
> Length
> 2
> Value
> Unsigned integer.
> SDF-ID
> Used to match all PDFs from the same Service Data Flow.
> Type
> 2
> Length
> 2
> Value
> Unsigned integer.
> Service-Profile-ID
> Identifies a pre-configured Flow Descriptor at the NAS.
> Type
> 3
> Length
> 4
> Value
> Unsigned integer.
> Direction
> Direction of the PDF.
> Type
> 4
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Uplink = 1

> • | Downlink = 2

> • | Bi-Directional = 3

> Activation-Trigger
> Specifies the trigger to be used for the activation of Service Flow.
> Type
> 5
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Provisioned = 0x01

> • | Admit = 0x02

> • | Activate = 0x04

> • | Dynamic = 0x08

> Transport-Type
> Type of transport (IP, Ethernet).
> Type
> 6
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | IPv4-CS = 1

> • | IPv6-CS = 2

> • | Ethernet = 3

> Uplink-QoS-ID
> Identifier of the QoS Descriptor for Uplink or Bidirection.
> Type
> 7
> Length
> 1
> Value
> Unsigned integer.
> Downlink-QoS-ID
> Identifier of the QoS Descriptor for Downlink.
> Type
> 8
> Length
> 1
> Value
> Unsigned integer.
> WiMAX-Packet-Flow-Classifier
> Describes Packet Flow Classifiers.
> Type
> 9
> Value
> Contains the following subattributes:
> Classifier-ID
> WiMAX Classifier ID.
> Type
> 1
> Length
> 1
> Value
> Unsigned integer.
> Priority
> WiMAX Classifier Priority.
> Type
> 2
> Length
> 1
> Value
> Unsigned integer.
> Protocol
> WiMAX Classifier Protocol, i.e TCP/UDP.
> Type
> 3
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | ICMP = 1

> • | TCP = 6

> • | UDP = 17

> Direction
> Direction of the PDF.
> Type
> 4
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Uplink = 1

> • | Downlink = 2

> • | Bi-Directional = 3

> Source-Specification
> Identifies WiMAX classifier rule params for source specification.
> Type
> 5
> Value
> Contains the following subattributes:
> IP-Address
> Contains source/destination address.
> Type
> 1
> Length
> 4
> Value
> IPv4 address.
> IP-Address-Range
> WiMAX Packet Classifier IP Address Range.
> Type
> 2
> Length
> 1
> Value
> Opaque value
> IP-Address-Mask
> WiMAX Packet Classifier IP Address Mask.
> Type
> 3
> Length
> 5
> Value
> Opaque value
> Port
> WiMAX Packet Classifier Port.
> Type
> 4
> Length
> 2
> Value
> Unsigned integer.
> Port-Range
> WiMAX Packet Classifier Port Range.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer.
> Inverted
> WiMAX Classifier Inverted.
> Type
> 6
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | FALSE = 0

> • | TRUE = 1

> Assigned
> WiMAX Classifier Assigned.
> Type
> 7
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Src_Assigned = 1

> • | Dest_Assigned = 2

> • | Src_Dest_Assigned = 3

> Destination-Specification
> Identifies WiMAX classifier rule params for destination specification.
> Type
> 6
> Value
> Contains the following subattributes:
> IP-Address
> Contains source/destination address.
> Type
> 1
> Length
> 4
> Value
> IPv4 address.
> IP-Address-Range
> WiMAX Packet Classifier IP Address Range.
> Type
> 2
> Length
> 8
> Value
> Opaque value
> IP-Address-Mask
> WiMAX Packet Classifier IP Address Mask.
> Type
> 3
> Length
> 5
> Value
> Opaque value
> Port
> WiMAX Packet Classifier Port.
> Type
> 4
> Length
> 2
> Value
> Unsigned integer.
> Port-Range
> WiMAX Packet Classifier Port Range.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer.
> Inverted
> WiMAX Classifier Inverted.
> Type
> 6
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | FALSE = 0

> • | TRUE = 1

> Assigned
> WiMAX Classifier Assigned.
> Type
> 7
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Src_Assigned = 1

> • | Dest_Assigned = 2

> • | Src_Dest_Assigned = 3

> IP-TOS-DSCP-Range-And-Mask
> WiMAX Classifier WiMAX-IP-TOS-DSCP-Range-And-Mask.
> Type
> 7
> Length
> 1–3
> Value
> Opaque value
> Action
> Wimax Classifier Action.
> Type
> 8
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Reserved = 0

> • | Permit = 1

> • | Deny = 2

> Paging-Preference
> WiMAX Paging Preference.
> Type
> 10
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | FALSE = 0

> • | TRUE = 1

> WiMAX-PDF-ID
> The value of this attribute matches all records from the same packet data flow. PDFID is assigned by the CSN and remains constant through all handover scenarios.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 26
> Length
> 2
> Value
> Unsigned integer
> WiMAX-PPAC
> The Prepaid-Accounting-Capability (PPAC) attribute is sent in the Access-Request message by a prepaid capable ASNGW, and is used to describe the prepaid capabilities of the ASNGW. The absence of this attribute indicates that the client is not capable of prepaid accounting and the session should not use prepaid accounting.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 35
> Value
> Contains the following subattribute:
> Available-In-Client
> The optional Available-In-Client subtype, generated by the PPC, indicates the metering capabilities of the NAS and is be bitmap encoded.
> Type
> 1
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Supported_None = 0

> • | Supported_Volume = 1

> • | Supported_Duration = 2

> • | Supported_Volume_And_Duration = 3

> WiMAX-PPAQ
> Prepaid Quota, used for charging, report usage, and request quota. This attribute specifies the characteristics for pre-paid accounting of the volume and/or duration of a packet data session. It should be present in all on-line RADIUS Access-Request and on-line RADIUS Access-Accept messages and may be included in other RADIUS Access-Accept messages. In Authorize-Only Access-Request messages, it is used for one-time charging, report usage and the request for further quota. In an Access-Accept message it is used in order to allocate the (initial and subsequent) quotas.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 37
> Value
> Contains the following subattributes:
> Quota-Identifier
> Is generated by the PPS together with the allocation of new quota.
> Type
> 1
> Length
> 1-4
> Value
> Opaque value
> Volume-Quota
> Indicates the volume in octets excluding control data.
> Type
> 2
> Length
> 4-12
> Value
> Opaque value
> Volume-Threshold
> Is generated by the PPS and indicates the volume (in octets) that be consumed before a new quota should be requested.
> Type
> 3
> Length
> 4-12
> Value
> Opaque value
> Duration-Quota
> 3GPP2 PrePaid Duration Quota. This is optionally present if duration-based charging is used. In RADIUS Access-Accept message, it indicates the duration (in seconds) allocated for the session by the PPS. In an on-line RADIUS Access-Accept message, it indicates the total duration (in seconds) since the start of the accounting session related to the QuotaID of the PPAQ in which it occurs.
> Type
> 4
> Length
> 4
> Value
> Unsigned integer
> Duration-Threshold
> 3GPP2 PrePaid Duration Quota Threshold. This is optionally present if Duration-Quota is present in a RADIUS Access-Accept message. It is generated by the PPS and indicates the duration (in seconds) that should be consumed before a new quota should be requested. This threshold should not be larger than the Duration-Quota.
> Type
> 5
> Length
> 4
> Value
> Unsigned integer
> Update-Reason
> Reason for initiating online quota update operation. This should be present in the Authorize-Only RADIUS Access-Request message. It indicates the reason for initiating the on-line quota update operation. Update reasons 6, 7, 8, and 9 indicate that the associated resources are released at the client side, and that therefore the PPS should not allocate a new quota in the RADIUS Access Accept message.
> Type
> 8
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Pre-Initialization = 1

> • | Initial-Request = 2

> • | Threshold-Reached = 3

> • | Quota-Reached = 4

> • | TITSU-Approaching = 5

> • | Remote-Forced-Disconnect = 6

> • | Client-Service-Termination = 7

> • | Access-Service-Terminated = 8

> • | Service-Not-Established = 9

> • | One-Time-Charging = 10

> Pre-Paid-Server
> PrePaid server IP address. This optional subtype indicates the address IPv4 of the serving PPS. If present, the Home RADIUS server uses this address to route the message to the serving PPS. The attribute may be sent by the Home RADIUS server. Multiple instances of this subtype MAY be present in a single PPAQ. If present in the incoming RADIUS Access-Accept message, the ASNGW should send this attribute back without modifying it in the subsequent RADIUS Access-Request message.
> Type
> 9
> Length
> 4
> Value
> IPv4 address
> Service-ID
> This value is a string that uniquely describes the service instance to which prepaid metering should be applied.
> Type
> 10
> Length
> 1-246
> Value
> Opaque value
> Termination-Action
> Describes action to take when PPS does not grant additional quota.
> Type
> 12
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Reserved = 0

> • | Terminate = 1

> • | Request-more-quota = 2

> • | Redirect/Filter = 3

> WiMAX-Prepaid-Indicator
> Indicates that this session was associated with a prepaid user (online accounting).
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 25
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Offline = 0

> • | Online = 1

> WiMAX-Prepaid-Tariff-Switch
> Attribute to indicate Tariff-Switch-Interval / Time-Interval-After-Tariff-Switch-Update by the PPS and Volume-Used-After-Tariff-Switch by the PPC.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 38
> Value
> Contains the following subattributes:
> Quota-Identifier
> It is generated by the PPS together with the allocation of new quota.
> Type
> 1
> Length
> 1-4
> Value
> Opaque value
> Volume-Used-After-Tariff-Switch
> Volume Quota used after Tariff Switch Happened
> Type
> 2
> Length
> 4
> Value
> Unsigned integer
> Tariff-Switch-Interval
> Tariff Switch Interval in seconds
> Type
> 3
> Length
> 4
> Value
> Unsigned integer
> Time-Interval-After-Tariff-Switch-Update
> Duration after TSI where an on-line RADIUS Access-Request is sent by PrePaid client to report VUATS before the next TS condition is triggered
> Type
> 4
> Length
> 4
> Value
> Unsigned integer
> WiMAX-QoS-Descriptor
> This attribute describes over the air QoS parameter that are associated with a flow. The QoS-Descriptor is only valid for the actual RADIUS transaction.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 29
> Length
> 6–700
> Value
> Contains the following 17 subattributes:
> QoS-ID
> Unique ID for the QoS specification in the packet
> Type
> 1
> Length
> 1
> Value
> Unsigned integer
> Global-Service-Class-Name
> Represents Global Service Class Name as defined in IEEE802.16e
> Type
> 2
> Length
> 6
> Value
> String
> Service-Class-Name
> Represents Service Class Name as defined in IEEE802.16e
> Type
> 3
> Length
> 2–127
> Value
> String
> Schedule-Type
> Specifies Uplink granted scheduling type.
> Type
> 4
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort = 2

> • | nrtPS = 3

> • | rtPS = 4

> • | Extended-rtPS = 5

> • | UGS = 6

> Traffic-Priority
> Specifies the priority assigned to a Service Flow.
> Type
> 5
> Length
> 1
> Value
> Unsigned integer
> Maximum-Sustained-Traffic-Rate
> Defines Peak Information Rate of the service in bits/second.
> Type
> 6
> Length
> 4
> Value
> Unsigned integer
> Minimum-Reserved-Traffic-Rate
> Defines Minimum Rate reserved for the Service Flow in bits/second.
> Type
> 7
> Length
> 4
> Value
> Unsigned integer
> Maximum-Traffic-Burst
> Defines Maximum Burst Size accommodated for the Service in bytes/second
> Type
> 8
> Length
> 4
> Value
> Unsigned integer
> Tolerated-Jitter
> Represents Maximum Delay Variation in milliseconds.
> Type
> 9
> Length
> 4
> Value
> Unsigned integer
> Maximum-Latency
> Represents Maximum Latency in milliseconds.
> Type
> 10
> Length
> 4
> Value
> Unsigned integer
> Reduced-Resources-Code
> Indicates that requesting entity will accept reduced resources if requested resources are unavailable.
> Type
> 11
> Length
> 1
> Value
> Unsigned integer
> Media-Flow-Type
> Describes the application type, used as a hint in admission decisions
> Type
> 12
> Length
> 1
> Value
> Enumerated integer. Supported values are:

> • | VoIP = 1

> • | Robust-Browser = 2

> • | Secure-Browser/VPN = 3

> • | Streaming-Video-On-Demand = 4

> • | Streaming-Live-TV = 5

> • | Music-Photo-Download = 6

> • | Multi-Player-Gaming = 7

> • | Location-Based-Services = 8

> • | Text-Audio-Books-With-Graphics = 9

> • | Video-Conversation = 10

> • | Message = 11

> • | Control = 12

> • | Data = 13

> Unsolicited-Grant-Interval
> Specifies nominal interval between successive data grant opportunities for the Service Flow, in milliseconds.
> Type
> 13
> Length
> 2
> Value
> Unsigned integer
> SDU-Size
> Represents the number of bytes in the fixed size SDU.
> Type
> 14
> Length
> 1
> Value
> Unsigned integer
> Unsolicited-Polling-Interval
> Specifies maximal nominal interval between successive polling grant opportunities for the Service Flow.
> Type
> 15
> Length
> 2
> Value
> Unsigned integer
> Transmission-Policy
> Include options for PDU formation, and for uplink service flows, restrictions on the types of bandwidth request options that may be use.
> Type
> 17
> Length
> In StarOS 9.0 and earlier: 4; in StarOS 10.0 and later: 1
> Value
> Enumerated integer. Supported values are:

> • | no-bcast =0x01

> • | no-mcast = 0x02

> • | no-piggy-back = 0x04

> • | no-fragment = 0x08

> • | no-sup-payload-header = 0x10

> • | no-multiple-sdu = 0x20

> • | no-crc = 0x40

> • | no-rohc-compression = 0x80

> DSCP
> DSCP
> Type
> 18
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Best-Effort=0

> • | AF11=10

> • | AF12=12

> • | AF13=14

> • | AF21=18

> • | AF22=20

> • | AF23=22

> • | AF31=26

> • | AF32=28

> • | AF33=30

> • | AF41=34

> • | AF42=36

> • | AF43=38

> • | EF=46

> WiMAX-RRQ-HA-IP
> IPv4 or IPv6 address of the HA as contained in the MIP Registration Request or the BU.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 18
> Length
> 4-16
> Value
> Opaque value
> WiMAX-SDF-ID
> The value of this attribute matches all records from the same packet data flow. SDFID is assigned by the CSN and remains constant through all handover scenarios.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 27
> Length
> 2
> Value
> Unsigned integer
> WiMAX-Session-Continue
> The value of this attribute matches all records from the same packet data flow. SDFID is assigned by the CSN and remains constant through all handover scenarios.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 21
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | False = 0

> • | True = 1

> WiMAX-Session-Term-Capability
> WiMAX session term capability. This attribute is included in a RADIUS Access-Request message to the RADIUS server and indicates whether or not the NAS supports Dynamic Authorization.
> Type
> 26
> Vendor ID
> 24757
> VSA Type
> 36
> Length
> 4
> Value
> Enumerated integer. Supported values are:

> • | Only_Dynamic_Auth_Extn_to_Radius = 0x00000001

> • | Only_Reg_Revocation_in_MIP = 0x00000002

> • | Both_Dynamic_Auth_And_Reg_Revocation_in_MIP = 0x00000003

> Win-Call-Id
> Opaque 1 byte value received from customer RADIUS server in access request. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 205
> Length
> 1 byte value.
> Value
> The system does not interpret this value, but it is copied in accounting messages.
> Win-Service-Name
> Opaque value value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 206
> Length
> 1 -256
> Value
> The system does not interpret this value, but it is copied in accounting messages.
> WSType
> Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages.
> Type
> 136
> Vendor ID
> 5535 (Reusing the 3GPP2 VID in a non-standard way.)
> VSA Type
> 197
> Length
> 1
> Value
> The system does not interpret this value, but it is copied in accounting messages.
> Attribute Notes
> This section contains notes that apply to groups of attributes that have been included in support of specific features and/or functionality.
> RFC 2868 Tunneling Attributes
> Tunnel attributes may be tagged, which means the leading byte in the value field may be used to group attributes together. This is used to return a number of different tunnel configurations that are available to the subscriber. The tagged group with the highest tunnel preference (the lowest value of the Tunnel-Preference attribute) has precedence over other tunnel configurations.
> Tags can be a value from 1 through 31. Any value outside of this range for the leading byte means the attribute is not tagged, and the leading byte is then interpreted as part of the attribute value. Integer attributes that are tagged are three bytes in length (the leading byte is ignored), but are four bytes in length when not tagged (the leading byte is incorporated).
> If Tunnel attributes appear more than once in the RADIUS Accept-Accept but are not tagged, then the system treats the attributes as having an implicit tag. The first instance of the attribute has a tag value of 32, the second instance has a tag value of 33, etc.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883