> Exec Mode Show Commands (M-P)
> This section includes the commands show m3ua statistics through show profile-id-qci-mapping.
> show mag-service
> Displays statistic and counter information for Mobile Access Gateway (MAG) services on this system.
> Product
> HSGW, S-GW
> Privilege
> Inspector
> Syntax
> show mag-service { all | name service_name | session [ all | callid id | counters | full | msid id | summary | username name ] | statistics [ name service_name ] } [ | { grep grep_options | more } ]
> all
> Displays information for all configured MAG services on this system.
> name service_name
> Displays configuration information for a specific MAG service configured on this system.
> service_name must be an existing MAG service, and be from 1 to 63 alpha and/or numeric characters in length.
> session [ all | callid id | counters | full | msid id | summary | username name ]
> all: Displays all active MAG sessions using MAG services on the system.
> callid id: Displays available session information for the specific call identification number. id must be an eight-digit HEX number.
> counters: Displays counters for all MAG services on the system.This keyword can also be filtered by the following:

> • | all

> • | callid

> • | msid

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> full: Displays additional session information for all active MAG sessions using MAG services on the system. This keyword includes the information in the output of the ‘all’ keyword plus additional information. This keyword can also be filtered by the following:

> • | all

> • | callid

> • | msid

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> msid id: Displays available information for a specific mobile station identification number or group of numbers based on wildcard entry. id must be a valid MSID number and can be a sequence of characters and/or wildcard characters ('$' and/or '*'). The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as wildcard enclose them in single quotes ( ‘). For example: ‘$’.
> summary: Displays the number of MAG sessions currently active for MAG services configured on the system.
> username name: Displays available session information for a specific user in a service session. name must be followed by an existing user name and must be from 1 to 127 alpha and/or numeric characters.
> statistics [ name service_name ]
> name service_name: Displays MAG service statistics for a specific MAG service. service_name must be an existing MAG service and be from 1 to 63 alpha and/or numeric characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for MAG services on this system.
> Example
> The following command displays service statistics for the MAG service named mag1:
> show mag-service name mag1
> show map-service
> Displays information configured for the Mobile Application Part (MAP) services, including MAP service features and operational configuration. Also includes some related configuration information for the HLR and EIR configuration parameters.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show map-service [ all | name srvc_name ]
> name srvc_name
> srvc_name: must be a string of 1 to 63 alphanumeric characters that identifies a specific existing MAP service.
> Usage
> Use this command to display all MAP service or the statistics for a particular MAP service.
> Example
> The following command displays configuration information for the MAP service named map-svc-1:
> show map-service name map-srvc-1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show map statistics
> Displays Mobile Application Part (MAP) statistics.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show map statistics [ name srvc_name ]
> name srvc_name
> srvc_name: must be a string of 1 to 63 alphanumeric characters that identifies a specific existing MAP service.
> Usage
> Use this command to display all MAP statistics or the statistics for a particular MAP service.
> Example
> The following command displays statistics for the MAP service named map-svc-1:
> show map statistics name map-svc-1
> The following command displays combined statistics for all MAP services in the current context:
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show maximum-temperatures
> Shows the maximum temperature reached by each card since the last temperature timestamp reset.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show maximum-temperatures [ verbose] [ | { grep grep_options | more } ]
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> verbose
> Indicates that the output is to contain detailed information.
> Usage
> Verify the maximum temperature reached by components in the chassis since the indicated timestamp.
> Important: This command is not supported on all platforms.
> Example
> show maximum-temperatures
> show maximum-tempteratures verbose
> show mbms bearer-service
> Displays configuration information for bearer service configured for multimedia broadcast and multicast facility on this system.
> Product
> GGSN, SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show mbms bearer-service [ all | apn apn_name mcast-addr ip_address | service-type { broadcast | multicast } | full | instance instance_id | summary ] + [ | { grep grep_options| more } ]
> all
> Displays information on all bearer services configured on the system.
> apn apn_name mcast-addr ip_address
> Displays bearer service information of MBMS for a specific APN apn_name bind to given BM-SC (Broadcast Multicast - Service Center) server address ip_address.
> apn_name is the name of the APN and can be from 1 to 62 alpha and/or numeric characters and is case sensitive.
> ip_address is the IP address of the BM-SC server in IPv4 dotted decimal notation bind to the APN.
> service-type { broadcast | multicast }
> Displays information for a specific type of service for MBMS.
> broadcast: Specifies the MBMS service type as broadcast only.
> multicast: Specifies the MBMS service type as multicast only.
> full
> Displays full information for specific or all instances of bearer service in MBMS feature on system.
> instance instance_id
> Displays session information filtered for specific instances of bearer service in MBMS feature on system.
> instance_id is the indicator for bearer service running for MBMS session and it must be an integer from 1 through 64.
> summary
> Displays summary information for specific or all instances of bearer service in MBMS feature on system.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more options, refer to the Regulating a Command’s Output section of the Command Line Interface Reference.
> Usage
> Use this command to verify the configuration of one or all bearer services and active instances of bearer services under MBMS feature. It is also useful for monitoring or troubleshooting purposes.
> If this command is executed from within the local context with the all keyword, information for all bearer service instances running under MBMS feature configured on the system will be displayed.
> Example
> The following command displays configuration information for all bearer service instances running on system:
> show mbms bearer-service full all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mipfa
> Displays the foreign agent information for the mobile IP calls specified.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show mipfa { [ [ counters | full | summary ] { all | callid call_id | msid ms_id | peer-address [ operator ] peer_address | reverse-tunnel { on | off } | username user_name } | statistics [ fa-service fa_name | peer-address [ peer_address | greater-than peer_address | less-than peer_address | > peer_address | < peer_address ] } ] | peers fa-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ] } [ | { grep grep_options | more } ]
> counters | full | summary
> Default: concise output.
> counters: indicates the output is to include the statistic counters.
> full: indicates detailed information is to be displayed.
> summary: indicates only summary information is to be displayed.
> These options are not available in conjunction with the statistics keyword.
> all | callid call_id | msid ms_id | peer-address peer_ip_address | reverse-tunnel { on | off } | username user_name
> all: indicates all available information is to be displayed.
> callid call_id: indicates the information only for calls with Id call_id are to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> msid ms_id: specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI and /or characters $ and * for wildcard filter.
> show mipha msid 01234567$$
> will show any subscriber with a MSID that match the upper 8 digits of MSID supplied, i.e. 01234567 and any 2 digits at remaining 2 places.
> peer-address peer_ip_address: specifies the peer IP address for which MIP call information is to be displayed. peer_ip_address must be specified using the standard IPv4 dotted decimal notation.
> reverse-tunnel { on | off }: specifies either the on or off reverse IP tunnels information is to be displayed.
> username user_name: specifies a user only for which MIP call information is to be displayed where the user is specified as user_name.
> user_name must be a sequence of character and /or wildcard characters $ and * for wildcard matching with a string length of 1 to 127 characters.
> statistics [ fa-service fa_name | peer-address [ peer_address | greater-than peer_address | less-than peer_address | > peer_address | < peer_address ]
> Indicates the statistics information is to be displayed for foreign agent service specified as fa_name or for the peer specified by the address peer_address.
> fa-service fa_name : indicates the statistic information for the peer specified is to be displayed. fa_name must be from 1 to 63 alpha and/or numeric characters.
> peer-address peer_address :indicates the statistic information for the peer specified is to be displayed. peer_address must be specified using the standard IPv4 dotted decimal notation.
> greater-than peer_address: Specifies the range of IPv4 addresses greater than peer_address.
> less-than peer_address: Specifies the range of IPv4 addresses less than peer_address.
> > peer_address: Specifies the range of IPv4 addresses greater than peer_address.
> < peer_address: Specifies the range of IPv4 addresses less than peer_address.
> peer-address [ operator ] peer_address
> In conjunction with mipfa [ summary ] peer-address keyword, indicates a range of peers is to be displayed.
> peer-address [ operator ] peer_address must be specified using the standard IPv4 dotted decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than to specified peer_address

> • | >: IP address less than to specified peer_address

> • | greater-than: IP address less than to specified peer_address

> • | less-than: IP address less than to specified peer_address

> peers fa-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ]
> Displays peer servers for the specified FA service.
> fa-service service_name: Specifies the name of the FA service from which the associated peer servers are to be dispalyed. service_name must be an existing FA service and be from 1 to 63 alpha and/or numeric characters in length.
> current-sessions: Displays only peer servers with current sessions meeting the following criteria:

> • | > | greater-than sessions: Displays only peer servers currently running sessions higher than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “greater-than” and the “>” symbol are interchangeable in this instance of the command.

> • | < sessions: Displays only peer servers that are currently running sessions higher than the greater-than peramter but less than the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> • | < | less-than sessions: Displays only peer servers currently running sessions lower than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “less-than” and the “<” symbol are interchangeable in this instance of the command.

> • | > sessions: Displays only peer servers that are currently running sessions lower than the less-than peramter but more than the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> • | sessions: Displays only peer servers currently running sessions that are equal to the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> peer-address address: Displays only peer servers matching the IP address entered in this parameter. address must be specified using IPv4 dotted decimal notation and can be followed by the netmask of the address.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View MIP foreign agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
> Example
> The following displays the call information for all mobile IP FA calls and statistics for fa1, respectively.
> show mipfa all
> The following command displays the statistics for the foreign agent service fa1.
> show mipfa statistics fa-service fa1
> The following commands displays call information for user user6@aaa in full detail and in summary.
> show mipfa full username user6@aaa
> show mipfa summary username user1
> The following displays MIP FA call information for calls from mobile subscriber 4412345678 and peer address 1.2.3.4, respectively.
> show mipfa msid 4412345678
> show mipfa peer-address 1.2.3.4
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mipha
> Displays the home agent information for the mobile IP calls specified.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show mipha { [ [ counters | full | summary ] { all | callid call_id | imsi imsi_num | ip-address ip_addr | msid msid_num | peer-address [ operator ] peer_address | reverse-tunnel { on | off } | username user_name } | statistics [ ha-service ha_name | peer-address peer_address ] } ] | peers ha-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ] } [ | { grep grep_options | more } ]
> counters | full | summary
> Default: concise output.
> counters: indicates the output is to include the statistic counters.
> full: indicates detailed information is to be displayed.
> summary: indicates only summary information is to be displayed.
> These options are not available in conjunction with the statistics keyword.
> msid msid_num
> Displays the subscriber with supplied MSID on HA.
> msid msid_num: specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits hexadecimal digit specified as an IMSI, MIN, or RMI and /or characters $ and * for wildcard filter.
> In case of enforce imsi-min equivalence is enabled on the chasis and MIN or IMSI numbers supplied, this keyword/ filter will show subscribers with a corresponding MSID (MIN or IMSI) whose lower 10 digits matches to lower 10 digits of the supplied MSID.
> show mipha msid ABCD0123456789 or
> show mipha msid 0123456789
> will show any subscriber with a MSID that match the lower 10 digits of MSID supplied, i.e. 0123456789.
> show mipha msid 01234567$$
> will show any subscriber with a MSID that match the upper 8 digits of MSID supplied, i.e. 01234567 and any 2 digits at remaining 2 places.
> all | callid call_id | imsi imsi_num | ip-address ip_addr | msid msid_num | peer-address [ operator ] peer_address | reverse-tunnel { on | off } | username user_name
> all: indicates all available information is to be displayed.
> callid call_id: indicates the information only for calls with Id call_id are to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> imsi imsi_num: Specifies an international mobile subscriber ID only for which information is to be displayed. The IMSI (International Mobile Subscriber Identity) ID is a 15 character field which identifies the subscriber’s home country and carrier.
> ip-address ip_addr: Show statistics for a call that has the specified IP address assigned. ip_addr must be an IPv4 address specified in decimal notation.
> msid msid_num: Specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> peer-address peer_address: indicates the statistic information for the peer specified is to be displayed. peer-address peer_address must be specified using the standard IPv4 dotted decimal notation.
> reverse-tunnel { on | off }: specifies either the on or off reverse IP tunnels information is to be displayed.
> username user_name: specifies a user only for which MIP call information is to be displayed where the user is specified as user_name.
> user_name must be a sequence of character and /or wildcard characters $ and * for wildcard matching with a string length of 1 to 127 characters.
> peer-address [ operator ] peer_address
> In conjunction with mipha [ summary ] peer-address keyword, indicates a range of peers is to be displayed.
> peer_address must be specified using the standard IPv4 dotted decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than to specified peer_address

> • | >: IP address less than to specified peer_address

> • | greater-than: IP address less than to specified peer_address

> • | less-than: IP address less than to specified peer_address

> statistics [ ha-service ha_name | peer-address peer_address ]
> Indicates the statistics information is to be displayed for home agent service specified as ha_name or for the peer specified by the address peer_address.
> ha-service ha_name: indicates the statistic information for the peer specified is to be displayed. ha_name must be from 1 to 63 alpha and/or numeric characters.
> peer-address peer_address: indicates the statistic information for the peer specified is to be displayed. peer-address peer_address must be specified using the standard IPv4 dotted decimal notation.
> peers ha-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ]
> Displays peer servers for the specified HA service.
> ha-service service_name: Specifies the name of the HA service from which the associated peer servers are to be dispalyed. service_name must be an existing HA service and be from 1 to 63 alpha and/or numeric characters in length.
> current-sessions: Displays only peer servers with current sessions meeting the following criteria:

> • | > | greater-than sessions: Displays only peer servers currently running sessions higher than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “greater-than” and the “>” symbol are interchangeable in this instance of the command.

> • | < sessions: Displays only peer servers that are currently running sessions higher than the greater-than peramter but less than the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> • | < | less-than sessions: Displays only peer servers currently running sessions lower than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “less-than” and the “<” symbol are interchangeable in this instance of the command.

> • | > sessions: Displays only peer servers that are currently running sessions lower than the less-than peramter but more than the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> • | sessions: Displays only peer servers currently running sessions that are equal to the value entered in this parameter. sessions must be an integer from 1 to 3000000.

> peer-address address: Displays only peer servers matching the IP address entered in this parameter. address must be specified using IPv4 dotted decimal notation and can be followed by the netmask of the address.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> View MIP home agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
> Example
> The following displays the call information for all mobile IP HA calls and statistics for ha1, respectively.
> show mipha allshow mipha statistics ha-service ha1
> The following commands displays call information for user isp1user1 in full detail and in summary.
> show mipha full username isp1user1 show mipha summary username user1
> The following displays MIP HA call information for calls from mobile subscribers with reverse tunneling off and peer address 1.2.3.4, respectively.
> show mipha reverse-tunnel off show mipha peer-address 1.2.3.4
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mipv6ha
> Displays MIPv6 Home Agent-based information about selected Mobile IP calls.
> Product
> PDSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show mipv6ha [ all | callid callid | counters filter | full filter | ipv6-address ip_addr| statistics mipv6ha-service mipv6ha-service_name | summary filter | username user_name ]
> all
> Displays all information for mipv6ha calls.
> callid call_id
> Specifies the Call Identification number.
> call_id must be an eight-digit HEX number.
> counters [ all | callid | ipv6-address | username ]
> Displays the counters associated with the HA-based MIPv6 service. The following filters are available:

> • | all

> • | callid:

> • | ipv6-address

> • | username

> full [ all | callid | ipv6-address | username ]
> Displays all available information for the associated display or filter keyword.
> The following filters are available:

> • | all

> • | callid:

> • | ipv6-address

> • | username

> ipv6-address ip_addr
> Displays information for subscribers connected via the packet control function with a specific or range of IP address ipv6_address. The address must be specified using the IPv6 colon notation.

> • | <: Filters output so that only information less than the specified IPv6 address value is displayed.

> • | >: Filters output so that only information greater than the specified IPv6 address value is displayed.

> • | less-than:Filters output so that only information less than the specified IPv6 address value is displayed.

> • | greater-than:Filters output so that only information greater than the specified IPv6 address value is displayed.

> statistics [ mipv6ha-service mipv6ha-service_name ]
> Total of collected information for specific protocol since last restart or clear command.
> This can be filtered according to a specified mipv6ha-service.
> summary [ all | callid | ipv6-address | username ]
> Displays summary information for defined sessions, based on defined parameters.
> The following filters are available:

> • | all

> • | callid:

> • | ipv6-address

> • | username

> username user_name
> Displays session information for a specific username.
> Usage
> View MIPv6 home agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
> Example
> The following displays the call information for all mobile IP HA calls and statistics for ha1, respectively.
> show mipv6ha all
> The following command displays call information for user mipv6hauser1 in full detail and in summary.
> show mipv6ha full username mipv6hauser1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-hss service
> Displays configuration and setup information of MME-HSS service(s) running on a peer or local system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-hss service { all | name svc_name } [verbose] [|{grep grep_options | more}]
> all
> Displays configuration/setup information for all MME-HSS services configured on this system.
> name service_name
> Displays configuration/setup information for a specific MME-HSS service configured on this system.
> service_name must be an existing MME-HSS service, and be from 1 to 63 alpha and/or numeric characters in length.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view configuration/setup information for MME-HSS services on this system.
> This command also displays the configured actions for failure handling on various type of messages.
> Example
> The following command displays service statistics for all MME-HSS services configured on the esystem:
> show mme-hss service all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-hss session
> Displays session information of MME-HSS service(s) running on a peer or local system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-hss session [summary | full] [all | call-id call_identifier | mdn mdn_string | nai nai_string] [verbose] [|{grep grep_options | more}]
> summary
> This keyword displays the summarized output of this command.
> full
> This keyword displays detailed output of this command.
> all
> This keyword displays information of all MME-HSS sessions running on this system.
> call-id call_identifier
> Displays summarized or detailed statistics of MME-HSS sessions running and filtered on the basis of the call identifier with an MME-HSS service configured on this system.
> call_identifier must an existing call identity in eight character Hex digit format running on an MME service on system.
> mdn mdn_string
> Displays summarized or detailed statistics of MME-HSS sessions running and filtered on the basis of mobile directory Number (MDN) with an MME-HSS service configured on this system.
> mdn_string must be an alpha and/or numeric string of 1 to100 charactes in length.
> nai nai_string
> Displays summarized or detailed statistics of MME-HSS sessions running and filtered on the basis of Network Access Identifier(NAI) with an MME service configured on this system.
> nai_string must be an alpha and/or numeric string of 1 to128 charactes in length.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | {grep grep_options | more}
> This argument searches the output of the root command and selects the lines matching one or more patterns/options. The types of patterns are controlled by the options specified with grep_options.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view detialed or summarized session statistics of MME-HSS sessions running on MME-HSS services on a system. This command also provides the various filter criteria to display the session statistics.
> Example
> The following command displays information of all MME-HSS sessions of MME-HSS services running on a system:
> show mme-hss session all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> The following command displays summarized session information of all MME-HSS sessions running on a system:
> show mme-hss session summary all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service
> Displays configuration information for Mobility Management Entity (MME) services on this system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-service { all | name svc_name } [verbose] [|{grep grep_options | more}]
> all
> Displays configuration information for all MME services configured on this system.
> name service_name
> Displays configuration information for a specific MME service configured on this system.
> service_name must be an existing MME service, and be from 1 to 63 alpha and/or numeric characters in length.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view configuration information for MME services on this system.
> Example
> The following command displays service statistics for the MME service named mme1:
> show mme-service name mme1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service db statistics
> This command displays the MME database statistics for MME sessions for all or specific session instances on this system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-service db statistics [instance smgr_instance] [verbose] [|{grep grep_options | more}]
> instance smgr_instance
> This keyword specifies that MME database statistics are to be displayed for a specific instance of session manager running for MME service.
> smgr_instance must be specified as an instance ID in the range 0 through 4294967295. If instance is not specified summary statistics are displayed.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | {grep grep_options | more}
> This argument searches the output of the root command and selects the lines matching one or more patterns/options. The types of patterns are controlled by the options specified with grep_options.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view database statistics for all or a particular instance of session manager for MME services on this system.
> Example
> The following command displays the summary database statistics for the MME service on a system:
> show mme-service db statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service db record
> This command displays the MME database records of MME sessions grouped in session instances on this system filtered with IMSI or GUTI as criteria.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-service db record {all | imsi imsi_identifier | callid call_id | guti plmn plmn_id group-id mme_grp_id code mme_code m-tmsi mtmsi_value} [verbose] [|{grep grep_options | more}]
> all
> This keyword specifies the criteria to display all database records of a session instance used for MME service.
> imsi imsi_identifier
> This keyword specifies the filter criteria as International Mobile Subscriber Identity (IMSI) imsi_identifier to display the database records of a session instance.
> imsi_identifier is a 15 character IMSI field which identifies the subscriber’s home country and carrier. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
> callid call_id
> This keyword specifies the filter criteria as call id call_id to display the database records of a session instance.
> call_id must be specified as an 8-byte hexadecimal number.
> guti plmn plmn_id group-id mme_grp_id code mme_code m-tmsi mtmsi_value
> This set of keyword specifies the filter criteria as Globally Unique Temporary Identifier (GUTI) to display the database records for an MME service.
> The GUTI is constructed from the GUMMEI and the M-TMSI where GUMMEI is constructed from PLMN (MMC and MNC) plmn_id and MME Identifier is constructed from an MME Group ID (MMEGI) mme_grp_id and an MME Code (MMEC) mme_code.
> Within the MME, the mobile is identified by the M-TMSI mtmsi_value.
> A GUTI has; 1) unique identity for MME which allocated the GUTI; and 2) the unique identity of the UE within the MME that allocated the GUTI.
> Within the MME, the mobile is identified by the M-TMSI. The Globally Unique MME Identifier (GUMMEI) is constructed from public land mobile network id (PLMN) which constructed with MCC and MNC. The MME Identifier (MMEI) is constructed from an MME Group ID (MMEGI) and an MME Code (MMEC).
> In other words The GUTI is constructed from the GUMMEI and the M-TMSI.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | {grep grep_options | more}
> This argument searches the output of the root command and selects the lines matching one or more patterns/options. The types of patterns are controlled by the options specified with grep_options.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view database records for all or a particular instance of session manager for MME services on this system with IMSI or GUTI as a filter criteria.
> Example
> The following command displays the summary database records of a session instance for subscriber having IMSI as 123455432112345 in the MME service:
> show mme-service db record imsi 123455432112345
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service enodeb-association
> Displays configuration information of associated eNodeB with an MME services on system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-service enodeb-association [summary | full ] [all | mme-service-name mme_svc_name | peer-address peer_ip_address | peer-id peer_identifier] [verbose] [|{grep grep_options | more }]
> summary
> This keyword displays the summarized output of this command.
> full
> This keyword displays detailed output of this command.
> all
> This keyword displays information of all eNodeBs associated with MME services on this system.
> mme-service-name mme_svc_name
> Displays summarized or detailed configuration information of eNodeBs associated with specific MME service mme_svc_name configured on this system.
> mme_svc_name must be an existing MME service on system.
> peer-address peer_ip_address
> Displays summarized or detailed configuration information of eNodeBs associated with specific MME peer address peer_ip_address configured with an MME service on this system.
> peer_ip_address must be a configured peer MME IP address in IPv4/IPv6 notation with an existing MME service on system.
> peer-id peer_identifier
> Displays summarized or detailed configuration information of eNodeBs associated with specific MME peer id peer_identifier configured with an MME service on this system.
> peer_identifier must be a configured peer MME Id between 1 through 4294967295 with an existing MME service on system.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | {grep grep_options | more}
> This argument searches the output of the root command and selects the lines matching one or more patterns/options. The types of patterns are controlled by the options specified with grep_options.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view configuration information of eNodeBs associated with an MME services on this system.
> Example
> The following command displays detailed service statistics of associated eNodeBs with MME service named mme1:
> show mme-service enodeb-association full mme-service-name mme1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service session
> Displays session information of MME service(s) running on a peer or local system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show mme-service session [summary | full | counters] [all | s1-peer s1_peer_ip_address | s11-peer s11_peer_ip_address | call-id call_identifier | pdn-address pdn_ip_address] [verbose] [|{grep grep_options | more}]
> summary
> This keyword displays the summarized output of this command.
> full
> This keyword displays detailed output of this command.
> counters
> This keyword displays all counters related events and messages for an MME session running on a system.
> all
> This keyword displays information of all MME sessions running on this system.
> s1-peer s1_peer_ip_address
> Displays summarized or detailed configuration information of MME session running and filtered on the basis of IP address of a peer connected through S1 interface with an MME service configured on this system.
> s1_peer_ip_address must be a configured IP address of a peer on S1 interface in IPv4/IPv6 notation with an existing MME service on system.
> s11-peer s11_peer_ip_address
> Displays summarized or detailed configuration information of MME session running and filtered on the basis of IP address of a peer connected through S11 interface with an MME service configured on this system.
> s11_peer_ip_address must be a configured IP address of a peer on S11 interface in IPv4/IPv6 notation with an existing MME service on system.
> call-id call_identifier
> Displays summarized or detailed configuration information of MME session running and filtered on the basis of the identifier of MME calls with an MME service configured on this system.
> call_identifier must an existing call identity in eight character Hex digit format running on an MME service on system.
> pdn-address pdn_ip_address
> Displays summarized or detailed configuration information of MME session running and filtered on the basis of IP address of connected PDN(s) with an MME service configured on this system.
> s11_peer_ip_address must be a configured IP address of a peer on S11 interface in IPv4/IPv6 notation with an existing MME service on system.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | {grep grep_options | more}
> This argument searches the output of the root command and selects the lines matching one or more patterns/options. The types of patterns are controlled by the options specified with grep_options.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view session information of MME session in an MME services on this system.
> Example
> The following command displays detailed session statistics of an MME service running on a system:
> show mme-service session full
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> The following command displays detailed session counters of an MME service running on a system:
> show mme-service session counters
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show mme-service statistics
> This command displays the service statistics of an MME service specified by various criteria.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> show mme-service statistics [sctp [mme-service mme_svc_name] | s1ap [mme-service mme_svc_name| peer-id peer_identifier]| [emm-only | esm-only] [mme-service mme_svc_name| peer-id peer_identifier] [verbose] [|{grep grep_options | more}]
> emm-only
> This keyword sets the filter criteria as MME service name or peer MME identifier to display all EPS mobility management (EMM) related statistics.
> esm-only
> This keyword sets the filter criteria as MME service name or peer MME identifier to display all EPS session management (ESM) related statistics.
> s1ap
> This keyword sets the filter criteria as MME service name of peer MME identifier to display all S1-AP statistics.
> sctp
> This keyword sets the filter criteria as MME service name of peer MME identifier to display all SCTP statistics.
> mme-service mme_svc_name
> This keyword sets the filter criteria as MME service name to display all type of statistics of an MME service; i.e. EMM, ESM, SCTP, S1-AP, and SCTP.
> peer-id peer_identifier
> This keyword sets the filter criteria as identifier of MME peer to display all service statistics of an MME service; i.e. EMM, ESM, SCTP, S1-AP, and SCTP.
> verbose
> This keyword displays the comprehensive information of specific or set of arguments.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> This command is used to display the statistical information of an MME service based on various filter criteria as local MME service or peer MME related to EMM, ESM, SCTP, S1-AP, and SCTP.
> Example
> The following command displays the service session statistics of all MME service on a system related to all; i.e. EMM, ESM, SCTP, S1-AP, and SCTP:
> show mme-service statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> The following command displays the service session statistics of all MME services on a system related to S1-AP:
> show mme-service statistics s1ap
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> The following command displays the service session statistics of all MME services on a system related to EMM only:
> show mme-service statistics emm-only
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show multicast-sessions
> Shows information for multicast sessions defined by the specified keywords. Keywords described under Command Keywords below are base commands that display distinctive different types of data. Keywords described under Filter Keywords are filters that modify or filter the output of the base commands. Not all filter keywords are available for all command keywords commands. Each command keyword lists the filter keywords that it accepts.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show multicast-sessions [command_keyword][filter_keywords] [ | { grep grep_options| more }
> command_keyword
> The following keywords are base commands that each have a distinct display output. Only one Command Keyword can entered on the command line.
> debug-info { callid id | flowid id }
> Displays internal call troubleshooting information for multicast sessions defined by the specified keywords.
> callid id: Displays subscriber information for the call specified by id. The call ID must be specified as an 8-byte hexadecimal number.
> flowid id: Displays information for a specifc BCMCS flow, defined by id. The flow ID must be a hexidecimal number.
> full
> Displays all available multicast session information. The following filter keywords are valid for this command:
> active, all, callid, card-num, dormant, flowid, flowid-type, mcast-address, pcf, pdsn-service, grep, more
> summary
> Only displays a summary of multicast session information. The following commands are valid for this command:
> active, all, callid, card-num, dormant, flowid, flowid-type, mcast-address, pcf, pdsn-service, grep, more
> filter_keywords
> The following keywords are filters that modify or filter the output of the Command Keywords. Not all filters are available for all Command Keywords. Multiple Filter Keywords can be entered on a command line.
> When multiple Filter Keywords are specified, the output conforms to all of the Filter Keywords specifications.
> active
> Only display information for multicast sessions that are currently active.
> all
> If no keywords are specified before all, information for all multicast sessions is displayed. If keywords are specified before all, all information is displayed with no further options being allowed.
> callid id
> Displays multicast session information for the call specified by id. The call must be specified as an 8-byte hexadecimal number.
> card-num card_num
> The slot number of the processing card by which the subscriber session is processed. card_num is a slot number from 1 through 7 or 10 through 16.
> dormant
> Shows information for subscriber sessions that are dormant (not transmitting or receiving data).
> flowid id
> Displays information for a specific BCMCS flow, defined by id. The flow ID must be a hexadecimal number.
> flowid-type [ flow | program ]
> Displays information for multicast sessions according to the type of flow.
> flow: Shows all multicast sessions for the flow ID type “flow”.
> program: Shows all multicast sessions for the flow ID type “program”.
> mcast-address ipv4_address
> Show multicast sessions for a specific multicast address. Must be followed by the IP address of an interface, using dotted decimal notation.
> pcf ipv4_address
> Displays information for multicast sessions connected via the packet control function, defined by ipv4_address. The address must be specified using the standard IPv4 dotted decimal notation.
> pdsn-service svc_name
> Displays information for multicast session connected to the packet data service svc_name.The packet data service must have been previously configured.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Command’s Output of Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to view information about multicast sessions.
> The output of this command may be considered for part of a periodic system auditing program by verifying active and dormant sessions.
> Example
> The following command displays the all broadcast-multicast sessions active in a context/system:
> show multicast-sessions all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show network-requested-pdp-context
> Displays information for the specified network-requested PDP context.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show network-requested-pdp-context imsi imsi_value
> imsi imsi_value
> Specifies that information will be displayed for a particular International Mobile Subscriber Identity (IMSI). imsi_value is an integer value from 1 to 15 characters.
> Usage
> USe this command to display information pertaining to network-requested PDP contexts.
> Example
> The following command displays network-requested PDP context information for a subscriber with an IMSI of 123456789:
> show network-requested-pdp-context imsi 123456789
> show network-service-entity
> Displays information regarding the network service entities (NSEs) in the network.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show network-service-entity { consolidated-status | fr-config [ peer-nsei nsei] | ip-config [ nsvl { all | instance value } }
> consolidated-status
> Displays NSVC status information for all network service entities in the network. This keyword is particularly useful for troubleshooting.
> fr-config [ peer-nsei nsei]
> Displays network service configurations for NSEs using Frame Relay configurations.
> peer-nsei nsei including this optional keyword limits the display to a specific peer NSE identified with an integer of 0 to 65535.
> ip-config [ nsvl { all | instance value }
> Displays network service configurations for NSEs using IP configurations.
> Including the nsvl keyword limits the display to all or a single ( instance 0 to 3 ) network service virtual link.
> Usage
> Use this command to display NSE information pertaining to the NSVCs of the NSEs in the networks or NSEs configured for Frame Relay or IP.
> Example
> The following command displays the status of all the NSVCs for all the NSEs in the network.
> show network-service-entity consolidated-status
> show nw-reachability server
> Show the configuration for the network reachability servers for the current context.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show nw-reachability server { all | name server_name }
> all
> Show configuration information for all network reachability servers in the current context.
> name server_name
> Show configuration information for the network reachability server with the specified name.
> server_name is the name of a previously configured reachability server and must be a string from 1 through 15 characters in length.
> Usage
> Use this command to display configuration information on network reachability servers configured in the current context.
> Example
> The following command displays information on all network reachability servers in the current context:
> show nw-reachability server all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ntp
> Displays the network timing protocol associations and status.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ntp { associations | status } [ address ip_address ] [ | { grep grep_options | more } ]
> associations
> associations: displays the current NTP server associations and related statistics.
> status
> status: displays the client permeates configured and the synchronization status.
> address ip_address
> address ip_address: the IP address of a specific NTP server/client in the current context. ip_address must be specified using the standard IPv4 dotted decimal notation.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> View network timing protocol information to troubleshooting system clock issues by displaying the associations and status of the local NTP client.
> Example
> The following displays the NTP associations and status, respectively.
> show ntp associationsshow ntp status
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show orbem
> Displays the ORB element manager information and statistics for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show orbem { client { id client_name | table } | event-notif-service filters | session { id session_name | table } | status } [ | { grep grep_options | more } ]
> client { id client_name | table }
> Indicates client information is to be displayed. The keyword table is used to output to the display information on all configured clients. The keyword id is used to specify a specific client for which information is to be displayed specified as client_name.
> client_name must refer to an existing client which is found using the table keyword option.
> event-notif-service filters
> Displays information pertaining to filters configured for the ORB Notification Service.
> session { id session_name | table }
> Indicates session information is to be displayed. The keyword table is used to output to the display information on all configured clients. The keyword id is used to specify a specific session for which information is to be displayed specified as session_name.
> session_name must refer to an existing session which is found using the table keyword option.
> status
> Indicates the ORB element manage server status information is to be displayed.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Display current sessions when ORBEM system response may appear sluggish. This command is also useful in periodic verification of the server status.
> Example
> The following commands will display the information for all clients.
> show orbem client table
> The following commands display the information for the clientName and sessionID, respectively:
> show orbem client id clientName show orbem session id sessionId
> The following command displays the ORBEM server status:
> show orbem status
> The following command displays the information for all sessions:
> show orbem session table
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show patch-progress
> This command displays the status of the on-going software patch installation.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show patch-progress
> Usage
> Use this command to show the status of an on-going software patch installation.
> Important: Software Patch Upgrades are not supported in this release.
> show pdg-service
> Displays configuration information about PDIF services configured on the system.
> Product
> PDG/TTG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show pdg-service { all | name service_name }
> all
> Displays information for all configured PDG services.
> name service_name
> Displays information for the specified PDG service only.
> service_name must be the name of an existing PDG service in the current context and from 1 to 63 alpha and/or numeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Use this command to display information for PDG services.
> Example
> The following command displays available information for all active PDG services:
> show pdg-service all
> show pdg-service statistics
> Displays statistics for the PDG/TTG since the last restart or clear command. The output includes the number of each type of protocol message. For example, the output includes the various types of EAP messages.
> Product
> PDG/TTG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show pdg-service statistics [ name service_name | peer-address ipv4_address ]
> name service_name
> Displays statistics for the specified PDG service.
> service_name must from 1 to 63 alpha and/or numeric characters.
> peer-address ipv4_address
> Displays statistics for a specific subscriber with the specified WLAN IPv4 address.
> ipv4_address must be entered in standard IPv4 dotted decimal notation.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Use this command to display PDG service statistics.
> Example
> The following command displays statistics for all active PDG services:
> show pdg-service statistics
> show pdif-service
> Displays configuration information about PDIF services configured on the system.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show pdif service { all [ counters ] | name name [ counters ] | statistics [ name name | peer-address address ] } [ | { grep grep_options | more } ]
> all [ counters ]
> Displays configuration information and statistic counters for all PDIF services in the system.
> name name [ counters ]
> Displays configuration information and statistic counters for a specified PDIF service in the system. name must be from 1 to 63 alpha and/or numeric characters and an existing PDIF service.
> statistics [ name name | peer-address address ]
> name name: Displays service statistics for a specific PDIF service. name must be from 1 to 63 alpha and/or numeric characters and an existing PDIF service.
> peer-address address: Displays service statistics for a specifid peer server. address must be specified in IP v4 dotted decimal notation.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Use this command to display configuration information and statistics about PDIF services on the system.
> Example
> The following example displays configuration information about a PDIF service named pdif23:
> show pdif service name pdif23
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show pdsn-service
> Displays information on configured packet data services for the current context.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show pdsn-service { all | name pdsn_name } [ pcf-status [ address ip_address | filter [ all | icmp-monitored | no-calls | summary | up ] ] ] [ | { grep grep_options | more } ]
> all | name pdsn_name
> all: indicates information is to be displayed for all configured packet data services.
> name pdsn_name: indicates information only for the PDSN service specified is displayed. pdsn_name must be the name of an existing PDSN service in the current context and must be from 1 to 79 alpha and/or numeric characters.
> pcf-status [ address ip_address | filter [ all | icmp-monitored | no-calls | summary | up ] ]
> pcf-status: This keyword by itself lists summary information for all PCFs.
> address ip_address: Only list information for the PCF with the specified IP address. ip_address must be specified in IP v4 dotted decimal notation.
> filter: Filter the output so only the specified information is displayed. If filter is specified with no keywords summary information for all PCFs is displayed.

> • | all: Show information for all the PCFs

> • | icmp-monitored: Show information only for PCFs which are ICMP monitored

> • | no-calls: Show information only for PCFs which have no active sessions

> • | summary: Show only a summary of the status of the PCFs

> • | up: Show information only for PCFs which are alive

> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Show the PDSN service information for standard system monitoring or troubleshooting.
> Example
> The following will display the information for the sampleService and for all configured services, respectively.
> show pdsn-service allshow pdsn-service name sampleService
> show pgw-service
> Displays configuration information for PDN Gateway (P-GW) services on this system.
> Product
> P-GW
> Privilege
> Inspector
> Syntax
> show pgw-service { all | name service_name | statistics { all | name service_name } } [ | { grep grep_options | more } ]
> all
> Displays configuration information for all P-GW services configured on this system.
> name service_name
> Displays configuration information for a specific P-GW service configured on this system.
> service_name must be an existing P-GW service, and be from 1 to 63 alpha and/or numeric characters in length.
> statistics { all | name service_name }
> Displays P-GW service statistics.
> all: Displays statistics for all P-GW services on the system.
> name service_name: Displays statistics for a specific P-GW service. name must be an existing P-GW srvice and be from 1 to 63 alpha and/or numeric characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send the output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for P-GW services on this system.
> Example
> The following command displays service statistics for the P-GW service named pgw1:
> show pgw-service name pgw1
> show port
> Displays information such as statistics and information on configured ports.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show port { datalink counters [ slot/port ] | info { slot/port } [ vlan vlan_id ] | npu counters [ slot/port [ tagged | untagged | vlan tag_id ] ] | table | utilization table } [ | { grep grep_options | more } ]
> datalink counters slot/port
> Display the information for all data links or only the one specified by slot/port. slot/port must refer to a previously configured port.
> info { slot/port } [ vlan vlan_id ]
> Display detailed information for all ports within the chassis or only the one specified by slot/port. slot/port must refer to a previously configured port.
> vlan vlan_id: Display detailed information about all VLANs in the port/slot. If the optional vlan_id is not specified, it will show port information for all VLANs in slot/port.
> npu counters [ slot/port [ tagged | untagged | vlan tag_id ] ] | bound | unbound ]
> Display the information for network processing unit ports. The information for all ports is output or only the one specified by slot/port. slot/port must refer to a previously configured port.
> tagged: Display stats for all tagged packets.
> untagged: Display statistics for all untagged packets.
> vlan tag_id: Display NPU counters for a specified VLAN. tag_id must be the VLAN tag ID of a previously configured VLAN.
> bound: Displays individual and cumulative npu port counters for the bound ports within the current context. If the command is invoked the local context all of the bound ports for all contexts and cumulative counter values for all contexts is displayed.
> unbound: Displays individual and cumulative npu port counters for all unbound ports within system.
> table
> Display information on all physical ports on rear-installed interface cards.
> utilization table
> Show average port utilization in Mbps. The output is a table that lists the current utilization average, a 5 minute average, and a 15 minute average, for all enabled ports.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Display port information for troubleshooting of network communications by viewing statistics and configuration information for physical ports.
> Example
> The following displays detailed information for port 1 in slot 17:
> show port info 17/1 show port table
> The following displays information for the data link port 33/1:
> show port datalink counters 33/1 show port npu counters 33/1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show power
> Displays information about installed cards with power supplied.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show power [ all | chassis | card_num ] [ | { grep grep_options | more } ]
> all | chassis | card_num ]
> Default: chassis
> all: indicates power information for all cards is to be displayed.
> chassis: indicates the chassis power source(s) are to be displayed.
> card_num: specifies a specific card for which power information is to be displayed. card_num must be a value in the range 1 through 48.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> View power source information to quickly check the power for all cards within a chassis.
> Important: On some platforms, only show power is supported with no other keywords or variables.
> Example
> The following displays power supply status for the chassis.
> show power
> The following command displays the power status for all slots
> show power all
> show ppp
> Displays the point-to-point protocol information, detailed or summarized, for one or all connections by the use of filtering options.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ppp { [ counters | full | summary ] { all | callid call_id | imsi id | msid ms_id | username user_name } | statistics [ pcf-address [pcf_ip_addr| all ] | pdsn-service pdsn_name ] } [ | { grep grep_options | more } ]
> counters | full | summary
> Provides an optional modifier to the output for the level and type of information.
> counters: indicates the point-to-point protocol statistics are to be displayed.
> full: indicates all available information is to be displayed.
> summary: indicates only a summary of available information is to be displayed.
> all | callid call_id | imsi imsi_id | msid ms_id | username user_name }]
> all: indicates all available information is to be displayed.
> callid call_id: indicates the PPP information only for the call specified by call_id is to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> imsi id: specifies that PPP information only for the subscriber with the specified id be displayed. The IMSI (International Mobile Subscriber Identity) id is a 15 character field which identifies the subscriber’s home country and carrier.
> msid ms_id: specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> username user_name: specifies a user only for which PPP information is to be displayed where the user is specified as user_name.
> statistics [ pcf-address [ pcf_ip_addr | all ] | pdsn-service pdsn_name ]
> Statistics for all packet data services is displayed.
> pcf-address [ pcf_ip_addr | all ] : Display statistics only for the time the session is connected to the specified PCF (Packet Control Function) or for all PCFs. pcf_ip_addr must be specified using the standard IPv4 dotted decimal notation.
> pdsn-service pdsn_name: Display statistics only for the service specified by pdsn_name. pdsn_name must be from 1 to 63 alpha and/or numeric characters.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> View the Point-to-Point Protocol information to support troubleshooting subscriber connections by viewing information for point-to-point connections for a specific subscriber.
> Example
> The following displays the PPP summary for all connections.
> show ppp summary all
> The following outputs the point-to-point detailed information for the user user1.
> show ppp full username user1
> The following command displays the standard information for the call with ID FF0E11CD.
> show ppp callid ff0e11cd
> The following command displays the PPP statistics for pdsn1.
> show ppp statistics pdsn-service pdsn1
> The following command provides summarized information for the PPP statistics.
> show ppp
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show prepaid 3gpp2
> This command displays prepaid accounting information for all services or only the service specified.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> all
> This keyword displays prepaid statistics for all services.
> ggsn-service
> Display statistics for GGSN service(s).
> ha-service
> Display statistics for HA service(s).
> lns-service
> Display statistics for LNS service(s).
> pdsn-service
> Display statistics for PDSN service(s).
> { all | name service_name }
> all: Display statistics for all services of the specified type.
> name service_name: Display statistics for the service named service_name of the specified service type.
> per-service-summary
> Displays prepaid statistics per service summary for all services.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Displays Pre-paid statistics for a particular named service or for all services.
> Example
> To display statistics for a PDSN service name PDSN1, enter the following command:
> show prepaid 3gpp2 statistics pdsn-service name PDSN1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show prepaid wimax
> This command displays prepaid WiMAX accounting information for all services or only the service specified.
> Product
> ASN GW
> Privilege
> Inspector
> Syntax
> show prepaid wimax statistics { all | asngw-service { all | name service_name} | ha-service { all | name service_name} | per-service-summary } [ | { grep grep_options | more } ]
> all
> This keyword displays prepaid statistics for all services.
> asngw-service
> Displays prepaid statistics for ASN GW service(s).
> ha-service
> Displays prepaid accounting statistics for HA service(s).
> { all | name service_name }
> all: Display statistics for all services of the specified type.
> name service_name: Display statistics for the service named service_name of the specified service type.
> per-service-summary
> Displays prepaid statistics per service summary for all services.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Use this command to display prepaid WiMAX accounting statistics for named service or for all services.
> Example
> The following command displays prepaid WiMAX accounting statistics for an ASN GW service name asn1:
> show prepaid wimax statistics asngw-service name asn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show profile-id-qci-mapping
> Displays QCI-RAN mapping tables configured on this system.
> Product
> HSGW
> Privilege
> Inspector
> Syntax
> show profile-id-qci-mapping table { all | name table_name } [ | { grep grep_options | more }]
> all
> Displays information for all QCI-RAN mapping tables configured on this system.
> name table_name
> Displays information for a QCI-RAN mapping tables configured for a specific QCI-RAN table on this system.
> table_name must be an existing QCI-RAN table, and be from 1 to 63 alpha and/or numeric characters in length.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Use this command to display the contents of a specific QCI-RAN mapping table or all mapping tables configured on this system.
> Example
> The following command displays the contents of a QCI-RAN mapping table named table1:
> show profile-id-qci-mapping table name table1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883