> show hnbgw
> This chapter includes the show hnbgw command output tables.
> show hnbgw counters
> show hnbgw counters Command Output Descriptions

> Field | Description
> Number of registered UEs | The total number of User Equipment devices registered with the HNB-GW.
> Number of UEs with IuPS connection | The total number of User Equipment devices that have established a connection with the Packet Switched network.
> Number of UEs with IuCS connection | The total number of User Equipment devices that have established a connection with the Circuit Switched network
> Number of UEs with IuPS and IuCS connection | The total number of User Equipment devices that have established connections to both the Packet Switched and Circuit Switched networks.
> Number of Idle UEs | The total number of User Equipment devices that have no active connections to either the Packet Switched or Circuit Switched networks.

> ‌
> show hnbgw counters hnbgw-service
> show hnbgw counters hnbgw-serivce Command Output Descriptions

> Field | Description
> HNBGW Service | The name that identifies this HNB-GW service.
> Number of registered HNBs | The total number of HNB devices registered with this HNB-GW service.
> Number of registered UEs | The total number of User Equipment devices registered with this HNB-GW service.
> Number of UEs with IuPS connection | The total number of User Equipment devices that have a Packet Switched network connection to a SGSN via this HNB-GW service.
> Number of UEs with IuCS connection | The total number of User Equipment devices that have established a Circuit Switched network connection to a MSC via this HNB-GW service.
> Number of UEs with IuPS and IuCS connection | The total number of User Equipment devices that have established Packet Switched (SGSN) and Circuit Switched (MSC) network connections via this HNB-GW service.
> Number of Idle UEs | The total number of User Equipment devices that do not have an active connection to a Packet Switched (SGSN) or Circuit Switched (MSC) network.

> ‌
> show hnbgw counters hnbid
> show hnbgw counters hnbid Command Output Descriptions

> Field | Description
> HNB Id | The HNB device ID sent to the HNB-GW during registration.
> Number of registered UEs | The number of User Equipment devices that have registered with this HNB.
> Number of UEs with IuPS connection | The number of User Equipment devices that have established a connection to a SGSN via the Packet Switched network.
> Number of UEs with IuCS connection | The number of User Equipment devices that have established a connection to a MSC via the Circuit Switched network.
> Number of UEs with IuPS and IuCS connection | The number of User Equipment devices that have established connections to an MSC via the Circuit Switched interface and an SGSN via the Packet Switched network.
> Number of Idle UEs | The number of User Equipment devices that do not have an active connection to Packet Switched (SGSN) or Circuit Switched (MSC) networks.

> ‌
> show hnbgw-service
> show hnbgw-serivce all Command Output Descriptions

> Field | Description
> Service name | The name used to identify the HNB-GW service to the system.
> Context name | The name of the system context in which the HNB-GW service is defined.
> SCTP IP Address | The IP address used to transmit SCTP messages from HNBs to the HNB-GW.
> SCTPPort | The HNB-GW uses this port to listen for SCTP messages from HNBs.
> GTP-U Service | The defined GTP-U service name(s) associated with the HNB-GW service in a Packet Switched network instance. The GTP-U service(s) are used for GTP-U tunneling towards the HNB-GW access network.
> RTP IP Address | This is the IP address used in the RAB request by the HNB-GW as the transport layer endpoint. The HNB will send RTP data (packetized voice) to this IP address.
> RTPPort Min | The lesser of two port numbers that define the RTP port range used in the binding-id in the RAB request sent to the HNB by the HNB-GW during voice call setup.
> RTPPort Max | The greater of two port numbers that define the RTP port range used in the binding-id in the RAB request sent to the HNB by the HNB-GW during voice call setup.
> RTP MUX | Indicates if RTP multiplexing is enabled or disabled. If enabled, multiple subscriber voice packets can be multiplexed and sent as one RTP packet towards the HNB-GW. This is explicitly negotiated between the HNB and the HNB-GW during HNB Registration.
> HNBGW Initiated Ranap Reset | Indicates if the HNB-GW Initiated RANAP Reset function is enabled or disabled.
> Ranap Reset Ack Timer | The timer value, in seconds, that defines how long the HNB-GW waits for a RESET ACK message from the SGSN or MSC after transmitting a RESET message. This setting is used only if the HNBGW Initiated RANAP Reset function is enabled.
> Ranap Reset Maximum Retransmissions | Sets the maximum number of retries allowed for the HNB-GW to transmit a RANAP RESET message to the SGSN or MSC if the RESET ACK timer expires. This setting is used only if the HNBGW Initiated RANAP Reset function is enabled.
> Ranap Reset Guard Timer | The timer that the HNB-GW starts after receiving a RESET message from the core network. While this timer is running, the HNB-GW discards any new RESET messages that it receives.
> Available Radio Network PLMN | The Public Land Mobile Network ID configured for this HNB-GW service. It consists of the MCC and MNC (see below).
> MCC | The Mobile Country Code defined for use with this HNB-GW service. It consists of the first 3 digits of the Available Radio Network PLMN ID.
> MNC | The Mobile Network Code defined for use with this HNB-GW service. It consists of the last 3 digits of the Available Radio Network PLMN ID.
> RNC-Id | The Radio Network Controller ID provided to HNBs for use by the core network for this HNB-GW service. It is configured under the PLMN-ID
> Lac | The defined Location Area Identifier provided to HNBs during registration with this HNB-GW service. The LAC signifies which location area this HNBGW service belongs to, and is configured under the PLMN-ID.
> Rac | The Routing Area Identifier provided to HNBs during registration with this HNB-GW service. The RAC signifies the routing area that this HNBGW service belongs to and is configured under the PLMN-ID
> PS Network Name | The PS-network to be used for selecting the packet-switched core-network (i.e., SGSN) and its point-code.
> CS Network Name | The CS-network to be used for selecting circuit-switched core-network (i.e., MSC) and its point-code.
> Service Status | The current operating status of this HNB-GW service. If the status does not read ‘enabled’ HNB-GW functionality is not available.
> Security GW service Address | The IP address of the HNB-Security Gateway associated with this HNB-GW service. Security Gateway configurations are used when the IPsec GW is co-located with the HNB-GW service on the ASR 5000. If the services are co-located, the SeGW IP address will be used as the IPsec tunnel endpoint by HNBs.
> Crypto-template | Specifies the Crypto-Map template being used by the HNB-GW service for secure IPsec IKEv2 tunneling for the configured Iuh (HNB to HNB-GW) interface. The Crypto-Map template is used only if the HNB-GW and SeGW are co-located on the ASR 5000.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883