> show aaa group name
> show aaa group name Command Output Descriptions

> Field | Description
> Group name | The AAA server group name.
> Context | The context name.
> Diameter config:
> Authentication:
> Dictionary | The Diameter dictionary used for authentication.
> Endpoint name | The Diameter endpoint used for authentication.
> Max-transmissions | The maximum number of transmission attempts for Diameter authentication.
> Max-retries | The number of retry attempts for Diameter authentication requests.
> Request-timeout | The Diameter authentication request timeout period.
> Redirect-host-avp | Indicates whether to use just one returned AVP, or use the first returned AVP as selecting the primary host and the second returned AVP as selecting the secondary host.
> Accounting:
> Dictionary | The Diameter dictionary used for accounting.
> Endpoint name | The Diameter endpoint used for accounting.
> Max-transmissions | The maximum number of transmission attempts for Diameter accounting.
> Max-retries | The number of retry attempts for Diameter accounting requests.
> Request-timeout | The Diameter accounting request timeout period.
> Radius Config:
> Dictionary | The RADIUS dictionary.
> Strip-domain | Indicates whether the domain is stripped from the user name prior to authentication or accounting.
> Authenticator-validation | Indicates whether the MD5 authentication of RADIUS user is enabled.
> Allow authentication-down | Indicates whether the system allows subscriber sessions when RADIUS authentication is unavailable.
> Allow accounting-down | Indicates whether the system allows subscriber sessions when RADIUS accounting is unavailable.
> Attributes:
> Nas-identifier | The attribute name by which the system is identified in Access-Request messages.
> Nas-ip | The AAA interface IP address(es) used to identify the system.
> Nas-ip backup | The IP address of the secondary interface to use in the current context.
> Nexthop | The next hop IP address for this NAS IP address.
> MPLS-label | Indicates the MPLS label used for traffic from the specified RADIUS client NAS IP address.
> Authentication:
> Algorithm | The RADIUS authentication server selection algorithm for the current context.
> Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
> Max-outstanding | The maximum number of messages a AAA manager will queue.
> Max-retries | The maximum number of times communication with a AAA server is attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
> Max-transmissions | The maximum number of re-transmissions for RADIUS authentication requests.
> Timeout | The time period to wait for a response from the RADIUS server before re-sending the messages, in seconds.
> Apn-to-be-included | The APN name included for RADIUS authentication.
> Authenticate null-username | Indicates whether authentication of user names that are blank or empty is enabled.
> Probe:
> Interval | The time period between two RADIUS authentication probes.
> Timeout | The timeout period for HAGR to wait for a response for RADIUS authentication probes.
> Max-retries | The maximum number of retries for RADIUS authentication probe response.
> Keepalive:
> Interval | The time period between two keepalive access requests.
> Timeout | The time period between two keepalive access request retries.
> Retries | The number of times the keepalive access request is sent before marking the server as unreachable.
> consecutive-response | The number of consecutive authentication responses after which the server is marked as reachable.
> Username | The user name used for authentication.
> Calling-station-id | The calling station ID used for keepalive authentication.
> Password | The password used for authentication.
> Allow access-reject | Indicates whether both access-accept and access-reject are considered as success for the keepalive authentication request.
> Detect-dead-server:
> Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
> Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.
> Keepalive | Indicates whether the AAA server alive-dead detect mechanism based on sending keepalive authentication messages to all authentication servers is enabled.
> Accounting:
> Algorithm | The RADIUS accounting server selection algorithm for the current context.
> Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
> Max-outstanding | The maximum number of messages a AAA manager will queue.
> Max-retries | The maximum number of times communication with a AAA server will be attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
> Max-transmissions | The maximum number of re-transmissions for RADIUS accounting requests.
> Max-pdu-size | The maximum sized packet data unit which can be accepted/generated, in bytes.
> Interim-timeout | The timeout period for sending accounting INTERIM-UPDATE records, in seconds.
> Interim-downlink-volume | The downlink volume limit that triggers RADIUS interim accounting, in bytes.
> Interim-uplink-volume | The uplink volume limit that triggers RADIUS interim accounting, in bytes.
> Interim-total-volume | The total volume limit for RADIUS interim accounting, in bytes.
> Timeout | The time period to wait for a response from a RADIUS server before retransmitting a request.
> Remote-address | Indicates whether remote IP address lists are configured, and collection of accounting data for the addresses in those lists on a per-subscriber basis is enabled.
> Archive | Indicates whether archiving of RADIUS Accounting messages in the system after the accounting message has exhausted retries to all available RADIUS Accounting servers is enabled.
> Apn-to-be-included | The APN name included for RADIUS accounting.
> R-P originated:
> Trigger active-start | Indicates whether when an Active-Start is received from the PCF and there has been a parameter change, an R-P event occurs.
> Trigger active-handoff | Indicates whether when an Active PCF-to-PFC Handoff occurs, a single or two R-P events will occur (one for the Connection Setup, and the second for the Active-Start).
> Trigger active-stop | Indicates whether when an Active-Stop is received from the PCF, an R-P event occurs.
> Trigger policy | the overall accounting policy for R-P sessions.
> Trigger stop-start | Indicates whether a stop/start RADIUS accounting pair is sent to the RADIUS server when an applicable R-P event occurs.
> Handoff policy | The overall accounting policy for R-P sessions.
> TOD | The time of day a RADIUS event is generated for accounting.
> GTP originated:
> Trigger policy | The RADIUS accounting policy for GTP.
> MIP HA:
> Policy | The RADIUS accounting policy for Mobile IP HA calls.
> Keepalive:
> Interval | The time period between the two keepalive access requests.
> Timeout | The time period between each keepalive access request retries.
> Retries | The number of times the keepalive access request is sent before marking the server as unreachable.
> consecutive-response | The number of consecutive authentication response after which the server is marked as reachable.
> Username | The user name used for authentication.
> Calling-station-id | The calling station ID used for keepalive authentication.
> Framed-ip-address | The framed-ip-address used for keepalive accounting.
> Detect-dead-server:
> Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
> Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.
> Keepalive | Indicates whether the AAA server alive-dead detect mechanism based on sending keepalive authentication messages to all authentication servers is enabled.
> Charging:
> Auth-algorithm | The RADIUS authentication algorithm.
> Acct-algorithm | The RADIUS accounting algorithm.
> Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
> Max-outstanding | The maximum number of messages a AAA manager will queue.
> Max-retries | The maximum number of times communication with a AAA server will be attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
> Max-transmissions | The maximum number of re-transmissions for RADIUS requests.
> Timeout | The time period to wait for a response from a RADIUS server before retransmitting a request.
> Detect-dead-server:
> Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
> Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883