> CSCF Schema Statistics
> The CSCF schema provides the following types of service-level statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> CSCF Schema Statistics

> Statistic | Description | Data Type
> vpnname | VPN Name | String (Fixed Value)
> vpnid | VPN ID | Int32 (Fixed Value)
> svcname | Service Name | String (Fixed Value)
> svcid | Service ID | Int32 (Fixed Value)
> curregusers | Current Registered Users | Int32 Gauge
> failedauth | Total number of Failed Authentications. | Int64
> regexp | Total number of Registration Expires. | Int64
> total-roaming-ue-regs | Total number of Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-regs | Total number of 200 OK Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-regs | Total number of Failed Registrations from Roaming UE. | Int64
> total-roaming-ue-regs-403 | Total number of 403 responses to Registration from Roaming UE. | Int64
> total-roaming-ue-re-regs | Total number of Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-re- regs | Total number of 200 OK Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-re-regs | Total number of Failed Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-re-regs-403 | Total number of 403 responses to Re-Registration from Roaming UE. | Int64
> total-roaming-ue-de-regs | Total number of De-Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-de-regs | Total number of 200 OK De-Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-de-regs | Total number of Failed De-Registrations from Roaming UE. | Int64
> total-roaming-ue-de-regs- 403 | Total number of 403 responses to De-Registration from Roaming UE. | Int64
> de-regs-fromue | Total number of De-registrations from UE. | Int64
> de-regs-fromnw | Total number of De-registrations from Network. | Int64
> sec-regs | Total number of Secure Registrations | Int64
> fail-sec-regs | Total number of Failed Secure Registrations | Int64
> callattrx | Total number of Call Attempts received. | Int64
> callatttx | Total number of Call Attempts transmitted. | Int64
> callsuccrx | Total number of Call Success received. | Int64
> callsucctx | Total number of Call Success transmitted. | Int64
> callfailrx | Total number of Call Failures received. | Int64
> callfailtx | Total number of Call Failures transmitted. | Int64
> curcscfsess | Total number of current CSCF Sessions. | Int32 Gauge
> totalcscfsess | Total number of CSCF Sessions. | Int64
> call-resp-3xxrx | Total number of Call 3xx Responses received. | Int64
> call-resp-3xxtx | Total number of Call 3xx Responses transmitted. | Int64
> call-resp-402rx | Total number of Call 402 Responses received. | Int64
> call-resp-402tx | Total number of Call 402 Responses transmitted. | Int64
> call-resp-403rx | Total number of Call 403 Responses received. | Int64
> call-resp-403tx | Total number of Call 403 Responses transmitted. | Int64
> call-resp-404rx | Total number of Call 404 Responses received. | Int64
> call-resp-404tx | Total number of Call 404 Responses transmitted. | Int64
> call-resp-407rx | Total number of Call 407 Responses received. | Int64
> call-resp-407tx | Total number of Call 407 Responses transmitted. | Int64
> call-resp-408rx | Total number of Call 408 Responses received. | Int64
> call-resp-408tx | Total number of Call 408 Responses transmitted. | Int64
> call-resp-420rx | Total number of Call 420 Responses received. | Int64
> call-resp-420tx | Total number of Call 420 Responses transmitted. | Int64
> call-resp-421rx | Total number of Call 421 Responses received. | Int64
> call-resp-421tx | Total number of Call 421 Responses transmitted. | Int64
> call-resp-480rx | Total number of Call 480 Responses received. | Int64
> call-resp-480tx | Total number of Call 480 Responses transmitted. | Int64
> call-resp-486rx | Total number of Call 486 Responses received. | Int64
> call-resp-486tx | Total number of Call 486 Responses transmitted. | Int64
> call-resp-487rx | Total number of Call 487 Responses received. | Int64
> call-resp-487tx | Total number of Call 487 Responses transmitted. | Int64
> call-resp-488rx | Total number of Call 488 Responses received. | Int64
> call-resp-488tx | Total number of Call 488 Responses transmitted. | Int64
> call-resp-4xxrx | Total number of Call 4xx Responses received. | Int64
> call-resp-4xxtx | Total number of Call 4xx Responses transmitted. | Int64
> call-resp-500rx | Total number of Call 500 Responses received. | Int64
> call-resp-500tx | Total number of Call 500 Responses transmitted. | Int64
> call-resp-503rx | Total number of Call 503 Responses received. | Int64
> call-resp-503tx | Total number of Call 503 Responses transmitted. | Int64
> call-resp-5xxrx | Total number of Call 5xx Responses received. | Int64
> call-resp-5xxtx | Total number of Call 5xx Responses transmitted. | Int64
> call-resp-6xxrx | Total number of Call 6xx Responses received. | Int64
> call-resp-6xxtx | Total number of Call 6xx Responses transmitted. | Int64
> call-rel-attrx | Total number of Call Release Attempts received. | Int64
> call-rel-atttx | Total number of Call Release Attempts transmitted. | Int64
> call-rel-succrx | Total number of Call Release Success received. | Int64
> call-rel-succtx | Total number of Call Release Success transmitted. | Int64
> call-rel-failrx | Total number of Call Release Failures received. | Int64
> call-rel-failtx | Total number of Call Release Failures transmitted. | Int64
> reg-attrx | Total number of Registration Attempts received. | Int64
> reg-atttx | Total number of Registration Attempts transmitted. | Int64
> reg-succrx | Total number of Registration Successes received. | Int64
> reg-succtx | Total number of Registration Successes transmitted. | Int64
> reg-failrx | Total number of Registration Failures received. | Int64
> reg-failtx | Total number of Registration Failures transmitted. | Int64
> reg-resp-401rx | Total number of Registration 401 Responses received. | Int64
> reg-resp-401tx | Total number of Registration 401 Responses transmitted. | Int64
> reg-resp-403rx | Total number of Registration 403 Responses received. | Int64
> reg-resp-403tx | Total number of Registration 403 Responses transmitted. | Int64
> reg-resp-404rx | Total number of Registration 404 Responses received. | Int64
> reg-resp-404tx | Total number of Registration 404 Responses transmitted. | Int64
> reg-resp-420rx | Total number of Registration 420 Responses received. | Int64
> reg-resp-420tx | Total number of Registration 420 Responses transmitted. | Int64
> reg-resp-4xxrx | Total number of Registration 4xx Responses received. | Int64
> reg-resp-4xxtx | Total number of Registration 4xx Responses transmitted. | Int64
> reg-resp-500rx | Total number of Registration 500 Responses received. | Int64
> reg-resp-500tx | Total number of Registration 500 Responses transmitted. | Int64
> reg-resp-5xxrx | Total number of Registration 5xx Responses received. | Int64
> reg-resp-5xxtx | Total number of Registration 5xx Responses transmitted. | Int64
> reg-resp-6xxrx | Total number of Registration 6xx Responses received. | Int64
> reg-resp-6xxtx | Total number of Registration 6xx Responses transmitted. | Int64
> rereg-attrx | Total number of Refresh Registration Attempts received. | Int64
> rereg-atttx | Total number of Refresh Registration Attempts transmitted. | Int64
> rereg-succrx | Total Refresh Registration Successes received. | Int64
> rereg-succtx | Total number of Refresh Registration Successes transmitted. | Int64
> rereg-failrx | Total number of Refresh Registration Failures received. | Int64
> rereg-failtx | Total number of Refresh Registration Failures transmitted. | Int64
> rereg-resp-401rx | Total number of Refresh Registration 401 Responses received. | Int64
> rereg-resp-401tx | Total number of Refresh Registration 401 Responses transmitted. | Int64
> rereg-resp-403rx | Total number of Refresh Registration 403 Responses received. | Int64
> rereg-resp-403tx | Total number of Refresh Registration 403 Responses transmitted. | Int64
> rereg-resp-404rx | Total number of Refresh Registration 404 Responses received. | Int64
> rereg-resp-404tx | Total number of Refresh Registration 404 Responses transmitted. | Int64
> rereg-resp-420rx | Total number of Refresh Registration 420 Responses received. | Int64
> rereg-resp-420tx | Total number of Refresh Registration 420 Responses transmitted. | Int64
> rereg-resp-4xxrx | Total number of Refresh Registration 4xx Responses received. | Int64
> rereg-resp-4xxtx | Total number of Refresh Registration 4xx Responses transmitted. | Int64
> rereg-resp-500rx | Total number of Refresh Registration 500 Responses received. | Int64
> rereg-resp-500tx | Total number of Refresh Registration 500 Responses transmitted. | Int64
> rereg-resp-5xxrx | Total number of Refresh Registration 5xx Responses received. | Int64
> rereg-resp-5xxtx | Total number of Refresh Registration 5xx Responses transmitted. | Int64
> rereg-resp-6xxrx | Total number of Refresh Registration 6xx Responses received. | Int64
> rereg-resp-6xxtx | Total number of Refresh Registration 6xx Responses transmitted. | Int64
> dereg-attrx | Total number of Deregistration Attempts received. | Int64
> dereg-atttx | Total number of Deregistration Attempts transmitted. | Int64
> dereg-succrx | Total number of Deregistration Successes received. | Int64
> dereg-succtx | Total number of Deregistration Successes transmitted. | Int64
> dereg-failrx | Total number of Deregistration Failures received. | Int64
> dereg-failtx | Total number of Deregistration Failures transmitted. | Int64
> dereg-resp-401rx | Total number of Deregister 401 Responses received. | Int64
> dereg-resp-401tx | Total number of Deregister 401 Responses transmitted. | Int64
> dereg-resp-403rx | Total number of Deregister 403 Responses received. | Int64
> dereg-resp-403tx | Total number of Deregister 403 Responses transmitted. | Int64
> dereg-resp-404rx | Total number of Deregister 404 Responses received. | Int64
> dereg-resp-404tx | Total number of Deregister 404 Responses transmitted. | Int64
> dereg-resp-420rx | Total number of Deregister 420 Responses received. | Int64
> dereg-resp-420tx | Total number of Deregister 420 Responses transmitted. | Int64
> dereg-resp-4xxrx | Total number of Deregister 4xx Responses received. | Int64
> dereg-resp-4xxtx | Total number of Deregister 4xx Responses transmitted. | Int64
> dereg-resp-500rx | Total number of Deregister 500 Responses received. | Int64
> dereg-resp-500tx | Total number of Deregister 500 Responses transmitted. | Int64
> dereg-resp-5xxrx | Total number of Deregister 5xx Responses received. | Int64
> dereg-resp-5xxtx | Total number of Deregister 5xx Responses transmitted. | Int64
> dereg-resp-6xxrx | Total number of Deregister 6xx Responses received. | Int64
> dereg-resp-6xxtx | Total number of Deregister 6xx Responses transmitted. | Int64
> subscribe-attempt-rx | Total number of Subscribe Attempts Received | Int64
> subscribe-attempt-tx | Total number of Subscribe Attempts Transmitted | Int64
> subscribe-success-rx | Total number of Subscribe Success Received | Int64
> subscribe-success-tx | Total number of Subscribe Success Transmitted | Int64
> subscribe-failure-rx | Total number of Subscribe Failure Received | Int64
> subscribe-failure-tx | Total number of Subscribe Failure Transmitted | Int64
> notify-attempt-rx | Total number of Notify Attempts Received | Int64
> notify-attempt-tx | Total number of Notify Attempts Transmitted | Int64
> notify-success-rx | Total number of Notify Success Received | Int64
> notify-success-tx | Total number of Notify Success Transmitted | Int64
> notify-failure-rx | Total number of Notify Failure Received | Int64
> notify-failure-tx | Total number of Notify Failure Transmitted | Int64
> publish-attempt-rx | Total number of Publish Attempts Received | Int64
> publish-attempt-tx | Total number of Publish Attempts Transmitted | Int64
> publish-success-rx | Total number of Publish Success Received | Int64
> publish-success-tx | Total number of Publish Success Transmitted | Int64
> publish-failure-rx | Total number of Publish Failure Received | Int64
> publish-failure-tx | Total number of Publish Failure Transmitted | Int64
> msgsum-subs-attrx | Total number of “msg-summary” Subscription Attempts received. | Int64
> msgsum-subs-atttx | Total number of “msg-summary” Subscription Attempts transmitted. | Int64
> msgsum-subs-succrx | Total number of “msg-summary” Subscription Successes received. | Int64
> msgsum-subs-succtx | Total number of “msg-summary” Subscription Successes transmitted. | Int64
> msgsum-subs-failrx | Total number of “msg-summary” Subscription Failures received. | Int64
> msgsum-subs-failtx | Total number of “msg-summary” Subscription Failures transmitted. | Int64
> msgsum-subs-resp-200rx | Total number of “msg-summary” Subscription 200 Responses received. | Int64
> msgsum-subs-resp-200tx | Total number of “msg-summary” Subscription 200 Responses transmitted. | Int64
> msgsum-subs-resp-202rx | Total number of “msg-summary” Subscription 202 Responses received. | Int64
> msgsum-subs-resp-202tx | Total number of “msg-summary” Subscription 202 Responses transmitted. | Int64
> msgsum-subs-resp-400rx | Total number of “msg-summary” Subscription 400 Responses received. | Int64
> msgsum-subs-resp-400tx | Total number of “msg-summary” Subscription 400 Responses transmitted. | Int64
> msgsum-subs-resp-403rx | Total number of “msg-summary” Subscription 403 Responses received. | Int64
> msgsum-subs-resp-403tx | Total number of “msg-summary” Subscription 403 Responses transmitted. | Int64
> msgsum-subs-resp-481rx | Total number of “msg-summary” Subscription 481 Responses received. | Int64
> msgsum-subs-resp-481tx | Total number of “msg-summary” Subscription 481 Responses transmitted. | Int64
> msgsum-subs-resp-489rx | Total number of “msg-summary” Subscription 489 Responses received. | Int64
> msgsum-subs-resp-489tx | Total number of “msg-summary” Subscription 489 Responses transmitted. | Int64
> msgsum-subs-resp-500rx | Total number of “msg-summary” Subscription 500 Responses received. | Int64
> msgsum-subs-resp-500tx | Total number of “msg-summary” Subscription 500 Responses transmitted. | Int64
> msgsum-subs-resp-3xxrx | Total number of “msg-summary” Subscription 3XX Responses received. | Int64
> msgsum-subs-resp-3xxtx | Total number of “msg-summary” Subscription 3XX Responses transmitted. | Int64
> msgsum-subs-resp-4xxrx | Total number of “msg-summary” Subscription 4XX Responses received. | Int64
> msgsum-subs-resp-4xxtx | Total number of “msg-summary” Subscription 4XX Responses transmitted. | Int64
> msgsum-subs-resp-5xxrx | Total number of “msg-summary” Subscription 5XX Responses received. | Int64
> msgsum-subs-resp-5xxtx | Total number of “msg-summary” Subscription 5XX Responses transmitted. | Int64
> msgsum-subs-resp-6xxrx | Total number of “msg-summary” Subscription 6XX Responses received. | Int64
> msgsum-subs-resp-6xxtx | Total number of “msg-summary” Subscription 6XX Responses transmitted. | Int64
> msgsum-resubs-attrx | Total number of “msg-summary” Refresh Subscription Attempts received. | Int64
> msgsum-resubs-atttx | Total number of “msg-summary” Refresh Subscription Attempts transmitted. | Int64
> msgsum-resubs-succrx | Total number of “msg-summary” Refresh Subscription Successes received. | Int64
> msgsum-resubs-succtx | Total number of “msg-summary” Refresh Subscription Successes transmitted. | Int64
> msgsum-resubs-failrx | Total number of “msg-summary” Refresh Subscription Failures received. | Int64
> msgsum-resubs-failtx | Total number of “msg-summary” Refresh Subscription Failures transmitted. | Int64
> msgsum-resubs-resp-200rx | Total number of “msg-summary” Refresh Subscription 200 Responses received. | Int64
> msgsum-resubs-resp-200tx | Total number of “msg-summary” Refresh Subscription 200 Responses transmitted. | Int64
> msgsum-resubs-resp-202rx | Total number of “msg-summary” Refresh Subscription 202 Responses received. | Int64
> msgsum-resubs-resp-202tx | Total number of “msg-summary” Refresh Subscription 202 Responses transmitted. | Int64
> msgsum-resubs-resp-400rx | Total number of “msg-summary” Refresh Subscription 400 Responses received. | Int64
> msgsum-resubs-resp-400tx | Total number of “msg-summary” Refresh Subscription 400 Responses transmitted. | Int64
> msgsum-resubs-resp-403rx | Total number of “msg-summary” Refresh Subscription 403 Responses received. | Int64
> msgsum-resubs-resp-403tx | Total number of “msg-summary” Refresh Subscription 403 Responses transmitted. | Int64
> msgsum-resubs-resp-481rx | Total number of “msg-summary” Refresh Subscription 481 Responses received. | Int64
> msgsum-resubs-resp-481tx | Total number of “msg-summary” Refresh Subscription 481 Responses transmitted. | Int64
> msgsum-resubs-resp-489rx | Total number of “msg-summary” Refresh Subscription 489 Responses received. | Int64
> msgsum-resubs-resp-489tx | Total number of “msg-summary” Refresh Subscription 489 Responses transmitted. | Int64
> msgsum-resubs-resp-500rx | Total number of “msg-summary” Refresh Subscription 500 Responses received. | Int64
> msgsum-resubs-resp-500tx | Total number of “msg-summary” Refresh Subscription 500 Responses transmitted. | Int64
> msgsum-resubs-resp-3xxrx | Total number of “msg-summary” Refresh Subscription 3XX Responses received. | Int64
> msgsum-resubs-resp-3xxtx | Total number of “msg-summary” Refresh Subscription 3XX Responses transmitted. | Int64
> msgsum-resubs-resp-4xxrx | Total number of “msg-summary” Refresh Subscription 4XX Responses received. | Int64
> msgsum-resubs-resp-4xxtx | Total number of “msg-summary” Refresh Subscription 4XX Responses transmitted. | Int64
> msgsum-resubs-resp-5xxrx | Total number of “msg-summary” Refresh Subscription 5XX Responses received. | Int64
> msgsum-resubs-resp-5xxtx | Total number of “msg-summary” Refresh Subscription 5XX Responses transmitted. | Int64
> msgsum-resubs-resp-6xxrx | Total number of “msg-summary” Refresh Subscription 6XX Responses received. | Int64
> msgsum-resubs-resp-6xxtx | Total number of “msg-summary” Refresh Subscription 6XX Responses transmitted. | Int64
> msgsum-unsubs-attrx | Total number of “msg-summary” Un-Subscription Attempts received. | Int64
> msgsum-unsubs-atttx | Total number of “msg-summary” Un-Subscription Attempts transmitted. | Int64
> msgsum-unsubs-succrx | Total number of “msg-summary” Un-Subscription Successes received. | Int64
> msgsum-unsubs-succtx | Total number of “msg-summary” Un-Subscription Successes transmitted. | Int64
> msgsum-unsubs-failrx | Total number of “msg-summary” Un-Subscription Failures received. | Int64
> msgsum-unsubs-failtx | Total number of “msg-summary” Un-Subscription Failures transmitted. | Int64
> msgsum-unsubs-resp-200rx | Total number of “msg-summary” Un-Subscription 200 Responses received. | Int64
> msgsum-unsubs-resp-200tx | Total number of “msg-summary” Un-Subscription 200 Responses transmitted. | Int64
> msgsum-unsubs-resp-202rx | Total number of “msg-summary” Un-Subscription 202 Responses received. | Int64
> msgsum-unsubs-resp-202tx | Total number of “msg-summary” Un-Subscription 202 Responses transmitted. | Int64
> msgsum-unsubs-resp-400rx | Total number of “msg-summary” Un-Subscription 400 Responses received. | Int64
> msgsum-unsubs-resp-400tx | Total number of “msg-summary” Un-Subscription 400 Responses transmitted. | Int64
> msgsum-unsubs-resp-403rx | Total number of “msg-summary” Un-Subscription 403 Responses received. | Int64
> msgsum-unsubs-resp-403tx | Total number of “msg-summary” Un-Subscription 403 Responses transmitted. | Int64
> msgsum-unsubs-resp-481rx | Total number of “msg-summary” Un-Subscription 481 Responses received. | Int64
> msgsum-unsubs-resp-481tx | Total number of “msg-summary” Un-Subscription 481 Responses transmitted. | Int64
> msgsum-unsubs-resp-489rx | Total number of “msg-summary” Un-Subscription 489 Responses received. | Int64
> msgsum-unsubs-resp-489tx | Total number of “msg-summary” Un-Subscription 489 Responses transmitted. | Int64
> msgsum-unsubs-resp-500rx | Total number of “msg-summary” Un-Subscription 500 Responses received. | Int64
> msgsum-unsubs-resp-500tx | Total number of “msg-summary” Un-Subscription 500 Responses transmitted. | Int64
> msgsum-unsubs-resp-3xxrx | Total number of “msg-summary” Un-Subscription 3XX Responses received. | Int64
> msgsum-unsubs-resp-3xxtx | Total number of “msg-summary” Un-Subscription 3XX Responses transmitted. | Int64
> msgsum-unsubs-resp-4xxrx | Total number of “msg-summary” Un-Subscription 4XX Responses received. | Int64
> msgsum-unsubs-resp-4xxtx | Total number of “msg-summary” Un-Subscription 4XX Responses transmitted. | Int64
> msgsum-unsubs-resp-5xxrx | Total number of “msg-summary” Un-Subscription 5XX Responses received. | Int64
> msgsum-unsubs-resp-5xxtx | Total number of “msg-summary” Un-Subscription 5XX Responses transmitted. | Int64
> msgsum-unsubs-resp-6xxrx | Total number of “msg-summary” Un-Subscription 6XX Responses received. | Int64
> msgsum-unsubs-resp-6xxtx | Total number of “msg-summary” Un-Subscription 6XX Responses transmitted. | Int64
> msgsum-notify-attrx | Total number of “msg-summary” Notify Attempts received. | Int64
> msgsum-notify-atttx | Total number of “msg-summary” Notify Attempts transmitted. | Int64
> msgsum-notify-succrx | Total number of “msg-summary” Notify Successes received. | Int64
> msgsum-notify-succtx | Total number of “msg-summary” Notify Successes transmitted. | Int64
> msgsum-notify-failrx | Total number of “msg-summary” Notify Failures received. | Int64
> msgsum-notify-failtx | Total number of “msg-summary” Notify Failures transmitted. | Int64
> msgsum-notify-resp-3xxrx | Total number of “msg-summary” Notify 3XX Responses received. | Int64
> msgsum-notify-resp-3xxtx | Total number of “msg-summary” Notify 3XX Responses transmitted. | Int64
> msgsum-notify-resp-400rx | Total number of “msg-summary” Notify 400 Responses received. | Int64
> msgsum-notify-resp-400tx | Total number of “msg-summary” Notify 400 Responses transmitted. | Int64
> msgsum-notify-resp-481rx | Total number of “msg-summary” Notify 481 Responses received. | Int64
> msgsum-notify-resp-481tx | Total number of “msg-summary” Notify 481 Responses transmitted. | Int64
> msgsum-notify-resp-489rx | Total number of “msg-summary” Notify 489 Responses received. | Int64
> msgsum-notify-resp-489tx | Total number of “msg-summary” Notify 489 Responses transmitted. | Int64
> msgsum-notify-resp-4xxrx | Total number of “msg-summary” Notify 4XX Responses received. | Int64
> msgsum-notify-resp-4xxtx | Total number of “msg-summary” Notify 4XX Responses transmitted. | Int64
> msgsum-notify-resp-500rx | Total number of “msg-summary” Notify 500 Responses received. | Int64
> msgsum-notify-resp-500tx | Total number of “msg-summary” Notify 500 Responses transmitted. | Int64
> msgsum-notify-resp-5xxrx | Total number of “msg-summary” Notify 5XX Responses received. | Int64
> msgsum-notify-resp-5xxtx | Total number of “msg-summary” Notify 5XX Responses transmitted. | Int64
> msgsum-notify-resp-6xxrx | Total number of “msg-summary” Notify 6XX Responses received. | Int64
> msgsum-notify-resp-6xxtx | Total number of “msg-summary” Notify 6XX Responses transmitted. | Int64
> msgsum-pub-attrx | Total number of “msg-summary” Publish Attempts received. | Int64
> msgsum-pub-atttx | Total number of “msg-summary” Publish Attempts transmitted. | Int64
> msgsum-pub-succrx | Total number of “msg-summary” Publish Successes received. | Int64
> msgsum-pub-succtx | Total number of “msg-summary” Publish Successes transmitted. | Int64
> msgsum-pub-failrx | Total number of “msg-summary” Publish Failures received. | Int64
> msgsum-pub-failtx | Total number of “msg-summary” Publish Failures transmitted. | Int64
> msgsum-pub-resp-3xxrx | Total number of “msg-summary” Publish 3XX Responses received. | Int64
> msgsum-pub-resp-3xxtx | Total number of “msg-summary” Publish 3XX Responses transmitted. | Int64
> msgsum-pub-resp-400rx | Total number of “msg-summary” Publish 400 Responses received. | Int64
> msgsum-pub-resp-400tx | Total number of “msg-summary” Publish 400 Responses transmitted. | Int64
> msgsum-pub-resp-404rx | Total number of “msg-summary” Publish 404 Responses received. | Int64
> msgsum-pub-resp-404tx | Total number of “msg-summary” Publish 404 Responses transmitted. | Int64
> msgsum-pub-resp-412rx | Total number of “msg-summary” Publish 412 Responses received. | Int64
> msgsum-pub-resp-412tx | Total number of “msg-summary” Publish 412 Responses transmitted. | Int64
> msgsum-pub-resp-423rx | Total number of “msg-summary” Publish 423 Responses received. | Int64
> msgsum-pub-resp-423tx | Total number of “msg-summary” Publish 423 Responses transmitted. | Int64
> msgsum-pub-resp-489rx | Total number of “msg-summary” Publish 489 Responses received. | Int64
> msgsum-pub-resp-489tx | Total number of “msg-summary” Publish 489 Responses transmitted. | Int64
> msgsum-pub-resp-4xxrx | Total number of “msg-summary” Publish 4XX Responses received. | Int64
> msgsum-pub-resp-4xxtx | Total number of “msg-summary” Publish 4XX Responses transmitted. | Int64
> msgsum-pub-resp-500rx | Total number of “msg-summary” Publish 500 Responses received. | Int64
> msgsum-pub-resp-500tx | Total number of “msg-summary” Publish 500 Responses transmitted. | Int64
> msgsum-pub-resp-503rx | Total number of “msg-summary” Publish 503 Responses received. | Int64
> msgsum-pub-resp-503tx | Total number of “msg-summary” Publish 503 Responses transmitted. | Int64
> msgsum-pub-resp-5xxrx | Total number of “msg-summary” Publish 5XX Responses received. | Int64
> msgsum-pub-resp-5xxtx | Total number of “msg-summary” Publish 5XX Responses transmitted. | Int64
> msgsum-pub-resp-6xxrx | Total number of “msg-summary” Publish 6XX Responses received. | Int64
> msgsum-pub-resp-6xxtx | Total number of “msg-summary” Publish 6XX Responses transmitted. | Int64
> msgsum-unpub-attrx | Total number of “msg-summary” Un-Publish Attempts received. | Int64
> msgsum-unpub-atttx | Total number of “msg-summary” Un-Publish Attempts transmitted. | Int64
> msgsum-unpub-succrx | Total number of “msg-summary” Un-Publish Successes received. | Int64
> msgsum-unpub-succtx | Total number of “msg-summary” Un-Publish Successes transmitted. | Int64
> msgsum-unpub-failrx | Total number of “msg-summary” Un-Publish Failures received. | Int64
> msgsum-unpub-failtx | Total number of “msg-summary” Un-Publish Failures transmitted. | Int64
> msgsum-unpub-resp-3xxrx | Total number of “msg-summary” Un-Publish 3XX Responses received. | Int64
> msgsum-unpub-resp-3xxtx | Total number of “msg-summary” Un-Publish 3XX Responses transmitted. | Int64
> msgsum-unpub-resp-400rx | Total number of “msg-summary” Un-Publish 400 Responses received. | Int64
> msgsum-unpub-resp-400tx | Total number of “msg-summary” Un-Publish 400 Responses transmitted. | Int64
> msgsum-unpub-resp-404rx | Total number of “msg-summary” Un-Publish 404 Responses received. | Int64
> msgsum-unpub-resp-404tx | Total number of “msg-summary” Un-Publish 404 Responses transmitted. | Int64
> msgsum-unpub-resp-412rx | Total number of “msg-summary” Un-Publish 412 Responses received. | Int64
> msgsum-unpub-resp-412tx | Total number of “msg-summary” Un-Publish 412 Responses transmitted. | Int64
> msgsum-unpub-resp-423rx | Total number of “msg-summary” Un-Publish 423 Responses received. | Int64
> msgsum-unpub-resp-423tx | Total number of “msg-summary” Un-Publish 423 Responses transmitted. | Int64
> msgsum-unpub-resp-489rx | Total number of “msg-summary” Un-Publish 489 Responses received. | Int64
> msgsum-unpub-resp-489tx | Total number of “msg-summary” Un-Publish 489 Responses transmitted. | Int64
> msgsum-unpub-resp-4xxrx | Total number of “msg-summary” Un-Publish 4XX Responses received. | Int64
> msgsum-unpub-resp-4xxtx | Total number of “msg-summary” Un-Publish 4XX Responses transmitted. | Int64
> msgsum-unpub-resp-500rx | Total number of “msg-summary” Un-Publish 500 Responses received. | Int64
> msgsum-unpub-resp-500tx | Total number of “msg-summary” Un-Publish 500 Responses transmitted. | Int64
> msgsum-unpub-resp-503rx | Total number of “msg-summary” Un-Publish 503 Responses received. | Int64
> msgsum-unpub-resp-503tx | Total number of “msg-summary” Un-Publish 503 Responses transmitted. | Int64
> msgsum-unpub-resp-5xxrx | Total number of “msg-summary” Un-Publish 5XX Responses received. | Int64
> msgsum-unpub-resp-5xxtx | Total number of “msg-summary” Un-Publish 5XX Responses transmitted. | Int64
> msgsum-unpub-resp-6xxrx | Total number of “msg-summary” Un-Publish 6XX Responses received. | Int64
> msgsum-unpub-resp-6xxtx | Total number of “msg-summary” Un-Publish 6XX Responses transmitted. | Int64
> pres-subs-attrx | Total number of “presence” Subscription Attempts received. | Int64
> pres-subs-atttx | Total number of “presence” Subscription Attempts transmitted. | Int64
> pres-subs-succrx | Total number of “presence” Subscription Successes received. | Int64
> pres-subs-succtx | Total number of “presence” Subscription Successes transmitted. | Int64
> pres-subs-failrx | Total number of “presence” Subscription Failures received. | Int64
> pres-subs-failtx | Total number of “presence” Subscription Failures transmitted. | Int64
> pres-subs-resp-200rx | Total number of “presence” Subscription 200 Responses received. | Int64
> pres-subs-resp-200tx | Total number of “presence” Subscription 200 Responses transmitted. | Int64
> pres-subs-resp-202rx | Total number of “presence” Subscription 202 Responses received. | Int64
> pres-subs-resp-202tx | Total number of “presence” Subscription 202 Responses transmitted. | Int64
> pres-subs-resp-400rx | Total number of “presence” Subscription 400 Responses received. | Int64
> pres-subs-resp-400tx | Total number of “presence” Subscription 400 Responses transmitted. | Int64
> pres-subs-resp-403rx | Total number of “presence” Subscription 403 Responses received. | Int64
> pres-subs-resp-403tx | Total number of “presence” Subscription 403 Responses transmitted. | Int64
> pres-subs-resp-481rx | Total number of “presence” Subscription 481 Responses received. | Int64
> pres-subs-resp-481tx | Total number of “presence” Subscription 481 Responses transmitted. | Int64
> pres-subs-resp-489rx | Total number of “presence” Subscription 489 Responses received. | Int64
> pres-subs-resp-489tx | Total number of “presence” Subscription 489 Responses transmitted. | Int64
> pres-subs-resp-500rx | Total number of “presence” Subscription 500 Responses received. | Int64
> pres-subs-resp-500tx | Total number of “presence” Subscription 500 Responses transmitted. | Int64
> pres-subs-resp-3xxrx | Total number of “presence” Subscription 3XX Responses received. | Int64
> pres-subs-resp-3xxtx | Total number of “presence” Subscription 3XX Responses transmitted. | Int64
> pres-subs-resp-4xxrx | Total number of “presence” Subscription 4XX Responses received. | Int64
> pres-subs-resp-4xxtx | Total number of “presence” Subscription 4XX Responses transmitted. | Int64
> pres-subs-resp-5xxrx | Total number of “presence” Subscription 5XX Responses received. | Int64
> pres-subs-resp-5xxtx | Total number of “presence” Subscription 5XX Responses transmitted. | Int64
> pres-subs-resp-6xxrx | Total number of “presence” Subscription 6XX Responses received. | Int64
> pres-subs-resp-6xxtx | Total number of “presence” Subscription 6XX Responses transmitted. | Int64
> pres-resubs-attrx | Total number of “presence” Refresh Subscription Attempts received. | Int64
> pres-resubs-atttx | Total number of “presence” Refresh Subscription Attempts transmitted. | Int64
> pres-resubs-succrx | Total number of “presence” Refresh Subscription Successes received. | Int64
> pres-resubs-succtx | Total number of “presence” Refresh Subscription Successes transmitted. | Int64
> pres-resubs-failrx | Total number of “presence” Refresh Subscription Failures received. | Int64
> pres-resubs-failtx | Total number of “presence” Refresh Subscription Failures transmitted. | Int64
> pres-resubs-resp-200rx | Total number of “presence” Refresh Subscription 200 Responses received. | Int64
> pres-resubs-resp-200tx | Total number of “presence” Refresh Subscription 200 Responses transmitted. | Int64
> pres-resubs-resp-202rx | Total number of “presence” Refresh Subscription 202 Responses received. | Int64
> pres-resubs-resp-202tx | Total number of “presence” Refresh Subscription 202 Responses transmitted. | Int64
> pres-resubs-resp-400rx | Total number of “presence” Refresh Subscription 400 Responses received. | Int64
> pres-resubs-resp-400tx | Total number of “presence” Refresh Subscription 400 Responses transmitted. | Int64
> pres-resubs-resp-403rx | Total number of “presence” Refresh Subscription 403 Responses received. | Int64
> pres-resubs-resp-403tx | Total number of “presence” Refresh Subscription 403 Responses transmitted. | Int64
> pres-resubs-resp-481rx | Total number of “presence” Refresh Subscription 481 Responses received. | Int64
> pres-resubs-resp-481tx | Total number of “presence” Refresh Subscription 481 Responses transmitted. | Int64
> pres-resubs-resp-489rx | Total number of “presence” Refresh Subscription 489 Responses received. | Int64
> pres-resubs-resp-489tx | Total number of “presence” Refresh Subscription 489 Responses transmitted. | Int64
> pres-resubs-resp-500rx | Total number of “presence” Refresh Subscription 500 Responses received. | Int64
> pres-resubs-resp-500tx | Total number of “presence” Refresh Subscription 500 Responses transmitted. | Int64
> pres-resubs-resp-3xxrx | Total number of “presence” Refresh Subscription 3XX Responses received. | Int64
> pres-resubs-resp-3xxtx | Total number of “presence” Refresh Subscription 3XX Responses transmitted. | Int64
> pres-resubs-resp-4xxrx | Total number of “presence” Refresh Subscription 4XX Responses received. | Int64
> pres-resubs-resp-4xxtx | Total number of “presence” Refresh Subscription 4XX Responses transmitted. | Int64
> pres-resubs-resp-5xxrx | Total number of “presence” Refresh Subscription 5XX Responses received. | Int64
> pres-resubs-resp-5xxtx | Total number of “presence” Refresh Subscription 5XX Responses transmitted. | Int64
> pres-resubs-resp-6xxrx | Total number of “presence” Refresh Subscription 6XX Responses received. | Int64
> pres-resubs-resp-6xxtx | Total number of “presence” Refresh Subscription 6XX Responses transmitted. | Int64
> pres-unsubs-attrx | Total number of “presence” Un-Subscription Attempts received. | Int64
> pres-unsubs-atttx | Total number of “presence” Un-Subscription Attempts transmitted. | Int64
> pres-unsubs-succrx | Total number of “presence” Un-Subscription Successes received. | Int64
> pres-unsubs-succtx | Total number of “presence” Un-Subscription Successes transmitted. | Int64
> pres-unsubs-failrx | Total number of “presence” Un-Subscription Failures received. | Int64
> pres-unsubs-failtx | Total number of “presence” Un-Subscription Failures transmitted. | Int64
> pres-unsubs-resp-200rx | Total number of “presence” Un-Subscription 200 Responses received. | Int64
> pres-unsubs-resp-200tx | Total number of “presence” Un-Subscription 200 Responses transmitted. | Int64
> pres-unsubs-resp-202rx | Total number of “presence” Un-Subscription 202 Responses received. | Int64
> pres-unsubs-resp-202tx | Total number of “presence” Un-Subscription 202 Responses transmitted. | Int64
> pres-unsubs-resp-400rx | Total number of “presence” Un-Subscription 400 Responses received. | Int64
> pres-unsubs-resp-400tx | Total number of “presence” Un-Subscription 400 Responses transmitted. | Int64
> pres-unsubs-resp-403rx | Total number of “presence” Un-Subscription 403 Responses received. | Int64
> pres-unsubs-resp-403tx | Total number of “presence” Un-Subscription 403 Responses transmitted. | Int64
> pres-unsubs-resp-481rx | Total number of “presence” Un-Subscription 481 Responses received. | Int64
> pres-unsubs-resp-481tx | Total number of “presence” Un-Subscription 481 Responses transmitted. | Int64
> pres-unsubs-resp-489rx | Total number of “presence” Un-Subscription 489 Responses received. | Int64
> pres-unsubs-resp-489tx | Total number of “presence” Un-Subscription 489 Responses transmitted. | Int64
> pres-unsubs-resp-500rx | Total number of “presence” Un-Subscription 500 Responses received. | Int64
> pres-unsubs-resp-500tx | Total number of “presence” Un-Subscription 500 Responses transmitted. | Int64
> pres-unsubs-resp-3xxrx | Total number of “presence” Un-Subscription 3XX Responses received. | Int64
> pres-unsubs-resp-3xxtx | Total number of “presence” Un-Subscription 3XX Responses transmitted. | Int64
> pres-unsubs-resp-4xxrx | Total number of “presence” Un-Subscription 4XX Responses received. | Int64
> pres-unsubs-resp-4xxtx | Total number of “presence” Un-Subscription 4XX Responses transmitted. | Int64
> pres-unsubs-resp-5xxrx | Total number of “presence” Un-Subscription 5XX Responses received. | Int64
> pres-unsubs-resp-5xxtx | Total number of “presence” Un-Subscription 5XX Responses transmitted. | Int64
> pres-unsubs-resp-6xxrx | Total number of “presence” Un-Subscription 6XX Responses received. | Int64
> pres-unsubs-resp-6xxtx | Total number of “presence” Un-Subscription 6XX Responses transmitted. | Int64
> pres-notify-attrx | Total number of “presence” Notify Attempts received. | Int64
> pres-notify-atttx | Total number of “presence” Notify Attempts transmitted. | Int64
> pres-notify-succrx | Total number of “presence” Notify Successes received. | Int64
> pres-notify-succtx | Total number of “presence” Notify Successes transmitted. | Int64
> pres-notify-failrx | Total number of “presence” Notify Failures received. | Int64
> pres-notify-failtx | Total number of “presence” Notify Failures transmitted. | Int64
> pres-notify-resp-3xxrx | Total number of “presence” Notify 3XX Responses received. | Int64
> pres-notify-resp-3xxtx | Total number of “presence” Notify 3XX Responses transmitted. | Int64
> pres-notify-resp-400rx | Total number of “presence” Notify 400 Responses received. | Int64
> pres-notify-resp-400tx | Total number of “presence” Notify 400 Responses transmitted. | Int64
> pres-notify-resp-481rx | Total number of “presence” Notify 481 Responses received. | Int64
> pres-notify-resp-481tx | Total number of “presence” Notify 481 Responses transmitted. | Int64
> pres-notify-resp-489rx | Total number of “presence” Notify 489 Responses received. | Int64
> pres-notify-resp-489tx | Total number of “presence” Notify 489 Responses transmitted. | Int64
> pres-notify-resp-4xxrx | Total number of “presence” Notify 4XX Responses received. | Int64
> pres-notify-resp-4xxtx | Total number of “presence” Notify 4XX Responses transmitted. | Int64
> pres-notify-resp-500rx | Total number of “presence” Notify 500 Responses received. | Int64
> pres-notify-resp-500tx | Total number of “presence” Notify 500 Responses transmitted. | Int64
> pres-notify-resp-5xxrx | Total number of “presence” Notify 5XX Responses received. | Int64
> pres-notify-resp-5xxtx | Total number of “presence” Notify 5XX Responses transmitted. | Int64
> pres-notify-resp-6xxrx | Total number of “presence” Notify 6XX Responses received. | Int64
> pres-notify-resp-6xxtx | Total number of “presence” Notify 6XX Responses transmitted. | Int64
> pres-pub-attrx | Total number of “presence” Publish Attempts received. | Int64
> pres-pub-atttx | Total number of “presence” Publish Attempts transmitted. | Int64
> pres-pub-succrx | Total number of “presence” Publish Successes received. | Int64
> pres-pub-succtx | Total number of “presence” Publish Successes transmitted. | Int64
> pres-pub-failrx | Total number of “presence” Publish Failures received. | Int64
> pres-pub-failtx | Total number of “presence” Publish Failures transmitted. | Int64
> pres-pub-resp-3xxrx | Total number of “presence” Publish 3XX Responses received. | Int64
> pres-pub-resp-3xxtx | Total number of “presence” Publish 3XX Responses transmitted. | Int64
> pres-pub-resp-400rx | Total number of “presence” Publish 400 Responses received. | Int64
> pres-pub-resp-400tx | Total number of “presence” Publish 400 Responses transmitted. | Int64
> pres-pub-resp-404rx | Total number of “presence” Publish 404 Responses received. | Int64
> pres-pub-resp-404tx | Total number of “presence” Publish 404 Responses transmitted. | Int64
> pres-pub-resp-412rx | Total number of “presence” Publish 412 Responses received. | Int64
> pres-pub-resp-412tx | Total number of “presence” Publish 412 Responses transmitted. | Int64
> pres-pub-resp-423rx | Total number of “presence” Publish 423 Responses received. | Int64
> pres-pub-resp-423tx | Total number of “presence” Publish 423 Responses transmitted. | Int64
> pres-pub-resp-489rx | Total number of “presence” Publish 489 Responses received. | Int64
> pres-pub-resp-489tx | Total number of “presence” Publish 489 Responses transmitted. | Int64
> pres-pub-resp-4xxrx | Total number of “presence” Publish 4XX Responses received. | Int64
> pres-pub-resp-4xxtx | Total number of “presence” Publish 4XX Responses transmitted. | Int64
> pres-pub-resp-500rx | Total number of “presence” Publish 500 Responses received. | Int64
> pres-pub-resp-500tx | Total number of “presence” Publish 500 Responses transmitted. | Int64
> pres-pub-resp-503rx | Total number of “presence” Publish 503 Responses received. | Int64
> pres-pub-resp-503tx | Total number of “presence” Publish 503 Responses transmitted. | Int64
> pres-pub-resp-5xxrx | Total number of “presence” Publish 5XX Responses received. | Int64
> pres-pub-resp-5xxtx | Total number of “presence” Publish 5XX Responses transmitted. | Int64
> pres-pub-resp-6xxrx | Total number of “presence” Publish 6XX Responses received. | Int64
> pres-pub-resp-6xxtx | Total number of “presence” Publish 6XX Responses transmitted. | Int64
> pres-unpub-attrx | Total number of “presence” Un-Publish Attempts received. | Int64
> pres-unpub-atttx | Total number of “presence” Un-Publish Attempts transmitted. | Int64
> pres-unpub-succrx | Total number of “presence” Un-Publish Successes received. | Int64
> pres-unpub-succtx | Total number of “presence” Un-Publish Successes transmitted. | Int64
> pres-unpub-failrx | Total number of “presence” Un-Publish Failures received. | Int64
> pres-unpub-failtx | Total number of “presence” Un-Publish Failures transmitted. | Int64
> pres-unpub-resp-3xxrx | Total number of “presence” Un-Publish 3XX Responses received. | Int64
> pres-unpub-resp-3xxtx | Total number of “presence” Un-Publish 3XX Responses transmitted. | Int64
> pres-unpub-resp-400rx | Total number of “presence” Un-Publish 400 Responses received. | Int64
> pres-unpub-resp-400tx | Total number of “presence” Un-Publish 400 Responses transmitted. | Int64
> pres-unpub-resp-404rx | Total number of “presence” Un-Publish 404 Responses received. | Int64
> pres-unpub-resp-404tx | Total number of “presence” Un-Publish 404 Responses transmitted. | Int64
> pres-unpub-resp-412rx | Total number of “presence” Un-Publish 412 Responses received. | Int64
> pres-unpub-resp-412tx | Total number of “presence” Un-Publish 412 Responses transmitted. | Int64
> pres-unpub-resp-423rx | Total number of “presence” Un-Publish 423 Responses received. | Int64
> pres-unpub-resp-423tx | Total number of “presence” Un-Publish 423 Responses transmitted. | Int64
> pres-unpub-resp-489rx | Total number of “presence” Un-Publish 489 Responses received. | Int64
> pres-unpub-resp-489tx | Total number of “presence” Un-Publish 489 Responses transmitted. | Int64
> pres-unpub-resp-4xxrx | Total number of “presence” Un-Publish 4XX Responses received. | Int64
> pres-unpub-resp-4xxtx | Total number of “presence” Un-Publish 4XX Responses transmitted. | Int64
> pres-unpub-resp-500rx | Total number of “presence” Un-Publish 500 Responses received. | Int64
> pres-unpub-resp-500tx | Total number of “presence” Un-Publish 500 Responses transmitted. | Int64
> pres-unpub-resp-503rx | Total number of “presence” Un-Publish 503 Responses received. | Int64
> pres-unpub-resp-503tx | Total number of “presence” Un-Publish 503 Responses transmitted. | Int64
> pres-unpub-resp-5xxrx | Total number of “presence” Un-Publish 5XX Responses received. | Int64
> pres-unpub-resp-5xxtx | Total number of “presence” Un-Publish 5XX Responses transmitted. | Int64
> pres-unpub-resp-6xxrx | Total number of “presence” Un-Publish 6XX Responses received. | Int64
> pres-unpub-resp-6xxtx | Total number of “presence” Un-Publish 6XX Responses transmitted. | Int64
> reg-subs-attrx | Total number of “reg” Subscription Attempts received. | Int64
> reg-subs-atttx | Total number of “reg” Subscription Attempts transmitted. | Int64
> reg-subs-succrx | Total number of “reg” Subscription Successes received. | Int64
> reg-subs-succtx | Total number of “reg” Subscription Successes transmitted. | Int64
> reg-subs-failrx | Total number of “reg” Subscription Failures received. | Int64
> reg-subs-failtx | Total number of “reg” Subscription Failures transmitted. | Int64
> reg-subs-resp-200rx | Total number of “reg” Subscription 200 Responses received. | Int64
> reg-subs-resp-200tx | Total number of “reg” Subscription 200 Responses transmitted. | Int64
> reg-subs-resp-202rx | Total number of “reg” Subscription 202 Responses received. | Int64
> reg-subs-resp-202tx | Total number of “reg” Subscription 202 Responses transmitted. | Int64
> reg-subs-resp-400rx | Total number of “reg” Subscription 400 Responses received. | Int64
> reg-subs-resp-400tx | Total number of “reg” Subscription 400 Responses transmitted. | Int64
> reg-subs-resp-403rx | Total number of “reg” Subscription 403 Responses received. | Int64
> reg-subs-resp-403tx | Total number of “reg” Subscription 403 Responses transmitted. | Int64
> reg-subs-resp-481rx | Total number of “reg” Subscription 481 Responses received. | Int64
> reg-subs-resp-481tx | Total number of “reg” Subscription 481 Responses transmitted. | Int64
> reg-subs-resp-489rx | Total number of “reg” Subscription 489 Responses received. | Int64
> reg-subs-resp-489tx | Total number of “reg” Subscription 489 Responses transmitted. | Int64
> reg-subs-resp-500rx | Total number of “reg” Subscription 500 Responses received. | Int64
> reg-subs-resp-500tx | Total number of “reg” Subscription 500 Responses transmitted. | Int64
> reg-subs-resp-3xxrx | Total number of “reg” Subscription 3XX Responses received. | Int64
> reg-subs-resp-3xxtx | Total number of “reg” Subscription 3XX Responses transmitted. | Int64
> reg-subs-resp-4xxrx | Total number of “reg” Subscription 4XX Responses received. | Int64
> reg-subs-resp-4xxtx | Total number of “reg” Subscription 4XX Responses transmitted. | Int64
> reg-subs-resp-5xxrx | Total number of “reg” Subscription 5XX Responses received. | Int64
> reg-subs-resp-5xxtx | Total number of “reg” Subscription 5XX Responses transmitted. | Int64
> reg-subs-resp-6xxrx | Total number of “reg” Subscription 6XX Responses received. | Int64
> reg-subs-resp-6xxtx | Total number of “reg” Subscription 6XX Responses transmitted. | Int64
> reg-resubs-attrx | Total number of “reg” Refresh Subscription Attempts received. | Int64
> reg-resubs-atttx | Total number of “reg” Refresh Subscription Attempts transmitted. | Int64
> reg-resubs-succrx | Total number of “reg” Refresh Subscription Successes received. | Int64
> reg-resubs-succtx | Total number of “reg” Refresh Subscription Successes transmitted. | Int64
> reg-resubs-failrx | Total number of “reg” Refresh Subscription Failures received. | Int64
> reg-resubs-failtx | Total number of “reg” Refresh Subscription Failures transmitted. | Int64
> reg-resubs-resp-200rx | Total number of “reg” Refresh Subscription 200 Responses received. | Int64
> reg-resubs-resp-200tx | Total number of “reg” Refresh Subscription 200 Responses transmitted. | Int64
> reg-resubs-resp-202rx | Total number of “reg” Refresh Subscription 202 Responses received. | Int64
> reg-resubs-resp-202tx | Total number of “reg” Refresh Subscription 202 Responses transmitted. | Int64
> reg-resubs-resp-400rx | Total number of “reg” Refresh Subscription 400 Responses received. | Int64
> reg-resubs-resp-400tx | Total number of “reg” Refresh Subscription 400 Responses transmitted. | Int64
> reg-resubs-resp-403rx | Total number of “reg” Refresh Subscription 403 Responses received. | Int64
> reg-resubs-resp-403tx | Total number of “reg” Refresh Subscription 403 Responses transmitted. | Int64
> reg-resubs-resp-481rx | Total number of “reg” Refresh Subscription 481 Responses received. | Int64
> reg-resubs-resp-481tx | Total number of “reg” Refresh Subscription 481 Responses transmitted. | Int64
> reg-resubs-resp-489rx | Total number of “reg” Refresh Subscription 489 Responses received. | Int64
> reg-resubs-resp-489tx | Total number of “reg” Refresh Subscription 489 Responses transmitted. | Int64
> reg-resubs-resp-500rx | Total number of “reg” Refresh Subscription 500 Responses received. | Int64
> reg-resubs-resp-500tx | Total number of “reg” Refresh Subscription 500 Responses transmitted. | Int64
> reg-resubs-resp-3xxrx | Total number of “reg” Refresh Subscription 3XX Responses received. | Int64
> reg-resubs-resp-3xxtx | Total number of “reg” Refresh Subscription 3XX Responses transmitted. | Int64
> reg-resubs-resp-4xxrx | Total number of “reg” Refresh Subscription 4XX Responses received. | Int64
> reg-resubs-resp-4xxtx | Total number of “reg” Refresh Subscription 4XX Responses transmitted. | Int64
> reg-resubs-resp-5xxrx | Total number of “reg” Refresh Subscription 5XX Responses received. | Int64
> reg-resubs-resp-5xxtx | Total number of “reg” Refresh Subscription 5XX Responses transmitted. | Int64
> reg-resubs-resp-6xxrx | Total number of “reg” Refresh Subscription 6XX Responses received. | Int64
> reg-resubs-resp-6xxtx | Total number of “reg” Refresh Subscription 6XX Responses transmitted. | Int64
> reg-unsubs-attrx | Total number of “reg” Un-Subscription Attempts received. | Int64
> reg-unsubs-atttx | Total number of “reg” Un-Subscription Attempts transmitted. | Int64
> reg-unsubs-succrx | Total number of “reg” Un-Subscription Successes received. | Int64
> reg-unsubs-succtx | Total number of “reg” Un-Subscription Successes transmitted. | Int64
> reg-unsubs-failrx | Total number of “reg” Un-Subscription Failures received. | Int64
> reg-unsubs-failtx | Total number of “reg” Un-Subscription Failures transmitted. | Int64
> reg-unsubs-resp-200rx | Total number of “reg” Un-Subscription 200 Responses received. | Int64
> reg-unsubs-resp-200tx | Total number of “reg” Un-Subscription 200 Responses transmitted. | Int64
> reg-unsubs-resp-202rx | Total number of “reg” Un-Subscription 202 Responses received. | Int64
> reg-unsubs-resp-202tx | Total number of “reg” Un-Subscription 202 Responses transmitted. | Int64
> reg-unsubs-resp-400rx | Total number of “reg” Un-Subscription 400 Responses received. | Int64
> reg-unsubs-resp-400tx | Total number of “reg” Un-Subscription 400 Responses transmitted. | Int64
> reg-unsubs-resp-403rx | Total number of “reg” Un-Subscription 403 Responses received. | Int64
> reg-unsubs-resp-403tx | Total number of “reg” Un-Subscription 403 Responses transmitted. | Int64
> reg-unsubs-resp-481rx | Total number of “reg” Un-Subscription 481 Responses received. | Int64
> reg-unsubs-resp-481tx | Total number of “reg” Un-Subscription 481 Responses transmitted. | Int64
> reg-unsubs-resp-489rx | Total number of “reg” Un-Subscription 489 Responses received. | Int64
> reg-unsubs-resp-489tx | Total number of “reg” Un-Subscription 489 Responses transmitted. | Int64
> reg-unsubs-resp-500rx | Total number of “reg” Un-Subscription 500 Responses received. | Int64
> reg-unsubs-resp-500tx | Total number of “reg” Un-Subscription 500 Responses transmitted. | Int64
> reg-unsubs-resp-3xxrx | Total number of “reg” Un-Subscription 3XX Responses received. | Int64
> reg-unsubs-resp-3xxtx | Total number of “reg” Un-Subscription 3XX Responses transmitted. | Int64
> reg-unsubs-resp-4xxrx | Total number of “reg” Un-Subscription 4XX Responses received. | Int64
> reg-unsubs-resp-4xxtx | Total number of “reg” Un-Subscription 4XX Responses transmitted. | Int64
> reg-unsubs-resp-5xxrx | Total number of “reg” Un-Subscription 5XX Responses received. | Int64
> reg-unsubs-resp-5xxtx | Total number of “reg” Un-Subscription 5XX Responses transmitted. | Int64
> reg-unsubs-resp-6xxrx | Total number of “reg” Un-Subscription 6XX Responses received. | Int64
> reg-unsubs-resp-6xxtx | Total number of “reg” Un-Subscription 6XX Responses transmitted. | Int64
> reg-notify-attrx | Total number of “reg” Notify Attempts received. | Int64
> reg-notify-atttx | Total number of “reg” Notify Attempts transmitted. | Int64
> reg-notify-succrx | Total number of “reg” Notify Successes received. | Int64
> reg-notify-succtx | Total number of “reg” Notify Successes transmitted. | Int64
> reg-notify-failrx | Total number of “reg” Notify Failures received. | Int64
> reg-notify-failtx | Total number of “reg” Notify Failures transmitted. | Int64
> reg-notify-resp-3xxrx | Total number of “reg” Notify 3XX Responses received. | Int64
> reg-notify-resp-3xxtx | Total number of “reg” Notify 3XX Responses transmitted. | Int64
> reg-notify-resp-400rx | Total number of “reg” Notify 400 Responses received. | Int64
> reg-notify-resp-400tx | Total number of “reg” Notify 400 Responses transmitted. | Int64
> reg-notify-resp-481rx | Total number of “reg” Notify 481 Responses received. | Int64
> reg-notify-resp-481tx | Total number of “reg” Notify 481 Responses transmitted. | Int64
> reg-notify-resp-489rx | Total number of “reg” Notify 489 Responses received. | Int64
> reg-notify-resp-489tx | Total number of “reg” Notify 489 Responses transmitted. | Int64
> reg-notify-resp-4xxrx | Total number of “reg” Notify 4XX Responses received. | Int64
> reg-notify-resp-4xxtx | Total number of “reg” Notify 4XX Responses transmitted. | Int64
> reg-notify-resp-500rx | Total number of “reg” Notify 500 Responses received. | Int64
> reg-notify-resp-500tx | Total number of “reg” Notify 500 Responses transmitted. | Int64
> reg-notify-resp-5xxrx | Total number of “reg” Notify 5XX Responses received. | Int64
> reg-notify-resp-5xxtx | Total number of “reg” Notify 5XX Responses transmitted. | Int64
> reg-notify-resp-6xxrx | Total number of “reg” Notify 6XX Responses received. | Int64
> reg-notify-resp-6xxtx | Total number of “reg” Notify 6XX Responses transmitted. | Int64
> reg-pub-attrx | Total number of “reg” Publish Attempts received. | Int64
> reg-pub-atttx | Total number of “reg” Publish Attempts transmitted. | Int64
> reg-pub-succrx | Total number of “reg” Publish Successes received. | Int64
> reg-pub-succtx | Total number of “reg” Publish Successes transmitted. | Int64
> reg-pub-failrx | Total number of “reg” Publish Failures received. | Int64
> reg-pub-failtx | Total number of “reg” Publish Failures transmitted. | Int64
> reg-pub-resp-3xxrx | Total number of “reg” Publish 3XX Responses received. | Int64
> reg-pub-resp-3xxtx | Total number of “reg” Publish 3XX Responses transmitted. | Int64
> reg-pub-resp-400rx | Total number of “reg” Publish 400 Responses received. | Int64
> reg-pub-resp-400tx | Total number of “reg” Publish 400 Responses transmitted. | Int64
> reg-pub-resp-404rx | Total number of “reg” Publish 404 Responses received. | Int64
> reg-pub-resp-404tx | Total number of “reg” Publish 404 Responses transmitted. | Int64
> reg-pub-resp-412rx | Total number of “reg” Publish 412 Responses received. | Int64
> reg-pub-resp-412tx | Total number of “reg” Publish 412 Responses transmitted. | Int64
> reg-pub-resp-423rx | Total number of “reg” Publish 423 Responses received. | Int64
> reg-pub-resp-423tx | Total number of “reg” Publish 423 Responses transmitted. | Int64
> reg-pub-resp-489rx | Total number of “reg” Publish 489 Responses received. | Int64
> reg-pub-resp-489tx | Total number of “reg” Publish 489 Responses transmitted. | Int64
> reg-pub-resp-4xxrx | Total number of “reg” Publish 4XX Responses received. | Int64
> reg-pub-resp-4xxtx | Total number of “reg” Publish 4XX Responses transmitted. | Int64
> reg-pub-resp-500rx | Total number of “reg” Publish 500 Responses received. | Int64
> reg-pub-resp-500tx | Total number of “reg” Publish 500 Responses transmitted. | Int64
> reg-pub-resp-503rx | Total number of “reg” Publish 503 Responses received. | Int64
> reg-pub-resp-503tx | Total number of “reg” Publish 503 Responses transmitted. | Int64
> reg-pub-resp-5xxrx | Total number of “reg” Publish 5XX Responses received. | Int64
> reg-pub-resp-5xxtx | Total number of “reg” Publish 5XX Responses transmitted. | Int64
> reg-pub-resp-6xxrx | Total number of “reg” Publish 6XX Responses received. | Int64
> reg-pub-resp-6xxtx | Total number of “reg” Publish 6XX Responses transmitted. | Int64
> reg-unpub-attrx | Total number of “reg” Un-Publish Attempts received. | Int64
> reg-unpub-atttx | Total number of “reg” Un-Publish Attempts transmitted. | Int64
> reg-unpub-succrx | Total number of “reg” Un-Publish Successes received. | Int64
> reg-unpub-succtx | Total number of “reg” Un-Publish Successes transmitted. | Int64
> reg-unpub-failrx | Total number of “reg” Un-Publish Failures received. | Int64
> reg-unpub-failtx | Total number of “reg” Un-Publish Failures transmitted. | Int64
> reg-unpub-resp-3xxrx | Total number of “reg” Un-Publish 3XX Responses received. | Int64
> reg-unpub-resp-3xxtx | Total number of “reg” Un-Publish 3XX Responses transmitted. | Int64
> reg-unpub-resp-400rx | Total number of “reg” Un-Publish 400 Responses received. | Int64
> reg-unpub-resp-400tx | Total number of “reg” Un-Publish 400 Responses transmitted. | Int64
> reg-unpub-resp-404rx | Total number of “reg” Un-Publish 404 Responses received. | Int64
> reg-unpub-resp-404tx | Total number of “reg” Un-Publish 404 Responses transmitted. | Int64
> reg-unpub-resp-412rx | Total number of “reg” Un-Publish 412 Responses received. | Int64
> reg-unpub-resp-412tx | Total number of “reg” Un-Publish 412 Responses transmitted. | Int64
> reg-unpub-resp-423rx | Total number of “reg” Un-Publish 423 Responses received. | Int64
> reg-unpub-resp-423tx | Total number of “reg” Un-Publish 423 Responses transmitted. | Int64
> reg-unpub-resp-489rx | Total number of “reg” Un-Publish 489 Responses received. | Int64
> reg-unpub-resp-489tx | Total number of “reg” Un-Publish 489 Responses transmitted. | Int64
> reg-unpub-resp-4xxrx | Total number of “reg” Un-Publish 4XX Responses received. | Int64
> reg-unpub-resp-4xxtx | Total number of “reg” Un-Publish 4XX Responses transmitted. | Int64
> reg-unpub-resp-500rx | Total number of “reg” Un-Publish 500 Responses received. | Int64
> reg-unpub-resp-500tx | Total number of “reg” Un-Publish 500 Responses transmitted. | Int64
> reg-unpub-resp-503rx | Total number of “reg” Un-Publish 503 Responses received. | Int64
> reg-unpub-resp-503tx | Total number of “reg” Un-Publish 503 Responses transmitted. | Int64
> reg-unpub-resp-5xxrx | Total number of “reg” Un-Publish 5XX Responses received. | Int64
> reg-unpub-resp-5xxtx | Total number of “reg” Un-Publish 5XX Responses transmitted. | Int64
> reg-unpub-resp-6xxrx | Total number of “reg” Un-Publish 6XX Responses received. | Int64
> reg-unpub-resp-6xxtx | Total number of “reg” Un-Publish 6XX Responses transmitted. | Int64
> winfo-subs-attrx | Total number of “winfo” Subscription Attempts received. | Int64
> winfo-subs-atttx | Total number of “winfo” Subscription Attempts transmitted. | Int64
> winfo-subs-succrx | Total number of “winfo” Subscription Successes received. | Int64
> winfo-subs-succtx | Total number of “winfo” Subscription Successes transmitted. | Int64
> winfo-subs-failrx | Total number of “winfo” Subscription Failures received. | Int64
> winfo-subs-failtx | Total number of “winfo” Subscription Failures transmitted. | Int64
> winfo-subs-resp-200rx | Total number of “winfo” Subscription 200 Responses received. | Int64
> winfo-subs-resp-200tx | Total number of “winfo” Subscription 200 Responses transmitted. | Int64
> winfo-subs-resp-202rx | Total number of “winfo” Subscription 202 Responses received. | Int64
> winfo-subs-resp-202tx | Total number of “winfo” Subscription 202 Responses transmitted. | Int64
> winfo-subs-resp-400rx | Total number of “winfo” Subscription 400 Responses received. | Int64
> winfo-subs-resp-400tx | Total number of “winfo” Subscription 400 Responses transmitted. | Int64
> winfo-subs-resp-403rx | Total number of “winfo” Subscription 403 Responses received. | Int64
> winfo-subs-resp-403tx | Total number of “winfo” Subscription 403 Responses transmitted. | Int64
> winfo-subs-resp-481rx | Total number of “winfo” Subscription 481 Responses received. | Int64
> winfo-subs-resp-481tx | Total number of “winfo” Subscription 481 Responses transmitted. | Int64
> winfo-subs-resp-489rx | Total number of “winfo” Subscription 489 Responses received. | Int64
> winfo-subs-resp-489tx | Total number of “winfo” Subscription 489 Responses transmitted. | Int64
> winfo-subs-resp-500rx | Total number of “winfo” Subscription 500 Responses received. | Int64
> winfo-subs-resp-500tx | Total number of “winfo” Subscription 500 Responses transmitted. | Int64
> winfo-subs-resp-3xxrx | Total number of “winfo” Subscription 3XX Responses received. | Int64
> winfo-subs-resp-3xxtx | Total number of “winfo” Subscription 3XX Responses transmitted. | Int64
> winfo-subs-resp-4xxrx | Total number of “winfo” Subscription 4XX Responses received. | Int64
> winfo-subs-resp-4xxtx | Total number of “winfo” Subscription 4XX Responses transmitted. | Int64
> winfo-subs-resp-5xxrx | Total number of “winfo” Subscription 5XX Responses received. | Int64
> winfo-subs-resp-5xxtx | Total number of “winfo” Subscription 5XX Responses transmitted. | Int64
> winfo-subs-resp-6xxrx | Total number of “winfo” Subscription 6XX Responses received. | Int64
> winfo-subs-resp-6xxtx | Total number of “winfo” Subscription 6XX Responses transmitted. | Int64
> winfo-resubs-attrx | Total number of “winfo” Refresh Subscription Attempts received. | Int64
> winfo-resubs-atttx | Total number of “winfo” Refresh Subscription Attempts transmitted. | Int64
> winfo-resubs-succrx | Total number of “winfo” Refresh Subscription Successes received. | Int64
> winfo-resubs-succtx | Total number of “winfo” Refresh Subscription Successes transmitted. | Int64
> winfo-resubs-failrx | Total number of “winfo” Refresh Subscription Failures received. | Int64
> winfo-resubs-failtx | Total number of “winfo” Refresh Subscription Failures transmitted. | Int64
> winfo-resubs-resp-200rx | Total number of “winfo” Refresh Subscription 200 Responses received. | Int64
> winfo-resubs-resp-200tx | Total number of “winfo” Refresh Subscription 200 Responses transmitted. | Int64
> winfo-resubs-resp-202rx | Total number of “winfo” Refresh Subscription 202 Responses received. | Int64
> winfo-resubs-resp-202tx | Total number of “winfo” Refresh Subscription 202 Responses transmitted. | Int64
> winfo-resubs-resp-400rx | Total number of “winfo” Refresh Subscription 400 Responses received. | Int64
> winfo-resubs-resp-400tx | Total number of “winfo” Refresh Subscription 400 Responses transmitted. | Int64
> winfo-resubs-resp-403rx | Total number of “winfo” Refresh Subscription 403 Responses received. | Int64
> winfo-resubs-resp-403tx | Total number of “winfo” Refresh Subscription 403 Responses transmitted. | Int64
> winfo-resubs-resp-481rx | Total number of “winfo” Refresh Subscription 481 Responses received. | Int64
> winfo-resubs-resp-481tx | Total number of “winfo” Refresh Subscription 481 Responses transmitted. | Int64
> winfo-resubs-resp-489rx | Total number of “winfo” Refresh Subscription 489 Responses received. | Int64
> winfo-resubs-resp-489tx | Total number of “winfo” Refresh Subscription 489 Responses transmitted. | Int64
> winfo-resubs-resp-500rx | Total number of “winfo” Refresh Subscription 500 Responses received. | Int64
> winfo-resubs-resp-500tx | Total number of “winfo” Refresh Subscription 500 Responses transmitted. | Int64
> winfo-resubs-resp-3xxrx | Total number of “winfo” Refresh Subscription 3XX Responses received. | Int64
> winfo-resubs-resp-3xxtx | Total number of “winfo” Refresh Subscription 3XX Responses transmitted. | Int64
> winfo-resubs-resp-4xxrx | Total number of “winfo” Refresh Subscription 4XX Responses received. | Int64
> winfo-resubs-resp-4xxtx | Total number of “winfo” Refresh Subscription 4XX Responses transmitted. | Int64
> winfo-resubs-resp-5xxrx | Total number of “winfo” Refresh Subscription 5XX Responses received. | Int64
> winfo-resubs-resp-5xxtx | Total number of “winfo” Refresh Subscription 5XX Responses transmitted. | Int64
> winfo-resubs-resp-6xxrx | Total number of “winfo” Refresh Subscription 6XX Responses received. | Int64
> winfo-resubs-resp-6xxtx | Total number of “winfo” Refresh Subscription 6XX Responses transmitted. | Int64
> winfo-unsubs-attrx | Total number of “winfo” Un-Subscription Attempts received. | Int64
> winfo-unsubs-atttx | Total number of “winfo” Un-Subscription Attempts transmitted. | Int64
> winfo-unsubs-succrx | Total number of “winfo” Un-Subscription Successes received. | Int64
> winfo-unsubs-succtx | Total number of “winfo” Un-Subscription Successes transmitted. | Int64
> winfo-unsubs-failrx | Total number of “winfo” Un-Subscription Failures received. | Int64
> winfo-unsubs-failtx | Total number of “winfo” Un-Subscription Failures transmitted. | Int64
> winfo-unsubs-resp-200rx | Total number of “winfo” Un-Subscription 200 Responses received. | Int64
> winfo-unsubs-resp-200tx | Total number of “winfo” Un-Subscription 200 Responses transmitted. | Int64
> winfo-unsubs-resp-202rx | Total number of “winfo” Un-Subscription 202 Responses received. | Int64
> winfo-unsubs-resp-202tx | Total number of “winfo” Un-Subscription 202 Responses transmitted. | Int64
> winfo-unsubs-resp-400rx | Total number of “winfo” Un-Subscription 400 Responses received. | Int64
> winfo-unsubs-resp-400tx | Total number of “winfo” Un-Subscription 400 Responses transmitted. | Int64
> winfo-unsubs-resp-403rx | Total number of “winfo” Un-Subscription 403 Responses received. | Int64
> winfo-unsubs-resp-403tx | Total number of “winfo” Un-Subscription 403 Responses transmitted. | Int64
> winfo-unsubs-resp-481rx | Total number of “winfo” Un-Subscription 481 Responses received. | Int64
> winfo-unsubs-resp-481tx | Total number of “winfo” Un-Subscription 481 Responses transmitted. | Int64
> winfo-unsubs-resp-489rx | Total number of “winfo” Un-Subscription 489 Responses received. | Int64
> winfo-unsubs-resp-489tx | Total number of “winfo” Un-Subscription 489 Responses transmitted. | Int64
> winfo-unsubs-resp-500rx | Total number of “winfo” Un-Subscription 500 Responses received. | Int64
> winfo-unsubs-resp-500tx | Total number of “winfo” Un-Subscription 500 Responses transmitted. | Int64
> winfo-unsubs-resp-3xxrx | Total number of “winfo” Un-Subscription 3XX Responses received. | Int64
> winfo-unsubs-resp-3xxtx | Total number of “winfo” Un-Subscription 3XX Responses transmitted. | Int64
> winfo-unsubs-resp-4xxrx | Total number of “winfo” Un-Subscription 4XX Responses received. | Int64
> winfo-unsubs-resp-4xxtx | Total number of “winfo” Un-Subscription 4XX Responses transmitted. | Int64
> winfo-unsubs-resp-5xxrx | Total number of “winfo” Un-Subscription 5XX Responses received. | Int64
> winfo-unsubs-resp-5xxtx | Total number of “winfo” Un-Subscription 5XX Responses transmitted. | Int64
> winfo-unsubs-resp-6xxrx | Total number of “winfo” Un-Subscription 6XX Responses received. | Int64
> winfo-unsubs-resp-6xxtx | Total number of “winfo” Un-Subscription 6XX Responses transmitted. | Int64
> winfo-notify-attrx | Total number of “winfo” Notify Attempts received. | Int64
> winfo-notify-atttx | Total number of “winfo” Notify Attempts transmitted. | Int64
> winfo-notify-succrx | Total number of “winfo” Notify Successes received. | Int64
> winfo-notify-succtx | Total number of “winfo” Notify Successes transmitted. | Int64
> winfo-notify-failrx | Total number of “winfo” Notify Failures received. | Int64
> winfo-notify-failtx | Total number of “winfo” Notify Failures transmitted. | Int64
> winfo-notify-resp-3xxrx | Total number of “winfo” Notify 3XX Responses received. | Int64
> winfo-notify-resp-3xxtx | Total number of “winfo” Notify 3XX Responses transmitted. | Int64
> winfo-notify-resp-400rx | Total number of “winfo” Notify 400 Responses received. | Int64
> winfo-notify-resp-400tx | Total number of “winfo” Notify 400 Responses transmitted. | Int64
> winfo-notify-resp-481rx | Total number of “winfo” Notify 481 Responses received. | Int64
> winfo-notify-resp-481tx | Total number of “winfo” Notify 481 Responses transmitted. | Int64
> winfo-notify-resp-489rx | Total number of “winfo” Notify 489 Responses received. | Int64
> winfo-notify-resp-489tx | Total number of “winfo” Notify 489 Responses transmitted. | Int64
> winfo-notify-resp-4xxrx | Total number of “winfo” Notify 4XX Responses received. | Int64
> winfo-notify-resp-4xxtx | Total number of “winfo” Notify 4XX Responses transmitted. | Int64
> winfo-notify-resp-500rx | Total number of “winfo” Notify 500 Responses received. | Int64
> winfo-notify-resp-500tx | Total number of “winfo” Notify 500 Responses transmitted. | Int64
> winfo-notify-resp-5xxrx | Total number of “winfo” Notify 5XX Responses received. | Int64
> winfo-notify-resp-5xxtx | Total number of “winfo” Notify 5XX Responses transmitted. | Int64
> winfo-notify-resp-6xxrx | Total number of “winfo” Notify 6XX Responses received. | Int64
> winfo-notify-resp-6xxtx | Total number of “winfo” Notify 6XX Responses transmitted. | Int64
> winfo-pub-attrx | Total number of “winfo” Publish Attempts received. | Int64
> winfo-pub-atttx | Total number of “winfo” Publish Attempts transmitted. | Int64
> winfo-pub-succrx | Total number of “winfo” Publish Successes received. | Int64
> winfo-pub-succtx | Total number of “winfo” Publish Successes transmitted. | Int64
> winfo-pub-failrx | Total number of “winfo” Publish Failures received. | Int64
> winfo-pub-failtx | Total number of “winfo” Publish Failures transmitted. | Int64
> winfo-pub-resp-3xxrx | Total number of “winfo” Publish 3XX Responses received. | Int64
> winfo-pub-resp-3xxtx | Total number of “winfo” Publish 3XX Responses transmitted. | Int64
> winfo-pub-resp-400rx | Total number of “winfo” Publish 400 Responses received. | Int64
> winfo-pub-resp-400tx | Total number of “winfo” Publish 400 Responses transmitted. | Int64
> winfo-pub-resp-404rx | Total number of “winfo” Publish 404 Responses received. | Int64
> winfo-pub-resp-404tx | Total number of “winfo” Publish 404 Responses transmitted. | Int64
> winfo-pub-resp-412rx | Total number of “winfo” Publish 412 Responses received. | Int64
> winfo-pub-resp-412tx | Total number of “winfo” Publish 412 Responses transmitted. | Int64
> winfo-pub-resp-423rx | Total number of “winfo” Publish 423 Responses received. | Int64
> winfo-pub-resp-423tx | Total number of “winfo” Publish 423 Responses transmitted. | Int64
> winfo-pub-resp-489rx | Total number of “winfo” Publish 489 Responses received. | Int64
> winfo-pub-resp-489tx | Total number of “winfo” Publish 489 Responses transmitted. | Int64
> winfo-pub-resp-4xxrx | Total number of “winfo” Publish 4XX Responses received. | Int64
> winfo-pub-resp-4xxtx | Total number of “winfo” Publish 4XX Responses transmitted. | Int64
> winfo-pub-resp-500rx | Total number of “winfo” Publish 500 Responses received. | Int64
> winfo-pub-resp-500tx | Total number of “winfo” Publish 500 Responses transmitted. | Int64
> winfo-pub-resp-503rx | Total number of “winfo” Publish 503 Responses received. | Int64
> winfo-pub-resp-503tx | Total number of “winfo” Publish 503 Responses transmitted. | Int64
> winfo-pub-resp-5xxrx | Total number of “winfo” Publish 5XX Responses received. | Int64
> winfo-pub-resp-5xxtx | Total number of “winfo” Publish 5XX Responses transmitted. | Int64
> winfo-pub-resp-6xxrx | Total number of “winfo” Publish 6XX Responses received. | Int64
> winfo-pub-resp-6xxtx | Total number of “winfo” Publish 6XX Responses transmitted. | Int64
> winfo-unpub-attrx | Total number of “winfo” Un-Publish Attempts received. | Int64
> winfo-unpub-atttx | Total number of “winfo” Un-Publish Attempts transmitted. | Int64
> winfo-unpub-succrx | Total number of “winfo” Un-Publish Successes received. | Int64
> winfo-unpub-succtx | Total number of “winfo” Un-Publish Successes transmitted. | Int64
> winfo-unpub-failrx | Total number of “winfo” Un-Publish Failures received. | Int64
> winfo-unpub-failtx | Total number of “winfo” Un-Publish Failures transmitted. | Int64
> winfo-unpub-resp-3xxrx | Total number of “winfo” Un-Publish 3XX Responses received. | Int64
> winfo-unpub-resp-3xxtx | Total number of “winfo” Un-Publish 3XX Responses transmitted. | Int64
> winfo-unpub-resp-400rx | Total number of “winfo” Un-Publish 400 Responses received. | Int64
> winfo-unpub-resp-400tx | Total number of “winfo” Un-Publish 400 Responses transmitted. | Int64
> winfo-unpub-resp-404rx | Total number of “winfo” Un-Publish 404 Responses received. | Int64
> winfo-unpub-resp-404tx | Total number of “winfo” Un-Publish 404 Responses transmitted. | Int64
> winfo-unpub-resp-412rx | Total number of “winfo” Un-Publish 412 Responses received. | Int64
> winfo-unpub-resp-412tx | Total number of “winfo” Un-Publish 412 Responses transmitted. | Int64
> winfo-unpub-resp-423rx | Total number of “winfo” Un-Publish 423 Responses received. | Int64
> winfo-unpub-resp-423tx | Total number of “winfo” Un-Publish 423 Responses transmitted. | Int64
> winfo-unpub-resp-489rx | Total number of “winfo” Un-Publish 489 Responses received. | Int64
> winfo-unpub-resp-489tx | Total number of “winfo” Un-Publish 489 Responses transmitted. | Int64
> winfo-unpub-resp-4xxrx | Total number of “winfo” Un-Publish 4XX Responses received. | Int64
> winfo-unpub-resp-4xxtx | Total number of “winfo” Un-Publish 4XX Responses transmitted. | Int64
> winfo-unpub-resp-500rx | Total number of “winfo” Un-Publish 500 Responses received. | Int64
> winfo-unpub-resp-500tx | Total number of “winfo” Un-Publish 500 Responses transmitted. | Int64
> winfo-unpub-resp-503rx | Total number of “winfo” Un-Publish 503 Responses received. | Int64
> winfo-unpub-resp-503tx | Total number of “winfo” Un-Publish 503 Responses transmitted. | Int64
> winfo-unpub-resp-5xxrx | Total number of “winfo” Un-Publish 5XX Responses received. | Int64
> winfo-unpub-resp-5xxtx | Total number of “winfo” Un-Publish 5XX Responses transmitted. | Int64
> winfo-unpub-resp-6xxrx | Total number of “winfo” Un-Publish 6XX Responses received. | Int64
> winfo-unpub-resp-6xxtx | Total number of “winfo” Un-Publish 6XX Responses transmitted. | Int64
> message-attrx | Total number of Message attempts received. | Int32
> message-atttx | Total number of Message attempts transmitted. | Int32
> message-succrx | Total number of Message success received. | Int32
> message-succtx | Total number of Message success transmitted. | Int32
> message-failrx | Total number of Message failures received. | Int32
> message-failtx | Total number of Message failures transmitted. | Int32
> message-3xx-rx | Total number of Message 3xx Responses received. | Int32
> message-3xx-tx | Total number of Message 3xx Responses transmitted. | Int32
> message-400-rx | Total number of Message 400 Responses received. | Int32
> message-400-tx | Total number of Message 400 Responses transmitted. | Int32
> message-403-rx | Total number of Message 403 Responses received. | Int32
> message-403-tx | Total number of Message 403 Responses transmitted. | Int32
> message-404-rx | Total number of Message 404 Responses received. | Int32
> message-404-tx | Total number of Message 404 Responses transmitted. | Int32
> message-415-rx | Total number of Message 415 Responses received. | Int32
> message-415-tx | Total number of Message 415 Responses transmitted. | Int32
> message-416-rx | Total number of Message 416 Responses received. | Int32
> message-416-tx | Total number of Message 416 Responses transmitted. | Int32
> message-420-rx | Total number of Message 420 Responses received. | Int32
> message-420-tx | Total number of Message 420 Responses transmitted. | Int32
> message-421-rx | Total number of Message 421 Response received. | Int32
> message-421-tx | Total number of Message 421 Responses transmitted. | Int32
> message-480-rx | Total number of Message 480 Responses received. | Int32
> message-480-tx | Total number of Message 480 Responses transmitted. | Int32
> message-488-rx | Total number of Message 488 Responses received. | Int32
> message-488-tx | Total number of Message 488 Responses transmitted. | Int32
> message-4xx-rx | Total number of Message 4xx Responses received. | Int32
> message-4xx-tx | Total number of Message 4xx Responses transmitted. | Int32
> message-500-rx | Total number of Message 500 Responses received. | Int32
> message-500-tx | Total number of Message 500 Responses transmitted. | Int32
> message-513-rx | Total number of Message 513 Responses received. | Int32
> message-513-tx | Total number of Message 513 Responses transmitted. | Int32
> message-5xx-rx | Total number of Message 5xx Responses received. | Int32
> message-5xx-tx | Total number of Message 5xx Responses transmitted. | Int32
> message-6xx-rx | Total number of Message 6xx Responses received. | Int32
> message-6xx-tx | Total number of Total Message 6xx Responses transmitted. | Int32
> callrejpdf | Total number of Call Rejects from PDF. | Int64
> callrejloc | Total number of Call Rejects from Proxy (local). | Int64
> sesstimeexp | Total number of Session Timer Expires. | Int64
> hssacc | Total number of HSS Accesses. | Int64
> emergcalls | Total number of Emergency Calls. | Int64
> emerg-priv-calls | Total number of User-requested Privacy Calls. Applicable only for E-CSCF. | Int64
> tollfreecalls | Total number of Toll Free Calls. | Int64
> premservcalls | Total number of Premium Service Calls. | Int64
> internationalcalls | Total number of International Calls. | Int64
> longDistancecalls | Total number of Long Distance Calls. | Int64
> opassistcalls | Total number of Operator Assisted Calls. | Int64
> dirassistcalls | Total number of Directory Assisted Calls. | Int64
> largerthansipmaxsize | Total number of Too Large SIP Messages. | Int64
> rtp-sent | Total number of RTP packets sent. | Int64
> rtp-recv | Total number of RTP packets received. | Int64
> msrp-sent | Total number of MSRP TCP packets sent. | Int64
> msrp-recv | Total number of MSRP TCP packets received. | Int64
> callrel-from-ue | Total number of Call Releases initiated by UE. | Int64
> callrel-from-nw | Total number of Call Releases initiated by Network. | Int64
> callrel-from-radioloss | Total number of Call Releases initiated by Radio Loss. | Int64
> callrel-from-local | Total number of Call Releases initiated by CSCF (Local). | Int64
> sigcomp-req-comp | Total number of Requests Compressed. | Int64
> sigcomp-req-decomp | Total number of Requests Decompressed. | Int64
> sigcomp-resp-comp | Total number of Responses Compressed. | Int64
> sigcomp-resp-decomp | Total number of Responses Decompressed. | Int64
> sigcomp-nack-rx | Total number of NACK Packets received. | Int64
> sigcomp-nack-tx | Total number of NACK Packets transmitted. | Int64
> sigcomp-comp-fail | Total number of Compression Failures. | Int64
> sigcomp-decomp-fail | Total number of Decompression Failures. | Int64
> sigcomp-bestout-compratio | Best Outgoing Message Compression Ratio | Float
> sigcomp-worstout-compratio | Worst Outgoing Message Compression Ratio | Float
> sigcomp-bestin-compratio | Best Incoming Message Compression Ratio | Float
> sigcomp-worstin-compratio | Worst Incoming Message Compression Ratio | Float
> sigcomp-averagein- compratio | Average Incoming Message Compression Ratio | Float
> sigcomp-averageout- compratio | Average Outgoing Message Compression Ratio | Float
> min-invite-proc-time | Minimum Invite Process Time | Int32
> max-invite-proc-time | Maximum Invite Process Timer | Int32
> min-first-resp-time | Minimum First Response Time | Int32
> max-first-resp-time | Maximum First Response Time | Int32
> min-post-dial-delay | Minimum Post-Dial Delay | Int32
> max-post-dial-delay | Maximum Post-Dial Delay | Int32
> min-session-setup-delay | Minimum Session Setup Delay | Int32
> max-session-setup-delay | Maximum Session Setup Delay | Int32
> min-post-answer-delay | Minimum Post Answer Delay | Int32
> max-post-answer-delay | Maximum Post Answer Delay | Int32
> min-session-rel-delay | Minimum Session Release Delay | Int32
> max-session-rel-delay | Maximum Session Release Delay | Int32
> active-tcp-conn | Total number of Active TCP connections. | Int64
> closed-tcp-conn | Total number of Closed TCP connections. | Int64
> succ-tcp-conn-out | Total number of Successful Outgoing connections. | Int64
> fail-tcp-conn-out | Total number of Failed Outgoing connections. | Int64
> succ-tcp-conn-in | Total number of Successful Incoming connections. | Int64
> fail-tcp-conn-in | Total number of Failed Incoming connections. | Int64
> migrated-tcp-conn | Total number of TCP connections migrated from Cscfmgr to Sessmgr for load balancing. | Int64
> packet-tcp-rx | Total number of TCP/IP packets received by CSCF service. | Int64
> packet-tcp-tx | Total number of TCP/IP packets transmitted by CSCF service. | Int64
> bytes-tcp-rx | Total number of TCP/IP bytes received by CSCF service. | Int64
> bytes-tcp-tx | Total number of TCP/IP bytes transmitted by CSCF service. | Int64
> message-tcp-request-rx | Total number of TCP requests received over TCP. | Int64
> message-tcp-request-tx | Total number of TCP requests transmitted over TCP. | Int64
> message-tcp-response-rx | Total number of TCP responses received over TCP. | Int64
> message-tcp-response-tx | Total number of TCP responses transmitted over TCP. | Int64
> message-tcp-mtu-switch | Total number of times CSCF switched from UDP to TCP because of message size larger than MTU. | Int64
> reg-rejdueto-secagree | Total number of Registration Rejects due to Security Agreement | Int64
> reg-rejdueto-algomismatch | Total number of Registration Rejects due to Algorithm Mismatch | Int64
> msg-drops-duetoerror | Total number of Message drops due to error. | Int64
> sec-rereg | Total number of Secure re-registrations | Int64
> sec-dereg | Total number of Secure de-registrations | Int64
> msgs-withincorr-sec-verify | Total number of Messages with Incorrect security Verify | Int64
> sec-assoc-rejects | Total number of Security Associations rejected. | Int64
> sub-with-sec-conn | Total number of Subscribers with secure connections. | Int32
> sub-with-unsec-conn | Total number of Subscribers with unsecure connections. | Int32
> ipsec-pktrx | Total number of IP-Sec Packets received. | Int64
> ipsec-pkttx | Total number of IP-Sec Packets transmitted. | Int64
> ipsec-octrx | Total number of IP-Sec Octets received. | Int64
> ipsec-octtx | Total number of IP-Sec Octets transmitted. | Int64
> active-ipsec-tcp-conn | Total number of Active IPSec TCP connections | Int64 Gauge
> closed-ipsec-tcp-conn | Total number of Closed IPSec TCP connections | Int64
> succ-ipsec-tcp-conn-out | Total number of Successful IPSec Outgoing connections | Int64
> fail-ipsec-tcp-conn-out | Total number of Failed IPSec Outgoing connections | Int64
> succ-ipsec-tcp-conn-in | Total number of Successful IPSec Incoming connections | Int64
> fail-ipsec-tcp-conn-in | Total number of Failed IPSec Incoming connections | Int64
> regreqrx | Total number of Register requests received. | Int64
> regreqtx | Total number of Register requests transmitted. | Int64
> invreqrx | Total number of Invite requests received. | Int64
> invreqtx | Total number of Invite requests transmitted. | Int64
> ackreqrx | Total number of ACK requests received. | Int64
> ackreqtx | Total number of ACK requests transmitted. | Int64
> byereqrx | Total number of Bye requests received. | Int64
> byereqtx | Total number of Bye requests transmitted. | Int64
> cancreqrx | Total number of Cancel requests received. | Int64
> cancreqtx | Total number of Cancel requests transmitted. | Int64
> optreqrx | Total number of Options requests received. | Int64
> optreqtx | Total number of Options requests transmitted. | Int64
> prackreqrx | Total number of PRACK requests received. | Int64
> prackreqtx | Total number of PRACK requests transmitted. | Int64
> subreqrx | Total number of Subscribe requests received. | Int64
> subreqtx | Total number of Subscribe requests transmitted. | Int64
> notreqrx | Total number of Notify requests received. | Int64
> notreqtx | Total number of Notify requests transmitted. | Int64
> refreqrx | Total number of Refer requests received. | Int64
> refreqtx | Total number of Refer requests transmitted. | Int64
> inforeqrx | Total number of Info requests received. | Int64
> inforeqtx | Total number of Info requests transmitted. | Int64
> updreqrx | Total number of Update requests received. | Int64
> updreqtx | Total number of Update requests transmitted. | Int64
> msgreqrx | Total number of Message requests received. | Int64
> msgreqtx | Total number of Message requests transmitted. | Int64
> pubreqrx | Total number of Publish requests received. | Int64
> pubreqtx | Total number of Publish requests transmitted. | Int64
> tryrsprx | Total number of Trying responses received. | Int64
> tryrsptx | Total number of Trying responses transmitted. | Int64
> rngrsprx | Total number of Ringing responses received. | Int64
> rngrsptx | Total number of Ringing responses transmitted. | Int64
> fwdrsprx | Total number of Forwarded responses received. | Int64
> fwdrsptx | Total number of Forwarded responses transmitted. | Int64
> quersprx | Total number of Queued responses received. | Int64
> quersptx | Total number of Queued responses transmitted. | Int64
> prgrsprx | Total number of Progress responses received. | Int64
> prgrsptx | Total number of Progress responses transmitted. | Int64
> 200-regrsprx | Total number of 200OK Register responses received. | Int64
> 200-regrsptx | Total number of 200OK Register responses transmitted. | Int64
> 200-invrsprx | Total number of 200OK Invite responses received. | Int64
> 200-invrsptx | Total number of 200OK Invite responses transmitted. | Int64
> 200-byersprx | Total number of 200OK Bye responses received. | Int64
> 200-byersptx | Total number of 200OK Bye responses transmitted. | Int64
> 200-cnlrsprx | Total number of 200OK Cancel responses received. | Int64
> 200-cnlrsptx | Total number of 200OK Cancel responses transmitted. | Int64
> 200-optrsprx | Total number of 200OK Options responses received. | Int64
> 200-optrsptx | Total number of 200OK Options responses transmitted. | Int64
> 200-prackrsprx | Total number of 200OK PRACK responses received. | Int64
> 200-prackrsptx | Total number of 200OK PRACK responses transmitted. | Int64
> 200-subrsprx | Total number of 200OK Subscribe responses received. | Int64
> 200-subrsptx | Total number of 200OK Subscribe responses transmitted. | Int64
> 200-notrsprx | Total number of 200OK Notify responses received. | Int64
> 200-notrsptx | Total number of 200OK Notify responses transmitted. | Int64
> 200-infrsprx | Total number of 200OK Info responses received. | Int64
> 200-infrsptx | Total number of 200OK Info responses transmitted. | Int64
> 200-updrsprx | Total number of 200OK Update responses received. | Int64
> 200-updrsptx | Total number of 200OK Update responses transmitted. | Int64
> 200-pubrsprx | Total number of 200OK Publish responses received. | Int64
> 200-pubrsptx | Total number of 200OK Publish responses transmitted. | Int64
> 200-refrsprx | Total number of 200OK Refer responses received. | Int64
> 200-refrsptx | Total number of 200OK Refer responses transmitted. | Int64
> 200-msgrsprx | Total number of 200OK Message responses received. | Int64
> 200-msgrsptx | Total number of 200OK Message responses transmitted. | Int64
> 202-refrsprx | Total number of 202Accepted Refer responses received. | Int64
> 202-refrsptx | Total number of 202Accepted Refer responses transmitted. | Int64
> 202-subrsprx | Total number of 202Accepted Subscribe responses received. | Int64
> 202-subrsptx | Total number of 202Accepted Subscribe responses transmitted. | Int64
> mchrsprx | Total number of Multiple Choices responses received. | Int64
> mchrsptx | Total number of Multiple Choices responses transmitted. | Int64
> mpersprx | Total number of Moved Permanently responses received. | Int64
> mpersptx | Total number of Moved Permanently responses transmitted. | Int64
> mtersprx | Total number of Moved Temporarily responses received. | Int64
> mtersptx | Total number of Moved Temporarily responses transmitted. | Int64
> upxrsprx | Total number of Use Proxy responses received. | Int64
> upxrsptx | Total number of Use Proxy responses transmitted. | Int64
> altrsprx | Total number of Alternative Service responses received. | Int64
> altrsptx | Total number of Alternative Service responses transmitted. | Int64
> brqerrrx | Total number of BadRequest errors received. | Int64
> brqerrtx | Total number of BadRequest errors transmitted. | Int64
> uauerrrx | Total number of UnAuthorized errors received. | Int64
> uauerrtx | Total number of UnAuthorized errors transmitted. | Int64
> prerrrx | Total number of Payment Required Errors received. | Int64
> prerrtx | Total number of Payment Required Errors transmitted. | Int64
> forerrrx | Total number of Forbidden errors received. | Int64
> forerrtx | Total number of Forbidden errors transmitted. | Int64
> nfderrrx | Total number of NotFound errors received. | Int64
> nfderrtx | Total number of NotFound errors transmitted. | Int64
> mnaerrrx | Total number of MethodNotAllowed errors received. | Int64
> mnaerrtx | Total number of MethodNotAllowed errors transmitted. | Int64
> nac406errrx | Total number of NotAcceptable(406) errors received. | Int64
> nac406errtx | Total number of NotAcceptable(406) errors transmitted. | Int64
> parerrrx | Total number of ProxyAuthRequired errors received. | Int64
> parerrtx | Total number of ProxyAuthRequired errors transmitted. | Int64
> rtoerrrx | Total number of RequestTimeout errors received. | Int64
> rtoerrtx | Total number of RequestTimeout errors transmitted. | Int64
> conferrrx | Total number of Conflict Errors received. | Int64
> conferrtx | Total number of Conflict Errors transmitted. | Int64
> lrerrrx | Total number of Length Required Errors received. | Int64
> lrerrtx | Total number of Length Required Errors transmitted. | Int64
> gonerrrx | Total number of Gone errors received. | Int64
> gonerrtx | Total number of Gone errors transmitted. | Int64
> crferrrx | Total number of ConditionalRequestFail errors received. | Int64
> crferrtx | Total number of ConditionalRequestFail errors transmitted. | Int64
> relerrrx | Total number of RequestEntityTooLarge errors received. | Int64
> relerrtx | Total number of RequestEntityTooLarge errors transmitted. | Int64
> rulerrrx | Total number of RequestURITooLong errors received. | Int64
> rulerrtx | Total number of RequestURITooLong errors transmitted. | Int64
> umterrrx | Total number of UnsupportedMediaType errors received. | Int64
> umterrtx | Total number of UnsupportedMediaType errors transmitted. | Int64
> uuserrrx | Total number of Unsupported URI Scheme errors received. | Int64
> uuserrtx | Total number of Unsupported URI Scheme errors transmitted. | Int64
> bexerrrx | Total number of BadExtension errors received. | Int64
> bexerrtx | Total number of BadExtension errors transmitted. | Int64
> exrerrrx | Total number of Extension Required errors received. | Int64
> exrerrtx | Total number of Extension Required errors transmitted. | Int64
> sitserrrx | Total number of Session Interval Too Small errors received | Int64
> sitserrtx | Total number of Session Interval Too Small errors transmitted | Int64
> fhloerrrx | Total number of First Hop Lacks Outbound Support (439) errors received. | Int64
> fhloerrtx | Total number of First Hop Lacks Outbound Support (439) errors transmitted. | Int64
> itberrrx | Total number of Interval Too Brief errors received. | Int64
> itberrtx | Total number of Interval Too Brief errors transmitted. | Int64
> blierrrx | Total number of Bad Location Information errors received. | Int64
> blierrtx | Total number of Bad Location Information errors transmitted. | Int64
> tnaerrrx | Total number of TempNotAvailable errors received. | Int64
> tnaerrtx | Total number of TempNotAvailable errors transmitted. | Int64
> tdnerrrx | Total number of Transaction Does Not Exist errors received. | Int64
> tdnerrtx | Total number of Transaction Does Not Exist errors transmitted. | Int64
> ldterrrx | Total number of LoopDetected errors received. | Int64
> ldterrtx | Total number of LoopDetected errors transmitted. | Int64
> tmherrrx | Total number of TooManyHops errors received. | Int64
> tmherrtx | Total number of TooManyHops errors transmitted. | Int64
> adierrrx | Total number of AddrIncomplete errors received. | Int64
> adierrtx | Total number of AddrIncomplete errors transmitted. | Int64
> amberrrx | Total number of Ambiguous errors received. | Int64
> amberrtx | Total number of Ambiguous errors transmitted. | Int64
> bhrerrrx | Total number of BusyHere errors received. | Int64
> bhrerrtx | Total number of BusyHere errors transmitted. | Int64
> rqcerrrx | Total number of RequestCancel errors received. | Int64
> rqcerrtx | Total number of RequestCancel errors transmitted. | Int64
> namerrrx | Total number of NotAcceptableMedia errors received. | Int64
> namerrtx | Total number of NotAcceptableMedia errors transmitted. | Int64
> beerrrx | Total number of Bad Event errors received. | Int64
> beerrtx | Total number of Bad Event errors transmitted. | Int64
> trperrrx | Total number of Request Pending errors received. | Int64
> trperrtx | Total number of Request Pending errors transmitted. | Int64
> udperrrx | Total number of Undecipherable errors received. | Int64
> udperrtx | Total number of Undecipherable errors transmitted. | Int64
> sarerrrx | Total number of sec-agree Required Errors received. | Int64
> sarerrtx | Total number of Sec-agree Required Errors transmitted. | Int64
> ineerrrx | Total number of InternalError errors received. | Int64
> ineerrtx | Total number of InternalError errors transmitted. | Int64
> nimerrrx | Total number of NotImplemented errors received. | Int64
> nimerrtx | Total number of NotImplemented errors transmitted. | Int64
> bgterrrx | Total number of BadGateway errors received. | Int64
> bgterrtx | Total number of BadGateway errors transmitted. | Int64
> suaerrrx | Total number of ServiceUnavailable errors received. | Int64
> suaerrtx | Total number of ServiceUnavailable errors transmitted. | Int64
> gtterrrx | Total number of GatewayTimeout errors received. | Int64
> gtterrtx | Total number of GatewayTimeout errors transmitted. | Int64
> bsverrrx | Total number of BadSipVersion errors received. | Int64
> bsverrtx | Total number of BadSipVersion errors transmitted. | Int64
> mtlerrrx | Total number of Message Too Large errors received. | Int64
> mtlerrtx | Total number of Message Too Large errors transmitted. | Int64
> pcferrrx | Total number of Precondition Failure errors received. | Int64
> pcferrtx | Total number of Precondition Failure errors transmitted. | Int64
> bewerrrx | Total BusyEverywhere errors received. Total number of | Int64
> bewerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> decerrrx | Total number of Decline errors received. | Int64
> decerrtx | Total number of Decline errors transmitted. | Int64
> neaerrrx | Total number of NotExistAnywhere errors received. | Int64
> neaerrtx | Total number of NotExistAnywhere errors transmitted. | Int64
> nac606errrx | Total number of NotAcceptable(606) errors received. | Int64
> nac606errtx | Total number of NotAcceptable(606) errors transmitted. | Int64
> callsetuptime | Sum of setup times – For calculating average call setup time. | Int64
> callscounted | Total number of calls, for which setup time is added in setup times. | Int64
> tot-sip-invalid-msgs-rx | Total number of SIP Invalid Messages received. | Int64
> tot-sip-msgs-rx | Total number of SIP Messages received. | Int64
> tot-sip-msgs-tx | Total number of SIP Messages transmitted. | Int64
> tot-sip-msgs-proc | Total number of SIP Messages Processed. | Int64
> regreqretx | Total number of REGISTER Requests Re-transmitted. | Int64
> invreqretx | Total number of INVITE Requests Re-transmitted. | Int64
> byereqretx | Total number of BYE Requests Re-transmitted. | Int64
> cancreqretx | Total number of CANCEL Requests Re-transmitted. | Int64
> ackreqretx | Total number of ACK Requests Re-Transmitted | Int64
> notifyreqretx | Total number of NOTIFY Requests Re-Transmitted | Int64
> publishreqretx | Total number of PUBLISH Requests Re-Transmitted | Int64
> referreqretx | Total number of REFER Requests Re-Transmitted | Int64
> subscribereqretx | Total number of SUBSCRIBE Requests Re-Transmitted | Int64
> req-retx | Total number of SIP Requests Re-transmitted. | Int64
> resp-retx | Total number of SIP Responses Re-Transmiited. | Int64
> reqresp-retx | Total number of SIP messages Re-transmitted. | Int64
> calldur-lt-01sec | Total calls with duration less than 01 sec. | Int32
> calldur-01to10sec | Total calls with duration between 01 and 10 seconds. | Int32
> calldur-10to30sec | Total calls with duration between 10 and 30 seconds. | Int32
> calldur-30to60sec | Total calls with duration between 30 and 60 seconds. | Int32
> calldur-60to90sec | Total calls with duration between 60 and 90 seconds. | Int32
> calldur-90to120sec | Total calls with duration between 90 and 120 seconds. | Int32
> calldur-120to150sec | Total calls with duration between 120 and 150 seconds. | Int32
> calldur-150to180sec | Total calls with duration between 150 and 180 seconds. | Int32
> calldur-03to04min | Total calls with duration between 03 and 04 minutes. | Int32
> calldur-04to05min | Total calls with duration between 04 and 05 minutes. | Int32
> calldur-05to06min | Total calls with duration between 05 and 06 minutes. | Int32
> calldur-06to07min | Total calls with duration between 06 and 07 minutes. | Int32
> calldur-07to08min | Total calls with duration between 07 and 08 minutes. | Int32
> calldur-08to09min | Total calls with duration between 08 and 09 minutes. | Int32
> calldur-09to11min | Total calls with duration between 09 and 11 minutes. | Int32
> calldur-11to13min | Total calls with duration between 11 and 13 minutes. | Int32
> calldur-13to15min | Total calls with duration between 13 and 15 minutes. | Int32
> calldur-15to17min | Total calls with duration between 15 and 17 minutes. | Int32
> calldur-17to19min | Total calls with duration between 17 and 19 minutes. | Int32
> calldur-19to21min | Total calls with duration between 19 and 21 minutes. | Int32
> calldur-21to23min | Total calls with duration between 21 and 23 minutes. | Int32
> calldur-23to25min | Total calls with duration between 23 and 25 minutes. | Int32
> calldur-25to27min | Total calls with duration between 25 and 27 minutes. | Int32
> calldur-27to29min | Total calls with duration between 27 and 29 minutes. | Int32
> calldur-29to60min | Total calls with duration between 29 and 60 minutes. | Int32
> calldur-gt-60min | Total calls with duration more than 60 minutes. | Int32
> subsetup<200ms | Total number of subscriptions setup in less than 200 milliseconds. | Int32
> subsetup200-400ms | Total number of subscriptions setup in 200 to 400 milliseconds. | Int32
> subsetup400-600ms | Total number of subscriptions setup in 400 to 600 milliseconds. | Int32
> subsetup600-800ms | Total number of subscriptions setup in 600 to 800 milliseconds. | Int32
> subsetup800-1000ms | Total number of subscriptions setup in 800 to 1000 milliseconds. | Int32
> subsetup1000-1200ms | Total number of subscriptions setup in 1000 to 1200 milliseconds. | Int32
> subsetup1200-1400ms | Total number of subscriptions setup in 1200 to 1400 milliseconds. | Int32
> subsetup1400-1600ms | Total number of subscriptions setup in 1400 to 1600 milliseconds. | Int32
> subsetup1600-1800ms | Total number of subscriptions setup in 1600 to 1800 milliseconds. | Int32
> subsetup1800-2000ms | Total number of subscriptions setup in 1800 to 2000 milliseconds. | Int32
> subsetup2000-2200ms | Total number of subscriptions setup in 2000 to 2200 milliseconds. | Int32
> subsetup2200-2400ms | Total number of subscriptions setup in 2200 to 2400 milliseconds. | Int32
> subsetup2400-2600ms | Total number of subscriptions setup in 2400 to 2600 milliseconds. | Int32
> subsetup2600-2800ms | Total number of subscriptions setup in 2600 to 2800 milliseconds. | Int32
> subsetup2800-3000ms | Total number of subscriptions setup in 2800 to 3000 milliseconds. | Int32
> subsetup3-5sec | Total number of subscriptions setup in 3 to 5 seconds. | Int32
> subsetup5-7sec | Total number of subscriptions setup in 5 to 7 seconds. | Int32
> subsetup7-9sec | Total number of subscriptions setup in 7 to 9 seconds. | Int32
> subsetup9-11sec | Total number of subscriptions setup in 9 to 11 seconds. | Int32
> subsetup11-13sec | Total number of subscriptions setup in 11 to 13 seconds. | Int32
> subsetup13-15sec | Total number of subscriptions setup in 13 to 15 seconds. | Int32
> subsetup15-17sec | Total number of subscriptions setup in 15 to 17 seconds. | Int32
> subsetup17-19sec | Total number of subscriptions setup in 17 to 19 seconds. | Int32
> subsetup19-21sec | Total number of subscriptions setup in 19 to 21 seconds. | Int32
> subsetup>21sec | Total number of subscriptions setup in more than 21 seconds. | Int32
> subdur<1hr | Total number of subscription duration less than 1 hour. | Int32
> subdur1-2hr | Total number of subscription duration 1 to 2 hours. | Int32
> subdur2-3hr | Total number of subscription duration 2 to 3 hours. | Int32
> subdur3-4hr | Total number of subscription duration 3 to 4 hours. | Int32
> subdur4-5hr | Total number of subscription duration 4 to 5 hours. | Int32
> subdur5-6hr | Total number of subscription duration 5 to 6 hours. | Int32
> subdur6-7hr | Total number of subscription duration 6 to 7 hours. | Int32
> subdur7-8hr | Total number of subscription duration 7 to 8 hours. | Int32
> subdur8-9hr | Total number of subscription duration 8 to 9 hours. | Int32
> subdur9-10hr | Total number of subscription duration 9 to 10 hours. | Int32
> subdur>10hr | Total number of subscription duration more than 10 hours. | Int32
> curr-reg-subs | Total number of currently registered users. | Int64
> active-reg-subs | Total number of active registered users. | Int64
> curr-sigcomp-subs | Total number of currently registered SIGCOMP users. | Int64
> active-sigcomp-subs | Total number of active registered SIGCOMP users. | Int64
> curr-ipsec-subs | Total number of currently registered IPSEC users. | Int64
> active-ipsec-subs | Total number of active registered IPSEC users. | Int64
> active-voip-subs | Active registered VOIP users. | Int64
> curr-presence-subs | Total number of currently registered PRESENCE users. | Int64
> active-presence-subs | Total number of active registered PRESENCE users. | Int64
> active-im-subs | Total number of active registered IM users. | Int64
> dpeca-curr-sessions | The total number of DPECA sessions currently active. | Int32
> dpeca-tot-sess-init | Total number of DPECA sessions initiated by sending AAR Initial Request message. | Int32
> dpeca-tot-sess-terminated | Total number of terminated DPECA sessions. | Int32
> dpeca-tot-sess-failovers | Total number of peer-switches attempted. | Int32
> dpeca-tot-sess-failover-err | Total number of peer-switches failed. | Int32
> dpeca-tot-msg-received | Total number of messages received. | Int32
> dpeca-tot-msg-sent | Total number of messages sent. | Int32
> dpeca-tot-aar-sent | Total number of AAR request messages sent from DPECA module. | Int32
> dpeca-tot-aaa-received | Total number of AAA answer messages received. | Int32
> dpeca-tot-uncorr-aaa | Total number of Uncorrelated AAA messages. | Int32
> dpeca-tot-uncorr-sta | Total number of Uncorrelated STA messages. | Int32
> dpeca-tot-aari-sent | Total number of AAR Initial requests sent. | Int32
> dpeca-tot-aaai-received | Total number of AAA answer messages received in response to the AAR-Initial requests. | Int32
> dpeca-tot-aaai-accepted | Total number of AAA messages accepted as successful without any errors. | Int32
> dpeca-tot-aaai-rejected | Total number of AAA messages rejected as erroneous. | Int32
> dpeca-tot-aaai-timeout | Total number of AAA answers to Initial request timed out. | Int32
> dpeca-tot-aaru-sent | Total number of AAR Update messages sent | Int32
> dpeca-tot-aaau-received | Total number of AAA answer messages received in response to the AAR-Update requests. | Int32
> dpeca-tot-aaau-timeout | Total number of AAA answers to Update request timed out. | Int32
> dpeca-tot-str-sent | Total number of STR messages sent. | Int32
> dpeca-tot-sta-received | Total number of STA messages received. | Int32
> dpeca-tot-sta-timeout | Total number of STA answers timed out. | Int32
> dpeca-tot-asr-received | Total number of ASR messages received. | Int32
> dpeca-tot-asa-sent | Total number of ASA messages sent. | Int32
> dpeca-tot-rar-received | Total number of RAR messages received. | Int32
> dpeca-tot-raa-sent | Total number of RAA messages sent. | Int32
> dpeca-tot-protocol-err | Total number of diameter protocol errors that were received from PCRF. | Int32
> dpeca-tot-aaa-parse-err | Total number of AAA parse-errors. | Int32
> dpeca-tot-unk-sess-req | Total number of unknown session requests. | Int32
> dpeca-tot-unk-cmd-codes | Total number of unknown command codes (unsupported command codes). | Int32
> dpeca-tc-logout | Total number of sessions terminated as the user logged out. | Int32
> dpeca-tc-service-not-prov | Total number of sessions terminated as the requested service is not provided. | Int32
> dpeca-tc-bad-ans | Total number of sessions terminated with a bad answer. | Int32
> dpeca-tc-administrative | Total number of sessions terminated administratively. | Int32
> dpeca-tc-link-broken | Total number of sessions terminated due to link broken. | Int32
> dpeca-tc-auth-expired | Total number of sessions terminated due to auth-expiry. | Int32
> dpeca-tc-user-moved | Total number of sessions terminated as the user-moved. | Int32
> dpeca-tc-session-timeout | Total number of sessions terminated due to session timeout. | Int32
> dpeca-auth-rejected | Total number of authorization rejected errors. | Int32
> dpeca-other-errors | Total number of other miscellaneous DPECA errors. | Int32
> dpeca-exp-res-invalid- service-info | Total number of answer messages received with Experimental-Result-Code as 5061 - INVALID_SERVICE_INFORMATION. | Int32
> dpeca-exp-res-filter- restrictions | Total number of answer messages received with Experimental-Result-Code as 5062 - FILTER_RESTRICTIONS. | Int32
> dpeca-exp-res-req-service- not-authorized | Total number of answer messages received with Experimental-Result-Code as 5063 - REQUESTED_SERVICE_NOT_AUTHORIZED. | Int32
> dpeca-exp-res-duplicated-af-session | Total number of answer messages received with Experimental-Result-Code as 5064 - DUPLICATED_AF_SESSION. | Int32
> dpeca-exp-res-ipcan-session-not-avail | Total number of answer messages received with Experimental-Result-Code as 5065 - IP_CAN_SESSION_NOT_AVAILABLE | Int32
> perf-att-init-reg | Total number of initial registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-init-reg-3gpp-geran | Total number of initial registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-3gpp-utran- fdd | Total number of initial registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-3gpp2-1x | Total number of initial registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-ieee-80211a | Total number of initial registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-ieee-80211b | Total number of initial registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-other-at | Total number of initial registrations received at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg | Total number of success responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-init-reg-3gpp- geran | Total number of success responses sent for initial registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-3gpp-utran-fdd | Total number of success responses sent for initial registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-3gpp2-1x | Total number of success responses sent for initial registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-ieee- 80211a | Total number of success responses sent for initial registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-ieee- 80211b | Total number of success responses sent for initial registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-other | Total number of success responses sent for initial registration for any other access technologies. Applicable only for P-CSCF. | Int64
> perf-fail-init-reg | Total number of failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-401 | Total number of (401 Unauthorized) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-403 | Total number of (403 Forbidden) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-404 | Total number of (404 Not Found) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-420 | Total number of (420 Bad Extension) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-500 | Total number of (500 Internal Error) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-other | Total number of other failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-mean-init-reg-setup | Average time (in milliseconds) between the instance REGISTER is received by P-CSCF and 200 response is sent for the REGISTER. The average is reset every 10 minutes. Applicable only for P-CSCF. | Int32/Gauge
> perf-att-rereg | Total number of refresh registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-rereg-3gpp-geran | Total number of refresh registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-rereg-3gpp-utran-fdd | Total number of refresh registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-rereg-3gpp2-1x | Total number of refresh registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-rereg-ieee-80211a | Total number of refresh registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-rereg-ieee-80211b | Total number of refresh registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-rereg-other-at | Total number of refresh registrations received at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-rereg | Total number of success responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-rereg-3gpp-geran | Total number of success responses sent for refresh registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-3gpp-utran- fdd | Total number of success responses sent for refresh registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-3gpp2-1x | Total number of success responses sent for refresh registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-ieee-80211a | Total number of success responses sent for refresh registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-ieee-80211b | Total number of success responses sent for refresh registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-other | Total number of success responses sent for refresh registration for any other access technology. Applicable only for P-CSCF. | Int64
> perf-fail-rereg | Total number of failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF | Int64
> perf-fail-rereg-401 | Total number of (401 Unauthorized) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-403 | Total number of (403 Forbidden) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-404 | Total number of (404 Not Found) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-420 | Total number of (420 Bad Extension) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-500 | Total number of (500 Internal Error) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-other | Total number of other failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-ue | Total number of de-registrations received from UE at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-ue-3gpp- geran | Total number of de-registrations received from UE at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-3gpp-utran-fdd | Total number of de-registrations received from UE at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-3gpp2-1x | Total number of de-registrations received from UE at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-ieee- 80211a | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-ieee- 80211b | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-other-at | Total number of de-registrations received from UE at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue | Total number of success responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-dereg-ue-3gpp- geran | Total number of success responses sent for de-registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-3gpp- utran-fdd | Total number of success responses sent for de-registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue- 3gpp2-1x | Total number of success responses sent for de-registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-ieee- 80211a | Total number of success responses sent for de-registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-ieee- 80211b | Total number of success responses sent for de-registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-other | Total number of success responses sent for de-registration for any other access technology. Applicable only for P-CSCF. | Int64
> perf-fail-dereg-ue | Total number of failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF | Int64
> perf-fail-dereg-ue-401 | Total number of (401 Unauthorized) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-403 | Total number of (403 Forbidden) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-404 | Total number of (404 Not Found) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-420 | Total number of (420 Bad Extension) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-500 | Total number of (500 Internal Error) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-other | Total number of other failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-hss | Total number of de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-dereg-hss | Total number of success responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss | Total number of failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-other | Total number of other failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-dereg-serv | Total number of de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-dereg-serv | Total number of success responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv | Total number of failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-other | Total number of other failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-3rdparty-reg | Total number of 3rd Party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-3rdparty-reg | Total number of success responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg | Total number of failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-401 | Total number of (401 Unauthorized) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-403 | Total number of (403 Forbidden) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-404 | Total number of (404 Not Found) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-420 | Total number of (420 Bad Extension) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-500 | Total number of (500 Internal Error) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-other | Total number of other failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-uar | Total number of user registration status query procedures attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-succ-uaa | Total number of success response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-fail-uaa | Total number of failure response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-att-sar | Total number of S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-succ-saa | Total number of success responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-fail-saa | Total number of failure responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-att-session | Total number of attempted session establishments at CSCF. | Int64
> perf-succ-session-180 | Total number of 180 responses for successful session establishments at CSCF. | Int64
> perf-succ-session-200 | Total number of 200 responses (without 180 response) for successful session establishments at CSCF. | Int64
> perf-ans-session | Total number of 200 responses for session establishments at CSCF. | Int64
> perf-fail-session | Total number of failure responses for session establishments at CSCF. | Int64
> perf-att-lir | Total number of user location query procedures attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-succ-lia | Total number of success responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-fail-lia | Total number of failure responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-att-session-frm-oth- domain | Total number of session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-frbdn-session-frm-oth- domain | Total number of forbidden sessions for session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-att-session-to-oth-domain | Total number of session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. |
> perf-frbdn-session-to-oth-domain | Total number of forbidden sessions for session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-att-init-reg-visited | Total number of initial registrations of visiting users from other IMS network domains. Applicable only for P-CSCF. | Int64
> perf-frbdn-init-reg-visited | Total number of forbidden messages sent for the visiting users. Applicable only for P-CSCF. | Int64
> perf-rmg-users-out | Total number of roaming users to other network domains. Applicable only for S-CSCF. | Int64
> perf-att-mar | Total number of Multimedia-Authentication-Requests attempted. Applicable only for S-CSCF. | Int64
> perf-succ-maa | Total number of successful Multimedia-Authentication-Answers received. Applicable only for S-CSCF. | Int64
> perf-fail-maa | Total number of failure Multimedia-Authentication-Answers received. Applicable only for S-CSCF. | Int64
> perf-att-ppr | Total number of HSS-initiated user profile updates attempted. Applicable only for S-CSCF. | Int64
> perf-succ-ppa | Total number of success responses for HSS-initiated user profile update. Applicable only for S-CSCF. | Int64
> perf-fail-ppa | Total number of failure responses for HSS-initiated user profile update. Applicable only for S-CSCF. | Int64
> perf-att-subscribe | Total number of subscription procedures attempted at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-subscribe | Total number of success responses for subscriptions. Applicable only for S-CSCF. | Int64
> perf-fail-subscribe | Total number of failure responses for subscriptions. Applicable only for S-CSCF. | Int64
> perf-att-notify | Total number of notify procedures attempted at S-CSCF. Applicable only for S-CSCF. | Int64Int64
> perf-succ-notify | Total number of success responses for notify. Applicable only for S-CSCF. | Int64
> perf-fail-notify | Total number of failure responses for notify. Applicable only for S-CSCF. | Int64
> de2a-session-init | Total number of DE2A sessions initiated by sending UDR message. | Int32
> de2a-session-active | Total number of DE2A sessions currently active. | Int32
> de2a-udr-sent | Total number UDR messages sent. | Int32
> de2a-uda-received | Total number of UDA messages received | Int32
> de2a-uda-err-3xxx | Total number of messages with protocol errors. | Int32
> de2a-uda-parse-err | Total number of bad UDA messages received. | Int32
> de2a-udr-err | Total number of UDR send errors. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883