> show ggsn-service
> This chapter includes the show ggsn-service command output tables.
> show ggsn-service sgsn-table
> show ggsn-service sgsn-table Command Output Descriptions

> Field | Description
> GTP Version | GPRS Tunnelling Protocol. (0) - GTPRS (1) - UMTS
> Active | GTP condition. (I) - Inactive (A) - Active
> GTPC Echo | GPRS Tunneling Protocol-Control message (D) - Disabled (E) - Enabled
> PLMN Type | Public land mobile network type. (H) - Home (F) - Foreign (U) - Unknown
> SGSN Stats | SGSN statistics. (A) - Available (U) - Unavailable
> Service ID | GGSN Service ID.
> SGSN Address | IP address of each active SGSN.
> Restart Counter | The restart counter sent by the SGSN. Increments by 1 with each restart.
> Number of Restarts | Number of times the restart of the particular SGSN is detected, i.e., the number of times a NEW restart counter is received from the SGSN in a GTPC request message.
> Curr Subs | Number of current subscribers to each SGSN.
> Max Subs | Maximum number of permitted subscribers to each SGSN.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883