> HNB-PS Network Configuration Mode Commands
> The HNB-PS Network Configuration Mode is used to create, provide, and manage the Packet Switched (PS) network instance on HNB-GW service to provide HNB access with PS core network in a 3G UMTS network.
> associate gtpu-service
> This command associates a previously configured GTP-U service to bind the HNB-GW service to provide a GTP-U tunnel with an SGSN towards the core network side. A GTP-U service must be configured in Context configuration mode before using this configuration.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate gtpu-service svc_name context ctx_name
> no associate gtpu-service
> no
> Removes the associated GTP-U service from this HNB-GW service configuration.
> svc_name
> Identifies the name of the GTP-U service preconfigured in Context configuration mode to associate with an HNB-GW service towards the Home-NodeB side.
> The svc_name is name of a preconfigured GTP-U service.
> context ctx_name
> Specifies the name of the context in which GTP-U service is configured.
> The ctx_name must be an existing context name in which this GTP-U service is configured.
> Usage
> Use this command to configure GTP-U data plan tunnel between HNB-GW service and GSNs in core network. The serivce defined for GTP-U tunnel must be configured in Context configuration mode.
> Important: Another GTP-U service can be used to bind the HNB-GW service to GTP-U tunnel with HNB in HNB access network and can be configured in HNB-GW Service Configuration mode. For more information on GTP-U service configuration, refer GTP-U Service Configuration Mode Commands.
> Example
> Following command associates GTP-U service gtpu_svc1 configured in conext named Ctx_gtpu1 with specific HNB-PS network instance for GTP-U tunnel towards GSN in core network:
> associate gtpu-service gtpu_svc1 context Ctx_gtpu1
> associate-sccp-network
> This command associates a previously defined Signaling Connection Control Part (SCCP) network id with the PS network instance in order to route the messages towards SGSN over IuPS interface.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate-sccp-network sccp_net_id
> no associate-sccp-network
> no
> Removes the associated SCCP network configuration instance from this HNB-PS network instance configuration.
> sccp_net_id
> Identifies a predefined SCCP network id to associate with an HNB-PS network instance over IuPS/IuFlex interface to enable connection with SGSN(s).
> The sccp_network_num must be a predefined SCCP instance in Global configuration mode.
> Usage
> Use this command to associate a predefined SCCP network id with the IuPS interface in HNB-GW service to connect with PS network elements; i.e. SGSN.
> Caution: The SCCP network id must be defined in Global Configuration mode before using it with this command.
> Important: A single SCCP network id can not be shared with multiple HNB-PS network instances.
> Example
> Following command associates SCCP network id 2 with specific HNB-PS network instance:
> associate-sccp-network 2
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> sgsn point-code
> This command is used to configure default SGSN point-code with HNB-PS network instance. This command is used when HNB-GW is to be connected to only one SGSN with in a PS network or as default SGSN for all HNBs connected through specific HNB-PS network instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] sgsn point-code point_code
> no
> Removes the configured default SGSN point code from specific HNB-PS network instance.
> Caution: Removing the SGSN point code is a disruptive operation and affects all HNB sessions which are connected to particular SGSN through an HNB-PS network instance.
> point_code
> Specifies SS7 address of default SGSN in PS network in point code value to this configured HNB-PS network instance.
> point_code must be in SS7 point code dotted-decimal ###.###.### format or 8-digit decimal ######## format.
> Only one instance of this command can be configured.
> Usage
> Use this command to configure a default SGSN to which HNB will connect for PS network access through HNB-GW service.
> Point-code is an SS7 address for an element in the SS7 network. Point-codes must be defined in dotted-decimal format in a string of 1 to 11 digits. Format options include:

> • | 0.0.1 to 7.255.7 for point-code in the ITU range.

> • | 0.0.1 to 255.255.255 for point-code in the ANSI range.

> • | 0.0.1 to 15.31.255 for point-code in the TTC Range.

> • | a string of 1 to 11 digits in dotted-decimal to represent a point-code in a different range.

> Important: This command can be entered only once. If entered again the previous value shall be overwritten.
> Example
> The following command configures a default SGSN with point code 1 01.201.101 for HNBs to access PS network through HNB-GW service in this HNB-PS network instance:
> sgsn point-code 101.201.101

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883