> Exec Mode Show Commands (T-Z)
> This section includes the commands show task through show version.
> show task
> Displays information about system tasks.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show task { info | resources | table } [ card card_num ] [ facility facility { all | instance id } ] [ process process_name all ] [ max ] [ | { grep grep_options | more } ]
> { info | resources | table }
> Specifies type of information to be displayed and scope of tasks to include in output.
> info: Display detailed task information.
> resources: Display resource allocation and usage information for all tasks.
> table: Display identification information in tabular format for all tasks.
> card card_num
> Default: all powered on cards.
> Specifies a single card for which task information is to be displayed where card_num must be from 1 to 48.
> facility facility { all | instance id }
> Default: all facilities.
> Specifies the list of facilities for which task information may be displayed. A specific instance of the facility may be displayed as specified by id or all instances may be displayed. The value of id must be in the range of 0 through 100000. facility must be one of:

> • | a11mgr: A11 Interface Manager facility

> • | aaamgr: AAA Manager Facility

> • | aaaproxy: AAA Proxy manager Facility

> • | acsctrl: Active Charging Service (ACS) Controller Facility

> • | acsmgr: Active Charging Service (ACS) Manager Facility

> • | asngwmgr: ASN Gateway Manager

> • | asnpcrmgr: ASN Paging/Location-Registry (ASN-PC) Manager

> • | bgp: Border Gateway Protocol (BGP) Facility

> • | bulkstat: Bulk Statistics Manager Facility

> • | cdrmod: Charging Detail Record Module

> • | cli: Command Line Interface Facility

> • | cscfmgr: SIP CSCF Manager

> • | cspctrl: Card Slot Port controller Facility

> • | cssctrl: Content Service Steering Controller

> • | dcardctrl: IPSEC Daughtercard Controller Logging Facility

> • | dcardmgr: IPSEC Daughtercard Manager Logging Facility

> • | dhmgr: Distributed Host Manager

> • | drvctrl: Driver Controller Facility

> • | egtpegmgr: EGTP Egress Demux Manager

> • | egtpinmgr: EGTP Ingress Demux Manager

> • | evlogd: Event Log Daemon Facility

> • | famgr: Foreign Agent Manager Facility

> • | gtpcmr: GTP-C Protocol Logging facility (GGSN product only)

> • | h248prt: H.248 Protocol Task

> • | hamgr: Home Agent Manager Facility

> • | hatcpu: High Availability Task CPU Facility

> • | hatsystem: High Availability Task Facility

> • | ipsecctrl: IP Security Controller Facility

> • | ipsecmgr: IP Security Manager Facility

> • | ipsgmgr: IP Services Gateway Facility

> • | l2tpdemux: L2TP Demultiplexor (LNS) Facility

> • | l2tpmgr: L2TP Manager Facility

> • | magmgr: Mobile Access Gateway Manager

> • | megadiammgr: MegaDiameter Manager

> • | mmedemux: MME Demux Manager logging facility

> • | mmemgr: MME Manager logging facility

> • | mmgr: SGSN/SS7 Master Manager

> • | mptest: Migration Performance Test on Packet Accelerator Card

> • | netwstrg: Network Storage Manager

> • | npuctrl: Network Processor Unit control Facility

> • | npumgr: Network Processor Unit Manager Facility

> • | nputst: Network Processor Unit Tester

> • | nsctrl: Charging Service Controller

> • | nsmgr: Charging Service Process Manager

> • | orbns: Object Request Broker Notification Server Facility

> • | orbs: Object Request Broker System Facility

> • | ospf: Open Shortest Path First Facility

> • | rct: Recovery Control Task Facility

> • | rdt: Redirect Task Facility

> • | rip: Routing Information Protocol Facility

> • | rmctrl: Resource Manager Controller Facility

> • | rmmgr: Resource Manager Facility

> • | sct: Shared Configuration Task Facility

> • | sessctrl: Session Controller Facility

> • | sessmgr: Session Manager Facility

> • | sft: Switch Fabric Monitoring Task

> • | sipcdprt: Sip Call Distributor Task

> • | sitmain: System Initialization Task Main Facility

> • | sitparent: Card based system initialization facility that applies to Packet Accelerator Cards and Switch Processor Cards

> Important: sitparent replaces the facilities sitpac, sitspc and sittac.

> • | snmp: SNMP Protocol Facility

> • | srdb: Static Rating Database

> • | threshold: Threshold Server Facility

> • | vpnctrl: Virtual Private Network Controller Facility

> • | vpnmgr: VPN Manager Facility

> • | zebos: ZEBOS™ OSPF Message Facility

> all: Display information for all instances of the specified facility.
> instance id: Display information for the specified instance of the specified facility only. id must be an integer from 0 through 10000000.
> process process_name all
> Display information for all instances of the specified process. must be one of the following process names:

> • | ftpd: File Transfer Protocol Daemon

> • | inetd: Internet Super-server Daemon

> • | nsproc: NetSpira Packet Processor

> • | ntpd: Network Time Protocol Daemon

> • | orbnsd: Object Request Broker Notification Server

> • | ping: Ping

> • | pvmd-wrapper: NetSpira Messenger Daemon

> • | pvmgs: NetSpira Messenger Daemon

> • | rlogin: Remote Login

> • | sftp-server: Secure File Transfer Protocol Server

> • | sitreap: System Initialization Task Cleanup Process

> • | sn_resolve: DNS Resolver Process

> • | ssh: Secure Shell

> • | sshd: Secure Shell Daemon

> • | telnet: Telnet

> • | telnetd: Telnet Daemon

> • | tftpd: Trivial File Transfer Protocol Daemon

> • | traceroute: Traceroute

> max
> Default: current usage levels are displayed.
> Displayed the maximum usage levels for tasks as opposed to the current usage levels.
> The keyword max is valid only in conjunction with the resources keyword.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Display task information as part of system troubleshooting unexpected behavior.
> Important: This command is not supported on all platforms.
> Example
> The following commands provide some examples of the combinations of options that may be used to display task information.
> show task info facility hatspc all
> show task info facility hatspc instance 456
> show task resources facility zebos all
> show task table facility ospf
> show task table card 8 facility cli all
> show task resources facility rip all max
> show temperature
> Displays the current temperature on all installed application and line cards. Also displays the temperature of upper and lower fan trays. Temperature readings are acquired from sensors located on theses components.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show temperature [ verbose] [ | { grep grep_options | more } ]
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> verbose
> Indicates that the output is to contain detailed information.
> Usage
> Verify current temperature of components in chassis.
> Example
> show temperature
> show tempterature verbose
> show terminal
> Displays the current terminal settings for number of lines in length and number of characters in width.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show terminal [ | { grep grep_options | more } ]
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Verify current terminal settings in case the output displayed appears to have line breaks/wraps in unexpected places.
> Example
> show terminal
> show threshold
> Displays thresholding information for the system.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show threshold [ default ]
> [ default ]
> Used to display the system’s thresholding default values.
> Usage
> Use this command to display information on threshold value configuration and activity.
> Example
> The following command displays configuration information pertaining to threshold values configured on the system:
> show threshold
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show timing
> Displays the information configured to define a transmit timing source other than the system clock. The display includes related information (such as port status, timing source priority, timing alarms, etc.) for all of the ports configured for either BITS or line timing.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show timing
> Usage
> Use this command to determine which line cards are recovering receive timing clocks.
> Important: This command is not supported on all platforms.
> Example
> The following command displays timing configuration and status information for the timing-configured ports.
> show timing
> show upgrade
> Displays the status of an on-going on-line software upgrade.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show upgrade
> Usage
> Use this command to show the status of an on-going on-line software upgrade.
> Important: This command is not supported on all platforms.
> show url-blacklisting database
> This command displays URL Blacklisting static database configurations.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show url-blacklisting database [ all | url url | facility acsmgr { all | instance instance } ] [ | { grep grep_options | more } ]
> all
> Displays configurations of all URL Blacklisting databases present in the default or override directory.
> facility acsmgr { all | instance instance }
> Displays configurations of URL Blacklisting database configuration per facility/ACSMgr instance.
> all: Displays URL Blacklisting database configuration of all ACSMgrs.
> instance instance: Displays URL Blacklisting database configuration of the specified instance. instance must be instance number of the database, and must be an integer from 1 through 10000000.
> url url
> Displays configurations of the URL Blacklisting database specified in the URL.
> url must be the database’s URL, and must be a string of 1 through 512 characters in length.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
> Usage
> Use this command to view configurations associated with in-memory and on-flash Blacklisting database. The show url-blacklisting database command displays the active database that is loaded, and is the one set by either the default or override CLI commands.
> Example
> The following command displays configurations of all the databases present in default or override directory, indicating one as ACTIVE and rest as NOT LOADED:
> show url-blacklisting database all
> The following command displays configurations of the /flash/bl/optblk.bin database:
> show url-blacklisting database url /flash/bl/optblk.bin
> The following command displays database configuration for the ACSMgr instance 1:
> show url-blacklisting database facility acsmgr instance 1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show version
> Displays the version information for the current system image or for a remote image.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show version [ url ] [ all | verbose ] [ | { grep grep_options | more } ]
> url
> Specifies the location of a configuration file to display version information for. The url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [ file: ]{ /flash | /pcmcia1 | /hd }[ /directory ]/file_name

> • | tftp://{ host[ :port# ] }[ /directory ]/file_name

> • | [ http: | ftp: | sftp: ]//[ username[ :password ]@ ] { host }[ :port# ][ /directory ]/file_name

> directory is the directory name.
> filename is the actual file of interest.
> username is the user to be authenticated.
> password is the password to use for authentication.
> host is the IP address or host name of the server.
> port# is the logical port number that the communication protocol is to use.
> all | verbose
> all: indicates all image information is to be displayed.
> verbose: indicates the output is to contain detailed information.
> The verbose keyword may not be used in conjunction with a URL specification.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Cisco ASR 500 Series Command Line Interface Reference.
> Usage
> Display the version information to verify the image versions loaded in preparation for maintenance, upgrades, etc.
> Important: This command is not supported on all platforms.
> Example
> The following commands display the version information with the basic level of output and the detailed level, respectively.
> show version
> show version verbose

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883