> SGSN Service Configuration Mode Commands
> The SGSN Service configuration mode is used within the global configuration mode to specify the 3G operations of the SGSN and the available SGSN services for a specific context.
> SGSN Service works with MAP Service, SGTP Service, GTPP Group, and IuPS Service. All five of these services must be configured to enable a 3G SGSN to communicate with other elements within a UMTS network.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> accounting
> This command defines the accounting context name and enables/disables specific types of CDR generation for the accounting in the SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> accounting ( cdr-types { mcdr | scdr | sms { mo-cdr | mt-cdr } } + | context cntx_name }
> default accounting cdr-types
> no accounting ( cdr-types | context }
> default
> Returns the system to default settings for the selected type of CDR.
> no
> Removes the pre-configured type of CDR generation for accounting from the SGSN service.
> cdr-types { mcdr | scdr | sms { mo-cdr | mt-cdr } +
> Default: enabled
> Defines the types of CDRs to be generate:d within the specified SGSN service for accounting:

> • | mcdr Enables generation of M-CDRs.

> • | scdr : Enables generation of S-CDRs.

> • | sms : Enables generation of SMS-type CDRs based on one of the following:

> • | mo-cd: : SMS CDRs orignates from the mobile.

> • | mt-cdr : SMS CDRs terminates at the mobile.

> +
> Specifies that the specified keywords with in the group can be entered multiple times with a single command.
> context cntx_name
> Specifies an accounting context to be associated with the SGSN service.
> cntx_name: Define a string of 1 to 79 alphanumeric characters.
> Usage
> Use this command to define the type of CDRs to generate for SGSN service. By default all type of CDRs are generated. Note that change of this configuration will be applied to new call and/or to new PDP contexts only.
> By default, generation of the S-CDR, M-CDR, SMS-MT-CDR, and SMS MO-CDR types is enabled.
> Example
> The following command configures the system to generate CDRs of M-CDR type for accounting in the current SGSN service:
> accounting cdr-types mcdr
> cc profile
> Configures the charging characteristic (CC) profile with the triggers for generating various types of CDR as defined with the accounting command.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> cc profile profile_bits [ buckets number | interval time | tariff time1 mins hours [ time2 mins hours ] [ time3 mins hours ] [ time4 mins hours ] | volume { downlink down_vol uplink up_vol | total total_vol } ] +
> [ no | default ] cc profile profile_bits [ buckets | interval | tariff | volumne ]
> no
> Removes a previously configured CC profile.
> default
> Returns the specified CC profile to the original default system settings.
> profile_bits
> Defines the value of the profile bits for the SGSN service.
> index can be configured to any integer value from 0 to 15. Some of the values have been predefined according to 3GPP standard:

> • | 1 for hot billing

> • | 2 for flat billing

> • | 4 for prepaid billing

> • | 8 for normal billing

> buckets number
> Specifies the number of statistics container changes in the CDR due to QoS changes or tariff times that can occur before an accounting record (CDR) is closed
> Default: 4
> number : Must be integer from 1 to 4.
> interval time
> Specifies the normal time duration (in seconds) that must elapse before closing an accounting record (CDR) provided that any or all of the following conditions occur:
> time : Enter any integer from 60 to 40000000.
> tariff time1 mins hours [ time2 mins hours time3 mins hours time4 mins hours ]
> Specifies the time-of-day (based on a 24-hour clock) to close the current statistics container in the CDR, but not necessarily the CDR itself. One tariff time must be defined and up to four tariff times can be specified.
> Important: The system assumes that the billing system uses the day/date to determine if the statistics container represents an actual tariff period.

> • | mins: The minutes of the hour. Enter an integer from 0 to 59.

> • | hours: The hour of the day. Enter an integer from 0 to 23.

> volume { downlink down_vol uplink up_vol | total total_vol }
> Specifies the downlink, uplink, and total volumes octet counts that must be met for the closure of the CDR.
> down_vol : Enter any integer from 100000 to 1345294336.
> up_vol : Enter any integer from 100000 to 400000000.
> total_vol : Enter any integer from 100000 to 400000000.
> Usage
> Charging characteristics consist of a profile index and behavior settings. This command configures the profile index for the SGSN’s charging characteristics. The SGSN supports up to 16 profile indexes.
> Example
> The following command configures a profile index of 10 with tariff times of 7:00 AM and 7:30 PM:
> cc profile 10 tariff time1 0 7 time2 30 19 time3 0 7 time4 30 19
> check-imei-timeout-action
> This command configures the action to be taken if a Check-IMEI fails due to a timeout. This command is available in releases 8.1 and higher.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> check-imei-timeout-action [ continue | reject ]
> default check-imei-timeout-action
> default
> Rejects the Attach or ISRAU procedure if a Check-IMEI timeout occurs.
> continue
> Instructs the SGSN to continue the Attach or ISRAU procedure if a Check-IMEI timeout occurs because the EIR is not reachable. This functionality matches standard call flow.
> reject
> Instructs the SGSN to reject the Attach or ISRAU procedure if a Check-IMEI timeout occurs.
> Usage
> Use this command only if the Gf interface (EIR) is available in the network. This command controls the SGSN reaction if the Check-IMEI procedure fails due to a timeout.
> The continue option allows the SGSN to go forward with the MS Attach or RAU, if the first Check-IMEI fails to reach the EIR due to a timeout. Any subsequent activity (such as a RAU or Service Request would force another Check-IMEI towards the EIR. If this subsequent MAP Check-IMEI should fail, then the same policy of continuing the procedure would apply.
> Example
> check-imei-timeout-action continue
> core-network
> This command specifies the numeric ID for a core network to identify which CN is to be used by the SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> core-network id cn_id
> no core-network id
> no
> Removes the currently configured core network ID from the current SGSN configuration.
> id cn_id
> This number identifies the core network to connect the SGSN service.
> cn_id : Must be an integer from 0 through 65535.
> Usage
> Use this command to set a global ID to identify this SGSN in the core network.
> Example
> The following command sets the core network ID for the current SGSN service to 127:
> core-network id 127
> disable/enable super-charger
> This command has been deprecated and replaced by the super-charger command. For the commands to configure the SuperCharger feature are explained the SGSN Operator Policy Configuration Mode chapter.
> Product
> SSGN
> dns israu-mcc-mnc-encoding
> Configures either decimal or hexadecimal format for the MCC and MNC values in the DNS query which is sent during the ISRAU.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> dns israu-mcc-mnc-encoding { decimal | hexidecimal }
> default dns israu-mcc-mnc-encoding
> default
> Resets the SGSN to send the MCC and MNC values in decimal format for DNS queries.
> decimal
> Default.
> Instructs the SGSN to send the MCC and MNC in decimal format in the DNS query.
> hexadecimal
> Instructs the SGSN to send the MCC and MNC in hexadecimal format in the DNS query.
> Usage
> Use this command to determine the type of encoding for the MCC and MNC to be included in the DNS query sent during the inter-SGSN RAU (ISRAU). The choice must match the format of the DNS server. For example:
> In decimal, the MNC/MCC in a DNS query would appear like:
> rac0017.lac42e3.mnc310.mcc722.gprs
> In hexadecimal, the MNC/MCC in a DNS query would appear like:
> rac0017.lac42e3.mnc0136.mcc02d2.gprs
> Example
> Use hexadecimal values for the MCC/MNC in the DNS query.
> dns israu-mcc-mnc-encoding hexadecimal
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the global configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> gmm
> This command defines the GPRS mobility management parameters for the SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmm { T3302-timeout t3302_dur | T3312-timeout t3312_dur | T3313-timeout initial t3313_init [ decrease t3313_decrement | increase t3313_increment ] | T3322-timeout t3322_dur | T3350-timeout t3350_dur | T3360-timeout t3360_dur | T3370-timeout t3370_dur | implicit-detach-timeout impli_detach_dur | max-auth-retransmission auth_retrans | max-identity-retransmission id_retrans | max-page-retransmission page_retrans | max-ptmsi-reloc-retransmission ptmsi_reloc_retrans | mobile-reachable-timeout ms_reach_dur | perform-identity-on-auth-failure | purge-timeout purge_dur | trau-timeout trau_dur}
> default gmm { T3302-timeout | T3312-timeout | T3313-timeout | T3322-timeout | T3350-timeout | T3360-timeout | T3370-timeout | implicit-detach-timeout | max-auth-retransmission |max-identity-retransmission | max-page-retransmission | max-ptmsi-reloc-retransmission | mobile-reachable-timeout | perform-identity-on-auth-failure | purge-timeout | trau-timeout }
> no gmm { implicit-detach-timeout | max-auth-retransmission | max-identity-retransmission | perform-identity-on-auth-failure }
> default
> Sets the default value for the specified parameter.
> T3302-timeout t3302_dur
> Default: 10
> Specifies the retransmission timer value to guard the GPRS attach or RAU procedure on MS side.
> t3302_dur is the waiting duration in minutes before retransmitting the specific message and must be an integer from 1 through 186.
> T3312-timeout t3312_dur
> Default: 54
> Specifies the retransmission timer value to guard the RAU procedure initiation on network side.
> t3312_dur is the waiting duration in minutes before retransmitting the specific message and must be an integer from 1 through 186.
> T3313-timeout initial t3313_init [ decrease t3313_decrement | increase t3313_increment ]
> Default: 5
> Specifies the retransmission timer value to guard the for paging request procedure initiation on network side.
> initial t3313_init is the initial wating duration in seconds before retransmitting the specific message. t3313_init must be an integer from 1 through 60.
> decrease t3313_decrement. specifies the decrement of the initial timer value in seconds. t3313_decrement must be an integer from 1 through 5.
> increase t3313_increment. specifies the increment of the initial timer value in seconds. t3313_decrement must be an integer from 1 through 5.
> T3322-timeout t3322_dur
> Default: 6
> Specifies the retransmission timer value to guard the GPRS detach request procedure on network side.
> t3322_dur is the waiting duration in seconds before retransmitting the specific message and must be an integer from 1 through 20.
> T3350-timeout t3350_dur
> Default: 6
> Specifies the retransmission timer value to guard the GPRS attach accept/RAU accept/realloc request procedure sent with P-TMSI and/or TMSI on network side.
> t3350_dur is the waiting duration in seconds before retransmitting the specific message and must be an integer from 1 through 20.
> T3360-timeout t3360_dur
> Default: 6
> Specifies the retransmission timer value to guard the authentication and cipher request procedure on network side.
> t3360_dur is the waiting duration in seconds before retransmitting the specific message and must be an integer from 1 through 20.
> T3370-timeout t3370_dur
> Default: 6
> Specifies the retransmission timer value to guard the identity request procedure on network side.
> t3370_dur is the waiting duration in seconds before retransmitting the specific message and must be an integer from 1 through 20.
> implicit-detach-timeout impli_detach_dur
> Default: 3600
> Specifies the retransmission timer value to guard the implicit detach procedure on network side.
> impli_detach_dur is the waiting duration in seconds before retransmitting the specific message and must be an integer from 1 through 3600.
> max-auth-retransmission auth_retrans
> Default: 4
> Specifies the maximum retransmission of authentication requests allowed.
> auth_retrans is the number of retries before declaring the authentication failure and must be an integer from 1 through 10.
> max-identity-retransmission id_retrans
> Default: 4
> Specifies the maximum retransmission of identity requests allowed.
> id_retrans is the number of retries before declaring the identity failure and must be an integer from 1 through 10.
> max-page-retransmission page_retrans
> Default: 5
> Specifies the maximum retransmission of page requests allowed.
> id_retrans is the number of retries before declaring the paging request failure and must be an integer from 1 through 5.
> max-ptmsi-reloc-retransmission ptmsi_reloc_retrans
> Default: 5
> Specifies the maximum retransmission for P-TMSI relocation procedure allowed.
> id_retrans is the number of retries before declaring the P-TMSI relocation procedure failure and must be an integer from 1 through 5.
> mobile-reachable-timeout ms_reach_dur
> Default: 58
> Specifies the retransmission timer value to guard the mobile reachability procedure on network side.
> impli_detach_dur is the waiting duration in minutes before retransmitting the specific message and must be an integer from 1 through 1440.
> perform-identity-on-auth-failure
> Default: Enabled
> Configures the SGSN service to perform an identity check to ascertain the IMSI after an authentication failure on a PTMSI-based message.
> purge-timeout purge_dur
> Default: 10080 (7 days)
> Specifies the timer value to guard the detach of MM context procedure on network side.
> impli_detach_dur is the waiting duration in minutes before retransmitting the specific message and must be an integer from 1 through 20160.
> Define the purge timer to hold detached mm-contexts. Default is 10080 mins (7 days).
> trau-timeout trau_dur
> This timer is available in releases 9.0 and higher.
> Default: 30
> Specifies the number of seconds the “old” 3G SGSN waits to purge the MS’s data. This timer is started by the “old” SGSN after completion of the inter-SGSN RAU.
> trau_dur : Must be an integer from 5 to 60.
> Usage
> Repeat this command as needed to configure multiple parameters for GPRS mobility management in a UMTS network. This command provides the configuration of timers for mobility procedures and retries for different messages. GMM layer is defined in the 3GPP TS 24.008 (Release 7).
> Example
> Following command configures the timer to wait for 5 mins before retransmitting the message for GPRS attach or RAU procedure on MS side with maximum number of retries as 6 for authentication:
> gmm T3302-timeout 5 max-auth-retransmission 6
> gs-service
> This command associates a previously defined Gs service interface to MSC/VLR along with its associated context with an SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gs-service gs_srvc_name context ctx_name
> no gs-service gs_srvc_name
> no
> Removes/disassociates the named Gs service from this SGSN service.
> gs_srvc_name
> Specifies the name of a specific Gs service for which to display information.
> svc_name is the name of a configured Gs service and can be from 1 to 63 alpha and/or numeric characters and is case sensitive.
> context ctx_name
> Specifies the specific context name where Gs service is configured. If this keywork is omitted, the named Gs service must be exist in the same context as the SGSN service.
> ctx_name is name of the configured context of Gs service. This can be from 1 to 63 alpha and/or numeric characters and is case sensitive.
> Usage
> Use this command to associate a specific Gs service interface with this SGSN service instance.
> Important: A single Gs service can be used with multiple SGSN and/or GPRS service.
> Example
> Following command associates a Gs service instance named stargs1, which is configured in context named star_ctx, with an SGSN service:
> gs-service stargs1 context star_ctx
> lac
> This command defines the location area code (LAC in hexidcimal format.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> lac hex
> no lac
> no
> Erases the lac configuration statement.
> hex
> Enter a hexadecimal number between 0x0 and 0xFFFF
> max-pdp-contexts
> Configures the maximum number of PDP contexts for a MS (mobile station) that will be supported on this SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> max-pdp-contexts per-ms number
> default max-pdp-contexts per-ms
> default
> Resets the maximum number of PDP contexts per mobile station to the default of 11 for the Gs service configuration
> per-ms number
> Default: 11
> Defines the combined total number of primary and secondary PDP contexts for the SGSN service.
> number can be an integer from 2 to 11.
> Usage
> The following example defines 5 as the maximum number of primary and secondary PDP contexts that this SGSN will support for any connected MS.
> Example
> max-pdp-contexts per-ms 5
> mobile-application-part
> This command identifies an already defined MAP service (Mobile Application Part service) to associate with the SGSN service. Although the MAP service does not need to be defined in the same context as the SGSN service, there is a one-to-one relationship between a MAP service and an SGSN service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> mobile-application-part service map_srvc [ context ctx_name ]
> no mobile-application-part service
> no
> Remove the MAP service association from the SGSN service configuration.
> service map_srvc
> Specifies the name of the MAP service to be associated with this SGSN service.
> map_srvc must be the name of a MAP service previously configured on the system.
> context ctx_name
> Specifies the name of the context where the MAP service is configured. If the MAP service is not configured in the current context, then the context where it is configured must be specified to enable the SGSN to reach the MAP service.
> If this keyword is not specified, the current context is used.
> ctxt_name: Must be the name of the context where the specified MAP service is configured.
> Usage
> Use this command to identify the MAP service configuration to be used by the SGSN service configuration. Also use this command to specify the context in which the MAP service configuration was created.
> If the MAP service is not identified or if the correct context is not identified, then the SGSN service will not START.
> Example
> The following command specifies a MAP service named map1 that is configured in the same context as the current SGSN service:
> mobile-application-part service map1
> network-sharing cs-ps-coordination
> Enables/disables the SGSN service to perform a CS-PS coordination check.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> network-sharing cs-ps-coordination
> default network-sharing cs-ps-coordination
> no network-sharing cs-ps-coordination
> default
> Including this keyword resets the SGSN service to allow the check to be performed.
> no
> Disables this feature for the SGSN service.
> Usage
> Use this command to facilitate the network sharing functionality. With this command, the SGSN can be instructed to perform a check to determine if CS-PS coordination is needed.
> 3GPP TS 25.231 section 4.2.5 describes the functionality of the SGSN to handle CS-PS (circuit-switching/packet-switching) coordination for attached networks not having a Gs-interface. In compliance with the standard, the SGSN rejects an Attach in a MOCN configuration with cause 'CS-PS coordination required', after learning the IMSI, to facilitate the RNC choosing the same operator for both CS and PS domains.
> Example
> Use the following syntax to disable the CS-PS coordination check:
> no network-sharing cs-ps-coordination
> nri length
> This command defines the Network Resource Identifier (NRI) of the SGSN that is stored in the P-TMSI (bits 23 to 18).
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> nri length nri_length { nri-value nri_value | null-nri-value null_nri_value non-broadcast mcc mcc mnc mnc lac lac_id rac rac_id [ nri-value value }
> no nri
> no
> Removes the configured NRI value and location in P-TMSI for retrieval by this SGSN operator policy.
> nri length nri_length
> Specifies the number of bits to be used in the P-TMSI, bits 23 to 18. to define the network resource identifier (NRI). The NRI length configuration also sets the maximum size of the pool. If not configured, the NRI length will be of zero length.
> nri_length : Must be an integer from 1 to 6 to identify the number of bits.
> null-nri-value null_nri_value
> This keyword is only available in releases 8.1 and higher.
> Configures the null NRI value which must be unique across the pool areas. This keyword is used for the offloading procedure for SGSN pooling (enabled with the sgsn offloading command, see the Exec Mode chapter).
> null_nri_value : 0 (zero) indicates the keyword is not to be used and 1 to 63 are used to identify the SGSN to be used for the offloading procedure for SGSN pooling. There is no default value for this parameter.
> non-broadcast mcc mcc mnc mnc lac lac_id rac rac_id
> This keyword set is only available in releases 8.1 and higher.
> Defines the non-broadcast LAC/RAC to be used in combination with the null-NRI for the offloading procedure. Including the MCC and MNC to specify the PLMN because the Iu-Flex feature supports multiple IuPS Services.
> mcc identifies the mobile country code, the first part of the PLMN ID. Must be an integer between 100 and 999.
> mnc identifies the mobile network code portion of the PLMN ID. Must be a 2- or 3-digit integer between 01 and 999.
> lac_id defines a location area code associated with an RNC. Must be an integer between 1 and 65535.
> rac_id defines the remote area code to be associated with an RNC. Must be an integer between 1 and 255.
> nri-value nri_value
> Specifies the MS-assigned value of the NRI to retrieve from the P-TMSI. This value must not exceed the maximum possible value specified by the NRI length. The NRI value must be unique across the pool or across all overlapping pools.
> nri_value must be an integer from 1 to 63 to identify a specific SGSN in a pool. Use of 0 (zero) value is not recommended.
> Multiple NRI values can be identified by providing multiple nri-values separated by a blank space for example: nri length 6 nri-value 29 43 61
> Usage
> Use this command to identify the SGSN identified with the NRI in the MS generated P-TMSI.
> This command adds or removes the Iu Flex configuration for this SGSN service. When using Iu Flex, all keywords must be defined. The command can be repeated to specify different values for any of the keyword parameters. If more than one NRI is configured, the SGSN service will round-robin between the available NRIs when new subscribers (re)connect.
> Use this command to retrieve the NRI (identity of an SGSN) stored in in bits 23 to 18 of the packet-temporary mobile subscriber identity (P-TMSI). If more than one NRI value is configured, the SGSN service will round-robin between the available NRIs when new subscribers (re)connect.
> When using MOCN mode for network sharing without SGSN pooling, the NRI length and the NRI value should both be used.
> Example
> The following command specifies the the NRI length as 5 bits, identifies SGSN 23 with LAC 222 and RAC 12 for offloading procedure with NRIs 6 and 41:
> nri length 5 null-nri-value 34 non-broadcast lac 222 rac 12 nri-value 6 41
> override-lac-li
> This command defines the override location area code (LAC) needed for the function of the lawful intercept feature.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> override-lac-li hex
> no override-lac-li
> no
> Erases the override location area code for this GGSN service from the configuration.
> hex
> Enter a hexadecimal number between 0x0 and 0xFFFF
> override-rac-li
> This command defines the override routing area code needed for the lawful intercept function.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> override-rac-li hex
> no override-rac-li
> no
> Erases the override routing area code for this GGSN service from the configuration.
> hex
> Enter a hexadecimal number between 0x0 and 0xFFFF
> rac
> This command defines the override routing area code needed for the lawful intercept function.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> rac hex
> no rac
> no
> Erases the routing area code configuration statement.
> hex
> Enter a hexadecimal number between 0x0 and 0xFFFF
> ran-protocol
> This command specifies the IuPS service for the SGSN service to use for communication with the RAN.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ran-protocol iups-service iups_srvc [ context ctx_name ]
> no ran-protocol iups-service
> no
> Removes the IuPS service information from the SGSN service configuration.
> iups-service iups_srvc
> Specifies the name of an IuPS service already configured on the system.
> iups_srvc : Enter an alphanumeric string of 1 to 63 characters.
> ctx_name
> ctx_name : Enter the name of the IuPS context, an alphanumeric string of 1 to 63 characters.
> Usage
> Use this command to configure the IuPS service context that the current SGSN service will use to communicate with the RAN. Up to 8 definitions can be defined for a single SGSN service to allow for multiple PLMNs support.
> Example
> The following command configures the SGSN service to use an IuPS service named iups1 that has been configured. in the same context as the SGSN service:
> ran-protocol iups-service iups1
> sgsn-number
> This command defines the E.164 number that identifies this particular SGSN service context.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn-number E.164_number
> no sgsn-number
> no
> Removes the SGSN number configuration from the SGSN service configuration.
> E.164_number
> Enter a maximum of 15 digits to define this ‘phone’ number associated with this SGSN service context.
> Usage
> To delete the sgsn-number associated with this SGSN service context, enter:
> Example
> no sgsn-number
> sgtp-service
> This command creates an instance of an SGTP service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgtp-service sgtp_srvc_name
> no sgtp-service
> sgtp_srvc_name
> Enter the name of an SGTP service that will be used by this SGSN service
> sgtp_srvc_name : Enter a string of 1 to 63 alphanumeric characters.
> Usage
> Use this command to access the SGTP Service configuration mode to configure SGTP parameters.
> Example
> sgtp-service sgtp1
> sm
> This command configures session management parameters for this SGSN service. This command can be repeated multiple times to configure each parameter individually.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sm { T3385-timeout time | T3386-timeout time | T3395-timeout time | max-actv-retransmission number | max-deactv-retransmission number | max-modf-retransmission number | rab-ass-timeout time | session-inactivity | rns-ctxt-rsp-timeout }
> default sm timer
> default
> Resets the selected timer to the system default value.
> T3385-timeout
> Retransmission timer for network-initiated Activate Request. Default is 8 sec
> T3386-timeout
> Retransmission timer for network-initiated Modify Request. Default is 8 sec
> T3395-timeout
> Retransmission timer for network-initiated Deactivate Request. Default is 8 sec
> max-actv-retransmission
> Configures maximum retries for activate PDP ctxt request. Default is 4
> max-deactv-retransmission
> Configures maximum retries for deactivate PDP ctxt request. Default is 4
> max-modf-retransmission
> Configures maximum retries for modify PDP ctxt request. Default is 4
> Usage
> Repeat the command to configure multiple session management parameters for the SGSN service.
> Example
> sm T3385-timeout 5

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883