> DLCI Configuration Mode Commands
> The DLCI configuration mode provides the commands to configure, bind and manage the DLCI associated with a specific port defined in the parent configuration mode, Channelized Port configuration mode.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> bind link
> This command configures an association (binds) between an IP interface or a pre-configured routing SS7/Frame Relay link and the specific port being configured with the Channelized Port configuration commands.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> bind link peer-nsei nse_id ns-vci ns-vc_id
> no bind link peer-nsei nse_id ns-vci ns-vc_id
> peer-nsei nse_id
> Defines the end-point network service entity identifier (NSEI). The NSEI must be an integer from 0 to 65535.
> ns-vc-id ns-vc_id
> Defines the network service virtual circuit identifier (NSVCI). The NSVCI must be an integer from 0 to 65535.
> no
> Deletes the bind configuration from the Operator Policy.
> Usage
> Bind this port to network service entity 2 and network service VC 234.
> Example
> bind link peer-nsei 2 ns-vci 234
> end
> Exits this sub-configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode and return to the Exec mode.
> exit
> Exits the this sub-configuration mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous configuration mode.
> shaping
> Defines egress traffic shaping to control flow for this DLCI.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> shaping type
> default shaping
> shaping type
> The following types of shaping provide flow management:

> • | cir: Commited Info Rate

> • | cir-eir: Commited Info Rate with Excess Rate

> • | ppr: Peak Packet Rate

> • | wfq: Weighted Fair Queuing

> default
> Resets the DLCI configuration to the system default.
> Usage
> Use this command to identify the type of signal shaping to be used on the DLCI.
> Example
> shaping cir
> shutdown
> Terminates all processes supporting the port or blocks the shutting down of the port. Conversely, this command with the no keyword enables the port.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> shutdown
> no shutdown
> no
> Enables the port’s administrative state. When omitted the card is shutdown (removed from service).
> Usage
> Shut down a port prior to re-cabling and/or other maintenance activities.
> This command with the no keyword is required to bring a port into service.
> Example
> shutdownno shutdown

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883