> ESS Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the ESS application.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).
> starentLESSMIB(101)
> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101).
> starLESSMIBObjects(1)

> Object: | starLESSNotifRaisedTime

> Object ID: | enterprises.8164.1.101.1.1

> Description: | This object indicates the time when this notification was generated. This will be current system's time in seconds.

> Syntax: | Integer32

> Access: | Accessible-for-notify

> Object: | starLESSNotifInfo

> Object ID: | enterprises.8164.1.101.1.2

> Description: | A textual description of L-ESS notification, which contains additional information (more than the type of alarm). If the text of the message exceeds 64 bytes, the message be truncated to 63 bytes and a '*' character will be appended to indicate that the message has been truncated.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Accessible-for-notify

> Object: | starLESSInstance

> Object ID: | enterprises.8164.1.101.1.3

> Description: | This object indicates the L-ESS Application Instance number.

> Syntax: | Integer32

> Access: | Accessible-for-notify

> Object: | starLESSNodeName

> Object ID: | enterprises.8164.1.101.1.4

> Description: | This object indicates the L-ESS Application node name.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Accessible-for-notify

> Object: | starLESSApplicationType

> Object ID: | enterprises.8164.1.101.1.5

> Description: | This object indicates the L-ESS Application Type (pull / push / transfer). Pull (1) is L-ESS Pull application Push (2) is L-ESS Push application Transfer (3) is L-ESS Transfer application

> Syntax: | INTEGER { unknown(0), pull(1), push(2), transfer(3) }

> Access: | Accessible-for-notify

> Object: | starLESSThreshInt

> Object ID: | enterprises.8164.1.101.1.6

> Description: | This object indicates the configured value of a thresholded parameter.

> Syntax: | Integer32

> Access: | Accessible-for-notify

> Object: | starLESSThreshMeasuredInt

> Object ID: | enterprises.8164.1.101.1.7

> Description: | This object indicates the measured value of a thresholded parameter.

> Syntax: | Integer32

> Access: | Accessible-for-notify

> Object: | starLESSRuleBaseName

> Object ID: | enterprises.8164.1.101.1.8

> Description: | This object indicates the name of the rulebase present in filename.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Accessible-for-notify

> Object: | starLESSSTXName

> Object ID: | enterprises.8164.1.101.1.9

> Description: | This object indicates the name of the STX.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Accessible-for-notify

> Object: | starLESSStartofMissedRange

> Object ID: | enterprises.8164.1.101.1.10

> Description: | This object indicates the beginning of the range within which L-ESS has missed files.

> Syntax: | DisplayString (SIZE (1..15))

> Access: | Accessible-for-notify

> Object: | starLESSEndofMissedRange

> Object ID: | enterprises.8164.1.101.1.11

> Description: | This object indicates the end of the range within which L-ESS has missed files.

> Syntax: | DisplayString (SIZE (1..15))

> Access: | Accessible-for-notify

> Object: | starLESSFileType

> Object ID: | enterprises.8164.1.101.1.12

> Description: | This object indicates the name of the rulebase present in filename.

> Syntax: | DisplayString (SIZE (1..3))

> Access: | Accessible-for-notify

> Object: | starLESSRemoteHostName

> Object ID: | enterprises.8164.1.101.1.13

> Description: | This object indicates the name of the STX.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | Accessible-for-notify

> Object: | starLessMountPoint

> Object ID: | enterprises.8164.1.101.1.14

> Description: | Mount point where disk is mounted

> Syntax: | DisplayString(SIZE(1..64)

> Access: | Accessible for Notifye

> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101)
> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101).
> starLESSMIBTraps(2)

> Object: | starLESSApplicationStart

> Object ID: | enterprises.8164.1.101.2.1

> Description: | This notification is generated when L-ESS application has started.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType

> Object: | starLESSApplicationReStart

> Object ID: | enterprises.8164.1.101.2.2

> Description: | This notification is generated when L-ESS application has restarted.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType

> Object: | starLESSApplicationStop

> Object ID: | enterprises.8164.1.101.2.3

> Description: | This notification is generated when L-ESS application has stopped.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSNotifInfo

> Object: | starLESSApplicationTerminated

> Object ID: | enterprises.8164.1.101.2.4

> Description: | This notification is generated when L-ESS application has been terminated.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType

> Object: | starLESSPullIntervalMissed

> Object ID: | enterprises.8164.1.101.2.5

> Description: | This notification is generated when L-ESS application has missed pull interval.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance

> Object: | starLESSThreshDiskUsage

> Object ID: | enterprises.8164.1.101.2.6

> Description: | This notification is generated when total disk space used is beyond configured threshold. Probable Cause: This is a user configurable threshold. Condition Clear Alarm: A starLESSThreshClearDiskUsage notification will be generated when the measured value falls below the configured threshold.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSThreshClearDiskUsage

> Object ID: | enterprises.8164.1.101.2.7

> Description: | This notification is generated when total disk used is below configured threshold.Threshold condition is now clear.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSFileMissed

> Object ID: | enterprises.8164.1.101.2.8

> Description: | This notification is generated when L-ESS application has missed pulling files from STX. Probable Cause: File at STX side has been deleted before L-ESS fetching it. Clear Condition: There is no clear condition for this notification. Condition Clear Alarm: There is no clear alarm for this notification.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSRuleBaseName starLESSFileType starLESSSTXName starLESSStartofMissedRange starLESSEndofMissedRange starLESSNotifInfo

> Object: | starLESSRemoteConnectionFail

> Object ID: | enterprises.8164.1.101.2.9

> Description: | This notification is generated when L-ESS application is unable to set up the connection with remote host. Probable Cause: No route to host, Authentication failure, Host Unreachable, etc. Clear Condition: This condition is cleared when L-ESS is able to setup the connection with remote host. Condition Clear Alarm: This condition is cleared by a starRemoteConnectionEstablished notification.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName starLESSNotifInfo

> Object: | starLESSRemoteConnectionEstablished

> Object ID: | enterprises.8164.1.101.2.10

> Description: | This notification is generated when L-ESS application is able to set up the connection with remote host. Probable Cause: Connection established with remote host.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName

> Object: | starLESSFileTransferFail

> Object ID: | enterprises.8164.1.101.2.11

> Description: | This notification is generated when L-ESS application is failing to transfer file. Probable Cause: This trap could be raised when pull or push process fails to transfer files continuously. Reasons for this failure could be network errors, disk space unavailable at destination, Destination directory unavailable, etc. Clear Condition: This condition is cleared when successful file transfer begins. Condition Clear Alarm: This condition is cleared by a starLESSFileTransferComplete notification.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName starLESSFileType starLESSNotifInfo

> Object: | starLESSFileTransferComplete

> Object ID: | enterprises.8164.1.101.2.12

> Description: | This notification is generated when L-ESS application is able to transfer file. Probable Cause: The problems due to which L-ESS was unable to transfer file have resolved and pull or push process has restarted file transfer.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSRemoteHostName starLESSFileType

> Object: | starLESSThreshPendingFiles

> Object ID: | enterprises.8164.1.101.2.13

> Description: | This notification is generated when total pending files for this host are beyond configured threshold. Probable Cause: This is a user configurable threshold. The starLESSThreshPendingFiles notification will be generated by pull or push process when the total number of files pending for transfer in source directory are beyond configured threshold. Clear Condition: This condition is cleared when number of pending files at source directory falls below configured threshold. Condition Clear Alarm: This condition is cleared by a starLESSThreshClearPendingFiles notification.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName starLESSFileType starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSThreshClearPendingFiles

> Object ID: | enterprises.8164.1.101.2.14

> Description: | This notification is generated when total pending files for this host are below configured threshold. Probable Cause: This is a user configurable threshold. The starLESSThreshPendingFiles notification will be generated by pull or push process when the total number of files pending for transfer in source directory falls below configured threshold.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName starLESSFileType starLESSThreshMeasuredInt starLESSThreshInt

> Object: | starLESSNewHostFound

> Object ID: | enterprises.8164.1.101.2.15

> Description: | This notification is generated when L-ESS transfer process has detected addition of host. Probable Cause: Operator has added host in L-ESS from which files should be transferred to destination.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName

> Object: | starLESSHostRemoved

> Object ID: | enterprises.8164.1.101.2.16

> Description: | This notification is generated when L-ESS transfer process has detected removal of existing host. Probable Cause: Operator has removed existing host from which L-ESS was already transferring files to destination.

> Objects: | starLESSNotifRaisedTime starLESSNodeName starLESSInstance starLESSApplicationType starLESSSTXName

> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101).
> starLESSMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101).
> starLESSMIBConformances(3).starLESSMIBCompliances(1)

> Object: | starLESSMIBCompliance

> Object ID: | enterprises.8164.1.101.3.1.1

> Description: | The compliance statements for entities which implement the STARENT L-ESS MIB.

> Objects: | starLESSNotifMgmtGroup starLESSNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentLESSMIB(101).
> starLESSMIBConformances(3).starLESSMIBGroups(2)

> Object: | starLESSNotifMgmtGroup

> Object ID: | enterprises.8164.1.101.3.2.1

> Description: | This group is a collection of objects related with notification management on L-ESS.

> Objects: | starLESSNotifRaisedTime starLESSNotifInfo starLESSInstance starLESSNodeName starLESSApplicationType starLESSThreshMeasuredInt starLESSThreshInt starLESSRuleBaseName starLESSSTXName starLESSStartofMissedRange starLESSEndofMissedRange starLESSFileType starLESSRemoteHostName

> Object: | starLESSNotifGroup

> Object ID: | enterprises.8164.1.101.3.2.2

> Description: | This group is a collection of notifications for L-ESS management.

> Objects: | starLESSApplicationStart starLESSApplicationReStart starLESSApplicationStop starLESSApplicationTerminated starLESSPullIntervalMissed starLESSThreshDiskUsage starLESSThreshClearDiskUsage starLESSFileMissed starLESSRemoteConnectionFail starLESSRemoteConnectionEstablished starLESSFileTransferFail starLESSFileTransferComplete starLESSThreshPendingFiles starLESSThreshClearPendingFiles starLESSNewHostFound starLESSHostRemoved

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883