> show active-charging
> This chapter includes the show active-charging command output tables.
> show active-charging analyzer statistics name dns
> show active-charging analyzer statistics name dns Command Output Descriptions

> Field | Description
> ACS DNS Session Stats:
> Total Uplink Bytes | The total number of DNS bytes detected in uplink direction.
> Total Downlink Bytes | The total number of DNS bytes detected in downlink direction.
> Total Uplink Pkts | The total number of DNS packets detected in uplink direction.
> Total Downlink Pkts | The total number of DNS packets detected in downlink direction.
> Unknown OPCODE | The total number of DNS packets with an unknown operational code.
> Invalid Pkts | The total number of invalid DNS packets detected.
> DNS Over TCP:
> Uplink Bytes | The total number of DNS uplink bytes that were detected over TCP.
> Downlink Bytes | The total number of DNS downlink bytes that were detected over TCP.
> Uplink Pkts | The total number of DNS uplink packets that were detected over TCP.
> Downlink Pkts | The total number of DNS downlink packets that were detected over TCP.
> Request:
> A Query Type | The total number of DNS requests received for A query types.
> CNAME Query Type | The total number of DNS requests received for CNAME query types.
> NS Query Type | The total number of DNS requests received for NS query types.
> PTR Query Type | The total number of DNS requests received for PTR query types.
> SRV Query Type | The total number of DNS requests received for SRV query types.
> Unknown Query Type | The total number of DNS requests received for unknown query types.
> AAAA Query Type | The total number of DNS requests received for AAAA query types.
> Response:
> A Query Type | The total number of DNS responses received for A query types.
> CNAME Query Type | The total number of DNS responses received for CNAME query types.
> NS Query Type | The total number of DNS responses received for NS query types.
> PTR Query Type | The total number of DNS responses received for PTR query types.
> SRV Query Type | The total number of DNS responses received for SRV query types.
> Unknown Query Type | The total number of DNS responses received for unknown query types.
> AAAA Query Type | The total number of DNS responses received for AAAA query types.

> ‌
> show active-charging analyzer statistics name icmpv6
> show active-charging analyzer statistics name icmpv6 Command Output Descriptions

> Field | Description
> ACS ICMPv6 Session Stats:
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Uplink Bytes Fragmented | Total number of uplink bytes that were fragmented.
> Downlink Bytes Fragmented | Total number of downlink bytes that were fragmented.
> Uplink Pkts Fragmented | Total number of uplink packets that were fragmented.
> Downlink Pkts Fragmented | Total number of downlink packets that were fragmented.
> Uplink Bytes Invalid | Total number of invalid uplink bytes.
> Downlink Bytes Invalid | Total number of invalid downlink bytes.
> Uplink Pkts Invalid | Total number of invalid uplink packets.
> Downlink Pkts Invalid | Total number of invalid downlink packets.

> ‌
> show active-charging analyzer statistics name ip verbose
> show active-charging analyzer statistics name ip verbose Command Output Descriptions

> Field | Description
> ACS IP Session Stats:
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Uplink Bytes Fragmented | Total number of uplink bytes that were fragmented.
> Downlink Bytes Fragmented | Total number of downlink bytes that were fragmented.
> Uplink Pkts Fragmented | Total number of uplink packets that were fragmented.
> Downlink Pkts Fragmented | Total number of downlink packets that were fragmented.
> Uplink Bytes Invalid Length | Total number of uplink bytes of invalid length.
> Downlink Bytes Invalid Length | Total number of downlink bytes of invalid length.
> Uplink Pkts Invalid Length | Total number of uplink packets of invalid length.
> Downlink Pkts Invalid Length | Total number of downlink packets of invalid length.
> Uplink Bytes Invalid Length (After Reassembly) | Total number of uplink bytes of invalid length after reassembly.
> Downlink Bytes Invalid Length (After Reassembly) | Total number of downlink bytes of invalid length after reassembly.
> Uplink Pkts Invalid Length (After Reassembly) | Total number of uplink packets of invalid length after reassembly.
> Downlink Pkts Invalid Length (After Reassembly) | Total number of downlink packets of invalid length after reassembly.
> Uplink Bytes Invalid Version | Total number of uplink bytes of invalid version.
> Downlink Bytes Invalid Version | Total number of downlink bytes of invalid version.
> Uplink Pkts Invalid Version | Total number of uplink packets of invalid version.
> Downlink Pkts Invalid Version | Total number of downlink packets of invalid version.
> Uplink Bytes Invalid Checksum | Total number of bytes received in uplink direction with invalid checksum errors.
> Downlink Bytes Invalid Checksum | Total number of bytes received in downlink direction with invalid checksum errors.
> Uplink Pkts Invalid Checksum | Total number of packets received in uplink direction with invalid checksum errors.
> Downlink Pkts Invalid Checksum | Total number of packets received in downlink direction with invalid checksum errors.
> Uplink Bytes IP reassembly Timeout | Total number of bytes in uplink traffic dropped due to IP reassembly timeout.
> Uplink Pkts IP reassembly Timeout | Total number of packets in uplink traffic dropped due to IP reassembly timeout.
> Downlink Bytes IP reassembly Timeout | Total number of bytes in downlink traffic dropped due to IP reassembly timeout.
> Downlink Pkts IP reassembly Timeout | Total number of packets in downlink traffic dropped due to IP reassembly timeout.
> Uplink Bytes IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in uplinked bytes reassembly.
> Uplink Pkts IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in uplinked packets reassembly.
> Downlink Bytes IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in downlinked bytes reassembly.
> Downlink Pkts IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in downlinked packets reassembly.
> Uplink Bytes received after reassembly | Total number of uplink bytes received after reassembly.
> Uplink Pkts received after reassembly | Total number of uplink packets received after reassembly.
> Downlink Bytes received after reassembly | Total number of downlink bytes received after reassembly.
> Downlink Pkts received after reassembly | Total number of downlink packets received after reassembly.

> ‌
> show active-charging analyzer statistics name ipv6
> show active-charging analyzer statistics name ipv6 Command Output Descriptions

> Field | Description
> ACS IPv6 Session Stats:
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Uplink Bytes Fragmented | Total number of uplink bytes that were fragmented.
> Downlink Bytes Fragmented | Total number of downlink bytes that were fragmented.
> Uplink Pkts Fragmented | Total number of uplink packets that were fragmented.
> Downlink Pkts Fragmented | Total number of downlink packets that were fragmented.
> Uplink Bytes Invalid | Total number of invalid uplink bytes.
> Downlink Bytes Invalid | Total number of invalid downlink bytes.
> Uplink Pkts Invalid | Total number of invalid uplink packets.
> Downlink Pkts Invalid | Total number of invalid downlink packets.

> ‌
> show active-charging analyzer statistics name ipv6 verbose
> show active-charging analyzer statistics name ipv6 verbose Command Output Descriptions

> Field | Description
> ACS IPv6 Session Stats:
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Uplink Bytes Fragmented | Total number of uplink bytes that were fragmented.
> Downlink Bytes Fragmented | Total number of downlink bytes that were fragmented.
> Uplink Pkts Fragmented | Total number of uplink packets that were fragmented.
> Downlink Pkts Fragmented | Total number of downlink packets that were fragmented.
> Uplink Bytes Invalid Length | Total number of uplink bytes of invalid length.
> Downlink Bytes Invalid Length | Total number of downlink bytes of invalid length.
> Uplink Pkts Invalid Length | Total number of uplink packets of invalid length.
> Downlink Pkts Invalid Length | Total number of downlink packets of invalid length.
> Uplink Bytes Invalid Length (After Reassembly) | Total number of uplink bytes of invalid length after reassembly.
> Downlink Bytes Invalid Length (After Reassembly) | Total number of downlink bytes of invalid length after reassembly.
> Uplink Pkts Invalid Length (After Reassembly) | Total number of uplink packets of invalid length after reassembly.
> Downlink Pkts Invalid Length (After Reassembly) | Total number of downlink packets of invalid length after reassembly.
> Uplink Bytes IP reassembly Timeout | Total number of bytes in uplink traffic dropped due to IP reassembly timeout.
> Uplink Pkts IP reassembly Timeout | Total number of packets in uplink traffic dropped due to IP reassembly timeout.
> Downlink Bytes IP reassembly Timeout | Total number of bytes in downlink traffic dropped due to IP reassembly timeout.
> Downlink Pkts IP reassembly Timeout | Total number of packets in downlink traffic dropped due to IP reassembly timeout.
> Uplink Bytes IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in uplinked bytes reassembly.
> Uplink Pkts IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in uplinked packets reassembly.
> Downlink Bytes IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in downlinked bytes reassembly.
> Downlink Pkts IP reassembly Max. Fragments reached | Total number of times Max fragments was reached in downlinked packets reassembly.

> ‌
> show active-charging analyzer statistics name p2p verbose
> show active-charging analyzer statistics name p2p verbose Command Output Descriptions

> Field | Description
> Non-P2P
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Skype non-voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Skype voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Bittorrent
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Edonkey
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Msn-non-voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Msn-voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Yahoo-non-voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Yahoo-voice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Orb
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Gnutella
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Jabber
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Slingbox
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Winny
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Fasttrack
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Manolito
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Pando
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Filetopia
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Soulseek
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Ppstream
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Qq
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Qqlive
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Mute
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Gadugadu
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Feidian
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Applejuice
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Zattoo
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Skinny
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Sopcast
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Ares
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Directconnect
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Imesh
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Pplive
> Uplink Bytes: | The total number of bytes uplinked.
> Downlink Bytes: | The total number of bytes downlinked.
> Uplink Pkts: | The total number of packets uplinked.
> Downlink Pkts: | The total number of packets downlinked.
> Oscar
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Popo
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Irc
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Steam
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Ddlink
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Halflife2
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Hamachivpn
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Tvants
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Tvuplayer
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Uusee
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Vpnx
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Vtun
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Winmx
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Wofwarcraft
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Xbox
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Iskoot
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Fring
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Oovoo
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Gtalk-non-voice
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Gtalk-voice
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Freenet
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Aimini
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Battlefld
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Openft
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Qqgame
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Quake
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Secondlife
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Actsync
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Nimbuzz
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Iax
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Paltalk
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Warcft3
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Rdp
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Iptv
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.
> Uplink Bytes | The total number of bytes uplinked.
> Pandora
> Uplink Bytes | The total number of bytes uplinked.
> Downlink Bytes | The total number of bytes downlinked.
> Uplink Pkts | The total number of packets uplinked.
> Downlink Pkts | The total number of packets downlinked.

> ‌
> show active-charging analyzer statistics name tcp verbose
> show active-charging analyzer statistics name tcp verbose Command Output Descriptions

> Field | Description
> ACS TCP Session Stats:
> Total Uplink Bytes | The total number of bytes uplinked.
> Total Downlink Bytes | The total number of bytes downlinked.
> Total Uplink Pkts | The total number of packets uplinked.
> Total Downlink Pkts | The total number of packets downlinked.
> Uplink Bytes Retrans | The number of uplink bytes that were retransmitted.
> Downlink Bytes Retrans | The number of downlink bytes that were retransmitted.
> Uplink Pkts Retrans | The number of uplink packets that were retransmitted.
> Downlink Pkts Retrans | The number of downlink packets that were retransmitted.
> Uplink Out of Order Pkts Successfully Analyzed | The number of uplink out of order packets that were successfully analyzed.
> Downlink Out of Order Pkts Successfully Analyzed | The number of downlink out of order packets that were successfully analyzed.
> Uplink Out of Order Pkts Failure | The number of uplink out of order packets that failed.
> Downlink Out of Order Pkts Failure | The number of downlink out of order packets that failed.
> Uplink Out of Order Pkts Retransmitted | The number of uplink out of order packets that retransmitted.
> Downlink Out of Order Pkts Retransmitted | The number of downlink out of order packets that retransmitted.
> Uplink Bytes Invalid Length | The number of uplink bytes of invalid length.
> Downlink Bytes Invalid Length | The number of downlink bytes of invalid length.
> Uplink Pkts Invalid Length | The number of uplink packets of invalid length.
> Downlink Pkts Invalid Length | The number of downlink packets of invalid length.
> Uplink Bytes Out of Sequence | The number of uplink bytes out of sequence.
> Downlink Bytes Out of Sequence | The number of downlink bytes out of sequence.
> Uplink Pkts Out of Sequence | The number of uplink packets that were out of sequence.
> Downlink Pkts Out of Sequence | The number of downlink packets that were out of sequence.
> Uplink Bytes Invalid Close Wait | The total number of bytes received in uplink direction while system is in invalid wait state to close connection.
> Downlink Bytes Invalid Close Wait | The total number of bytes received in downlink direction while system is in invalid wait state to close connection.
> Uplink Pkts Invalid Close Wait | The total number of packets received in uplink direction while system is in invalid wait state to close connection.
> Downlink Pkts Invalid Close Wait | The total number of bytes received in downlink direction while system is in invalid wait state to close connection.
> Uplink Bytes Invalid Close State | The total number of bytes received in uplink direction while connection is in invalid closed state.
> Downlink Bytes Invalid Close State | The total number of bytes received in downlink direction while connection is in invalid closed state.
> Uplink Pkts Invalid Close State | The total number of packets received in uplink direction while connection is in invalid closed state.
> Downlink Pkts Invalid Close State | Total number of packets received in downlink direction while connection is in invalid closed state.
> Uplink Bytes Out of Order Timeout Failure | The total number of bytes received in uplink direction while timeout duration to wait for out of order packets is exhausted.
> Downlink Bytes Out of Order Timeout Failure | The total number of bytes received in downlink direction while timeout duration to wait for out of order packets is exhausted.
> Uplink Pkts Out of Order Timeout Failure | The total number of packets received in uplink direction while timeout duration to wait for out of order packets is exhausted.
> Downlink Pkts Out of Order Timeout Failure | The total number of bytes received in downlink direction while timeout duration to wait for out of order packets is exhausted.
> Uplink Bytes Out of Order Failure in Allocation | The total number of bytes received in uplink direction while allocation of out of order packet is failed.
> Downlink Bytes Out of Order Failure in Allocation | The total number of bytes received in downlink direction while allocation of out of order packet is failed.
> Uplink Pkts Out of Order Failure in Allocation | The total number of packets received in uplink direction while allocation of out of order packet is failed.
> Downlink Pkts Out of Order Failure in Allocation | The total number of packets received in downlink direction while allocation of out of order packet is failed.
> Uplink Pkts Invalid Window Size | The total number of packets received in uplink direction with invalid window size for buffer.
> Uplink Bytes Invalid Window Size | The total number of bytes received in uplink direction with invalid window size for buffer.
> Downlink Pkts Invalid Window Size | The total number of packets received in downlink direction with invalid window size for buffer.
> Downlink Bytes Invalid Window Size | Total total number of bytes received in downlink direction with invalid window size for buffer.
> Uplink Pkts Invalid Checksum | The total number of packets received in uplink direction with invalid checksum errors.
> Uplink Bytes Invalid Checksum | The total number of bytes received in uplink direction with invalid checksum errors.
> Downlink Pkts Invalid Checksum | The total number of packets received in downlink direction with invalid checksum errors.
> Downlink Bytes Invalid Checksum | The total number of bytes received in downlink direction with invalid checksum errors.

> ‌
> show active-charging analyzer statistics name tftp
> show active-charging analyzer statistics name tftp Command Output Descriptions

> Field | Description
> ACS TFTP Session Stats:
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total Uplink Packets | Total number of packets uplinked.
> Total Downlink Packets | Total number of packets downlinked.
> Total Read Sessions | Total number of read sessions.
> Total Write Sessions | Total number of write sessions.
> Total Invalid Control Packets | Total number of invalid control packets.
> Total Invalid Data Packets | Total number of invalid data packets.
> Total Packets with Unknown Request Type | Total number of packets with unknown request type.

> ‌
> show active-charging bandwidth-policy name
> show active-charging bandwidth-policy name Command Output Descriptions

> Field | Description
> Service Name | Name of the Active Charging Service.
> Bandwidth Policy Name | Name of the bandwidth policy.
> Flow Limit-for-Bandwidth ID and Group-ID Associations:
> Flow Limit-for-Bandwidth ID | The ACS flow limit-for-bandwidth ID.
> Group-ID | The ACS Bandwidth Policy Group ID.
> Total number of bw-ids configured in Bandwidth-Policy <policy> | The total number of bandwidth IDs configured in the specified bandwidth policy.
> Group-Limits for Group-ID | The group limits set for the group ID.
> Rates & Actions | Lists the following rates and actions:
> • | Peak Data Rate
> • | Peak Burst Size
> • | Violate Action
> • | Committed Data Rate
> • | Committed Burst Size
> • | Exceed Action
> Uplink | For bandwidth control in uplink direction indicates:
> • | Peak data rate in bits per second
> • | Peak burst size in bytes
> • | Violate action configured: discard/lower-ip-precedence
> • | Committed data rate in bits per second
> • | Committed burst size in bytes
> • | Exceed action configured: discard/lower-ip-precedence
> Downlink | For bandwidth control in downlink direction indicates:
> • | Peak data rate in bits per second
> • | Peak burst size in bytes
> • | Violate action configured: discard/lower-ip-precedence
> • | Committed data rate in bits per second
> • | Committed burst size in bytes
> • | Exceed action configured: discard/lower-ip-precedence
> Total number of group-limits configured in Bandwidth-Policy <policy> | The total number of group limits configured in the specified bandwidth policy.
> Total bandwidth-policies found | The total number of bandwidth policies matching the specified criteria.

> ‌
> show active-charging charging-action all
> show active-charging charging-action all Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | Name of the Active Charging Service.
> Charging Action Name | Name of the charging action. There may be several charging actions per charging service.
> Content ID | The content ID to use in the generated billing records as the Rating-Group Attribute Value Pair (AVP) for this charging action.
> Service ID | Service identifier value configured in the Charging Action mode.
> EDRs | Indicates whether Event Detail Record billing action for packets matching this charging action is enabled, and the EDR format.
> EGCDRs | Indicates whether eG-CDRs for billing of the packets matching with this charging action is enabled.
> UDRs | Indicates whether UDR generation is enabled.
> Flow Idle Timeout | Displays the idle-timeout for flows inspected by ECS.
> Limit For Flow Type | Indicates whether Limit For Flow Type is enabled/disabled.
> Limit For Uplink Bandwidth | Indicates whether Limit For Uplink Bandwidth is enabled/disabled.
> QoS Renegotiate Traffic-Class | Indicates whether QoS Renegotiate Traffic-Class is enabled/disabled.
> Limit For Downlink Bandwidth | Indicates whether Limit For Downlink Bandwidth is enabled/disabled.
> QoS Class Identifier | Indicates whether QoS Class Identifier is configured.
> IP Type of Service | Indicates whether IP Type of Service is configured.
> Count Retransmissions | Indicates whether Count Retransmissions is enabled.
> Content Filtering | Indicates whether Content Filtering is enabled.
> Type of Service | Displays the service type (PDSN, GGSN, etc.)
> Count Retries | Indicates if the ECS service is counting retransmitted packets per subscriber.
> GCDRs | Indicates if GCDRs are enabled or disabled.
> Discard | Specifies if the packets that match the flow should be discarded.
> Credit Control | Specifies if credit control is being used in this charging action
> Flow Action
> Redirect URL | Indicates whether the redirection of URL for packets that matches a rule definition is enabled/disabled. If enabled, redirects the HTTP packets matched to this Ruledef to the specified URL.
> Clear Quota Retry Timer | Indicates whether Clear Quota Retry Timer is enabled/disabled. If enabled, resets the Credit Control Application quota retry timer for specific subscriber upon redirection.
> Conditional Redirect | Indicates whether Conditional Redirect end token action is enabled/disabled. If enabled, conditionally redirects the HTTP packets matched to a configured user-agent to a specified URL.
> Discard | Indicates whether discard action is enabled/disabled. If enabled, discards the packet associated with the charging action.
> Terminate-Flow | Indicates whether terminate flow action is enabled/disabled. If enabled, terminates the TCP connection gracefully between the subscriber and external server and sends a TCP FIN to the subscriber and a TCP RST to the server. If the flow does not use TCP, this option simply discard the packets. This option is used for flows that use TCP only.
> Billing Action
> Event Data Record | Indicates whether EDRs are enabled/disabled.
> GGSN charging Data Record | Indicates whether GGSN CDRs are enabled/disabled.
> User Data Record | Indicates whether UDRs are enabled/disabled.
> Radius Accounting Record | Indicates whether RADIUS accounting records is enabled/disabled.
> Charge Volume | Indicates the charge volume for packet-length (payload).
> Total charging action(s) found | The number of charging actions that matched the criteria.

> ‌
> show active-charging charging-action statistics name
> show active-charging charging-action statistics name Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | Name of the Active Charging Service.
> Charging Action Name | Name of the charging action. There are be several charging actions per charging service.
> Uplink Pkts Retrans | Total number of uplink packets that were retransmitted.
> Downlink Pkts Retrans | Total number of downlink packets that were retransmitted.
> Uplink Bytes Retrans | Total number of uplink bytes that were retransmitted.
> Downlink Bytes Retrans | Total number of downlink bytes that were retransmitted.
> Upl Pkts Readdressed | Total number of readdressed uplink packets.
> Dnl Pkts Readdressed | Total number of readdressed downlink packets.
> Upl Bytes Readdressed | Total number of readdressed uplink bytes.
> Dnl Bytes Readdressed | Total number of readdressed downlink bytes.
> PP Upl Pkts Readdressed | Total number of post-processed uplink packets readdressed.
> PP Dnl Pkts Readdressed | Total number of post-processed downlink packets readdressed.
> PP Upl Bytes Readdressed | Total number of post-processed uplink bytes readdressed.
> PP Dnl Bytes Readdressed | Total number of post-processed downlink bytes readdressed.
> XHeader Information:
> XHeader Bytes Injected | Total number of x-header bytes injected.
> XHeader Pkts Injected | Total number of x-header packets injected.
> NCQoS Discarded Packets:
> Rule Bound elsewhere | Total number of rules bound elsewhere.
> Rule Binding pending | Total number of rule binding pending.
> Unbound Rule hit | Total number of unbound rule hits.
> Statistic | Statistic type.
> flow-action | Total number of matching flows/sessions/packets for the statistic.
> pp-flow-action | Total number of matching flows/sessions/packets for the statistic.
> flow-limit | Total number of matching flows/sessions/packets for the statistic.
> bandwidth-limit | Total number of matching flows/sessions/packets for the statistic.
> Total Charging Action(s) matched | Total number of charging actions matching the criteria.

> ‌
> show active-charging content-filtering category policy-id all
> show active-charging content-filtering category policy-id all Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | The Active Charging Service name.
> Content Filtering Policy | The Content Filtering Policy ID.
> Content Filtering Categories
> Category | Category of the content rated.
> Priority | Priority of the CF category in the CF Policy.
> Action | Action taken for the indicated result of CF analysis.
> Content Insert | The content string inserted in place of message returned from prohibited or restricted site or content server.
> Redirect | The URL to redirect subscribers.
> Reply Code | The reply code specified for www-reply-code-and-terminate-flow action.
> EDR | The EDR file format name to generate separate CF EDRs based on action and content category.
> Failure Action | The failure end condition if rating cannot be performed.
> Discarded-Flow-Content-ID | The content ID for the discarded flows. If not configured, this field is not displayed.

> ‌
> show active-charging content-filtering category statistics rulebase name
> show active-charging content-filtering category statistics rulebase name Command Output Descriptions

> Field | Description
> Service Name | Specifies name of the active charging service in which category-based content filtering application is configured.
> Rulebase Name | Specifies the name of Rulebase for category-based content filtering application.
> Content Filtering Statistics
> Flows discarded | Total number of flows discarded in content filtering application.
> Flows redirected | Total number of flows redirected in content filtering application.
> Flows allowed | Total number of flows allowed in content filtering application.
> Flows terminated | Total number of flows terminated in content filtering application.
> Flows discarded with content insertion | Total number of flows discarded and information content inserted in header of flow in content filtering application.
> Total Flows blocked | Total number of flows blocked in content filtering application.
> Total Number of dynamic DB lookups | Total number of lookups in dynamic database for Category-based Content Filtering application. This counter is not available in StarOS 9.0 and later releases.
> Total number of static DB lookups | Total number of lookups in static URL database for category based content filtering application.
> Total number of successful Cache lookups | Specifies the total number of successful lookups in cache memory for URLs.
> Total number of unknown URLs | Total number of flows/requests with unknown URL.
> Actions For Rating Attempts Not Completed
> Flows discarded | Total number of flows discarded in content filtering application.
> Flows redirected | Total number of flows redirected in content filtering application.
> Flows allowed | Total number of flows allowed in content filtering application.
> Flows terminated | Total number of flows terminated in content filtering application.
> Flows discarded with content insertion | Total number of flows discarded and information content inserted in header of flow in content filtering application.
> Total Flows blocked | Total number of flows blocked in content filtering application.
> Time taken for rating | A URL is classified (rated) as belonging to a distinct category (search, portal, etc.). This column displays the time taken to rate the URL in ms, in time slots of 100 ms, up to 1000 ms, and above 1000 ms.
> Number of URLs | Indicates the number of URLs rated in each time slot.
> Number of URLs (SRDB) | Indicates the number of URLs rated in a specific time slot from static rating database (SRDB).
> Number of URLs (Cache) | Indicates the number of URLs rated in a specific time slot from the cached list of URLs in memory.
> Attempts not completed | Indicates the number of URL rating attempts not completed.
> Total rulebases matched | Total number of rulebases that matched the criteria.

> ‌
> show active-charging content-filtering category statistics
> show active-charging content-filtering category statistics Command Output Descriptions

> Field | Description
> Service Name | Name of the Active Charging Service in which category-based content filtering application is configured.
> Cumulative Content Filtering Statistics:
> Flows discarded | Total number of flows discarded.
> Flows redirected | Total number of flows redirected.
> Flows allowed | Total number of flows allowed.
> Flows terminated | Total number of flows terminated.
> Flows discarded with content insertion | Total number of flows discarded and content inserted in header of flow.
> Total Flows blocked | Total number of flows blocked.
> Total Number of dynamic DB lookups | Total number of lookups in dynamic database. This counter is not available in StarOS 9.0 and later releases.
> Total number of static DB lookups | Total number of lookups in static URL database.
> Total number of successful Cache lookups | Total number of successful URL lookups in cache memory.
> Total number of unknown URLs | Total number of flows/requests with unknown URL.
> Failure Action (Rating Attempts Not Completed):
> Flows discarded | Total number of flows discarded due to failure action.
> Flows redirected | Total number of flows redirected due to failure action.
> Flows allowed | Total number of flows allowed due to failure action.
> Flows terminated | Total number of flows terminated due to failure action.
> Flows discarded with content insertion | Total number of flows discarded and information content inserted in header of flow due to failure action.
> Total Flows blocked | Total number of flows blocked due to failure action.
> Time taken for rating | A URL is classified (rated) as belonging to a distinct category (search, portal, etc.). This column displays the time taken to rate the URL in ms, in time slots of 100 ms, up to 1000 ms, and above 1000 ms.
> Number of URLs | Total number of URLs rated in each time slot.
> Attempts not completed | Total number of URL rating attempts not completed.
> Cumulative Dynamic Content Filtering Statistics
> Dynamic Flows discarded | Total number of dynamic flows discarded.
> Dynamic Flows redirected | Total number of dynamic flows redirected.
> Dynamic Flows allowed | Total number of dynamic flows allowed.
> Dynamic Flows terminated | Total number of dynamic flows terminated.
> Dynamic Flows discarded with content insertion | Total number of dynamic flows discarded and content inserted in header of flow.
> Total Dynamic Flows blocked | Total number of dynamic flows blocked.
> Total Number of dynamic lookups | Total number of dynamic lookups.
> Total number of unknown URLs | Total number of flows/requests with unknown URLs.
> Response codes not in range 2xx | Number of responses that were not sent for dynamic rating as the response was not in the 2xx range.
> Dynamic Failure Action (Rating Attempts Not Completed):
> Flows discarded | Total number of flows discarded due to failure action.
> Flows redirected | Total number of flows redirected due to failure action.
> Flows allowed | Total number of flows allowed due to failure action.
> Flows terminated | Total number of flows terminated due to failure action.
> Flows discarded with content insertion | Total number of flows discarded and information content inserted in header of flow due to failure action.
> Total Flows blocked | Total number of flows blocked due to failure action.
> Time taken for Dynamic rating | A URL is classified (rated) as belonging to a distinct category (search, portal, etc.). This column displays the time taken to rate the URL in ms, in time slots of 100 ms, up to 1000 ms, and above 1000 ms.
> Number of URLs | Total number of URLs rated in each time slot.
> Attempts not completed | Total number of URL rating attempts not completed.
> Number of Packets Hit per Category | Indicates the specific category and the number of packets hit per category. If during runtime, an x-category was added, the x-category is also displayed.
> Number of Packets Blocked per Category | Indicates the specific category and the number of packets blocked per category. If during runtime, an x-category was added, the x-category is also displayed.

> ‌
> show active-charging content-filtering server-group name
> show active-charging content-filtering server-group name Command Output Descriptions

> Field | Description
> Content Filtering Group | The Content Filtering Server Group (CFSG) name.
> Context | The context in which the CFSG is configured.
> Origin Address | IP address of the origin endpoint or ICAP client.
> ICAP Address (Port) | IP address and port number of ICAP server with in CF Server Group.
> Max Outstanding | The total number of unanswered outstanding messages to this ICAP server.
> Response Timeout | The response-timeout duration configured to wait for response.
> Connection Retry Timeout | The connection retry timeout duration configured to check the TCP connection status between ICAP sever and client.
> Dictionary | The dictionary used for encoding requests to the server(s).
> Timeout Action | The action configured for connection timeout.
> Deny Message | The text string message that is returned to the subscriber in a deny response.
> URl-extraction | The ICAP URL extraction mode:
> • | after-parsing: Percent-encoded hex characters in URLs sent from the ACF client to the ICAP server are converted to corresponding ASCII characters and sent.
> • | raw: The URLs contain percent-encoded hex characters as is.
> Content Filtering Group Connections | The total number of CF server group connections open.
> ACSMgr Instance | Number of ACS Manager instance.
> Connection State | Status of ACS Manager instance for CF server group connection.
> Total content filtering groups matching specified criteria | The total number of CFSG matching the criteria.

> ‌
> show active-charging content-filtering server-group statistics verbose
> show active-charging content-filtering server-group statistics verbose Command Output Descriptions

> Field | Description
> Content Filtering Group | Name of the Content Filtering Server Group (CFSG).
> Connection Statistics
> Current Open Connections | Total number of open connections.
> Connection DHOST requests | Total number of DHOST requests.
> Successful Connections | Total number of successful connections.
> Connections DHOST remove | Total number of connections removed from DHOST.
> Connection SHUTDOWN req | Total number of requests for SHUTDOWN.
> ACF Unreachable(read) | Total number of attempts for Active Content Filter server (ICAP server) to read.
> ACF Unreachable(write) | Total number of attempts for Active Content Filter server (ICAP server) to write.
> Reconnect attempts | Total number of reconnect attempts for ACF server (ICAP server).
> Connection Timeout | Total number of connections timeout after reconnect attempts for ACF server (ICAP server).
> Connection Failure Statistics
> Connection DHOST errors | Total number of DHOST errors in connection.
> Connection CONNECT error | Total number of CONNECT errors in connection.
> Socket open errors | Total number of errors due to SOCKET open in connection.
> Connection bind errors | Total number of BIND errors in connection.
> Connection setvr errors | Total number of SETVER errors in connection.
> Connection NONBLOCK errors | Total number of NONBLOCK errors in connection.
> Connection SHUTDOWN errors | Total number of SHUTDOWN errors in connection.
> Incomplete 3-way handshaking | Total number of errors due to incomplete 3-way handshaking in TCP connection.
> ACF Statistics
> ACF Requests Created | Total number of requests created for ACF.
> Response Timeout | Total number of response timeout for requests to ACF.
> Write request success | Total number of successful WRITE requests.
> Write request failed | Total number of failed WRITE requests.
> Read response success | Total number of successful READ response.
> Read response failed | Total number of failed READ response.
> HTTP Permit | Total number of HTTP URLs permitted from ACF.
> WAP Permit | Total number of WAP URLs permitted from ACF.
> HTTP Denny | Total number of HTTP URLs denied from ACF.
> WAP Denny | Total number of WAP URLs denied from ACF.
> HTTP Redirect | Total number of HTTP URLs redirected from ACF.
> WAP Redirect | Total number of WAP URLs redirected from ACF.
> Invalid ACTION | Total number of invalid ACTION message from ACF.
> Redirect URL not defined | Total number of errors due to undefined redirect URL.
> Buffer List Empty | Total number of errors due to empty buffer list.
> Failure Action (communication failure with server-group):
> Permit | Total number of connections permitted after connection failure.
> Content Insertion | Total number of connections with content inserted after connection failure.
> Discard | Total number of connections discarded after connection failure.
> Terminate Flow | Total number of connections terminated after connection failure.
> Redirect URL | Total number of connections redirected after connection failure.
> Total action taken | Total number of actions taken after connection failure.
> Num pkts dropped for DENY | Total number of packets dropped after denying the connection due to failure in connection.
> Num pkts dropped for REDIRECT | Total number of packets dropped after redirecting the connection due to failure in connection.
> Num pkts dropped for DENY Timeout action | Total number of packets dropped after denying the connection due to timeout action.
> Num pkts dropped for REDIRECT Timeout action | Total number of packets dropped after redirecting the connection due to timeout action.
> Failure Action (communication with server-group not attempted): | ICAP stats indicating failure (like memory allocation failure, server connection error, etc) on ICAP before a request is sent to the ICAP server.
> Permit | Total number of connections permitted after connection failure.
> Content Insertion | Total number of connections with content inserted after connection failure.
> Discard | Total number of connections discarded after connection failure.
> Terminate Flow | Total number of connections terminated after connection failure.
> Redirect URL | Total number of connections redirected after connection failure.
> ACF Resp Parse Statistics | Statistics related to ACF response parsing.
> Parse ACF resp success | Total number of successful ACF parse response.
> Parse ACF resp ver err | Total number of successful ACF parse response version error.
> Misc Statistics | Miscellaneous statistics.
> Total pkts sent | Total number of packets sent through ICAP connection.
> Invalid ACF group config | Total number of errors due to invalid CF Server Group (Active Content Filter server groups) configuration.
> Invalid bind address | Total number of errors due to invalid binding address configuration.
> Invalid ICAP address | Total number of errors due to invalid ICAP server addresses.
> ICAP queue length statistics |
> SessionMgr ID | Session Manager ID.
> ICAP queue length | Queue size of outstanding ICAP requests per Session Manager.
> Histogram of ICAP Server's Response time
> Response Time(ms) | Response time slots, in milliseconds.
> No Of Responses | Number of responses per time slot.

> ‌
> show active-charging credit-control statistics
> show active-charging credit-control statistics Command Output Descriptions

> Field | Description
> Active Charging Service | The Active Charging Service name.
> Credit Control Group | The Credit Control Group name. This field is displayed only if there are credit control group(s) configured.
> CC Session Stats
> Total Current Sessions | The total number of Credit Control sessions active.
> Total ECS Adds | The total number of ECS sessions added to Credit Control application.
> Total CC Starts | The total number of Credit Control sessions started.
> Total Session Updates | The total number of Credit Control sessions updated.
> Total Terminated | The total number of Credit Control sessions terminated.
> CC Session Failovers | The total Credit Control sessions failed.
> CC Message Stats
> Total Messages Received | The total Credit Control messages received.
> Total Messages Sent | The total Credit Control messages sent.
> Total CC Requests | The total number of CCRs (Credit Control Request) messages that went out from system to the Credit Control Server. The CCR can be Initial/Update or Terminate.
> Total CC Answers | The total number of CCA (Credit Control Answer) messages that came into system from Credit Control Server.
> CCR-Initial | The total number of CCR-Initial (Initial Credit Control Request) messages that went out from system to the Credit Control Server.
> CCA-Initial | The total number of CCA-Initial (Initial Credit Control Answer) messages that came into system from Diameter Server.
> CCA-Initial Accept | The total number of CCA-Initial-Accept (Initial Credit Control Answer sent and accepted) messages that came into system from Credit Control Server.
> CCA-Initial Reject | The total number of CCA-Initial-Reject (Initial Credit Control Answer sent and rejected.) messages that came into system from Credit Control Server.
> CCA-Initial Timeouts | The total number of CCA-Initial-Timeouts (Initial Credit Control Answer sent and timed out) messages that came into system from Credit Control Server.
> CCR-Update | The total number of CCR-Updates (Credit Control Request with Update) messages that went out from system to the Credit Control Server.
> CCA-Update | The total number of CCA-Update (Credit Control Answer for update) messages that came into system from Credit Control Server.
> CCA-Update Timeouts | The total number of CCA-Update Timeouts (Credit Control Answer for update sent and timed out) messages that came into system from Credit Control Server.
> CCR-Final | The total number of CCR-Final (Credit Control Request with Final) messages that went out from system to the Credit Control Server.
> CCA-Final | The total number of CCA-Final (Credit Control Answer for final update sent) messages that came into system from Credit Control Server.
> CCA-Final Timeouts | The total number of CCA-Final Timeouts (Credit Control Answer for final update sent and time-out) messages that came into system from Credit Control Server.
> ASR | The total number of Abort-Session Request messages came into system from Credit Control Server.
> ASA | The total number of Abort-Session Accept messages sent from system to Credit Control server. This message will be followed by a CCR- Terminate to terminate the session.
> RAR | The total number of ReAuth Request messages came into system from Diameter Server
> RAA | The total number of ReAuth Accept messages sent from system to Credit Control server. This message is followed by a CCR-Update to update the Credit Control server about the session.
> CCA Dropped | The total number of CCA (Credit Control Answers) messages dropped by system.
> CC Message Error Stats
> Diameter Protocol Errs | The total message errors due to DIAMTER protocol.
> Bad Answers | The total message errors due to invalid response.
> Unknown Session Reqs | The total message errors due to invalid session requests.
> Unknown Command Code | The total message errors due to invalid/unknown command code (ASR, RAR).
> Request Timeouts | The total message errors due to request timeout.
> Parse Errors | The total message errors due to parsing errors.
> Unknown Rating Group | The total message errors due to invalid/unknown Rating Groups. Rating group is used to identify a particular type of traffic.
> Unknown Rulebase | The total message errors due to invalid/unknown Rulebase applied.
> Unk Failure Handling | The total message errors due to invalid/unknown reasons.
> CC Update Reporting Reason Stats
> Threshold | For each of the Rating group, the Credit Control server send a threshold (this is also configurable in a system) after which a update needs to be sent. For example, a subscriber quota of 1000 bytes with 900 as threshold is sent to Credit Control Application. When 900 bytes have consumed by the system, an update message is sent for quota. This counter gives the number of updates sent because of threshold.
> QHT | The total number of updates sent due to expiry of Quota Hold Timer (QHT).
> Final | The total number of updates sent due to expiry of final unit of quota.
> Quota Exhausted | The total number updates sent due to quota of subscriber was exhausted.
> Validity Time | The total number of updates sent because of the session validity time expired.
> Other Quota | The total number updates sent due to request for additional quota for subscriber.
> Rating Condition Change | The total number of updates sent due change in RAT/QOS/SGSN/CELLID/LAC.
> Forced Reauthorization | The total number of updates sent because of RAR.
> CC Termination Cause Stats
> Diameter Logout | The total number of Credit Control Application session terminated due to subscriber logout.
> Service Not Provided | The total number of Credit Control Application session terminated as service was not available.
> Bad Answer | The total number of Credit Control Application session terminated due to invalid/unknown response received.
> Administrative | The total number of Credit Control Application session terminated by administrator.
> Link Broken | The total number of Credit Control Application session terminated due to broken/down link.
> Auth Expired | The total number of Credit Control Application session terminated due to authorization of subscriber expired.
> User Moved | The total number of Credit Control Application session terminated as subscriber moved to out of service area.
> Session Timeout | The total number of Credit Control Application session terminated due to timeout.
> CC Traffic Category Stats
> Category Creates | The total traffic categories created.
> Category Deletes | The total traffic categories deleted.
> Category Lookups | The total traffic categories available.
> Hits | The total traffic categories triggered.
> Misses | The total traffic categories triggered and missed.
> Trigger Events | The total traffic categories triggered.
> Final Unit Consumed | The total units consumed by subscriber during session.
> Category Success | The total number of successful traffic category sessions.
> Rating Failed | The total Rating Groups failed during session.
> Service Denied | The total number of services denied during session.
> Limit Reached | The total number of events when subscriber reached quota limit.
> Auth Rejected | The total number of authorization rejected.
> Other Errors | The total number of miscellaneous/unknown errors not specified by system.

> ‌
> show active-charging edr-format all
> show active-charging edr-format all Command Output Descriptions

> Field | Description
> Service Name | Name of the Active Charging Service.
> EDR Format Name | Name of the configured EDR format.
> Attribute | Attribute information configured in specific EDR format.
> Total edr-format(s) found | The total number of configured existing EDR formats.

> ‌
> show active-charging edr-format statistics
> show active-charging edr-format statistics Command Output Descriptions

> Field | Description
> Total edr-formats | The total number of EDR formats configured.
> Total edrs generated | The total number of EDRs generated.
> Total NAT bind records generated | The total number of Network Address Translation (NAT) bind records generated. This field is only displayed, if configured, in StarOS 8.3 and later.

> ‌
> show active-charging edr-udr-file flow-control-counters
> show active-charging edr-udr-file flow-control-counters Command Output Descriptions

> Field | Description
> Num of Times Flow Control initiated | Total number of times the flow control initiated.
> Num of Outstanding Messages | Total number outstanding messages for flow control.
> Num of unsent Messages | Total number unsent messages for flow control.
> Num of CDR records Discarded due to flow control | Total number of charging detail records (CDRs) discarded due to flow control action.
> Last flow control occurrence | Date and time of the last occurrence of flow control action.

> ‌
> show active-charging edr-udr-file statistics
> show active-charging edr-udr-file statistics Command Output Descriptions

> Field | Description
> Overall Stats
> Files rotated | Total number of EDR and UDR files rotated.
> Files rotated due to volume limit | Total number of EDR and UDR files rotated due to volume limit.
> Files rotated due to time limit | Total number of EDR and UDR files rotated due to time limit.
> Files rotated due to records limit | Total number of files rotated because of record limits.
> File rotation failure | Total number of rotation failed for EDR and UDR file.
> Files deleted | Total number of EDR and UDR files deleted.
> Files received | Total number of EDR and UDR files received by service.
> Current open files | Total number of EDR and UDR files open.
> Time of last file deletion | Date and time of last EDR/UDR file deleted.
> EDR Specific Stats
> EDR files rotated | Total number of EDR files rotated.
> EDR files rotated due to volume limit | Total number of EDR files rotated due to volume limit.
> EDR files rotated due to time limit | Total number of EDR files rotated due to time limit.
> EDR files rotated due to records limit | Total number of EDR files rotated due to records limit
> EDR files rotation failure | Total number of rotation failed for EDR file.
> EDR files deleted | Total number of EDR files deleted.
> EDR records deleted | Total number of EDR records deleted.
> EDR records received | Total number of EDR records received.
> Current open EDR files | Total number of EDR files open.
> Time of last EDR file deletion | Date and time of last EDR file deleted.
> UDR Specific Stats
> UDR files rotated | Total number of UDR files rotated.
> UDR files rotated due to volume limit | Total number of UDR files rotated due to volume limit.
> UDR files rotated due to time limit | Total number of UDR files rotated due to time limit.
> UDR files rotated due to records limit | Total number of UDR files rotated due to records limit.
> UDR files rotation failure | Total number of rotation failed for UDR file.
> UDR files rotated due to records limit | Total number of UDR files that were rotated due to records limit
> UDR files deleted | Total number of UDR files deleted.
> UDR records deleted | Total number of UDR records deleted.
> UDR records received | Total number of UDR records received.
> Current open UDR files | Total number of UDR files open.
> Time of last UDR file deletion | Date and time of last UDR file deleted.

> ‌
> show active-charging firewall statistics
> show active-charging firewall statistics Command Output Descriptions

> Field | Description
> Firewall Statistics for context | The context name.
> Data Stats:
> Total Packets Received | Total number of packets received by the firewall.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of uplink packets dropped by the firewall.
> Uplink Bytes Dropped | Total number of uplink bytes dropped by the firewall.
> Downlink Packets Dropped | Total number of downlink packets dropped by the firewall.
> Downlink Bytes Dropped | Total number of downlink bytes dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics nat-realm
> show active-charging firewall statistics nat-realm Command Output Descriptions

> Field | Description
> Firewall Statistics for NAT-realm | The NAT realm name for which the statistics are displayed.
> Data Stats:
> Total Packets Received | Total number of packets received by the NAT realm.
> Total Bytes Received | Total number of bytes received by the NAT realm.
> Total Packets Sent | Total number of packets sent by the NAT realm.
> Total Bytes Sent | Total number of bytes sent by the NAT realm.
> Total Packets Injected | Total number of packets injected by the NAT realm.
> Total Bytes Injected | Total number of bytes injected by the NAT realm.
> Uplink Packets Dropped | Total number of uplink packets dropped by the NAT realm.
> Uplink Bytes Dropped | Total number of uplink bytes dropped by the NAT realm.
> Downlink Packets Dropped | Total number of downlink packets dropped by the NAT realm.
> Downlink Bytes Dropped | Total number of downlink bytes dropped by the NAT realm.
> Total Malformed Packets | Total number of malformed packets detected by the NAT realm.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the NAT realm.
> Total Flows Processed by NAT-realm | Total number of flows processed by the NAT realm.

> ‌
> show active-charging firewall statistics verbose
> show active-charging firewall statistics verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Context | The context name.
> IP Stats:
> Land Attacks | Total number of Land attacks detected by firewall.
> Jolt Attacks | Total number of Jolt attacks detected by firewall.
> Teardrop Attacks | Total number of Teardrop attacks detected by firewall.
> Zero Length IP Option | Total number of Zero-length IP option attacks detected by firewall.
> IP Source-router Attacks | Total number of IP Source-router attacks detected by firewall.
> Packets with IP-Unaligned-Timestamp | Total number of packets with IP unaligned timestamps detected by firewall.
> Packets with Short IP Header Length | Total number of packets with short IP header length detected by firewall.
> Packets Dropped due to IP Checksum Errors | Total number of packets dropped due to IP Checksum error.
> Downlink Dropped Bytes on IP Reassembly Failure | Total number of downlink bytes dropped on IP Reassembly failure.
> Uplink Dropped Bytes on IP Reassembly Failure | Total number of uplink bytes dropped on IP Reassembly failure.
> TCP Stats:
> Data Packets Received After RST/FIN | Total number of data packets received after receiving RST (reset) request by the firewall.
> Invalid SEQ Number Received with RST | Total number of invalid sequence-number received with RST (reset) request by the firewall.
> Data without Connection Established | Total number of data packets received before the establishment of connection by the firewall.
> Invalid TCP Connection Requests | Total number of invalid TCP connection requests received by the firewall.
> Invalid TCP pre-connection Requests | Total number of invalid TCP pre-connection requests received by firewall.
> Invalid ACK Value (Cookie Enabled) | Total number of invalid ACK values (to enable cookies) received by firewall.
> Invalid TCP Packet Length | Total number of TCP packets with invalid length received by firewall.
> Packets with Short TCP Header Length | Total number of TCP packets with invalid/short header length received by firewall.
> Packets Dropped due to TCP Checksum Errors | Total number of packets dropped due to TCP Checksum error.
> Packets with SEQ/ACK Out-of-range | Total number of packets with out of range SEQ/ACK.
> TCP Null Scan Attacks | Total number of TCP Null Scan attacks detected by firewall.
> Post Connection SYN | Total number of Post Connection SYN attacks detected by firewall.
> Unable to Send SYN Packet | Total number of attempts detected by the firewall when node failed to send SYN packets.
> Send Final ACK to Target Failed | Total number of attempts detected by the firewall when node failed to send Final ACK packet to target node.
> Invalid TCP Packet: SYN-ACK Expected | Total number of invalid TCP packets received by the firewall in place of SYN+ACK packets.
> No TCP Flags Set | Total number of TCP packets received with no flags set.
> All TCP Flags Set | Total number of TCP flags received with all flags set.
> Invalid TCP Packets | Total number of invalid TCP packets including all type of errors and attacks received by the firewall.
> Flows Closed by RST before 3-Way Handshake | Total number flows closed by RST (reset) message before the 3-way handshaking.
> Flows Timed-out in SYN_RCVD1 State | Total number of flows timed out in SYN_RCVD1 state.
> Flows Timed-out in SYN_RCVD2 State | Total number of flows timed out in SYN_RCVD2 state.
> Flows Terminated due to WinNuke Attack | Total number of flows terminated due to WinNuke attacks by the firewall.
> TCP-SYN Flood Attacks | Total number of TCP-SYN Flood attacks detected by firewall.
> Packets Dropped on TCP-SYN Flood Attack | Total number of packets dropped by the firewall in TCP-SYN Flood attacks.
> FTP-Bounce Attacks | Total number of FTP-Bounce attacks detected by the firewall.
> Mime-Flood Attacks | Total number of Mime-Flood attacks detected by the firewall.
> Proxy Handshakes Completed | Total number of times proxy handshake was completed.
> Packets Dropped due to source port zero | Total number of packets dropped due to source port zero error.
> SYN Packets Dropped due to ECE/CWR Set | Total number of SYN packets dropped due to ECE/CWR Flags Set.
> UDP Stats:
> Invalid UDP Echo Response | Total number of invalid UDP echo responses.
> Invalid UDP Packet Length | Total number of invalid UDP packet length.
> Packets Dropped due to UDP Checksum Errors | Total number of packets dropped due to UDP Checksum errors.
> Packets with Short UDP Header Length | Total number of packets with short UDP header length.
> Packets Dropped on UDP Flood Attack | Total number of packets dropped by the firewall in UDP flood attacks.
> Packets Dropped due to exceeding ICMP dest unreachable threshold | Total number of packets dropped due to exceeding ICMP destination unreachable threshold.
> ICMP Stats:
> Invalid ICMP Response | Total number of invalid ICMP responses.
> ICMP Reply Error | Total number of ICMP reply errors.
> Invalid ICMP Type Packet | Total number of invalid ICMP type packets.
> ICMP Error Message Replay Attacks | Total number of ICMP error message replay attacks detected by the firewall.
> ICMP Packets with Duplicate Sequence Number | Total number of ICMP packets with duplicate sequence numbers.
> Packets with Short ICMP Header Length | Total number of packets with short ICMP header length.
> Packets Dropped on ICMP Flood Attack | Total number of packets dropped by the firewall in ICMP flood attacks.
> Ping Of Death Attacks | Total number of Ping-of-Death attacks detected by the firewall.
> Packets Dropped due to ICMP Checksum Errors | Total number of packets dropped due to ICMP Checksum error.
> ICMP Packets With Destination Unreachable Message | Total number of ICMP packets with destination unreachable message.
> General Stats:
> Packets without Any Data Received | Total number of packets received without any data.
> No Matching Uplink Ruledef | Total number of uplink packets with no matching ruledef.
> No Matching Downlink Ruledef | Total number of downlink packets with no matching ruledef.
> Deny Ruledef Matched | Total number of times deny ruledef was matched.
> Packets Dropped due to No Ruledef in Rulebase | Total number of packets dropped due to no ruledef in rulebase.
> Packets Dropped due to Miscellaneous Errors | Total number of packets dropped due to miscellaneous errors.
> Flows Timed-out | Total number of flows that timed out.
> Flows Not Established from External Network | Total number of flows from external networks that were not established.
> Max Flows Limit Reached | Total number of times the maximum flows limit was reached.
> ALG statistics:
> Packets dropped by SIP ALG | Total number of packets dropped by SIP ALG.
> Packets injected by SIP ALG | Total number of packets injected by SIP ALG.
> Data Stats:
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics protocol icmp verbose
> show active-charging firewall statistics protocol icmp verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Protocol: ICMP
> ICMP Stats
> Invalid ICMP Response | Total number of invalid ICMP responses.
> ICMP Reply Error | Total number of ICMP reply errors.
> Invalid ICMP Type Packet | Total number of invalid ICMP type packets.
> ICMP Error Message Replay Attacks | Total number of ICMP error message replay attacks detected by the firewall.
> ICMP Packets with Duplicate Sequence Number | Total number of ICMP packets with duplicate sequence numbers.
> Packets with Short ICMP Header Length | Total number of packets with short ICMP header length.
> Invalid ICMP Packet Length | Total number of packets with invalid ICMP packet length.
> Packets Dropped on ICMP Flood Attack | Total number of packets dropped by the firewall in ICMP flood attacks.
> Ping Of Death Attacks | Total number of Ping-of-Death attacks detected by the firewall.
> Packets Dropped due to ICMP Checksum Errors | Total number of packets dropped due to ICMP Checksum error.
> ICMP Packets With Destination Unreachable Message | Total number of ICMP packets with destination unreachable message.
> Data Stats
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics protocol ip verbose
> show active-charging firewall statistics protocol ip verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Protocol IP in Context | The context name.
> IP Stats:
> Land Attacks | Total number of Land attacks detected.
> Jolt Attacks | Total number of Jolt attacks detected.
> Teardrop Attacks | Total number of Teardrop attacks detected.
> Zero Length IP Option | Total number of Zero-length IP Option attacks detected.
> IP Source-router Attacks | Total number of IP Source-router attacks detected.
> Packets with IP-Unaligned-Timestamp | Total number of packets with IP-Unaligned-Timestamp.
> Packets with Short IP Header Length | Total number of packets with short IP header length.
> Packets Dropped due to IP Checksum Errors | Total number of packets dropped due to checksum errors.
> Downlink Dropped Bytes on IP Reassembly Failure | Total number of bytes dropped in downlink flow on IP Reassembly failure.
> Uplink Dropped Bytes on IP Reassembly Failure | Total number of bytes dropped in uplink flow on IP Reassembly failure.
> Data Stats:
> Total Packets Received | Total number of packets received by the firewall.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of uplink packets dropped by the firewall.
> Uplink Bytes Dropped | Total number of uplink bytes dropped by the firewall.
> Downlink Packets Dropped | Total number of downlink packets dropped by the firewall.
> Downlink Bytes Dropped | Total number of downlink bytes dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics protocol udp verbose
> show active-charging firewall statistics protocol udp verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Protocol: UDP
> UDP Stats
> Invalid UDP Echo Response | Total number of invalid UDP echo responses.
> Invalid UDP Packet Length | Total number of invalid UDP packet length.
> Packets Dropped due to UDP Checksum Errors | Total number of packets dropped due to UDP Checksum errors.
> Packets with Short UDP Header Length | Total number of packets with short UDP header length.
> Packets Dropped on UDP Flood Attack | Total number of packets dropped by the firewall in UDP flood attacks.
> Packets Dropped due to exceeding ICMP dest unreachable threshold | Total number of packets dropped due to exceeding ICMP destination unreachable threshold.
> Data Stats
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics callid <call_id> verbose
> show active-charging firewall statistics callid <call_id> verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Callid: <call_id>
> IP Stats:
> Land Attacks | Total number of Land attacks detected by firewall.
> Jolt Attacks | Total number of Jolt attacks detected by firewall.
> Teardrop Attacks | Total number of Teardrop attacks detected by firewall.
> Invalid IP Option Length | Total number of Invalid IP Option Length attacks detected by firewall.
> IP Source-router Attacks | Total number of IP Source-router attacks detected by firewall.
> Packets with IP-Unaligned-Timestamp | Total number of packets with IP unaligned timestamps detected by firewall.
> Packets with Short IP Header Length | Total number of packets with short IP header length detected by firewall.
> Packets Dropped due to IP Checksum Errors | Total number of packets dropped due to IP Checksum error.
> Downlink Dropped Bytes on IP Reassembly Failure | Total number of downlink bytes dropped on IP Reassembly failure.
> Uplink Dropped Bytes on IP Reassembly Failure | Total number of uplink bytes dropped on IP Reassembly failure.
> TCP Stats:
> Data Packets Received After RST/FIN | Total number of data packets received after receiving RST (reset) request by the firewall.
> Invalid SEQ Number Received with RST | Total number of invalid sequence-number received with RST (reset) request by the firewall.
> Data without Connection Established | Total number of data packets received before the establishment of connection by the firewall.
> Invalid TCP Connection Requests | Total number of invalid TCP connection requests received by the firewall.
> Invalid TCP pre-connection Requests | Total number of invalid TCP pre-connection requests received by firewall.
> Invalid ACK Value (Cookie Enabled) | Total number of invalid ACK values (to enable cookies) received by firewall.
> Invalid TCP Packet Length | Total number of TCP packets with invalid length received by firewall.
> Packets with Short TCP Header Length | Total number of TCP packets with invalid/short header length received by firewall.
> Packets Dropped due to TCP Checksum Errors | Total number of packets dropped due to TCP Checksum error.
> Packets with SEQ/ACK Out-of-range | Total number of packets with out of range SEQ/ACK.
> TCP Null Scan Attacks | Total number of TCP Null Scan attacks detected by firewall.
> Post Connection SYN | Total number of Post Connection SYN attacks detected by firewall.
> Unable to Send SYN Packet | Total number of attempts detected by the firewall when node failed to send SYN packets.
> Send Final ACK to Target Failed | Total number of attempts detected by the firewall when node failed to send Final ACK packet to target node.
> Invalid TCP Packet: SYN-ACK Expected | Total number of invalid TCP packets received by the firewall in place of SYN+ACK packets.
> No TCP Flags Set | Total number of TCP packets received with no flags set.
> All TCP Flags Set | Total number of TCP flags received with all flags set.
> Invalid TCP Packets | Total number of invalid TCP packets including all type of errors and attacks received by the firewall.
> Flows Closed by RST before 3-Way Handshake | Total number flows closed by RST (reset) message before the 3-way handshaking.
> Flows Timed-out in SYN_RCVD1 State | Total number of flows timed out in SYN_RCVD1 state.
> Flows Timed-out in SYN_RCVD2 State | Total number of flows timed out in SYN_RCVD2 state.
> Flows Terminated due to WinNuke Attack | Total number of flows terminated due to WinNuke attacks by the firewall.
> TCP-SYN Flood Attacks | Total number of TCP-SYN Flood attacks detected by firewall.
> Packets Dropped on TCP-SYN Flood Attack | Total number of packets dropped by the firewall in TCP-SYN Flood attacks.
> FTP-Bounce Attacks | Total number of FTP-Bounce attacks detected by the firewall.
> Mime-Flood Attacks | Total number of Mime-Flood attacks detected by the firewall.
> Proxy Handshakes Completed | Total number of times proxy handshake was completed.
> Packets Dropped during Proxy Handshake | Total number of packets dropped during proxy handshake.
> UDP Stats:
> Invalid UDP Echo Response | Total number of invalid UDP echo responses.
> Invalid UDP Packet Length | Total number of invalid UDP packet length.
> Packets Dropped due to UDP Checksum Errors | Total number of packets dropped due to UDP Checksum errors.
> Packets with Short UDP Header Length | Total number of packets with short UDP header length.
> Packets Dropped on UDP Flood Attack | Total number of packets dropped by the firewall in UDP flood attacks.
> Packets Dropped due to exceeding ICMP dest unreachable threshold | Total number of packets dropped due to exceeding ICMP destination unreachable threshold.
> ICMP Stats:
> Invalid ICMP Response | Total number of invalid ICMP responses.
> ICMP Reply Error | Total number of ICMP reply errors.
> Invalid ICMP Type Packet | Total number of invalid ICMP type packets.
> ICMP Error Message Replay Attacks | Total number of ICMP error message replay attacks detected by the firewall.
> ICMP Packets with Duplicate Sequence Number | Total number of ICMP packets with duplicate sequence numbers.
> Packets with Short ICMP Header Length | Total number of packets with short ICMP header length.
> Invalid ICMP Packet Length | Total number of packets with invalid ICMP packet length.
> Packets Dropped on ICMP Flood Attack | Total number of packets dropped by the firewall in ICMP flood attacks.
> Ping Of Death Attacks | Total number of Ping-of-Death attacks detected by the firewall.
> Packets Dropped due to ICMP Checksum Errors | Total number of packets dropped due to ICMP Checksum errors.
> ICMP Packets With Destination Unreachable Message | Total number of ICMP packets with Destination Unreachable Message.
> General Stats:
> Packets without Any Data Received | Total number of packets received without any data.
> No Matching Uplink Ruledef | Total number of uplink packets with no matching ruledef.
> No Matching Downlink Ruledef | Total number of downlink packets with no matching ruledef.
> Deny Ruledef Matched | Total number of times deny ruledef was matched.
> Packets Dropped due to No Ruledef in Rulebase | Total number of packets dropped due to no ruledef in rulebase.
> Packets Dropped due to Miscellaneous Errors | Total number of packets dropped due to miscellaneous errors.
> Flows Timed-out | Total number of flows that timed out.
> Flows Not Established from External Network | Total number of flows from external networks that were not established.
> Max Flows Limit Reached | Total number of times the maximum flows limit was reached.
> IP Retransmitted Packets Dropped | Total number of IP retransmitted packets dropped.
> Data Stats:
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics domainname <domain_name> verbose
> show active-charging firewall statistics domainname <domain_name> verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for 2 Sessions with Domain-name: <domain_name>
> IP Stats:
> Land Attacks | Total number of Land attacks detected by firewall.
> Jolt Attacks | Total number of Jolt attacks detected by firewall.
> Teardrop Attacks | Total number of Teardrop attacks detected by firewall.
> Invalid IP Option Length | Total number of Invalid IP Option Length attacks detected by firewall.
> IP Source-router Attacks | Total number of IP Source-router attacks detected by firewall.
> Packets with IP-Unaligned-Timestamp | Total number of packets with IP unaligned timestamps detected by firewall.
> Packets with Short IP Header Length | Total number of packets with short IP header length detected by firewall.
> Packets Dropped due to IP Checksum Errors | Total number of packets dropped due to IP Checksum error.
> Downlink Dropped Bytes on IP Reassembly Failure | Total number of downlink bytes dropped on IP Reassembly failure.
> Uplink Dropped Bytes on IP Reassembly Failure | Total number of uplink bytes dropped on IP Reassembly failure.
> TCP Stats:
> Data Packets Received After RST/FIN | Total number of data packets received after receiving RST (reset) request by the firewall.
> Invalid SEQ Number Received with RST | Total number of invalid sequence-number received with RST (reset) request by the firewall.
> Data without Connection Established | Total number of data packets received before the establishment of connection by the firewall.
> Invalid TCP Connection Requests | Total number of invalid TCP connection requests received by the firewall.
> Invalid TCP pre-connection Requests | Total number of invalid TCP pre-connection requests received by firewall.
> Invalid ACK Value (Cookie Enabled) | Total number of invalid ACK values (to enable cookies) received by firewall.
> Invalid TCP Packet Length | Total number of TCP packets with invalid length received by firewall.
> Packets with Short TCP Header Length | Total number of TCP packets with invalid/short header length received by firewall.
> Packets Dropped due to TCP Checksum Errors | Total number of packets dropped due to TCP Checksum error.
> Packets with SEQ/ACK Out-of-range | Total number of packets with out of range SEQ/ACK.
> TCP Null Scan Attacks | Total number of TCP Null Scan attacks detected by firewall.
> Post Connection SYN | Total number of Post Connection SYN attacks detected by firewall.
> Unable to Send SYN Packet | Total number of attempts detected by the firewall when node failed to send SYN packets.
> Send Final ACK to Target Failed | Total number of attempts detected by the firewall when node failed to send Final ACK packet to target node.
> Invalid TCP Packet: SYN-ACK Expected | Total number of invalid TCP packets received by the firewall in place of SYN+ACK packets.
> No TCP Flags Set | Total number of TCP packets received with no flags set.
> All TCP Flags Set | Total number of TCP flags received with all flags set.
> Invalid TCP Packets | Total number of invalid TCP packets including all type of errors and attacks received by the firewall.
> Flows Closed by RST before 3-Way Handshake | Total number flows closed by RST (reset) message before the 3-way handshaking.
> Flows Timed-out in SYN_RCVD1 State | Total number of flows timed out in SYN_RCVD1 state.
> Flows Timed-out in SYN_RCVD2 State | Total number of flows timed out in SYN_RCVD2 state.
> Flows Terminated due to WinNuke Attack | Total number of flows terminated due to WinNuke attacks by the firewall.
> TCP-SYN Flood Attacks | Total number of TCP-SYN Flood attacks detected by firewall.
> Packets Dropped on TCP-SYN Flood Attack | Total number of packets dropped by the firewall in TCP-SYN Flood attacks.
> FTP-Bounce Attacks | Total number of FTP-Bounce attacks detected by the firewall.
> Mime-Flood Attacks | Total number of Mime-Flood attacks detected by the firewall.
> Proxy Handshakes Completed | Total number of times proxy handshake was completed.
> Packets Dropped during Proxy Handshake | Total number of packets dropped during proxy handshake.
> UDP Stats:
> Invalid UDP Echo Response | Total number of invalid UDP echo responses.
> Invalid UDP Packet Length | Total number of invalid UDP packet length.
> Packets Dropped due to UDP Checksum Errors | Total number of packets dropped due to UDP Checksum errors.
> Packets with Short UDP Header Length | Total number of packets with short UDP header length.
> Packets Dropped on UDP Flood Attack | Total number of packets dropped by the firewall in UDP flood attacks.
> Packets Dropped due to exceeding ICMP dest unreachable threshold | Total number of packets dropped due to exceeding ICMP destination unreachable threshold.
> ICMP Stats:
> Invalid ICMP Response | Total number of invalid ICMP responses.
> ICMP Reply Error | Total number of ICMP reply errors.
> Invalid ICMP Type Packet | Total number of invalid ICMP type packets.
> ICMP Error Message Replay Attacks | Total number of ICMP error message replay attacks detected by the firewall.
> ICMP Packets with Duplicate Sequence Number | Total number of ICMP packets with duplicate sequence numbers.
> Packets with Short ICMP Header Length | Total number of packets with short ICMP header length.
> Invalid ICMP Packet Length | Total number of packets with invalid ICMP packet length.
> Packets Dropped on ICMP Flood Attack | Total number of packets dropped by the firewall in ICMP flood attacks.
> Ping Of Death Attacks | Total number of Ping-of-Death attacks detected by the firewall.
> Packets Dropped due to ICMP Checksum Errors | Total number of packets dropped due to ICMP Checksum errors.
> ICMP Packets With Destination Unreachable Message | Total number of ICMP packets with Destination Unreachable Message.
> General Stats:
> Packets without Any Data Received | Total number of packets received without any data.
> No Matching Uplink Ruledef | Total number of uplink packets with no matching ruledef.
> No Matching Downlink Ruledef | Total number of downlink packets with no matching ruledef.
> Deny Ruledef Matched | Total number of times deny ruledef was matched.
> Packets Dropped due to No Ruledef in Rulebase | Total number of packets dropped due to no ruledef in rulebase.
> Packets Dropped due to Miscellaneous Errors | Total number of packets dropped due to miscellaneous errors.
> Flows Timed-out | Total number of flows that timed out.
> Flows Not Established from External Network | Total number of flows from external networks that were not established.
> Max Flows Limit Reached | Total number of times the maximum flows limit was reached.
> IP Retransmitted Packets Dropped | Total number of IP retransmitted packets dropped.
> Data Stats:
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall statistics username <user_name> verbose
> show active-charging firewall statistics username <user_name> verbose Command Output Descriptions

> Field | Description
> Firewall Statistics for Username: <user_name>
> IP Stats:
> Land Attacks | Total number of Land attacks detected by firewall.
> Jolt Attacks | Total number of Jolt attacks detected by firewall.
> Teardrop Attacks | Total number of Teardrop attacks detected by firewall.
> Invalid IP Option Length | Total number of Invalid IP Option Length attacks detected by firewall.
> IP Source-router Attacks | Total number of IP Source-router attacks detected by firewall.
> Packets with IP-Unaligned-Timestamp | Total number of packets with IP unaligned timestamps detected by firewall.
> Packets with Short IP Header Length | Total number of packets with short IP header length detected by firewall.
> Packets Dropped due to IP Checksum Errors | Total number of packets dropped due to IP Checksum error.
> Downlink Dropped Bytes on IP Reassembly Failure | Total number of downlink bytes dropped on IP Reassembly failure.
> Uplink Dropped Bytes on IP Reassembly Failure | Total number of uplink bytes dropped on IP Reassembly failure.
> TCP Stats:
> Data Packets Received After RST/FIN | Total number of data packets received after receiving RST (reset) request by the firewall.
> Invalid SEQ Number Received with RST | Total number of invalid sequence-number received with RST (reset) request by the firewall.
> Data without Connection Established | Total number of data packets received before the establishment of connection by the firewall.
> Invalid TCP Connection Requests | Total number of invalid TCP connection requests received by the firewall.
> Invalid TCP pre-connection Requests | Total number of invalid TCP pre-connection requests received by firewall.
> Invalid ACK Value (Cookie Enabled) | Total number of invalid ACK values (to enable cookies) received by firewall.
> Invalid TCP Packet Length | Total number of TCP packets with invalid length received by firewall.
> Packets with Short TCP Header Length | Total number of TCP packets with invalid/short header length received by firewall.
> Packets Dropped due to TCP Checksum Errors | Total number of packets dropped due to TCP Checksum error.
> Packets with SEQ/ACK Out-of-range | Total number of packets with out of range SEQ/ACK.
> TCP Null Scan Attacks | Total number of TCP Null Scan attacks detected by firewall.
> Post Connection SYN | Total number of Post Connection SYN attacks detected by firewall.
> Unable to Send SYN Packet | Total number of attempts detected by the firewall when node failed to send SYN packets.
> Send Final ACK to Target Failed | Total number of attempts detected by the firewall when node failed to send Final ACK packet to target node.
> Invalid TCP Packet: SYN-ACK Expected | Total number of invalid TCP packets received by the firewall in place of SYN+ACK packets.
> No TCP Flags Set | Total number of TCP packets received with no flags set.
> All TCP Flags Set | Total number of TCP flags received with all flags set.
> Invalid TCP Packets | Total number of invalid TCP packets including all type of errors and attacks received by the firewall.
> Flows Closed by RST before 3-Way Handshake | Total number flows closed by RST (reset) message before the 3-way handshaking.
> Flows Timed-out in SYN_RCVD1 State | Total number of flows timed out in SYN_RCVD1 state.
> Flows Timed-out in SYN_RCVD2 State | Total number of flows timed out in SYN_RCVD2 state.
> Flows Terminated due to WinNuke Attack | Total number of flows terminated due to WinNuke attacks by the firewall.
> TCP-SYN Flood Attacks | Total number of TCP-SYN Flood attacks detected by firewall.
> Packets Dropped on TCP-SYN Flood Attack | Total number of packets dropped by the firewall in TCP-SYN Flood attacks.
> FTP-Bounce Attacks | Total number of FTP-Bounce attacks detected by the firewall.
> Mime-Flood Attacks | Total number of Mime-Flood attacks detected by the firewall.
> Proxy Handshakes Completed | Total number of times proxy handshake was completed.
> Packets Dropped during Proxy Handshake | Total number of packets dropped during proxy handshake.
> UDP Stats:
> Invalid UDP Echo Response | Total number of invalid UDP echo responses.
> Invalid UDP Packet Length | Total number of invalid UDP packet length.
> Packets Dropped due to UDP Checksum Errors | Total number of packets dropped due to UDP Checksum errors.
> Packets with Short UDP Header Length | Total number of packets with short UDP header length.
> Packets Dropped on UDP Flood Attack | Total number of packets dropped by the firewall in UDP flood attacks.
> Packets Dropped due to exceeding ICMP dest unreachable threshold | Total number of packets dropped due to exceeding ICMP destination unreachable threshold.
> ICMP Stats:
> Invalid ICMP Response | Total number of invalid ICMP responses.
> ICMP Reply Error | Total number of ICMP reply errors.
> Invalid ICMP Type Packet | Total number of invalid ICMP type packets.
> ICMP Error Message Replay Attacks | Total number of ICMP error message replay attacks detected by the firewall.
> ICMP Packets with Duplicate Sequence Number | Total number of ICMP packets with duplicate sequence numbers.
> Packets with Short ICMP Header Length | Total number of packets with short ICMP header length.
> Invalid ICMP Packet Length | Total number of packets with invalid ICMP packet length.
> Packets Dropped on ICMP Flood Attack | Total number of packets dropped by the firewall in ICMP flood attacks.
> Ping Of Death Attacks | Total number of Ping-of-Death attacks detected by the firewall.
> Packets Dropped due to ICMP Checksum Errors | Total number of packets dropped due to ICMP Checksum errors.
> ICMP Packets With Destination Unreachable Message | Total number of ICMP packets with Destination Unreachable Message.
> General Stats:
> Packets without Any Data Received | Total number of packets received without any data.
> No Matching Uplink Ruledef | Total number of uplink packets with no matching ruledef.
> No Matching Downlink Ruledef | Total number of downlink packets with no matching ruledef.
> Deny Ruledef Matched | Total number of times deny ruledef was matched.
> Packets Dropped due to No Ruledef in Rulebase | Total number of packets dropped due to no ruledef in rulebase.
> Packets Dropped due to Miscellaneous Errors | Total number of packets dropped due to miscellaneous errors.
> Flows Timed-out | Total number of flows that timed out.
> Flows Not Established from External Network | Total number of flows from external networks that were not established.
> Max Flows Limit Reached | Total number of times the maximum flows limit was reached.
> IP Retransmitted Packets Dropped | Total number of IP retransmitted packets dropped.
> Data Stats:
> Total Packets Received | Total number of packets received in uplink and downlink flows.
> Total Bytes Received | Total number of bytes received by the firewall.
> Total Packets Sent | Total number of packets sent by the firewall.
> Total Bytes Sent | Total number of bytes sent by the firewall.
> Total Packets Injected | Total number of packets injected by the firewall.
> Total Bytes Injected | Total number of bytes injected by the firewall.
> Uplink Packets Dropped | Total number of packets in uplink flow dropped by the firewall.
> Uplink Bytes Dropped | Total number of bytes in uplink flow dropped by the firewall.
> Downlink Packets Dropped | Total number of packets in downlink flow dropped by the firewall.
> Downlink Bytes Dropped | Total number of bytes in downlink flow dropped by the firewall.
> Total Malformed Packets | Total number of malformed packets detected by the firewall.
> Total DOS Attacks | Total number of Denial-of-Service attacks detected by the firewall.
> Total Flows Processed by Firewall | Total number of flows processed by the firewall.

> ‌
> show active-charging firewall track-list attacking-servers
> show active-charging firewall track-list attacking-servers Command Output Descriptions

> Field | Description
> Attacking Servers:
> Server IP address | IP address of server being tracked for involvement in Denial-of-Service (DOS) attacks.
> Time of last attack | Date and time of last attack from the server.
> Time of first attack | Date and time of first attack from the server.
> Total attacks | Total number of attacks from the server.
> Last Attack Type | The last DOS attack type from the server.
> Total attacking servers found | Total number of attacking servers found.

> ‌
> show active-charging fw-and-nat policy name
> show active-charging fw-and-nat policy name Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | Name of the Active Charging Service.
> Firewall Policy Name | Name of the Firewall-and-NAT Policy.
> Firewall Status | Indicates whether Stateful Firewall is enabled or disabled in the Firewall-and-NAT policy.
> NAT Status | Indicates whether NAT is enabled or disabled in the Firewall-and-NAT policy.
> Firewall and NAT Action Priorities
> Ruledef Name | Name of the access ruledef.
> Type | Indicates the ruledef type.
> • | FD: Firewall Dynamic Ruledef — Predefined and disabled rules that can be enabled/disabled by the policy server.
> • | FS: Firewall Static Ruledef — Predefined and enabled rules that cannot be modified by the policy server.
> • | FSDP: Firewall Static & Dynamic Ruledef —Predefined and enabled rules that can be enabled/disabled by the policy server.
> Priority | Priority of the access ruledef in the Firewall-and-NAT policy.
> Charging-action | The charging action configured with the access ruledef.
> Port-trigger aux-ports:direction | The auxiliary ports open for traffic, and the direction from which the auxiliary connection is initiated.
> NAT Realm | Name of the NAT realm.
> Firewall Configuration
> Dos-Protection
> Source-Route | Indicates status of protection against IP Source Route IP Option attacks.
> Win-Nuke | Indicates status of protection against Win Nuke attacks.
> Mime-Flood | Indicates status of protection against MIME Flood attacks.
> FTP-Bounce | Indicates status of protection against FTP Bounce attacks.
> IP-Unaligned-Timestamp | Indicates status of protection against IP Unaligned Timestamp attacks.
> TCP-Window-Containment | Indicates status of protection against TCP Window Containment.
> Teardrop | Indicates status of protection against Teardrop attacks.
> UDP Flooding | Indicates status of protection against UDP Flooding attacks.
> ICMP Flooding | Indicates status of protection against ICMP Flooding attacks.
> SYN Flooding | Indicates status of protection against SYN Flooding attacks.
> Port Scan | Indicates status of protection against Port Scan attacks.
> Max-Packet-Size
> ICMP | For ICMP protocol, the maximum IP packet size (after IP reassembly) allowed over firewall.
> Non-ICMP | For non-ICMP protocol, the maximum IP packet size (after IP reassembly) allowed over firewall.
> Flooding
> ICMP limit | The maximum number of ICMP packets allowed during a sampling interval.
> UDP limit | The maximum number of UDP packets allowed during a sampling interval.
> TCP-SYN limit | The maximum number of TCP-SYN packets allowed during a sampling interval.
> Sampling Interval | The flooding sampling interval, in seconds.
> TCP-SYN Flood Intercept
> Mode | The TCP SYN flood intercept mode.
> • | none
> • | intercept
> • | watch
> Watch-timeout | The TCP intercept watch timeout, in seconds.
> Mime-Flood Params
> HTTP Header-Limit | The maximum number of headers allowed in an HTTP packet.
> HTTP Max-Header-Field-Size | The maximum header field size allowed in an HTTP header, in bytes.
> No Firewall Ruledef Match Action
> Uplink Action | Action configured for uplink packets with no access ruledef matches.
> Uplink Charging-Action | Charging action configured for uplink packets with no access ruledef matches.
> Downlink Action | Action configured for downlink packets with no access ruledef matches.
> Downlink Charging-Action | Charging action configured for downlink packets with no access ruledef matches.
> ICMP Dest-Unreachable Threshold | Indicates whether a threshold limit is set on the number of ICMP error messages sent by the subscriber for a particular data flow.
> ICMP Dest-Unreachable Threshold Value | The threshold value set for the number of ICMP error messages sent by the subscriber for a particular data flow.
> Action upon receiving TCP SYN packet with ECN/CWR Flag set | Indicates the action to be taken on receiving a TCP SYN packet with ECN/CWR Flag set.
> Action upon receiving a malformed packet | Indicates the action to be taken on receiving a malformed packet.
> Action upon IP Reassembly Failure | Indicates the action to be taken on IP reassembly failure.
> Action upon receiving an IP packet with invalid Options | Indicates the action to be taken on receiving an IP packet with invalid options.
> Action upon receiving an TCP packet with invalid Options | Indicates the action to be taken on receiving a TCP packet with invalid options.
> Action upon receiving an ICMP packet with invalid Checksum | Indicates the action to be taken on receiving an ICMP packet with invalid checksum.
> Action upon receiving a TCP packet with invalid Checksum | Indicates the action to be taken on receiving a TCP packet with invalid checksum.
> Action upon receiving an UDP packet with invalid Checksum | Indicates the action to be taken on receiving a UDP packet with invalid checksum.
> TCP Stateful Checks | Indicates whether stateful checks for TCP is enabled or disabled.
> First Packet Non-SYN Action | Indicates the action to be taken on flows with first packet Non-SYN.
> ICMP Stateful Checks | Indicates whether Stateful checks for ICMP is enabled or disabled.
> NAT Configuration
> NBR Format | Displats the NAT Binding Record format.
> Private IP NPU Flow Timeout | The time period for private IP NPU Flow, in seconds.
> Suppress sending NAT bind update to AAA | Indicates if the NAT bind update sent to AAA is suppressed or not.

> ‌
> show active-charging flows full
> For a TCP flow.
> show active-charging flows full Command Output Descriptions

> Command Output DescriptionsField | Description
> Flow-ID | Identifier for Flows.
> Session-ID | Identifier for Active Charging session.
> Uplink Packets | Total number of packets uplinked.
> Uplink Bytes | Total number of bytes uplinked.
> Downlink Packets | Total number of packets downlinked.
> Downlink Bytes | Total number of bytes downlinked.
> MS IP | The MS IP address.
> MS NAT IP | The MS NAT IP address.
> Server IP | The server IP address.
> Transport Protocol | The transport protocol: TCP, UDP, ICMP
> Application Protocol | The application protocol.
> TCP MS Port | The TCP MS port number.
> TCP MS NAT Port | The TCP MS NAT port number. This field is not displayed for one-to-one NAT.
> TCP Server Port | The TCP server port number.
> TCP State | Indicates the TCP state.
> TCP Prev State | Indicates the previous TCP state.
> MS Window Size | The mobile window size.
> Server Window Size | The server window size.
> MS Retries | Total number of mobile subscriber retries.
> Server Retries | Total number of server retries.
> ITC Action Applied | Indicates the ITC action applied.
> Buffering Statistics:
> Buffered Uplink Packets | Total buffered uplink packets.
> Buffered Uplink Bytes | Total buffered uplink bytes.
> Buffered Downlink Packets | Total buffered downlink packets.
> Buffered Downlink Bytes | Total buffered downlink bytes.
> Uplink Packets in Buffer | Total uplink packets in the buffer.
> Uplink Bytes in Buffer | Total uplink bytes in the buffer.
> Downlink Packets in Buffer | Total downlink packets in the buffer.
> Downlink Bytes in Buffer | Total downlink bytes in the buffer.
> Buff Over-limit Uplink Pkts | Total number of uplink packets that are over the limit in the buffer.
> Buff Over-limit Uplink Bytes | Total number of uplink bytes that are over the limit in the buffer.
> Buff Over-limit Downlink Pkts | Total number of downlink packets that are over the limit in the buffer.
> Buff Over-limit Downlink Bytes | Total number of downlink bytes that are over the limit in the buffer.

> ‌
> show active-charging flows full type p2p
> show active-charging flows full type p2p Command Output Descriptions

> Field | Description
> Flow-ID | Identifier for Flows.
> Session-ID | Identifier for Active Charging session with P2P.
> Uplink Packets | Total packets uplinked .
> Downlink Packets | Total packets downlinked.
> Uplink Bytes | Total bytes uplinked .
> Downlink Bytes | Total bytes downlinked.
> Transport Protocol | The protocol used for data transport.
> Application Protocol | The type of application protocol used for this session.
> UDP Client Port | UDP port on client communication.
> UDP Server Port | UDP port on server for communication.
> ITC Action Applied | Status of intelligent traffic control (ITC) on this session traffic.

> ‌
> show active-charging flows type p2p
> show active-charging flows type p2p Command Output Descriptions

> Field | Description
> Flow-ID | Identifier for Flows.
> Session-ID | Identifier for Active Charging session with P2P.
> Flow-num | Identifies the flow number.
> Application Protocol (VV) | The protocol used for application. Supported application protocols are:
> • | HT- HTTP
> • | HS - HTTPS
> • | SM - SMTP
> • | P3 - POP3
> • | WT - WTP
> • | WS - WSP
> • | DN - DNS
> • | RT - RTP
> • | EM - EMAIL
> • | MM - MMS
> • | FT - FTP
> • | SI - SIP
> • | WW - WWW
> • | RS - RTSP
> • | IM - IMAP
> • | P2 - P2P
> • | WC - WSP Connection Oriented
> • | WX - WSP Connection-less
> • | XX - Unknown
> Transport Protocol (v) | The protocol used for data transport. Supported data transport protocols are:
> • | T - TCP
> • | U - UDP
> • | I - ICMP
> • | X - Unknown
> Bytes-Up | Total bytes uplinked .
> Bytes-Down | Total bytes downlinked.
> Packets-Up | Total packets uplinked .
> Packets-Down | Total packets downlinked.
> Uplink Bytes | Total bytes uplinked .
> Downlink Bytes | Total bytes downlinked.
> Transport Protocol | The protocol used for data transport.
> Application Protocol | The type of application protocol used for this session.
> UDP Client Port | UDP port on client communication.
> UDP Server Port | UDP port on server for communication.
> ITC Action Applied | Status of intelligent traffic control (ITC) on this session traffic.

> ‌
> show active-charging group-of-ruledefs name
> show active-charging group-of-ruledefs name Command Output Descriptions

> Field | Description
> Service Name | The service in which the specified group-of-ruledefs is configured.
> Group-of-Ruledefs Name | Name of the group-of-ruledefs.
> Ruledef Name | Names of the ruledefs added to the group-of-ruledefs.
> Priority | The priorities configured for each of the ruledefs in the group-of-ruledefs.
> Total group(s)-of-ruledefs found | The total number of group(s)-of-ruledefs matching the specified criteria.

> ‌
> show active-charging nat statistics
> show active-charging nat statistics Command Output Descriptions

> Field | Description
> NAT Realm Utilization:
> Realm Name | Name of the NAT realm.
> Context | Context in which the NAT realm is configured.
> Current IP Address-In-Use | The number of IP addresses from the NAT realm currently in use.
> Total IP Address | The total number of IP addresses for the NAT realm.
> Current Calls Using-Realm | The number of current calls using the NAT realm.
> Current Port-Chunks Available | The number of port chunks currently available.
> Current Port-Chunks-In-Use | The number of port chunks currently in use.
> Total Port-Chunks | The total number of port chunks for the NAT realm.
> Port-Chunk Size | The size of the port chunks.
> Statistics:
> Total AAA alloc msgs sent | The total number of AAA allocation messages sent.
> Total AAA dealloc msgs sent | The total number of AAA deallocation messages sent.
> Total flows denied IP | The total number of subscriber flows that were denied NAT IP address.
> Total flows denied port | The total number of subscriber flows that were denied a port.
> Total bytes Transferred | The total number of bytes transferred.
> Total flows processed | The total number of flows processed.
> Average TCP port usage | The average TCP port usage in the allocated TCP ports, i.e out of allocated TCP ports how many got used.
> Average UDP port usage | The average UDP port usage in the allocated UDP ports, i.e out of allocated UDP ports how many got used.
> Average Others port usage | The average Others (ICMP or GRE) port usage in the allocated others ports, i.e out of allocated ‘Others’ ports how many got used.
> Port-Chunks distribution
> Max no.of chunks used | The maximum number of port chunks used.
> Total no.of subscribers | Total number of subscribers using maximum number of port chunks.
> Current no.of subscribers | Total number of current subscribers using maximum number of port chunks.
> Total Realms | The total number of NAT realms found.

> ‌
> show active-charging p2p-dynamic-rules verbose
> show active-charging p2p-dynamic-rules verbose Command Output Descriptions

> Field | Description
> Version | The signature file’s version number.
> Description | Description of the signature file.
> Sessions | Number of subscribers using the signature file.
> Status | Indicates whether the signature file is active or inactive.
> Rule Count | Total number of rules in the signature file.
> Protocol | Number of protocols for which rules are available.
> Hooks | Number of hooks instrumented in the signature file. For debugging purpose.
> Flow Spec | Number of flow descriptions across all hooks. For debugging purpose.
> Stage | Number of stages. For debugging purpose.
> Rules | Number of rules. For debugging purpose.

> ‌
> show active-charging rulebase name
> show active-charging rulebase name Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | Name of the Active Charging Service.
> Rule Base Name | Name of the rulebase.
> Charging Action Priorities
> Name | Name of the charging ruledef / group-of-ruledefs.
> Type | The ruledef / group-of-ruledefs type.
> • | RD: Dynamic ruledef
> • | RS: Static ruledef
> • | RSD: Static and dynamic ruledef
> • | GD: Dynamic group-of-ruledefs
> • | GS: Static group-of-ruledefs
> • | GSD: Static and dynamic group-of-ruledefs
> Priority | Priority of the ruledef / group-of-ruledefs in the rulebase.
> Charging-action | The charging action configured with the ruledef / group-of-ruledefs.
> Timedef | The time definition configured with the ruledef / group-of-ruledefs.
> Description | Description of the charging ruledef / group-of-ruledefs configuration.
> Post-processing Action Priorities
> Name | Name of the Post-processing ruledef.
> Type | The Post-processing ruledef type.
> Priority | Priority of the Post-processing ruledef in the rulebase.
> Charging-action | The charging action configured.
> Description | Description of the Post-processing ruledef configuration.
> Routing Action Priorities
> Ruledef Name | Name of the routing action ruledef.
> Priority | Priority of the routing action ruledef in the rulebase.
> Analyzer | Name of the applicable analyzer to routing action ruledef.
> Description | Description of the routing ruledef configuration.
> Firewall Action Priorities
> Ruledef Name | Name of the Firewall ruledef.
> Type | Indicates the Firewall ruledef type.
> • | FD: Firewall Dynamic Ruledef—Predefined and disabled firewall rules that can be enabled/disabled by the policy server.
> • | FS: Firewall Static Ruledef—Predefined and enabled firewall rules that cannot be modified by the policy server.
> • | FSDP: Firewall Static & Dynamic Ruledef—Predefined and enabled firewall rules that can be disabled/enabled by the policy server.
> Priority | Priority of the firewall ruledef in the rulebase.
> Charging-action | The charging action configured.
> Port-trigger aux-ports:direction | The auxiliary ports open for traffic, and the direction from which the auxiliary connection is initiated.
> EGCDR Fields
> Tariff Time thresholds (min:hrs) | Threshold for tariff in minutes and hours.
> Internal Threshold | Internal threshold to generate eG-CDRs in seconds.
> Uplink Octets | Total number of octets uplinked.
> Downlink Octets | Total number of octets downlinked.
> Total Octets | Total number of octets uplinked and downlinked.
> Time Based Metering | Status of time based metering.
> Content Filtering Group | Status of Content Filtering Server Group support for offline content filtering server (ICAP) support.
> Content Filtering Flow Any Error | Indicates whether Content Filtering packets are allowed/discarded in case of ACS error scenarios. This field is displayed only if either the Content Filtering mode or, ICAP server-group is configured.
> Content Filtering Policy | The Content Filtering policy.
> Content Filtering Mode | Indicates the Content Filtering mode.
> • | Static
> • | Static-and-dynamic
> URL-Blacklisting Action | Indicates action to be taken on URL Blacklisting match.
> UDR Fields
> Tariff Time thresholds (min:hrs) | Threshold for tariff in minutes and hours.
> Internal Threshold | Internal threshold to generate UDRs in seconds.
> Uplink Octets | Total number of octets uplinked.
> Downlink Octets | Total number of octets downlinked.
> Total Octets | Total number of octets uplinked and downlinked.
> CCA Fields | Information regarding Credit Control Application for prepaid charging.
> RADIUS charging context | Name of the RADIUS charging context.
> RADIUS Charging Group | Name of RADIUS Charging Server Group.
> RADIUS interim interval | Interim interval for RADIUS charging generation.
> DIAMETER Requested Service Unit | Information regarding requested service unit for prepaid charging through Diameter.
> Uplink Octets | Total number of octets uplinked in Diameter charging.
> Downlink Octets | Total number of octets downlinked in Diameter charging.
> Total Octets | Total number of octets uplinked and downlinked in Diameter charging.
> Quota Retry Time | Duration set to retry for prepaid credit limit.
> Quota Holding Time (QHT) | Status of quota holding time configuration.
> Quota Time Duration Algorithms | Applicable algorithm for quota time duration.
> Flow End Condition | Status of flow end condition configuration.
> Handoff | Indicates whether EDRs are generated for handoffs.
> Timeout | Indicates whether EDRs are generated for timeouts.
> Normal-end-signaling | Indicates whether EDRs are generated for normal end signaling.
> Session-end | Indicates whether EDRs are generated for session ends.
> Hagr | Indicates whether EDRs are generated for HAGR.
> Content-Filtering | Indicates whether EDRs are generated for Content Filtering.
> edr-format | The EDR format name.
> Flow Any Error Charging Action | Indicates the charging action configured for accounting action on packets dropped by Firewall due to any error. If disabled, no accounting is performed on such packets.
> Billing Records | Status of billing record generation.
> Limit For Total Flows | Status of flow limit setting across all applications.
> Limit For TCP Flows | Status of TCP flow limit setting.
> Limit For Non-TCP Flows | Status of non-TCP flow limit setting.
> Charging Rule Optimization | Type of optimization rule setting for charging.
> Firewall Configuration
> Dos-Protection
> Source-Route | Indicates status of protection against IP Source Route IP Option attacks.
> Win-Nuke | Indicates status of protection against Win Nuke attacks.
> Mime-Flood | Indicates status of protection against MIME Flood attacks.
> FTP-Bounce | Indicates status of protection against FTP Bounce attacks.
> IP-Unaligned-Timestamp | Indicates status of protection against IP Unaligned Timestamp attacks.
> Seq-Number-Prediction | Indicates status of protection against Sequence Number Prediction attacks.
> TCP-Window-Containment | Indicates status of protection against TCP Window Containment.
> Teardrop | Indicates status of protection against Teardrop attacks.
> UDP Flooding | Indicates status of protection against UDP Flooding attacks.
> ICMP Flooding | Indicates status of protection against ICMP Flooding attacks.
> SYN Flooding | Indicates status of protection against SYN Flooding attacks.
> Port Scan | Indicates status of protection against Port Scan attacks.
> Max-Packet-Size
> ICMP | For ICMP protocol, the maximum IP packet size (after IP reassembly) allowed over firewall.
> Non-ICMP | For non-ICMP protocol, the maximum IP packet size (after IP reassembly) allowed over firewall.
> Flooding
> ICMP limit | The maximum number of ICMP packets allowed during a sampling interval.
> UDP limit | The maximum number of UDP packets allowed during a sampling interval.
> TCP-SYN limit | The maximum number of TCP-SYN packets allowed during a sampling interval.
> Sampling Interval | The flooding sampling interval, in seconds.
> TCP-SYN Flood Intercept
> Mode | The TCP SYN flood intercept mode.
> • | none
> • | intercept
> • | watch
> Max-Attempts | The maximum number of attempts for sending proxy SYN to the target.
> Retrans-timeout | The SYN-Proxy retransmit timeout, in seconds.
> Watch-timeout | The TCP intercept watch timeout, in seconds.
> Mime-Flood Params
> HTTP Header-Limit | The maximum number of headers allowed in an HTTP packet.
> HTTP Max-Header-Field-Size | The maximum header field size allowed in an HTTP header, in bytes.
> No Firewall Ruledef Match Action
> Uplink Action | Action configured for uplink packets with no Firewall ruledef matches.
> Uplink Charging-Action | Charging action configured for uplink packets with no Firewall ruledef matches.
> Downlink Action | Action configured for downlink packets with no Firewall ruledef matches.
> Downlink Charging-Action | Charging action configured for downlink packets with no Firewall ruledef matches.
> ICMP Dest-Unreachable Threshold | Indicates whether a threshold limit is set on the number of ICMP error messages sent by the subscriber for a particular data flow.
> ICMP Dest-Unreachable Threshold Value | The threshold value set for the number of ICMP error messages sent by the subscriber for a particular data flow.
> QoS Renegotiation Timeout | The timeout setting for the Quality of Service (QoS) Renegotiation feature.
> EDR Suppress zero byte records | Indicates whether EDR suppression of zero byte records is enabled.
> EDR Timestamp Rounding | Type of timestamp rounding set for Event Detail Records.
> EGCDR Timestamp Rounding | Type of timestamp rounding set for eG-CDRs.
> RTP Dynamic Routing | Status of RTP dynamic routing configuration.
> Ignore port no. in application headers | Status of ignoring port numbers in application headers.
> Delayed Charging | Status of charging configuration to exclude initial handshaking TCP packets from charging.
> IP Reassembly-Timeout | IP reassembly timeout period in milliseconds.
> IP Reset ToS field | Status of IP Reset ToS field.
> TCP Out-of-Order-Timeout | TCP out-of-order timeout period in milliseconds.
> TCP 2MSL Timeout | TCP 2MSL timeout period in seconds.
> WTP Out-of-Order-Timeout | WTP out-of-order timeout period in milliseconds.
> TCP transmit-out-of-order-packets | Status of transmitting TCP out-of-order packets.
> Verify TCP checksum | Status of verifying TCP checksum errors.
> Verify UDP checksum | Status of verifying UDP checksum errors.
> P2P Dynamic Routing | Status of P2P dynamic routing.
> Total rulebase(s) found | Total number of rulebases matching the criteria.

> ‌
> show active-charging rulebase statistics
> show active-charging rulebase statistics Command Output Descriptions

> Command Output DescriptionsField | Description
> Service Name | Name of the Active Charging Service.
> Rulebase Name | Name of the rulebase.
> Uplink Pkts | Total number of packets uplinked.
> Uplink Bytes | Total number of bytes uplinked.
> Downlink Pkts | Total number of packets downlinked.
> Downlink Bytes | Total number of bytes downlinked.
> Readdressed Upl Pkts | Total number of readdressed uplinked packets.
> Readdressed Upl Bytes | Total number of readdressed uplinked bytes.
> Readdressed Dnl Pkts | Total number of readdressed downlinked packets.
> Readdressed Dnl Bytes | Total number of readdressed downlinked bytes.
> TCP MSS Inserted Pkts | Total number of TCP Maximum Segment Size (MSS) inserted packets.
> TCP MSS Limited Pkts | Total number of TCP MSS limited packets.
> ITC Terminated Flows | Total number of ITC terminated flows.
> Total PP Dropped Packets | Total number of packets dropped.
> Total PP Dropped Packet Bytes | Total number of bytes dropped.
> R7Gx Rule-Matching Failure Stats:
> Total Dropped Packets | Total number of packets dropped by R7Gx due to rule matching failure, for the rulebase.
> Total Dropped Packet Bytes | Total number of bytes dropped by R7Gx due to rule matching failure, for the rulebase.
> EDRs
> Total EDRs generated | Total number of EDRs generated.
> EDRs generated for handoff | Total number of EDRs generated for handoffs.
> EDRs generated for timeout | Total number of EDRs generated for timeouts.
> EDRs generated for normal-end-signaling | Total number of EDRs generated for normal end signalling.
> EDRs generated for session end | Total number of EDRs generated for session ending.
> EDRs generated for rule match | Total number of EDRs generated for rule matches.
> EDRs generated for hagr | Total number of EDRs generated for HAGR.
> EDRs generated for flow-end content-filtering | Total number of EDRs generated for flow-end content filtering.
> EDRs generated for content-filtering | Total number of EDRs generated for Category-based Content Filtering.
> EDRs generated for url-blacklisting | Total number of EDRs generated for URL Blacklisting.
> EDRs generated for any-error packets | Total number of EDRs generated for any-error packets.
> EDRs generated for firewall deny rule match | Total number of EDRs generated for firewall deny rule match.
> EDRs generated for transaction completion | Total number of EDRs generated for completion of transactions.
> EDRs generated for voip call end | Total number of EDRs generated on completion of voice calls.
> UDRs
> Total UDRs generated | Total number of UDRs generated.
> UDRs generated for handoff | Total number of UDRs generated for handoffs.
> UDRs generated for time limit | Total number of UDRs generated for time limits.
> UDRs generated for volume limit | Total number of UDRs generated for volume limits.
> UDRs generated for call end | Total number of UDRs generated for call endings.
> UDRs generated for hagr | Total number of UDRs generated for HAGR.
> GCDRs
> Total EGCDRs generated | Total number of eG-CDRs generated.
> GCDRs for Normal Release | Total number of G-CDRs generated for normal releases.
> GCDRs for Abnormal Release | Total number of G-CDRs generated for abnormal releases.
> GCDRs for Volume Limit | Total number of G-CDRs generated for volume limits.
> GCDRs for Time Limit | Total number of G-CDRs generated for time limits.
> GCDRs for SGSN Change | Total number of G-CDRs generated for SGSN change.
> GCDRs for Max Change Cond | Total number of G-CDRs generated for maximum change condition.
> GCDRs for Mgmt Intervention | Total number of G-CDRs generated for management interventions.
> GCDRs for RAT Change | Total number of G-CDRs generated for RAT changes.
> GCDRs for MS Timezone Change | Total number of G-CDRs generated for MS timezone changes.
> GCDRs for SGSN PLMN ID Change | Total number of G-CDRs generated for SGSN PLMN ID changes.
> PGWCDRs for Normal Release | Total number of PGW-CDRs generated for normal releases.
> PGWCDRs for Abnormal Release | Total number of PGW-CDRs generated for abnormal releases.
> PGWCDRs for Volume Limit | Total number of PGW-CDRs generated for volume limits.
> PGWCDRs for Time Limit | Total number of PGW-CDRs generated for time limits.
> PGWCDRs for ServingNode Change | Total number of PGW-CDRs generated for Serving Node change.
> PGWCDRs for Max Change Cond | Total number of PGW-CDRs generated for maximum change condition.
> PGWCDRs for Mgmt Intervention | Total number of PGW-CDRs generated for management interventions.
> PGWCDRs for RAT Change | Total number of PGW-CDRs generated for RAT changes.
> PGWCDRs for MS Timezone Change | Total number of PGW-CDRs generated for MS timezone changes.
> PGWCDRs for SGSN PLMN ID Change | Total number of PGW-CDRs generated for SGSN PLMN ID changes.
> NBRs | NAT Binding Record (NBR) statistics. These fields are displayed, only if configured, in StarOS 8.3 and later.
> Total NBRs generated | Total number of NBRs generated.
> NBRs generated for port chunk allocation | Total number of NBRs generated for port chunk allocation.
> NBRs generated for port chunk release | Total number of NBRs generated for port chunk release.
> Total rulebases matched | The total number of rulebases that matched the specified criteria.

> ‌
> show active-charging rulebase statistics name
> show active-charging rulebase statistics name Command Output Descriptions

> Field | Description
> Service Name | Name of the Active Charging Service.
> Rulebase Name | Name of the Active Charging Service rulebase.
> Uplink Pkts | Total number of packets uplinked.
> Uplink Bytes | Total number of bytes uplinked.
> Downlink Pkts | Total number of packets downlinked.
> Downlink Bytes | Total number of bytes downlinked.
> Readdressed Upl Pkts | Total number of readdressed uplink packets.
> Readdressed Upl Bytes | Total number of readdressed uplink bytes.
> Readdressed Dnl Pkts | Total number of readdressed downlink packets.
> Readdressed Dnl Bytes | Total number of readdressed downlink bytes.
> TCP MSS Inserted Pkts | Total number of Maximum Segment Size (MSS) inserted packets.
> TCP MSS Limited Pkts | Total number of MSS limited packets.
> ITC Terminated Flows | Total number of flows terminated by Intelligent Traffic Control service.
> Total PP Dropped Packets | Total number of packets dropped.
> Total PP Dropped Packet Bytes | Total number of bytes dropped.
> R7Gx Rule-Matching Failure Stats:
> Total Dropped Packets | Total number of packets dropped by R7Gx due to rule matching failure, for the rulebase.
> Total Dropped Packet Bytes | Total number of bytes dropped by R7Gx due to rule matching failure, for the rulebase.
> P2P random drop stats:
> Total Dropped Packets | Total number of packets dropped due to random drop to degrade voice quality.
> Total Dropped Packet Bytes | Total number of bytes dropped due to random drop to degrade voice quality.
> EDRs:
> Total EDRs generated | Total number of EDRs generated.
> EDRs generated for handoff | Total number of EDRs generated for handoffs.
> EDRs generated for timeout | Total number of EDRs generated for timeouts.
> EDRs generated for normal-end-signaling | Total number of EDRs generated for normal end signaling.
> EDRs generated for session end | Total number of EDRs generated for session ends.
> EDRs generated for rule match | Total number of EDRs generated for rule matches.
> EDRs generated for hagr | Total number of EDRs generated for HAGR.
> EDRs generated for flow-end content-filtering | Total number of EDRs generated for flow-end content filtering.
> EDRs generated for content-filtering | Total number of EDRs generated for content filtering.
> EDRs generated for any-error packets | Total number of EDRs generated for packets dropped by Firewall due to any error.
> EDRs generated for firewall deny rule match | Total number of EDRs generated for firewall deny rule matches.
> UDRs:
> Total UDRs generated | Total number of UDRs generated.
> UDRs generated for handoff | Total number of UDRs generated for handoffs.
> UDRs generated for time limit | Total number of UDRs generated for time limits.
> UDRs generated for volume limit | Total number of UDRs generated for volume limits.
> UDRs generated for call end | Total number of UDRs generated for call ends.
> UDRs generated for hagr | Total number of UDRs generated for HAGR.
> GCDRs:
> Total EGCDRs generated | Total number of eGCDRs generated.
> GCDRs for Normal Release | Total number of GCDRs generated for normal releases.
> GCDRs for Abnormal Release | Total number of GCDRs generated for abnormal releases.
> GCDRs for Volume Limit | Total number of GCDRs generated for volume limits.
> GCDRs for Time Limit | Total number of GCDRs generated for time limits.
> GCDRs for SGSN Change | Total number of GCDRs generated for SGSN changes.
> GCDRs for Max Change Cond | Total number of GCDRs generated for maximum change condition.
> GCDRs for Mgmt Intervention | Total number of GCDRs generated for management interventions.
> GCDRs for RAT Change | Total number of GCDRs generated for RAT changes.
> GCDRs for MS Timezone Change | Total number of GCDRs generated for MS timezone changes.
> GCDRs for SGSN PLMN ID Change | Total number of GCDRs generated for SGSN PLMN ID changes.
> Total rulebases matched | Total number of rulebases that matched the specified criteria.

> ‌
> show active-charging ruledef firewall
> show active-charging ruledef firewall Command Output Descriptions

> Field | Description
> Service Name | The service name.
> Ruledef Name | The rule definition name.
> tcp dst-port | The TCP destination port number.
> tcp src-port | The TCP source port number.
> udp dst-port | The UDP destination port number.
> udp src-port | The TCP source port number.
> ip any-match | Indicates whether the rule definition analyzes user traffic based on IP analyzed state—true/false.
> Rule Application Type | The rule application type—firewall.
> Create-log-record | Indicates whether logging is enabled or disabled.
> Total ruledef(s) configured | Total number of firewall rule definitions configured.

> ‌
> show active-charging ruledef statistics
> show active-charging ruledef statistics Command Output Descriptions

> Field | Description
> Total Charging Ruledefs | Total number of Charging rule definitions configured.
> Uplink Packets | Total number of packets received in uplink flow.
> Uplink Bytes | Total number of bytes received in uplink flow.
> Downlink Packets | Total number of packets received in downlink flow.
> Downlink Bytes | Total number of bytes received in downlink flow.
> Hits | Total number of events.
> Total Post-processing Ruledefs | Total number of Post-processing rule definitions configured.
> Uplink Packets | Total number of packets received in uplink flow.
> Uplink Bytes | Total number of bytes received in uplink flow.
> Downlink Packets | Total number of packets received in downlink flow.
> Downlink Bytes | Total number of bytes received in downlink flow.
> Hits | Total number of events.
> Total Firewall Ruledefs | Total number of Firewall rule definitions configured.
> Uplink Packets | Total number of packets received in uplink flow.
> Uplink Bytes | Total number of bytes received in uplink flow.
> Downlink Packets | Total number of packets received in downlink flow.
> Downlink Bytes | Total number of bytes received in downlink flow.
> Uplink Packets Dropped | Total number of packets dropped in uplink flow.
> Uplink Bytes Dropped | Total number of bytes dropped in uplink flow.
> Downlink Packets Dropped | Total number of packets dropped in downlink flow.
> Downlink Bytes Dropped | Total number of bytes dropped in downlink flow.
> Hits | Total number of events.

> ‌
> show active-charging ruledef statistics all firewall wide
> show active-charging ruledef statistics all firewall wide Command Output Descriptions

> Field | Description
> Ruledef Name | The Firewall ruledef name.
> Packets-Down | Total number of packets downlinked.
> Bytes-Down | Total number of bytes downlinked.
> Packets-Up | Total number of packets uplinked.
> Bytes-Up | Total number of bytes uplinked.
> Pkts-Drop-Dn | Total number of downlink packets dropped.
> Bytes-Drop-Dn | Total number of downlink bytes dropped.
> Pkts-Drop-Up | Total number of uplink packets dropped.
> Bytes-Drop-Up | Total number of uplink bytes dropped.
> Hits | Total number of events.
> Total Ruledef(s) | Total number of ruledefs.

> ‌
> show active-charging ruledef statistics all charging
> show active-charging ruledef statistics all charging Command Output Descriptions

> Field | Description
> Ruledef Name | The Charging rule definition name.
> Packets-Down | Total number of packets downlinked.
> Bytes-Down | Total number of bytes downlinked.
> Packets-Up | Total number of packets uplinked.
> Bytes-Up | Total number of bytes uplinked.
> Hits | Total number of events.
> Total Ruledef(s) | Total number of charging rule definitions.

> ‌
> show active-charging service all
> show active-charging service all Command Output Descriptions

> Command Output DescriptionsField | Description
> Service name | The Active Charging Service name.
> TCP Flow Idle Timeout | TCP flow idle timeout period, in seconds.
> UDP Flow Idle Timeout | UDP flow idle timeout period, in seconds.
> ICMP Flow Idle Timeout | ICMP flow idle timeout period, in seconds.
> ALG Media Idle Timeout | The configured ALG media idle timeout value, in seconds.
> Deep Packet Inspection | Indicates whether Deep Packet Inspection is enabled.
> Passive Mode | Indicates whether Passive Mode is enabled.
> CDR Flow Control | Indicates whether CDR Flow Control is enabled.
> Content Filtering | Indicates whether Category-based Content Filtering is enabled.
> Dynamic Content Filtering | Indicates whether Dynamic Content Filtering is enabled.
> URL-Blacklisting | Indicates whether URL Blacklisting is enabled.
> URL-Blacklisting Match-method | Indicates the URL Blacklisting method to look up URLs in the URL Blacklisting database.
> Content Filtering Match-method | Indicates the match method to look up URLs in the category-based content filtering database.
> Credit Control:
> Mode | Indicates the pre-paid charging application mode—Diameter or RADIUS.
> APN-name-to-be-included | Indicates the APN name to be sent in CCA messages.
> Failure-Handling | Indicates the failure handling behavior in the event of a communication failure with the pre-paid server.
> Trigger-Type | Indicates the credit control reauthorization trigger type.
> Diameter:
> Endpoint | The Diameter endpoint name.
> Endpoint-Realm | The Diameter endpoint realm.
> Dictionary | The Diameter dictionary used for Credit Control.
> Session-Failover | Indicates whether Session Failover is supported.
> Pending-Timeout | Indicates the pending timeout period, in seconds.
> Peer-Select:
> Peer | Indicates the peer name.
> Realm | Indicates the realm for the peer.
> Secondary-Peer | Indicates the secondary peer.
> Realm | Indicates the realm for the secondary peer.
> IMSI-Based Start-Value | To select the peer based on the International Mobile Subscriber Identification (IMSI) number, specifies the start of range in integer value of IMSI.
> IMSI-Based End-Value | Specifies the end of range in integer value of IMSI.
> Quota
> Request-Trigger | Indicates the trigger action on packets on crossing the threshold limit of subscriber quota in the pre-paid credit control service.
> Holding-Time | Indicates the Quota Holding Time (QHT).
> Validity-Time | Indicates the validity lifetime of the quota in seconds.
> Time-Threshold | Indicates the time threshold for pre-paid credit control quota.
> Units-Threshold | Indicates the units threshold for DCCA quota in percentage.
> Volume-Threshold | Indicates the volume threshold for pre-paid credit control quota.
> Pending-Traffic-Treatment
> Trigger | Indicates the trigger status.
> Forced-Reauth | Indicates status of the Diameter credit control pending traffic treatment for forced reauthorization.
> No-Quota | Indicates status of the Diameter credit control pending traffic treatment quota.
> Quota-Exhausted | Indicates status of the Diameter credit control pending traffic treatment for exhausted quota.
> Validity-Expired | Indicates status of the Diameter credit control pending traffic treatment for validity.

> ‌
> show active-charging sessions firewall required
> show active-charging sessions firewall required Command Output Descriptions

> Field | Description
> SESSIONID | Active charging session ID.
> CALLID | Call identification.
> IMSI/MSID | International Mobile Subscriber Identification/Mobile Station ID.
> IP | IP address of client.
> USERNAME | Name of the subscriber.
> Total acs sessions matching specified criteria | Total number of ACS sessions with firewall enabled.

> ‌
> show active-charging sessions full
> show active-charging session full Command Output Descriptions

> Field | Description
> Session-ID | The active charging session ID.
> Username | Name of the subscriber.
> Callid | Call identification.
> IMSI/MSID | Indicates the International Mobile Subscriber Identification/Mobile Station ID.
> ACSMgr Instance | Total instance of ACS Manager.
> ACSMgr Card/Cpu | Total number of ACS Manager Card/CPU.
> Client-IP | Indicates the IP address of Client.
> SessMgr Instance | Total instance of session manager.
> NAS-IP | Indicates the IP address of Network Access Server.
> NAS-PORT | Indicates the TCP port of Network Access Server.
> Access-NAS-IP(FA) | Indicates the IP address of accessed Network Access Server Foreign Agent (FA).
> NSAPI | Total instances of NS APIs used.
> Acct-Session-ID | Indicates the accounting session ID.
> NAS-ID | The Network Access Server identifier.
> Access-NAS-ID(FA) | Indicates the identifier of accessed Network Access Server Foreign Agent (FA).
> 3GPP2-BSID | Indicates the 3GPP2 base station identifier.
> Access-Correlation-ID(FA) | Indicates the access correlation ID for FA.
> 3GPP2-Correlation-ID | Indicates the Mobile IP Correlation ID.
> MEID | Indicates the Mobile equipment’s unique Mobile Equipment IDentifier (MEID).
> Carrier-ID | Indicates the Carrier or service Id.
> ESN | Indicates the Electronic Serial Number (ESN) of mobile equipment.
> Uplink Bytes | Total bytes uploaded.
> Downlink Bytes | Total bytes downloaded.
> Uplink Packets | Total packets uploaded.
> Downlink Packets | Total packets downloaded.
> Injected Uplink Bytes | Total bytes injected to upload.
> Injected Downlink Bytes | Total bytes injected to download.
> Injected Uplink Packets | Total packets injected to upload.
> Injected Downlink Packets | Total packets injected to download.
> Buffered Uplink Packets | Total buffered packets for uplink.
> Buffered Downlink Packets | Total buffered packets for downlink.
> Buffered Uplink Bytes | Total buffered bytes for uplink.
> Buffered Downlink Bytes | Total buffered bytes for uplink.
> Uplink Packets in Buffer | Total number of uplink packets in the buffer.
> Uplink Bytes in Buffer | Total number of uplink bytes in the buffer.
> Downlink Packets in Buffer | Total number of downlink packets in the buffer.
> Downlink Bytes in Buffer | Total number of downlink bytes in the buffer.
> Buff Over-limit Uplink Pkts | Total number of uplink packets that were over the buffer limit.
> Buff Over-limit Uplink Bytes | Total number of uplink bytes that were over the buffer limit.
> Buff Over-limit Downlink Pkts | Total number of downlink packets that were over the buffer limit.
> Buff Over-limit Downlink Bytes | Total number of downlink bytes that were over the buffer limit.
> Processed Uplink Packets | Total packets processed for upload.
> Processed Downlink Packets | Total packets processed for download.
> Dropped Uplink Packets | Total packets dropped in uplink direction.
> Dropped Downlink Packets | Total packets dropped in downlink direction.
> Uplink Out of Order Packets | Total out of order packets in uplink direction.
> Downlink Out of Order Packets | Total out of order packets in downlink direction.
> ITC Terminated Flows | Total number of flows terminated by Intelligent Traffic Control service.
> ITC Redirected Flows | Total number of flows redirected by Intelligent Traffic Control service.
> ITC Dropped Packets | Total number of packets dropped by Intelligent Traffic Control service.
> ITC ToS Remarked Flows | Total number of flows marked with Type of Service (ToS) by Intelligent Traffic Control service.
> R7Gx Dropped Upl Packets | Total number of packets dropped by R7Gx in uplink direction.
> R7Gx Dropped Dnl Packets | Total number of packets dropped by R7Gx in downlink direction.
> R7Gx Dropped Upl Pkts RuleMatch Fail | Total number of packets dropped by R7Gx in uplink direction due to rulematch failure—no matching rule is found.
> R7Gx Dropped Upl Bytes RuleMatch Fail | Total number of bytes dropped by R7Gx in uplink direction due to rulematch failure.
> R7Gx Dropped Dnl Pkts RuleMatch Fail | Total number of packets dropped by R7Gx in downlink direction due to rulematch failure.
> R7Gx Dropped Dnl Bytes RuleMatch Fail | Total number of bytes dropped by R7Gx in downlink direction due to rulematch failure.
> CC Dropped Uplink Packets | Total number of packets dropped by credit control in uplink direction.
> CC Dropped Uplink Bytes | Total number of bytes dropped by credit control in uplink direction.
> CC Dropped Downlink Packets | Total number of packets dropped by credit control in downlink direction.
> CC Dropped Downlink Bytes | Total number of bytes dropped by credit control in downlink direction.
> Creation Time | Time display in UTC format.
> Last Pkt Time | Time of last packet created.
> Duration | Duration of session.
> Active Charging Service name | Name of the active charging service.
> Rule Base name | Name of the rulebase applied.
> Firewall Policy | Indicates whether firewall processing is required.
> CF Policy ID | The content filtering policy identifier applicable for subscriber.
> Dynamic Charging | Status of dynamic charging functionality.
> Dynamic Chrg Msg Received | Total number of messages received for dynamic charging.
> Rule Definitions Received | Total number of ruledefs received.
> Installs Received | Total number of “Charging-Rule-Install” messages received.
> Removes Received | Total number of “Charging-Rule-Remove” messages received.
> Installs Succeeded | Total number of charging rules installed successfully.
> Installs Failed | Total number of charging rules installation failed.
> Removes Succeeded | Total number of charging rules removed successfully.
> Removes Failed | Total number of charging rules removal failed.
> Uplink Dynamic Rule Packets | Total number of packets uplinked with dynamic rules.
> Uplink Dynamic Rule Bytes | Total number of bytes uplinked with dynamic rules.
> Downlink Dynamic Rule Packets | Total number of packets downlinked with dynamic rules.
> Downlink Dynamic Rule Bytes | Total number of bytes downlinked with dynamic rules.
> Credit-Control | Status of DCCA (on/off).
> Current IP Flows | Total number of current IP flows.
> Current ICMP Flows | Total number of current ICMP flows.
> Current TCP Flows | Total number of current TCP flows.
> Current UDP Flows | Total number of current UDP flows.
> Current HTTP Flows | Total number of current HTTP flows.
> Current HTTPS Flows | Total number of current HTTPS flows.
> Current FTP Flows | Total number of current FTP flows.
> Current POP3 Flows | Total number of current POP3 flows.
> Current SMTP Flows | Total number of current SMTP flows.
> Current SIP Flows | Total number of current SIP flows.
> Current RTSP Flows | Total number of current RTSP flows.
> Current RTP Flows | Total number of current RTP flows.
> Current RTCP Flows | Total number of current RTCP flows.
> Current IMAP Flows | Total number of current IMAP flows.
> Current WSP-CO Flows | Total number of current WSP-CO flows.
> Current WSP-CL Flows | Total number of current WSP-CL flows.
> Current MMS Flows | Total number of current MMS flows.
> Current DNS Flows | Total number of current DNS flows.
> Current P2P Flows | Total number of current P2P flows.
> Current UNKNOWN Flows | Total number of current UNKNOWN flows.
> Current TFTP Flows | Total number of current TFTP flows.
> Ruledef Name | The ACS ruledef name.
> Pkts-Down | Total number of packets downlinked.
> Bytes-Down | Total number of bytes downlinked.
> Pkts-Up | Total number of packets uplinked.
> Bytes-Up | Total number of bytes uplinked.
> Hits | Total number of packets handled in uplink and downlink directions.
> Firewall-Ruledef Name | The Firewall ruledef name.
> Pkts-Down | Total number of packets downlinked.
> Bytes-Down | Total number of bytes downlinked.
> Pkts-Up | Total number of packets uplinked.
> Bytes-Up | Total number of bytes uplinked.
> Hits | Total number of packets handled in uplink and downlink directions.
> Dynamic Charging Rule Name Statistics | Dynamic Charging rule name statistics.
> Dynamic Charging Rule Name Configured | Dynamic Charging rule name configured.
> Predefined Rules Enabled List | List of enabled predefined rules.
> Predefined Firewall Rules Enabled List | List of enabled predefined Firewall rules.
> NCQoS NRUPC Req Made | Total number of network-controlled QOS Network Requested Update PDP Context requests made.
> NCQoS NRSPCA Req Made | Total number of network-controlled QOS Network Requested Secondary PDP Context Activation requests made.
> NCQoS NRUPC Req Failed | Total number of network-controlled QOS Network Requested Update PDP Context requests failed.
> NCQoS NRSPCA Req Failed | Total number of network-controlled QOS Network Requested Secondary PDP Context Activation requests failed.
> NCQoS NRUPC Req Success | Total number of network-controlled QOS Network Requested Update PDP Context requests succeeded.
> NCQoS NRSPCA Req Success | Total number of network-controlled QOS Network Requested Secondary PDP Context Activation requests succeeded.
> Total acs sessions matching specified criteria | Total number of ACS sessions matching the specified criteria.

> ‌
> show active-charging sessions full all
> show active-charging sessions full all Command Output Descriptions

> Field | Description
> Session-ID | The active charging session ID.
> Username | Name of the subscriber.
> Callid | Call identification.
> IMSI/MSID | Indicates the International Mobile Subscriber Identification/Mobile Station ID.
> ACSMgr Instance | Total instance of ACS Manager.
> ACSMgr Card/Cpu | Total number of ACS Manager Card/CPU.
> Client-IP | Indicates the IP address of Client.
> SessMgr Instance | Total instance of session manager.
> NAS-IP | Indicates the IP address of Network Access Server.
> NAS-PORT | Indicates the TCP port of Network Access Server.
> Access-NAS-IP(FA) | Indicates the IP address of accessed Network Access Server Foreign Agent (FA).
> NSAPI | Total instances of NS APIs used.
> Acct-Session-ID | Indicates the accounting session Id.
> NAS-ID | The Network Access Server identifier.
> Access-NAS-ID(FA) | Indicates the identifier of accessed Network Access Server Foreign Agent (FA).
> 3GPP2-BSID | Indicates the 3GPP2 base station identifier.
> Access-Correlation-ID(FA) | Indicates the access correlation Id for FA.
> 3GPP2-Correlation-ID | Indicates the Mobile IP Correlation Id.
> MEID | Indicates the Mobile equipment’s unique Mobile Equipment IDentifier (MEID).
> Carrier-ID | Indicates the Carrier or service Id.
> ESN | Indicates the Electronic Serial Number (ESN) of mobile equipment.
> Uplink Bytes | Total bytes uploaded.
> Downlink Bytes | Total bytes downloaded.
> Uplink Packets | Total packets uploaded.
> Downlink Packets | Total packets downloaded.
> Injected Uplink Bytes | Total bytes injected to upload.
> Injected Downlink Bytes | Total bytes injected to download.
> Injected Uplink Packets | Total packets injected to upload.
> Injected Downlink Packets | Total packets injected to download.
> Buffered Uplink Packets | Total buffered packets for uplink.
> Buffered Downlink Packets | Total buffered packets for downlink.
> Buffered Uplink Bytes | Total buffered bytes for uplink.
> Buffered Downlink Bytes | Total buffered bytes for uplink.
> Uplink Packets in Buffer | Total number of uplink packets in the buffer.
> Uplink Bytes in Buffer | Total number of uplink bytes in the buffer.
> Downlink Packets in Buffer | Total number of downlink packets in the buffer.
> Downlink Bytes in Buffer | Total number of downlink bytes in the buffer.
> Buff Over-limit Uplink Pkts | Total number of uplink packets that were over the buffer limit.
> Buff Over-limit Uplink Bytes | Total number of uplink bytes that were over the buffer limit.
> Buff Over-limit Downlink Pkts | Total number of downlink packets that were over the buffer limit.
> Buff Over-limit Downlink Bytes | Total number of downlink bytes that were over the buffer limit.
> Processed Uplink Packets | Total packets processed for upload.
> Processed Downlink Packets | Total packets processed for download.
> Dropped Uplink Packets | Total packets dropped in uplink direction.
> Dropped Downlink Packets | Total packets dropped in downlink direction.
> Uplink Out of Order Packets | Total out of order packets in uplink direction.
> Downlink Out of Order Packets | Total out of order packets in downlink direction.
> ITC Terminated Flows | Total number of flows terminated by Intelligent Traffic Control service.
> ITC Redirected Flows | Total number of flows redirected by Intelligent Traffic Control service.
> ITC Dropped Packets | Total number of packets dropped by Intelligent Traffic Control service.
> ITC ToS Remarked Flows | Total number of flows marked with Type of Service (ToS) by Intelligent Traffic Control service.
> R7Gx Dropped Upl Packets | Total number of packets dropped by R7Gx in uplink direction.
> R7Gx Dropped Dnl Packets | Total number of packets dropped by R7Gx in downlink direction.
> R7Gx Dropped Upl Pkts RuleMatch Fail | Total number of packets dropped by R7Gx in uplink direction due to rulematch failure—no matching rule is found.
> R7Gx Dropped Upl Bytes RuleMatch Fail | Total number of bytes dropped by R7Gx in uplink direction due to rulematch failure.
> R7Gx Dropped Dnl Pkts RuleMatch Fail | Total number of packets dropped by R7Gx in downlink direction due to rulematch failure.
> R7Gx Dropped Dnl Bytes RuleMatch Fail | Total number of bytes dropped by R7Gx in downlink direction due to rulematch failure.
> CC Dropped Uplink Packets | Total number of packets dropped by credit control in uplink direction.
> CC Dropped Uplink Bytes | Total number of bytes dropped by credit control in uplink direction.
> CC Dropped Downlink Packets | Total number of packets dropped by credit control in downlink direction.
> CC Dropped Downlink Bytes | Total number of bytes dropped by credit control in downlink direction.
> Current Readdressed Sessions | Total number of current readdressed sessions.
> Total Readdressed Uplink Pkts | Total number of readdressed uplink packets.
> Total Readdressed Uplink Bytes | Total number of readdressed uplink bytes.
> Total Readdressed Downlink Pkts | Total number of readdressed downlink packets.
> Total Readdressed Downlink Bytes | Total number of readdressed downlink bytes.
> Creation Time | Time display in UTC format.
> Last Pkt Time | Time of last packet created.
> Duration | Duration of session.
> Active Charging Service name | Name of the Active Charging Service.
> Rule Base name | Name of the ACS rulebase applied.
> Firewall Policy | Indicates whether firewall processing is required.
> Bandwidth Policy | The ACS bandwidth policy applicable for subscriber.
> CF Policy ID | The content filtering policy identifier applicable for subscriber.
> Dynamic Charging | Status of dynamic charging functionality.
> Dynamic Chrg Msg Received | Total number of messages received for dynamic charging.
> Rule Definitions Received | Total number of ruledefs received.
> Installs Received | Total number of “Charging-Rule-Install” messages received.
> Removes Received | Total number of “Charging-Rule-Remove” messages received.
> Installs Succeeded | Total number of charging rules installed successfully.
> Installs Failed | Total number of charging rules installation failed.
> Removes Succeeded | Total number of charging rules removed successfully.
> Removes Failed | Total number of charging rules removal failed.
> Uplink Dynamic Rule Packets | Total number of packets uplinked with dynamic rules.
> Uplink Dynamic Rule Bytes | Total number of bytes uplinked with dynamic rules.
> Downlink Dynamic Rule Packets | Total number of packets downlinked with dynamic rules.
> Downlink Dynamic Rule Bytes | Total number of bytes downlinked with dynamic rules.
> Credit-Control | Status of DCCA (on/off).
> Current IP Flows | Total number of current IP flows.
> Current ICMP Flows | Total number of current ICMP flows.
> Current IPv6 Flows | Total number of current IPv6 flows.
> Current ICMPv6 Flows | Total number of current ICMPv6 flows.
> Current TCP Flows | Total number of current TCP flows.
> Current UDP Flows | Total number of current UDP flows.
> Current HTTP Flows | Total number of current HTTP flows.
> Current HTTPS Flows | Total number of current HTTPS flows.
> Current FTP Flows | Total number of current FTP flows.
> Current POP3 Flows | Total number of current POP3 flows.
> Current SMTP Flows | Total number of current SMTP flows.
> Current SIP Flows | Total number of current SIP flows.
> Current RTSP Flows | Total number of current RTSP flows.
> Current RTP Flows | Total number of current RTP flows.
> Current RTCP Flows | Total number of current RTCP flows.
> Current IMAP Flows | Total number of current IMAP flows.
> Current WSP-CO Flows | Total number of current WSP-CO flows.
> Current WSP-CL Flows | Total number of current WSP-CL flows.
> Current MMS Flows | Total number of current MMS flows.
> Current DNS Flows | Total number of current DNS flows.
> Current P2P Flows | Total number of current P2P flows.
> Current UNKNOWN Flows | Total number of current UNKNOWN flows.
> CF Packets Allowed | Total number of packets allowed after applying content filtering service.
> CF Packets Discarded without Responding | Total number of packets discarded without sending any response after applying content filtering service.
> CF Packets Discarded with Flow Redirection | Total number of packets discarded with traffic flow redirection after applying content filtering service.
> CF Packets Discarded with Flow Termination | Total number of packets discarded and traffic flow terminated after applying content filtering service.
> CF Packets Discarded with Flow Content Insertion | Total number of packets discarded and content inserted in response message after applying content filtering service.
> CF Static DB Look-ups | Total number of lookups in static rating database for content filtering service.
> CF Successful Cache Look-ups | Total number of lookups in cache memory for static rating of URLs and returned successful after applying content filtering service.
> Charging ruledef(s) matching the specified criteria | Charging ruledef(s) matching the specified criteria.
> Firewall ruledef(s) match the specified criteria | Firewall ruledef(s) matching the specified criteria.
> Dynamic Charging Rule Name Statistics | Dynamic Charging rule name statistics.
> Dynamic Charging Rule Name Configured | Dynamic Charging rule name configured.
> Total Dynamic Charging Rule Names | Total number of dynamic Charging rules.
> Total Dynamic Firewall Rule Names | Total number of dynamic Firewall rules.
> Predefined Rules Enabled List | List of enabled predefined rules.
> Predefined Firewall Rules Enabled List | List of enabled predefined Firewall rules.
> Total acs sessions matching specified criteria | Total number of ACS sessions matching the specified criteria.

> ‌
> show active-charging sessions summary
> show active-charging sessions summary Command Output Descriptions

> Field | Description
> Session-ID | The active charging session Id.
> Username | Name of the subscriber.
> Callid | Call identification.
> IMSI/MSID | Indicates the International Mobile Subscriber Identification / Mobile Station ID.
> ACSMgr Instance | Total instance of ACS Manager.
> ACSMgr Card/Cpu | Total number of ACS Manager Card/CPU.
> Client-IP | Indicates the IP address of Client.
> SessMgr Instance | Total instance of session manager.
> NAS-IP | Indicates the IP address of Network Access Server.
> NAS-PORT | Indicates the TCP port of Network Access Server.
> Access-NAS-IP(FA) | Indicates the IP address of accessed Network Access Server Foreign Agent (FA).
> Acct-Session-ID | Indicates the accounting session ID.
> 3GPP2-Correlation-ID | Indicates the Mobile IP Correlation ID.
> Access-Correlation-ID(FA) | Indicates the access correlation Id for FA.
> MEID | Indicates the Mobile equipment’s unique Mobile Equipment IDentifier (MEID).
> Carrier-ID | Indicates the Carrier or service Id.
> ESN | Indicates the Electronic Serial Number (ESN) of mobile equipment.
> Uplink Bytes | Total bytes uploaded.
> Downlink Bytes | Total bytes downloaded.
> Uplink Packets | Total packets uploaded.
> Downlink Packets | Total packets downloaded.
> Injected Uplink Bytes | Total bytes injected to upload.
> Injected Downlink Bytes | Total bytes injected to download.
> Injected Uplink Packets | Total packets injected to upload.
> Injected Downlink Packets | Total packets injected to download.
> Uplink Out of Order Packets | Total out of order packets in uplink direction.
> Downlink Out of Order Packets | Total out of order packets in downlink direction.
> Creation Time | Time display in UTC format.
> Last Pkt Time | Time of last packet created.
> Duration | Duration of session.
> Active Charging Service name | Name of the active charging service.
> Rule Base name | Name of the Rule base applied.
> Credit-Control | Status of DCCA (on/off).
> CC peer | Peer name of Credit control (CC).
> CC Failure Handling | Action to handle CC failure.
> CC Session Failover | Status of CC session failover.
> Rating-Group | ID of Rating group.
> State | Status of Rating group.
> Pending Update | Status update pending.
> Last CCA | Time of last Credit control application.
> Time Threshold | Threshold for CC.
> Quota | Quota assigned for pre-paid subscriber.
> Usage | Usage by subscriber.
> Ruledef Name | Name of the Ruledef.
> Pkts-Down | Total packets in downlink direction.
> Bytes-Down | Total byte in downlink direction.
> Pkts-Up | Total Packets in upward direction.
> Bytes-Up | Total bytes in upward direction.
> Hits | Total packets in upload and download direction.
> Current IP Sessions | Total number of current IP sessions.
> Current ICMP Sessions | Total number of current ICMP sessions.
> Current TCP Sessions | Total number of current TCP sessions.
> Current UDP Sessions | Total number of current UDP sessions.
> Current HTTP Sessions | Total number of current HTTP sessions.
> Current HTTPS Sessions | Total number of current HTTPS sessions.
> Current FTP Sessions | Total number of current FTP sessions.
> Current POP3 Sessions | Total number of current POP3 sessions.
> Current SMTP Sessions | Total number of current SMTP sessions.
> Current SIP Sessions | Total number of current SIP sessions.
> Current RTSP Sessions | Total number of current RTSP sessions.
> Current RTP Sessions | Total number of current RTP sessions.
> Current RTCP Sessions | Total number of current RTCP sessions.
> Current IMAP Sessions | Total number of current IMAP sessions.
> Current WSP-CO Sessions | Total number of current WSP-CO sessions.
> Current WSP-CL Sessions | Total number of current WSP-CL sessions.
> Current MMS Sessions | Total number of current MMS sessions.
> Current DNS Sessions | Total number of current DNS sessions.
> Current P2P Sessions | Total number of current P2P sessions.
> Current UNKNOWN Sessions | Total number of current UNKNOWN sessions.
> Current TFTP Sessions | Total number of current TFTP sessions.
> Current SKYPE Sessions | Total number of current SKYPE sessions.
> Current YAHOO Sessions | Total number of current YAHOO sessions.
> Current SKYPE voice Sessions | Total number of current SKYPE voice sessions.
> Current YAHOO voice Sessions | Total number of current YAHOO voice sessions.
> Current SKYPE non-voice Sessions | Total number of current SKYPE non-voice sessions.
> Current YAHOO non-voice Sessions | Total number of current YAHOO non-voice sessions.
> Current EDONKEY Sessions | Total number of current EDONKEY sessions.
> Current ORB Sessions | Total number of current ORB sessions.
> Current MSN Sessions | Total number of current MSN sessions.
> Current GNUTELLA Sessions | Total number of current GNUTELLA sessions.
> Current MSN voice Sessions | Total number of current MSN voice sessions.
> Current BITTORRENT Sessions | Total number of current BITTORRENT sessions.
> Current MSN non-voice Sessions | Total number of current MSN non-voice sessions.
> Current JABBER Sessions | Total number of current JABBER sessions.
> Current WINNY Sessions | Total number of current WINNY sessions.
> Current SLINGBOX Sessions | Total number of current SLINGBOX sessions.
> Current MANOLITO Sessions | Total number of current MANOLITO sessions.
> Current PANDO Sessions | Total number of current PANDO sessions.
> Current FILETOPIA Sessions | Total number of current FILETOPIA sessions.
> Current SOULSEEK Sessions | Total number of current SOULSEEK sessions.
> Current PPSTREAM Sessions | Total number of current PPSTREAM sessions.
> Current QQ Sessions | Total number of current QQ sessions.
> Current QQLIVE Sessions | Total number of current QQLIVE sessions.
> Current IMESH Sessions | Total number of current IMESH sessions.
> Current MUTE Sessions | Total number of current MUTE sessions.
> Current PPLIVE Sessions | Total number of current PPLIVE sessions.
> Current GADUGADU Sessions | Total number of current GADUGADU sessions.
> Current FEIDIAN Sessions | Total number of current FEIDIAN sessions.
> Current APPLEJUICE Sessions | Total number of current APPLEJUICE sessions.
> Current fasttrack Sessions | Total number of current Fasttrack sessions.
> Current ZATTOO Sessions | Total number of current ZATTOO sessions.
> Current SKINNY Sessions | Total number of current SKINNY sessions.
> Current SOPCAST Sessions | Total number of current SOPCAST sessions.
> Current DIRECTCONNECT Sessions | Total number of current DIRECTCONNECT sessions.
> Current ARES Sessions | Total number of current ARES sessions.
> Current OSCAR Sessions | Total number of current OSCAR sessions.
> Current POPO Sessions | Total number of current POPO sessions.
> Current IRC Sessions | Total number of current IRC sessions.
> Current STEAM Sessions | Total number of current STEAM sessions.
> Current DDLINK Sessions | Total number of current DDLINK sessions.
> Current HALFLIFE2 Sessions | Total number of current HALFLIFE2 sessions.
> Current HAMACHIVPN Sessions | Total number of current HAMACHIVPN sessions.
> Current TVANTS Sessions | Total number of current TVANTS sessions.
> Current TVUPLAYER Sessions | Total number of current TVUPLAYER sessions.
> Current UUSEE Sessions | Total number of current UUSEE sessions.
> Current VPNX Sessions | Total number of current VPNX sessions.
> Current VTUN Sessions | Total number of current VTUN sessions.
> Current WINMX Sessions | Total number of current WINMX sessions.
> Current WOFWARCRAFT Sessions | Total number of current WOFWARCRAFT sessions.
> Current XBOX Sessions | Total number of current XBOX sessions.
> Current FREENET Sessions | Total number of current FREENET sessions.
> Current AIMINI Sessions | Total number of current AIMINI sessions.
> Current BATTLEFIELD Sessions | Total number of current BATTLEFIELD sessions.
> Current OPENFT Sessions | Total number of current OPENFT sessions.
> Current QQGAME Sessions | Total number of current QQGAME sessions.
> Current QUAKE Sessions | Total number of current QUAKE sessions.
> Current SECONDLIFE Sessions | Total number of current SECONDLIFE sessions.
> Current ACTIVESYNC Sessions | Total number of current ACTIVESYNC sessions.
> Current NIMBUZZ Sessions | Total number of current NIMBUZZ sessions.
> Current IAX Sessions | Total number of current IAX sessions.
> Current PALTALK Sessions | Total number of current PALTALK sessions.
> Current WARCRAFT3 Sessions | Total number of current WARCRAFT3 sessions.
> Current IPTV Sessions | Total number of current IPTV sessions.
> Current RDP Sessions | Total number of current RDP sessions.
> Current PANDORA Sessions | Total number of current PANDORA sessions.

> ‌
> show active-charging sessions summary type p2p
> show active-charging sessions summary type p2p Command Output Descriptions

> Field | Description
> Total Active Charging Sessions | The total number of active charging sessions.
> Uplink Bytes | Total bytes uploaded.
> Downlink Bytes | Total bytes downloaded.
> Uplink Packets | Total packets uploaded.
> Downlink Packets | Total packets downloaded.
> Current IP Sessions | Total number of current IP sessions.
> Current ICMP Sessions | Total number of current ICMP sessions.
> Current TCP Sessions | Total number of current TCP sessions.
> Current UDP Sessions | Total number of current UDP sessions.
> Current HTTP Sessions | Total number of current HTTP sessions.
> Current HTTPS Sessions | Total number of current HTTPS sessions.
> Current FTP Sessions | Total number of current FTP sessions.
> Current POP3 Sessions | Total number of current POP3 sessions.
> Current SMTP Sessions | Total number of current SMTP sessions.
> Current SIP Sessions | Total number of current SIP sessions.
> Current RTSP Sessions | Total number of current RTSP sessions.
> Current RTP Sessions | Total number of current RTP sessions.
> Current RTCP Sessions | Total number of current RTCP sessions.
> Current IMAP Sessions | Total number of current IMAP sessions.
> Current WSP-CO Sessions | Total number of current WSP-CO sessions.
> Current WSP-CL Sessions | Total number of current WSP-CL sessions.
> Current MMS Sessions | Total number of current MMS sessions.
> Current DNS Sessions | Total number of current DNS sessions.
> Current P2P Sessions | Total number of current P2P sessions.
> Current UNKNOWN Sessions | Total number of current UNKNOWN sessions.
> Current SKYPE Sessions | Total number of current SKYPE sessions.
> Current YAHOO Sessions | Total number of current YAHOO sessions.
> Current SKYPE voice Sessions | Total number of current SKYPE voice sessions.
> Current YAHOO voice Sessions | Total number of current YAHOO voice sessions.
> Current SKYPE non-voice Sessions | Total number of current SKYPE non-voice sessions.
> Current YAHOO non-voice Sessions | Total number of current YAHOO non-voice sessions.
> Current EDONKEY Sessions | Total number of current EDONKEY sessions.
> Current ORB Sessions | Total number of current ORB sessions.
> Current MSN Sessions | Total number of current MSN sessions.
> Current GNUTELLA Sessions | Total number of current GNUTELLA sessions.
> Current MSN voice Sessions | Total number of current MSN voice sessions.
> Current BITTORRENT Sessions | Total number of current BITTORRENT sessions.
> Current MSN non-voice Sessions | Total number of current MSN non-voice sessions.
> Current JABBER Sessions | Total number of current JABBER sessions.
> Current WINNY Sessions | Total number of current WINNY sessions.
> Current SLINGBOX Sessions | Total number of current SLINGBOX sessions.
> Current MANOLITO Sessions | Total number of current MANOLITO sessions.
> Current PANDO Sessions | Total number of current PANDO sessions.
> Current FILETOPIA Sessions | Total number of current FILETOPIA sessions.
> Current SOULSEEK Sessions | Total number of current SOULSEEK sessions.
> Current PPSTREAM Sessions | Total number of current PPSTREAM sessions.
> Current QQ Sessions | Total number of current QQ sessions.
> Current QQLIVE Sessions | Total number of current QQLIVE sessions.
> Current IMESH Sessions | Total number of current IMESH sessions.
> Current MUTE Sessions | Total number of current MUTE sessions.
> Current PPLIVE Sessions | Total number of current PPLIVE sessions.
> Current GADUGADU Sessions | Total number of current GADUGADU sessions.
> Current FEIDIAN Sessions | Total number of current FEIDIAN sessions.
> Current APPLEJUICE Sessions | Total number of current APPLEJUICE sessions.
> Current fasttrack Sessions | Total number of current Fasttrack sessions.
> Current ZATTOO Sessions | Total number of current ZATTOO sessions.
> Current SKINNY Sessions | Total number of current SKINNY sessions.
> Current SOPCAST Sessions | Total number of current SOPCAST sessions.
> Current DIRECTCONNECT Sessions | Total number of current DIRECTCONNECT sessions.
> Current ARES Sessions | Total number of current ARES sessions.
> Current OSCAR Sessions | Total number of current OSCAR sessions.
> Current POPO Sessions | Total number of current POPO sessions.
> Current IRC Sessions | Total number of current IRC sessions.
> Current STEAM Sessions | Total number of current STEAM sessions.
> Current DDLINK Sessions | Total number of current DDLINK sessions.
> Current HALFLIFE2 Sessions | Total number of current HALFLIFE2 sessions.
> Current HAMACHIVPN Sessions | Total number of current HAMACHIVPN sessions.
> Current TVANTS Sessions | Total number of current TVANTS sessions.
> Current TVUPLAYER Sessions | Total number of current TVUPLAYER sessions.
> Current UUSEE Sessions | Total number of current UUSEE sessions.
> Current VPNX Sessions | Total number of current VPNX sessions.
> Current VTUN Sessions | Total number of current VTUN sessions.
> Current WINMX Sessions | Total number of current WINMX sessions.
> Current WOFWARCRAFT Sessions | Total number of current WOFWARCRAFT sessions.
> Current XBOX Sessions | Total number of current XBOX sessions.
> Current FREENET Sessions | Total number of current FREENET sessions.
> Current AIMINI Sessions | Total number of current AIMINI sessions.
> Current BATTLEFIELD Sessions | Total number of current BATTLEFIELD sessions.
> Current OPENFT Sessions | Total number of current OPENFT sessions.
> Current QQGAME Sessions | Total number of current QQGAME sessions.
> Current QUAKE Sessions | Total number of current QUAKE sessions.
> Current SECONDLIFE Sessions | Total number of current SECONDLIFE sessions.
> Current ACTIVESYNC Sessions | Total number of current ACTIVESYNC sessions.
> Current NIMBUZZ Sessions | Total number of current NIMBUZZ sessions.
> Current IAX Sessions | Total number of current IAX sessions.
> Current PALTALK Sessions | Total number of current PALTALK sessions.
> Current WARCRAFT3 Sessions | Total number of current WARCRAFT3 sessions.
> Current IPTV Sessions | Total number of current IPTV sessions.
> Current RDP Sessions | Total number of current RDP sessions.
> Current PANDORA Sessions | Total number of current PANDORA sessions.

> ‌
> show active-charging subsystem all
> show active-charging subsystem all Command Output Descriptions

> Command Output DescriptionsField | Description
> Total ACS Managers | Total number of Active Charging Service session managers running on the system.
> Session Creation Succ | Total number of sessions created successfully.
> Session Creation Fail | Total number of session creation failures.
> Total subscribers | Total number of subscribers configured on system.
> Current subscribers | Total number of subscriber active on system.
> Total CF subscribers | Total number of Content Filtering subscribers configured on the system.
> Current CF subscribers | Total number of Content Filtering subscribers active on the system.
> Total Flows Connected | Total number of flows connected.
> Total Flows Disconnected | Total number of flows disconnected.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total ICMP flows | Total number of ICMP flows.
> Current ICMP flows | Total number of current ICMP flows.
> Total TCP flows | Total number of TCP flows.
> Current TCP flows | Total number of current TCP flows.
> Total UDP flows | Total number of UDP flows.
> Current UDP flows | Total number of current UDP flows.
> Total DNS flows | Total number of DNS flows.
> Current DNS flows | Total number of current DNS flows.
> Total FTP flows | Total number of FTP flows.
> Current FTP flows | Total number of current FTP flows.
> Total HTTP flows | Total number of HTTP flows.
> Current HTTP flows | Total number of current HTTP flows.
> Total HTTPS flows | Total number of HTTPS flows.
> Current HTTPS flows | Total number of current HTTPS flows.
> Total POP3 flows | Total number of POP3 flows.
> Current POP3 flows | Total number of current POP3 flows.
> Total SMTP flows | Total number of SMTP flows.
> Current SMTP flows | Total number of current SMTP flows.
> Total SIP flows | Total number of SIP flows.
> Current SIP flows | Total number of current SIP flows.
> Total RTSP flows | Total number of RTSP flows.
> Current RTSP flows | Total number of current RTSP flows.
> Total RTP flows | Total number of RTP flows.
> Current RTP flows | Total number of current RTP flows.
> Total RTCP flows | Total number of RTCP flows.
> Current RTCP flows | Total number of current RTCP flows.
> Total IMAP flows | Total number of IMAP flows.
> Current IMAP flows | Total number of current IMAP flows.
> Total WSP-CO flows | Total number of WSP-CO flows.
> Current WSP-CO flows | Total number of current WSP-CO flows.
> Total WSP-CL flows | Total number of WSP-CL flows.
> Current WSP-CL flows | Total number of current WSP-CL flows.
> Total MMS flows | Total number of MMS flows.
> Current MMS flows | Total number of current MMS flows.
> Total TFTP flows | Total number of TFTP flows.
> Current TFTP flows | Total number of current TFTP flows.
> Total P2P flows | Total number of P2P flows.
> Current P2P flows | Total number of current P2P flows.
> Total P2P Voice flows | Total number of P2P voice flows.
> Current P2P Voice flows | Total number of current P2P voice flows.
> Total Rule-Hits | Total number of rule hits.
> Total P2P Sessions | Total number of P2P sessions formed from start.
> Total PP Rule-Hits | Total number of Post-processing rule hits.
> Total P2P Subscribers | Total number of P2P subscribers.
> Total Firewall Subscribers | Total number of Firewall subscribers.
> Total NAT Subscribers | Total number of Network Address Translation subscribers.
> Total Blacklisted URL hits | Total number of Blacklisted URL hits.
> Total Blacklisted URL misses | Total number of Blacklisted URL misses.
> Total Readdr flows | Total number of readdressed flows.
> Current Readdr flows | Current number of readdressed flows.
> Total URLs Outstanding for Rating (SRDB) | Total number of URLs outstanding for Static Rating Database rating.
> RADIUS Prepaid Statistics | Indicates the group of statistics for RADIUS prepaid session.
> Total prepaid sess | Total number of active/dormant/inactive prepaid sessions.
> Current prepaid sess | Total number of prepaid sessions currently active.
> Total prepaid auth req | Total number of AAA authorization requests for prepaid sessions.
> Total prepaid auth success | Total number of successful AAA authorization for prepaid sessions.
> Total prepaid auth fail | Total number of failed AAA authorization for prepaid sessions.
> Total prepaid errors | Total number of errors occurred in prepaid sessions.
> Content Filtering URL Cache Statistics | Indicates URL caching statistics for Content Filtering.
> Total cached entries | Total number of cached entries in memory.
> Total hits | Total number of attempts to access URLs which are cached in memory with rating.
> Total misses | Total number of attempts failed to access URLs which are cached in memory with rating.
> Total has-path hits | Total number of attempts to access URLs which are cached in memory with rating with specified path.
> Total flushes | total number of flushing of URL cache to clear memory with stale URL list and rating.
> Total URLs not cached | Total number of URLs accessed but not cached in memory.
> Total Cache size | Total cache size adding maximum cache size for all volume provided for URLs caching.
> Percentage Full | Indicates the percentage of memory used out of allocated space for URL caching.
> Last Flush request received Time | Indicates the time of last flush request received for cache flushing.
> Total Control Pkts Rx | Total number of control packets received.
> Total Control Pkts Tx | Total number of control packets transmitted.
> Data statistics | Statistics of data flow.
> Receive Pkts | Total number of packets received in different size based frequency
> Transmit pkts | Total number of packets transmitted in different size based frequency
> User Data statistics | Indicates the group of statistics of user data traffic.
> Data octets from User | Total number of bytes originated from user.
> Data packets from User | Total number of data packets originated from user.
> Data octets to User | Total number of bytes sent to user.
> Data packets to User | Total number of data packets sent to user.
> EDR/UDR statistics
> Records Generated | The total number of EDR/UDR records generated.
> Msgs sent to CDRMOD | The total number of EDR/UDR messages sent to CDRMOD.
> Records sent to CDRMOD | The total number of EDR/UDR records sent to CDRMOD.
> Msgs bounced from CDRMOD | The total number of EDR/UDR messages that were bounced from CDRMOD.
> Records bounced from CDRMOD | The total number of EDR/UDR records that were bounced from CDRMOD.
> Successful Msgs sent to CDRMOD | The total number of successful EDR/UDR messages that were sent to CDRMOD.
> Successful records sent to CDRMOD | The total number of successful EDR/UDR records that were sent to CDRMOD.

> ‌
> show active-charging subsystem facility acsmgr instance
> show active-charging subsystem facility acsmgr instance Command Output Descriptions

> Field | Description
> ACSMgr Instance | The ACS Manager instance.
> Card/CPU | The card and CPU ID.
> Session Creation Succ | Total number of sessions created successfully.
> Session Creation Fail | Total number of session creation failures.
> Total subscribers | Total number of subscribers configured on system.
> Current subscribers | Total number of subscriber active on system.
> Total CF subscribers | Total number of Content Filtering subscribers configured on the system.
> Current CF subscribers | Total number of Content Filtering subscribers active on the system.
> Total Flows Connected | Total number of flows connected.
> Total Flows Disconnected | Total number of flows disconnected.
> Total Uplink Pkts | Total number of packets uplinked.
> Total Uplink Bytes | Total number of bytes uplinked.
> Total Downlink Pkts | Total number of packets downlinked.
> Total Downlink Bytes | Total number of bytes downlinked.
> Total ICMP flows | Total number of ICMP flows.
> Current ICMP flows | Total number of current ICMP flows.
> Total TCP flows | Total number of TCP flows.
> Current TCP flows | Total number of current TCP flows.
> Total UDP flows | Total number of UDP flows.
> Current UDP flows | Total number of current UDP flows.
> Total DNS flows | Total number of DNS flows.
> Current DNS flows | Total number of current DNS flows.
> Total FTP flows | Total number of FTP flows.
> Current FTP flows | Total number of current FTP flows.
> Total HTTP flows | Total number of HTTP flows.
> Current HTTP flows | Total number of current HTTP flows.
> Total HTTPS flows | Total number of HTTPS flows.
> Current HTTPS flows | Total number of current HTTPS flows.
> Total POP3 flows | Total number of POP3 flows.
> Current POP3 flows | Total number of current POP3 flows.
> Total SMTP flows | Total number of SMTP flows.
> Current SMTP flows | Total number of current SMTP flows.
> Total SIP flows | Total number of SIP flows.
> Current SIP flows | Total number of current SIP flows.
> Total RTSP flows | Total number of RTSP flows.
> Current RTSP flows | Total number of current RTSP flows.
> Total RTP flows | Total number of RTP flows.
> Current RTP flows | Total number of current RTP flows.
> Total RTCP flows | Total number of RTCP flows.
> Current RTCP flows | Total number of current RTCP flows.
> Total IMAP flows | Total number of IMAP flows.
> Current IMAP flows | Total number of current IMAP flows.
> Total WSP-CO flows | Total number of WSP-CO flows.
> Current WSP-CO flows | Total number of current WSP-CO flows.
> Total WSP-CL flows | Total number of WSP-CL flows.
> Current WSP-CL flows | Total number of current WSP-CL flows.
> Total MMS flows | Total number of MMS flows.
> Current MMS flows | Total number of current MMS flows.
> Total P2P flows | Total number of P2P flows.
> Current P2P flows | Total number of current P2P flows.
> Total Rule-Hits | Total number of rule hits.
> Blacklisted URL hits | The number of Blacklisted URL hits.
> Blacklisted URL misses | The number of Blacklisted URL misses.
> Total URLs Outstanding for Rating (SRDB) | Total number of URLs outstanding for Static Rating Database rating.
> RADIUS Prepaid Statistics | Indicates the group of statistics for RADIUS prepaid session.
> Total prepaid sess | Total number of active/dormant/inactive prepaid sessions.
> Current prepaid sess | Total number of prepaid sessions currently active.
> Total prepaid auth req | Total number of AAA authorization requests for prepaid sessions.
> Total prepaid auth success | Total number of successful AAA authorization for prepaid sessions.
> Total prepaid auth fail | Total number of failed AAA authorization for prepaid sessions.
> Total prepaid errors | Total number of errors occurred in prepaid sessions.
> Content Filtering Policy <policy> for Service <service> Matched
> Content Filtering URL Cache Statistics | Indicates the group of statistics of URL caching for content filtering service.
> Total cached entries | Total number of cached entries in memory.
> Total hits | Total number of attempts to access URLs which are cached in memory with rating.
> Total misses | Total number of attempts failed to access URLs which are cached in memory with rating.
> Total has-path hits | Total number of attempts to access URLs which are cached in memory with rating with specified path.
> Total flushes | Total number of flushing of URL cache to clear memory with stale URL list and rating.
> Total Cache size (all volumes) | Total cache size adding maximum cache size for all volume provided for URLs caching.
> Percentage Full | Indicates the percentage of memory used out of allocated space for URL caching.
> Last Flush request received time | Indicates the time of last flush request received for cache flushing.
> Volume - <volume> | The volume.
> Cached entries | For the volume, indicates the total number of cached entries in memory.
> Hits | For the volume, indicates the total number of attempts failed to access URLs which are cached in memory with rating.
> Misses | For the volume, indicates the total number of attempts failed to access URLs which are cached in memory with rating.
> has-path hits | For the volume, indicates the total number of attempts to access URLs which are cached in memory with rating with specified path.
> Flushes | For the volume, indicates the total number of times the URL cache has been flushed to clear memory with stale URL list and rating.
> Percentage Full | For the volume, indicates the percentage of memory used out of allocated space for URL caching.
> Last Access Time | For the volume, indicates the last access time.
> Last Flush Time | For the volume, indicates the last flush time.
> Data statistics
> Receive Pkts | Total number of packets received.
> Transmit Pkts | Total number of packets transmitted.

> ‌
> show active-charging timedef all
> show active-charging udr-format all Command Output Descriptions

> Field | Description
> Service Name | Name of the Active Charging Service.
> Timedef Name | Name of the time definition.
> Start Day | Start day configured for each timeslot in the timedef. If the day is not configured, shows “Daily”.
> Start Time | Start time configured for each timeslot in the timedef.
> End Day | End day configured for each timeslot in the timedef. If the day is not configured, shows “Daily”.
> End Time | End time configured for each timeslot in the timedef.
> Total timedef(s) found | The total number of timedefs found.

> ‌
> show active-charging udr-format all
> show active-charging udr-format all Command Output Descriptions

> Field | Description
> Service Name | The name of the Active Charging Service.
> UDR Format Name | Name of the configured existing UDR format.
> Attribute | Attribute informations configured in specific UDR format.
> Total udr-format(s) found | The total number of the configured existing UDR formats.

> ‌
> show active-charging url-blacklisting statistics
> show active-charging url-blacklisting statistics Command Output Descriptions

> Field | Description
> Service name | Name of the Active Charging Service.
> Cumulative URL-Blacklisting Statistics
> Total Blacklisted URL hits | The total number of Blacklisted URL hits.
> Total Blacklisted URL misses | The total number of Blacklisted URL misses.

> ‌
> show active-charging url-blacklisting statistics rulebase name
> show active-charging url-blacklisting statistics rulebase name Command Output Descriptions

> Field | Description
> Service name | Name of the Active Charging Service.
> Rulebase name | Name of the rulebase.
> Blacklisted URL hits | The total number of Blacklisted URL hits.
> Blacklisted URL misses | The total number of Blacklisted URL misses.
> Total rulebases matched | The total number of rulebases matching the specified criteria.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883