> SGTP Schema Statistics
> The SGTP schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> SGTP Schema Statistics

> Statistics | Description | Data Type
> vpn-id | Identifier for the VPN context in which this SGTP service is running. | Int32
> vpn-name | Name of the VPN context in which this SGTP service is running. | String
> service-name | Name of the SGTP service for which this bulk statistics are collected. | String
> iups-service | Name of the corresponding Iu-PS interface service for this SGTP service. | String
> rnc-address | Address of the corresponding radio network controller (RNC) for this SGTP service. | String
> ggsn-address | Address of the corresponding GGSN node for this SGTP service. This statistic is obsoleted in release 9.0. | String
> sgtpc-total-cpc-req | Total GTP-C messages for create PDP context requests received. | Int32
> sgtpc-cpc-req-v1-pri | Total GTP-Cv1 messages for create primary PDP context requests received. | Int32
> sgtpc-cpc-req-v0-pri | Total GTP-Cv0 messages for create primary PDP context requests received. | Int32
> sgtpc-cpc-req-sec | Total GTP-C (v1 and v0) messages for create secondary PDP context requests received. | Int32
> sgtpc-cpc-req-accept | Total GTP-C (v1 and v0) messages for create PDP context requests accepted. | Int32
> sgtpc-cpc-req-denied | This statistics has been obsoleted | Int32
> sgtpc-cpc-rsp-v1-pri | Total GTP-Cv1 messages response sent for create primary PDP context requests. | Int32
> sgtpc-cpc-rsp-v0-pri | Total GTP-Cv0 messages response sent for create primary PDP context requests. | Int32
> sgtpc-cpc-rsp-sec | Total GTP (v1 and v0) message response for create secondary PDP context requests sent. | Int32
> sgtpc-total-upc-req | Total GTP-C (v1 and v0) messages for update PDP context requests received. | Int32
> sgtpc-upc-req-v1-tx | Total GTP-Cv1 message response for update PDP context requests sent. | Int32
> sgtpc-upc-req-v0-tx | Total GTP-Cv0 message response for update PDP context requests sent. | Int32
> sgtpc-upc-req-v1-rx | Total GTP-Cv1 messages for update PDP context requests received. | Int32
> sgtpc-upc-req-v0-rx | This statistics has been obsoleted. | Int32
> sgtpc-upc-req-accept-tx | Total GTP-C update PDP context request accept messages sent. | Int32
> sgtpc-upc-req-accept-rx | Total GTP-C update PDP context request accept messages received. | Int32
> sgtpc-upc-req-accept-v1-tx | Total GTP-C v1 update PDP context requests accept messages sent. | Int32
> sgtpc-upc-req-accept-v1-rx | Total GTP-Cv1 message response for update PDP context requests received. | Int32
> sgtpc-upc-req-accept-v0-rx | Total GTP-C v0 update PDP context requests accept messages received. | Int32
> sgtpc-upc-req-denied-tx | Total GTP-C (v1 and v0) update PDP context requests denied messages sent. | Int32
> sgtpc-upc-req-denied-rx | Total GTP-C (v1 and v0) update PDP context requests denied messages received. | Int32
> sgtpc-total-dpc-req | Total GTP-C (v1 and v0) messages for delete PDP context requests received. | Int32
> sgtpc-dpc-req-v1-tx | Total GTP-Cv1 message response for delete PDP context requests sent. | Int32
> sgtpc-dpc-req-v0-tx | Total GTP-Cv0 message response for delete PDP context requests sent. | Int32
> sgtpc-dpc-req-v1-rx | Total GTP-Cv1 messages for update PDP delete requests received. | Int32
> sgtpc-dpc-req-v0-rx | Total GTP-Cv0 message response for delete PDP context requests received. | Int32
> sgtpc-dpc-req-accept-tx | Total GTP-C delete PDP context request accept messages sent. | Int32
> sgtpc-dpc-req-accept-rx | Total GTP-C delete PDP context request accept messages received. | Int32
> sgtpc-dpc-req-accept-v1-tx | Total GTP-Cv1 delete PDP context requests accept messages sent. | Int32
> sgtpc-dpc-req-accept-v0-tx | Total GTP-Cv0 delete PDP context requests accept messages received. | Int32
> sgtpc-dpc-req-accept-v1-rx | Total GTP-Cv1 delete PDP context requests accept messages received. | Int32
> sgtpc-dpc-req-accept-v0-rx | Total GTP-Cv0 delete PDP context requests accept messages received. | sgtpc-dpc-req-accept-v1-rx
> sgtpc-dpc-req-denied-tx | Total GTP-C (v1 and v0) delete PDP context requests denied messages sent. | Int32
> sgtpc-dpc-req-denied-rx | Total GTP-C (v1 and v0) delete PDP context requests denied messages received. | Int32
> sgtpc-total-pdu-not-req | Total number of GTP-C (v1 and v0) PDUs not requested but received for primary PDP context. | Int32
> sgtpc-pdu-not-req-v1-pri | Total number of GTP-Cv1 PDUs not requested but received for primary PDP context. | Int32
> sgtpc-pdu-not-req-v0-pri | Total number of GTP-Cv0 PDUs not requested but received for primary PDP context. | Int32
> sgtpc-pdu-not-req-sec | Total number of GTP-C (v1 and v0) PDUs not requested but received for secondary PDP context. | Int32
> sgtpc-pdu-not-req-v1-pri-ret | Total number of GTP-Cv1 PDUs not requested but received for primary PDP context and retried. | Int32
> sgtpc-pdu-not-req-v0-pri-ret | Total number of GTP-Cv0 PDUs not requested but received for primary PDP context and retried | Int32
> sgtpc-pdu-not-req-sec-ret | Total number of GTP-C (v1 and v0) PDUs not requested but received for secondary PDP context retried. | Int32
> sgtpc-pdu-not-req-accept-v1 | Total number of GTP-Cv1 PDUs not requested but received for secondary PDP context and accepted. | Int32
> sgtpc-pdu-not-req-accept-v0 | Total number of GTP-Cv0 PDUs not requested but received for secondary PDP context accepted. | Int32
> sgtpc-pdu_not-req-denied | Total number of GTP-C (v1 and v0) PDUs not requested but received and denied. | Int32
> sgtpc-total-pdu-not-rej-req | Total number of GTP-C (v1 and v2) PDUs requested and not rejected. | Int32
> sgtpc-pdu-not-rej-req-v1-pri | Total number of GTP-Cv1 PDUs requested and not rejected for primary PDP context. | Int32
> sgtpc-pdu-not-rej-req-v0-pri | Total number of GTP-Cv0 PDUs requested and not rejected for primary PDP context. | Int32
> sgtpc-pdu-not-rej-req-v1-pri-ret | Total number of GTP-Cv1 PDUs requested and not rejected for primary PDP context but retransmitted. | Int32
> sgtpc-pdu-not-rej-req-v0-pri-ret | Total number of GTP-Cv0 PDUs not requested and not rejected for primary PDP context but retransmitted. | Int32
> sgtpc-pdu-not-rej-req-accept-v1 | Total number of GTP-Cv1 PDUs requested and not rejected for primary PDP context. | Int32
> sgtpc-pdu-not-rej-req-accept-v0 | Total number of GTP-Cv0 PDUs requested and not rejected for primary PDP context. | Int32
> sgtpc-pdu_not-rej-req-denied | Total number of PDU notification requests which were not accepted. | Int32
> sgtpc-total-sri-req | Total number of GTP-C (v1 and v0) Send Routing Information (SRI) request messages transmitted to the HLR(s). |
> sgtpc-sri-req-v1 | Total number of GTP-Cv1 Send Routing Information (SRI) request messages transmitted to the HLR(s). |
> sgtpc-sri-req-v0 | Total number of GTP-Cv0 Send Routing Information (SRI) request messages transmitted to the HLR(s). |
> sgtpc-sri-req-v1-ret | The total number of Total number of GTP-Cv1 Send Routing Information (SRI) request messages retransmitted to the HLR(s). |
> sgtpc-sri-req-v0-ret | Total number of GTP-Cv0 Send Routing Information (SRI) request messages retransmitted to the HLR(s). |
> sgtpc-sri-req-denied | Total number of GTP-C (v1 and v0) Send Routing Information (SRI) request messages transmitted to the HLR(s) and denied. |
> sgtpc-total-fail-rpt-req | Total number of GTP-C (v1 and v0) fail report messages requested. |
> sgtpc-fail-rpt-req-v1 | Total number of GTP-Cv1 fail report messages requested. |
> sgtpc-fail-rpt-req-v0 | Total number of GTP-Cv1 fail report messages requested. |
> sgtpc-fail-rpt-req-v1-ret | Total number of GTP-Cv1 fail report messages requested and retransmitted. |
> sgtpc-fail-rpt-req-v0-ret | Total number of GTP-Cv0 fail report messages requested and retransmitted. |
> sgtpc-fail-rpt-req-denied | Total number of GTP-Cv1 fail report messages requested and denied. |
> sgtpc-ident-req-v1-tx | Total GTP-C v1 identification request messages sent. | Int32
> sgtpc-ident-req-v0-tx | Total GTP-C v0 identification request messages sent. | Int32
> sgtpc-ident-req-v1-rx | Total GTP-C v1 identification request messages received. | Int32
> sgtpc-ident-req-v0-rx | Total GTP-C v0 identification request messages received. | Int32
> sgtpc-ident-req-accept-tx | Total GTP-C identification request accept messages sent. | Int32
> sgtpc-ident-req-accept-rx | Total GTP-C identification request accept messages received. | Int32
> sgtpc-ident-req-accept-v1-tx | Total GTP-Cv1 identification request accept messages sent. | Int32
> sgtpc-ident-req-accept-v0-tx | Total GTP-Cv0 identification request accept messages sent. | Int32
> sgtpc-ident-req-accept-v1-rx | Total GTP-Cv1 identification request accept messages received. | Int32
> sgtpc-ident-req-accept-v0-rx | Total GTP-Cv0 identification request accept messages received. | Int32
> sgtpc-ident-req-denied-tx | Total GTP-C (v1 and v0) identification request denied messages sent. | Int32
> sgtpc-ident-req-denied-rx | Total GTP-C (v1 and v0) identification request denied messages received. | Int32
> sgtpc-sgsn-ctxt-req-v1-tx | Total GTP-Cv1 SGSN context request messages sent. | Int32
> sgtpc-sgsn-ctxt-req-v0-tx | Total GTP-Cv0 SGSN context request messages sent. | Int32
> sgtpc-sgsn-ctxt-req-v1-rx | Total GTP-Cv1 SGSN context request messages received. | Int32
> sgtpc-sgsn-ctxt-req-v0-rx | Total GTP-Cv0 SGSN context request messages received. | Int32
> sgtpc-sgsn-ctxt-req-accept-tx | Total GTP-C SGSN context request accept messages sent. | Int32
> sgtpc-sgsn-ctxt-req-accept-rx | Total GTP-C SGSN context request accept messages received. | Int32
> sgtpc-sgsn-ctxt-req-accept-v1-tx | Total GTP-Cv1 SGSN context request accept messages sent. | Int32
> sgtpc-sgsn-ctxt-req-accept-v0-tx | Total GTP-Cv0 SGSN context request accept messages sent. | Int32
> sgtpc-sgsn-ctxt-req-accept-v1-rx | Total GTP-Cv1 SGSN context request accept messages received. | Int32
> sgtpc-sgsn-ctxt-req-accept-v0-rx | Total GTP-Cv0 SGSN context request accept messages received. | Int32
> sgtpc-sgsn-ctxt-req-denied-tx | Total GTP-C (v1 and v0) SGSN context request denied messages sent. | Int32
> sgtpc-sgsn-ctxt-req-denied-rx | Total GTP-C (v1 and v0) SGSN context request denied messages received. | Int32
> sgtpc-sgsn-ctxt-ack-accept-tx | Total GTP-C SGSN context acknowledgement accept messages sent. | Int32
> sgtpc-sgsn-ctxt-ack-accept-ex | Total GTP-C SGSN context acknowledgement accept messages sent. | Int32
> sgtpc-sgsn-ctxt-ack-accept-v1-tx | Total GTP-Cv1 SGSN context request accept acknowledge messages sent. | Int32
> sgtpc-sgsn-ctxt-ack-accept-v0-tx | Total GTP-Cv0 SGSN context request accept acknowledge messages sent. | Int32
> sgtpc-sgsn-ctxt-ack-accept-v1_rx | Total GTP-Cv1 SGSN context request accept acknowledge messages received. | Int32
> sgtpc-sgsn-ctxt-ack-accept-v0_rx | Total GTP-Cv0 SGSN context request accept acknowledge messages received. | Int32
> sgtpc-sgsn-ctxt-ack-denied-tx | Total GTP-C (v1 and v0) SGSN context request denial acknowledge messages sent. | Int32
> sgtpc-sgsn-ctxt-ack-denied-rx | Total GTP-C (v1 and v0) SGSN context request denial acknowledge messages received. | Int32
> sgtpc-fwd-reloc-req-tx | Total GTP-C (v1 and v0) forward relocation request messages sent. | Int32
> sgtpc-fwd-reloc-req-rx | Total GTP-C (v1 and v0) forward relocation request messages received. | Int32
> sgtpc-fwd-reloc-discard-tx | This statistics has been obsoleted. | Int32
> sgtpc-fwd-reloc-req-accept-tx | Total GTP-C (v1 and v0) forward relocation request accept response messages sent. | Int32
> sgtpc-fwd-reloc-req-accept-rx | Total GTP-C (v1 and v0) forward relocation request accept response messages received. | Int32
> sgtpc-fwd-reloc-denied-tx | Total GTP-C (v1 and v0) forward relocation request denied response messages sent. | Int32
> sgtpc-fwd-reloc-denied-rx | Total GTP-C (v1 and v0) forward relocation request denied response messages received. | Int32
> sgtpc-fwd-srnsctxt-req-tx | Total GTP-C (v1 and v0) forward relocation request messages with serving radio network subsystem (SRNS) context request sent. | Int32
> sgtpc-fwd-srnsctxt-req-rx | Total GTP-C (v1 and v0) forward relocation request messages with SRNS context request received. | Int32
> sgtpc-fwd-srnsctxt-discard-rx | This statistics has been obsoleted. | Int32
> sgtpc-fwd-srnsctxt-ack-tx | Total GTP-C (v1 and v0) forward relocation request messages with SRNS context request acknowledge sent. | Int32
> sgtpc-fwd-srnsctxt-ack-rx | Total GTP-C (v1 and v0) forward relocation request messages with SRNS context request acknowledge received. | Int32
> sgtpc-fwd-srnsctxt-ack-denied-tx | Total GTP-C (v1 and v0) forward relocation request messages with SRNS context request denied sent. | Int32
> sgtpc-fwd-srnsctxt-ack-denied-rx | Total GTP-C (v1 and v0) forward relocation request messages with SRNS context request denied received. | Int32
> sgtpc-fwd-reloc-compl-tx | Total GTP-C (v1 and v0) forward relocation request messages with procedure complete message sent. | Int32
> sgtpc-fwd-reloc-compl-rx | Total GTP-C (v1 and v0) forward relocation request messages with procedure complete message received. | Int32
> sgtpc-fwd-rel-compl-ack-accept-tx | Total GTP-C (v1 and v0) forward relocation request messages for procedure complete acknowledge sent. | Int32
> sgtpc-fwd-rel-compl-ack-accept-rx | Total GTP-C (v1 and v0) forward relocation request messages for procedure complete acknowledge received. | Int32
> sgtpc-fwd-rel-compl-ack-denied-tx | Total GTP-C (v1 and v0) forward relocation request messages for procedure complete sent with ACK denial. | Int32
> sgtpc-fwd-rel-compl-ack-denied-rx | Total GTP-C (v1 and v0) forward relocation request messages for procedure complete received with ACK denial. | Int32
> sgtpc-reloc-cncl-req-tx | Total GTP-C (v1 and v0) messages sent with relocation cancel request. | Int32
> sgtpc-reloc-cncl-req-rx | Total GTP-C (v1 and v0) message response received for relocation cancel request. | Int32
> sgtpc-reloc-cncl-req-accept-tx | Total GTP-C (v1 and v0) messages sent with acceptance for relocation cancel request. | Int32
> sgtpc-reloc-cncl-req-accept-rx | Total GTP-C (v1 and v0) message response received with acceptance for relocation cancel request. | Int32
> sgtpc-reloc-cncl-denied-tx | Total GTP-C (v1 and v0) messages sent with denial for relocation cancel request. | Int32
> sgtpc-reloc-cncl-denied-rx | Total GTP-C (v1 and v0) message response with received with denial for relocation cancel request. | Int32
> sgtpc-paket-discarded | Total GTP-C (v1 and v0) packets discarded. | Int32
> sgtpc-v1-echo-req-tx | Total GTP-C v1 echo request messages sent. | Int32
> sgtpc-v0-echo-req-tx | Total GTP-C v1 echo request messages sent. | Int32
> sgtpc-v1-retrnas-echo-req-tx | Total GTP-C v1 echo request messages retransmited. | Int32
> sgtpc-v0-retrnas-echo-req-tx | Total GTP-C v0 echo request messages retransmited. | Int32
> sgtpc-v1-echo-req-rx | Total GTP-C v1 echo request messages received. | Int32
> sgtpc-v0-echo-req-rx | Total GTP-C v0 echo request messages received. | Int32
> sgtpc-ret-v1-echo-req-rx | Total GTP-C v1 echo request retransmitted messages received. | Int32
> sgtpc-ret-v0-echo-req-rx | Total GTP-C v0 echo request retransmitted messages received. | Int32
> sgtpc-v1-echo-rsp-tx | Total GTP-C v1 echo response messages sent. | Int32
> sgtpc-v0-echo-rsp-tx | Total GTP-C v0 echo response messages sent. | Int32
> sgtpc-v1-echo-rsp-rx | Total GTP-C v1 echo response messages received. | Int32
> sgtpc-v0-echo-rsp-rx | Total GTP-C v0 echo response messages received. | Int32
> sgtpc-ver-not-supported-rx | Total GTP-C messages of not supported version of GTP received. | Int32
> sgtpc-ver-not-supported-tx | Total GTP-C messages of not supported version of GTP messages sent. | Int32
> sgtpc-supp-extn-hdr-notif-rx | Total GTP messages with supported extension headers notification received. | Int32
> sgtpc-supp-extn-hdr-notif-tx | Total GTP messages with supported extension headers notification sent. | Int32
> sgtpu-ggsn-pkt-sent | Total packets for GTP-U messages sent to GGSN. | Int64
> sgtpu-ggsn-byts-sent | Description: Total number of GTP-U messages bytes sent to GGSN at a given instance of time. Triggers: Gauge changes every time an uplink packet is sent to the GGSN. Availability: Across all SGTP services, per SGTP service, per GGSN Type: Counter | Int64
> sgtpu-rnc-pkt-sent | Total packets for GTP-U messages sent to RNC. | Int64
> sgtpu-rnc-byts-sent | Description: Total number of bytes for GTP-U messages sent to the RNC at a given instance in time. Triggers: Gauge changes every time a downlink packet is sent to the RNC. Availability: Across all SGTP services, per SGTP service, per RNC Type: Counter | Int64
> sgtpu-sgsn-pkt-sent | Total packets for GTP-U messages sent to SGSN. | Int64
> sgtpu-sgsn-byts-sent | Description: Total number of GTP-U message bytes sent to the peer SGSN at a given instance of time. Triggers: Gauge changes every time a packet is sent to a “new” SGSN during an Inter SGSN handoff. Availability: Across all SGTP services, per SGTP service Type: Counter | Int64
> sgtpu-ggsn-pkt-rcvd | Total packets for GTP-U messages received from GGSN. | Int64
> sgtpu-ggsn-byts-rcvd | Description: Total number of GTP-U message bytes received from the GGSN at a given instance of time. Triggers: Gauge changes every time a downlink packet is received from the GGSN. Availability: Across all SGTP services, per SGTP service, per GGSN Type: Counter | Int64
> sgtpu-ggsn-pkt-queued | Total packets queued for GTP-U messages from GGSN. | Int64
> sgtpu-ggsn-byts-queued | Total bytes queued for GTP-U messages from GGSN. | Int64
> sgtpu-ggsn-pkt-forwarded | Description: This proprietary counter indicates the total number of packets that are forwarded from the GGSN queue. Triggers: Increments when a packet is forwarded from the GGSN queue. Availability: Per SGTP service Type: Counter | Int64
> sgtpu-ggsn-byts-forwarded | Description: This proprietary counter indicates the total number of bytes that are forwarded from the GGSN queue. Triggers: Increments when a byte is forwarded from the GGSN queue. Availability: Per SGTP service Type: Counter | Int64
> sgtpu-total-ggsn-pkt-drop | Total packets dropped for GTP-U messages from GGSN. | Int64
> sgtpu-total-ggsn-byts-drop | Total bytes dropped for GTP-U messages from GGSN. | Int64
> sgtpu-ggsn-pkt-queue-full | Total packets dropped due to queued buffer limit full for GTP-U messages from GGSN. | Int64
> sgtpu-ggsn-byts-queue-full | Total bytes dropped due to queued buffer limit full for GTP-U messages from GGSN. | Int64
> sgtpu-total-pkt-ctxt-preserved | Total number of GTP packets from GGSN dropped in preserved context. | Int64
> sgtpu-total-byts-ctxt-preserved | Total number of GTP bytes from GGSN dropped in preserved with context. | Int64
> sgtpu-ggsn-pkt-unkwn-sess | Total number of GTP packets from GGSN dropped in unknown session. | Int64
> sgtpu-ggsn-byts-unkwn-sess | Total number of GTP bytes from GGSN dropped in unknown session. | Int64
> sgtpu-ggsn-pkt-drop-suspend-dealloc-st | Total number of GTP packets from GGSN dropped due to session de-allocation state was in suspended state. | Int64
> sgtpu-ggsn-byts-drop-suspend-dealloc-st | Total number of GTP bytes from GGSN dropped due to session de-allocation state was in suspended state. | Int64
> sgtpu-ggsn-pkt-page-fail | Total number of GTP packets dropped due to paging failure when there was downlink data from GGSN. | Int64
> sgtpu-ggsn-byts-page-fail | Total number of GTP bytes dropped due to paging failure when there was downlink data from GGSN. | Int64
> sgtpu-ggsn-pkt-v0-seq-num-nt-pres | Total number of packets from GGSN dropped as GTP-Uv0 messages received with sequence number flag set to false. | Int64
> sgtpu-ggsn-byts-v0-seq-num-nt-pres | Total number of bytes from GGSN dropped as GTP-Uv0 messages received with sequence number flag set to false. | Int64
> sgtpu-ggsn-pkt-unknown-version | Total number of GTP-U packets received from GGSN with unknown GTP version. | Int64
> sgtpu-ggsn-byts-unknown-version | Total number of GTP-U bytes received from GGSN with unknown GTP version. | Int64
> sgtpu-ggsn-pkt-invalid-msg-length | Total number of GTP packets from GGSN dropped as GTP-U messages received with invalid message length. | Int64
> sgtpu-ggsn-byts-invalid-msg-length | Total number of GTP bytes from GGSN dropped due to GTP-U messages received with invalid message length. | Int64
> sgtpu-ggsn-pkt-traffic-policing | Total number of GTP-U packets received from GGSN under subscriber traffic policing support. | Int64
> sgtpu-ggsn-byts-traffic-policing | Total number of GTP-U bytes received from GGSN under subscriber traffic policing support. | Int64
> sgtpu-ggsn-pkt-iu-release | Description: Total number of downlink packets that were queued but dropped due to IU/RAB release. Triggers: Counter at the new SGSN increments when Iu/RAB gets released while inter-SGSN-RAU is in progress and downlink data is queued during RAU. Availability: Per SGTP service Type: Counter | Int64
> sgtpu-ggsn-byts-iu-release | Description: Total number of downlink bytes that were queued but dropped due to IU/RAB release. Triggers: Counter at the new SGSN increments when Iu/RAB gets released while inter-SGSN-RAU is in progress and downlink data is queued during RAU. Availability: per SGTP service Type: Counter | Int64
> sgtpu-ggsn-pkt-t3-tmr-expiry | Description: Total number of downlink packets that were queued but dropped due to T3-tunnel timer expiry during inter-SGSN RAU procedure. Triggers: During inter-SGSN RAU at the old SGSN, neither Cancel Location or SGSN Context Ack are received when t3-tunnel timer is fired causing the RAU procedure to abort. If old RABs are not available, the data queued during the RAU will be dropped. Availability: per SGTP service Type: Counter | Int64
> sgtpu-ggsn-byts-t3-tmr-expiry | Description: Total number of downlink bytes that were queued but dropped due to T3-tunnel timer expiry during inter-SGSN RAU procedure. Triggers: During inter-SGSN RAU at the old SGSN, neither Cancel Location or SGSN Context Ack are received when t3-tunnel timer is fired causing the RAU procedure to abort. If old RABs are not available, the data queued during the RAU will be dropped. Availability: per SGTP service Type: Counter | Int64
> sgtpu-ggsn-pkt-bvc-block | Description: This proprietary counter indicates the total number of packets that are dropped from the GGSN queue, because of BVC Block or BVC Reset messages received for the MM context. Triggers: Increments when a packet is dropped from the GGSN queue because of BVC Reset/BVC Block received for the MM context. Availability: per SGTP service Type: Counter | Int64
> sgtpu-ggsn-byts-bvc-block | Description: This proprietary counter indicates the total number of bytes that are dropped from the GGSN queue, because of BVC Block or BVC Reset messages received for the MM context. Triggers: Increments when a byte is dropped from the GGSN queue because of BVC Reset/BVC Block received for the MM context. Availability: per SGTP service Type: Counter | Int64
> sgtpu-rnc-pkt-rcvd | Total packets for GTP-U messages received from RNC. | Int64
> sgtpu-rnc-byts-rcvd | Description: Total number of GTP-U messages bytes received from the RNC at a given instance of time. Triggers: Increments when SGSN receives an uplink packet from an RNC. Availability: Across all SGTP services, per SGTP service, per RNC Type: Counter | Int64
> sgtpu-rnc-pkt-queued | Total packets queued for GTP-U messages from RNC. | Int64
> sgtpu-rnc-byts-queued | Total bytes queued for GTP-U messages from RNC. | Int64
> sgtpu-total-rnc-pkt-drop | Total packets dropped for GTP-U messages from RNC. | Int64
> sgtpu-total-rnc-byts-drop | Total bytes dropped for GTP-U messages from RNC. | Int64
> sgtpu-rnc-pkt-queue-full | Total packets dropped due to queued buffer limit full for GTP-U messages from RNC. | Int64
> sgtpu-rnc-byts-queue-full | Total bytes dropped due to queued buffer limit full for GTP-U messages from RNC. | Int64
> sgtpu-rnc-pkt-unkwn-sess | Total number of GTP packets from RNC dropped in unknown session. | Int64
> sgtpu-rnc-byts-unkwn-sess | Total number of GTP bytes from RNC dropped in unknown session. | Int64
> sgtpu-rnc-pkt-rau-in-active-reg-st | Total number of GTP packets from RNC dropped due to routing area update procedure in active registration state. | Int64
> sgtpu-rnc-byts-rau_in_active-reg-st | Total number of GTP bytes from RNC dropped due to routing area update procedure in active registration state. | Int64
> sgtpu-rnc-pkt-drop-suspended-dealloc-st | Total number of GTP packets from RNC dropped due to session de-allocation state was in suspended state. | Int64
> sgtpu-rnc-byts-drop-suspended-dealloc-st | Total number of GTP bytes from RNC dropped due to session de-allocation state was in suspended state. | Int64
> sgtpu-rnc-pkt-unknown-version | Total number of GTP-U packets received from RNC with unknown GTP version. | Int64
> sgtpu-rnc-byts-unknown-version | Total number of GTP-U bytes received from RNC for packets with unknown GTP version. | Int64
> sgtpu-rnc-pkt-invalid-msg-length | Total number of GTP packets from RNC dropped due to GTP-Uv0 messages received with invalid message length. | Int64
> sgtpu-rnc-byts-invalid-msg-length | Total number of GTP bytes from RNC dropped due to TP-Uv0 messages received with invalid message length. | Int64
> sgtpu-rnc-pkt-source-ip-viol | Total number of GTP packets from RNC dropped as received GTP-Uv0 message shows source IP violation. | Int64
> sgtpu-rnc-byts-source-ip-viol | Total number of GTP bytes from RNC dropped as received GTP-Uv0 message shows source IP violation. | Int64
> sgtpu-rnc-pkt-traffic-policing | Total number of GTP-U packets received from RNC under subscriber traffic policing support. | Int64
> sgtpu-rnc-byts-traffic-policing | Total number of GTP-U bytes received from RNC under subscriber traffic policing support. | Int64
> sgtpu-sgsn-pkt-rcvd | Total packets for GTP-U messages received from peer SGSN. | Int64
> sgtpu-sgsn-byts-rcvd | Total bytes for GTP-U messages received from peer SGSN. | Int64
> sgtpu-sgsn-pkt-queued | Total packets queued for GTP-U messages from peer SGSN. | Int64
> sgtpu-sgsn-byts-queued | Total bytes queued for GTP-U messages from peer SGSN. | Int64
> sgtpu-total-sgsn-pkt-drop | Total packets dropped for GTP-U messages from peer SGSN. | Int64
> sgtpu-total-sgsn-byts-drop | Total bytes dropped for GTP-U messages from peer SGSN. | Int64
> sgtpu-sgsn-pkt-queue-full | Total packets dropped due to queued buffer limit full for GTP-U messages from peer SGSN. | Int64
> sgtpu-sgsn-byts-queue-full | Total bytes dropped due to queued buffer limit full for GTP-U messages from peer SGSN. | Int64
> sgtpu-sgsn-pkt-unkwn-sess | Total number of GTP packets from peer SGSN dropped in unknown session. | Int64
> sgtpu-sgsn-byts-unkwn-sess | Total number of GTP bytes from peer SGSN dropped in unknown session. | Int64
> sgtpu-sgsn-pkt-iu-release | Total number of GTP packets from peer SGSN received with Iu release message. | Int64
> sgtpu-sgsn-byts-iu-release | Total number of GTP bytes from peer SGSN received with Iu release message. | Int64
> sgtpu-sgsn-pkt-inconsistent-tunnel-state | Total number of GTP packets from peer SGSN received during inconsistent tunnel state. | Int64
> sgtpu-sgsn-byts-inconsistent-tunnel-state | Total number of GTP bytes from peer SGSN received during inconsistent tunnel state. | Int64
> sgtpu-sgsn-pkt-sess-dealloc | Total number of GTP packets from peer SGSN received during session deallocation procedure. | Int64
> sgtpu-sgsn-byts-sess-dealloc | Total number of GTP bytes from peer SGSN received during session deallocation procedure. | Int64
> sgtpu-sgsn-pkt-unknown-version | Total number of GTP-U packets received from peer SGSN with unknown GTP version. | Int64
> sgtpu-sgsn-byts-unknown-version | Total number of GTP-U bytes received from peer SGSN with unknown GTP version. | Int64
> sgtpu-sgsn-pkt-invalid-msg-length | Total number of GTP packets from peer SGSN received with invalid message length. | Int64
> sgtpu-sgsn-byts-invalid-msg-length | Total number of GTP bytes from peer SGSN received with invalid message length. | Int64
> sgtpu-echo-req-tx | Total number of GTP-U echo request messages sent. | Int32
> sgtpu-echo-req-rx | Total number of GTP-U echo request messages received. | Int32
> sgtpu-echo-res-tx | Total number of GTP-U echo response messages sent. | Int32
> sgtpu-echo-res-rx | Total number of GTP-U echo response messages received. | Int32
> sgtpu-v1-echo-req-tx | Total GTP-Uv1 echo request messages sent. | Int32
> sgtpu-v0-echo-req-tx | Total GTP-Uv0 echo request messages sent. | Int32
> sgtpu-v1-echo-req-rx | Total GTP-Uv1 echo request messages received. | Int32
> sgtpu-v0-echo-req-rx | Total GTP-Uv0 echo request messages received. | Int32
> sgtpu-v1-echo-rsp-tx | Total GTP-Uv1 echo request response messages sent. | Int32
> sgtpu-v0-echo-rsp-tx | Total GTP-Uv0 echo request response messages sent. | Int32
> sgtpu-v1-echo-rsp-rx | Total GTP-Uv1 echo request response messages received. | Int32
> sgtpu-v0-echo-rsp-rx | Total GTP-Uv0 echo request response messages received. | Int32
> sgtpu-v1-echo-req-retrans | Total GTP-Uv1 echo request response messages retransmitted. | Int32
> sgtpu-v0-echo-req-retrans | Total GTP-Uv0 echo request response messages retransmitted. | Int32
> sgtpu-ggsn-errind-sent | Total GTP-U (v1 and v0) messages sent to GGSN with error indication. | Int32
> sgtpu-ggsn-errind-rcvd | Total GTP-U (v1 and v0) messages received from GGSN with error indication. | Int32
> sgtpu-rnc-errind-sent | Total GTP-U (v1 and v0) messages sent to RNC with error indication. | Int32
> sgtpu-rnc-errind-rcvd | Total GTP-U (v1 and v0) messages received from RNC with error indication. | Int32
> sgtpu-sgsn-unknown-errind | Total GTP-U (v1 and v0) messages sent to peer SGSN with unknown error indication. | Int32
> sgtpu-sgsn-unsolicited-data-pkt | Total GTP-U (v1 and v0) messages received with unsolicited data packets in GTP-U messages. | Int32
> sgtpu-sgsn-err-ind-for-unsolicited-pkt | Total GTP-U (v1 and v0) messages received with error indication for unsolicited pata packets in GTP-U messages. | Int32
> sgtpu-total-active-ggsn | Total active GGSN nodes. This statistic value is of Gauge. | Int32
> sgtpu-total-active-rnc | Total active RNC nodes. This statistic value is of Gauge. | Int32
> sgtpu-errors-payload-length-mismatch | Description: Total number of “invalid” packets received from GGSN or RNC with errors due to mismatch in payload length. Triggers: Increments when received GTP-U (v1 and v0) header does not match with the actual payload length field. Availability: Across all SGTP services, per SGTP service Type: Counter | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883