> ASN RAN Peer Map Configuration Mode Commands
> The RAN Peer Map Configuration Mode is used to create and manage global mapping tables of base station peers.
> end
> This command exits the current mode and returns to the Executive Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Executive mode.
> exit
> This command exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> ran-peer
> Configures the MAC and IP addresses of base station peers being added to this map.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> [ no ] ran-peer id mac_address address ip_address[mode{non-legacy | legacy}]
> no
> Removes the base station peer entry from this map.
> id mac_address address ip_address
> id mac_address: Configures the MAC address of the base station peer in this map.
> mac_address must be in one of the following formats:
> nn:nn:nn:nn:nn:nn or nn-nn-nn-nn-nn-nn
> address ip_address: Specifies the IP address of the base station peer. ip_address must be expressed in IPv4 or IPv6 dotted decimal notation.
> mode {non-legacy | legacy}: Default mode is non-legacy.
> Usage
> Use this command to add base station peers to this peer map.
> Example
> The following command adds a base station peer to this map:
> ran-peer id 00:05:47:00:37:44 address 12.345.76.789

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883