> Diameter Authentication Schema Statistics
> This chapter describes the Diameter Authentication schema statistics.
> Important: The Diameter Authentication schema is only available in StarOS 10.0 and later releases.
> The Diameter Authentication schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described in the Schema Format String Syntax section of the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
> Important: All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed.
> The following variables are supported:
> Diameter Authentication Schema Statistics

> Statistic | Description | Data Type
> vpnid | The identification number of the context currently facilitating Diameter Authentication configuration. | Int32
> vpnname | The name of the context currently facilitating Diameter Authentication configuration. | String
> ipaddr | The IP address of the server for which statistics are being collected. | String
> port | The server port being used for exchange of data. | Int32
> servertype | The type of server for which statistics are being collected. | String
> group | The name of the AAA Diameter Group. | String
> der-req-id-sent | The total number of DER messages sent. | Int32
> der-req-aka-chal-sent | The total number of der-request-AKA-CHALLENGE messages sent. | Int32
> der-req-retried | The total number of retries for DER messages. | Int32
> dea-chal-rcvd | The total number of DEA Challenge messages received. | Int32
> dea-acpt-rcvd | The total number of DEA Accept messages received. | Int32
> dea-timeout | The total number of DEA timeout messages. | Int32
> dea-badauth | The total number of DEA Bad-Authentication messages. | Int32
> dea-malformed | The total number of DEA Malformed messages. | Int32
> dea-malformed-avp | The total number of DEA Malformed AVP messages. | Int32
> dea-dropped | The total number of dropped DEA messages. | Int32
> rar-req-rcvd | The total number of RAR messages received. | Int32
> raa-ans-accpt-sent | The total number of RAA messages sent. | Int32
> aar-req-sent | The total number of AAR messages sent. | Int32
> str-req-sent | The total number of STR requests sent. | Int32
> str-req-retried | The total number of retries for STR messages. | Int32
> sta-ans-accpt-rcvd | The total number of received STA messages. | Int32
> asr-req-rcvd | The total number of number of ASR requests received. | Int32
> asa-rsp-accpt-sent | The total number of ASA Messages sent. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883