> show gtpp
> This chapter includes the show gtpp command output tables.
> show gtpp accounting servers
> show gtpp accounting servers Command Output Descriptions

> Field | Description
> Context Name | The name of the system context in which the CGF is configured.
> Primary Accounting server address | The IP address of the CGF.
> port | The TCP port over which GTPP messaging is performed.
> priority | The configured priority of the CGF.
> State | The status of the CGF as Active or Inactive.
> Group | The GTPP server group name in which this server is configured.

> ‌
> show gtpp counters all
> show gtpp counters all Command Output Descriptions

> Field | Description
> Outstanding GCDRs | The current total number of G-CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding GCDRs | The total number of G-CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived GCDRs | The current total number of G-CDRs achieved by CGF.
> GCDRs buffered with AAAPROXY | The current total number of G-CDRs buffered by the system’s AAA Proxy tasks.
> GCDRs buffered with AAAMGR | The current total number of G-CDRs buffered by the system’s AAA Manager tasks.
> Outstanding MCDRs | The current total number of M-CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding MCDRs | The total number of M-CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived MCDRs | The current total number of M-CDRs achieved by CGF.
> MCDRs buffered with AAAPROXY | The current total number of M-CDRs buffered by the system’s AAA Proxy tasks.
> MCDRs buffered with AAAMGR | The current total number of M-CDRs buffered by the system’s AAA Manager tasks.
> Outstanding SCDRs | The current total number of S-CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding SCDRs | The total number of S-CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived SCDRs | The current total number of S-CDRs achieved by CGF.
> SCDRs buffered with AAAPROXY | The current total number of S-CDRs buffered by the system’s AAA Proxy tasks.
> SCDRs buffered with AAAMGR | The current total number of S-CDRs buffered by the system’s AAA Manager tasks.
> Outstanding S-SMO-CDRs | The current total number of S-SMO-CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding S-SMO-CDRs | The total number of S-SMO-CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived S-SMO-CDRs | The current total number of S-SMO-CDRs achieved by CGF.
> S-SMO-CDRs buffered with AAAPROXY | The current total number of S-SMO-CDRs buffered by the system’s AAA Proxy tasks.
> S-SMO-CDRs buffered with AAAMGR | The current total number of S-SMO-CDRs buffered by the system’s AAA Manager tasks.
> Outstanding S-SMT-CDRs | The current total number of S-SMT-CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding S-SMT-CDRs | The total number of S-SMT-CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived S-SMT-CDRs | The current total number of S-SMT-CDRs achieved by CGF.
> S-SMT-CDRs buffered with AAAPROXY | The current total number of S-SMT-CDRs buffered by the system’s AAA Proxy tasks.
> S-SMT-CDRs buffered with AAAMGR | The current total number of S-SMT-CDRs buffered by the system’s AAA Manager tasks.
> Outstanding GMBH CDRs | The current total number of GMBH CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding GMBH CDRs | The total number of GMBH CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived GMBH CDRs | The current total number of GMBH CDRs achieved by CGF.
> GMBH CDRs buffered with AAAPROXY | The current total number of GMBH CDRs buffered by the system’s AAA Proxy tasks.
> GMBH CDRs buffered with AAAMGR | The current total number of GMBH CDRs buffered by the system’s AAA Manager tasks.
> Outstanding SGW CDRs | The current total number of S-GW CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding SGW CDRs | The total number of S-GW CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived SGW CDRs | The current total number of S-GW CDRs achieved by CGF.
> SGW CDRs buffered with AAAPROXY | The current total number of S-GW CDRs buffered by the system’s AAA Proxy tasks.
> SGW CDRs buffered with AAAMGR | The current total number of S-GW CDRs buffered by the system’s AAA Manager tasks.
> Outstanding SMBMS CDRs | The current total number of SMBMS CDRs sent to the CGF(s) for which no response was received.
> Possibly Duplicate Outstanding SMBMS CDRs | The total number of SMBMS CDRs sent to the CGF(s) with a packet transfer command of “Send Possibly Duplicated Data Record Packet”
> Archived SMBMS CDRs | The current total number of SMBMS CDRs achieved by CGF.
> SMBMS CDRs buffered with AAAPROXY | The current total number of SMBMS CDRs buffered by the system’s AAA Proxy tasks.
> SMBMS CDRs buffered with AAAMGR | The current total number of SMBMS CDRs buffered by the system’s AAA Manager tasks.

> ‌
> show gtpp group
> show gtpp group Command Output Descriptions

> Field | Description
> Group name | The GTPP server group name.
> Context | The context name of the configured GTPP group.
> CDR timeout | Indicates the configured timeout duration in seconds for CDRs.
> CDR max-retries | Indicates the configured maximum retries for CDR.
> ECHO timeout | Indicates the configured timeout duration in seconds for ECHO message.
> ECHO max-retries | Indicates the configured maximum retries for ECHO message.
> Dead time | Indicates the dead time for specific GTPP group.
> Detect-dead-server consecutive-failures | Indicates the total consecutive failure of dead server detection probe.
> Duplicate-hold-time minutes | Configured time in minutes to hold duplicate CDRs.
> Redirection allowed | Indicates whether redirection is allowed or not.
> Source-port-validation | Indicates whether source port validation is enabled or not.
> Charging-agent address | Indicates the IP address of configured charging agent.
> Charging-agent port | Indicates the port number of configured charging agent.
> Max CDR size | Indicates the maximum CDR size allowed in bytes.
> Max CDRs in msg | Indicates the maximum CDRs allowed in a message.
> Max CDRs wait-time | Indicates the maximum wait/live time allowed for CDRs.
> Dictionary | Indicates the applicable GTPP dictionary for CDR encoding.
> Data-req start seq-num | Indicates the starting sequence number of data request message.
> Storage Server | This group indicates the storage server information if CDR storage mode is remote. This counter is applicable for the ASR 5000 only.
> Mode | Indicates the mode of the CDR storage. Possible modes are:
> • | Local: CDRs stored on local HDD on SMC card.
> • | Remote: CDRs stored on remote GSS server.
> This counter is applicable for the ASR 5000 only.
> Storage-server address | Indicates the configured GTPP storage server IP address.
> Storage-server port | Indicates the port number of configured GTPP storage server.
> Storage-server timeout | indicates the timeout in seconds configured for GTPP storage server.
> Storage-server max-retries | Indicates the maximum retries configured for the GSS messages.
> Local Storage | This group indicates the storage server information, if CDR storage mode is local. This counter group is applicable for the ASR 5000 only.
> File rotation volume-limit | Indicates the volume of CDR file in MB after which CDR file rotation will happen. This counter group is applicable for the ASR 5000 only.
> File rotation CDR-count | Indicates the number of CDRs to include in a CDR file after which CDR file rotation will happen. This counter group is applicable for the ASR 5000 only.
> File rotation time-interval | Indicates the time duration in seconds after after which CDR file rotation will happen. This counter group is applicable for the ASR 5000 only.
> Force File rotation by time-interval | Indicates whether force file rotation is enabled or not. If this is enabled it forces the system for file-rotation at specified interval even if there are no CDRs generated.
> File compression | Indicates the whether file compression is configured or not on CDR files. This counter group is applicable for the ASR 5000 only.
> File format | Indicates the format name of file to store CDRs in specified format in CDR file. This counter group is applicable for the ASR 5000 only.
> Purge-processed-files | Indicates the configuration of purge interval duration of processed files. This is an optional setting and can be configured with purge-interval purge_dur keyword with gtpp storage-server local file purge-processed-files command in GTPP Group Configuration Mode.
> Attributes
> Diagnostics present | Indicates whether diagnostic attribute is present or not.
> MSISDN present | Indicates whether MSISDN attribute is present or not.
> IMEI present | Indicates whether IMEI attribute is present or not.
> RAT present | Indicates whether RAT attribute is present or not.
> Duration in milliseconds | Indicates the configured duration in ms.
> PLMN-id present | Indicates whether public land mobile network identifier attribute is present or not.
> PLMN-id unknown-use | Indicates whether a public land mobile network identifier which is of unknown use present or not.
> Local-rec-seq-num present | Indicates whether local record sequence number attribute is present or not.
> Node-id suffix | Indicates server node id present in attribute or not.
> Cell-plmn-id | Indicates whether cell public land mobile network identifier attribute is present or not.
> Sms | Indicates the SMS attribute information.
> Recording entity | Indicates the whether SMS recording entity present in attribute or not.
> Service centre | Indicates the whether SMS service center information present in attribute or not.
> Destination number | Indicates the whether destination number for SMS present in attribute or not.
> Record extensions: | Indicates the information for record extensions
> Rat | Indicates whether radio access type information present in record extension attributes or not.
> Triggers
> Volume-limit | Indicates the status of configured volume limit trigger. Possible status are:
> • | Enabled
> • | Disabled
> Time-limit | Indicates the status of configured time limit trigger. Possible status are:
> • | Enabled
> • | Disabled
> Tariff-time-change | Indicates the status of configured trigger for tariff time change. Possible status are:
> • | Enabled
> • | Disabled
> SGSN-change-limit | Indicates the status of configured trigger for SGSN change limit. Possible status are:
> • | Enabled
> • | Disabled
> Intra-SGSN-group-change | Indicates the status of configured trigger for intra-SGSN group change. Possible status are:
> • | Enabled
> • | Disabled
> Inter-plmn-sgsn-change | Indicates the status of configured trigger for SGSN change between PLMN. Possible status are:
> • | Enabled
> • | Disabled
> Egcdr-max-losdv-limit | Indicates the status of configured trigger for maximum list of service data volume (LoSDV) limit for eG-CDRs. Possible status are:
> • | Enabled
> • | Disabled
> Qos-change | Indicates the status of configured trigger for QoS change. Possible status are:
> • | Enabled
> • | Disabled
> RAT-change | Indicates the status of configured trigger for RAT change. Possible status are:
> • | Enabled
> • | Disabled
> MS-timezone-change | Indicates the status of configured trigger for change in time zone of MS. Possible status are:
> • | Enabled
> • | Disabled
> Routing-area-update | Indicates the status of configured trigger for update in routing area. Possible status are:
> • | Enabled
> • | Disabled
> Direct-tunnel | Indicates the status of configured trigger for direct tunnel. Possible status are:
> • | Enabled
> • | Disabled
> Mbms config | Specifies the MBMS configuration information.
> Buckets | Indicates the total number of data buckets configured for MBMS service.
> Interval | Indicates the interval duration configured for MBMS service.
> Volume | Indicates the data volume configured for MBMS service.
> Tarif: | Specifies the tariff configuration for MBMS service.
> Time1 | Indicates the tariff configuration for time slot 1 in MBMS service.
> Time2 | Indicates the tariff configuration for time slot 2 in MBMS service.
> Time3 | Indicates the tariff configuration for time slot 3 in MBMS service.
> Time4 | Indicates the tariff configuration for time slot 4 in MBMS service.
> EGCDR | Specifies the configuration for eG-CDRs.
> Lotdv-max-containers | Indicates the maximum number of containers configured for list of traffic data volume (LoTDV) for eG-CDRs.
> Losdv-max-containers | Indicates the maximum number of containers configured for list of service data volume (LoSDV) for eG-CDRs.
> Service-idle-timeout | Indicates the idle timeout duration configured in seconds for service for eG-CDRs.
> Service-interval | Indicates whether interval duration configured in seconds to retry for eG-CDRs.
> Service-uplink | Indicates the total bytes uplinked for service in eG-CDRs.
> Service-downlink | Indicates the total bytes downlinked for service in eG-CDRs.
> Service-total | Indicates the total bytes in traffic (uplinked+ downlinked) for service in eG-CDRs.
> Closing-cause-unique | Indicates whether any unique closing cause set for eG-CDR closing.
> Include-all-losdvs | Indicates whether eG-CDR configured to include all LoSDV.
> Delete-service-thresholds | indicates the configured threshold in eG-CDR to delete the service.

> ‌
> show gtpp statistics
> show gtpp statistics Command Output Descriptions

> Field | Description
> Accumulated Statistics
> Start Collection Req | Total number of Start Collection requests.
> Normal Release Req | Total number of Normal Release requests.
> Management Intervention Req | Total number of Management Intervention requests.
> Abnormal Release Req | Total number of Abnormal Release requests.
> Time Limit Req | Total number of Time Limit requests.
> Volume Limit Req | Total number of Volume Limit requests.
> SGSN Change Req | Total number of SGSN Change requests.
> Maximum Change Condition Req | Total number of Maximum Change Condition requests.
> RAT Change Req | Total number of RAT Change requests.
> MS Time Zone Change Req | Total number of MS Time Zone Change requests.
> List of Down Stream Node Change | List of down-stream node change.
> Intra SGSN Intersystem Change Req | Total number of Intra SGSN Intersystem Change requests.
> FOCS/ODB ACL Violation Req | Indicates the total number of FOCS enabled sessions closed due to ACL rule violation recieved for FOCS and/or ODB.
> Inactivity Timeout (FOCS enabled): | Indicates the total number of FOCS enabled sessions closed due to inactivity timeout.
> Total G-CDR transmission | Total number of G-CDR transmissions.
> Total S-CDR transmission | Total number of S-CDR transmissions.
> Total M-CDR transmission | Total number of M-CDR transmissions.
> Total S-SMO-CDR transmission | Total number of S-SMO-CDR transmissions.
> Total S-SMT-CDR transmission | Total number of S-SMT-CDR transmissions.
> Total G-MB-CDR transmission | Total number of G-MB-CDR transmissions.
> Total G-CDR retransmission | Total number of G-CDR retransmissions.
> Total S-CDR retransmission | Total number of S-CDR retransmissions.
> Total M-CDR retransmission | Total number of M-CDR retransmissions.
> Total S-SMO-CDR retransmission | Total number of S-SMO-CDR retransmissions.
> Total S-SMT-CDR retransmission | Total number of S-SMT-CDR retransmissions.
> Total G-MB-CDR retransmission | Total number of G-MB-CDR retransmissions.
> Total G-CDR accepted | Total number of G-CDR accepted.
> Total S-CDR accepted | Total number of S-CDR accepted.
> Total M-CDR accepted | Total number of M-CDR accepted.
> Total S-SMO-CDR accepted | Total number of S-SMO-CDR accepted.
> Total S-SMT-CDR accepted | Total number of S-SMT-CDR accepted.
> Total G-MB-CDR accepted | Total number of G-MB-CDR accepted.
> Total G-CDR transmission failures | Total number of G-CDR transmission failures.
> Total S-CDR transmission failures | Total number of S-CDR transmission failures.
> Total M-CDR transmission failures | Total number of M-CDR transmission failures.
> Total S-SMO-CDR transmission failures | Total number of S-SMO-CDR transmission failures.
> Total S-SMT-CDR transmission failures | Total number of S-SMT-CDR transmission failures.
> Total G-MB-CDR transmission failures | Total number of G-MB-CDR transmission failures.
> G-CDR transmission failure percent | G-CDR transmission failure percentage.
> S-CDR transmission failure percent | S-CDR transmission failure percentage.
> M-CDR transmission failure percent | M-CDR transmission failure percentage.
> S-SMO-CDR transmission failure percent | S-SMO-CDR transmission failure percentage.
> S-SMT-CDR transmission failure percent | S-SMT-CDR transmission failure percentage.
> G-MB-CDR transmission failure percent | G-MB-CDR transmission failure percentage.
> CDRs purged by dead-server suppress-cdrs | Total number of CDRs purged in all GTPP server groups configured on system when gtpp dead-server suppress-cdrs command is enabled.
> Charging Characteristics Statistics
> Hot | The charging characteristic setting.
> Normal | The charging characteristic setting.
> Prepaid | The charging characteristic setting.
> Flat | The charging characteristic setting.
> Unknown | The charging characteristic setting.
> CGF Specific Statistics
> Data Record Transfer Requests Sent When the primary CGF goes down, all outstanding requests with the primary CGF are marked as Possibly Duplicate and sent to the secondary CGF. This is because of the uncertainty as to whether the primary CGF processed the requests or not. So the seq-numbers (for primary CGF) for these requests are stored. When the primary CGF comes back again, an Empty DRT with the stored seq-numbers is sent to the primary CGF. The CGF can reply either REQ_ALREADY_FULFILLED (primary CGF processed the request. Cancel request is sent to the secondary CGF to delete the request) or REQUEST_ACCEPTED (primary CGF has not got this request before. Release request is sent to secondary to store the request).
> Send | Total number of DRT requests sent.
> Possibly Duplicate | Total number of possibly duplicate DRT requests sent.
> Cancel | Total number of cancel DRT requests sent.
> Release | Total number of release DRT requests sent.
> Empty | Total number of empty DRT requests sent.
> Data Record Transfer Requests Retried
> Send | Total number of DRT request retried.
> Possibly Duplicate | Total number of DRT requests marked possibly duplicate retried.
> Cancel | Total number of cancel DRT requests retried.
> Release | Total number of release DRT requests retried.
> Empty | Total number of empty DRT requests retried.
> Data Record Transfer Requests Success
> Send | Total number of DRT requests sent successfully.
> Possibly Duplicate | Total number of DRT requests marked possibly duplicate sent successfully.
> Cancel | Total number of canceled DRT requests sent successfully.
> Release | Total number of release DRT requests sent successfully.
> Empty | Total number of empty DRT requests sent successfully.
> Data Record Transfer Response Cause
> Accepted | Total number of DRT response messages with cause as “accepted”.
> Not Fulfilled | Total number of DRT response messages with cause as “not fulfilled”.
> Already Fulfilled | Total number of DRT response messages with cause as “already fulfilled”.
> Dup Already Fulfilled | Total number of DRT response messages with cause as “duplicate already fulfilled”.
> Invalid Msg Format | Total number of DRT response messages with cause as “invalid message format”.
> Mandatory IE Missing | Total number of DRT response messages with cause as “mandatory IE missing”.
> Service not supported | Total number of DRT response messages with cause as ‘service not supported”.
> Version not supported | Total number of DRT response messages with cause as “version not supported”.
> Mandatory IE incorrect | Total number of DRT response messages with cause as “mandatory IE incorrect”.
> Optional IE incorrect | Total number of DRT response messages with cause as “optional IE incorrect”.
> No Resources | Total number of DRT response messages with cause as “no resources”.
> System Failure | Total number of DRT response messages with cause as “system failure”.
> CDR Decode Error | Total number of DRT response messages with cause as “CDR decode error”.
> Seq No incorrect | Total number of DRT response messages with cause as “sequence number incorrect”.
> Unknown Cause | Total number of DRT response messages with unknown cause.
> GTPP Echo Messages
> Echo Req Sent | Total number of echo request messages sent.
> Echo Req Rcvd | Total number of echo request messages received.
> Echo Rsp Rcvd | Total number of echo response messages received.
> Echo Rsp Sent | Total number of echo response messages sent.
> Redirection Req/Rsp Messages
> Redirection Req Rcvd | Total number of redirection request messages received.
> Redirection Rsp Sent | Total number of redirection response messages sent.
> Redirection Request Cause
> Trans Buffer full | Total number of redirection requests with cause code as “transmit buffers are full”.
> Recv Buffer Full | Total number of redirection requests with cause code as “receive buffers are full”.
> Other Node Down | Total number of redirection requests with cause code as “other node is about to go down.
> Self Node down | Total number of redirection requests with cause code as “this node is about to go down”.
> System Failure | Total number of redirection requests with cause code as “system failure”.
> Redirection Response Cause
> Accepted | Total number of redirection responses with cause code as “accepted”.
> Service Not Supported | Total number of redirection responses with cause code as “service not supported”.
> System Failure | Total number of redirection responses with cause code as “system failure”.
> Mandatory IE Incorrect | Total number of redirection responses with cause code as “mandatory IE incorrect”.
> Mandatory IE Missing | Total number of redirection responses with cause code as “mandatory IE missing”.
> Optional IE incorrect | Total number of redirection responses with cause code as “optional IE incorrect”.
> Invalid Msg Format | Total number of redirection responses with cause code as “invalid message format”.
> Version Not Supported | Total number of redirection responses with cause code as “version not supported”.
> No Resources | Total number of redirection responses with cause code as “no resources”.
> Node Alive Req/Rsp Messages
> Node Alive Req Rcvd | Total number of node alive request messages received.
> Node Alive Req Sent | Total number of node alive request messages sent.
> Node Alive Rsp Sent | Total number of node alive response messages sent.
> Node Alive Rsp Rcvd | Total number of node alive response messages received.
> Invalid messages received
> Invalid Sequence Number | Total number of messages with invalid sequence number received.
> Unknown CGF | Total number of messages received with unknown CGF.
> Unknown Msg type | Total number of messages received with unknown message type.
> Round Trip Time
> Last DRT Round Trip Time | Time taken for the last DRT round trip.
> Average DRT Round Trip Time | Average time taken for DRT round trip.

> ‌
> show gtpp statistics cgf-address
> show gtpp statistics cgf-address Command Output Descriptions

> Field | Description
> Accumulated Statistics
> Start Collection Req | The total number of accounting start requests generated. NOTE: These requests are not sent to CGF. The requests are just a system record that accounting for a session has started and in future releases may be required to be sent to CGF.
> Normal Release Req | The total number of requests generated because of normal PDP context deletion (i.e. PDP context deletion initiated by SGSN or GGSN).
> Management Intervention Req | The total number of requests generated because of management intervention (request due to O&M reasons, e.g. clear subscribers all)
> Abnormal Release Req | The total number of requests generated because of abnormal termination of session (e.g. Session Manager failure results in abnormal release of PDP contexts active for that Session Manager.
> Time Limit Req | The number of interim requests generated because of the time limit being reached. The time limit is configured using the cc profile command in the GGSN service configuration mode.
> Volume Limit Req | The number of interim requests generated because of volume limit being reached. The volume limit is configured using cc profile command in the GGSN service configuration mode.
> SGSN Change Req | The number of interim requests generated because of the number of inter SGSN switch-overs reaching the configured limit or because of an SGSN switchover resulting in a new RAI (Routing Area Identity). The maximum number of SGSN changes is configured using the cc profile command in the GGSN service configuration mode.
> Maximum Change Condition Req | The number of interim requests generated because of the “List of traffic Volume" Containers reaching the configured limit. This value is configured using the cc profile command in the GGSN service configuration mode.
> Total G-CDR transmission | The total number of GTPP Requests sent to the CGF. NOTE: This counter does not include requests re-transmitted to the CGF.
> Total G-CDR retransmission | The total number of GTPP Requests retransmitted to the CGF. NOTE: This counter does not include the requests that were originally transmitted to the CGF.
> Total G-CDR accepted | The total number of G-CDRs accepted by the CGF.
> Total G-CDR transmission failures | The total number of GTPP Requests that were not responded to by CGFs. NOTE: This statistic is not displayed if the cgf_address optional keyword is used.
> G-CDR transmission failure percent | The failure percentage of DRT requests. This is calculated as (Total G-CDR Trans failures/(Total GCDR Trans Failures + Total G-CDR accepted) *100).
> Charging Characteristics Statistics
> Hot | The number of times that PDP Context Requests were processed with a charging characteristic profile index value of “1”, representing “hot” billing.
> Normal | The number of times that PDP Context Requests were processed with a charging characteristic profile index value of “8”, representing “normal” billing.
> Prepaid | The number of times that PDP Context Requests were processed with a charging characteristic profile index value of “4”, representing “prepaid billing.
> Flat | The number of times that PDP Context Requests were processed with a charging characteristic profile index value of “2”, representing “flat-rate” billing.
> Unknown | The number of times that PDP Context Requests were processed with an unknown charging characteristic profile index value.
> CGF Specific Statistics
> Data Record Transfer Requests Sent
> Send | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet". NOTE: This counter counts "Send Data Record Packet" with length more than 0.
> Possibly Duplicate | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send possibly duplicated Data Record Packet".
> Cancel | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Cancel Data Record Packet".
> Release | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Release Data Record Packet".
> Empty | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet". NOTE: This counter counts "Send Data Record Packet" with length equal to 0.
> Data Record Transfer Requests Retried
> Send | The total number of re-transmitted "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet". NOTE: This counter counts "Send Data Record Packet" with length more than 0.
> Possibly Duplicate | The total number of re-transmitted "Data Record Transfer Requests" sent with the Packet transfer command "Send possibly duplicated Data Record Packet".
> Cancel | The total number of re-transmitted "Data Record Transfer Requests" sent with the Packet transfer command "Cancel Data Record Packet".
> Release | The total number of re-transmitted "Data Record Transfer Requests" sent with the Packet transfer command "Release Data Record Packet".
> Empty | The total number of re-transmitted "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet". NOTE: This counter counts "Send Data Record Packet" with length equal to 0.
> Data Record Transfer Requests Success
> Send | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet" for which a response from the CGF was received. NOTE: This counter counts "Send Data Record Packet" with length more than 0.
> Possibly Duplicate | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send possibly duplicated Data Record Packet" for which a response from the CGF was received.
> Cancel | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Cancel Data Record Packet" for which a response from the CGF was received.
> Release | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Release Data Record Packet" for which a response from the CGF was received.
> Empty | The total number of "Data Record Transfer Requests" sent with the Packet transfer command "Send Data Record Packet" for which a response from the CGF was received. NOTE: This counter counts "Send Data Record Packet" with length equal to 0.
> Data Record Transfer Response Cause
> Accepted | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 128 (80H, Request accepted).
> Not Fulfilled | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 255 (FFH, Request not fulfilled).
> Already Fulfilled | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 253 (FDH, Request already fulfilled).
> Dup Already Fulfilled | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 252 (FCH, Request related to possibly duplicated packets already fulfilled).
> Invalid Msg Format | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 193 (C1H, Invalid message format).
> Mandatory IE Missing | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 202 (CAH, Mandatory IE missing).
> Service not supported | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 200 (C8H, Service not supported).
> Version not supported | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 198 (C6, Version not supported).
> Mandatory IE incorrect | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 201 (C9H, Mandatory IE incorrect).
> Optional IE incorrect | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 203 (CBH, Optional IE incorrect).
> No Resources | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 199 (C7H, No resources available).
> System Failure | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 204 (CCH, System failure).
> CDR Decode Error | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 177. The cause value "CDR decoding error" is primarily intended to inform the CDR generating node that the receiving node can not decode the CDR.
> Seq No incorrect | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code of 254.
> Unknown Cause | The total number of Data Record Transfer Response messages received from the CGF that indicated a cause code which is other than mentioned above.
> GTPP Echo Messages
> Echo Req Sent | The total number of Echo Request messages transmitted to the CGF.
> Echo Req Rcvd | The total number of Echo Request messages received from the CGF.
> Echo Rsp Rcvd | The total number of Echo Response messages received from the CGF.
> Echo Rsp Sent | The total number of Echo Response messages transmitted to the CGF.
> Redirection Req/Rsp Messages
> Redirection Req Rcvd | The total number of Redirection Request messages received from the CGF.
> Redirection Rsp Sent | The total number of Redirection Response messages transmitted to the CGF.
> Redirection Request Cause
> Trans Buffer full | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 60 (3CH, The transmit buffers are becoming full).
> Recv Buffer Full | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 61 (3DH, The receive buffers are becoming full).
> Other Node Down | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 62 (3EH, Another node is about to go down).
> Self Node down | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 63 (3FH, This node is about to go down).
> System Failure | The total number of Redirection Request messages received from the CGF(s) containing a cause information element of 59 (3BH, System failure).
> Redirection Response Cause
> Accepted | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 128 (80H, Request accepted).
> Service Not Supported | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 200 (C8H, Service not supported).
> System Failure | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 204 (CCH, System failure).
> Mandatory IE Incorrect | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 201 (C9H, Mandatory IE incorrect).
> Mandatory IE Missing | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 202 (CAH, Mandatory IE missing).
> Optional IE incorrect | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 203 (CBH, Optional IE incorrect).
> Invalid Msg Format | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 193 (C1H, Invalid message format).
> Version Not Supported | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 198 (C6H, Version not supported).
> No Resources | The total number of Redirection Response messages transmitted to the CGF(s) containing a cause information element of 199 (C7H, No resources available).
> Node Alive Req/Rsp Messages
> Node Alive Req Rcvd | The total number of Node Alive Request messages received.
> Node Alive Rsp Sent | The total number of Node Alive Response messages transmitted.
> Node Alive Req Sent | The total number of Node Alive Request messages sent.
> Node Alive Rsp Rcvd | The total number of Node Alive Response messages received.
> Invalid messages received
> Invalid Sequence Number | The total number of requests received from a pre-configured CGF, with sequence number that is not in the system's buffers.
> Round Trip Time | This section shows average latency on Ga/Gz interface per CGF.
> Last DRT Round Trip Time | Total time taken in milliseconds for round trip of previous data record transfer message.
> Average DRT Round Trip Time | Average time taken in milliseconds for round trip of all data record transfer messages.

> ‌
> show gtpp storage-server statistics
> show gtpp storage-server statistics Command Output Descriptions

> Field | Description
> Store Requests (GTPP Requests)
> Sent | The total number of GTPP Requests Messages sent by AAAProxy to GSS for storage. Each GTPP Request corresponds to one Store request to GSS. Therefore, each store request may contain one or more GCDR.
> Retried | The total number of GTPP Requests Messages re-sent by AAAProxy to GSS for storage.
> Success | The total number of GTPP Requests Messages successfully sent by AAAProxy to GSS for storage.
> Failed | The total number of GTPP Requests Messages that failed to be sent by AAAProxy to GSS for storage.
> Store Requests (GCDRs)
> Sent | The total number of G-CDRs in the GTPP Requests sent for "store".
> Retried | The total number of G-CDRs in the GTPP Requests re-sent for "store".
> Success | The total number of G-CDRs in the GTPP Requests successfully sent for "store".
> Failed | The total number of G-CDRs in the GTPP Requests that failed to be sent for "store".
> Store Requests (MCDRs)
> Sent | The total number of M-CDRs in the GTPP Requests sent for "store".
> Retried | The total number of M-CDRs in the GTPP Requests re-sent for "store".
> Success | The total number of M-CDRs in the GTPP Requests successfully sent for "store".
> Failed | The total number of M-CDRs in the GTPP Requests that failed to be sent for "store".
> Store Requests (SCDRs)
> Sent | The total number of S-CDRs in the GTPP Requests sent for "store".
> Retried | The total number of S-CDRs in the GTPP Requests re-sent for "store".
> Success | The total number of S-CDRs in the GTPP Requests successfully sent for "store".
> Failed | The total number of S-CDRs in the GTPP Requests that failed to be sent for "store".
> Store Requests (S-SMO-CDRs)
> Sent | The total number of S-SMO-CDRs in the GTPP Requests sent for "store".
> Retried | The total number of S-SMO-CDRs in the GTPP Requests re-sent for "store".
> Success | The total number of S-SMO-CDRs in the GTPP Requests successfully sent for "store".
> Failed | The total number of S-SMO-CDRs in the GTPP Requests that failed to be sent for "store".
> Store Requests (S-SMT-CDRs)
> Sent | The total number of S-SMT-CDRs in the GTPP Requests sent for "store".
> Retried | The total number of S-SMT-CDRs in the GTPP Requests re-sent for "store".
> Success | The total number of S-SMT-CDRs in the GTPP Requests successfully sent for "store".
> Failed | The total number of S-SMT-CDRs in the GTPP Requests that failed to be sent for “store”.
> Store Requests(GMBMSCDRs)
> Sent | The total number of GMBMS CDRs in the GTPP Requests sent for “store”.
> Retried | The total number of GMBMS CDRs in the GTPP Requests re-sent for “store”.
> Success | The total number of GMBMS CDRs in the GTPP Requests successfully sent for “store”.
> Failed | The total number of GMBMS CDRs in the GTPP Requests that failed to be sent for “store”.
> Store Requests(SMBMSCDRs)
> Sent | The total number of SMBMS CDRs in the GTPP Requests sent for “store”.
> Retried | The total number of SMBMS CDRs in the GTPP Requests re-sent for “store”.
> Success | The total number of SMBMS CDRs in the GTPP Requests successfully sent for “store”.
> Failed | The total number of SMBMS CDRs in the GTPP Requests that failed to be sent for “store”.
> Store Requests(SGWCDRs)
> Sent | The total number of S-GW CDRs in the GTPP Requests sent for “store”.
> Retried | The total number of S-GW CDRs in the GTPP Requests re-sent for “store”.
> Success | The total number of S-GW CDRs in the GTPP Requests successfully sent for “store”.
> Failed | The total number of S-GW CDRs in the GTPP Requests that failed to be sent for “store”.
> AAAProxy Recover Requests
> Sent | The total number of AAA Proxy Recover Requests sent by the AAA Proxy to the GSS. These requests are sent when the AAA Proxy is restarted after an outage.
> Retried | The total number of AAA Proxy Recover Requests re-sent by the AAA Proxy to the GSS.
> Success | The total number of AAA Proxy Recover Requests successfully sent by the AAA Proxy to the GSS.
> Failed | The total number of AAA Proxy Recover Requests that failed to be sent by the AAA Proxy to the GSS.
> Get Next Requests
> Sent | The total number of Get Next requests sent by the AAA Proxy to the GSS. The AAA Proxy maintains a limited buffer. When the buffer gets filled because of a delay in the CGF response, the AAA proxy starts sending the request to the GSS. To get these requests from the GSS, the AAA Proxy sends Get Next Requests to the GSS.
> Retried | The total number of Get Next requests re-sent by the AAA Proxy to the GSS.
> Success | The total number of Get Next requests successfully sent by the AAA Proxy to the GSS.
> Failed | The total number of Get Next requests that failed to be sent by the AAA Proxy to the GSS.
> Update CGF Requests
> Sent | The total number of requests sent by the AAA Proxy to the GSS to indicate a change in the status of the CGFs (i.e. from up to down or vice versa).
> Retried | The total number of requests re-sent by the AAA Proxy to the GSS to indicate a change in the status of the CGFs
> Success | The total number of requests successfully sent by the AAA Proxy to the GSS to indicate a change in the status of the CGFs
> Failed | The total number of requests that failed to be sent by the AAA Proxy to the GSS to indicate a change in the status of the CGFs
> AAAMgr Recover Requests
> Sent | The total number of AAAMGR Recovery Requests sent by the system to the GSS. These requests are sent when a AAA Mgr software task is restarted after an outage.
> Retried | The total number of AAAMGR Recovery Requests re-sent by the system to the GSS.
> Success | The total number of AAAMGR Recovery Requests successfully sent by the system to the GSS.
> Failed | The total number of AAAMGR Recovery Requests that failed to be sent by the system to the GSS.
> Clear DataBase Requests
> Sent | The total number of Clear Database Requests sent by the AAA Proxy to the GSS. These requests are sent after the AAA Proxy discovers that the GSS has come up again after a period of dormancy (i.e. the GSS moves from "down" to "up" state) so as to bring the GSS in sync with the state that the AAA Proxy is in.
> Retried | The total number of Clear Database Requests re-sent by the AAA Proxy to the GSS.
> Success | The total number of Clear Database Requests successfully sent by the AAA Proxy to the GSS.
> Failed | The total number of Clear Database Requests that failed to be sent by the AAA Proxy to the GSS.
> GCDR Purge Requests
> Received | The total number of G-CDR Purge Request messages received by the storage server. This request is sent by the GSS notifying the AAA Proxy of the purging of GTPP Requests due to buffer overflow.
> Responded | The total number of responses sent from the AAA Proxy to the GSS in response to "purge Requests".
> Generated File Requests
> Received | The total number of Generate File Request messages received by the storage server. This request is sent by the GSS notifying the AAA Proxy of the generation of unAcked files. The GTPP Requests purged by the GSS as a result of buffer overflow are moved to a file. This request indicates the completion of the moving of purged G-CDRs to the file.
> Responded | The total number of responses sent by the AAA Proxy to the GSS for the "Generated File Requests" received.
> Notification Received
> Outstanding GCDRs | The total number of notification for outstanding G-CDRs.
> Responded | The total number notifications received and responded for outstanding G-CDRs.
> Outstanding GCDRs cleared | The total number of notification for cleared outstanding G-CDRs.
> Responded | The total number notifications received and responded for clearing outstanding G-CDRs.
> CPU Usage Overlimit | The total number of notification received for CPU usage overlimit.
> Responded | The total number notifications received and responded for CPU usage overlimit.
> CPU Usage Normal | The total number of notification received for normal usage of CPU.
> Responded | The total number of notification received and responded for normal usage of CPU.
> Disk Usage Overlimit | The total number of notification received for disk usage overlimit.
> Responded | The total number notifications received and responded for disk usage overlimit.
> Disk Usage Normal | The total number of notification received for disk usage is in normal limit.
> Responded | The total number notifications received and responded for disk usage in normal limit.
> Cluster State Change | The total number of notification received for change in Cluster node status.
> Responded | The total number notifications received and responded for change in Cluster node status.
> Cluster Switchover | The total number of notification received for Cluster node switchover.
> Responded | The total number notifications received and responded for Cluster node switchover.
> Cluster Disk Path Failure | The total number of notification received for failure in Cluster disk path failure.
> Responded | The total number notifications received and responded for failure in Cluster disk path failure.
> Cluster Disk Path Normal | The total number of notification received for change in Cluster disk path from failure to normal.
> Responded | The total number notifications received and responded for change in Cluster disk path from failure to normal.
> Cluster Interconnect Failure | The total number of notification received for failure of interconnection between Cluster nodes.
> Responded | The total number notifications received and responded for failure of interconnection between Cluster nodes.
> Cluster Interconnect Normal | The total number of notification received for change in interconnection between Cluster nodes from failure to normal.
> Responded | The total number notifications received and responded for change in interconnection between Cluster nodes from failure to normal.
> Cluster Interface Failure | The total number of notification received for failure of interface of Cluster node.
> Responded | The total number notifications received and responded for failure of Cluster node interface.
> Cluster Interface Normal | The total number of notification received for change in status of Cluster node interface from failure to normal.
> Responded | The total number notifications received and responded for change in status of Cluster node interface from failure to normal.
> Cluster Memory Low | The total number of notification received for low memory at Cluster node.
> Responded | The total number notifications received and responded for low memory at Cluster node.
> Cluster Memory Normal | The total number of notification received for change in status of low memory to normal memory at Cluster node.
> Responded | The total number notifications received and responded for change in status of low memory to normal memory at Cluster node.
> Storage Server Counter Requests
> Sent | The total number of times the AAA Proxy sent "Storage Server Counter" requests to the GSS. This request is sent when "show gtpp storage-server counter" CLI is executed.
> Failed | The total number of times that the AAA Proxy failed to be send "Storage Server Counter" requests to the GSS.
> Success | The total number of times the AAA Proxy successfully sent "Storage Server Counter" requests to the GSS.
> Storage Server Status Requests
> Sent | The total number of times the AAA Proxy sent "Storage Server Status" requests to the GSS. This request is sent when "show gtpp storage-server status" CLI is executed.
> Failed | The total number of times that the AAA Proxy failed to be send "Storage Server Status" requests to the GSS.
> Success | The total number of times the AAA Proxy successfully sent "Storage Server Status" requests to the GSS.
> Fetch Requests
> Sent | The total number of "Fetch Requests" sent by the AAA Proxy to the GSS. This request is sent to discover the status of a particular GTPP Request (i.e. if it has been successfully stored but not sent to CGF, or if it is successfully stored and sent to CGF, or if it has not been received by GSS at all).
> Retried | The total number of "Fetch Requests" re-sent by the AAA Proxy to the GSS.
> Success | The total number of "Fetch Requests" successfully sent by the AAA Proxy to the GSS.
> Failed | The total number of "Fetch Requests" that failed to be sent by the AAA Proxy to the GSS.
> Echo Requests
> Sent | The total number of Echo requests sent by the AAA Proxy to the GSS.
> Success | The total number of Echo requests successfully sent by the AAA Proxy to the GSS.
> Commit Requests
> Sent | The total number of "commit requests" sent by the AAA Proxy to the GSS. This request is sent as a result of executing the "gtpp force-save" Exec mode command.
> Success | The total number of "commit requests" successfully sent by the AAA Proxy to the GSS.
> Update Requests
> Sent | The total number of requests sent by the AAA Proxy to the GSS to indicate the success of a request from the CGF.
> Invalid Request
> Received | The total number of invalid requests sent by the GSS to the AAA Proxy (i.e. when a GSS is reconfigured, all the requests from the old GSS are marked as invalid).
> Message Statistics
> Total Req Sent | The total number of requests sent to GSS.
> Total Store Req Sent | The total number of requests sent to GSS to store G-CDRs.
> Total Rsp Rcvd | The total number of requests responded to GSS.
> Total Store Req Sent | The total number of requests to store G-CDRs responded.
> Total Notif Msg Rcvd | The total number of notification messages received.
> Total Notif Rsp Sent | The total number of notification messages responded.
> Total Req Sent Failure | The total number of requests failed during sent.
> Invalid Socket State | The total number of requests failed during sent due to invalid socket state.
> MED/Socket Tx Failure | The total number of requests failed during sent due to Tx failure of mediation or socket.
> Store Response Time Statistics | Statistical information of response time for STORE messages.
> Get Next Response Time Statistics | Statistical information of response time of GET NEXT messages.
> GCDR distribution in DRT Messages | Distribution of G-CDRs in Data Request Transfer (DRT) messages.

> ‌
> show gtpp storage-server counters
> show gtpp storage-server counters Command Output Descriptions

> Field | Description
> Archived GTPP Requests | The total number of GTPP Requests archived with the GSS that have been responded to by the CGF.
> Archived Unack GTPP Requests | The total number of GTPP Requests archived with the GSS that have not yet been responded to by the CGF.
> Archived GCDRs | The total number of G-CDRs archived in "Acknowledged GTPPRequests".
> Archived Unack GCDRs | The total number of G-CDRs archived in "Unacknowledged GTPP Requests".

> ‌
> show gtpp storage-server local file counters
> show gtpp storage-server local file counters Command Output Descriptions

> Field | Description
> GTPP Req pending write | The total number of pending GTPP requests to write files to the hard disk..
> GTPP Req pending response | The total number responses sent to GTPP requests.
> File related counters
> Current file CDR count | The total number of files compressed.
> Files pending sync | The number of files that were not able to be compressed.
> Compr files pending sync | The number of files waiting to be synced.
> Compression in progress | The number of files being compressed.

> ‌
> show gtpp storage-server local file statistics
> show gtpp storage-server local file statistics Command Output Descriptions

> Field | Description
> Total CDR written | The total number of GTPP CDR files written to the hard disk.
> Total File Rotations | The total number of file rotation processes completed.
> File Rotation Type
> CDR-Count-limit | The total number of CDR files that have been rotated.
> Time-limit | Identifies the time limit for file rotation..
> Forced (0 CDRs) | Identifies the total number of zero-cdr files created at the local storage due to enabling of “force-file-rotation” trigger.
> Others | Total number of file rotations happened due to triggers not listed in this table when for local CDR files.
> File Compression
> Compression Success | The total number of files compressed.
> Compression Failures | The number of files that were not able to be compressed.

> ‌
> show gtpp storage-server status
> show gtpp storage server status Command Output Descriptions

> Field | Description
> Configuration
> Execution Mode | Execution mode of the G-CDRs.
> File Format | Specifies the file format used for CDRs.
> Max GCDRs per filet | Maximum number of G-CDRs per file.
> Notification Type | Type of notification.
> Poll Interval (min) | Poll interval in Minutes.
> Resource Monitor
> Outstanding GCDRs File Period (min) | Outstanding G-CDRs file period in minutes.
> CPU Usage(%) | CPU usage in percentage.
> Available Disk Gss Datafile Path (GB) | Threshold value for available disk size for path or partition on GSS node where CDR files are generated and stored by GSS Filegen application. Example: /sharedgss
> Available Disk Gss Install Path (GB) | Threshold value for available disk size for path or partition on GSS node where basic components of GSS like bin directory, config files, postgres bin directory and local log files are present. Example: /gss
> Available Disk Gss Database Path (GB) | Threshold value for available disk size for path or partition on GSS node where postgres database is installed. Example: /sharedpostgres
> Available Memory (MB) | Available memory at a given time.
> Resource Monitor Status
> Outstanding GCDRs File Period (min) | Number of outstanding G-CDR files during a given period of time (in minutes).
> State | State of the G-CDR collection.
> CPU Usage (%) | CPU usage in percentage.
> State | State of the CPU.
> Available Disk Gss Datafile Path (GB) State | Measured or current value for disk size for path or partition on GSS node where CDR files are generated and stored by GSS Filegen application. Example: /sharedgss If Measured or current value for disk size (GB) falls below configured limit (Threshold value), then Alarm is generated.
> Available Disk Gss Install Path (GB) State | Measured or current value for disk size for path or partition on GSS node where basic components of gss like bin directory, config files and postgres bin directory and local log files are present. Example : /gss If Measured or current value for disk size (GB) falls below configured limit (Threshold value), then Alarm is generated.
> Available Disk Gss Database Path (GB) State | Measured or current value for available disk size for path or partition on GSS node where postgres database is installed. Example: /sharedpostgres If Measured or current value for disk size (GB) falls below configured limit (Threshold value), then Alarm is generated.
> Available Memory (MB) | Amount of memory available for additional G-CDR files.
> State: | Condition of the available memory.
> Cluster Status
> Cluster Name | Name of the gss cluster.
> Online Cluster Node | Name of cluster node(s) that are online at the status collection time.
> Cluster Node List | Name(s) of the node(s) included in the cluster.

> ‌
> show gtpp storage-server streaming file statistics
> show gtpp storage-server streaming file statistics Command Output Descriptions

> Field | Description
> Total CDR written | Total number of streaming CDRs written into the RAM-Disk when gtpp storage-server “streaming” mode was enabled.
> Total CDR sent to remote | Total number of streaming CDRs sent to CGF from the HDD once the CGF/GTPP is up.
> Total Files Failed | During streaming if the CDR file is corrupted, the file will not stream to CGF and renamed to *.fail. This counters indicates the total number of such failed files.
> Total File Rotations | Total number of file rotations based on File Size, CDR count, time-limit when “streaming” mode was enabled. The file rotation triggers are configurable in GTPP Group Configuration mode.
> File Rotation Type
> File-Size-limit | Total number of file rotations happened due to “File-Size-limit” trigger when “streaming” mode was enabled.
> CDR-Count-limit | Total number of file rotations happened due to “CDR-Count-limit” trigger when “streaming” mode was enabled.
> Time-limit | Total number of file rotations happened due to “Time-limit” trigger when “streaming” mode was enabled.
> Forced (0 CDRs) | Identifies the total number of zero-cdr files created at the local storage due to enabling of “force-file-rotation” trigger.
> Others | Total number of file rotations happened due to triggers not listed in this table when “streaming” mode was enabled.

> ‌
> show gtpp storage-server streaming file statistics verbose
> show gtpp storage-server streaming file statistics verbose Command Output Descriptions

> Field | Description
> Accumulated Statistics:
> Total CDR written | Total number of streaming CDRs written into the RAM-Disk when gtpp storage-server “streaming” mode was enabled.
> Total CDR sent to remote | Total number of streaming CDRs sent to CGF from the HDD once the CGF/GTPP is up.
> Total CDR accepted | Total number of CDRs that are acknowledged by CGF (successfully streamed by the ASR 5000).
> Total CDR req already fulfilled | Total number of CDR requests that are already acknowledged by CGF. Important: When streaming is in progress from a file, the AAA proxy may crash. When AAA proxy is recovered, requests will not be sent from files that are acknowledged by CGF. Instead, the counter is incremented.
> Total Files sent to remote | Total number of CDR files sent to GTPP Storage Sever and acknowledged by CGF. Important: When streaming is in progress from a file, the AAA proxy may crash. When AAA proxy is recovered, requests will not be sent from files that are acknowledged by CGF. Instead, the counter is incremented.
> Total Files Failed | During streaming if the CDR file is corrupted, the file will not stream to CGF and renamed to *.fail. This counters indicates the total number of such failed files.
> Total File Rotations | Total number of file rotations based on File Size, CDR count, time-limit when “streaming” mode was enabled. The file rotation triggers are configurable in GTPP Group Configuration mode.
> File Rotation Type
> File-Size-limit | Total number of file rotations happened due to “File-Size-limit” trigger when “streaming” mode was enabled.
> CDR-Count-limit | Total number of file rotations happened due to “CDR-Count-limit” trigger when “streaming” mode was enabled.
> Time-limit | Total number of file rotations happened due to “Time-limit” trigger when “streaming” mode was enabled.
> Forced (0 CDRs) | Identifies the total number of zero-cdr files created at the local storage due to enabling of “force-file-rotation” trigger.
> Others | Total number of file rotations happened due to triggers not listed in this table when “streaming” mode was enabled.
> CDR distribution in DRT Messages
> 0: | Total number of Data Request Transfer (DRT) requests sent with no CDRs.
> 1: | Total number of Data Request Transfer (DRT) requests sent with one CDR.
> 2..5: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 2 to 5.
> 6..10: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 6 to 10.
> 11..15: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 11 to 15.
> 16..20: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 16 to 20.
> 21..40: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 21 to 40.
> 41..60: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 41 to 60.
> 61..80: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 61 to 80.
> 81..100: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 81 to 100.
> 101..150: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 101 to 150.
> 151..200: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 151 to 200.
> 201..254: | Total number of Data Request Transfer (DRT) requests sent where each request contains CDRs from 201 to 254.
> 255: | Total number of Data Request Transfer (DRT) requests sent where each request contains 255 CDRs.

> ‌
> show gtpp storage-server streaming file counters all
> show gtpp storage-server streaming file counters all Command Output Descriptions

> Field | Description
> GTPP Req pending write | Total number of CDR request queued up and not yet stored in RAM-Disk when “streaming” mode was enabled.
> GTPP Req pending response | Total number of GTPP request yet to send acknowledgement to the AAAMgr after storing the CDRs successfully in RAM-Disk when “streaming” mode was enabled.
> File related counters
> Current file CDR count | Total number of CDRs stored in RAM-disk file which is not yet synced to the HDD when “streaming” mode was enabled.
> Files pending sync | Total number of files waiting for the sync response from HDD when “streaming” mode was enabled.
> Current Pending CDRs in HDD | Total number of CDRs written into the hard-disk (Indicates the CDR count of rotated files) when “streaming” mode was enabled.
> Current Pending Files in HDD | Total number of files stored in hard-disk when “streaming” mode was enabled.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883