> HNB-CS Network Configuration Mode Commands
> The HNB-CS Network Configuration Mode is used to create, provide, and manage the Circuit Switched (CS) network instance on HNB-GW service to provide HNB access with CS core network in a 3G UMTS network.
> associate alcap-service
> This command associates a previously defined Access Link Control Application Part (ALCAP) service with the CS network instance for multiplexing of different users onto one AAL2 transmission path using channel IDs (CIDs). This configuration is provided to support IuCS-over-ATM functionality
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate alcap-service svc_name context ctx_name
> no associate alcap-service
> no
> Removes the associated ALCAP service from this HNB-CS network instance configuration.
> svc_name
> Identifies the name of the ALCAP service preconfigured in Context configuration mode to associate with an HNB-CS network instance for multiplexing of different users onto one AAL2 transmission path using channel IDs (CIDs).
> The svc_name must be a preconfigured ALCAP service.
> Only one instance of this command can be configured.
> Caution: If this CLI is not configured any RAB-ASST-REQ requesting AAL2 connection setup shall be rejected with an appropriate cause.
> context ctx_name
> Specifies the name of the context in which ALCAP service is configured.
> The ctx_name must be an existing context name in which this ALCAP service is configured.
> Usage
> Use this command to configure IuCS-over-ATM support. This association of ALCAP protocol service configuration in HNB-CS network instance provides multiplexing of different users onto one AAL2 transmission path using channel IDs (CIDs).
> Caution: If this CLI is not configured any RAB-ASST-REQ message requesting AAL2 connection setup shall be rejected with an appropriate cause.
> Important: This command must not be used more than once to configure IuCS-over-ATM support.
> Example
> Following command associates ALCAP service alcap_svc1 configured in conext named Ctx_alcap1 with specific HNB-CS network instance:
> associate alcap-service alcap_svc1 context Ctx_alcap1
> associate rtp pool
> This command associates a previously defined RTP pool (IP pool) with the CS network instance to be used for assignment of IP address/port as RTP streams end point address over IuCS interface. This configuration support is provided for RTP stream management feature in an HNB-GW service.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate rtp pool pool_name context ctx_name
> no associate rtp pool
> no
> Removes the associated RTP pool (IP pool) from this HNB-CS network instance configuration.
> pool_name
> Identifies the name of the RTP IP pool preconfigured in Context configuration mode to associate with an HNB-CS network instance to be used for assignment of IP address/port over the IuCS interface RTP streams.
> The pool_name must be an existing IP pool name configured in Context configuration mode.
> Important: For IP pool (RTP pool) configuration, refer Context Configuration Commands Mode chapter.
> context ctx_name
> Specifies the name of the context in which RTP pool (IP pool) is configured.
> The ctx_name must be an existing context name in which this IP pool is configured.
> Usage
> Use this command to associate RTP pool (IP Pool) with an HNB-CS network instance for allotment of IP address/port over IuCS interface for RTP streams across all sessions. A fixed range of RTP ports from 5000 through 65000 shall be used to allocate to RTP stream.
> Important: This command must be used to provide IP address/port for RTP streams end point address over IuCS interface.
> Important: This configuration support is provided for RTP stream management feature on an HNB-GW service.
> Example
> Following command associates RTP pool named rtp_1 with specific HNB-CS network instance:
> associate rtp pool rtp_1
> associate sccp-network
> This command associates a predefined Signaling Connection Control Part (SCCP) network id with the CS network instance in order to route the messages towards MSC/VLR over IuCS interface.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> associate-sccp-network sccp_net_id
> no associate-sccp-network
> no
> Removes the associated SCCP network id from this HNB-CS network instance configuration.
> sccp_network_id
> Identifies the predefined SCCP network id to associate with an HNB-CS network instance over IuCS/IuFlex interface to enable connection with MSC/VLR(s).
> The sccp_network_id must be a predefined SCCP network id in Global configuration mode.
> Usage
> Use this command to associate a preconfigured SCCP network id over IuCS interface in HNB-GW service to connect with CS network elements; i.e. MSC.
> Caution: The SCCP network id must be defined in Global Configuration mode before using it with this command.
> Important: A single SCCP network configuration instance can not be shared with multiple HNB-CS network instances.
> Example
> Following command associates SCCP network 2 with specific HNB-CS network instance:
> associate-sccp-network 2
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> msc point-code
> This command is used to configure default MSC point-code with HNB-CS network instance. This command is used when HNB-GW is to be connected to only one MSC with in a CS network or as default MSC for all HNBs connected through specific HNB-CS network instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] msc point-code point_code
> no
> Removes the configured default MSC point code from specific HNB-CS network instance.
> Caution: Removing the MSC point code is a disruptive operation and affects all HNB sessions which are connected to particular MSC through an HNB-CS network instance.
> msc point_code
> Specifies SS7 address of default MSC in CS network in point code value to this configured HNB-CS network instance.
> point_code must be in SS7 point code dotted-decimal ###.###.### format or 8-digit decimal ######## format.
> Only one instance of this command can be configured.
> Usage
> Use this command to configure a default MSC to which HNB will connect for CS network access through HNB-GW service.
> Point-code is an SS7 address for an element in the SS7 network. Point-codes must be defined in dotted-decimal format in a string of 1 to 11 digits. Format options include:

> • | 0.0.1 to 7.255.7 for point-code in the ITU range.

> • | 0.0.1 to 255.255.255 for point-code in the ANSI range.

> • | 0.0.1 to 15.31.255 for point-code in the TTC Range.

> • | a string of 1 to 11 digits in dotted-decimal to represent a point-code in a different range.

> Important: This command can be entered only once. If entered again the previous value shall be overwritten.
> Example
> The following command configures a default MSC with point code 01.201.101 for HNBs to access CS network through HNB-GW service in this HNB-CS network instance:
> msc point-code 101.201.101

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883